TIMETRA-BIER-MIB DEFINITIONS ::= BEGIN

IMPORTS
    InetAddress, InetAddressType
                                                         FROM INET-ADDRESS-MIB
    MODULE-COMPLIANCE, NOTIFICATION-GROUP,
    OBJECT-GROUP
                                                         FROM SNMPv2-CONF
    Counter32, MODULE-IDENTITY,
    NOTIFICATION-TYPE, OBJECT-TYPE,
    Unsigned32
                                                         FROM SNMPv2-SMI
    RowStatus, TEXTUAL-CONVENTION,
    TimeStamp, TruthValue
                                                         FROM SNMPv2-TC
    timetraSRMIBModules, tmnxSRConfs,
    tmnxSRNotifyPrefix, tmnxSRObjs
                                                         FROM TIMETRA-GLOBAL-MIB
    TLNamedItemOrEmpty, TNamedItem,
    TmnxAdminState, TmnxLongDisplayString,
    TmnxOperState
                                                         FROM TIMETRA-TC-MIB
    vRtrID, vRtrIfIndex
                                                         FROM TIMETRA-VRTR-MIB
    ;

timetraBierMIBModule             MODULE-IDENTITY
    LAST-UPDATED "201801010000Z"
    ORGANIZATION "Nokia"
    CONTACT-INFO
        "Nokia SROS Support
         Web: http://www.nokia.com"
    DESCRIPTION
        "This document is the SNMP MIB module to manage and provision the
         extensions to the BIER routing protocol for the Nokia SROS device.

         Copyright 2008-2018 Nokia.  All rights reserved.  Reproduction of this
         document is authorized on the condition that the foregoing copyright
         notice is included.

         This SNMP MIB module (Specification) embodies Nokia's proprietary
         intellectual property.  Nokia retains all title and ownership in the
         Specification, including any revisions.

         Nokia grants all interested parties a non-exclusive license to use and
         distribute an unmodified copy of this Specification in connection with
         management of Nokia products, and without fee, provided this copyright
         notice and license appear on all copies.

         This Specification is supplied 'as is', and Nokia makes no warranty,
         either express or implied, as to the use, operation, condition, or
         performance of the Specification."

    REVISION    "201801010000Z"
    DESCRIPTION
        "Rev 0.1                01 Jan 2018 00:00
         Initial version of the TIMETRA-BIER-MIB."

    ::= { timetraSRMIBModules 123 }

TmnxBierMultiTopology            ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "TmnxBierMultiTopology is an enumerated integer that specifies the ISIS
         Multi Topology."
    SYNTAX      INTEGER {
        ipv4-unicast   (0),
        ipv6-unicast   (2),
        ipv4-multicast (3),
        ipv6-multicast (4)
    }

tmnxBierObjs                     OBJECT IDENTIFIER ::= { tmnxSRObjs 123 }

vRtrBierGeneralTableLastChanged  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierGeneralTableLastChanged indicates the sysUpTime
         at the time of the last modification of an entry in the
         vRtrBierGeneralTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxBierObjs 1 }

vRtrBierGeneralTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierGeneralEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierGeneralTable contains objects for general control and
         management of the BIER protocol instance within a virtual router."
    ::= { tmnxBierObjs 2 }

vRtrBierGeneralEntry             OBJECT-TYPE
    SYNTAX      VRtrBierGeneralEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of the BIER protocol running
         within a virtual router.

         Row entries can be created or deleted via SNMP SET
         requests.  A row with default attribute values is created
         by setting vRtrBierGeneralRowStatus to 'createAndGo'. A row
         entry can be destroyed by setting vRtrBierGeneralRowStatus
         to 'destroy'."
    INDEX       { vRtrID }
    ::= { vRtrBierGeneralTable 1 }

VRtrBierGeneralEntry             ::= SEQUENCE
{
    vRtrBierGeneralRowStatus         RowStatus,
    vRtrBierGeneralAdminState        TmnxAdminState,
    vRtrBierGeneralRowLastChange     TimeStamp,
    vRtrBierGeneralFrr               TruthValue,
    vRtrBierGeneralBfdEnabled        BITS,
    vRtrBierGenServRsvdLblBlockName  TLNamedItemOrEmpty
}

vRtrBierGeneralRowStatus         OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrBierGeneralRowStatus is used to control the creation and deletion
         of rows in the vRtrBierGeneralTable.

         A row can be created by setting
         vRtrBierGeneralRowStatus to 'createAndGo'.  The agent
         should assign the default attribute values and change
         the row status to 'active'.

         A row entry can be destroyed by setting vRtrBierGeneralRowStatus to
         'destroy'."
    ::= { vRtrBierGeneralEntry 1 }

vRtrBierGeneralAdminState        OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierGeneralAdminState specifies the current
         administrative state of this BIER instance."
    DEFVAL      { outOfService }
    ::= { vRtrBierGeneralEntry 2 }

vRtrBierGeneralRowLastChange     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierGeneralRowLastChange indicates the sysUpTime when
         this row was last modified."
    ::= { vRtrBierGeneralEntry 3 }

vRtrBierGeneralFrr               OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierGeneralFrr specifies whether fast reroute for
         BIER is enabled or disabled."
    DEFVAL      { false }
    ::= { vRtrBierGeneralEntry 4 }

vRtrBierGeneralBfdEnabled        OBJECT-TYPE
    SYNTAX      BITS {
        ipv4 (0)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierGeneralBfdEnabled specifies whether BFD tracking
         is enabled for BIER next-hops. When this object has a value of 'ipv4',
         BFD tracking is enabled for each resolved ipv4 next-hop. When this
         object has value of 0, BFD tracking is disabled."
    DEFVAL      { {} }
    ::= { vRtrBierGeneralEntry 5 }

vRtrBierGenServRsvdLblBlockName  OBJECT-TYPE
    SYNTAX      TLNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierGenServRsvdLblBlockName specifies the reserved
         static label block. The reserved label block name is defined by
         vRtrMplsReservedLblBlkName and is the index for
         TIMETRA-MPLS-MIB::vRtrMplsReservedLblBlkTable."
    DEFVAL      { "" }
    ::= { vRtrBierGeneralEntry 6 }

vRtrBierTemplateTableLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTemplateTableLastChanged indicates the sysUpTime
         at the time of the last modification of an entry in the
         vRtrBierTemplateTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxBierObjs 3 }

vRtrBierTemplateTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierTemplateEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierTemplateTable lists BIER policies for a particular BIER
         instance. BIER template depicts how BIER routing underlay should
         advertise the BIER information throughout the network."
    ::= { tmnxBierObjs 4 }

vRtrBierTemplateEntry            OBJECT-TYPE
    SYNTAX      VRtrBierTemplateEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry corresponds to a BIER template which indicates a BIER
         Domain. One such template entry would be associated with routing for
         BIER routing overlay.

         Row entries can be created or deleted via SNMP SET
         requests.  A row with default attribute values is created
         by setting vRtrBierTemplateRowStatus to 'createAndGo'. A
         row entry can be destroyed by setting
         vRtrBierTemplateRowStatus to 'destroy'."
    INDEX       {
        vRtrID,
        vRtrBierTemplateName
    }
    ::= { vRtrBierTemplateTable 1 }

VRtrBierTemplateEntry            ::= SEQUENCE
{
    vRtrBierTemplateName             TNamedItem,
    vRtrBierTemplateRowStatus        RowStatus,
    vRtrBierTemplateAdminState       TmnxAdminState,
    vRtrBierTemplateRowLastChange    TimeStamp
}

vRtrBierTemplateName             OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTemplateName specifies the template name of
         vRtrBierTemplateEntry"
    ::= { vRtrBierTemplateEntry 1 }

vRtrBierTemplateRowStatus        OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrBierTemplateRowStatus is used to control the creation and deletion
         of rows in the vRtrBierTemplateTable.

         A row can be created by setting
         vRtrBierTemplateRowStatus to 'createAndGo'.  The agent
         should assign the default attribute values and change
         the row status to 'active'.

         A row entry can be destroyed by setting vRtrBierTemplateRowStatus to
         'destroy'."
    ::= { vRtrBierTemplateEntry 2 }

vRtrBierTemplateAdminState       OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTemplateAdminState specifies the current
         administrative state of this BIER instance."
    DEFVAL      { outOfService }
    ::= { vRtrBierTemplateEntry 3 }

vRtrBierTemplateRowLastChange    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTemplateRowLastChange indicates the sysUpTime
         when this row was last modified."
    ::= { vRtrBierTemplateEntry 4 }

vRtrBierSubDomainTableLstChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierSubDomainTableLstChanged indicates the sysUpTime
         at the time of the last modification of an entry in the
         vRtrBierSubDomainTableLstChanged.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxBierObjs 5 }

vRtrBierSubDomainTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierSubDomainEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierSubDomainTable contains objects for general control and
         management of the BIER sub-domains within the corresponding template
         specified in vRtrBierTemplateTable."
    ::= { tmnxBierObjs 6 }

vRtrBierSubDomainEntry           OBJECT-TYPE
    SYNTAX      VRtrBierSubDomainEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of the BIER sub- domain running
         within the corresponding template specified in vRtrBierTemplateTable.

         A BIER Template is a BIER domain which may contain one or more
         sub-domain. Each BIER domain must contain at least one sub-domain in
         order for the template to be advertised.

         Row entries can be created or deleted via SNMP SET
         requests.  A row with default attribute values is created
         by setting vRtrBierSubDomainRowStatus to 'createAndGo'. A
         row entry can be destroyed by setting
         vRtrBierSubDomainRowStatus to 'destroy'."
    INDEX       {
        vRtrID,
        vRtrBierTemplateName,
        vRtrBierSubDomainStart,
        vRtrBierSubDomainEnd
    }
    ::= { vRtrBierSubDomainTable 1 }

VRtrBierSubDomainEntry           ::= SEQUENCE
{
    vRtrBierSubDomainStart           Unsigned32,
    vRtrBierSubDomainEnd             Unsigned32,
    vRtrBierSubDomainPrefixType      InetAddressType,
    vRtrBierSubDomainPrefix          InetAddress,
    vRtrBierSubDomainBfrId           Unsigned32,
    vRtrBierSubDomainMT              TmnxBierMultiTopology,
    vRtrBierSubDomainRowStatus       RowStatus,
    vRtrBierSubDomainRowLastChange   TimeStamp
}

vRtrBierSubDomainStart           OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierSubDomainStart specifies the BIER sub-domain
         start value."
    ::= { vRtrBierSubDomainEntry 1 }

vRtrBierSubDomainEnd             OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierSubDomainEnd specifies the BIER sub-domain end
         value. For single sub-domain range the start and end value is same. "
    ::= { vRtrBierSubDomainEntry 2 }

vRtrBierSubDomainPrefixType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierSubDomainPrefixType specifies the address type of
         vRtrBierSubDomainPrefix address."
    DEFVAL      { unknown }
    ::= { vRtrBierSubDomainEntry 3 }

vRtrBierSubDomainPrefix          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierSubDomainPrefix specifies the address of the BFR
         prefix to be advertised in this sub-domain or the sub Domain range."
    ::= { vRtrBierSubDomainEntry 4 }

vRtrBierSubDomainBfrId           OBJECT-TYPE
    SYNTAX      Unsigned32 (0..4096)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierSubDomainBfrId specifies the BFR ID within the
         BIER sub-domain. A BFR ID uniquely identifies a BFIR/BFER within the
         sub-domain. A value of '0' indicates that the sub-domain range will
         not be advertised."
    DEFVAL      { 0 }
    ::= { vRtrBierSubDomainEntry 5 }

vRtrBierSubDomainMT              OBJECT-TYPE
    SYNTAX      TmnxBierMultiTopology
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object vRtrBierSubDomainMT specifies the ISIS
         multi-topology ID where the BIER template should be applied."
    DEFVAL      { ipv4-unicast }
    ::= { vRtrBierSubDomainEntry 6 }

vRtrBierSubDomainRowStatus       OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrBierSubDomainRowStatus is used to control the creation and
         deletion of rows in the vRtrBierSubDomainTable.

         A row can be created by setting
         vRtrBierSubDomainRowStatus to 'createAndGo'.  The agent
         should assign the default attribute values and change
         the row status to 'active'.

         A row entry can be destroyed by setting vRtrBierSubDomainRowStatus to
         'destroy'."
    ::= { vRtrBierSubDomainEntry 7 }

vRtrBierSubDomainRowLastChange   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierSubDomainRowLastChange indicates the sysUpTime
         when this row was last modified."
    ::= { vRtrBierSubDomainEntry 8 }

vRtrBierDatabaseTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierDatabaseEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierDatabaseTable contains objects for BIER database of the
         BIER protocol instance within a virtual router."
    ::= { tmnxBierObjs 7 }

vRtrBierDatabaseEntry            OBJECT-TYPE
    SYNTAX      VRtrBierDatabaseEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row represents an entry in vRtrBierDatabaseTable."
    INDEX       {
        vRtrID,
        vRtrBierTemplateName,
        vRtrBierDatabaseSubDomainId
    }
    ::= { vRtrBierDatabaseTable 1 }

VRtrBierDatabaseEntry            ::= SEQUENCE
{
    vRtrBierDatabaseSubDomainId      Unsigned32,
    vRtrBierDatabaseBitStringLen     Unsigned32,
    vRtrBierDatabasePrefixType       InetAddressType,
    vRtrBierDatabasePrefix           InetAddress,
    vRtrBierDatabaseBfrId            Unsigned32,
    vRtrBierDatabaseMT               TmnxBierMultiTopology,
    vRtrBierDatabaseMplsLabelStart   Unsigned32,
    vRtrBierDatabaseMplsLabelEnd     Unsigned32,
    vRtrBierDatabaseMplsLabelTotal   Unsigned32
}

vRtrBierDatabaseSubDomainId      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierDatabaseSubDomainId indicates the BIER sub-domain
         start value."
    ::= { vRtrBierDatabaseEntry 1 }

vRtrBierDatabaseBitStringLen     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierDatabaseBitStringLen indicates the current
         supported bit string length."
    ::= { vRtrBierDatabaseEntry 2 }

vRtrBierDatabasePrefixType       OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierDatabasePrefixType indicates the address type of
         vRtrBierSubDomainPrefix address."
    DEFVAL      { unknown }
    ::= { vRtrBierDatabaseEntry 3 }

vRtrBierDatabasePrefix           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierDatabasePrefix indicates the address of the BFR
         prefix to be advertised in this sub-domain or the sub-domain range."
    ::= { vRtrBierDatabaseEntry 4 }

vRtrBierDatabaseBfrId            OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierDatabaseBfrId indicates the BFR ID within the
         BIER sub-domain. A BFR ID uniquely identifies a BFIR/BFER within the
         sub-domain. A value of '0' indicates that the sub-domain range will
         not be advertised."
    ::= { vRtrBierDatabaseEntry 5 }

vRtrBierDatabaseMT               OBJECT-TYPE
    SYNTAX      TmnxBierMultiTopology
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object vRtrBierDatabaseMT indicates the ISIS
         Multi-topology ID where the BIER template should be applied."
    ::= { vRtrBierDatabaseEntry 6 }

vRtrBierDatabaseMplsLabelStart   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object vRtrBierDatabaseMplsLabelStart indicates the
         mpls start label."
    ::= { vRtrBierDatabaseEntry 7 }

vRtrBierDatabaseMplsLabelEnd     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object vRtrBierDatabaseMplsLabelEnd indicates the
         mpls end label."
    ::= { vRtrBierDatabaseEntry 8 }

vRtrBierDatabaseMplsLabelTotal   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object vRtrBierDatabaseMplsLabelTotal indicates the
         total number of mpls labels."
    ::= { vRtrBierDatabaseEntry 9 }

vRtrBierForwardingTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierForwardingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierForwardingTable contains objects for BIER forwarding of
         the BIER protocol instance within a virtual router."
    ::= { tmnxBierObjs 8 }

vRtrBierForwardingEntry          OBJECT-TYPE
    SYNTAX      VRtrBierForwardingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row represents an entry in vRtrBierForwardingTable."
    INDEX       {
        vRtrID,
        vRtrBierForwardingSubDomainId,
        vRtrBierForwardingBitStringLen,
        vRtrBierForwardingNhopPrefixType,
        vRtrBierForwardingNhopPrefix,
        vRtrBierForwardingNhopIfIndex,
        vRtrBierForwardingBierSetId
    }
    ::= { vRtrBierForwardingTable 1 }

VRtrBierForwardingEntry          ::= SEQUENCE
{
    vRtrBierForwardingSubDomainId    Unsigned32,
    vRtrBierForwardingBitStringLen   Unsigned32,
    vRtrBierForwardingNhopPrefixType InetAddressType,
    vRtrBierForwardingNhopPrefix     InetAddress,
    vRtrBierForwardingNhopIfIndex    Unsigned32,
    vRtrBierForwardingBierSetId      Unsigned32,
    vRtrBierForwardingNbrPrefixType  InetAddressType,
    vRtrBierForwardingNbrPrefix      InetAddress,
    vRtrBierForwardingBitMask        TmnxLongDisplayString,
    vRtrBierForwardingMplsLabel      Unsigned32,
    vRtrBierForwardingBkupNbrPfxType InetAddressType,
    vRtrBierForwardingBkupNbrPrefix  InetAddress,
    vRtrBierFwrdingBkupNhopPfxType   InetAddressType,
    vRtrBierForwardingBkupNhopPrefix InetAddress,
    vRtrBierForwardingBkupNhopIfIdx  Unsigned32,
    vRtrBierForwardingBkupBitMask    TmnxLongDisplayString,
    vRtrBierForwardingBkupMplsLabel  Unsigned32
}

vRtrBierForwardingSubDomainId    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingSubDomainId indicates the BIER
         sub-domain start value."
    ::= { vRtrBierForwardingEntry 1 }

vRtrBierForwardingBitStringLen   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingBitStringLen indicates the current
         supported bit string length."
    ::= { vRtrBierForwardingEntry 2 }

vRtrBierForwardingNhopPrefixType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingNhopPrefixType indicates the address
         type of vRtrBierForwardingNhopPrefix address."
    DEFVAL      { unknown }
    ::= { vRtrBierForwardingEntry 3 }

vRtrBierForwardingNhopPrefix     OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingNhopPrefix indicates the address of the
         next hop prefix."
    ::= { vRtrBierForwardingEntry 4 }

vRtrBierForwardingNhopIfIndex    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingNhopIfIndex indicated the next hope
         interface index."
    ::= { vRtrBierForwardingEntry 5 }

vRtrBierForwardingBierSetId      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingBierSetId indicates the set identifier."
    ::= { vRtrBierForwardingEntry 6 }

vRtrBierForwardingNbrPrefixType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingNbrPrefixType indicates the address
         type of vRtrBierSubDomainPrefix address."
    ::= { vRtrBierForwardingEntry 7 }

vRtrBierForwardingNbrPrefix      OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingNbrPrefix indicates the address of the
         BFR prefix to be advertised in this sub-domain or the sub-domain
         range."
    ::= { vRtrBierForwardingEntry 8 }

vRtrBierForwardingBitMask        OBJECT-TYPE
    SYNTAX      TmnxLongDisplayString (SIZE (0..256))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingBitMask indicates the Forwarding Bit
         Mask (F-BM) for a particular BFR neighbor and SI."
    ::= { vRtrBierForwardingEntry 9 }

vRtrBierForwardingMplsLabel      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingMplsLabel indicates the service BIER
         label for the sender tunnel."
    ::= { vRtrBierForwardingEntry 10 }

vRtrBierForwardingBkupNbrPfxType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingBkupNbrPfxType indicates the address
         type of vRtrBierForwardingBkupNbrPrefix address."
    ::= { vRtrBierForwardingEntry 11 }

vRtrBierForwardingBkupNbrPrefix  OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingBkupNbrPrefix indicates the address of
         the backup neighbor's BFR prefix."
    ::= { vRtrBierForwardingEntry 12 }

vRtrBierFwrdingBkupNhopPfxType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierFwrdingBkupNhopPfxType indicates the address type
         of vRtrBierForwardingBkupNhopPrefix address."
    ::= { vRtrBierForwardingEntry 13 }

vRtrBierForwardingBkupNhopPrefix OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingBkupNhopPrefix indicates the address of
         the backup next hop prefix."
    ::= { vRtrBierForwardingEntry 14 }

vRtrBierForwardingBkupNhopIfIdx  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingBkupNhopIfIdx indicates the interface
         index of the backup next-hop."
    ::= { vRtrBierForwardingEntry 15 }

vRtrBierForwardingBkupBitMask    OBJECT-TYPE
    SYNTAX      TmnxLongDisplayString (SIZE (0..256))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingBkupBitMask indicates the Forwarding
         Bit Mask (F-BM) for the backup BFR neighbor."
    ::= { vRtrBierForwardingEntry 16 }

vRtrBierForwardingBkupMplsLabel  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierForwardingBkupMplsLabel indicates the BIER label
         for the backup next-hop."
    ::= { vRtrBierForwardingEntry 17 }

vRtrBierRoutingTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierRoutingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierRoutingTable contains objects for BIER routing of the BIER
         protocol instance within a virtual router."
    ::= { tmnxBierObjs 9 }

vRtrBierRoutingEntry             OBJECT-TYPE
    SYNTAX      VRtrBierRoutingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row represents an entry in vRtrBierRoutingTable."
    INDEX       {
        vRtrID,
        vRtrBierRoutingSubDomainId,
        vRtrBierRoutingBitStringLen,
        vRtrBierRoutingNhopPrefixType,
        vRtrBierRoutingNhopPrefix,
        vRtrBierRoutingNhopIfIndex,
        vRtrBierRoutingDestPrefixType,
        vRtrBierRoutingDestPrefix
    }
    ::= { vRtrBierRoutingTable 1 }

VRtrBierRoutingEntry             ::= SEQUENCE
{
    vRtrBierRoutingSubDomainId       Unsigned32,
    vRtrBierRoutingBitStringLen      Unsigned32,
    vRtrBierRoutingNhopPrefixType    InetAddressType,
    vRtrBierRoutingNhopPrefix        InetAddress,
    vRtrBierRoutingNhopIfIndex       Unsigned32,
    vRtrBierRoutingDestPrefixType    InetAddressType,
    vRtrBierRoutingDestPrefix        InetAddress,
    vRtrBierRoutingNbrPrefixType     InetAddressType,
    vRtrBierRoutingNbrPrefix         InetAddress,
    vRtrBierRoutingBfrId             Unsigned32,
    vRtrBierRoutingLastUpdated       TimeStamp,
    vRtrBierRoutingBkupNbrPfxType    InetAddressType,
    vRtrBierRoutingBkupNbrPrefix     InetAddress,
    vRtrBierRoutingBkupNhopPfxType   InetAddressType,
    vRtrBierRoutingBkupNhopPrefix    InetAddress,
    vRtrBierRoutingBkupNhopIfIndex   Unsigned32
}

vRtrBierRoutingSubDomainId       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingSubDomainId indicates the BIER sub-domain
         start value."
    ::= { vRtrBierRoutingEntry 1 }

vRtrBierRoutingBitStringLen      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingBitStringLen indicates the current
         supported bit string length."
    ::= { vRtrBierRoutingEntry 2 }

vRtrBierRoutingNhopPrefixType    OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingNhopPrefixType indicates the address type
         of vRtrBierRoutingNhopPrefix address."
    DEFVAL      { unknown }
    ::= { vRtrBierRoutingEntry 3 }

vRtrBierRoutingNhopPrefix        OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingNhopPrefix indicates the address of
         destination prefix."
    ::= { vRtrBierRoutingEntry 4 }

vRtrBierRoutingNhopIfIndex       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingNhopIfIndex indicates the next hop
         interface index."
    ::= { vRtrBierRoutingEntry 5 }

vRtrBierRoutingDestPrefixType    OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingDestPrefixType indicates the address type
         of vRtrBierRoutingDestPrefix address."
    DEFVAL      { unknown }
    ::= { vRtrBierRoutingEntry 6 }

vRtrBierRoutingDestPrefix        OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingDestPrefix indicates the address of
         destination prefix."
    ::= { vRtrBierRoutingEntry 7 }

vRtrBierRoutingNbrPrefixType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingNbrPrefixType indicates the address type
         of vRtrBierRoutingNbrPrefix address."
    ::= { vRtrBierRoutingEntry 8 }

vRtrBierRoutingNbrPrefix         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingNbrPrefix indicates the address of the BFR
         prefix to be advertised in this sub-domain or the sub-domain range."
    ::= { vRtrBierRoutingEntry 9 }

vRtrBierRoutingBfrId             OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingBfrId indicates the BFR ID within the BIER
         sub-domain. A BFR ID uniquely identifies a BFIR/BFER within the
         sub-domain. A value of '0' indicates that the sub-domain range will
         not be advertised."
    ::= { vRtrBierRoutingEntry 10 }

vRtrBierRoutingLastUpdated       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingLastUpdated indicates the sysUpTime when
         this route was last updated."
    ::= { vRtrBierRoutingEntry 11 }

vRtrBierRoutingBkupNbrPfxType    OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingBkupNbrPfxType indicates the address type
         of vRtrBierRoutingBkupNbrPrefix address."
    ::= { vRtrBierRoutingEntry 12 }

vRtrBierRoutingBkupNbrPrefix     OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingBkupNbrPrefix indicates the address of the
         backup BFR neighbor prefix."
    ::= { vRtrBierRoutingEntry 13 }

vRtrBierRoutingBkupNhopPfxType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingBkupNhopPfxType indicates the address type
         of vRtrBierRoutingBkupNhopPrefix address."
    ::= { vRtrBierRoutingEntry 14 }

vRtrBierRoutingBkupNhopPrefix    OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingBkupNhopPrefix indicates the address of
         the backup next-hop."
    ::= { vRtrBierRoutingEntry 15 }

vRtrBierRoutingBkupNhopIfIndex   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierRoutingBkupNhopIfIndex indicates the interface
         index of the backup next-hop."
    ::= { vRtrBierRoutingEntry 16 }

vRtrBierTunnelTable              OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierTunnelEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierTunnelTable contains objects for BIER Tunnel of the BIER
         protocol instance within a virtual router."
    ::= { tmnxBierObjs 10 }

vRtrBierTunnelEntry              OBJECT-TYPE
    SYNTAX      VRtrBierTunnelEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row represents an entry in vRtrBierTunnelTable."
    INDEX       {
        vRtrID,
        vRtrIfIndex
    }
    ::= { vRtrBierTunnelTable 1 }

VRtrBierTunnelEntry              ::= SEQUENCE
{
    vRtrBierTunnelType               INTEGER,
    vRtrBierTunnelPrefixType         InetAddressType,
    vRtrBierTunnelPrefix             InetAddress,
    vRtrBierTunnelSubDomain          Unsigned32,
    vRtrBierTunnelMplsLabel          Unsigned32,
    vRtrBierTunnelBfrId              Unsigned32,
    vRtrBierTunnelOperState          TmnxAdminState,
    vRtrBierTunnelNumLeaves          Unsigned32,
    vRtrBierTunnelLastOperDownReason Unsigned32,
    vRtrBierTunnelIsInBand           TruthValue
}

vRtrBierTunnelType               OBJECT-TYPE
    SYNTAX      INTEGER {
        tx (0),
        rx (1)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTunnelType indicates whether this tunnel is of
         type transmitter or receiver."
    ::= { vRtrBierTunnelEntry 1 }

vRtrBierTunnelPrefixType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTunnelPrefixType indicates the address type of
         vRtrBierSubDomainPrefix address."
    ::= { vRtrBierTunnelEntry 2 }

vRtrBierTunnelPrefix             OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTunnelPrefix indicates the address of the BFR
         prefix to be advertised in this sub-domain or the sub Domain range."
    ::= { vRtrBierTunnelEntry 3 }

vRtrBierTunnelSubDomain          OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTunnelSubDomain indicates the sub domain
         identifier."
    ::= { vRtrBierTunnelEntry 4 }

vRtrBierTunnelMplsLabel          OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTunnelMplsLabel indicates the service BIER level
         label."
    ::= { vRtrBierTunnelEntry 5 }

vRtrBierTunnelBfrId              OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTunnelBfrId indicates the BFD ID."
    ::= { vRtrBierTunnelEntry 6 }

vRtrBierTunnelOperState          OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTunnelOperState indicates the tunnel operational
         status."
    ::= { vRtrBierTunnelEntry 7 }

vRtrBierTunnelNumLeaves          OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTunnelNumLeaves indicates number of leaves per tx
         tunnels."
    ::= { vRtrBierTunnelEntry 8 }

vRtrBierTunnelLastOperDownReason OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTunnelLastOperDownReason indicates the last
         operdown reason."
    ::= { vRtrBierTunnelEntry 9 }

vRtrBierTunnelIsInBand           OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTunnelIsInBand indicates whether bier tunnel is
         inBand or not."
    ::= { vRtrBierTunnelEntry 10 }

vRtrBierTxTunnelLeafTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierTxTunnelLeafEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierTxTunnelLeafTable contains objects for BIER Tunnel Leaf of
         the BIER protocol instance within a virtual router."
    ::= { tmnxBierObjs 11 }

vRtrBierTxTunnelLeafEntry        OBJECT-TYPE
    SYNTAX      VRtrBierTxTunnelLeafEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row represents an entry in vRtrBierTunnelTable."
    INDEX       {
        vRtrID,
        vRtrIfIndex,
        vRtrBierTxTunnelLeafPrefixType,
        vRtrBierTxTunnelLeafPrefix
    }
    ::= { vRtrBierTxTunnelLeafTable 1 }

VRtrBierTxTunnelLeafEntry        ::= SEQUENCE
{
    vRtrBierTxTunnelLeafPrefixType   InetAddressType,
    vRtrBierTxTunnelLeafPrefix       InetAddress,
    vRtrBierTxTunnelMvpnId           Unsigned32,
    vRtrBierTxTunnelOperState        TmnxAdminState,
    vRtrBierTxTunnelPtaPrefixType    InetAddressType,
    vRtrBierTxTunnelPtaPrefix        InetAddress,
    vRtrBierTxTunnelPtaBfrId         Unsigned32,
    vRtrBierTxTunnelPtaSubDomain     Unsigned32,
    vRtrBierTxTunnelPtaMplsLabel     Unsigned32,
    vRtrBierTxTunnelLeafBfrID        Unsigned32
}

vRtrBierTxTunnelLeafPrefixType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTxTunnelLeafPrefixType indicates the address type
         of vRtrBierSubDomainPrefix address."
    DEFVAL      { unknown }
    ::= { vRtrBierTxTunnelLeafEntry 2 }

vRtrBierTxTunnelLeafPrefix       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTxTunnelLeafPrefix indicates the address of the
         BFR prefix to be advertised in this sub-domain or the sub Domain
         range."
    ::= { vRtrBierTxTunnelLeafEntry 3 }

vRtrBierTxTunnelMvpnId           OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTxTunnelMvpnId indicates the MVPN ID."
    ::= { vRtrBierTxTunnelLeafEntry 4 }

vRtrBierTxTunnelOperState        OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTxTunnelOperState indicates the current
         administrative state of this tunnel."
    ::= { vRtrBierTxTunnelLeafEntry 5 }

vRtrBierTxTunnelPtaPrefixType    OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTxTunnelPtaPrefixType indicates the address type
         of vRtrBierTxTunnelPtaPrefix address."
    ::= { vRtrBierTxTunnelLeafEntry 6 }

vRtrBierTxTunnelPtaPrefix        OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTxTunnelPtaPrefix indicates the address of the
         BFR prefix to be advertised in this sub-domain or the sub Domain
         range."
    ::= { vRtrBierTxTunnelLeafEntry 7 }

vRtrBierTxTunnelPtaBfrId         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTxTunnelPtaBfrId indicates the BFD ID."
    ::= { vRtrBierTxTunnelLeafEntry 8 }

vRtrBierTxTunnelPtaSubDomain     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTxTunnelPtaSubDomain indicates the sub domain ID."
    ::= { vRtrBierTxTunnelLeafEntry 9 }

vRtrBierTxTunnelPtaMplsLabel     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTxTunnelPtaMplsLabel indicates the service BIER
         level label for this transmitter tunnel."
    ::= { vRtrBierTxTunnelLeafEntry 10 }

vRtrBierTxTunnelLeafBfrID        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTxTunnelLeafBfrID specifies the address of the
         BFR prefix to be advertised in this sub-domain or the sub Domain
         range."
    ::= { vRtrBierTxTunnelLeafEntry 11 }

vRtrBierStatsTable               OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierStatsTable contains objects for BIER statistics for a
         particular router instance."
    ::= { tmnxBierObjs 12 }

vRtrBierStatsEntry               OBJECT-TYPE
    SYNTAX      VRtrBierStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row represents an entry in vRtrBierStatsTable."
    INDEX       { vRtrID }
    ::= { vRtrBierStatsTable 1 }

VRtrBierStatsEntry               ::= SEQUENCE
{
    vRtrBierStatsTotalLearntRoutes   Counter32,
    vRtrBierStatsTotalValidRoutes    Counter32,
    vRtrBierStatsValidNbrNextHops    Counter32,
    vRtrBierStatsRxInvalidBierInfo   Counter32,
    vRtrBierStatsRxInvalidBfrInfo    Counter32,
    vRtrBierStatsRxInvalidEncapInfo  Counter32,
    vRtrBierStatsRxInvalidMplsInfo   Counter32,
    vRtrBierStatsDiscardTunnelNhop   Counter32,
    vRtrBierStatsDiscardNonNtwIfNhop Counter32,
    vRtrBierStatsDiscardNonFp4Nhop   Counter32,
    vRtrBierStatsSdBslMismatch       Counter32,
    vRtrBierStatsMultiTopoMismatch   Counter32,
    vRtrBierStatsUnsupIpv6Routes     Counter32,
    vRtrBierStatsBfrIdDuplicate      Counter32
}

vRtrBierStatsTotalLearntRoutes   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsTotalLearntRoutes indicates the total number
         of learnt BFR prefixes."
    ::= { vRtrBierStatsEntry 1 }

vRtrBierStatsTotalValidRoutes    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsTotalValidRoutes indicates the total number
         of BFR prefixes with valid BFR info."
    ::= { vRtrBierStatsEntry 2 }

vRtrBierStatsValidNbrNextHops    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsValidNbrNextHops indicates the total number
         of neighbors or next-hops with valid BFR info."
    ::= { vRtrBierStatsEntry 3 }

vRtrBierStatsRxInvalidBierInfo   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsRxInvalidBierInfo indicates the number of
         learnt BFR prefixes with invalid BIER info."
    ::= { vRtrBierStatsEntry 4 }

vRtrBierStatsRxInvalidBfrInfo    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsRxInvalidBfrInfo indicates the number of
         learnt BFR prefixes with invalid BFR info."
    ::= { vRtrBierStatsEntry 5 }

vRtrBierStatsRxInvalidEncapInfo  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsRxInvalidEncapInfo indicates the number of
         learnt BFR prefixes with invalid ENCAP info."
    ::= { vRtrBierStatsEntry 6 }

vRtrBierStatsRxInvalidMplsInfo   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsRxInvalidMplsInfo indicates the number of
         learnt BFR prefixes with invalid MPLS info."
    ::= { vRtrBierStatsEntry 7 }

vRtrBierStatsDiscardTunnelNhop   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsDiscardTunnelNhop indicates the number of
         tunnel next-hops discarded."
    ::= { vRtrBierStatsEntry 8 }

vRtrBierStatsDiscardNonNtwIfNhop OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsDiscardNonNtwIfNhop indicates the
          number of non network next-hops discarded."
    ::= { vRtrBierStatsEntry 9 }

vRtrBierStatsDiscardNonFp4Nhop   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsDiscardNonFp4Nhop indicates the number of
         non FP4 next-hops discarded."
    ::= { vRtrBierStatsEntry 10 }

vRtrBierStatsSdBslMismatch       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsSdBslMismatch indicates the number of BFR
         prefixes received with sub-domain and BSL values different from
         configured values."
    ::= { vRtrBierStatsEntry 11 }

vRtrBierStatsMultiTopoMismatch   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsMultiTopoMismatch indicates the number of
         BFR prefixes received with multi-topology value different from the
         configured value."
    ::= { vRtrBierStatsEntry 12 }

vRtrBierStatsUnsupIpv6Routes     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsUnsupIpv6Routes indicates the number of BFR
         prefixes learnt with ipv6 address."
    ::= { vRtrBierStatsEntry 13 }

vRtrBierStatsBfrIdDuplicate      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierStatsBfrIdDuplicate indicates the number of
         duplicate BFR id received in multiple BFR prefixes."
    ::= { vRtrBierStatsEntry 14 }

vRtrBierNotificationObjs         OBJECT IDENTIFIER ::= { tmnxBierObjs 13 }

vRtrBierNotifySubDomainId        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierNotifySubDomainId indicates the configured BIER
         sub-domain value."
    ::= { vRtrBierNotificationObjs 1 }

vRtrBierNotifyRecvSubDomainId    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierNotifyRecvSubDomainId indicates the received BIER
         sub-domain value."
    ::= { vRtrBierNotificationObjs 2 }

vRtrBierNotifyBsl                OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierNotifyBsl indicates the BIER BSL value."
    ::= { vRtrBierNotificationObjs 3 }

vRtrBierNotifyBfrId              OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierNotifyBfrId indicates the BIER BFR Id value."
    ::= { vRtrBierNotificationObjs 4 }

vRtrBierNotifyMTId               OBJECT-TYPE
    SYNTAX      TmnxBierMultiTopology
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierNotifyMTId indicates the configured ISIS
         multi-topology value."
    ::= { vRtrBierNotificationObjs 5 }

vRtrBierNotifyRecvMTId           OBJECT-TYPE
    SYNTAX      TmnxBierMultiTopology
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierNotifyRecvMTId indicates the received ISIS
         multi-topology value."
    ::= { vRtrBierNotificationObjs 6 }

vRtrBierPrefix1AddrType          OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierPrefix1AddrType indicates the address type of
         vRtrBierPrefix1Address address."
    ::= { vRtrBierNotificationObjs 7 }

vRtrBierPrefix1Address           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierPrefix1Address indicates the BFR prefix."
    ::= { vRtrBierNotificationObjs 8 }

vRtrBierPrefix2AddrType          OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierPrefix2AddrType indicates the address type of
         vRtrBierPrefix2Address address."
    ::= { vRtrBierNotificationObjs 9 }

vRtrBierPrefix2Address           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierPrefix2Address indicates the BFR prefix."
    ::= { vRtrBierNotificationObjs 10 }

vRtrBierNextHopAddrType          OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierNextHopAddrType indicates the address type of
         vRtrBierNextHopAddress address."
    ::= { vRtrBierNotificationObjs 11 }

vRtrBierNextHopAddress           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierNextHopAddress indicates the next hop address."
    ::= { vRtrBierNotificationObjs 12 }

vRtrBierNextHopeType             OBJECT-TYPE
    SYNTAX      INTEGER {
        tunnel    (0),
        non-nw-if (1),
        non-fp4   (2)
    }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierNextHopeType indicates the type of next hop."
    ::= { vRtrBierNotificationObjs 13 }

vRtrBierUnsupportedNhopState     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierUnsupportedNhopState indicates if an unsupported
         next-hop was found for a given prefix.

         When the value of vRtrBierUnsupportedNhopState is 'true', it indicates
         that an unsupported next-hop was found.

         When the value of vRtrBierUnsupportedNhopState is 'false', it
         indicates that the unsupported next-hop was cleared and the correct
         next-hop was received."
    ::= { vRtrBierNotificationObjs 14 }

vRtrBierGeneralOperTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierGeneralOperEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierGeneralOperTable contains the operational state objects
         for the general control and management of the BIER protocol instance
         within a virtual router."
    ::= { tmnxBierObjs 14 }

vRtrBierGeneralOperEntry         OBJECT-TYPE
    SYNTAX      VRtrBierGeneralOperEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents the operational values of the BIER protocol
         instance running within a virtual router."
    INDEX       { vRtrID }
    ::= { vRtrBierGeneralOperTable 1 }

VRtrBierGeneralOperEntry         ::= SEQUENCE
{
    vRtrBierGeneralOperState         TmnxOperState,
    vRtrBierGeneralOperDownReason    INTEGER
}

vRtrBierGeneralOperState         OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierGeneralOperState indicates the current
         operational state of this BIER instance."
    DEFVAL      { outOfService }
    ::= { vRtrBierGeneralOperEntry 1 }

vRtrBierGeneralOperDownReason    OBJECT-TYPE
    SYNTAX      INTEGER {
        none       (0),
        admin-down (1)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierGeneralOperDownReason indicates the reason due to
         which BIER instance is operationally down."
    ::= { vRtrBierGeneralOperEntry 2 }

vRtrBierTemplateOperTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierTemplateOperEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierTemplateOperTable lists the operational state objects
         within the BIER policies for a particular BIER instance."
    ::= { tmnxBierObjs 15 }

vRtrBierTemplateOperEntry        OBJECT-TYPE
    SYNTAX      VRtrBierTemplateOperEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry corresponds to the operational values of the BIER template
         which indicates a BIER Domain."
    INDEX       {
        vRtrID,
        vRtrBierTemplateName
    }
    ::= { vRtrBierTemplateOperTable 1 }

VRtrBierTemplateOperEntry        ::= SEQUENCE
{ vRtrBierTemplateOperState        TmnxOperState }

vRtrBierTemplateOperState        OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierTemplateOperState indicates the current
         operational state of this BIER instance."
    DEFVAL      { outOfService }
    ::= { vRtrBierTemplateOperEntry 1 }

vRtrBierSvcRsvdLblTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrBierSvcRsvdLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrBierSvcRsvdLblTable contains objects for BIER service reserved
         labels."
    ::= { tmnxBierObjs 16 }

vRtrBierSvcRsvdLblEntry          OBJECT-TYPE
    SYNTAX      VRtrBierSvcRsvdLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry corresponds to the service ID for the corresponding label."
    INDEX       {
        vRtrID,
        vRtrBierSvcRsvdLbl
    }
    ::= { vRtrBierSvcRsvdLblTable 1 }

VRtrBierSvcRsvdLblEntry          ::= SEQUENCE
{
    vRtrBierSvcRsvdLbl               Unsigned32,
    vRtrBierSvcRsvdLblVRtrId         Unsigned32
}

vRtrBierSvcRsvdLbl               OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierSvcRsvdLbl indicates the service reserved label
         in use by BIER."
    ::= { vRtrBierSvcRsvdLblEntry 1 }

vRtrBierSvcRsvdLblVRtrId         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrBierSvcRsvdLblVRtrId indicates the vrf index for the
         service reserved label in use by BIER."
    ::= { vRtrBierSvcRsvdLblEntry 2 }

tmnxBierConformance              OBJECT IDENTIFIER ::= { tmnxSRConfs 123 }

tmnxBierCompliances              OBJECT IDENTIFIER ::= { tmnxBierConformance 1 }

tmnxBierV16v0Compliance          MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of BIER on Nokia SROS series
         systems 16.0 release."
    MODULE
        MANDATORY-GROUPS {
            tmnxBierV16v0Group,
            tmnxBierNotificationV16v0Group,
            tmnxBierOperStateGroup
        }
    ::= { tmnxBierCompliances 1 }

tmnxBierV19v0Compliance          MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of BIER on Nokia SROS series
         systems 19.0 release."
    MODULE
        MANDATORY-GROUPS {
            tmnxBierV19v0Group
        }
    ::= { tmnxBierCompliances 2 }

tmnxBierV21v0Compliance          MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of BIER on Nokia SROS series
         systems 21.0 release."
    MODULE
        MANDATORY-GROUPS {
            tmnxBierV21v0Group
        }
    ::= { tmnxBierCompliances 3 }

tmnxBierV25v0Compliance          MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of BIER on Nokia SROS series
         systems 25.0 release."
    MODULE
        MANDATORY-GROUPS {
            tmnxBierV25v0Group
        }
    ::= { tmnxBierCompliances 4 }

tmnxBierGroups                   OBJECT IDENTIFIER ::= { tmnxBierConformance 2 }

tmnxBierV16v0Group               OBJECT-GROUP
    OBJECTS     {
        vRtrBierGeneralTableLastChanged,
        vRtrBierGeneralRowStatus,
        vRtrBierGeneralAdminState,
        vRtrBierGeneralRowLastChange,
        vRtrBierTemplateTableLastChanged,
        vRtrBierTemplateRowStatus,
        vRtrBierTemplateAdminState,
        vRtrBierTemplateRowLastChange,
        vRtrBierSubDomainTableLstChanged,
        vRtrBierSubDomainPrefixType,
        vRtrBierSubDomainPrefix,
        vRtrBierSubDomainBfrId,
        vRtrBierSubDomainMT,
        vRtrBierSubDomainRowStatus,
        vRtrBierSubDomainRowLastChange,
        vRtrBierDatabaseBitStringLen,
        vRtrBierDatabasePrefixType,
        vRtrBierDatabasePrefix,
        vRtrBierDatabaseBfrId,
        vRtrBierDatabaseMT,
        vRtrBierDatabaseMplsLabelStart,
        vRtrBierDatabaseMplsLabelEnd,
        vRtrBierDatabaseMplsLabelTotal,
        vRtrBierForwardingNbrPrefixType,
        vRtrBierForwardingNbrPrefix,
        vRtrBierForwardingBitMask,
        vRtrBierForwardingMplsLabel,
        vRtrBierRoutingNbrPrefixType,
        vRtrBierRoutingNbrPrefix,
        vRtrBierRoutingBfrId,
        vRtrBierRoutingLastUpdated,
        vRtrBierTunnelType,
        vRtrBierTunnelPrefixType,
        vRtrBierTunnelPrefix,
        vRtrBierTunnelSubDomain,
        vRtrBierTunnelMplsLabel,
        vRtrBierTunnelBfrId,
        vRtrBierTunnelOperState,
        vRtrBierTunnelNumLeaves,
        vRtrBierTunnelLastOperDownReason,
        vRtrBierTxTunnelMvpnId,
        vRtrBierTxTunnelOperState,
        vRtrBierTxTunnelPtaPrefixType,
        vRtrBierTxTunnelPtaPrefix,
        vRtrBierTxTunnelPtaBfrId,
        vRtrBierTxTunnelPtaSubDomain,
        vRtrBierTxTunnelPtaMplsLabel,
        vRtrBierTxTunnelLeafBfrID,
        vRtrBierStatsTotalLearntRoutes,
        vRtrBierStatsTotalValidRoutes,
        vRtrBierStatsValidNbrNextHops,
        vRtrBierStatsRxInvalidBierInfo,
        vRtrBierStatsRxInvalidBfrInfo,
        vRtrBierStatsRxInvalidEncapInfo,
        vRtrBierStatsRxInvalidMplsInfo,
        vRtrBierStatsDiscardTunnelNhop,
        vRtrBierStatsDiscardNonNtwIfNhop,
        vRtrBierStatsDiscardNonFp4Nhop,
        vRtrBierStatsSdBslMismatch,
        vRtrBierStatsMultiTopoMismatch,
        vRtrBierStatsUnsupIpv6Routes,
        vRtrBierStatsBfrIdDuplicate
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of BIER on Nokia
         SROS series systems 16.0 release."
    ::= { tmnxBierGroups 1 }

tmnxBierNotifyObjsGroup          OBJECT-GROUP
    OBJECTS     {
        vRtrBierNotifySubDomainId,
        vRtrBierNotifyRecvSubDomainId,
        vRtrBierNotifyBsl,
        vRtrBierNotifyBfrId,
        vRtrBierNotifyMTId,
        vRtrBierNotifyRecvMTId,
        vRtrBierPrefix1AddrType,
        vRtrBierPrefix1Address,
        vRtrBierPrefix2AddrType,
        vRtrBierPrefix2Address,
        vRtrBierNextHopAddrType,
        vRtrBierNextHopAddress,
        vRtrBierNextHopeType,
        vRtrBierUnsupportedNhopState
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting BIER notifications on Nokia SROS
         series systems."
    ::= { tmnxBierGroups 2 }

tmnxBierNotificationV16v0Group   NOTIFICATION-GROUP
    NOTIFICATIONS {
        vRtrBierBfrIdCollision,
        vRtrBierMtMismatch,
        vRtrBierSubDomainMismatch,
        vRtrBierUnsupportedNhop
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting BIER protocol on Nokia SROS
         series systems."
    ::= { tmnxBierGroups 3 }

tmnxBierOperStateGroup           OBJECT-GROUP
    OBJECTS     {
        vRtrBierGeneralOperState,
        vRtrBierTemplateOperState
    }
    STATUS      current
    DESCRIPTION
        "The group of operational objects supporting general management of BIER
         on Nokia SROS series systems 16.0 release."
    ::= { tmnxBierGroups 4 }

tmnxBierV19v0Group               OBJECT-GROUP
    OBJECTS     {
        vRtrBierTunnelIsInBand
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of BIER on Nokia
         SROS series systems 19.0 release."
    ::= { tmnxBierGroups 5 }

tmnxBierV21v0Group               OBJECT-GROUP
    OBJECTS     {
        vRtrBierGeneralFrr,
        vRtrBierGeneralBfdEnabled,
        vRtrBierRoutingBkupNbrPfxType,
        vRtrBierRoutingBkupNbrPrefix,
        vRtrBierRoutingBkupNhopPfxType,
        vRtrBierRoutingBkupNhopPrefix,
        vRtrBierRoutingBkupNhopIfIndex,
        vRtrBierForwardingBkupNbrPfxType,
        vRtrBierForwardingBkupNbrPrefix,
        vRtrBierFwrdingBkupNhopPfxType,
        vRtrBierForwardingBkupNhopPrefix,
        vRtrBierForwardingBkupNhopIfIdx,
        vRtrBierForwardingBkupBitMask,
        vRtrBierForwardingBkupMplsLabel,
        vRtrBierGeneralOperDownReason
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of BIER on Nokia
         SROS series systems 21.0 release."
    ::= { tmnxBierGroups 7 }

tmnxBierV25v0Group               OBJECT-GROUP
    OBJECTS     {
        vRtrBierGenServRsvdLblBlockName,
        vRtrBierSvcRsvdLblVRtrId
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of BIER on Nokia
         SROS series systems 25.0 release."
    ::= { tmnxBierGroups 8 }

vRtrBierNotifyPrefix             OBJECT IDENTIFIER ::= { tmnxSRNotifyPrefix 123 }

vRtrBierNotifications            OBJECT IDENTIFIER ::= { vRtrBierNotifyPrefix 0 }

vRtrBierBfrIdCollision           NOTIFICATION-TYPE
    OBJECTS     {
        vRtrBierNotifySubDomainId,
        vRtrBierNotifyBsl,
        vRtrBierPrefix1AddrType,
        vRtrBierPrefix1Address,
        vRtrBierPrefix2AddrType,
        vRtrBierPrefix2Address,
        vRtrBierNotifyBfrId
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrBierBfrIdCollision is generated when BFR ID received
         from two different routes is the same.

         [EFFECT] We will remove the duplicate BFR Id from neighbors
          f-BM (forwarding Bit Mask).

         [RECOVERY] An operator intervention is needed to remove the
          duplicate BFR ID from the configuration."
    ::= { vRtrBierNotifications 1 }

vRtrBierMtMismatch               NOTIFICATION-TYPE
    OBJECTS     {
        vRtrBierNotifySubDomainId,
        vRtrBierNotifyBsl,
        vRtrBierNotifyMTId,
        vRtrBierNotifyRecvMTId
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrBierMtMismatch is generated when the multi-topology
         sent by the peer is different from what is configured locally.

         [EFFECT] We will ignore the advertisement.

         [RECOVERY] N/A"
    ::= { vRtrBierNotifications 2 }

vRtrBierSubDomainMismatch        NOTIFICATION-TYPE
    OBJECTS     {
        vRtrBierNotifySubDomainId,
        vRtrBierNotifyBsl,
        vRtrBierNotifyRecvSubDomainId
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrBierSubDomainMismatch is generated when the sub-domain
         in the received route is not configured locally.

         [EFFECT] We will ignore the sub TLV.

         [RECOVERY] Operator may need to configure the mismatched sub-domains."
    ::= { vRtrBierNotifications 3 }

vRtrBierUnsupportedNhop          NOTIFICATION-TYPE
    OBJECTS     {
        vRtrBierNextHopeType,
        vRtrBierUnsupportedNhopState,
        vRtrBierPrefix1AddrType,
        vRtrBierPrefix1Address,
        vRtrBierNextHopAddrType,
        vRtrBierNextHopAddress,
        vRtrIfIndex
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrBierUnsupportedNhop is generated when the
          next hop indicated by vRtrBierNextHopAddress is
          unsupported by the system.

         [EFFECT] We will ignore it while calculating the next hop.

         [RECOVERY] The recovery is caused on receiving the subsequent
          correct next hop and clearing this trap by setting
          vRtrBierUnsupportedNhopState to 'false'."
    ::= { vRtrBierNotifications 4 }

END
