TIMETRA-MSDP-NG-MIB DEFINITIONS ::= BEGIN

IMPORTS
    InetAddress, InetAddressPrefixLength,
    InetAddressType
                                                         FROM INET-ADDRESS-MIB
    MODULE-COMPLIANCE, NOTIFICATION-GROUP,
    OBJECT-GROUP
                                                         FROM SNMPv2-CONF
    Counter32, Gauge32, Integer32,
    MODULE-IDENTITY, NOTIFICATION-TYPE,
    OBJECT-TYPE, Unsigned32
                                                         FROM SNMPv2-SMI
    RowStatus, TimeInterval, TimeStamp,
    TruthValue
                                                         FROM SNMPv2-TC
    timetraSRMIBModules, tmnxSRConfs,
    tmnxSRNotifyPrefix, tmnxSRObjs
                                                         FROM TIMETRA-GLOBAL-MIB
    TNamedItem, TNamedItemOrEmpty,
    TPolicyStatementNameOrEmpty,
    TmnxAdminState
                                                         FROM TIMETRA-TC-MIB
    vRtrID
                                                         FROM TIMETRA-VRTR-MIB
    ;

timetraMsdpNgMIBModule           MODULE-IDENTITY
    LAST-UPDATED "201601010000Z"
    ORGANIZATION "Nokia"
    CONTACT-INFO
        "Nokia SROS Support
         Web: http://www.nokia.com"
    DESCRIPTION
        "This is the SNMP MIB module to manage and provision MSDP protocol on
         Nokia SROS equipment. The Multicast Source Discovery Protocol (MSDP)
         is used to connect multicast routing domains. It typically runs on the
         same router as the Protocol Independent Multicast (PIM) sparse-mode
         rendezvous point (RP). Each MSDP router establishes adjacencies with
         internal and external MSDP peers similar to the Border Gateway
         Protocol (BGP). These peer routers inform each other about active
         sources within the domain. When they detect active sources, the
         routers can send PIM sparse-mode explicit join messages to the active
         source.

         Copyright 2014-2018 Nokia. All rights reserved. Reproduction of this
         document is authorized on the condition that the foregoing copyright
         notice is included.

         This SNMP MIB module (Specification) embodies Nokia's
         proprietary intellectual property.  Nokia retains
         all title and ownership in the Specification, including any
         revisions.

         Nokia grants all interested parties a non-exclusive license to use and
         distribute an unmodified copy of this Specification in connection with
         management of Nokia products, and without fee, provided this copyright
         notice and license appear on all copies.

         This Specification is supplied 'as is', and Nokia makes no warranty,
         either express or implied, as to the use, operation, condition, or
         performance of the Specification."

    REVISION    "201601010000Z"
    DESCRIPTION
        "Rev 14.0               1 Jan 2016 00:00
         14.0 release of the TIMETRA-MSDP-MIB."

    REVISION    "201411010000Z"
    DESCRIPTION
        "Rev 0.1                1 Nov 2014 00:00
         Initial version of the TIMETRA-MSDP-MIB."

    ::= { timetraSRMIBModules 104 }

tmnxMsdpNgObjects                OBJECT IDENTIFIER ::= { tmnxSRObjs 104 }

tmnxMsdpNgGlobals                OBJECT IDENTIFIER ::= { tmnxMsdpNgObjects 1 }

tmnxMsdpNgGeneralTableLstChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgGeneralTableLstChanged indicates the sysUpTime
         at the time of the last modification of an entry in the
         tmnxMsdpNgGeneralTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxMsdpNgGlobals 1 }

tmnxMsdpNgGeneralTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxMsdpNgGeneralEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgGeneralTable contains objects for general control and
         management of the MSDP protocol instance within a virtual router."
    ::= { tmnxMsdpNgObjects 2 }

tmnxMsdpNgGeneralEntry           OBJECT-TYPE
    SYNTAX      TmnxMsdpNgGeneralEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of the MSDP protocol running
         within a virtual router.  Entries in this table cannot be
         created and deleted via SNMP SET operations."
    INDEX       { vRtrID }
    ::= { tmnxMsdpNgGeneralTable 1 }

TmnxMsdpNgGeneralEntry           ::= SEQUENCE
{
    tmnxMsdpNgMaxActiveSources       Integer32,
    tmnxMsdpNgMsgRcvRate             Unsigned32,
    tmnxMsdpNgMsgRcvRateTime         Unsigned32,
    tmnxMsdpNgMsgRcvRateThd          Gauge32,
    tmnxMsdpNgDataEncapsulation      TruthValue,
    tmnxMsdpNgAdminState             TmnxAdminState,
    tmnxMsdpNgExportPolicy1          TPolicyStatementNameOrEmpty,
    tmnxMsdpNgExportPolicy2          TPolicyStatementNameOrEmpty,
    tmnxMsdpNgExportPolicy3          TPolicyStatementNameOrEmpty,
    tmnxMsdpNgExportPolicy4          TPolicyStatementNameOrEmpty,
    tmnxMsdpNgExportPolicy5          TPolicyStatementNameOrEmpty,
    tmnxMsdpNgImportPolicy1          TPolicyStatementNameOrEmpty,
    tmnxMsdpNgImportPolicy2          TPolicyStatementNameOrEmpty,
    tmnxMsdpNgImportPolicy3          TPolicyStatementNameOrEmpty,
    tmnxMsdpNgImportPolicy4          TPolicyStatementNameOrEmpty,
    tmnxMsdpNgImportPolicy5          TPolicyStatementNameOrEmpty,
    tmnxMsdpNgLocalAddressType       InetAddressType,
    tmnxMsdpNgLocalAddress           InetAddress,
    tmnxMsdpNgStatusPeerCount        Gauge32,
    tmnxMsdpNgStatusPeersEstablished Gauge32,
    tmnxMsdpNgStatusSACount          Gauge32,
    tmnxMsdpNgStatusLastTimeUp       TimeStamp,
    tmnxMsdpNgStatusActSrcLimExceed  Counter32,
    tmnxMsdpNgRpfLookupSequence      INTEGER,
    tmnxMsdpNgSACacheLifetime        Unsigned32,
    tmnxMsdpNgSARejectExportPolicy   Counter32,
    tmnxMsdpNgSARejectImportPolicy   Counter32
}

tmnxMsdpNgMaxActiveSources       OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..1000000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgMaxActiveSources specifies the maximum number
         of source active messages that will be accepted by MSDP. This
         effectively controls the number of source active messages that can be
         stored on the system.

         By default, no limit is placed on the number of source active
         messages and this is specified by the value '-1'.  A value of
         '0' means that no source active messages will be accepted."
    DEFVAL      { -1 }
    ::= { tmnxMsdpNgGeneralEntry 1 }

tmnxMsdpNgMsgRcvRate             OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 10..10000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgMsgRcvRate specifies the  number of  MSDP
         messages (including source active messages) that are read from the
         TCP session per tmnxMsdpNgMsgRcvRateTime seconds.

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value '0'.

         Once the number of MSDP packets defined in tmnxMsdpNgMsgRcvRateThd
         have been processed the rate of all other MSDP packets is rate limited
         by no longer accepting messages from the TCP session until
         tmnxMsdpNgMsgRcvRateTime seconds have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgGeneralEntry 2 }

tmnxMsdpNgMsgRcvRateTime         OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 1..600)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgMsgRcvRateTime specifies the time in seconds
         that together with tmnxMsdpNgMsgRcvRate defines the number of  MSDP
         messages (including source active messages) that are read from the
         TCP session within the configured number of seconds.

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value '0'.

         Once the number of MSDP packets defined in tmnxMsdpNgMsgRcvRateThd
         have been processed the rate of all other MSDP packets is rate limited
         by no longer accepting messages from the TCP session until
         tmnxMsdpNgMsgRcvRateTime seconds have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgGeneralEntry 3 }

tmnxMsdpNgMsgRcvRateThd          OBJECT-TYPE
    SYNTAX      Gauge32 (0 | 1..1000000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgMsgRcvRateThd specifies the number of MSDP
         messages that can be processed before tmnxMsdpNgMsgRcvRate is set.
         This is useful during system startup and initialization.

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value '0'.

         Once the number of MSDP packets defined in tmnxMsdpNgMsgRcvRateThd
         have been processed the rate of all other MSDP packets is rate limited
         by no longer accepting messages from the TCP session until
         tmnxMsdpNgMsgRcvRateTime seconds have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgGeneralEntry 4 }

tmnxMsdpNgDataEncapsulation      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgDataEncapsulation is used to configure a
         rendezvous point (RP) using MSDP to encapsulate multicast data
         received in MSDP register messages inside forwarded MSDP source-active
         messages.

         By default data encapsulation is enabled."
    DEFVAL      { true }
    ::= { tmnxMsdpNgGeneralEntry 5 }

tmnxMsdpNgAdminState             OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgAdminState specifies the desired administrative
         state for MSDP. When MSDP is 'outOfService' the operational state of
         MSDP as well as the operational state of other entities under it, like
         peer or peer group is also disabled."
    DEFVAL      { inService }
    ::= { tmnxMsdpNgGeneralEntry 6 }

tmnxMsdpNgExportPolicy1          OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgExportPolicy1 specifies the first export policy
         to export Source Active (SA) state from the SA list into MSDP.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 7 }

tmnxMsdpNgExportPolicy2          OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgExportPolicy2 specifies the second export
         policy to export Source Active (SA) state from the SA list into MSDP.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 8 }

tmnxMsdpNgExportPolicy3          OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgExportPolicy3 specifies the third export policy
         to export Source Active (SA) state from the SA list into MSDP.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 9 }

tmnxMsdpNgExportPolicy4          OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgExportPolicy4 specifies the fourth export
         policy to export Source Active (SA) state from the SA list into MSDP.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 10 }

tmnxMsdpNgExportPolicy5          OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgExportPolicy5 specifies the fifth export policy
         to export Source Active (SA) state from the SA list into MSDP.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 11 }

tmnxMsdpNgImportPolicy1          OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgImportPolicy1 specifies the first import policy
         to import Source Active (SA) state from the SA list into MSDP.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 12 }

tmnxMsdpNgImportPolicy2          OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgImportPolicy2 specifies the second import
         policy to import Source Active (SA) state from the SA list into MSDP.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 13 }

tmnxMsdpNgImportPolicy3          OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgImportPolicy3 specifies the third import policy
         to import Source Active (SA) state from the SA list into MSDP.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 14 }

tmnxMsdpNgImportPolicy4          OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgImportPolicy4 specifies the fourth import
         policy to import Source Active (SA) state from the SA list into MSDP.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 15 }

tmnxMsdpNgImportPolicy5          OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgImportPolicy5 specifies the fifth import policy
         to import Source Active (SA) state from the SA list into MSDP.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 16 }

tmnxMsdpNgLocalAddressType       OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgLocalAddressType specifies the type of
         tmnxMsdpNgLocalAddress."
    DEFVAL      { unknown }
    ::= { tmnxMsdpNgGeneralEntry 17 }

tmnxMsdpNgLocalAddress           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgLocalAddress is used to configure the local
         end of a MSDP session. In order for MSDP to function at least one
         peer must be configured.  When configuring a peer, the local end
         of the MSDP session must be configured.  This address is used to
         validate incoming connections to the peer and to establish
         connections to the remote peer.

         By default no local address is configured."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgGeneralEntry 18 }

tmnxMsdpNgStatusPeerCount        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgStatusPeerCount indicates the number of
         configured peers."
    ::= { tmnxMsdpNgGeneralEntry 19 }

tmnxMsdpNgStatusPeersEstablished OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgStatusPeersEstablished indicates the number of
         peers in established state."
    ::= { tmnxMsdpNgGeneralEntry 20 }

tmnxMsdpNgStatusSACount          OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgStatusSACount indicates the number of source
         active configured in cache."
    ::= { tmnxMsdpNgGeneralEntry 21 }

tmnxMsdpNgStatusLastTimeUp       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgStatusLastTimeUp indicates the last time the
         protocol was enabled."
    ::= { tmnxMsdpNgGeneralEntry 22 }

tmnxMsdpNgStatusActSrcLimExceed  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgStatusActSrcLimExceed indicates the number of
         times the global active source limit has been exceeded."
    ::= { tmnxMsdpNgGeneralEntry 23 }

tmnxMsdpNgRpfLookupSequence      OBJECT-TYPE
    SYNTAX      INTEGER {
        mucastRouteTable (0),
        ucastRouteTable  (1),
        both             (2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "tmnxMsdpNgRpfLookupSequence is used to configure the sequence of route
         tables that MSDP uses for finding a Reverse Path Forwarding(RPF)
         interface for a particular multicast route.

         'mucastRouteTable' is the unicast route table to be used only by
         multicast protocols(MSDP) which will contain routes submitted by
         multi-protocol BGP, ISIS and OSPF.

         'ucastRouteTable' is the regular unicast route table which will
         contain routes submitted by all the unicast routing protocols. By
         default, only the 'ucastRouteTable' is looked up by MSDP for
         calculating RPF interface towards the source/rendezvous point. However
         the operator can specify the following: a) Use unicast route table
         only b) Use multicast unicast route table only or c) Use both the
         route tables.

         In case of (c), MSDP will always lookup first in the
         'mucastRouteTable' and if there is a route, it will use it. If MSDP
         does not find a route in the first lookup, it will try to find it in
         the 'ucastRouteTable'."
    DEFVAL      { ucastRouteTable }
    ::= { tmnxMsdpNgGeneralEntry 24 }

tmnxMsdpNgSACacheLifetime        OBJECT-TYPE
    SYNTAX      Unsigned32 (90..600)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSACacheLifetime specifies lifetime given to SA
         cache entries in seconds when created or refreshed.

         This object does not measure time per se; instead, it is the delta
         from the time at which an SA message is received at which it should be
         expired if not refreshed. (i.e., it is the value of
         tmnxMsdpNgSAExpiryTime immediately after receiving an SA message
         applying to that row.)"
    DEFVAL      { 90 }
    ::= { tmnxMsdpNgGeneralEntry 25 }

tmnxMsdpNgSARejectExportPolicy   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejectExportPolicy indicates number of SA
         messages that were not sent due to export policy."
    ::= { tmnxMsdpNgGeneralEntry 26 }

tmnxMsdpNgSARejectImportPolicy   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejectImportPolicy indicates number of SA
         messages that were rejected due to import policy."
    ::= { tmnxMsdpNgGeneralEntry 27 }

tmnxMsdpNgPeerTable              OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxMsdpNgPeerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgPeerTable table provides information on the properties
         of a MSDP peer."
    ::= { tmnxMsdpNgObjects 3 }

tmnxMsdpNgPeerEntry              OBJECT-TYPE
    SYNTAX      TmnxMsdpNgPeerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxMsdpNgPeerEntry represents a row entry in tmnxMsdpNgPeerTable for
         a MSDP peer.

         Entries can be created and deleted via SNMP SET operations through
         tmnxMsdpNgPeerRowStatus. "
    INDEX       {
        vRtrID,
        tmnxMsdpNgPeerAddressType,
        tmnxMsdpNgPeerAddress
    }
    ::= { tmnxMsdpNgPeerTable 1 }

TmnxMsdpNgPeerEntry              ::= SEQUENCE
{
    tmnxMsdpNgPeerAddressType        InetAddressType,
    tmnxMsdpNgPeerAddress            InetAddress,
    tmnxMsdpNgPeerRowStatus          RowStatus,
    tmnxMsdpNgPeerMaxActiveSources   Integer32,
    tmnxMsdpNgPeerMsgRcvRate         Unsigned32,
    tmnxMsdpNgPeerMsgRcvRateTime     Unsigned32,
    tmnxMsdpNgPeerMsgRcvRateThd      Gauge32,
    tmnxMsdpNgPeerAuthKey            OCTET STRING,
    tmnxMsdpNgPeerAuthKeyEncrypted   TruthValue,
    tmnxMsdpNgPeerDefaultPeer        TruthValue,
    tmnxMsdpNgPeerAdminState         TmnxAdminState,
    tmnxMsdpNgPeerExportPolicy1      TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerExportPolicy2      TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerExportPolicy3      TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerExportPolicy4      TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerExportPolicy5      TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerImportPolicy1      TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerImportPolicy2      TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerImportPolicy3      TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerImportPolicy4      TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerImportPolicy5      TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerLocalAddressType   InetAddressType,
    tmnxMsdpNgPeerLocalAddress       InetAddress,
    tmnxMsdpNgPeerState              INTEGER,
    tmnxMsdpNgPeerLastUpOrDown       TimeStamp,
    tmnxMsdpNgPeerConRetry           Counter32,
    tmnxMsdpNgPeerStateTimer         Unsigned32,
    tmnxMsdpNgPeerTimeout            Unsigned32,
    tmnxMsdpNgPeerSAAccepted         Gauge32,
    tmnxMsdpNgPeerSARx               Gauge32,
    tmnxMsdpNgPeerLastASLimit        TimeStamp,
    tmnxMsdpNgPeerOperLclAddrType    InetAddressType,
    tmnxMsdpNgPeerOperLclAddr        InetAddress
}

tmnxMsdpNgPeerAddressType        OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerAddressType indicates the type of
         tmnxMsdpNgPeerAddress."
    ::= { tmnxMsdpNgPeerEntry 1 }

tmnxMsdpNgPeerAddress            OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerAddress indicates the address of the MSDP
         peer."
    ::= { tmnxMsdpNgPeerEntry 2 }

tmnxMsdpNgPeerRowStatus          OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "tmnxMsdpNgPeerRowStatus is the object used for creating and deleting
         row entries in this table."
    ::= { tmnxMsdpNgPeerEntry 3 }

tmnxMsdpNgPeerMaxActiveSources   OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..1000000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerMaxActiveSources specifies the maximum
         number of source active messages that will be accepted by MSDP. This
         effectively controls the number of active sources that can be stored
         on the system.

         By default, no limit is placed on the number of source active
         messages and this is specified by the value '-1'.  A value of
         0 means that no source active messages will be accepted."
    DEFVAL      { -1 }
    ::= { tmnxMsdpNgPeerEntry 4 }

tmnxMsdpNgPeerMsgRcvRate         OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 10..10000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerMsgRcvRate specifies the  number of  MSDP
         messages (including source active messages) that are read from the
         TCP session per tmnxMsdpNgPeerMsgRcvRateTime seconds.

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value 0.

         Once the number of MSDP packets defined in tmnxMsdpNgPeerMsgRcvRateThd
         have been processed the rate of all other MSDP packets is rate limited
         by no longer accepting messages from the TCP session until
         tmnxMsdpNgPeerMsgRcvRateTime seconds have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgPeerEntry 5 }

tmnxMsdpNgPeerMsgRcvRateTime     OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 1..600)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerMsgRcvRateTime specifies the time in
         seconds that together with tmnxMsdpNgPeerMsgRcvRate defines the number
         of MSDP messages (including source active messages) that are read from
         the TCP session within the configured number of seconds.

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value 0.

         Once the number of MSDP packets defined in tmnxMsdpNgPeerMsgRcvRateThd
         have been processed the rate of all other MSDP packets is rate limited
         by no longer accepting messages from the TCP session until
         tmnxMsdpNgPeerMsgRcvRateTime seconds have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgPeerEntry 6 }

tmnxMsdpNgPeerMsgRcvRateThd      OBJECT-TYPE
    SYNTAX      Gauge32 (0 | 1..1000000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerMsgRcvRateThd specifies the number of
         MSDP messages that can be processed before tmnxMsdpNgPeerMsgRcvRate is
         set.  This is useful during system startup and initialization.

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value 0.

         Once the number of MSDP packets defined in tmnxMsdpNgPeerMsgRcvRateThd
         have been processed the rate of all other MSDP packets is rate limited
         by no longer accepting messages from the TCP session until
         tmnxMsdpNgPeerMsgRcvRateTime seconds have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgPeerEntry 7 }

tmnxMsdpNgPeerAuthKey            OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..256))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerAuthKey specifies the authentication
         key to be used for a specific MSDP peering session.  Authentication
         is done using the MD-5 message based digest protocol.  Authentication
         cannot be configured globally and can be applied per peer only.
         The authentication key can be any combination of letters or numbers.
         Note that the string may contain embedded nulls.

         By default, all MSDP messages are accepted and the MD5 signature
         option authentication key is disabled"
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 8 }

tmnxMsdpNgPeerAuthKeyEncrypted   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When the value of tmnxMsdpNgPeerAuthKeyEncrypted is 'true', the
         password specified by tmnxMsdpNgPeerAuthKey is in the encrypted form.

         When the value of tmnxMsdpNgPeerAuthKeyEncrypted is 'false', the
         password specified by tmnxMsdpNgPeerAuthKey is in plain text.

         tmnxMsdpNgPeerAuthKey and tmnxMsdpNgPeerAuthKeyEncrypted, which
         indicates whether or not the password string is encrypted, must be set
         together in the same SNMP request PDU or else the set request will
         fail with an inconsistentValue error."
    DEFVAL      { true }
    ::= { tmnxMsdpNgPeerEntry 9 }

tmnxMsdpNgPeerDefaultPeer        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerDefaultPeer is used to configure a peer as
         the default Msdp peer due to which all source-active messages from the
         peer will be accepted without the usual peer-reverse-path-forwarding
         (RPF) check."
    DEFVAL      { false }
    ::= { tmnxMsdpNgPeerEntry 10 }

tmnxMsdpNgPeerAdminState         OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerAdminState specifies the desired
         administrative state for a MSDP peer. When a MSDP peer is
         'outOfService' the operational state of MSDP as well as the
         operational state of other entities under it, like peer group is also
         disabled.

         By default, the state of a MSDP peer is 'inService'."
    DEFVAL      { inService }
    ::= { tmnxMsdpNgPeerEntry 11 }

tmnxMsdpNgPeerExportPolicy1      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerExportPolicy1 specifies the export policy
         to export Source Active (SA) state from the SA list into MSDP. A
         maximum of five policy names can be specified.
         tmnxMsdpNgPeerExportPolicy1 specifies policy number 1 at the protocol
         level.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 12 }

tmnxMsdpNgPeerExportPolicy2      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerExportPolicy2 specifies the export policy
         to export Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerExportPolicy2 specifies policy number 2 at the protocol
         level.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 13 }

tmnxMsdpNgPeerExportPolicy3      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerExportPolicy3 specifies the export policy
         to export Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerExportPolicy3 specifies policy number 3 at the protocol
         level.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 14 }

tmnxMsdpNgPeerExportPolicy4      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerExportPolicy4 specifies the export policy
         to export Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerExportPolicy4 specifies policy number 4 at the protocol
         level.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 15 }

tmnxMsdpNgPeerExportPolicy5      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerExportPolicy5 specifies the export policy
         to export Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerExportPolicy1 specifies policy number 5 at the protocol
         level.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 16 }

tmnxMsdpNgPeerImportPolicy1      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerImportPolicy1 specifies the import policy
         to import Source Active (SA) state from the SA list into MSDP.  A
         maximum of five policy names can be specified.
         tmnxMsdpNgPeerImportPolicy1 specifies policy number 1 at the protocol
         level.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 17 }

tmnxMsdpNgPeerImportPolicy2      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerImportPolicy2 specifies the import policy
         to import Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerImportPolicy2 specifies policy number 2 at the protocol
         level.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 18 }

tmnxMsdpNgPeerImportPolicy3      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerImportPolicy3 specifies the import policy
         to import Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerImportPolicy3 specifies policy number 3 at the protocol
         level.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 19 }

tmnxMsdpNgPeerImportPolicy4      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerImportPolicy4 specifies the import policy
         to import Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerImportPolicy4 specifies policy number 4 at the protocol
         level.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 20 }

tmnxMsdpNgPeerImportPolicy5      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerImportPolicy5 specifies the import policy
         to import Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerImportPolicy5 specifies policy number 5 at the protocol
         level.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 21 }

tmnxMsdpNgPeerLocalAddressType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerLocalAddressType is used to configure the
         type of tmnxMsdpNgPeerLocalAddress."
    DEFVAL      { unknown }
    ::= { tmnxMsdpNgPeerEntry 22 }

tmnxMsdpNgPeerLocalAddress       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerLocalAddress is used to configure the
         local end of a MSDP session. In order for MSDP to function at least
         one peer must be configured.  When configuring a peer,  the local
         end of the MSDP session must be configured.  This address is used
         to validate incoming connections to the peer and to establish
         connections to the remote peer.

         By default no local address is configured."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerEntry 23 }

tmnxMsdpNgPeerState              OBJECT-TYPE
    SYNTAX      INTEGER {
        listen      (0),
        established (1),
        inactive    (2),
        disabled    (3),
        connecting  (4)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerState indicates the status of the
         connection."
    ::= { tmnxMsdpNgPeerEntry 24 }

tmnxMsdpNgPeerLastUpOrDown       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerLastUpOrDown indicates the time at which
         the most recent peer-state change occurred."
    ::= { tmnxMsdpNgPeerEntry 25 }

tmnxMsdpNgPeerConRetry           OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerConRetry indicates number of peer
         connection retry attempts."
    ::= { tmnxMsdpNgPeerEntry 26 }

tmnxMsdpNgPeerStateTimer         OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStateTimer indicates the number of seconds
         to wait before another message is sent to a peer."
    ::= { tmnxMsdpNgPeerEntry 27 }

tmnxMsdpNgPeerTimeout            OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerTimeout indicates the number of seconds to
         wait for a response from the peer before declaring the peer
         unavailable."
    ::= { tmnxMsdpNgPeerEntry 28 }

tmnxMsdpNgPeerSAAccepted         OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerSAAccepted indicates the number of entries
         in the source-active cache accepted from the peer."
    ::= { tmnxMsdpNgPeerEntry 29 }

tmnxMsdpNgPeerSARx               OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerSARx indicates the number of entries in the
         source-active cache received by the peer."
    ::= { tmnxMsdpNgPeerEntry 30 }

tmnxMsdpNgPeerLastASLimit        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerLastASLimit indicates the time that the
         last active source limit was triggered."
    ::= { tmnxMsdpNgPeerEntry 31 }

tmnxMsdpNgPeerOperLclAddrType    OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerOperLclAddrType indicates the address type
         of tmnxMsdpNgPeerOperLclAddr."
    ::= { tmnxMsdpNgPeerEntry 32 }

tmnxMsdpNgPeerOperLclAddr        OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerOperLclAddr indicates the operational value
         of the local address."
    ::= { tmnxMsdpNgPeerEntry 33 }

tmnxMsdpNgPeerGroupTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxMsdpNgPeerGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgPeerGroupTable provides a listing of all MSDP Peer
         Groups."
    ::= { tmnxMsdpNgObjects 4 }

tmnxMsdpNgPeerGroupEntry         OBJECT-TYPE
    SYNTAX      TmnxMsdpNgPeerGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxMsdpNgPeerGroupEntry represents a MSDP Peer Group. Entries can be
         created and deleted via SNMP SET operations."
    INDEX       {
        vRtrID,
        tmnxMsdpNgPeerGroupName
    }
    ::= { tmnxMsdpNgPeerGroupTable 1 }

TmnxMsdpNgPeerGroupEntry         ::= SEQUENCE
{
    tmnxMsdpNgPeerGroupName          TNamedItem,
    tmnxMsdpNgPeerGroupRowStatus     RowStatus,
    tmnxMsdpNgPeerGroupMsgRcvRate    Unsigned32,
    tmnxMsdpNgPeerGrpMsgRcvRateTime  Unsigned32,
    tmnxMsdpNgPeerGroupMsgRcvRateThd Gauge32,
    tmnxMsdpNgPeerGroupAdminState    TmnxAdminState,
    tmnxMsdpNgPeerGroupExportPolicy1 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGroupExportPolicy2 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGroupExportPolicy3 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGroupExportPolicy4 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGroupExportPolicy5 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGroupImportPolicy1 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGroupImportPolicy2 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGroupImportPolicy3 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGroupImportPolicy4 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGroupImportPolicy5 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGroupLocalAddrType InetAddressType,
    tmnxMsdpNgPeerGroupLocalAddress  InetAddress,
    tmnxMsdpNgPeerGroupMode          INTEGER,
    tmnxMsdpNgPeerGroupMaxActSources Integer32,
    tmnxMsdpNgPeerGroupActMsgsExMax  Counter32,
    tmnxMsdpNgPeerGrpSARejExpPolicy  Counter32,
    tmnxMsdpNgPeerGrpSARejImpPolicy  Counter32
}

tmnxMsdpNgPeerGroupName          OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupName indicates the peer group name."
    ::= { tmnxMsdpNgPeerGroupEntry 1 }

tmnxMsdpNgPeerGroupRowStatus     OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "tmnxMsdpNgPeerGroupRowStatus is the object used for creating and
         deleting row entries in this table."
    ::= { tmnxMsdpNgPeerGroupEntry 2 }

tmnxMsdpNgPeerGroupMsgRcvRate    OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 10..10000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupMsgRcvRate specifies the  number of
         MSDP messages (including source active messages) that are read from
         the TCP session per tmnxMsdpNgMsgRcvRateTime seconds

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value 0.

         Once the number of MSDP packets defined in tmnxMsdpNgMsgRcvRateThd
         have been processed the rate of all other MSDP packets is rate limited
         by no longer accepting messages from the TCP session until
         tmnxMsdpNgMsgRcvRateTime seconds have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgPeerGroupEntry 3 }

tmnxMsdpNgPeerGrpMsgRcvRateTime  OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 1..600)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpMsgRcvRateTime specifies the maximum
         number of source active messages that will be accepted by MSDP. This
         effectively controls the number of source active messages that can be
         stored on the system. By default, no MSDP messages are read from the
         TCP session and this is specified by the value 0.

         Once the number of MSDP packets defined in
         tmnxMsdpNgPeerGroupMsgRcvRateThd have been processed the rate of all
         other MSDP packets is rate limited by no longer accepting messages
         from the TCP session until tmnxMsdpNgPeerGrpMsgRcvRateTime seconds
         have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgPeerGroupEntry 4 }

tmnxMsdpNgPeerGroupMsgRcvRateThd OBJECT-TYPE
    SYNTAX      Gauge32 (0 | 1..1000000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupMsgRcvRateThd specifies the
         number of MSDP messages that can be processed before
         tmnxMsdpNgPeerGroupMsgRcvRate is set.  This is useful during system
         startup and initialization.

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value 0.

         Once the number of MSDP packets defined in
         tmnxMsdpNgPeerGroupMsgRcvRateThd have been processed the rate of all
         other MSDP packets is rate limited by no longer accepting messages
         from the TCP session until tmnxMsdpNgPeerGrpMsgRcvRateTime seconds
         have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgPeerGroupEntry 5 }

tmnxMsdpNgPeerGroupAdminState    OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupAdminState specifies the desired
         administrative state for a MSDP peer group. When
         tmnxMsdpNgPeerGroupAdminState is 'outOfService' the operational state
         of the MSDP peer group as well as the operational state of other
         entities under it, like other peers is also disabled.

         By default, the state of a MSDP peer group is 'inService'."
    DEFVAL      { inService }
    ::= { tmnxMsdpNgPeerGroupEntry 6 }

tmnxMsdpNgPeerGroupExportPolicy1 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupExportPolicy1 specifies the export
         policy number 1 at peer group level."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 7 }

tmnxMsdpNgPeerGroupExportPolicy2 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupExportPolicy2 specifies the export
         policy number 2 at peer group protocol level."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 8 }

tmnxMsdpNgPeerGroupExportPolicy3 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupExportPolicy3 specifies the export
         policy number 3 at peer group protocol level."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 9 }

tmnxMsdpNgPeerGroupExportPolicy4 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupExportPolicy4 specifies the export
         policy number 4 at peer group protocol level."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 10 }

tmnxMsdpNgPeerGroupExportPolicy5 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupExportPolicy5 specifies the export
         policy number 5 at peer group protocol level."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 11 }

tmnxMsdpNgPeerGroupImportPolicy1 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupImportPolicy1 specifies the import
         policy number 1  at peer group level."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 12 }

tmnxMsdpNgPeerGroupImportPolicy2 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupImportPolicy2 specifies the import
         policy number 2 at peer group level."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 13 }

tmnxMsdpNgPeerGroupImportPolicy3 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupImportPolicy3 specifies the import
         policy number 3 at peer group level."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 14 }

tmnxMsdpNgPeerGroupImportPolicy4 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupImportPolicy4 specifies the import
         policy number 4 at peer group level."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 15 }

tmnxMsdpNgPeerGroupImportPolicy5 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupImportPolicy5 specifies the import
         policy number 5 at peer group level."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 16 }

tmnxMsdpNgPeerGroupLocalAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupLocalAddrType is used to configure the
         type of tmnxMsdpNgPeerGroupLocalAddress."
    DEFVAL      { unknown }
    ::= { tmnxMsdpNgPeerGroupEntry 17 }

tmnxMsdpNgPeerGroupLocalAddress  OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupLocalAddress is used to configure the
         local end of a MSDP session. In order for MSDP to function at least
         one peer must be configured.  When configuring a peer,  the local
         end of the MSDP session must be configured.  This address is used
         to validate incoming connections to the peer and to establish
         connections to the remote peer.

         By default no local address is configured."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGroupEntry 18 }

tmnxMsdpNgPeerGroupMode          OBJECT-TYPE
    SYNTAX      INTEGER {
        standard   (1),
        mesh-group (2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupMode is used to configure groups of
         peers in a full mesh topology.

         MSDP peers can be grouped in a full-mesh topology that prevents
         excessive flooding of source-active messages to neighboring peers.
         When operating in meshed mode, source-active messages received from
         a mesh group member are always accepted but are not flooded to other
         members of the same mesh group.  As a result, these source-active
         messages are only flooded to non-mesh group peers or members of
         other mesh groups.

         By default 'standard' (non-meshed) mode is used."
    DEFVAL      { standard }
    ::= { tmnxMsdpNgPeerGroupEntry 19 }

tmnxMsdpNgPeerGroupMaxActSources OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..1000000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupMaxActSources specifies the
         maximum number of source active messages that will be accepted by
         this MSDP peer group.  This effectively controls the number of
         active sources that can be stored on the system.

         By default, no limit is placed on the number of source active
         messages and this is specified by the value '-1'.  A value of
         0 means that no source active messages will be accepted."
    DEFVAL      { -1 }
    ::= { tmnxMsdpNgPeerGroupEntry 20 }

tmnxMsdpNgPeerGroupActMsgsExMax  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGroupActMsgsExMax indicates the number of
         source active messages received from this group that exceeded the
         established maximum number."
    ::= { tmnxMsdpNgPeerGroupEntry 21 }

tmnxMsdpNgPeerGrpSARejExpPolicy  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpSARejExpPolicy indicates the number of
         source active messages received from this group that were were not
         sent due to export policy."
    ::= { tmnxMsdpNgPeerGroupEntry 22 }

tmnxMsdpNgPeerGrpSARejImpPolicy  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpSARejImpPolicy indicates the number of
         source active messages received from this group that were rejected due
         to import policy."
    ::= { tmnxMsdpNgPeerGroupEntry 23 }

tmnxMsdpNgPeerGrpPeerTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxMsdpNgPeerGrpPeerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgPeerGrpPeerTable table provides a listing of all peers
         under MSDP Peer Groups."
    ::= { tmnxMsdpNgObjects 5 }

tmnxMsdpNgPeerGrpPeerEntry       OBJECT-TYPE
    SYNTAX      TmnxMsdpNgPeerGrpPeerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry representing a peer in an MSDP Peer Group. Entries can be
         created and deleted via SNMP SET operations."
    INDEX       {
        vRtrID,
        tmnxMsdpNgPeerGroupName,
        tmnxMsdpNgPeerGrpPeerAddressType,
        tmnxMsdpNgPeerGrpPeerAddress
    }
    ::= { tmnxMsdpNgPeerGrpPeerTable 1 }

TmnxMsdpNgPeerGrpPeerEntry       ::= SEQUENCE
{
    tmnxMsdpNgPeerGrpPeerAddressType InetAddressType,
    tmnxMsdpNgPeerGrpPeerAddress     InetAddress,
    tmnxMsdpNgPeerGrpPeerRowStatus   RowStatus,
    tmnxMsdpNgPeerGrpPeerMaxActSrcs  Integer32,
    tmnxMsdpNgPeerGrpPeerMsgRcvRt    Unsigned32,
    tmnxMsdpNgPeerGrpPeerMsgRxRtTime Unsigned32,
    tmnxMsdpNgPeerGrpPeerMsgRcvRtThd Gauge32,
    tmnxMsdpNgPeerGrpPeerAuthKey     OCTET STRING,
    tmnxMsdpNgPeerGrpPeerAKeyEncrypt TruthValue,
    tmnxMsdpNgPeerGrpPeerDefaultPeer TruthValue,
    tmnxMsdpNgPeerGrpPeerAdminState  TmnxAdminState,
    tmnxMsdpNgPeerGrpPeerExportPlcy1 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGrpPeerExportPlcy2 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGrpPeerExportPlcy3 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGrpPeerExportPlcy4 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGrpPeerExportPlcy5 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGrpPeerImportPlcy1 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGrpPeerImportPlcy2 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGrpPeerImportPlcy3 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGrpPeerImportPlcy4 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGrpPeerImportPlcy5 TPolicyStatementNameOrEmpty,
    tmnxMsdpNgPeerGrpPeerLocAddrType InetAddressType,
    tmnxMsdpNgPeerGrpPeerLocalAddr   InetAddress,
    tmnxMsdpNgPeerGrpPeerState       INTEGER,
    tmnxMsdpNgPeerGrpPeerLstUpOrDwn  TimeStamp,
    tmnxMsdpNgPeerGrpPeerConRetry    Counter32,
    tmnxMsdpNgPeerGrpPeerStateTimer  Unsigned32,
    tmnxMsdpNgPeerGrpPeerTimeout     Unsigned32,
    tmnxMsdpNgPeerGrpPeerSAAccepted  Gauge32,
    tmnxMsdpNgPeerGrpPeerSARx        Gauge32,
    tmnxMsdpNgPeerGrpPeerLastASLimit TimeStamp,
    tmnxMsdpNgPeerGrpPeerOpAddrType  InetAddressType,
    tmnxMsdpNgPeerGrpPeerOpAddr      InetAddress
}

tmnxMsdpNgPeerGrpPeerAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerAddressType indicates the type of
         address of the MSDP peer."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 1 }

tmnxMsdpNgPeerGrpPeerAddress     OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerAddress indicates the address of the
         MSDP peer."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 2 }

tmnxMsdpNgPeerGrpPeerRowStatus   OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "tmnxMsdpNgPeerGrpPeerRowStatus is the object used for creating and
         deleting row entries in this table."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 3 }

tmnxMsdpNgPeerGrpPeerMaxActSrcs  OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..1000000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerMaxActSrcs specifies the maximum
         number of source active messages that will be accepted by MSDP peer
         group peer. This effectively controls the number of active sources
         that can be stored on the system.

         By default, no limit is placed on the number of source active messages
         and this is specified by the value '-1'.  A value of
         0 means that no source active messages will be accepted."
    DEFVAL      { -1 }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 4 }

tmnxMsdpNgPeerGrpPeerMsgRcvRt    OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 10..10000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerMsgRcvRt specifies the  number
         of MSDP messages (including source active messages) that are read
         from the TCP session per tmnxMsdpNgPeerGrpPeerMsgRxRtTime seconds.

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value 0.

         Once the number of MSDP packets defined in
         tmnxMsdpNgPeerGrpPeerMsgRcvRtThd have been processed the rate of all
         other MSDP packets is rate limited by no longer accepting messages
         from the TCP session until tmnxMsdpNgPeerGrpPeerMsgRxRtTime seconds
         have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 5 }

tmnxMsdpNgPeerGrpPeerMsgRxRtTime OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 1..600)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerMsgRxRtTime specifies the time
         in seconds that together with tmnxMsdpNgPeerGrpPeerMsgRcvRt
         defines the number of  MSDP messages (including source active
         messages) that are read from the TCP session within the configured
         number of seconds.

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value 0.

         Once the number of MSDP packets defined in
         tmnxMsdpNgPeerGrpPeerMsgRcvRtThd have been processed the rate of all
         other MSDP packets is rate limited by no longer accepting messages
         from the TCP session until tmnxMsdpNgPeerGrpPeerMsgRxRtTime seconds
         have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 6 }

tmnxMsdpNgPeerGrpPeerMsgRcvRtThd OBJECT-TYPE
    SYNTAX      Gauge32 (0 | 1..1000000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerMsgRcvRtThd specifies the number of
         MSDP messages that can be processed before
         tmnxMsdpNgPeerGrpPeerMsgRcvRt is set. This is useful during system
         startup and initialization.

         By default, no MSDP messages are read from the TCP session and this is
         specified by the value 0.

         Once the number of MSDP packets defined in
         tmnxMsdpNgPeerGrpPeerMsgRcvRtThd have been processed the rate of all
         other MSDP packets is rate limited by no longer accepting messages
         from the TCP session until tmnxMsdpNgPeerGrpPeerMsgRxRtTime seconds
         have elapsed."
    DEFVAL      { 0 }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 7 }

tmnxMsdpNgPeerGrpPeerAuthKey     OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..256))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerAuthKey specifies the
         authentication key to be used for a specific MSDP peer group peering
         session.  Authentication is done using the MD-5 message based digest
         protocol.  Authentication cannot be configured globally and can be
         applied per peer only.  The authentication key can be any
         combination of letters or numbers.  Note that the string may
         contain embedded nulls.

         By default all MSDP messages are accepted and the MD5 signature option
         authentication key is disabled"
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 8 }

tmnxMsdpNgPeerGrpPeerAKeyEncrypt OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When the value of tmnxMsdpNgPeerGrpPeerAKeyEncrypt is 'true', the
         password specified by tmnxMsdpNgPeerGrpPeerAuthKey is in the encrypted
         form.

         When the value of tmnxMsdpNgPeerGrpPeerAKeyEncrypt is 'false', the
         password specified by tmnxMsdpNgPeerGrpPeerAuthKey is in plain text.

         tmnxMsdpNgPeerGrpPeerAuthKey and tmnxMsdpNgPeerGrpPeerAKeyEncrypt,
         which indicates whether or not the password string is encrypted, must
         be set together in the same SNMP request PDU or else the set request
         will fail with an inconsistentValue error."
    DEFVAL      { true }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 9 }

tmnxMsdpNgPeerGrpPeerDefaultPeer OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerDefaultPeer is used to configure a
         peer as the default MSDP peer due to which all source-active messages
         from the peer will be accepted without the usual
         peer-reverse-path-forwarding (RPF) check."
    DEFVAL      { false }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 10 }

tmnxMsdpNgPeerGrpPeerAdminState  OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerAdminState specifies the desired
         administrative state for a peer under a MSDP peer group. When
         tmnxMsdpNgPeerGrpPeerAdminState is 'outOfService' the operational
         state of the MSDP peer is disabled.

         By default, tmnxMsdpNgPeerGrpPeerAdminState is 'inService'."
    DEFVAL      { inService }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 11 }

tmnxMsdpNgPeerGrpPeerExportPlcy1 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerExportPlcy1 specifies the export
         policy to export Source Active (SA) state from the SA list into MSDP.
         A maximum of five policy names can be specified.
         tmnxMsdpNgPeerGrpPeerExportPlcy1 specifies policy number 1 at the
         protocol level.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 12 }

tmnxMsdpNgPeerGrpPeerExportPlcy2 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerExportPlcy2 specifies the export
         policy to export Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerGrpPeerExportPlcy2 specifies policy number 2 at the
         protocol level.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 13 }

tmnxMsdpNgPeerGrpPeerExportPlcy3 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerExportPlcy3 specifies the export
         policy to export Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerGrpPeerExportPlcy3 specifies policy number 3 at the
         protocol level.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 14 }

tmnxMsdpNgPeerGrpPeerExportPlcy4 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerExportPlcy4 specifies the export
         policy to export Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerGrpPeerExportPlcy4 specifies policy number 4 at the
         protocol level.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 15 }

tmnxMsdpNgPeerGrpPeerExportPlcy5 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerExportPlcy5 specifies the export
         policy to export Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerGrpPeerExportPlcy1 specifies policy number 5 at the
         protocol level.

         By default no export policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 16 }

tmnxMsdpNgPeerGrpPeerImportPlcy1 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerImportPlcy1 specifies the import
         policy to import Source Active (SA) state from the SA list into MSDP.
         A maximum of five policy names can be specified.
         tmnxMsdpNgPeerGrpPeerImportPlcy1 specifies policy number 1 at the
         protocol level.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 17 }

tmnxMsdpNgPeerGrpPeerImportPlcy2 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerImportPlcy2 specifies the import
         policy to import Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerGrpPeerImportPlcy2 specifies policy number 2 at the
         protocol level.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 18 }

tmnxMsdpNgPeerGrpPeerImportPlcy3 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerImportPlcy3 specifies the import
         policy to import Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerGrpPeerImportPlcy3 specifies policy number 3 at the
         protocol level.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 19 }

tmnxMsdpNgPeerGrpPeerImportPlcy4 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerImportPlcy4 specifies the import
         policy to import Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerGrpPeerImportPlcy4 specifies policy number 4 at the
         protocol level.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 20 }

tmnxMsdpNgPeerGrpPeerImportPlcy5 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerImportPlcy5 specifies the import
         policy to import Source Active (SA) state from the SA list into MSDP.
         tmnxMsdpNgPeerGrpPeerImportPlcy5 specifies policy number 5 at the
         protocol level.

         By default no import policies are applied and all SA entries are
         announced."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 21 }

tmnxMsdpNgPeerGrpPeerLocAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerLocAddrType specifies the type of
         tmnxMsdpNgPeerGrpPeerLocalAddr."
    DEFVAL      { unknown }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 22 }

tmnxMsdpNgPeerGrpPeerLocalAddr   OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerLocalAddr is used to configure
         the local end of a MSDP session. In order for MSDP to function at
         least one peer must be configured.  When configuring a peer, the
         local end of the MSDP session must be configured.  This address is
         used to validate incoming connections to the peer and to establish
         connections to the remote peer.

         By default no local address is configured."
    DEFVAL      { ''H }
    ::= { tmnxMsdpNgPeerGrpPeerEntry 23 }

tmnxMsdpNgPeerGrpPeerState       OBJECT-TYPE
    SYNTAX      INTEGER {
        listen      (0),
        established (1),
        inactive    (2),
        disabled    (3),
        connecting  (4)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerState indicates the status of the
         connection."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 24 }

tmnxMsdpNgPeerGrpPeerLstUpOrDwn  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerLstUpOrDwn indicates the time at
         which the most recent peer-state change occurred."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 25 }

tmnxMsdpNgPeerGrpPeerConRetry    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerConRetry indicates number of peer
         connection retry attempts."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 26 }

tmnxMsdpNgPeerGrpPeerStateTimer  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerStateTimer indicates the number of
         seconds to wait before another message is sent to a peer."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 27 }

tmnxMsdpNgPeerGrpPeerTimeout     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerTimeout indicates the number of
         seconds to wait for a response from the peer before declaring the peer
         unavailable."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 28 }

tmnxMsdpNgPeerGrpPeerSAAccepted  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerSAAccepted indicates the number of
         entries in the source-active cache accepted from the peer."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 29 }

tmnxMsdpNgPeerGrpPeerSARx        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerSARx indicates the number of entries
         in the source-active cache received by the peer."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 30 }

tmnxMsdpNgPeerGrpPeerLastASLimit OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerLastASLimit indicates the time that
         the last active source limit was triggered."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 31 }

tmnxMsdpNgPeerGrpPeerOpAddrType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerOpAddrType indicates the type of
         tmnxMsdpNgPeerGrpPeerOpAddr."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 32 }

tmnxMsdpNgPeerGrpPeerOpAddr      OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerGrpPeerOpAddr indicates the operational
         value of the local end of a MSDP session."
    ::= { tmnxMsdpNgPeerGrpPeerEntry 33 }

tmnxMsdpNgSourceTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxMsdpNgSourceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgSourceTable provides a listing of all MSDP Source
         configuration."
    ::= { tmnxMsdpNgObjects 6 }

tmnxMsdpNgSourceEntry            OBJECT-TYPE
    SYNTAX      TmnxMsdpNgSourceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An tmnxMsdpNgSourceEntry represents a MSDP Source configuration.

         Entries can be created and deleted via SNMP SET operations."
    INDEX       {
        vRtrID,
        tmnxMsdpNgSourcePrefixType,
        tmnxMsdpNgSourcePrefix,
        tmnxMsdpNgSourceMask
    }
    ::= { tmnxMsdpNgSourceTable 1 }

TmnxMsdpNgSourceEntry            ::= SEQUENCE
{
    tmnxMsdpNgSourcePrefixType       InetAddressType,
    tmnxMsdpNgSourcePrefix           InetAddress,
    tmnxMsdpNgSourceMask             InetAddressPrefixLength,
    tmnxMsdpNgSourceRowStatus        RowStatus,
    tmnxMsdpNgSourceMaxActiveSources Integer32,
    tmnxMsdpNgSourceDiscMethod       INTEGER,
    tmnxMsdpNgSourceSrcActMsgsExMax  Counter32,
    tmnxMsdpNgSourceLastExEventTime  TimeStamp
}

tmnxMsdpNgSourcePrefixType       OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSourcePrefixType indicates the type of
         tmnxMsdpNgSourcePrefix."
    ::= { tmnxMsdpNgSourceEntry 1 }

tmnxMsdpNgSourcePrefix           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSourcePrefix indicates the IP address of the
         sources from which the source active messages would be accepted."
    ::= { tmnxMsdpNgSourceEntry 2 }

tmnxMsdpNgSourceMask             OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..128)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSourceMask indicates the mask to be used along
         with tmnxMsdpNgSourcePrefix to obtain the range of addresses from
         which the router can accept source active messages. "
    ::= { tmnxMsdpNgSourceEntry 3 }

tmnxMsdpNgSourceRowStatus        OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "tmnxMsdpNgSourceRowStatus is the object used for creating and deleting
         row entries in this table."
    ::= { tmnxMsdpNgSourceEntry 4 }

tmnxMsdpNgSourceMaxActiveSources OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..1000000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSourceMaxActiveSources specifies the maximum
         number of source active messages that will be accepted by MSDP. This
         effectively controls the number of active sources that can be stored
         on the system.

         By default, no limit is placed on the number of source active messages
         and this is specified by the value '-1'.  A value of
         0 means that no source active messages will be accepted."
    DEFVAL      { -1 }
    ::= { tmnxMsdpNgSourceEntry 5 }

tmnxMsdpNgSourceDiscMethod       OBJECT-TYPE
    SYNTAX      INTEGER {
        dynamic    (0),
        configured (1)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSourceDiscMethod indicates the discovery method
         for this multicast source. If the source entry was created by an user,
         the value of this field is 'configured'. If the source was created
         dynamically, the value is 'dynamic'"
    ::= { tmnxMsdpNgSourceEntry 6 }

tmnxMsdpNgSourceSrcActMsgsExMax  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSourceSrcActMsgsExMax indicates the number of
         source active messages received from this source that exceeded the
         established maximum number."
    ::= { tmnxMsdpNgSourceEntry 7 }

tmnxMsdpNgSourceLastExEventTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSourceLastExEventTime indicates the time the
         last exceed event was triggered."
    ::= { tmnxMsdpNgSourceEntry 8 }

tmnxMsdpNgSATable                OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxMsdpNgSAEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgSATable table stores the MSDP Source Active(SA)
         advertisements currently in the MSDP speaker's cache."
    ::= { tmnxMsdpNgObjects 7 }

tmnxMsdpNgSAEntry                OBJECT-TYPE
    SYNTAX      TmnxMsdpNgSAEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry representing an MSDP SA advertisement.  The INDEX to
         this table includes msdpSACacheOriginRP for diagnosing
         incorrect MSDP advertisements; normally a Source and Group
         pair would be unique.

         This is a read-only table."
    INDEX       {
        vRtrID,
        tmnxMsdpNgSAGroupAddrType,
        tmnxMsdpNgSAGroupAddr,
        tmnxMsdpNgSASourceAddrType,
        tmnxMsdpNgSASourceAddr,
        tmnxMsdpNgSAOriginRPType,
        tmnxMsdpNgSAOriginRP
    }
    ::= { tmnxMsdpNgSATable 1 }

TmnxMsdpNgSAEntry                ::= SEQUENCE
{
    tmnxMsdpNgSAGroupAddrType        InetAddressType,
    tmnxMsdpNgSAGroupAddr            InetAddress,
    tmnxMsdpNgSASourceAddrType       InetAddressType,
    tmnxMsdpNgSASourceAddr           InetAddress,
    tmnxMsdpNgSAOriginRPType         InetAddressType,
    tmnxMsdpNgSAOriginRP             InetAddress,
    tmnxMsdpNgSAPrLearnFrType        InetAddressType,
    tmnxMsdpNgSAPeerLearntFrom       InetAddress,
    tmnxMsdpNgSARPFPeerType          InetAddressType,
    tmnxMsdpNgSARPFPeer              InetAddress,
    tmnxMsdpNgSAUpTime               TimeInterval,
    tmnxMsdpNgSAExpiryTime           TimeInterval
}

tmnxMsdpNgSAGroupAddrType        OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSAGroupAddrType indicates the address type of
         tmnxMsdpNgSAGroupAddr."
    ::= { tmnxMsdpNgSAEntry 1 }

tmnxMsdpNgSAGroupAddr            OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSAGroupAddr indicates the group address of the
         Source Active entry."
    ::= { tmnxMsdpNgSAEntry 2 }

tmnxMsdpNgSASourceAddrType       OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSASourceAddrType indicates the address type of
         tmnxMsdpNgSASourceAddr."
    ::= { tmnxMsdpNgSAEntry 3 }

tmnxMsdpNgSASourceAddr           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSASourceAddr indicates the source address of
         the Source Active entry."
    ::= { tmnxMsdpNgSAEntry 4 }

tmnxMsdpNgSAOriginRPType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSAOriginRPType indicates the address type of
         tmnxMsdpNgSAOriginRP."
    ::= { tmnxMsdpNgSAEntry 5 }

tmnxMsdpNgSAOriginRP             OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSAOriginRP indicates the origin RP address of
         the Source Active entry."
    ::= { tmnxMsdpNgSAEntry 6 }

tmnxMsdpNgSAPrLearnFrType        OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSAPrLearnFrType indicates the address type of
         tmnxMsdpNgSAPeerLearntFrom."
    ::= { tmnxMsdpNgSAEntry 7 }

tmnxMsdpNgSAPeerLearntFrom       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSAPeerLearntFrom indicates the peer from which
         this Source Active entry was last accepted."
    ::= { tmnxMsdpNgSAEntry 8 }

tmnxMsdpNgSARPFPeerType          OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARPFPeerType indicates the address type of
         tmnxMsdpNgSARPFPeer."
    ::= { tmnxMsdpNgSAEntry 9 }

tmnxMsdpNgSARPFPeer              OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARPFPeer indicates the peer from which
         an SA message corresponding to this cache entry would be accepted
         (i.e. the RPF peer for tmnxMsdpNgSAOriginRP).  This may be
         different than tmnxMsdpNgSAPeerLearntFrom if this entry was
         created by an MSDP SA-Response."
    ::= { tmnxMsdpNgSAEntry 10 }

tmnxMsdpNgSAUpTime               OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSAUpTime indicates the time since this entry
         was first placed in the Source Active (SA) cache.

         It is the difference between the time that the entry was first placed
         in the SA cache and the current time."
    ::= { tmnxMsdpNgSAEntry 11 }

tmnxMsdpNgSAExpiryTime           OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSAExpiryTime indicates the time remaining
         before this entry will expire from the Source Active (SA) cache.

         It is difference between the current time and the time that the entry
         will expire."
    ::= { tmnxMsdpNgSAEntry 12 }

tmnxMsdpNgPeerStatsTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxMsdpNgPeerStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The  table tmnxMsdpNgPeerStatsTable is the statistics information
         related to a MSDP peer."
    ::= { tmnxMsdpNgObjects 8 }

tmnxMsdpNgPeerStatsEntry         OBJECT-TYPE
    SYNTAX      TmnxMsdpNgPeerStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxMsdpNgPeerStatsEntry is an entry (conceptual row) in the
         tmnxMsdpNgPeerStatsTable. Each entry represents a MSDP peer related
         statistics information."
    INDEX       {
        vRtrID,
        tmnxMsdpNgPeerAddressType,
        tmnxMsdpNgPeerAddress
    }
    ::= { tmnxMsdpNgPeerStatsTable 1 }

TmnxMsdpNgPeerStatsEntry         ::= SEQUENCE
{
    tmnxMsdpNgPeerStatsActSrcLimExcd Counter32,
    tmnxMsdpNgPeerStatsLastStChange  TimeInterval,
    tmnxMsdpNgPeerStatsLastMsgPeer   TimeInterval,
    tmnxMsdpNgPeerStatsRPFFailures   Counter32,
    tmnxMsdpNgPeerStatsRemoteCloses  Counter32,
    tmnxMsdpNgPeerStatsPeerTimeouts  Counter32,
    tmnxMsdpNgPeerStatsSAMsgsSent    Counter32,
    tmnxMsdpNgPeerStatsSAMsgsRx      Counter32,
    tmnxMsdpNgPeerStatsSAReqMsgsSent Counter32,
    tmnxMsdpNgPeerStatsSAReqMsgsRx   Counter32,
    tmnxMsdpNgPeerStatsSAResMsgsSent Counter32,
    tmnxMsdpNgPeerStatsSAResMsgsRx   Counter32,
    tmnxMsdpNgPeerStatsKAMsgsSent    Counter32,
    tmnxMsdpNgPeerStatsKAMsgsRx      Counter32,
    tmnxMsdpNgPeerStatsUnknMsgsRx    Counter32,
    tmnxMsdpNgPeerStatsErrMsgsRx     Counter32,
    tmnxMsdpNgPeerStatsSALearnt      Gauge32,
    tmnxMsdpNgPeerStatsSARejExpPlcy  Counter32,
    tmnxMsdpNgPeerStatsSARejImpPlcy  Counter32,
    tmnxMsdpNgPeerStatsResvMsgsRx    Counter32
}

tmnxMsdpNgPeerStatsActSrcLimExcd OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsActSrcLimExcd indicates the number of
         times the global active source limit has been exceeded by this peer
         instance."
    ::= { tmnxMsdpNgPeerStatsEntry 1 }

tmnxMsdpNgPeerStatsLastStChange  OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsLastStChange indicates how long ago
         the peer state changed."
    ::= { tmnxMsdpNgPeerStatsEntry 2 }

tmnxMsdpNgPeerStatsLastMsgPeer   OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsLastMsgPeer indicates how long ago the
         last message was received from this peer instance."
    ::= { tmnxMsdpNgPeerStatsEntry 3 }

tmnxMsdpNgPeerStatsRPFFailures   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsRPFFailures indicates number of
         reverse path forwarding (RPF) failures."
    ::= { tmnxMsdpNgPeerStatsEntry 4 }

tmnxMsdpNgPeerStatsRemoteCloses  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsRemoteCloses indicates the number of
         times the remote peer closed."
    ::= { tmnxMsdpNgPeerStatsEntry 5 }

tmnxMsdpNgPeerStatsPeerTimeouts  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsPeerTimeouts indicates the number of
         peer timeouts."
    ::= { tmnxMsdpNgPeerStatsEntry 6 }

tmnxMsdpNgPeerStatsSAMsgsSent    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsSAMsgsSent indicates the number of
         source-active messages sent."
    ::= { tmnxMsdpNgPeerStatsEntry 7 }

tmnxMsdpNgPeerStatsSAMsgsRx      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsSAMsgsRx indicates the number of
         source-active messages received."
    ::= { tmnxMsdpNgPeerStatsEntry 8 }

tmnxMsdpNgPeerStatsSAReqMsgsSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsSAReqMsgsSent indicates the number of
         source-active request messages sent."
    ::= { tmnxMsdpNgPeerStatsEntry 9 }

tmnxMsdpNgPeerStatsSAReqMsgsRx   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsSAReqMsgsRx indicates the number of
         source-active request messages received."
    ::= { tmnxMsdpNgPeerStatsEntry 10 }

tmnxMsdpNgPeerStatsSAResMsgsSent OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsSAResMsgsSent indicates the number of
         source-active response messages sent."
    ::= { tmnxMsdpNgPeerStatsEntry 11 }

tmnxMsdpNgPeerStatsSAResMsgsRx   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsSAResMsgsRx indicates the number of
         source-active response messages received."
    ::= { tmnxMsdpNgPeerStatsEntry 12 }

tmnxMsdpNgPeerStatsKAMsgsSent    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsKAMsgsSent indicates the number of
         keep-alive messages sent."
    ::= { tmnxMsdpNgPeerStatsEntry 13 }

tmnxMsdpNgPeerStatsKAMsgsRx      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsKAMsgsRx indicates the number of
         keep-alive messages received."
    ::= { tmnxMsdpNgPeerStatsEntry 14 }

tmnxMsdpNgPeerStatsUnknMsgsRx    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsUnknMsgsRx indicates the number of
         unknown messages received."
    ::= { tmnxMsdpNgPeerStatsEntry 15 }

tmnxMsdpNgPeerStatsErrMsgsRx     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsErrMsgsRx indicates number of error
         messages received."
    ::= { tmnxMsdpNgPeerStatsEntry 16 }

tmnxMsdpNgPeerStatsSALearnt      OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsSALearnt indicates the number of
         unique source active entries in the cache learned from the peer."
    ::= { tmnxMsdpNgPeerStatsEntry 17 }

tmnxMsdpNgPeerStatsSARejExpPlcy  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsSARejExpPlcy indicates the number of
         source active messages from the peer that were not sent due to export
         policy."
    ::= { tmnxMsdpNgPeerStatsEntry 18 }

tmnxMsdpNgPeerStatsSARejImpPlcy  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsSARejImpPlcy indicates the number of
         source active messages from the peer that were rejected due to import
         policy."
    ::= { tmnxMsdpNgPeerStatsEntry 19 }

tmnxMsdpNgPeerStatsResvMsgsRx    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgPeerStatsResvMsgsRx indicates the number of
         MSDP messages received with type 'Reserved'."
    ::= { tmnxMsdpNgPeerStatsEntry 20 }

tmnxMsdpNgSrcActRejTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxMsdpNgSrcActRejEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgSrcActRejTable table stores the MSDP Source Active(SA)
         advertisements rejected from the MSDP speaker's cache."
    ::= { tmnxMsdpNgObjects 9 }

tmnxMsdpNgSrcActRejEntry         OBJECT-TYPE
    SYNTAX      TmnxMsdpNgSrcActRejEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry representing an MSDP SA advertisement that is rejected.

         This is a read-only table."
    INDEX       {
        vRtrID,
        tmnxMsdpNgSARejPeerGroupName,
        tmnxMsdpNgSARejGroupAddrType,
        tmnxMsdpNgSARejGroupAddr,
        tmnxMsdpNgSARejSourceAddrType,
        tmnxMsdpNgSARejSourceAddr,
        tmnxMsdpNgSARejOriginRPType,
        tmnxMsdpNgSARejOriginRP,
        tmnxMsdpNgSARejPeerAddrType,
        tmnxMsdpNgSARejPeerAddr
    }
    ::= { tmnxMsdpNgSrcActRejTable 1 }

TmnxMsdpNgSrcActRejEntry         ::= SEQUENCE
{
    tmnxMsdpNgSARejPeerGroupName     TNamedItemOrEmpty,
    tmnxMsdpNgSARejGroupAddrType     InetAddressType,
    tmnxMsdpNgSARejGroupAddr         InetAddress,
    tmnxMsdpNgSARejSourceAddrType    InetAddressType,
    tmnxMsdpNgSARejSourceAddr        InetAddress,
    tmnxMsdpNgSARejOriginRPType      InetAddressType,
    tmnxMsdpNgSARejOriginRP          InetAddress,
    tmnxMsdpNgSARejPeerAddrType      InetAddressType,
    tmnxMsdpNgSARejPeerAddr          InetAddress,
    tmnxMsdpNgSARejFailureReason     INTEGER
}

tmnxMsdpNgSARejPeerGroupName     OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejPeerGroupName indicates the peer group
         name of the Source Active entry that is rejected."
    ::= { tmnxMsdpNgSrcActRejEntry 1 }

tmnxMsdpNgSARejGroupAddrType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejGroupAddrType indicates the address type
         of tmnxMsdpNgSARejGroupAddr."
    ::= { tmnxMsdpNgSrcActRejEntry 2 }

tmnxMsdpNgSARejGroupAddr         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejGroupAddr indicates the group address of
         the Source Active entry that is rejected."
    ::= { tmnxMsdpNgSrcActRejEntry 3 }

tmnxMsdpNgSARejSourceAddrType    OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejSourceAddrType indicates the address type
         of tmnxMsdpNgSARejSourceAddr."
    ::= { tmnxMsdpNgSrcActRejEntry 4 }

tmnxMsdpNgSARejSourceAddr        OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejSourceAddr indicates the source address of
         the Source Active entry that is rejected."
    ::= { tmnxMsdpNgSrcActRejEntry 5 }

tmnxMsdpNgSARejOriginRPType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejOriginRPType indicates the address type of
         tmnxMsdpNgSARejOriginRP."
    ::= { tmnxMsdpNgSrcActRejEntry 6 }

tmnxMsdpNgSARejOriginRP          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejOriginRP indicates the origin rendezvous
         point (RP) address of the Source Active entry that is rejected."
    ::= { tmnxMsdpNgSrcActRejEntry 7 }

tmnxMsdpNgSARejPeerAddrType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejPeerAddrType indicates the address type of
         tmnxMsdpNgSARejPeerAddr."
    ::= { tmnxMsdpNgSrcActRejEntry 8 }

tmnxMsdpNgSARejPeerAddr          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejPeerAddr indicates the peer from which
         this rejected Source Active entry was last received."
    ::= { tmnxMsdpNgSrcActRejEntry 9 }

tmnxMsdpNgSARejFailureReason     OBJECT-TYPE
    SYNTAX      INTEGER {
        importPolicyFailure          (1),
        exportPolicyFailure          (2),
        rpfFailure                   (3),
        actSrcLimitExceeded          (4),
        srcActSrcLimitExceeded       (5),
        peerActSrcLimitExceeded      (6),
        groupActSrcLimitExceeded     (7),
        groupPeerActSrcLimitExceeded (8)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMsdpNgSARejFailureReason indicates the reason why
         this Source Active entry is rejected."
    ::= { tmnxMsdpNgSrcActRejEntry 10 }

tmnxMsdpNgConformance            OBJECT IDENTIFIER ::= { tmnxSRConfs 104 }

tmnxMsdpNgCompliances            OBJECT IDENTIFIER ::= { tmnxMsdpNgConformance 1 }

tmnxMsdpNgV13v0Compliance        MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of MSDP features on Nokia 7x50
         SR series systems."
    MODULE
        MANDATORY-GROUPS {
            tmnxMsdpNgGeneralGroup,
            tmnxMsdpNgPeerGroup,
            tmnxMsdpNgPeerGroupGroup,
            tmnxMsdpNgSourceGroup,
            tmnxMsdpNgSAGroup,
            tmnxMsdpNgSARejGroup,
            tmnxMsdpNgNotificationGroup
        }
    ::= { tmnxMsdpNgCompliances 1 }

tmnxMsdpNgGroups                 OBJECT IDENTIFIER ::= { tmnxMsdpNgConformance 2 }

tmnxMsdpNgGeneralGroup           OBJECT-GROUP
    OBJECTS     {
        tmnxMsdpNgGeneralTableLstChanged,
        tmnxMsdpNgMaxActiveSources,
        tmnxMsdpNgMsgRcvRate,
        tmnxMsdpNgMsgRcvRateTime,
        tmnxMsdpNgMsgRcvRateThd,
        tmnxMsdpNgDataEncapsulation,
        tmnxMsdpNgAdminState,
        tmnxMsdpNgExportPolicy1,
        tmnxMsdpNgExportPolicy2,
        tmnxMsdpNgExportPolicy3,
        tmnxMsdpNgExportPolicy4,
        tmnxMsdpNgExportPolicy5,
        tmnxMsdpNgImportPolicy1,
        tmnxMsdpNgImportPolicy2,
        tmnxMsdpNgImportPolicy3,
        tmnxMsdpNgImportPolicy4,
        tmnxMsdpNgImportPolicy5,
        tmnxMsdpNgLocalAddress,
        tmnxMsdpNgLocalAddressType,
        tmnxMsdpNgStatusPeerCount,
        tmnxMsdpNgStatusPeersEstablished,
        tmnxMsdpNgStatusSACount,
        tmnxMsdpNgStatusLastTimeUp,
        tmnxMsdpNgStatusActSrcLimExceed,
        tmnxMsdpNgRpfLookupSequence,
        tmnxMsdpNgSACacheLifetime,
        tmnxMsdpNgSARejectExportPolicy,
        tmnxMsdpNgSARejectImportPolicy
    }
    STATUS      current
    DESCRIPTION
        "A collection of global objects supporting management of MSDP protocol
         on Nokia 7x50 SR series systems."
    ::= { tmnxMsdpNgGroups 1 }

tmnxMsdpNgPeerGroup              OBJECT-GROUP
    OBJECTS     {
        tmnxMsdpNgPeerRowStatus,
        tmnxMsdpNgPeerMaxActiveSources,
        tmnxMsdpNgPeerMsgRcvRate,
        tmnxMsdpNgPeerMsgRcvRateTime,
        tmnxMsdpNgPeerMsgRcvRateThd,
        tmnxMsdpNgPeerAuthKey,
        tmnxMsdpNgPeerAuthKeyEncrypted,
        tmnxMsdpNgPeerDefaultPeer,
        tmnxMsdpNgPeerAdminState,
        tmnxMsdpNgPeerExportPolicy1,
        tmnxMsdpNgPeerExportPolicy2,
        tmnxMsdpNgPeerExportPolicy3,
        tmnxMsdpNgPeerExportPolicy4,
        tmnxMsdpNgPeerExportPolicy5,
        tmnxMsdpNgPeerImportPolicy1,
        tmnxMsdpNgPeerImportPolicy2,
        tmnxMsdpNgPeerImportPolicy3,
        tmnxMsdpNgPeerImportPolicy4,
        tmnxMsdpNgPeerImportPolicy5,
        tmnxMsdpNgPeerLocalAddressType,
        tmnxMsdpNgPeerLocalAddress,
        tmnxMsdpNgPeerGrpPeerRowStatus,
        tmnxMsdpNgPeerGrpPeerMaxActSrcs,
        tmnxMsdpNgPeerGrpPeerMsgRcvRt,
        tmnxMsdpNgPeerGrpPeerMsgRxRtTime,
        tmnxMsdpNgPeerGrpPeerMsgRcvRtThd,
        tmnxMsdpNgPeerGrpPeerAuthKey,
        tmnxMsdpNgPeerGrpPeerAKeyEncrypt,
        tmnxMsdpNgPeerGrpPeerDefaultPeer,
        tmnxMsdpNgPeerGrpPeerAdminState,
        tmnxMsdpNgPeerGrpPeerExportPlcy1,
        tmnxMsdpNgPeerGrpPeerExportPlcy2,
        tmnxMsdpNgPeerGrpPeerExportPlcy3,
        tmnxMsdpNgPeerGrpPeerExportPlcy4,
        tmnxMsdpNgPeerGrpPeerExportPlcy5,
        tmnxMsdpNgPeerGrpPeerImportPlcy1,
        tmnxMsdpNgPeerGrpPeerImportPlcy2,
        tmnxMsdpNgPeerGrpPeerImportPlcy3,
        tmnxMsdpNgPeerGrpPeerImportPlcy4,
        tmnxMsdpNgPeerGrpPeerImportPlcy5,
        tmnxMsdpNgPeerGrpPeerLocAddrType,
        tmnxMsdpNgPeerGrpPeerLocalAddr,
        tmnxMsdpNgPeerStatsActSrcLimExcd,
        tmnxMsdpNgPeerStatsLastStChange,
        tmnxMsdpNgPeerStatsLastMsgPeer,
        tmnxMsdpNgPeerStatsRPFFailures,
        tmnxMsdpNgPeerStatsRemoteCloses,
        tmnxMsdpNgPeerStatsPeerTimeouts,
        tmnxMsdpNgPeerStatsSAMsgsSent,
        tmnxMsdpNgPeerStatsSAMsgsRx,
        tmnxMsdpNgPeerStatsSAReqMsgsSent,
        tmnxMsdpNgPeerStatsSAReqMsgsRx,
        tmnxMsdpNgPeerStatsSAResMsgsSent,
        tmnxMsdpNgPeerStatsSAResMsgsRx,
        tmnxMsdpNgPeerStatsKAMsgsSent,
        tmnxMsdpNgPeerStatsKAMsgsRx,
        tmnxMsdpNgPeerStatsUnknMsgsRx,
        tmnxMsdpNgPeerStatsErrMsgsRx,
        tmnxMsdpNgPeerStatsSALearnt,
        tmnxMsdpNgPeerStatsSARejExpPlcy,
        tmnxMsdpNgPeerStatsSARejImpPlcy,
        tmnxMsdpNgPeerStatsResvMsgsRx,
        tmnxMsdpNgPeerState,
        tmnxMsdpNgPeerLastUpOrDown,
        tmnxMsdpNgPeerConRetry,
        tmnxMsdpNgPeerStateTimer,
        tmnxMsdpNgPeerTimeout,
        tmnxMsdpNgPeerSAAccepted,
        tmnxMsdpNgPeerSARx,
        tmnxMsdpNgPeerLastASLimit,
        tmnxMsdpNgPeerOperLclAddrType,
        tmnxMsdpNgPeerOperLclAddr,
        tmnxMsdpNgPeerGrpPeerState,
        tmnxMsdpNgPeerGrpPeerLstUpOrDwn,
        tmnxMsdpNgPeerGrpPeerConRetry,
        tmnxMsdpNgPeerGrpPeerStateTimer,
        tmnxMsdpNgPeerGrpPeerTimeout,
        tmnxMsdpNgPeerGrpPeerSAAccepted,
        tmnxMsdpNgPeerGrpPeerSARx,
        tmnxMsdpNgPeerGrpPeerLastASLimit,
        tmnxMsdpNgPeerGrpPeerOpAddrType,
        tmnxMsdpNgPeerGrpPeerOpAddr
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects supporting management of MSDP peers on Nokia
         7x50 SR series systems."
    ::= { tmnxMsdpNgGroups 2 }

tmnxMsdpNgPeerGroupGroup         OBJECT-GROUP
    OBJECTS     {
        tmnxMsdpNgPeerGroupRowStatus,
        tmnxMsdpNgPeerGroupMsgRcvRate,
        tmnxMsdpNgPeerGrpMsgRcvRateTime,
        tmnxMsdpNgPeerGroupMsgRcvRateThd,
        tmnxMsdpNgPeerGroupAdminState,
        tmnxMsdpNgPeerGroupExportPolicy1,
        tmnxMsdpNgPeerGroupExportPolicy2,
        tmnxMsdpNgPeerGroupExportPolicy3,
        tmnxMsdpNgPeerGroupExportPolicy4,
        tmnxMsdpNgPeerGroupExportPolicy5,
        tmnxMsdpNgPeerGroupImportPolicy1,
        tmnxMsdpNgPeerGroupImportPolicy2,
        tmnxMsdpNgPeerGroupImportPolicy3,
        tmnxMsdpNgPeerGroupImportPolicy4,
        tmnxMsdpNgPeerGroupImportPolicy5,
        tmnxMsdpNgPeerGroupLocalAddrType,
        tmnxMsdpNgPeerGroupLocalAddress,
        tmnxMsdpNgPeerGroupMode,
        tmnxMsdpNgPeerGroupMaxActSources,
        tmnxMsdpNgPeerGroupActMsgsExMax,
        tmnxMsdpNgPeerGrpSARejExpPolicy,
        tmnxMsdpNgPeerGrpSARejImpPolicy
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects supporting management of MSDP peer groups on
         Nokia 7x50 SR series systems."
    ::= { tmnxMsdpNgGroups 3 }

tmnxMsdpNgSourceGroup            OBJECT-GROUP
    OBJECTS     {
        tmnxMsdpNgSourceRowStatus,
        tmnxMsdpNgSourceMaxActiveSources,
        tmnxMsdpNgSourceDiscMethod,
        tmnxMsdpNgSourceSrcActMsgsExMax,
        tmnxMsdpNgSourceLastExEventTime
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects supporting management of MSDP sources on Nokia
         7x50 SR series systems."
    ::= { tmnxMsdpNgGroups 4 }

tmnxMsdpNgSAGroup                OBJECT-GROUP
    OBJECTS     {
        tmnxMsdpNgSAPrLearnFrType,
        tmnxMsdpNgSAPeerLearntFrom,
        tmnxMsdpNgSARPFPeerType,
        tmnxMsdpNgSARPFPeer,
        tmnxMsdpNgSAUpTime,
        tmnxMsdpNgSAExpiryTime
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects supporting management of MSDP source active
         information on Nokia 7x50 SR series systems."
    ::= { tmnxMsdpNgGroups 5 }

tmnxMsdpNgNotificationGroup      NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxMsdpNgActSrcLimExcd,
        tmnxMsdpNgPeerActSrcLimExcd,
        tmnxMsdpNgRPFFailure,
        tmnxMsdpNgSourceSrcActMsgsExcd,
        tmnxMsdpNgGroupSrcActMsgsExcd
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting management of the MSDP
         operations on Nokia 7x50 SR series systems."
    ::= { tmnxMsdpNgGroups 6 }

tmnxMsdpNgSARejGroup             OBJECT-GROUP
    OBJECTS     {
        tmnxMsdpNgSARejFailureReason
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects supporting management of MSDP rejected source
         active information on Nokia 7x50 SR series systems."
    ::= { tmnxMsdpNgGroups 7 }

tmnxMsdpNgNotifyPrefix           OBJECT IDENTIFIER ::= { tmnxSRNotifyPrefix 104 }

tmnxMsdpNgNotifications          OBJECT IDENTIFIER ::= { tmnxMsdpNgNotifyPrefix 0 }

tmnxMsdpNgActSrcLimExcd          NOTIFICATION-TYPE
    OBJECTS     {
        tmnxMsdpNgMaxActiveSources,
        tmnxMsdpNgStatusActSrcLimExceed
    }
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgActSrcLimExcd event is generated whenever the global
         active source limit has been exceeded."
    ::= { tmnxMsdpNgNotifications 1 }

tmnxMsdpNgPeerActSrcLimExcd      NOTIFICATION-TYPE
    OBJECTS     {
        tmnxMsdpNgPeerStatsActSrcLimExcd
    }
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgPeerActSrcLimExcd event is generated whenever the active
         source limit has been exceeded for the peer."
    ::= { tmnxMsdpNgNotifications 2 }

tmnxMsdpNgRPFFailure             NOTIFICATION-TYPE
    OBJECTS     {
        tmnxMsdpNgSARPFPeerType,
        tmnxMsdpNgSARPFPeer
    }
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgRPFFailure event is generated whenever a RPF(Reverse
         Path Forwarding) failure occurs for a source configured by user."
    ::= { tmnxMsdpNgNotifications 3 }

tmnxMsdpNgSourceSrcActMsgsExcd   NOTIFICATION-TYPE
    OBJECTS     {
        tmnxMsdpNgSourceMaxActiveSources,
        tmnxMsdpNgSourceSrcActMsgsExMax
    }
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgSourceSrcActMsgsExcd event is generated when the source
         active messages received from this source has exceeded the established
         maximum number."
    ::= { tmnxMsdpNgNotifications 4 }

tmnxMsdpNgGroupSrcActMsgsExcd    NOTIFICATION-TYPE
    OBJECTS     {
        tmnxMsdpNgPeerGroupMaxActSources,
        tmnxMsdpNgPeerGroupActMsgsExMax
    }
    STATUS      current
    DESCRIPTION
        "The tmnxMsdpNgGroupSrcActMsgsExcd event is generated when the source
         active messages received from this group has exceeded the established
         maximum number."
    ::= { tmnxMsdpNgNotifications 5 }

END
