TIMETRA-VIDEO-MIB DEFINITIONS ::= BEGIN

IMPORTS
    CounterBasedGauge64
                                                         FROM HCNUM-TC
    InetAddress, InetAddressPrefixLength,
    InetAddressType, InetPortNumber
                                                         FROM INET-ADDRESS-MIB
    MODULE-COMPLIANCE, NOTIFICATION-GROUP,
    OBJECT-GROUP
                                                         FROM SNMPv2-CONF
    Counter32, Counter64, Gauge32,
    MODULE-IDENTITY, NOTIFICATION-TYPE,
    OBJECT-TYPE, Unsigned32
                                                         FROM SNMPv2-SMI
    DateAndTime, RowStatus,
    TEXTUAL-CONVENTION, TimeStamp,
    TruthValue
                                                         FROM SNMPv2-TC
    tmnxCardSlotNum, tmnxChassisIndex,
    tmnxMDASlotNum
                                                         FROM TIMETRA-CHASSIS-MIB
    TFilterID
                                                         FROM TIMETRA-FILTER-MIB
    timetraSRMIBModules, tmnxSRConfs,
    tmnxSRNotifyPrefix, tmnxSRObjs
                                                         FROM TIMETRA-GLOBAL-MIB
    TmnxMcPathVdoBufferSize,
    TmnxMcPathVdoChlType
                                                         FROM TIMETRA-MCAST-PATH-MGMT-MIB
    svcId
                                                         FROM TIMETRA-SERV-MIB
    InterfaceIndex, TCpmProtPolicyID,
    TItemDescription, TNamedItem,
    TNamedItemOrEmpty, TSapEgressPolicyID,
    TSapIngressPolicyID, TmnxAdminState,
    TmnxEnabledDisabled, TmnxEsaNum,
    TmnxEsaVappNum, TmnxOperState,
    TmnxServId, TmnxStrSapId,
    TmnxVdoAnalyzerAlarm,
    TmnxVdoAnalyzerAlarmStates,
    TmnxVdoFccServerMode, TmnxVdoGrpId,
    TmnxVdoGrpIdIndex, TmnxVdoIfName,
    TmnxVdoOutputFormat, TmnxVdoStatInt
                                                         FROM TIMETRA-TC-MIB
    ;

timetraVideoMIBModule            MODULE-IDENTITY
    LAST-UPDATED "201701010000Z"
    ORGANIZATION "Nokia"
    CONTACT-INFO
        "Nokia SROS Support
         Web: http://www.nokia.com"
    DESCRIPTION
        "This document is the SNMP MIB module to manage and provision the
         video-related features including Fast Channel Change (FCC), Reliable
         Delivery (RD) and Ad Insert (ADI) for the Nokia SROS device.

         Copyright 2008-2018 Nokia. All rights reserved. Reproduction of this
         document is authorized on the condition that the foregoing copyright
         notice is included.

         This SNMP MIB module (Specification) embodies Nokia's proprietary
         intellectual property. Nokia retains all title and ownership in the
         Specification, including any revisions.

         Nokia grants all interested parties a non-exclusive license to use and
         distribute an unmodified copy of this Specification in connection with
         management of Nokia products, and without fee, provided this copyright
         notice and license appear on all copies.

         This Specification is supplied 'as is', and Nokia makes no warranty,
         either express or implied, as to the use, operation, condition, or
         performance of the Specification."

    REVISION    "201701010000Z"
    DESCRIPTION
        "Rev 15.0               1 Jan 2017 00:00
         15.0 release of the TIMETRA-VIDEO-MIB.mib."

    REVISION    "201601010000Z"
    DESCRIPTION
        "Rev 14.0               1 Jan 2016 00:00
         14.0 release of the TIMETRA-VIDEO-MIB.mib."

    REVISION    "201102010000Z"
    DESCRIPTION
        "Rev 9.0                1 Feb 2011 00:00
         9.0 release of the TIMETRA-VIDEO-MIB.mib."

    REVISION    "200902280000Z"
    DESCRIPTION
        "Rev 7.0                28 Feb 2009 00:00
         7.0 release of the TIMETRA-VIDEO-MIB.mib."

    REVISION    "200807250000Z"
    DESCRIPTION
        "Rev 0.1            15 July 2008 00:00
         Initial version of the TIMETRA-VIDEO-MIB."

    ::= { timetraSRMIBModules 61 }

TmnxVdoPIDType                   ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "TmnxVdoPIDType is an enumerated integer whose value indicates the type
         of stream carried by this PID.

         other  (0) - Unspecified stream type
         audio  (1) - audio stream
         video  (2) - video stream
         data   (3) - data stream
         ca     (4) - conditional access stream
         scte35 (5) - Society of Cable Telecommunications
                      Engineers 35 stream
         pat    (6) - program association table
         pcr    (7) - program clock reference
         pmt    (8) - program map table."
    SYNTAX      INTEGER {
        other  (0),
        audio  (1),
        video  (2),
        data   (3),
        ca     (4),
        scte35 (5),
        pat    (6),
        pcr    (7),
        pmt    (8)
    }

TmnxVdoPTS                       ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The data type describes the Presentation Timestamp (PTS) which
         indicates the time of presentation in the system decoder of a
         presentation unit of an elementary stream. The value of PTS is
         measured in units of 90-KHz clock periods.

         Format of PTS is a 33-bit string, left bit first, where left is the
         order in which bit strings are written in 13818-1 International
         Standard. The most significant 7 bits will be padded with zeroes."
    REFERENCE
        "ISO/IEC 13818-1:2000(E), Section 2.2.6"
    SYNTAX      OCTET STRING (SIZE (5))

TmnxMDILossRate                  ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "TmnxMDILossRate is an octet string encoding of Media Delivery Index
         (MDI) loss rate that is represented as an 64-bit unsigned fixed-point
         number. The integer part is in the first 32 bits and the fraction part
         is in the last 32 bits."
    REFERENCE
        "RFC-4445, April 2006, Section 3.2"
    SYNTAX      OCTET STRING (SIZE (8))

TmnxWmPercent                    ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The percentage type for bandwidth and session watermarks."
    SYNTAX      Unsigned32 (1..99)

tmnxVdo                          OBJECT IDENTIFIER ::= { tmnxSRObjs 61 }

tmnxVdoObjs                      OBJECT IDENTIFIER ::= { tmnxVdo 1 }

tmnxVdoIfTable                   OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxVdoIfTable has an entry for each video interface configured in
         the system."
    ::= { tmnxVdoObjs 1 }

tmnxVdoIfEntry                   OBJECT-TYPE
    SYNTAX      TmnxVdoIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a video interface in the system. Entries can
         be created and deleted by the user."
    INDEX       {
        svcId,
        tmnxVdoIfName
    }
    ::= { tmnxVdoIfTable 1 }

TmnxVdoIfEntry                   ::= SEQUENCE
{
    tmnxVdoIfName                    TmnxVdoIfName,
    tmnxVdoIfRowStatus               RowStatus,
    tmnxVdoIfLastChanged             TimeStamp,
    tmnxVdoIfAdminState              TmnxAdminState,
    tmnxVdoIfOperState               TmnxOperState,
    tmnxVdoIfVrtrIfIndex             InterfaceIndex,
    tmnxVdoIfDescription             TItemDescription,
    tmnxVdoIfVdoGrpId                TmnxVdoGrpId,
    tmnxVdoIfIngressQosPolicyId      TSapIngressPolicyID,
    tmnxVdoIfEgressQosPolicyId       TSapEgressPolicyID,
    tmnxVdoIfAdi                     TruthValue,
    tmnxVdoIfRTClientAddrType        InetAddressType,
    tmnxVdoIfRTClientAddr            InetAddress,
    tmnxVdoIfGatewayAddrType         InetAddressType,
    tmnxVdoIfGatewayAddr             InetAddress,
    tmnxVdoIfMcastSvcId              TmnxServId,
    tmnxVdoIfIngressIpFilterId       TFilterID,
    tmnxVdoIfIngressMacFilterId      TFilterID,
    tmnxVdoIfEgressIpFilterId        TFilterID,
    tmnxVdoIfEgressMacFilterId       TFilterID,
    tmnxVdoIfScte30ControlAddrType   InetAddressType,
    tmnxVdoIfScte30ControlAddr       InetAddress,
    tmnxVdoIfScte30DataAddrType      InetAddressType,
    tmnxVdoIfScte30DataAddr          InetAddress,
    tmnxVdoIfSapId                   TmnxStrSapId,
    tmnxVdoIfMcastProtocol           INTEGER,
    tmnxVdoIfSessions                Unsigned32,
    tmnxVdoIfCpmProtectPolicyId      TCpmProtPolicyID,
    tmnxVdoIfRTMcastReply            TmnxEnabledDisabled,
    tmnxVdoIfRTCount                 Unsigned32,
    tmnxVdoIfRTInterval              Unsigned32,
    tmnxVdoIfRTHoldTime              Unsigned32,
    tmnxVdoIfAcctPolicyId            Unsigned32,
    tmnxVdoIfOutputFormat            TmnxVdoOutputFormat
}

tmnxVdoIfName                    OBJECT-TYPE
    SYNTAX      TmnxVdoIfName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfName specifies the unique administrative name
         for this video interface. The name must begin with a letter and is
         restricted to a maximum length of 29 characters during row creation
         using the 'tmnxVdoIfRowStatus' object. The remaining 3 characters are
         used internally by the agent to distinguish between user created video
         interfaces and agent created video interfaces. The agent created video
         interfaces have the same name as the user created video interfaces but
         are appended with a suffix of '-S' or '-S2'. These agent created video
         interfaces can be viewed using SNMP operations only in MIB tables that
         hold video interface statistical values namely -
         'tmnxVdoGrpSrcStatTable', 'tmnxVdoPIDTable', 'tmnxVdoGrpSrcVqmTable'
         and 'tmnxVdoGrpSrcVqmStatTable'."
    ::= { tmnxVdoIfEntry 1 }

tmnxVdoIfRowStatus               OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfRowStatus specifies the row status of this row.
         It is used for creation/deletion of this video interface."
    ::= { tmnxVdoIfEntry 2 }

tmnxVdoIfLastChanged             OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfLastChanged indicates the timestamp of last
         change to this row in tmnxVdoIfTable."
    ::= { tmnxVdoIfEntry 3 }

tmnxVdoIfAdminState              OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfAdminState specifies the desired administrative
         state of this video interface."
    DEFVAL      { outOfService }
    ::= { tmnxVdoIfEntry 4 }

tmnxVdoIfOperState               OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfOperState indicates the current operational
         status of this video interface."
    ::= { tmnxVdoIfEntry 5 }

tmnxVdoIfVrtrIfIndex             OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfVrtrIfIndex indicates the secondary index in the
         TIMETRA-VRTR-MIB::vRtrIfTable corresponding to this video interface.
         The value of svcId specifies the primary index in the
         TIMETRA-VRTR-MIB::vRtrIfTable."
    ::= { tmnxVdoIfEntry 6 }

tmnxVdoIfDescription             OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfDescription specifies the user provided
         description string for this video interface."
    DEFVAL      { ''H }
    ::= { tmnxVdoIfEntry 7 }

tmnxVdoIfVdoGrpId                OBJECT-TYPE
    SYNTAX      TmnxVdoGrpId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfVdoGrpId specifies the row index in the
         TIMETRA-VIDEO-MIB::tmnxVdoGrpTable for the video group information for
         this multicast information policy bundle.

         A value '0' indicates that no video-group is assigned to this video
         interface."
    DEFVAL      { 0 }
    ::= { tmnxVdoIfEntry 8 }

tmnxVdoIfIngressQosPolicyId      OBJECT-TYPE
    SYNTAX      TSapIngressPolicyID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfIngressQosPolicyId specifies the row index in
         the TIMETRA-QOS-MIB::tSapIngressTable corresponding to this ingress
         QoS policy. It has a value of '1' if no policy is specified.

         The value of this object can be set only when the value of
         tmnxVdoIfVdoGrpId has been set to a value other than '0'."
    DEFVAL      { 1 }
    ::= { tmnxVdoIfEntry 9 }

tmnxVdoIfEgressQosPolicyId       OBJECT-TYPE
    SYNTAX      TSapEgressPolicyID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfEgressQosPolicyId specifies the row index in the
         TIMETRA-QOS-MIB::tSapEgressTable corresponding to this egress QoS
         policy. It has a value of '1' if no policy is specified.

         The value of this object can be set only when the value of
         tmnxVdoIfVdoGrpId has been set to a value other than '0'."
    DEFVAL      { 1 }
    ::= { tmnxVdoIfEntry 10 }

tmnxVdoIfAdi                     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfAdi specifies whether Ad-Insertion (ADI) is
         enabled on this video interface.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { false }
    ::= { tmnxVdoIfEntry 11 }

tmnxVdoIfRTClientAddrType        OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfRTClientAddrType specifies the type of address
         represented by tmnxVdoIfRTClientAddr.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { unknown }
    ::= { tmnxVdoIfEntry 12 }

tmnxVdoIfRTClientAddr            OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfRTClientAddr specifies the IP address for the
         retransmission (RT) client in the video interface within the service.

         The RT client IP address is the originating address used for
         communication with upstream RT servers. If no RT client address is
         assigned, the RT client is operationally down as the RT client
         configuration is incomplete.

         For a VPLS service, the RT client address cannot be the same as an
         existing address for the video interface, but it must be an address
         within a video interface subnet. For IES and VPRN services, the RT
         client address can be the same as an existing address for the video
         interface or an address within a video interface subnet.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { ''H }
    ::= { tmnxVdoIfEntry 13 }

tmnxVdoIfGatewayAddrType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfGatewayAddrType specifies the type of address
         represented by tmnxVdoIfGatewayAddr.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { unknown }
    ::= { tmnxVdoIfEntry 14 }

tmnxVdoIfGatewayAddr             OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfGatewayAddr specifies the gateway IP address for
         the video Interface within the VPLS service.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { ''H }
    ::= { tmnxVdoIfEntry 15 }

tmnxVdoIfMcastSvcId              OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfMcastSvcId specifies the multicast service to be
         used for sending replies in the multicast service instance. In
         situations where multicast and unicast are carried in separate service
         instances, the value of this object should be set on the unicast video
         interface to form an association with the multicast service.

         The default value of this object is same as the value of corresponding
         TIMETRA-SERV-MIB::svcId."
    ::= { tmnxVdoIfEntry 16 }

tmnxVdoIfIngressIpFilterId       OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfIngressIpFilterId specifies the row index in
         the TIMETRA-FILTER-MIB::tIPFilterTable corresponding to this ingress
         filter. Filters control the forwarding and dropping of packets based
         on IP criteria.  A value of zero (0) indicates that there is no
         ip-filter-id associated with this interface.

         The value of this object can be set only when the value of
         tmnxVdoIfVdoGrpId has been set to a value other than '0'."
    DEFVAL      { 0 }
    ::= { tmnxVdoIfEntry 17 }

tmnxVdoIfIngressMacFilterId      OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfIngressMacFilterId specifies the row index in
         the TIMETRA-FILTER-MIB::tMacFilterTable corresponding to this ingress
         filter. Filters control the forwarding and dropping of packets based
         on IP criteria.  A value of zero (0) indicates that there is no
         mac-filter-id associated with this interface.

         The value of this object can be set only when the value of
         tmnxVdoIfVdoGrpId has been set to a value other than '0'."
    DEFVAL      { 0 }
    ::= { tmnxVdoIfEntry 18 }

tmnxVdoIfEgressIpFilterId        OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfEgressIpFilterId specifies the row index in
         the TIMETRA-FILTER-MIB::tIPFilterTable corresponding to this egress
         filter. Filters control the forwarding and dropping of packets based
         on IP criteria.  A value of zero (0) indicates that there is no
         ip-filter-id associated with this interface.

         The value of this object can be set only when the value of
         tmnxVdoIfVdoGrpId has been set to a value other than '0'."
    DEFVAL      { 0 }
    ::= { tmnxVdoIfEntry 19 }

tmnxVdoIfEgressMacFilterId       OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfEgressMacFilterId specifies the row index in
         the TIMETRA-FILTER-MIB::tMacFilterTable corresponding to this egress
         filter. Filters control the forwarding and dropping of packets based
         on IP criteria.  A value of zero (0) indicates that there is no
         mac-filter-id associated with this interface.

         The value of this object can be set only when the value of
         tmnxVdoIfVdoGrpId has been set to a value other than '0'."
    DEFVAL      { 0 }
    ::= { tmnxVdoIfEntry 20 }

tmnxVdoIfScte30ControlAddrType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfScte30ControlAddrType specifies the type of
         address represented by tmnxVdoIfScte30ControlAddr.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { unknown }
    ::= { tmnxVdoIfEntry 21 }

tmnxVdoIfScte30ControlAddr       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfScte30ControlAddr specifies the local IP address
         to which ad servers send Society of Cable Telecommunications Engineers
         30 (scte30) ad control streams. This address should be in the same
         subnet as the ip address assigned to the video interface.

         The values of tmnxVdoIfScte30ControlAddr and tmnxVdoIfScte30DataAddr,
         which specifies the local IP address to which ad servers send scte30
         ad data streams, must be set together in the same SNMP request PDU or
         else the set request will fail with an inconsistentValue error.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { ''H }
    ::= { tmnxVdoIfEntry 22 }

tmnxVdoIfScte30DataAddrType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfScte30DataAddrType specifies the type of address
         represented by tmnxVdoIfScte30DataAddr.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { unknown }
    ::= { tmnxVdoIfEntry 23 }

tmnxVdoIfScte30DataAddr          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfScte30DataAddr specifies the local IP address to
         which ad servers send Society of Cable Telecommunications Engineers 30
         (scte30) ad data streams. This address should be in the same subnet as
         the ip address assigned to the video interface.

         The values of tmnxVdoIfScte30DataAddr and tmnxVdoIfScte30ControlAddr,
         which specifies the local IP address to which ad servers send scte30
         ad control streams, must be set together in the same SNMP request PDU
         or else the set request will fail with an inconsistentValue error.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { ''H }
    ::= { tmnxVdoIfEntry 24 }

tmnxVdoIfSapId                   OBJECT-TYPE
    SYNTAX      TmnxStrSapId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfSapId indicates the control SAP for this video
         interface."
    ::= { tmnxVdoIfEntry 25 }

tmnxVdoIfMcastProtocol           OBJECT-TYPE
    SYNTAX      INTEGER {
        none         (1),
        pim          (2),
        igmpSnooping (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfMcastProtocol indicates the multicast routing
         protocol where this video interface is configured. For video control
         and data traffic to flow correctly to the video ISA, the video
         interface must be configured in the corresponding multicast routing
         protocol.

         In the VPLS case, the video sap is automatically added to
         IGMP-snooping and so the value of this object will be set to
         'igmpSnooping'."
    DEFVAL      { none }
    ::= { tmnxVdoIfEntry 26 }

tmnxVdoIfSessions                OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfSessions indicates the number of active sessions
         on this interface."
    ::= { tmnxVdoIfEntry 27 }

tmnxVdoIfCpmProtectPolicyId      OBJECT-TYPE
    SYNTAX      TCpmProtPolicyID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfCpmProtectPolicyId specifies the row index in
         the TIMETRA-SECURITY-MIB::tmnxCpmProtPolTable corresponding to the CPM
         Protection policy that would be applied to all RTCP control traffic
         destined to this video interface.

         If the value of this object is set to '0', then no CPM protection
         policy has been provisioned for this video interface and the DOS
         protection is disabled."
    DEFVAL      { 0 }
    ::= { tmnxVdoIfEntry 28 }

tmnxVdoIfRTMcastReply            OBJECT-TYPE
    SYNTAX      TmnxEnabledDisabled
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfRTMcastReply specifies whether or not the use of
         multicast retransmission packets is enabled by the Retransmission
         Server in response to a number of identical retransmission requests."
    DEFVAL      { disabled }
    ::= { tmnxVdoIfEntry 29 }

tmnxVdoIfRTCount                 OBJECT-TYPE
    SYNTAX      Unsigned32 (2..1024)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfRTCount specifies the integer number of
         identical retransmission requests received for a packet in a sampling
         interval after which a reply will be sent as multicast Payload Type
         33."
    DEFVAL      { 5 }
    ::= { tmnxVdoIfEntry 30 }

tmnxVdoIfRTInterval              OBJECT-TYPE
    SYNTAX      Unsigned32 (100..8000)
    UNITS       "milliseconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfRTInterval specifies the integer number of
         milliseconds for a sampling interval."
    DEFVAL      { 100 }
    ::= { tmnxVdoIfEntry 31 }

tmnxVdoIfRTHoldTime              OBJECT-TYPE
    SYNTAX      Unsigned32 (0..1000)
    UNITS       "milliseconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfRTHoldTime specifies the integer number of
         milliseconds after a multicast reply is sent that the Retransmission
         Server will wait before starting a new sampling period."
    DEFVAL      { 50 }
    ::= { tmnxVdoIfEntry 32 }

tmnxVdoIfAcctPolicyId            OBJECT-TYPE
    SYNTAX      Unsigned32 (0..99)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfAcctPolicyId specifies the accounting policy
         associated with the given video interface.  The value 0 specifies that
         no accounting policy is associated."
    DEFVAL      { 0 }
    ::= { tmnxVdoIfEntry 33 }

tmnxVdoIfOutputFormat            OBJECT-TYPE
    SYNTAX      TmnxVdoOutputFormat
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfOutputFormat specifies the output format of the
         associated video stream."
    DEFVAL      { rtp-udp }
    ::= { tmnxVdoIfEntry 34 }

tmnxVdoIfAddrTable               OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoIfAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxVdoIfAddrTable has an entry for each IP address configured for
         a video interface in the system. Each interface may have more than one
         IP address assigned to it."
    ::= { tmnxVdoObjs 2 }

tmnxVdoIfAddrEntry               OBJECT-TYPE
    SYNTAX      TmnxVdoIfAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an IP address assigned to a video interface.
         Entries can be created and deleted by the user."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoIfAddrIpAddrType,
        tmnxVdoIfAddrIpAddress,
        tmnxVdoIfAddrPrefixLen
    }
    ::= { tmnxVdoIfAddrTable 1 }

TmnxVdoIfAddrEntry               ::= SEQUENCE
{
    tmnxVdoIfAddrIpAddrType          InetAddressType,
    tmnxVdoIfAddrIpAddress           InetAddress,
    tmnxVdoIfAddrPrefixLen           InetAddressPrefixLength,
    tmnxVdoIfAddrRowStatus           RowStatus
}

tmnxVdoIfAddrIpAddrType          OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfAddrIpAddrType specifies the type of the
         tmnxVdoIfAddrIpAddress address assigned to the video interface."
    ::= { tmnxVdoIfAddrEntry 1 }

tmnxVdoIfAddrIpAddress           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfAddrIpAddress specifies the IP address of the
         video interface."
    ::= { tmnxVdoIfAddrEntry 2 }

tmnxVdoIfAddrPrefixLen           OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfAddrPrefixLen specifies the length of the IP
         netmask for this video interface address."
    ::= { tmnxVdoIfAddrEntry 3 }

tmnxVdoIfAddrRowStatus           OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfAddrRowStatus specifies the row status of this
         row. The row status is used for creation, deletion or control of
         tmnxVdoIfAddrTable entries."
    ::= { tmnxVdoIfAddrEntry 4 }

tmnxVdoGrpTable                  OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoGrpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxVdoGrpTable has an entry for each video group configured in the
         system.

         The table tmnxVdoGrpTable is used to create and remove Video ISA
         groups. A Video ISA group is used to configure properties relating to
         video interfaces and services."
    ::= { tmnxVdoObjs 3 }

tmnxVdoGrpEntry                  OBJECT-TYPE
    SYNTAX      TmnxVdoGrpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a video group in the system. Entries can be
         created and deleted by the user."
    INDEX       { tmnxVdoGrpId }
    ::= { tmnxVdoGrpTable 1 }

TmnxVdoGrpEntry                  ::= SEQUENCE
{
    tmnxVdoGrpId                     TmnxVdoGrpIdIndex,
    tmnxVdoGrpRowStatus              RowStatus,
    tmnxVdoGrpLastChanged            TimeStamp,
    tmnxVdoGrpAdminState             TmnxAdminState,
    tmnxVdoGrpOperState              TmnxOperState,
    tmnxVdoGrpDescription            TItemDescription,
    tmnxVdoGrpLocalRTServerState     TruthValue,
    tmnxVdoGrpFCCServerState         TruthValue,
    tmnxVdoGrpADIServerState         TruthValue,
    tmnxVdoGrpResvRet                Unsigned32,
    tmnxVdoGrpAnalyzerState          TruthValue,
    tmnxVdoGrpStreamSelectionState   TruthValue,
    tmnxVdoGrpEnableRtClient         TruthValue,
    tmnxVdoGrpWmBwFcc                TmnxWmPercent,
    tmnxVdoGrpWmBwRet                TmnxWmPercent,
    tmnxVdoGrpWmBwTotal              TmnxWmPercent,
    tmnxVdoGrpWmSesFcc               TmnxWmPercent,
    tmnxVdoGrpWmSesRet               TmnxWmPercent,
    tmnxVdoGrpWmSesTotal             TmnxWmPercent
}

tmnxVdoGrpId                     OBJECT-TYPE
    SYNTAX      TmnxVdoGrpIdIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpId specifies the identifier for this video
         group."
    ::= { tmnxVdoGrpEntry 1 }

tmnxVdoGrpRowStatus              OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpRowStatus specifies the row status of this row.
         It is used for creation/deletion of a video group."
    ::= { tmnxVdoGrpEntry 2 }

tmnxVdoGrpLastChanged            OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpLastChanged indicates the timestamp of the last
         change to this row in tmnxVdoGrpTable."
    ::= { tmnxVdoGrpEntry 3 }

tmnxVdoGrpAdminState             OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpAdminState specifies the desired administrative
         state of this video group."
    DEFVAL      { outOfService }
    ::= { tmnxVdoGrpEntry 4 }

tmnxVdoGrpOperState              OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpOperState indicates the current operational
         status of this video group."
    ::= { tmnxVdoGrpEntry 5 }

tmnxVdoGrpDescription            OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpDescription specifies the user provided
         description string for this video group."
    DEFVAL      { ''H }
    ::= { tmnxVdoGrpEntry 6 }

tmnxVdoGrpLocalRTServerState     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpLocalRTServerState specifies whether or not
         local Retransmission (RT) server is enabled on this video group."
    DEFVAL      { false }
    ::= { tmnxVdoGrpEntry 7 }

tmnxVdoGrpFCCServerState         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpFCCServerState specifies whether of not Fast
         Channel Change (FCC) server is enabled on this video group."
    DEFVAL      { false }
    ::= { tmnxVdoGrpEntry 8 }

tmnxVdoGrpADIServerState         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpADIServerState specifies whether or not Ad
         Insert (ADI) server is enabled on this video group.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { false }
    ::= { tmnxVdoGrpEntry 9 }

tmnxVdoGrpResvRet                OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "megabps"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpResvRet specifies to reserve egress bandwidth
         for Retransmission (RET) in all the ISAs within a video group. If the
         amount of egress bandwidth is less than the reserved amount, the Fast
         Channel Change (FCC) requests are discarded and only the
         Retransmission (RET) requests are processed."
    DEFVAL      { 0 }
    ::= { tmnxVdoGrpEntry 10 }

tmnxVdoGrpAnalyzerState          OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpAnalyzerState specifies whether or not the
         video analyzer is enabled for all streams on this video group."
    DEFVAL      { false }
    ::= { tmnxVdoGrpEntry 11 }

tmnxVdoGrpStreamSelectionState   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpStreamSelectionState specifies whether or not
         stream selection is enabled on this video group."
    DEFVAL      { false }
    ::= { tmnxVdoGrpEntry 12 }

tmnxVdoGrpEnableRtClient         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpEnableRtClient specifies whether the
         Retransmission (RET) capability for the client should be kept enabled
         or not.

         This object was obsoleted in the 23.0 release."
    DEFVAL      { true }
    ::= { tmnxVdoGrpEntry 13 }

tmnxVdoGrpWmBwFcc                OBJECT-TYPE
    SYNTAX      TmnxWmPercent
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpWmBwFcc specifies a limit at which an SNMP trap
         is sent per ISA. It is the percentage of total bandwidth for Fast
         Channel Change (FCC)."
    DEFVAL      { 90 }
    ::= { tmnxVdoGrpEntry 14 }

tmnxVdoGrpWmBwRet                OBJECT-TYPE
    SYNTAX      TmnxWmPercent
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpWmBwRet specifies a limit at which an SNMP trap
         is sent per ISA. It is the percentage of total bandwidth for
         Retransmission requests (RET)"
    DEFVAL      { 90 }
    ::= { tmnxVdoGrpEntry 15 }

tmnxVdoGrpWmBwTotal              OBJECT-TYPE
    SYNTAX      TmnxWmPercent
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpWmBwTotal specifies a limit at which an SNMP
         trap is sent per ISA. It is the percentage of total bandwidth."
    DEFVAL      { 90 }
    ::= { tmnxVdoGrpEntry 16 }

tmnxVdoGrpWmSesFcc               OBJECT-TYPE
    SYNTAX      TmnxWmPercent
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpWmSesFcc specifies a limit at which an SNMP
         trap is sent per ISA. It is the percentage of total number of session
         for Fast Channel Change (FCC)."
    DEFVAL      { 90 }
    ::= { tmnxVdoGrpEntry 17 }

tmnxVdoGrpWmSesRet               OBJECT-TYPE
    SYNTAX      TmnxWmPercent
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpWmSesRet specifies a limit at which an SNMP
         trap is sent per ISA. It is the percentage of total number of sessions
         for Retransmission requests (RET)."
    DEFVAL      { 90 }
    ::= { tmnxVdoGrpEntry 18 }

tmnxVdoGrpWmSesTotal             OBJECT-TYPE
    SYNTAX      TmnxWmPercent
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpWmSesTotal specifies a limit at which an SNMP
         trap is sent per ISA. It is the percentage of total number of
         sessions."
    DEFVAL      { 90 }
    ::= { tmnxVdoGrpEntry 19 }

tmnxVdoGrpMDATable               OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoGrpMDAEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxVdoGrpMDATable has an entry for each MDA configured for the
         Video ISP Group in the system. A specific MDA is configured for only a
         tmnxVdoGrpId."
    ::= { tmnxVdoObjs 4 }

tmnxVdoGrpMDAEntry               OBJECT-TYPE
    SYNTAX      TmnxVdoGrpMDAEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an MDA configured for a Video ISA Group in
         the system. Entries are created and deleted by the user."
    INDEX       {
        tmnxVdoGrpId,
        tmnxChassisIndex,
        tmnxCardSlotNum,
        tmnxMDASlotNum
    }
    ::= { tmnxVdoGrpMDATable 1 }

TmnxVdoGrpMDAEntry               ::= SEQUENCE
{
    tmnxVdoGrpMdaRowStatus           RowStatus,
    tmnxVdoGrpMdaAdminState          TmnxAdminState,
    tmnxVdoGrpMdaOperState           TmnxOperState,
    tmnxVdoGrpMdaUsedMemory          Gauge32,
    tmnxVdoGrpMdaAvailableMemory     Gauge32,
    tmnxVdoGrpMdaChannels            Gauge32,
    tmnxVdoGrpMdaChannelAllocFails   Counter32,
    tmnxVdoGrpMdaMaxBwExceeded       Counter32,
    tmnxVdoGrpMdaBwInUse             Gauge32,
    tmnxVdoGrpMdaActiveRtcpSessions  Gauge32,
    tmnxVdoGrpMdaEgressStreamResets  Counter32,
    tmnxVdoGrpMdaIngressStreamResets Counter32,
    tmnxVdoGrpMdaAdStreamResets      Counter32,
    tmnxVdoGrpMdaAdStreamAborts      Counter32,
    tmnxVdoGrpMdaSsrcCollisions      Counter32,
    tmnxVdoGrpMdaRxDataPackets       Counter64,
    tmnxVdoGrpMdaRxDataPacketsLow32  Counter32,
    tmnxVdoGrpMdaRxDataPacketsHigh32 Counter32,
    tmnxVdoGrpMdaRxDataOctets        Counter64,
    tmnxVdoGrpMdaRxDataOctetsLow32   Counter32,
    tmnxVdoGrpMdaRxDataOctetsHigh32  Counter32,
    tmnxVdoGrpMdaRxDataPacketErrors  Counter64,
    tmnxVdoGrpMdaRxDataPktErrsLow32  Counter32,
    tmnxVdoGrpMdaRxDataPktErrsHigh32 Counter32,
    tmnxVdoGrpMdaTxDataPackets       Counter64,
    tmnxVdoGrpMdaTxDataPacketsLow32  Counter32,
    tmnxVdoGrpMdaTxDataPacketsHigh32 Counter32,
    tmnxVdoGrpMdaTxDataOctets        Counter64,
    tmnxVdoGrpMdaTxDataOctetsLow32   Counter32,
    tmnxVdoGrpMdaTxDataOctetsHigh32  Counter32,
    tmnxVdoGrpMdaTxDataPacketErrors  Counter64,
    tmnxVdoGrpMdaTxDataPktErrsLow32  Counter32,
    tmnxVdoGrpMdaTxDataPktErrsHigh32 Counter32,
    tmnxVdoGrpMdaRtcpParseErrors     Counter32,
    tmnxVdoGrpMdaRtcpConfigErrors    Counter32,
    tmnxVdoGrpMdaRtcpIpcErrors       Counter32,
    tmnxVdoGrpMdaRtcpSgErrors        Counter32,
    tmnxVdoGrpMdaRtcpSubErrors       Counter32,
    tmnxVdoGrpMdaRtcpIntErrors       Counter32,
    tmnxVdoGrpMdaTxLostPackets       Counter32,
    tmnxVdoGrpMdaRequestedRtpPkts    Counter32,
    tmnxVdoGrpMdaHighPktPoolLimitHit Counter32,
    tmnxVdoGrpMdaMallocFailures      Counter32,
    tmnxVdoGrpMdaDentDroppedPkts     Counter32,
    tmnxVdoGrpMdaBwPeak              Gauge32,
    tmnxVdoGrpMdaCurTotalRetBw       Gauge32,
    tmnxVdoGrpMdaPeakRetBw           Gauge32,
    tmnxVdoGrpMdaCurFccBw            Gauge32,
    tmnxVdoGrpMdaFccDropCntReq       Gauge32,
    tmnxVdoGrpMdaMcRtcp              Counter64,
    tmnxVdoGrpMdaMcRtcpLow32         Counter32,
    tmnxVdoGrpMdaMcRtcpHigh32        Counter32,
    tmnxVdoGrpMdaMcRudp              Counter64,
    tmnxVdoGrpMdaMcRudpLow32         Counter32,
    tmnxVdoGrpMdaMcRudpHigh32        Counter32,
    tmnxVdoGrpMdaMcRetReqCrt         Counter64,
    tmnxVdoGrpMdaMcRetReqCrtLow32    Counter32,
    tmnxVdoGrpMdaMcRetReqCrtHigh32   Counter32,
    tmnxVdoGrpMdaRetReqQnc           Counter64,
    tmnxVdoGrpMdaRetReqQncLow32      Counter32,
    tmnxVdoGrpMdaRetReqQncHigh32     Counter32,
    tmnxVdoGrpMdaPktsLostInSeq10     Counter32,
    tmnxVdoGrpMdaPktsLostInSeq20     Counter32,
    tmnxVdoGrpMdaPktsLostInSeq30     Counter32,
    tmnxVdoGrpMdaPktsLostInSeq40     Counter32,
    tmnxVdoGrpMdaPktsLostInSeqMore   Counter32,
    tmnxVdoGrpMdaPeakFccBw           Gauge32,
    tmnxVdoGrpMdaPeakFccBwTime       TimeStamp,
    tmnxVdoGrpMdaPeakAbsRetBw        Gauge32,
    tmnxVdoGrpMdaPeakAbsRetBwTime    TimeStamp,
    tmnxVdoGrpMdaPeakFccSession      Gauge32,
    tmnxVdoGrpMdaPeakFccSessionTime  TimeStamp,
    tmnxVdoGrpMdaPeakRetSession      Gauge32,
    tmnxVdoGrpMdaPeakRetSessionTime  TimeStamp,
    tmnxVdoGrpMdaPeakFccRetTotBw     Gauge32,
    tmnxVdoGrpMdaPeakFccRetTotBwTime TimeStamp,
    tmnxVdoGrpMdaPeakFccRetTotSess   Gauge32,
    tmnxVdoGrpMdaPeakFccRetTotSeTime TimeStamp,
    tmnxVdoGrpMdaCurAbsRetBw         Gauge32,
    tmnxVdoGrpMdaCurFccRetTotalBw    Gauge32,
    tmnxVdoGrpMdaActFccSess          Gauge32,
    tmnxVdoGrpMdaActRetSess          Gauge32,
    tmnxVdoGrpMdaActFccRetTotalSess  Gauge32,
    tmnxVdoGrpMdaLhPkFccBw           Gauge32,
    tmnxVdoGrpMdaLhPkFccBwTime       TimeStamp,
    tmnxVdoGrpMdaLhPkAbsRetBw        Gauge32,
    tmnxVdoGrpMdaLhPkAbsRetBwTime    TimeStamp,
    tmnxVdoGrpMdaLhPkFccSession      Gauge32,
    tmnxVdoGrpMdaLhPkFccSessionTime  TimeStamp,
    tmnxVdoGrpMdaLhPkRetSession      Gauge32,
    tmnxVdoGrpMdaLhPkRetSessionTime  TimeStamp,
    tmnxVdoGrpMdaLhPkFccRetTotBw     Gauge32,
    tmnxVdoGrpMdaLPFccRetTotBwTime   TimeStamp,
    tmnxVdoGrpMdaLhPkFccRetTotSess   Gauge32,
    tmnxVdoGrpMdaLPFccRetTotSeTime   TimeStamp,
    tmnxVdoGrpMdaChPkFccBw           Gauge32,
    tmnxVdoGrpMdaChPkFccBwTime       TimeStamp,
    tmnxVdoGrpMdaChPkAbsRetBw        Gauge32,
    tmnxVdoGrpMdaChPkAbsRetBwTime    TimeStamp,
    tmnxVdoGrpMdaChPkFccSession      Gauge32,
    tmnxVdoGrpMdaChPkFccSessionTime  TimeStamp,
    tmnxVdoGrpMdaChPkRetSession      Gauge32,
    tmnxVdoGrpMdaChPkRetSessionTime  TimeStamp,
    tmnxVdoGrpMdaChPkFccRetTotBw     Gauge32,
    tmnxVdoGrpMdaCPFccRetTotBwTime   TimeStamp,
    tmnxVdoGrpMdaChPkFccRetTotSess   Gauge32,
    tmnxVdoGrpMdaCPFccRetTotSeTime   TimeStamp
}

tmnxVdoGrpMdaRowStatus           OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRowStatus specifies the row status of this
         row entry. It is used for the association or removal of an MDA in the
         Video ISA Group."
    ::= { tmnxVdoGrpMDAEntry 1 }

tmnxVdoGrpMdaAdminState          OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaAdminState indicates the administrative
         state of the video group on this MDA."
    ::= { tmnxVdoGrpMDAEntry 2 }

tmnxVdoGrpMdaOperState           OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaOperState indicates the current operational
         state of the video group on this MDA."
    ::= { tmnxVdoGrpMDAEntry 3 }

tmnxVdoGrpMdaUsedMemory          OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaUsedMemory indicates the amount of cache
         being used by the video group for storing the video stream."
    ::= { tmnxVdoGrpMDAEntry 4 }

tmnxVdoGrpMdaAvailableMemory     OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaAvailableMemory indicates the amount of
         cache available on the MDA for storing the video stream."
    ::= { tmnxVdoGrpMDAEntry 5 }

tmnxVdoGrpMdaChannels            OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChannels indicates the number of channels
         being served on this MDA."
    ::= { tmnxVdoGrpMDAEntry 6 }

tmnxVdoGrpMdaChannelAllocFails   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChannelAllocFails indicates the number of
         failed channel allocations on this MDA."
    ::= { tmnxVdoGrpMDAEntry 7 }

tmnxVdoGrpMdaMaxBwExceeded       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMaxBwExceeded indicates the number of times
         maximum allowed bandwidth has been exceeded for each egress stream."
    ::= { tmnxVdoGrpMDAEntry 8 }

tmnxVdoGrpMdaBwInUse             OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaBwInUse indicates the total aggregate
         bandwidth of the currently running egress streams."
    ::= { tmnxVdoGrpMDAEntry 9 }

tmnxVdoGrpMdaActiveRtcpSessions  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaActiveRtcpSessions indicates the number of
         active Real Time Transport Control Protocol (RTCP) sessions on this
         MDA."
    ::= { tmnxVdoGrpMDAEntry 10 }

tmnxVdoGrpMdaEgressStreamResets  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaEgressStreamResets indicates the number of
         egress stream resets on this MDA. An egress stream reset occurs when
         there are no packets to transmit on the MDA."
    ::= { tmnxVdoGrpMDAEntry 11 }

tmnxVdoGrpMdaIngressStreamResets OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaIngressStreamResets indicates the number of
         ingress stream resets on this MDA. An ingress stream reset occurs when
         the ingress stream stopped coming in for more than one second."
    ::= { tmnxVdoGrpMDAEntry 12 }

tmnxVdoGrpMdaAdStreamResets      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpMdaAdStreamResets indicates the number of ad
         stream resets on this MDA. An ad stream reset occurs when the ingress
         ad stream stops.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpMDAEntry 13 }

tmnxVdoGrpMdaAdStreamAborts      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpMdaAdStreamAborts indicates the number of ad
         stream aborts on this MDA. An ad stream abort could happen when an
         egress reset happens.
         +
         +                             This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpMDAEntry 14 }

tmnxVdoGrpMdaSsrcCollisions      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaSsrcCollisions indicates the number of
         synchronization source (SSRC) id collisions on this MDA."
    ::= { tmnxVdoGrpMDAEntry 15 }

tmnxVdoGrpMdaRxDataPackets       OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRxDataPackets indicates the number of data
         packets received on this MDA."
    ::= { tmnxVdoGrpMDAEntry 16 }

tmnxVdoGrpMdaRxDataPacketsLow32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRxDataPacketsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpMdaRxDataPackets."
    ::= { tmnxVdoGrpMDAEntry 17 }

tmnxVdoGrpMdaRxDataPacketsHigh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRxDataPacketsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpMdaRxDataPackets."
    ::= { tmnxVdoGrpMDAEntry 18 }

tmnxVdoGrpMdaRxDataOctets        OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRxDataOctets indicates the number of data
         octets received on this MDA."
    ::= { tmnxVdoGrpMDAEntry 19 }

tmnxVdoGrpMdaRxDataOctetsLow32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRxDataOctetsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpMdaRxDataOctets."
    ::= { tmnxVdoGrpMDAEntry 20 }

tmnxVdoGrpMdaRxDataOctetsHigh32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRxDataOctetsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpMdaRxDataOctets."
    ::= { tmnxVdoGrpMDAEntry 21 }

tmnxVdoGrpMdaRxDataPacketErrors  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRxDataPacketErrors indicates the number of
         malformed or non-RTP (Real Time Transport Protocol) packets received
         on this MDA."
    ::= { tmnxVdoGrpMDAEntry 22 }

tmnxVdoGrpMdaRxDataPktErrsLow32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRxDataPktErrsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpMdaRxDataPacketErrors."
    ::= { tmnxVdoGrpMDAEntry 23 }

tmnxVdoGrpMdaRxDataPktErrsHigh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRxDataPktErrsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpMdaRxDataPacketErrors."
    ::= { tmnxVdoGrpMDAEntry 24 }

tmnxVdoGrpMdaTxDataPackets       OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaTxDataPackets indicates the number of data
         packets transmitted on this MDA."
    ::= { tmnxVdoGrpMDAEntry 25 }

tmnxVdoGrpMdaTxDataPacketsLow32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaTxDataPacketsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpMdaTxDataPackets."
    ::= { tmnxVdoGrpMDAEntry 26 }

tmnxVdoGrpMdaTxDataPacketsHigh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaTxDataPacketsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpMdaTxDataPackets."
    ::= { tmnxVdoGrpMDAEntry 27 }

tmnxVdoGrpMdaTxDataOctets        OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaTxDataOctets indicates the number of data
         octets transmitted on this MDA."
    ::= { tmnxVdoGrpMDAEntry 28 }

tmnxVdoGrpMdaTxDataOctetsLow32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaTxDataOctetsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpMdaTxDataOctets."
    ::= { tmnxVdoGrpMDAEntry 29 }

tmnxVdoGrpMdaTxDataOctetsHigh32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaTxDataOctetsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpMdaTxDataOctets."
    ::= { tmnxVdoGrpMDAEntry 30 }

tmnxVdoGrpMdaTxDataPacketErrors  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaTxDataPacketErrors indicates the number of
         failed data packets due to lack of resources to be transmitted on this
         MDA."
    ::= { tmnxVdoGrpMDAEntry 31 }

tmnxVdoGrpMdaTxDataPktErrsLow32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaTxDataPktErrsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpMdaTxDataPacketErrors."
    ::= { tmnxVdoGrpMDAEntry 32 }

tmnxVdoGrpMdaTxDataPktErrsHigh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaTxDataPktErrsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpMdaTxDataPacketErrors."
    ::= { tmnxVdoGrpMDAEntry 33 }

tmnxVdoGrpMdaRtcpParseErrors     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRtcpParseErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) packet parsing errors on
         this MDA."
    ::= { tmnxVdoGrpMDAEntry 34 }

tmnxVdoGrpMdaRtcpConfigErrors    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRtcpConfigErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) config errors on this MDA.
         These errors occur when there is inconsistency between the RTCP values
         and the configured values."
    ::= { tmnxVdoGrpMDAEntry 35 }

tmnxVdoGrpMdaRtcpIpcErrors       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRtcpIpcErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) inter-process
         communication message processing errors on this MDA."
    ::= { tmnxVdoGrpMDAEntry 36 }

tmnxVdoGrpMdaRtcpSgErrors        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRtcpSgErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) channel errors on this
         MDA. These errors occur when a channel is not found for a given
         interface to process RTCP packets."
    ::= { tmnxVdoGrpMDAEntry 37 }

tmnxVdoGrpMdaRtcpSubErrors       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRtcpSubErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) subscriber parameter
         errors on this MDA. These errors occur when the subscriber
         calculations exceed the maximum allowed bandwidth."
    ::= { tmnxVdoGrpMDAEntry 38 }

tmnxVdoGrpMdaRtcpIntErrors       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRtcpIntErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) interface related errors
         on this MDA."
    ::= { tmnxVdoGrpMDAEntry 39 }

tmnxVdoGrpMdaTxLostPackets       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaTxLostPackets indicates the number of
         packets not found in the video MDA buffer for retransmission. When a
         retransmission request arrives, packets are checked in the buffer and
         if they are not found, the value of this object is incremented."
    ::= { tmnxVdoGrpMDAEntry 40 }

tmnxVdoGrpMdaRequestedRtpPkts    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRequestedRtpPkts indicates the number of
         Real-time Transport Protocol (RTP) packets requested in the Real-time
         Transport Control Protocol (RTCP) feedback (FB) messages received on
         this MDA."
    ::= { tmnxVdoGrpMDAEntry 41 }

tmnxVdoGrpMdaHighPktPoolLimitHit OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaHighPktPoolLimitHit indicates the number of
         times the high packet pool limit has been hit. A high value of this
         object indicates potential failure in ingress packet storage."
    ::= { tmnxVdoGrpMDAEntry 42 }

tmnxVdoGrpMdaMallocFailures      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMallocFailures indicates the number of
         memory allocation failures on the management core of the video MDA."
    ::= { tmnxVdoGrpMDAEntry 43 }

tmnxVdoGrpMdaDentDroppedPkts     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaDentDroppedPkts indicates the number of
         packets dropped by the video MDA due to denting."
    ::= { tmnxVdoGrpMDAEntry 44 }

tmnxVdoGrpMdaBwPeak              OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaBwPeak indicates the maximum bandwidth of
         the currently running egress streams since the last clear event."
    ::= { tmnxVdoGrpMDAEntry 45 }

tmnxVdoGrpMdaCurTotalRetBw       OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaCurTotalRetBw indicates the current total
         Retransmission (RET) bandwidth in use."
    ::= { tmnxVdoGrpMDAEntry 46 }

tmnxVdoGrpMdaPeakRetBw           OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakRetBw indicates the maximum
         Retransmission (RET) bandwidth used since the last clear event."
    ::= { tmnxVdoGrpMDAEntry 47 }

tmnxVdoGrpMdaCurFccBw            OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaCurFccBw indicates the current Fast Channel
         Change (FCC) bandwidth in use."
    ::= { tmnxVdoGrpMDAEntry 48 }

tmnxVdoGrpMdaFccDropCntReq       OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaFccDropCntReq indicates the drop count for
         the Fast Channel Change (FCC) requests due to reserved Retransmission
         (RET) bandwidth."
    ::= { tmnxVdoGrpMDAEntry 49 }

tmnxVdoGrpMdaMcRtcp              OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMcRtcp indicates the number of multicast
         retransmissions done in response to Real Time Transport Control
         Protocol (RTCP) requests."
    ::= { tmnxVdoGrpMDAEntry 50 }

tmnxVdoGrpMdaMcRtcpLow32         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMcRtcpLow32 indicates the lower 32 bits of
         the value of tmnxVdoGrpMdaMcRtcp."
    ::= { tmnxVdoGrpMDAEntry 51 }

tmnxVdoGrpMdaMcRtcpHigh32        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMcRtcpHigh32 indicates the higher 32 bits of
         the value of tmnxVdoGrpMdaMcRtcp."
    ::= { tmnxVdoGrpMDAEntry 52 }

tmnxVdoGrpMdaMcRudp              OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMcRudp indicates the number of multicast
         retransmissions done in response to Reliable User Datagram Protocol
         (RUDP) requests."
    ::= { tmnxVdoGrpMDAEntry 53 }

tmnxVdoGrpMdaMcRudpLow32         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMcRudpLow32 indicates the lower 32 bits of
         the value of tmnxVdoGrpMdaMcRudp."
    ::= { tmnxVdoGrpMDAEntry 54 }

tmnxVdoGrpMdaMcRudpHigh32        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMcRudpHigh32 indicates the higher 32 bits of
         the value of tmnxVdoGrpMdaMcRudp."
    ::= { tmnxVdoGrpMDAEntry 55 }

tmnxVdoGrpMdaMcRetReqCrt         OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMcRetReqCrt indicates the total number of
         mcast retransmission requests created in response to the unicast
         retransmission requests."
    ::= { tmnxVdoGrpMDAEntry 56 }

tmnxVdoGrpMdaMcRetReqCrtLow32    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMcRetReqCrtLow32 indicates the lower 32 bits
         of the value of tmnxVdoGrpMdaMcRetReqCrt."
    ::= { tmnxVdoGrpMDAEntry 57 }

tmnxVdoGrpMdaMcRetReqCrtHigh32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaMcRetReqCrtHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpMdaMcRetReqCrt."
    ::= { tmnxVdoGrpMDAEntry 58 }

tmnxVdoGrpMdaRetReqQnc           OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRetReqQnc indicates the total number of
         unicast retransmission requests quenched with the multicast
         retransmission."
    ::= { tmnxVdoGrpMDAEntry 59 }

tmnxVdoGrpMdaRetReqQncLow32      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRetReqQncLow32 indicates the lower 32 bits
         of the value of tmnxVdoGrpMdaRetReqQnc."
    ::= { tmnxVdoGrpMDAEntry 60 }

tmnxVdoGrpMdaRetReqQncHigh32     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaRetReqQncHigh32 indicates the higher 32 bits
         of the value of tmnxVdoGrpMdaRetReqQnc."
    ::= { tmnxVdoGrpMDAEntry 61 }

tmnxVdoGrpMdaPktsLostInSeq10     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPktsLostInSeq10 indicates the total number
         of packets within sequences of 2 to 10 consecutive lost packets of the
         video group on this MDA."
    ::= { tmnxVdoGrpMDAEntry 62 }

tmnxVdoGrpMdaPktsLostInSeq20     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPktsLostInSeq20 indicates the total number
         of packets within sequences of 11 to 20 consecutive lost packets of
         the video group on this MDA."
    ::= { tmnxVdoGrpMDAEntry 63 }

tmnxVdoGrpMdaPktsLostInSeq30     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPktsLostInSeq30 indicates the total number
         of packets within sequences of 21 to 30 consecutive lost packets of
         the video group on this MDA."
    ::= { tmnxVdoGrpMDAEntry 64 }

tmnxVdoGrpMdaPktsLostInSeq40     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPktsLostInSeq40 indicates the total number
         of packets within sequences of 31 to 40 consecutive lost packets of
         the video group on this MDA."
    ::= { tmnxVdoGrpMDAEntry 65 }

tmnxVdoGrpMdaPktsLostInSeqMore   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPktsLostInSeqMore indicates the total number
         of packets within sequences of 41 or more consecutive lost packets of
         the video group on this MDA."
    ::= { tmnxVdoGrpMDAEntry 66 }

tmnxVdoGrpMdaPeakFccBw           OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakFccBw indicates the peak value of
         bandwidth for Fast Channel Change (FCC) requests since the last
         reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 67 }

tmnxVdoGrpMdaPeakFccBwTime       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakFccBwTime indicates the time (timestamp)
         when tmnxVdoGrpMdaPeakFccBw occurred since the last reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 68 }

tmnxVdoGrpMdaPeakAbsRetBw        OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakAbsRetBw indicates the absolute peak
         value of bandwidth for Retransmission requests (RET) since the last
         reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 69 }

tmnxVdoGrpMdaPeakAbsRetBwTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakAbsRetBwTime indicates the time
         (timestamp) when tmnxVdoGrpMdaPeakAbsRetBw occurred since the last
         reboot/clear.."
    ::= { tmnxVdoGrpMDAEntry 70 }

tmnxVdoGrpMdaPeakFccSession      OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakFccSession indicates the peak number of
         Fast Channel Change (FCC) sessions since the last reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 71 }

tmnxVdoGrpMdaPeakFccSessionTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakFccSessionTime indicates the time
         (timestamp) when tmnxVdoGrpMdaPeakFccSession occurred since the last
         reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 72 }

tmnxVdoGrpMdaPeakRetSession      OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakRetSession indicates the peak number of
         Retransmission (RET) sessions since the last reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 73 }

tmnxVdoGrpMdaPeakRetSessionTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakRetSessionTime indicates the time
         (timestamp) when tmnxVdoGrpMdaPeakRetSession occurred since the last
         reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 74 }

tmnxVdoGrpMdaPeakFccRetTotBw     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakFccRetTotBw indicates the total peak
         value of bandwidth for Channel Change (FCC) and Retransmission (RET)
         requests since the last reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 75 }

tmnxVdoGrpMdaPeakFccRetTotBwTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakFccRetTotBwTime indicates the time
         (timestamp) when tmnxVdoGrpMdaPeakFccRetTotBw occurred since the last
         reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 76 }

tmnxVdoGrpMdaPeakFccRetTotSess   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakFccRetTotSess indicates the total peak
         number of sessions for Fast Channel Change (FCC) and Retransmission
         (RET) since the last reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 77 }

tmnxVdoGrpMdaPeakFccRetTotSeTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaPeakFccRetTotSeTime indicates the time
         (timestamp) when tmnxVdoGrpMdaPeakFccRetTotSess occurred since the
         last reboot/clear."
    ::= { tmnxVdoGrpMDAEntry 78 }

tmnxVdoGrpMdaCurAbsRetBw         OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaCurAbsRetBw indicates the current
         Retransmission (RET) bandwidth in use."
    ::= { tmnxVdoGrpMDAEntry 79 }

tmnxVdoGrpMdaCurFccRetTotalBw    OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaCurFccRetTotalBw indicates the current total
         Fast Channel Change (FCC) and  Retransmission (RET) bandwidth in use."
    ::= { tmnxVdoGrpMDAEntry 80 }

tmnxVdoGrpMdaActFccSess          OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaActFccSess indicates the number of active
         Real Time Transport Control Protocol (RTCP) sessions allocated for
         Fast Channel Change (FCC) on this MDA."
    ::= { tmnxVdoGrpMDAEntry 81 }

tmnxVdoGrpMdaActRetSess          OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaActRetSess indicates the number of active
         Real Time Transport Control Protocol (RTCP) sessions allocated for
         Retransmission (RET) on this MDA."
    ::= { tmnxVdoGrpMDAEntry 82 }

tmnxVdoGrpMdaActFccRetTotalSess  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaActFccRetTotalSess indicates the number of
         active Real Time Transport Control Protocol (RTCP) sessions allocated
         for Fast Channel Change (FCC) and Retransmission (RET) on this MDA."
    ::= { tmnxVdoGrpMDAEntry 83 }

tmnxVdoGrpMdaLhPkFccBw           OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLhPkFccBw indicates the peak value of
         bandwidth for Fast Channel Change (FCC) requests in the last hour."
    ::= { tmnxVdoGrpMDAEntry 84 }

tmnxVdoGrpMdaLhPkFccBwTime       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLhPkFccBwTime indicates the time (timestamp)
         when tmnxVdoGrpMdaLhPkFccBw occurred in the last hour."
    ::= { tmnxVdoGrpMDAEntry 85 }

tmnxVdoGrpMdaLhPkAbsRetBw        OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLhPkAbsRetBw indicates the absolute peak
         value of bandwidth for Retransmission requests (RET) in the last hour."
    ::= { tmnxVdoGrpMDAEntry 86 }

tmnxVdoGrpMdaLhPkAbsRetBwTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLhPkAbsRetBwTime indicates the time
         (timestamp) when tmnxVdoGrpMdaLhPkAbsRetBw occurred in the last hour.."
    ::= { tmnxVdoGrpMDAEntry 87 }

tmnxVdoGrpMdaLhPkFccSession      OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLhPkFccSession indicates the peak number of
         Fast Channel Change (FCC) sessions in the last hour."
    ::= { tmnxVdoGrpMDAEntry 88 }

tmnxVdoGrpMdaLhPkFccSessionTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLhPkFccSessionTime indicates the time
         (timestamp) when tmnxVdoGrpMdaLhPkFccSession occurred in the last
         hour."
    ::= { tmnxVdoGrpMDAEntry 89 }

tmnxVdoGrpMdaLhPkRetSession      OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLhPkRetSession indicates the peak number of
         Retransmission (RET) sessions in the last hour."
    ::= { tmnxVdoGrpMDAEntry 90 }

tmnxVdoGrpMdaLhPkRetSessionTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLhPkRetSessionTime indicates the time
         (timestamp) when tmnxVdoGrpMdaLhPkRetSession occurred in the last
         hour."
    ::= { tmnxVdoGrpMDAEntry 91 }

tmnxVdoGrpMdaLhPkFccRetTotBw     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLhPkFccRetTotBw indicates the total peak
         value of bandwidth for Channel Change (FCC) and Retransmission (RET)
         requests in the last hour."
    ::= { tmnxVdoGrpMDAEntry 92 }

tmnxVdoGrpMdaLPFccRetTotBwTime   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLPFccRetTotBwTime indicates the time
         (timestamp) when tmnxVdoGrpMdaLhPkFccRetTotBw occurred in the last
         hour."
    ::= { tmnxVdoGrpMDAEntry 93 }

tmnxVdoGrpMdaLhPkFccRetTotSess   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLhPkFccRetTotSess indicates the total peak
         number of sessions for Fast Channel Change (FCC) and Retransmission
         (RET) in the last hour."
    ::= { tmnxVdoGrpMDAEntry 94 }

tmnxVdoGrpMdaLPFccRetTotSeTime   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaLPFccRetTotSeTime indicates the time
         (timestamp) when tmnxVdoGrpMdaLhPkFccRetTotSess occurred in the last
         hour."
    ::= { tmnxVdoGrpMDAEntry 95 }

tmnxVdoGrpMdaChPkFccBw           OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChPkFccBw indicates the peak value of
         bandwidth for Fast Channel Change (FCC) requests in the current hour."
    ::= { tmnxVdoGrpMDAEntry 96 }

tmnxVdoGrpMdaChPkFccBwTime       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChPkFccBwTime indicates the time (timestamp)
         when tmnxVdoGrpMdaChPkFccBw occurred in the current hour."
    ::= { tmnxVdoGrpMDAEntry 97 }

tmnxVdoGrpMdaChPkAbsRetBw        OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChPkAbsRetBw indicates the absolute peak
         value of bandwidth for Retransmission requests (RET) in the current
         hour."
    ::= { tmnxVdoGrpMDAEntry 98 }

tmnxVdoGrpMdaChPkAbsRetBwTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChPkAbsRetBwTime indicates the time
         (timestamp) when tmnxVdoGrpMdaChPkAbsRetBw occurred in the current
         hour."
    ::= { tmnxVdoGrpMDAEntry 99 }

tmnxVdoGrpMdaChPkFccSession      OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChPkFccSession indicates the peak number of
         Fast Channel Change (FCC) sessions in the current hour."
    ::= { tmnxVdoGrpMDAEntry 100 }

tmnxVdoGrpMdaChPkFccSessionTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChPkFccSessionTime indicates the time
         (timestamp) when tmnxVdoGrpMdaChPkFccSession occurred in the current
         hour."
    ::= { tmnxVdoGrpMDAEntry 101 }

tmnxVdoGrpMdaChPkRetSession      OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChPkRetSession indicates the peak number of
         Retransmission (RET) sessions in the current hour."
    ::= { tmnxVdoGrpMDAEntry 102 }

tmnxVdoGrpMdaChPkRetSessionTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChPkRetSessionTime indicates the time
         (timestamp) when tmnxVdoGrpMdaChPkRetSession occurred in the current
         hour."
    ::= { tmnxVdoGrpMDAEntry 103 }

tmnxVdoGrpMdaChPkFccRetTotBw     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChPkFccRetTotBw indicates the total peak
         value of bandwidth for Channel Change (FCC) and Retransmission (RET)
         requests in the current hour."
    ::= { tmnxVdoGrpMDAEntry 104 }

tmnxVdoGrpMdaCPFccRetTotBwTime   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaCPFccRetTotBwTime indicates the time
         (timestamp) when tmnxVdoGrpMdaChPkFccRetTotBw occurred in the current
         hour."
    ::= { tmnxVdoGrpMDAEntry 105 }

tmnxVdoGrpMdaChPkFccRetTotSess   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaChPkFccRetTotSess indicates the total peak
         number of sessions for Fast Channel Change (FCC) and Retransmission
         (RET) in the current hour."
    ::= { tmnxVdoGrpMDAEntry 106 }

tmnxVdoGrpMdaCPFccRetTotSeTime   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMdaCPFccRetTotSeTime indicates the time
         (timestamp) when tmnxVdoGrpMdaChPkFccRetTotSess occurred in the
         current hour."
    ::= { tmnxVdoGrpMDAEntry 107 }

tmnxVdoAdiChlTable               OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoAdiChlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxVdoAdiChlTable has an entry for each channel configured for
         the ADI (Ad Insertion) in the system. It lists the IP multicast groups
         and corresponding IP multicast sources."
    ::= { tmnxVdoObjs 5 }

tmnxVdoAdiChlEntry               OBJECT-TYPE
    SYNTAX      TmnxVdoAdiChlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a source address from which receivers are
         interested or not interested in receiving multicast traffic."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoAdiChlGrpAddrType,
        tmnxVdoAdiChlGrpAddress,
        tmnxVdoAdiChlSrcAddrType,
        tmnxVdoAdiChlSrcAddress
    }
    ::= { tmnxVdoAdiChlTable 1 }

TmnxVdoAdiChlEntry               ::= SEQUENCE
{
    tmnxVdoAdiChlGrpAddrType         InetAddressType,
    tmnxVdoAdiChlGrpAddress          InetAddress,
    tmnxVdoAdiChlSrcAddrType         InetAddressType,
    tmnxVdoAdiChlSrcAddress          InetAddress,
    tmnxVdoAdiChlRowStatus           RowStatus,
    tmnxVdoAdiChlName                TNamedItem,
    tmnxVdoAdiChlDescription         TItemDescription,
    tmnxVdoAdiChlForwardScte35       TruthValue
}

tmnxVdoAdiChlGrpAddrType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiChlGrpAddrType indicates the type of address to
         be used for IP multicast group address."
    ::= { tmnxVdoAdiChlEntry 1 }

tmnxVdoAdiChlGrpAddress          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiChlGrpAddress indicates the IP multicast group
         address for which this entry contains information."
    ::= { tmnxVdoAdiChlEntry 2 }

tmnxVdoAdiChlSrcAddrType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiChlSrcAddrType indicates the type of address to
         be used for source address."
    ::= { tmnxVdoAdiChlEntry 3 }

tmnxVdoAdiChlSrcAddress          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiChlSrcAddress indicates the source address for
         which this entry contains information."
    ::= { tmnxVdoAdiChlEntry 4 }

tmnxVdoAdiChlRowStatus           OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiChlRowStatus specifies the row status of this
         row entry."
    ::= { tmnxVdoAdiChlEntry 5 }

tmnxVdoAdiChlName                OBJECT-TYPE
    SYNTAX      TNamedItem (SIZE (1..30))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiChlName specifies the name for this channel."
    ::= { tmnxVdoAdiChlEntry 6 }

tmnxVdoAdiChlDescription         OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiChlDescription specifies the user provided
         description string for this channel."
    DEFVAL      { ''H }
    ::= { tmnxVdoAdiChlEntry 7 }

tmnxVdoAdiChlForwardScte35       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiChlForwardScte35 specifies whether the Society
         of Cable Telecommunications Engineers 35 (scte35) cue avails in the
         stream need to be forwarded or not. If the value of this object is set
         to 'true', then scte35 messages will be forwarded in the downstream."
    DEFVAL      { true }
    ::= { tmnxVdoAdiChlEntry 8 }

tmnxVdoAdiZoneChlTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoAdiZoneChlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxVdoAdiZoneChlTable has an entry for each zone channel
         configured for the ADI (Ad Insertion) in the system. It lists the IP
         multicast groups and corresponding IP multicast sources."
    ::= { tmnxVdoObjs 6 }

tmnxVdoAdiZoneChlEntry           OBJECT-TYPE
    SYNTAX      TmnxVdoAdiZoneChlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a source address from which receivers are
         interested or not interested in receiving multicast traffic."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoAdiChlGrpAddrType,
        tmnxVdoAdiChlGrpAddress,
        tmnxVdoAdiChlSrcAddrType,
        tmnxVdoAdiChlSrcAddress,
        tmnxVdoAdiZoneChlGrpAddrType,
        tmnxVdoAdiZoneChlGrpAddress,
        tmnxVdoAdiZoneChlSrcAddrType,
        tmnxVdoAdiZoneChlSrcAddress
    }
    ::= { tmnxVdoAdiZoneChlTable 1 }

TmnxVdoAdiZoneChlEntry           ::= SEQUENCE
{
    tmnxVdoAdiZoneChlGrpAddrType     InetAddressType,
    tmnxVdoAdiZoneChlGrpAddress      InetAddress,
    tmnxVdoAdiZoneChlSrcAddrType     InetAddressType,
    tmnxVdoAdiZoneChlSrcAddress      InetAddress,
    tmnxVdoAdiZoneChlRowStatus       RowStatus,
    tmnxVdoAdiZoneChlName            TNamedItem
}

tmnxVdoAdiZoneChlGrpAddrType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiZoneChlGrpAddrType indicates the type of
         address to be used for IP multicast group address."
    ::= { tmnxVdoAdiZoneChlEntry 1 }

tmnxVdoAdiZoneChlGrpAddress      OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiZoneChlGrpAddress indicates the IP multicast
         group address for which this entry contains information."
    ::= { tmnxVdoAdiZoneChlEntry 2 }

tmnxVdoAdiZoneChlSrcAddrType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiZoneChlSrcAddrType indicates the type of
         address to be used for source address."
    ::= { tmnxVdoAdiZoneChlEntry 3 }

tmnxVdoAdiZoneChlSrcAddress      OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiZoneChlSrcAddress indicates the source address
         for which this entry contains information."
    ::= { tmnxVdoAdiZoneChlEntry 4 }

tmnxVdoAdiZoneChlRowStatus       OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiZoneChlRowStatus specifies the row status of
         this row entry."
    ::= { tmnxVdoAdiZoneChlEntry 5 }

tmnxVdoAdiZoneChlName            OBJECT-TYPE
    SYNTAX      TNamedItem (SIZE (1..30))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiZoneChlName specifies the name for this zone
         channel."
    ::= { tmnxVdoAdiZoneChlEntry 6 }

tmnxVdoGrpSrcStatTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoGrpSrcStatEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxVdoGrpSrcStatTable contains channel information and statistics for
         the multicast groups."
    ::= { tmnxVdoObjs 7 }

tmnxVdoGrpSrcStatEntry           OBJECT-TYPE
    SYNTAX      TmnxVdoGrpSrcStatEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoGrpSrcStatTable. Each entry represents a source
         address for the corresponding multicast group."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoGrpSrcGrpAddrType,
        tmnxVdoGrpSrcGroupAddress,
        tmnxVdoGrpSrcSrcAddrType,
        tmnxVdoGrpSrcSourceAddress
    }
    ::= { tmnxVdoGrpSrcStatTable 1 }

TmnxVdoGrpSrcStatEntry           ::= SEQUENCE
{
    tmnxVdoGrpSrcGrpAddrType         InetAddressType,
    tmnxVdoGrpSrcGroupAddress        InetAddress,
    tmnxVdoGrpSrcSrcAddrType         InetAddressType,
    tmnxVdoGrpSrcSourceAddress       InetAddress,
    tmnxVdoGrpSrcStreamType          INTEGER,
    tmnxVdoGrpSrcVdoGrpId            TmnxVdoGrpId,
    tmnxVdoGrpSrcAdminRTBufferSize   TmnxMcPathVdoBufferSize,
    tmnxVdoGrpSrcSSRCId              Unsigned32,
    tmnxVdoGrpSrcUDPSrcPort          InetPortNumber,
    tmnxVdoGrpSrcUDPDestPort         InetPortNumber,
    tmnxVdoGrpSrcUptime              Unsigned32,
    tmnxVdoGrpSrcAdminBW             Unsigned32,
    tmnxVdoGrpSrcBufferSize          Gauge32,
    tmnxVdoGrpSrcRxBytes             Counter64,
    tmnxVdoGrpSrcRxPackets           Counter64,
    tmnxVdoGrpSrcRxInvalidPackets    Counter64,
    tmnxVdoGrpSrcTxBytes             Counter64,
    tmnxVdoGrpSrcTxPackets           Counter64,
    tmnxVdoGrpSrcTxFailedPackets     Counter64,
    tmnxVdoGrpSrcRTClientAdminState  TmnxAdminState,
    tmnxVdoGrpSrcRTClntRTSvrAddrType InetAddressType,
    tmnxVdoGrpSrcRTClntRTSvrAddr     InetAddress,
    tmnxVdoGrpSrcRTClientRTSrvrPort  InetPortNumber,
    tmnxVdoGrpSrcRTClientRxReTxBytes Counter64,
    tmnxVdoGrpSrcRTClientRxReTxPkts  Counter64,
    tmnxVdoGrpSrcRTClientTxRTReq     Counter32,
    tmnxVdoGrpSrcRTClientTxRTReqReTx Counter32,
    tmnxVdoGrpSrcRTClientGapsDetectd Counter32,
    tmnxVdoGrpSrcRTClientFailedReq   Counter32,
    tmnxVdoGrpSrcRTSrvrAdminState    TmnxAdminState,
    tmnxVdoGrpSrcRTSrvrRtpPktsReq    Counter32,
    tmnxVdoGrpSrcRTSrvrRxRTReq       Counter32,
    tmnxVdoGrpSrcRTSrvrRxFailedReq   Counter32,
    tmnxVdoGrpSrcRTSrvrTxRTReplies   Counter32,
    tmnxVdoGrpSrcRTSrvrTxBytes       Counter64,
    tmnxVdoGrpSrcRTSrvrTxPackets     Counter64,
    tmnxVdoGrpSrcFCCSrvrAdminState   TmnxAdminState,
    tmnxVdoGrpSrcFCCSrvrChnlType     TmnxMcPathVdoChlType,
    tmnxVdoGrpSrcFCCSrvrRxFCCReq     Counter32,
    tmnxVdoGrpSrcFCCSrvrRxFailedReq  Counter32,
    tmnxVdoGrpSrcFCCSrvrTxFCCReplies Counter32,
    tmnxVdoGrpSrcFCCSrvrTxBytes      Counter64,
    tmnxVdoGrpSrcFCCSrvrTxPackets    Counter64,
    tmnxVdoGrpSrcADIAdminState       TmnxAdminState,
    tmnxVdoGrpSrcADICurrentState     INTEGER,
    tmnxVdoGrpSrcADIPATVersion       Unsigned32,
    tmnxVdoGrpSrcADIPMTVersion       Unsigned32,
    tmnxVdoGrpSrcADIPATChanges       Counter32,
    tmnxVdoGrpSrcADIPMTChanges       Counter32,
    tmnxVdoGrpSrcADIRxPackets        Counter64,
    tmnxVdoGrpSrcADITxPackets        Counter64,
    tmnxVdoGrpSrcADIRxSCTE35Msgs     Counter32,
    tmnxVdoGrpSrcADIRxSCTE35MsgEnc   Counter32,
    tmnxVdoGrpSrcADIRxSCTE35MsgUnsup Counter32,
    tmnxVdoGrpSrcADIRxSCTE35MsgDisc  Counter32,
    tmnxVdoGrpSrcADIUnsuppTSLenPkts  Counter32,
    tmnxVdoGrpSrcRTClientPort        Unsigned32,
    tmnxVdoGrpSrcDupSeqNumber        Counter32,
    tmnxVdoGrpSrcRTSTxMcRetPkts      Counter64,
    tmnxVdoGrpSrcRTSTxMcRetPktsL32   Counter32,
    tmnxVdoGrpSrcRTSTxMcRetPktsH32   Counter32,
    tmnxVdoGrpSrcRTSTxMcRetBytes     Counter64,
    tmnxVdoGrpSrcRTSTxMcRetBytesL32  Counter32,
    tmnxVdoGrpSrcRTSTxMcRetBytesH32  Counter32,
    tmnxVdoGrpSrcRTSTxMcRetErrs      Counter64,
    tmnxVdoGrpSrcRTSTxMcRetErrsL32   Counter32,
    tmnxVdoGrpSrcRTSTxMcRetErrsH32   Counter32,
    tmnxVdoGrpSrcRTSRetReqQnc        Counter64,
    tmnxVdoGrpSrcRTSRetReqQncL32     Counter32,
    tmnxVdoGrpSrcRTSRetReqQncH32     Counter32,
    tmnxVdoGrpSrcRTSRetReqCrt        Counter64,
    tmnxVdoGrpSrcRTSRetReqCrtL32     Counter32,
    tmnxVdoGrpSrcRTSRetReqCrtH32     Counter32,
    tmnxVdoGrpSrcRxDupSsrcDrops      Counter32,
    tmnxVdoGrpSrcDupSsrc             Counter32,
    tmnxVdoGrpSrcFccMinDuration      Unsigned32,
    tmnxVdoGrpSrcAudioReorder        Unsigned32,
    tmnxVdoGrpSrcRxBytesSaved        Counter64,
    tmnxVdoGrpSrcRxBytesSavedL32     Counter32,
    tmnxVdoGrpSrcRxBytesSavedH32     Counter32,
    tmnxVdoGrpSrcRxPacketsSaved      Counter64,
    tmnxVdoGrpSrcRxPacketsSavedL32   Counter32,
    tmnxVdoGrpSrcRxPacketsSavedH32   Counter32,
    tmnxVdoGrpSrcStatOperBW          Unsigned32,
    tmnxVdoGrpSrcRouterIfName        TNamedItemOrEmpty,
    tmnxVdoGrpSrcNumFccDentedPkts    Counter32
}

tmnxVdoGrpSrcGrpAddrType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcGrpAddrType indicates the type of IP
         multicast group address represented by tmnxVdoGrpSrcGroupAddress."
    ::= { tmnxVdoGrpSrcStatEntry 1 }

tmnxVdoGrpSrcGroupAddress        OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcGroupAddress indicates the IP multicast
         group address for which this entry contains information."
    ::= { tmnxVdoGrpSrcStatEntry 2 }

tmnxVdoGrpSrcSrcAddrType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcSrcAddrType indicates the type of IP
         multicast source address represented by tmnxVdoGrpSrcSourceAddress."
    ::= { tmnxVdoGrpSrcStatEntry 3 }

tmnxVdoGrpSrcSourceAddress       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcSourceAddress indicates the IP multicast
         source address for which this entry contains information."
    ::= { tmnxVdoGrpSrcStatEntry 4 }

tmnxVdoGrpSrcStreamType          OBJECT-TYPE
    SYNTAX      INTEGER {
        network (0),
        zone    (1)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcStreamType indicates the type of stream
         being transmitted from the video ISA perspective. Network stream is
         the stream ingressing the video ISA and being stored by it. Zone
         stream is the stream egressing the video ISA into which AD streams
         will be inserted."
    ::= { tmnxVdoGrpSrcStatEntry 5 }

tmnxVdoGrpSrcVdoGrpId            OBJECT-TYPE
    SYNTAX      TmnxVdoGrpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVdoGrpId indicates the identifier of the
         video group."
    ::= { tmnxVdoGrpSrcStatEntry 6 }

tmnxVdoGrpSrcAdminRTBufferSize   OBJECT-TYPE
    SYNTAX      TmnxMcPathVdoBufferSize
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcAdminRTBufferSize indicates the number of
         milliseconds worth of channel packets to store for the Retransmission
         (RT) server."
    ::= { tmnxVdoGrpSrcStatEntry 7 }

tmnxVdoGrpSrcSSRCId              OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcSSRCId indicates the synchronization source
         (SSRC) identifier carried in the Real-time Transport Protocol (RTP)
         header to identify the source of a stream of RTP packets."
    ::= { tmnxVdoGrpSrcStatEntry 8 }

tmnxVdoGrpSrcUDPSrcPort          OBJECT-TYPE
    SYNTAX      InetPortNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcUDPSrcPort indicates the UDP source port in
         the received RTP multicast stream."
    ::= { tmnxVdoGrpSrcStatEntry 9 }

tmnxVdoGrpSrcUDPDestPort         OBJECT-TYPE
    SYNTAX      InetPortNumber
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcUDPDestPort indicates the UDP destination
         port in the received RTP multicast stream."
    ::= { tmnxVdoGrpSrcStatEntry 10 }

tmnxVdoGrpSrcUptime              OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcUptime indicates the time since this source
         group entry was created."
    ::= { tmnxVdoGrpSrcStatEntry 11 }

tmnxVdoGrpSrcAdminBW             OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcAdminBW indicates the administrative
         bandwidth of the multicast group."
    ::= { tmnxVdoGrpSrcStatEntry 12 }

tmnxVdoGrpSrcBufferSize          OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcBufferSize indicates the number of
         milliseconds worth of channel packets stored by the Retransmission
         (RT) server or Fast Channel Change (FCC) server on this channel."
    ::= { tmnxVdoGrpSrcStatEntry 13 }

tmnxVdoGrpSrcRxBytes             OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRxBytes indicates the total number of bytes
         received on this multicast channel."
    ::= { tmnxVdoGrpSrcStatEntry 14 }

tmnxVdoGrpSrcRxPackets           OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRxPackets indicates the total number of
         packets received on this multicast channel."
    ::= { tmnxVdoGrpSrcStatEntry 15 }

tmnxVdoGrpSrcRxInvalidPackets    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRxInvalidPackets indicates the total number
         of invalid packets received on this multicast channel."
    ::= { tmnxVdoGrpSrcStatEntry 16 }

tmnxVdoGrpSrcTxBytes             OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcTxBytes indicates the total number of bytes
         transmitted on this multicast channel."
    ::= { tmnxVdoGrpSrcStatEntry 17 }

tmnxVdoGrpSrcTxPackets           OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcTxPackets indicates the total number of
         packets transmitted on this multicast channel."
    ::= { tmnxVdoGrpSrcStatEntry 18 }

tmnxVdoGrpSrcTxFailedPackets     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcTxFailedPackets indicates the total number
         of failures during the transmission of packets on this multicast
         channel. Failure happens when the packet to be sent is not stored in
         the video cache."
    ::= { tmnxVdoGrpSrcStatEntry 19 }

tmnxVdoGrpSrcRTClientAdminState  OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClientAdminState indicates the
         administrative state of the retransmission client.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 20 }

tmnxVdoGrpSrcRTClntRTSvrAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClntRTSvrAddrType indicates the type of
         address represented by tmnxVdoGrpSrcRTClntRTSvrAddr.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 21 }

tmnxVdoGrpSrcRTClntRTSvrAddr     OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClntRTSvrAddr indicates the address of the
         Retransmission (RT) server for this channel.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 22 }

tmnxVdoGrpSrcRTClientRTSrvrPort  OBJECT-TYPE
    SYNTAX      InetPortNumber
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClientRTSrvrPort indicates the
         Retransmission (RT) server port for this channel.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 23 }

tmnxVdoGrpSrcRTClientRxReTxBytes OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClientRxReTxBytes indicates the total
         number of retransmitted bytes received by the Retransmission (RT)
         client.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 24 }

tmnxVdoGrpSrcRTClientRxReTxPkts  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClientRxReTxPkts indicates the total
         number of retransmitted packets received by the Retransmission (RT)
         client.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 25 }

tmnxVdoGrpSrcRTClientTxRTReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClientTxRTReq indicates the total number
         of Retransmission (RT) requests sent by the RT client.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 26 }

tmnxVdoGrpSrcRTClientTxRTReqReTx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClientTxRTReqReTx indicates the total
         number of repeat Retransmission (RT) requests attempted by the RT
         client.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 27 }

tmnxVdoGrpSrcRTClientGapsDetectd OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClientGapsDetectd indicates the total
         number of gaps in the sequence numbers detected by the Retransmission
         (RT) client.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 28 }

tmnxVdoGrpSrcRTClientFailedReq   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClientFailedReq indicates the total number
         of Retransmission (RT) requests that could not be generated by the RT
         client due to gaps in the sequence numbers.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 29 }

tmnxVdoGrpSrcRTSrvrAdminState    OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSrvrAdminState indicates the
         administrative state of the Retransmission (RT) server."
    ::= { tmnxVdoGrpSrcStatEntry 30 }

tmnxVdoGrpSrcRTSrvrRtpPktsReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSrvrRtpPktsReq indicates the total number
         of Real-time Transport Protocol (RTP) packets requested in the
         Real-time Transport Control Protocol (RTCP) feedback (FB) messages
         received on this channel."
    ::= { tmnxVdoGrpSrcStatEntry 31 }

tmnxVdoGrpSrcRTSrvrRxRTReq       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSrvrRxRTReq indicates the total number of
         RT requests received by the Retransmission (RT) server."
    ::= { tmnxVdoGrpSrcStatEntry 32 }

tmnxVdoGrpSrcRTSrvrRxFailedReq   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSrvrRxFailedReq indicates the total number
         of failed requests at the Retransmission (RT) server due to congestion
         or lack of resources."
    ::= { tmnxVdoGrpSrcStatEntry 33 }

tmnxVdoGrpSrcRTSrvrTxRTReplies   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSrvrTxRTReplies indicates the total number
         of Retransmission (RT) replies sent by the RT server."
    ::= { tmnxVdoGrpSrcStatEntry 34 }

tmnxVdoGrpSrcRTSrvrTxBytes       OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSrvrTxBytes indicates the total number of
         bytes sent by the Retransmission (RT) server."
    ::= { tmnxVdoGrpSrcStatEntry 35 }

tmnxVdoGrpSrcRTSrvrTxPackets     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSrvrTxPackets indicates the total number
         of packets sent by the Retransmission (RT) server."
    ::= { tmnxVdoGrpSrcStatEntry 36 }

tmnxVdoGrpSrcFCCSrvrAdminState   OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcFCCSrvrAdminState indicates whether the Fast
         Channel Change (FCC) server is enabled on this channel."
    ::= { tmnxVdoGrpSrcStatEntry 37 }

tmnxVdoGrpSrcFCCSrvrChnlType     OBJECT-TYPE
    SYNTAX      TmnxMcPathVdoChlType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcFCCSrvrChnlType indicates the type of
         channel served by the Fast Channel Change (FCC) server."
    ::= { tmnxVdoGrpSrcStatEntry 38 }

tmnxVdoGrpSrcFCCSrvrRxFCCReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcFCCSrvrRxFCCReq indicates the total number
         of Fast Channel Change (FCC) requests received by the FCC server."
    ::= { tmnxVdoGrpSrcStatEntry 39 }

tmnxVdoGrpSrcFCCSrvrRxFailedReq  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcFCCSrvrRxFailedReq indicates the total
         number of failed requests at the Fast Channel Change (FCC) server."
    ::= { tmnxVdoGrpSrcStatEntry 40 }

tmnxVdoGrpSrcFCCSrvrTxFCCReplies OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcFCCSrvrTxFCCReplies indicates the total
         number of Fast Channel Change (FCC) replies sent by the FCC server."
    ::= { tmnxVdoGrpSrcStatEntry 41 }

tmnxVdoGrpSrcFCCSrvrTxBytes      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcFCCSrvrTxBytes indicates the total number of
         bytes sent by the Fast Channel Change (FCC) server."
    ::= { tmnxVdoGrpSrcStatEntry 42 }

tmnxVdoGrpSrcFCCSrvrTxPackets    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcFCCSrvrTxPackets indicates the total number
         of packets sent by the Fast Channel Change (FCC) server."
    ::= { tmnxVdoGrpSrcStatEntry 43 }

tmnxVdoGrpSrcADIAdminState       OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIAdminState indicates whether Ad Insertion
         is enabled on the video ISA."
    ::= { tmnxVdoGrpSrcStatEntry 44 }

tmnxVdoGrpSrcADICurrentState     OBJECT-TYPE
    SYNTAX      INTEGER {
        network (0),
        ad      (1)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADICurrentState indicates whether the video
         ISA is transmitting network stream or ads."
    ::= { tmnxVdoGrpSrcStatEntry 45 }

tmnxVdoGrpSrcADIPATVersion       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIPATVersion indicates the version of the
         Program Association Table (PAT)."
    ::= { tmnxVdoGrpSrcStatEntry 46 }

tmnxVdoGrpSrcADIPMTVersion       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIPMTVersion indicates the version of the
         Program Map Table (PMT)."
    ::= { tmnxVdoGrpSrcStatEntry 47 }

tmnxVdoGrpSrcADIPATChanges       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIPATChanges indicates the total number of
         Program Association Table (PAT) version changes."
    ::= { tmnxVdoGrpSrcStatEntry 48 }

tmnxVdoGrpSrcADIPMTChanges       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIPMTChanges indicates the total number of
         Program Map Table (PMT) version changes."
    ::= { tmnxVdoGrpSrcStatEntry 49 }

tmnxVdoGrpSrcADIRxPackets        OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIRxPackets indicates the total number of
         Ad Insert (ADI) packets received by the video ISA."
    ::= { tmnxVdoGrpSrcStatEntry 50 }

tmnxVdoGrpSrcADITxPackets        OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADITxPackets indicates the total number of
         Ad Insert (ADI) packets sent by the video ISA."
    ::= { tmnxVdoGrpSrcStatEntry 51 }

tmnxVdoGrpSrcADIRxSCTE35Msgs     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIRxSCTE35Msgs indicates the total number
         of Society of Cable Telecommunications Engineers (SCTE-35) messages
         received by the video ISA."
    ::= { tmnxVdoGrpSrcStatEntry 52 }

tmnxVdoGrpSrcADIRxSCTE35MsgEnc   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIRxSCTE35MsgEnc indicates the total number
         of encrypted Society of Cable Telecommunications Engineers (SCTE-35)
         messages received by the video ISA."
    ::= { tmnxVdoGrpSrcStatEntry 53 }

tmnxVdoGrpSrcADIRxSCTE35MsgUnsup OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIRxSCTE35MsgUnsup indicates the total
         number of unsupported Society of Cable Telecommunications Engineers
         (SCTE-35) messages received by the video ISA."
    ::= { tmnxVdoGrpSrcStatEntry 54 }

tmnxVdoGrpSrcADIRxSCTE35MsgDisc  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIRxSCTE35MsgDisc indicates the total
         number of Society of Cable Telecommunications Engineers (SCTE-35)
         messages received by the video ISA and discarded. SCTE-35 messages
         with unsupported commands and encrypted SCTE-35 messages are
         discarded."
    ::= { tmnxVdoGrpSrcStatEntry 55 }

tmnxVdoGrpSrcADIUnsuppTSLenPkts  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcADIUnsuppTSLenPkts indicates the total
         number of data packets received whose size is not equal to 188 bytes.
         The value of this object is valid only when the corresponding
         tmnxVdoGrpADIServerState value is set to 'true'."
    ::= { tmnxVdoGrpSrcStatEntry 56 }

tmnxVdoGrpSrcRTClientPort        OBJECT-TYPE
    SYNTAX      Unsigned32 (6000..8000)
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTClientPort indicates the local port on
         which the Retransmission (RT) requests are received.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpSrcStatEntry 57 }

tmnxVdoGrpSrcDupSeqNumber        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcDupSeqNumber indicates the total number of
         Real-time Transport Protocol (RTP) packets detected with a duplicate
         sequence number."
    ::= { tmnxVdoGrpSrcStatEntry 58 }

tmnxVdoGrpSrcRTSTxMcRetPkts      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSTxMcRetPkts indicates the total number of
         multicast packets sent in response to retransmission requests."
    ::= { tmnxVdoGrpSrcStatEntry 59 }

tmnxVdoGrpSrcRTSTxMcRetPktsL32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSTxMcRetPktsL32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcRTSTxMcRetPkts."
    ::= { tmnxVdoGrpSrcStatEntry 60 }

tmnxVdoGrpSrcRTSTxMcRetPktsH32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSTxMcRetPktsH32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcRTSTxMcRetPkts."
    ::= { tmnxVdoGrpSrcStatEntry 61 }

tmnxVdoGrpSrcRTSTxMcRetBytes     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSTxMcRetBytes indicates the total number
         of multicast bytes sent in response to retransmission requests."
    ::= { tmnxVdoGrpSrcStatEntry 62 }

tmnxVdoGrpSrcRTSTxMcRetBytesL32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSTxMcRetBytesL32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcRTSTxMcRetBytes."
    ::= { tmnxVdoGrpSrcStatEntry 63 }

tmnxVdoGrpSrcRTSTxMcRetBytesH32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSTxMcRetBytesH32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcRTSTxMcRetBytes."
    ::= { tmnxVdoGrpSrcStatEntry 64 }

tmnxVdoGrpSrcRTSTxMcRetErrs      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSTxMcRetErrs indicates the total number
         of errors occurred while doing  multicast retransmission in response to
         requests."
    ::= { tmnxVdoGrpSrcStatEntry 65 }

tmnxVdoGrpSrcRTSTxMcRetErrsL32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSTxMcRetErrsL32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcRTSTxMcRetErrs."
    ::= { tmnxVdoGrpSrcStatEntry 66 }

tmnxVdoGrpSrcRTSTxMcRetErrsH32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSTxMcRetErrsH32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcRTSTxMcRetErrs."
    ::= { tmnxVdoGrpSrcStatEntry 67 }

tmnxVdoGrpSrcRTSRetReqQnc        OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSRetReqQnc indicates the total number of
         unicast retransmission requests quenched by carrying out multicast
         response requests."
    ::= { tmnxVdoGrpSrcStatEntry 68 }

tmnxVdoGrpSrcRTSRetReqQncL32     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSRetReqQncL32 indicates the lower 32 bits
         of the value of tmnxVdoGrpSrcRTSRetReqQnc."
    ::= { tmnxVdoGrpSrcStatEntry 69 }

tmnxVdoGrpSrcRTSRetReqQncH32     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSRetReqQncH32 indicates the higher 32 bits
         of the value of tmnxVdoGrpSrcRTSRetReqQnc."
    ::= { tmnxVdoGrpSrcStatEntry 70 }

tmnxVdoGrpSrcRTSRetReqCrt        OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSRetReqCrt indicates the total number of
         multicast retransmission requests created in response to the unicast
         retransmission."
    ::= { tmnxVdoGrpSrcStatEntry 71 }

tmnxVdoGrpSrcRTSRetReqCrtL32     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSRetReqCrtL32 indicates the lower 32 bits
         of the value of tmnxVdoGrpSrcRTSRetReqCrt."
    ::= { tmnxVdoGrpSrcStatEntry 72 }

tmnxVdoGrpSrcRTSRetReqCrtH32     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRTSRetReqCrtH32 indicates the higher 32 bits
         of the value of tmnxVdoGrpSrcRTSRetReqCrt."
    ::= { tmnxVdoGrpSrcStatEntry 73 }

tmnxVdoGrpSrcRxDupSsrcDrops      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRxDupSsrcDrops indicates the number of
         receive-packets dropped with a duplicate synchronization source (SSRC)
         identifier."
    ::= { tmnxVdoGrpSrcStatEntry 74 }

tmnxVdoGrpSrcDupSsrc             OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcDupSsrc indicates the number of packets
         detected with a duplicate synchronization source (SSRC) identifier."
    ::= { tmnxVdoGrpSrcStatEntry 75 }

tmnxVdoGrpSrcFccMinDuration      OBJECT-TYPE
    SYNTAX      Unsigned32 (1..100000)
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcFccMinDuration indicates the minimum FCC
         duration in msecs for FCC requests for this channel."
    ::= { tmnxVdoGrpSrcStatEntry 76 }

tmnxVdoGrpSrcAudioReorder        OBJECT-TYPE
    SYNTAX      Unsigned32 (1..100000)
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcAudioReorder indicates in msecs how much
         earlier the audio frames are sent during an FCC burst to achieve a
         good audio fast-channel-change experience."
    ::= { tmnxVdoGrpSrcStatEntry 77 }

tmnxVdoGrpSrcRxBytesSaved        OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRxBytesSaved indicates the total number of
         received bytes that are saved on this multicast channel."
    ::= { tmnxVdoGrpSrcStatEntry 78 }

tmnxVdoGrpSrcRxBytesSavedL32     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRxBytesSavedL32 indicates the lower 32 bits
         of the value of tmnxVdoGrpSrcRxBytesSaved."
    ::= { tmnxVdoGrpSrcStatEntry 79 }

tmnxVdoGrpSrcRxBytesSavedH32     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRxBytesSavedH32 indicates the higher 32 bits
         of the value of tmnxVdoGrpSrcRxBytesSaved."
    ::= { tmnxVdoGrpSrcStatEntry 80 }

tmnxVdoGrpSrcRxPacketsSaved      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRxPacketsSaved indicates the total number of
         received packets that are saved on this multicast channel."
    ::= { tmnxVdoGrpSrcStatEntry 81 }

tmnxVdoGrpSrcRxPacketsSavedL32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRxPacketsSavedL32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcRxPacketsSaved."
    ::= { tmnxVdoGrpSrcStatEntry 82 }

tmnxVdoGrpSrcRxPacketsSavedH32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRxPacketsSavedH32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcRxPacketsSaved."
    ::= { tmnxVdoGrpSrcStatEntry 83 }

tmnxVdoGrpSrcStatOperBW          OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcStatOperBW indicates the most recently
         computed bandwidth of the video stream averaged over the last one
         second."
    ::= { tmnxVdoGrpSrcStatEntry 84 }

tmnxVdoGrpSrcRouterIfName        OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcRouterIfName indicates the ingress interface
         name for this video channel."
    ::= { tmnxVdoGrpSrcStatEntry 85 }

tmnxVdoGrpSrcNumFccDentedPkts    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcNumFccDentedPkts indicates the number of
         packets in the unicast FCC stream that were dropped due to denting."
    ::= { tmnxVdoGrpSrcStatEntry 86 }

tmnxVdoSGStatV1Table             OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoSGStatV1Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxVdoSGStatV1Table provides an extension of the
         tmnxVdoGrpSrcStatTable and contains channel statistics for the
         multicast groups."
    ::= { tmnxVdoObjs 8 }

tmnxVdoSGStatV1Entry             OBJECT-TYPE
    SYNTAX      TmnxVdoSGStatV1Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoSGStatV1Table containing channel statistics.

         The counters in this table are defined as 32-bit entries which hold
         the values of 64-bit entries in tmnxVdoGrpSrcStatTable."
    AUGMENTS    { tmnxVdoGrpSrcStatEntry }
    ::= { tmnxVdoSGStatV1Table 1 }

TmnxVdoSGStatV1Entry             ::= SEQUENCE
{
    tmnxVdoSGV1RxBytesLow32          Counter32,
    tmnxVdoSGV1RxBytesHigh32         Counter32,
    tmnxVdoSGV1RxPacketsLow32        Counter32,
    tmnxVdoSGV1RxPacketsHigh32       Counter32,
    tmnxVdoSGV1RxInvalidPacketsLow32 Counter32,
    tmnxVdoSGV1RxInvalidPacketsHgh32 Counter32,
    tmnxVdoSGV1TxBytesLow32          Counter32,
    tmnxVdoSGV1TxBytesHigh32         Counter32,
    tmnxVdoSGV1TxPacketsLow32        Counter32,
    tmnxVdoSGV1TxPacketsHigh32       Counter32,
    tmnxVdoSGV1TxFailedPacketsLow32  Counter32,
    tmnxVdoSGV1TxFailedPacketsHigh32 Counter32,
    tmnxVdoSGV1RTClntRxReTxBytsLow32 Counter32,
    tmnxVdoSGV1RTClntRxReTxBytsHgh32 Counter32,
    tmnxVdoSGV1RTClntRxReTxPktsLow32 Counter32,
    tmnxVdoSGV1RTClntRxReTxPktsHgh32 Counter32,
    tmnxVdoSGV1RTSrvrTxBytesLow32    Counter32,
    tmnxVdoSGV1RTSrvrTxBytesHigh32   Counter32,
    tmnxVdoSGV1RTSrvrTxPacketsLow32  Counter32,
    tmnxVdoSGV1RTSrvrTxPacketsHigh32 Counter32,
    tmnxVdoSGV1FCCSrvrTxBytesLow32   Counter32,
    tmnxVdoSGV1FCCSrvrTxBytesHigh32  Counter32,
    tmnxVdoSGV1FCCSrvrTxPacketsLow32 Counter32,
    tmnxVdoSGV1FCCSrvrTxPacketsHgh32 Counter32,
    tmnxVdoSGV1ADIRxPacketsLow32     Counter32,
    tmnxVdoSGV1ADIRxPacketsHigh32    Counter32,
    tmnxVdoSGV1ADITxPacketsLow32     Counter32,
    tmnxVdoSGV1ADITxPacketsHigh32    Counter32
}

tmnxVdoSGV1RxBytesLow32          OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RxBytesLow32 indicates the lower 32 bits of
         the value of tmnxVdoGrpSrcRxBytes."
    ::= { tmnxVdoSGStatV1Entry 1 }

tmnxVdoSGV1RxBytesHigh32         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RxBytesHigh32 indicates the higher 32 bits of
         the value of tmnxVdoGrpSrcRxBytes."
    ::= { tmnxVdoSGStatV1Entry 2 }

tmnxVdoSGV1RxPacketsLow32        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RxPacketsLow32 indicates the lower 32 bits of
         the value of tmnxVdoGrpSrcRxPackets."
    ::= { tmnxVdoSGStatV1Entry 3 }

tmnxVdoSGV1RxPacketsHigh32       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RxPacketsHigh32 indicates the higher 32 bits
         of the value of tmnxVdoGrpSrcRxPackets."
    ::= { tmnxVdoSGStatV1Entry 4 }

tmnxVdoSGV1RxInvalidPacketsLow32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RxInvalidPacketsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcRxInvalidPackets."
    ::= { tmnxVdoSGStatV1Entry 5 }

tmnxVdoSGV1RxInvalidPacketsHgh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RxInvalidPacketsHgh32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcRxInvalidPackets."
    ::= { tmnxVdoSGStatV1Entry 6 }

tmnxVdoSGV1TxBytesLow32          OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1TxBytesLow32 indicates the lower 32 bits of
         the value of tmnxVdoGrpSrcTxBytes."
    ::= { tmnxVdoSGStatV1Entry 7 }

tmnxVdoSGV1TxBytesHigh32         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1TxBytesHigh32 indicates the higher 32 bits of
         the value of tmnxVdoGrpSrcTxBytes."
    ::= { tmnxVdoSGStatV1Entry 8 }

tmnxVdoSGV1TxPacketsLow32        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1TxPacketsLow32 indicates the lower 32 bits of
         the value of tmnxVdoGrpSrcTxPackets."
    ::= { tmnxVdoSGStatV1Entry 9 }

tmnxVdoSGV1TxPacketsHigh32       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1TxPacketsHigh32 indicates the higher 32 bits
         of the value of tmnxVdoGrpSrcTxPackets."
    ::= { tmnxVdoSGStatV1Entry 10 }

tmnxVdoSGV1TxFailedPacketsLow32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1TxFailedPacketsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcTxFailedPackets."
    ::= { tmnxVdoSGStatV1Entry 11 }

tmnxVdoSGV1TxFailedPacketsHigh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1TxFailedPacketsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcTxFailedPackets."
    ::= { tmnxVdoSGStatV1Entry 12 }

tmnxVdoSGV1RTClntRxReTxBytsLow32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RTClntRxReTxBytsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcRTClientRxReTxBytes."
    ::= { tmnxVdoSGStatV1Entry 13 }

tmnxVdoSGV1RTClntRxReTxBytsHgh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RTClntRxReTxBytsHgh32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcRTClientRxReTxBytes."
    ::= { tmnxVdoSGStatV1Entry 14 }

tmnxVdoSGV1RTClntRxReTxPktsLow32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RTClntRxReTxPktsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcRTClientRxReTxPkts."
    ::= { tmnxVdoSGStatV1Entry 15 }

tmnxVdoSGV1RTClntRxReTxPktsHgh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RTClntRxReTxPktsHgh32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcRTClientRxReTxPkts."
    ::= { tmnxVdoSGStatV1Entry 16 }

tmnxVdoSGV1RTSrvrTxBytesLow32    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RTSrvrTxBytesLow32 indicates the lower 32 bits
         of the value of tmnxVdoGrpSrcRTSrvrTxBytes."
    ::= { tmnxVdoSGStatV1Entry 17 }

tmnxVdoSGV1RTSrvrTxBytesHigh32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RTSrvrTxBytesHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcRTSrvrTxBytes."
    ::= { tmnxVdoSGStatV1Entry 18 }

tmnxVdoSGV1RTSrvrTxPacketsLow32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RTSrvrTxPacketsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcRTSrvrTxPackets."
    ::= { tmnxVdoSGStatV1Entry 19 }

tmnxVdoSGV1RTSrvrTxPacketsHigh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1RTSrvrTxPacketsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcRTSrvrTxPackets."
    ::= { tmnxVdoSGStatV1Entry 20 }

tmnxVdoSGV1FCCSrvrTxBytesLow32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1FCCSrvrTxBytesLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcFCCSrvrTxBytes."
    ::= { tmnxVdoSGStatV1Entry 21 }

tmnxVdoSGV1FCCSrvrTxBytesHigh32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1FCCSrvrTxBytesHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcFCCSrvrTxBytes."
    ::= { tmnxVdoSGStatV1Entry 22 }

tmnxVdoSGV1FCCSrvrTxPacketsLow32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1FCCSrvrTxPacketsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcFCCSrvrTxPackets."
    ::= { tmnxVdoSGStatV1Entry 23 }

tmnxVdoSGV1FCCSrvrTxPacketsHgh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1FCCSrvrTxPacketsHgh32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcFCCSrvrTxPackets."
    ::= { tmnxVdoSGStatV1Entry 24 }

tmnxVdoSGV1ADIRxPacketsLow32     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1ADIRxPacketsLow32 indicates the lower 32 bits
         of the value of tmnxVdoGrpSrcADIRxPackets."
    ::= { tmnxVdoSGStatV1Entry 25 }

tmnxVdoSGV1ADIRxPacketsHigh32    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1ADIRxPacketsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcADIRxPackets."
    ::= { tmnxVdoSGStatV1Entry 26 }

tmnxVdoSGV1ADITxPacketsLow32     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1ADITxPacketsLow32 indicates the lower 32 bits
         of the value of tmnxVdoGrpSrcADITxPackets."
    ::= { tmnxVdoSGStatV1Entry 27 }

tmnxVdoSGV1ADITxPacketsHigh32    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSGV1ADITxPacketsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcADITxPackets."
    ::= { tmnxVdoSGStatV1Entry 28 }

tmnxVdoSessionTable              OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxVdoSessionTable contains information and statistics for each
         session."
    ::= { tmnxVdoObjs 9 }

tmnxVdoSessionEntry              OBJECT-TYPE
    SYNTAX      TmnxVdoSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoSessionTable. Each entry represents the source
         address for the session."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoSessionSourceAddrType,
        tmnxVdoSessionSourceAddr,
        tmnxVdoSessionSourcePort
    }
    ::= { tmnxVdoSessionTable 1 }

TmnxVdoSessionEntry              ::= SEQUENCE
{
    tmnxVdoSessionSourceAddrType     InetAddressType,
    tmnxVdoSessionSourceAddr         InetAddress,
    tmnxVdoSessionSourcePort         InetPortNumber,
    tmnxVdoSessionSSRCId             Counter32,
    tmnxVdoSessionUpTime             Unsigned32,
    tmnxVdoSessionExpireTime         Unsigned32,
    tmnxVdoSessionCName              TNamedItem,
    tmnxVdoSessionDestAddrType       InetAddressType,
    tmnxVdoSessionDestAddr           InetAddress,
    tmnxVdoSessionRxFCCRequests      Counter32,
    tmnxVdoSessionTxFCCReplies       Counter32,
    tmnxVdoSessionTxFCCPackets       Counter32,
    tmnxVdoSessionTxFCCOctets        Counter32,
    tmnxVdoSessionTxFCCFailedPackets Counter32,
    tmnxVdoSessionRxRTRequests       Counter32,
    tmnxVdoSessionTxRTReplies        Counter32,
    tmnxVdoSessionTxRTPackets        Counter32,
    tmnxVdoSessionTxRTOctets         Counter32,
    tmnxVdoSessionTxRTFailedPackets  Counter32,
    tmnxVdoSessionRequestedRtpPkts   Counter32,
    tmnxVdoSessionRTReqQuenched      Counter32,
    tmnxVdoSessionRTMcastReqCreated  Counter32,
    tmnxVdoSessionPktsLostInSeq10    Counter32,
    tmnxVdoSessionPktsLostInSeq20    Counter32,
    tmnxVdoSessionPktsLostInSeq30    Counter32,
    tmnxVdoSessionPktsLostInSeq40    Counter32,
    tmnxVdoSessionPktsLostInSeqMore  Counter32
}

tmnxVdoSessionSourceAddrType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionSourceAddrType indicates the type of
         address represented by tmnxVdoSessionSourceAddr."
    ::= { tmnxVdoSessionEntry 1 }

tmnxVdoSessionSourceAddr         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionSourceAddr indicates the address of the
         Fast Channel Change (FCC) server or Retransmission (RT) server."
    ::= { tmnxVdoSessionEntry 2 }

tmnxVdoSessionSourcePort         OBJECT-TYPE
    SYNTAX      InetPortNumber
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionSourcePort indicates the server port on
         which the Fast Channel Change or Retransmission services are being
         provided."
    ::= { tmnxVdoSessionEntry 3 }

tmnxVdoSessionSSRCId             OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionSSRCId indicates the synchronization source
         (SSRC) identifier of the server."
    ::= { tmnxVdoSessionEntry 4 }

tmnxVdoSessionUpTime             OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionUpTime indicates how long it has been since
         the session was established."
    ::= { tmnxVdoSessionEntry 5 }

tmnxVdoSessionExpireTime         OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionExpireTime indicates the expiry time of
         this session. The value of this object ticks backwards and indicates
         the remaining time that the row may exist before it is aged out."
    ::= { tmnxVdoSessionEntry 6 }

tmnxVdoSessionCName              OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionCName indicates the canonical name of the
         server."
    ::= { tmnxVdoSessionEntry 7 }

tmnxVdoSessionDestAddrType       OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionDestAddrType indicates the type of address
         represented by tmnxVdoSessionDestAddr."
    ::= { tmnxVdoSessionEntry 8 }

tmnxVdoSessionDestAddr           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionDestAddr indicates the address of the
         destination in this session."
    ::= { tmnxVdoSessionEntry 9 }

tmnxVdoSessionRxFCCRequests      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionRxFCCRequests indicates the total number of
         Fast Channel Change (FCC) requests received by the server."
    ::= { tmnxVdoSessionEntry 10 }

tmnxVdoSessionTxFCCReplies       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionTxFCCReplies indicates the total number of
         Fast Channel Change (FCC) replies sent by the server."
    ::= { tmnxVdoSessionEntry 11 }

tmnxVdoSessionTxFCCPackets       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionTxFCCPackets indicates the total number of
         Fast Channel Change (FCC) packets sent by the server."
    ::= { tmnxVdoSessionEntry 12 }

tmnxVdoSessionTxFCCOctets        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionTxFCCOctets indicates the total number of
         Fast Channel Change (FCC) octets sent by the server."
    ::= { tmnxVdoSessionEntry 13 }

tmnxVdoSessionTxFCCFailedPackets OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionTxFCCFailedPackets indicates the total
         number of failures during the transmission of Fast Channel Change
         (FCC) packets. Failure happens when the packet to be sent is not
         stored in the video cache."
    ::= { tmnxVdoSessionEntry 14 }

tmnxVdoSessionRxRTRequests       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionRxRTRequests indicates the total number of
         Retransmission (RT) requests received by the server."
    ::= { tmnxVdoSessionEntry 15 }

tmnxVdoSessionTxRTReplies        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionTxRTReplies indicates the total number of
         Retransmission (RT) replies sent by the server."
    ::= { tmnxVdoSessionEntry 16 }

tmnxVdoSessionTxRTPackets        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionTxRTPackets indicates the total number of
         Retransmission (RT) packets sent by the server."
    ::= { tmnxVdoSessionEntry 17 }

tmnxVdoSessionTxRTOctets         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionTxRTOctets indicates the total number of
         Retransmission (RT) octets sent by the server."
    ::= { tmnxVdoSessionEntry 18 }

tmnxVdoSessionTxRTFailedPackets  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionTxRTFailedPackets indicates the total
         number of failures during the transmission of Retransmission (RT)
         packets. Failure happens when the packet to be sent is not stored in
         the video cache."
    ::= { tmnxVdoSessionEntry 19 }

tmnxVdoSessionRequestedRtpPkts   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionRequestedRtpPkts indicates the number of
         Real-time Transport Protocol (RTP) packets requested in the Real-time
         Transport Control Protocol (RTCP) feedback (FB) messages received in
         this session."
    ::= { tmnxVdoSessionEntry 20 }

tmnxVdoSessionRTReqQuenched      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionRTReqQuenched indicates the number of
         unicast retransmission requests quenched with multicast retransmission
         in this session."
    ::= { tmnxVdoSessionEntry 21 }

tmnxVdoSessionRTMcastReqCreated  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionRTMcastReqCreated indicates the number of
         multicast retransmission requests created in response to unicast
         retransmission requests in this session."
    ::= { tmnxVdoSessionEntry 22 }

tmnxVdoSessionPktsLostInSeq10    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionPktsLostInSeq10 indicates the total number
         of packets within sequences of 2 to 10 consecutive lost packets in
         this session."
    ::= { tmnxVdoSessionEntry 23 }

tmnxVdoSessionPktsLostInSeq20    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionPktsLostInSeq20 indicates the total number
         of packets within sequences of 11 to 20 consecutive lost packets in
         this session."
    ::= { tmnxVdoSessionEntry 24 }

tmnxVdoSessionPktsLostInSeq30    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionPktsLostInSeq30 indicates the total number
         of packets within sequences of 21 to 30 consecutive lost packets in
         this session."
    ::= { tmnxVdoSessionEntry 25 }

tmnxVdoSessionPktsLostInSeq40    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionPktsLostInSeq40 indicates the total number
         of packets within sequences of 31 to 40 consecutive lost packets in
         this session."
    ::= { tmnxVdoSessionEntry 26 }

tmnxVdoSessionPktsLostInSeqMore  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoSessionPktsLostInSeqMore indicates the total
         number of packets within sequences of 41 or more consecutive lost
         packets in this session."
    ::= { tmnxVdoSessionEntry 27 }

tmnxVdoIfStatTable               OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoIfStatEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxVdoIfStatTable contains information and statistics for each video
         interface configured in the system."
    ::= { tmnxVdoObjs 10 }

tmnxVdoIfStatEntry               OBJECT-TYPE
    SYNTAX      TmnxVdoIfStatEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoIfStatTable. Each row entry represents an IP
         address assigned to a video interface."
    AUGMENTS    { tmnxVdoIfAddrEntry }
    ::= { tmnxVdoIfStatTable 1 }

TmnxVdoIfStatEntry               ::= SEQUENCE
{
    tmnxVdoIfStatHdRTServerState     TruthValue,
    tmnxVdoIfStatSdRTServerState     TruthValue,
    tmnxVdoIfStatPipRTServerState    TruthValue,
    tmnxVdoIfStatRTSvrSdRtpPktsReq   Counter64,
    tmnxVdoIfStatRTSvrHdRtpPktsReq   Counter64,
    tmnxVdoIfStatRTSvrPipRtpPktsReq  Counter64,
    tmnxVdoIfStatRTSvrRxSdRTReq      Counter64,
    tmnxVdoIfStatRTSvrRxSdFailedReq  Counter64,
    tmnxVdoIfStatRTSvrRxHdRTReq      Counter64,
    tmnxVdoIfStatRTSvrRxHdFailedReq  Counter64,
    tmnxVdoIfStatRTSvrRxPipRTReq     Counter64,
    tmnxVdoIfStatRTSvrRxPipFailedReq Counter64,
    tmnxVdoIfStatRTSvrTxSdRTReplies  Counter64,
    tmnxVdoIfStatRTSvrTxSdBytes      Counter64,
    tmnxVdoIfStatRTSvrTxSdPackets    Counter64,
    tmnxVdoIfStatRTSvrTxHdRTReplies  Counter64,
    tmnxVdoIfStatRTSvrTxHdBytes      Counter64,
    tmnxVdoIfStatRTSvrTxHdPackets    Counter64,
    tmnxVdoIfStatRTSvrTxPipRTReplies Counter64,
    tmnxVdoIfStatRTSvrTxPipBytes     Counter64,
    tmnxVdoIfStatRTSvrTxPipPackets   Counter64,
    tmnxVdoIfStatHdFCCServerMode     TmnxVdoFccServerMode,
    tmnxVdoIfStatSdFCCServerMode     TmnxVdoFccServerMode,
    tmnxVdoIfStatPipFCCServerMode    TmnxVdoFccServerMode,
    tmnxVdoIfStatFCCSrRxSdFCCReq     Counter64,
    tmnxVdoIfStatFCCSrRxSdFailedReq  Counter64,
    tmnxVdoIfStatFCCSrRxHdFCCReq     Counter64,
    tmnxVdoIfStatFCCSrRxHdFailedReq  Counter64,
    tmnxVdoIfStatFCCSrRxPipFCCReq    Counter64,
    tmnxVdoIfStatFCCSrRxPipFailedReq Counter64,
    tmnxVdoIfStatFCCSrTxSdFCCReplies Counter64,
    tmnxVdoIfStatFCCSrTxSdBytes      Counter64,
    tmnxVdoIfStatFCCSrTxSdPackets    Counter64,
    tmnxVdoIfStatFCCSrTxHdFCCReplies Counter64,
    tmnxVdoIfStatFCCSrTxHdBytes      Counter64,
    tmnxVdoIfStatFCCSrTxHdPackets    Counter64,
    tmnxVdoIfStatFCCSrTxPipFCCRplies Counter64,
    tmnxVdoIfStatFCCSrTxPipBytes     Counter64,
    tmnxVdoIfStatFCCSrTxPipPackets   Counter64,
    tmnxVdoIfStatTxFailedPackets     Counter64,
    tmnxVdoIfScte30TcpSessions       Counter32,
    tmnxVdoIfScte30InitSessions      Counter32,
    tmnxVdoIfStatRTSSdMcRdPktsReq    Counter64,
    tmnxVdoIfStatRTSSdMcRdPktsReqL32 Counter32,
    tmnxVdoIfStatRTSSdMcRdPktsReqH32 Counter32,
    tmnxVdoIfStatRTSHDMcRdPktsReq    Counter64,
    tmnxVdoIfStatRTSHDMcRdPktsReqL32 Counter32,
    tmnxVdoIfStatRTSHDMcRdPktsReqH32 Counter32,
    tmnxVdoIfStatRTSPipMcRdPktReq    Counter64,
    tmnxVdoIfStatRTSPipMcRdPktReqL32 Counter32,
    tmnxVdoIfStatRTSPipMcRdPktReqH32 Counter32,
    tmnxVdoIfStatSDPktLostInSeq10    Counter32,
    tmnxVdoIfStatSDPktLostInSeq20    Counter32,
    tmnxVdoIfStatSDPktLostInSeq30    Counter32,
    tmnxVdoIfStatSDPktLostInSeq40    Counter32,
    tmnxVdoIfStatSDPktLostInSeqMore  Counter32,
    tmnxVdoIfStatHDPktLostInSeq10    Counter32,
    tmnxVdoIfStatHDPktLostInSeq20    Counter32,
    tmnxVdoIfStatHDPktLostInSeq30    Counter32,
    tmnxVdoIfStatHDPktLostInSeq40    Counter32,
    tmnxVdoIfStatHDPktLostInSeqMore  Counter32,
    tmnxVdoIfStatPipPktLostInSeq10   Counter32,
    tmnxVdoIfStatPipPktLostInSeq20   Counter32,
    tmnxVdoIfStatPipPktLostInSeq30   Counter32,
    tmnxVdoIfStatPipPktLostInSeq40   Counter32,
    tmnxVdoIfStatPipPktLostInSeqMore Counter32
}

tmnxVdoIfStatHdRTServerState     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatHdRTServerState indicates whether the High
         Definition (HD) retransmission server is enabled on this interface."
    ::= { tmnxVdoIfStatEntry 1 }

tmnxVdoIfStatSdRTServerState     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatSdRTServerState indicates whether the
         Standard Definition (SD) retransmission server is enabled on this
         interface."
    ::= { tmnxVdoIfStatEntry 2 }

tmnxVdoIfStatPipRTServerState    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatPipRTServerState indicates whether the
         Picture-in-Picture (PIP) retransmission server is enabled on this
         interface."
    ::= { tmnxVdoIfStatEntry 3 }

tmnxVdoIfStatRTSvrSdRtpPktsReq   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrSdRtpPktsReq indicates the total number
         of Standard Definition (SD) channel Real-time Transport Protocol (RTP)
         packets requested in the Real-time Transport Control Protocol (RTCP)
         feedback (FB) messages received on this interface."
    ::= { tmnxVdoIfStatEntry 4 }

tmnxVdoIfStatRTSvrHdRtpPktsReq   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrHdRtpPktsReq indicates the total number
         of High Definition (HD) channel Real-time Transport Protocol (RTP)
         packets requested in the Real-time Transport Control Protocol (RTCP)
         feedback (FB) messages received on this interface."
    ::= { tmnxVdoIfStatEntry 5 }

tmnxVdoIfStatRTSvrPipRtpPktsReq  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrPipRtpPktsReq indicates the total
         number of Picture-In-Picture (PIP) channel Real-time Transport
         Protocol (RTP) packets requested in the Real-time Transport Control
         Protocol (RTCP) feedback (FB) messages received on this interface."
    ::= { tmnxVdoIfStatEntry 6 }

tmnxVdoIfStatRTSvrRxSdRTReq      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrRxSdRTReq indicates the total number of
         Retransmission (RT) requests received from Standard Definition (SD)
         channels on this interface."
    ::= { tmnxVdoIfStatEntry 7 }

tmnxVdoIfStatRTSvrRxSdFailedReq  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrRxSdFailedReq indicates the total
         number of failed Retransmission (RT) requests received from Standard
         Definition (SD) channels on this interface."
    ::= { tmnxVdoIfStatEntry 8 }

tmnxVdoIfStatRTSvrRxHdRTReq      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrRxHdRTReq indicates the total number of
         Retransmission (RT) requests received from High Definition (HD)
         channels on this interface."
    ::= { tmnxVdoIfStatEntry 9 }

tmnxVdoIfStatRTSvrRxHdFailedReq  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrRxHdFailedReq indicates the total
         number of failed Retransmission (RT) requests received from High
         Definition (HD) channels on this interface."
    ::= { tmnxVdoIfStatEntry 10 }

tmnxVdoIfStatRTSvrRxPipRTReq     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrRxPipRTReq indicates the total number
         of Retransmission (RT) requests received from Picture-In-Picture (PIP)
         channels on this interface."
    ::= { tmnxVdoIfStatEntry 11 }

tmnxVdoIfStatRTSvrRxPipFailedReq OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrRxPipFailedReq indicates the total
         number of failed Retransmission (RT) requests received from
         Picture-In-Picture (PIP) channels on this interface."
    ::= { tmnxVdoIfStatEntry 12 }

tmnxVdoIfStatRTSvrTxSdRTReplies  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrTxSdRTReplies indicates the total
         number of Standard Definition (SD) channel Retransmission (RT) replies
         sent from this interface."
    ::= { tmnxVdoIfStatEntry 13 }

tmnxVdoIfStatRTSvrTxSdBytes      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrTxSdBytes indicates the total number of
         Standard Definition (SD) channel bytes sent from this interface."
    ::= { tmnxVdoIfStatEntry 14 }

tmnxVdoIfStatRTSvrTxSdPackets    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrTxSdPackets indicates the total number
         of Standard Definition (SD) channel packets sent from this interface."
    ::= { tmnxVdoIfStatEntry 15 }

tmnxVdoIfStatRTSvrTxHdRTReplies  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrTxHdRTReplies indicates the total
         number of High Definition (HD) channel Retransmission (RT) replies
         sent from this interface."
    ::= { tmnxVdoIfStatEntry 16 }

tmnxVdoIfStatRTSvrTxHdBytes      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrTxHdBytes indicates the total number of
         High Definition (HD) channel bytes sent from this interface."
    ::= { tmnxVdoIfStatEntry 17 }

tmnxVdoIfStatRTSvrTxHdPackets    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrTxHdPackets indicates the total number
         of High Definition (HD) channel packets sent from this interface."
    ::= { tmnxVdoIfStatEntry 18 }

tmnxVdoIfStatRTSvrTxPipRTReplies OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrTxPipRTReplies indicates the total
         number of Picture-In-Picture (PIP) channel Retransmission (RT) replies
         sent from this interface."
    ::= { tmnxVdoIfStatEntry 19 }

tmnxVdoIfStatRTSvrTxPipBytes     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrTxPipBytes indicates the total number
         of Picture-In-Picture (PIP) channel bytes sent from this interface."
    ::= { tmnxVdoIfStatEntry 20 }

tmnxVdoIfStatRTSvrTxPipPackets   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSvrTxPipPackets indicates the total number
         of Picture-In-Picture (PIP) channel packets sent from this interface."
    ::= { tmnxVdoIfStatEntry 21 }

tmnxVdoIfStatHdFCCServerMode     OBJECT-TYPE
    SYNTAX      TmnxVdoFccServerMode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatHdFCCServerMode indicates the mode of the
         High Definition (HD) Fast Channel Change (FCC) server on this
         interface."
    ::= { tmnxVdoIfStatEntry 22 }

tmnxVdoIfStatSdFCCServerMode     OBJECT-TYPE
    SYNTAX      TmnxVdoFccServerMode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatSdFCCServerMode indicates the mode of the
         Standard Definition (SD) Fast Channel Change (FCC) server on this
         interface."
    ::= { tmnxVdoIfStatEntry 23 }

tmnxVdoIfStatPipFCCServerMode    OBJECT-TYPE
    SYNTAX      TmnxVdoFccServerMode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatPipFCCServerMode indicates the mode of the
         Picture-in-Picture (PIP) Fast Channel Change (FCC) server on this
         interface."
    ::= { tmnxVdoIfStatEntry 24 }

tmnxVdoIfStatFCCSrRxSdFCCReq     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrRxSdFCCReq indicates the total number
         of Fast Channel Change (FCC) requests received from Standard
         Definition (SD) channels on this interface."
    ::= { tmnxVdoIfStatEntry 25 }

tmnxVdoIfStatFCCSrRxSdFailedReq  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrRxSdFailedReq indicates the total
         number of failed Fast Channel Change (FCC) requests received from
         Standard Definition (SD) channels on this interface."
    ::= { tmnxVdoIfStatEntry 26 }

tmnxVdoIfStatFCCSrRxHdFCCReq     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrRxHdFCCReq indicates the total number
         of Fast Channel Change (FCC) requests received from High Definition
         (HD) channels on this interface."
    ::= { tmnxVdoIfStatEntry 27 }

tmnxVdoIfStatFCCSrRxHdFailedReq  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrRxHdFailedReq indicates the total
         number of failed Fast Channel Change (FCC) requests received from High
         Definition (HD) channels on this interface."
    ::= { tmnxVdoIfStatEntry 28 }

tmnxVdoIfStatFCCSrRxPipFCCReq    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrRxPipFCCReq indicates the total number
         of Fast Channel Change (FCC) requests received from Picture-In-Picture
         (PIP) channels on this interface."
    ::= { tmnxVdoIfStatEntry 29 }

tmnxVdoIfStatFCCSrRxPipFailedReq OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrRxPipFailedReq indicates the total
         number of failed Fast Channel Change (FCC) requests received from
         Picture-In-Picture (PIP) channels on this interface."
    ::= { tmnxVdoIfStatEntry 30 }

tmnxVdoIfStatFCCSrTxSdFCCReplies OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrTxSdFCCReplies indicates the total
         number of Standard Definition (SD) channel Fast Channel Change (FCC)
         replies sent from this interface."
    ::= { tmnxVdoIfStatEntry 31 }

tmnxVdoIfStatFCCSrTxSdBytes      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrTxSdBytes indicates the total number of
         Standard Definition (SD) channel bytes sent from this interface."
    ::= { tmnxVdoIfStatEntry 32 }

tmnxVdoIfStatFCCSrTxSdPackets    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrTxSdPackets indicates the total number
         of Standard Definition (SD) channel packets sent from this interface."
    ::= { tmnxVdoIfStatEntry 33 }

tmnxVdoIfStatFCCSrTxHdFCCReplies OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrTxHdFCCReplies indicates the total
         number of High Definition (HD) channel Fast Channel Change (FCC)
         replies sent from this interface."
    ::= { tmnxVdoIfStatEntry 34 }

tmnxVdoIfStatFCCSrTxHdBytes      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrTxHdBytes indicates the total number of
         High Definition (HD) channel bytes sent from this interface."
    ::= { tmnxVdoIfStatEntry 35 }

tmnxVdoIfStatFCCSrTxHdPackets    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrTxHdPackets indicates the total number
         of High Definition (HD) channel packets sent from this interface."
    ::= { tmnxVdoIfStatEntry 36 }

tmnxVdoIfStatFCCSrTxPipFCCRplies OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrTxPipFCCRplies indicates the total
         number of Picture-In-Picture (PIP) channel Fast Channel Change (FCC)
         replies sent from this interface."
    ::= { tmnxVdoIfStatEntry 37 }

tmnxVdoIfStatFCCSrTxPipBytes     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrTxPipBytes indicates the total number
         of Picture-In-Picture (PIP) channel bytes sent from this interface."
    ::= { tmnxVdoIfStatEntry 38 }

tmnxVdoIfStatFCCSrTxPipPackets   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatFCCSrTxPipPackets indicates the total number
         of Picture-In-Picture (PIP) channel packets sent from this interface."
    ::= { tmnxVdoIfStatEntry 39 }

tmnxVdoIfStatTxFailedPackets     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatTxFailedPackets indicates the total number
         of failures during the transmission of packets from this video
         interface. Failure happens when the packet to be sent is not stored in
         the video cache."
    ::= { tmnxVdoIfStatEntry 40 }

tmnxVdoIfScte30TcpSessions       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfScte30TcpSessions indicates the total number of
         scte30 tcp sessions with the Ad Insert (ADI) servers for this
         interface.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoIfStatEntry 41 }

tmnxVdoIfScte30InitSessions      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfScte30InitSessions indicates the total number of
         scte30 init sessions with the Ad Insert (ADI) servers for this
         interface.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoIfStatEntry 42 }

tmnxVdoIfStatRTSSdMcRdPktsReq    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSSdMcRdPktsReq indicates the total number
         of multicast retransmission requests created for Standard Definition
         (SD) channels on this interface."
    ::= { tmnxVdoIfStatEntry 43 }

tmnxVdoIfStatRTSSdMcRdPktsReqL32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSSdMcRdPktsReqL32 indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSSdMcRdPktsReq."
    ::= { tmnxVdoIfStatEntry 44 }

tmnxVdoIfStatRTSSdMcRdPktsReqH32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSSdMcRdPktsReqH32 indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSSdMcRdPktsReq."
    ::= { tmnxVdoIfStatEntry 45 }

tmnxVdoIfStatRTSHDMcRdPktsReq    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSHDMcRdPktsReq indicates the total
         number of multicast retransmission requests created for High Definition
          (HD) channels on this interface."
    ::= { tmnxVdoIfStatEntry 46 }

tmnxVdoIfStatRTSHDMcRdPktsReqL32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSHDMcRdPktsReqL32 indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSHDMcRdPktsReq."
    ::= { tmnxVdoIfStatEntry 47 }

tmnxVdoIfStatRTSHDMcRdPktsReqH32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSHDMcRdPktsReqH32 indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSHDMcRdPktsReq."
    ::= { tmnxVdoIfStatEntry 48 }

tmnxVdoIfStatRTSPipMcRdPktReq    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSPipMcRdPktReq indicates the total number
         of multicast retransmission requests created for Picture-In-Picture
         (PIP) channels on this interface."
    ::= { tmnxVdoIfStatEntry 49 }

tmnxVdoIfStatRTSPipMcRdPktReqL32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSPipMcRdPktReqL32 indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSPipMcRdPktReq."
    ::= { tmnxVdoIfStatEntry 50 }

tmnxVdoIfStatRTSPipMcRdPktReqH32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatRTSPipMcRdPktReqH32 indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSPipMcRdPktReq."
    ::= { tmnxVdoIfStatEntry 51 }

tmnxVdoIfStatSDPktLostInSeq10    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatSDPktLostInSeq10 indicates the total number
         of packets within sequences of 2 to 10 consecutive lost packets for
         Standard Definition (SD) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 52 }

tmnxVdoIfStatSDPktLostInSeq20    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatSDPktLostInSeq20 indicates the total number
         of packets within sequences of 11 to 20 consecutive lost packets for
         Standard Definition (SD) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 53 }

tmnxVdoIfStatSDPktLostInSeq30    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatSDPktLostInSeq30 indicates the total number
         of packets within sequences of 21 to 30 consecutive lost packets for
         Standard Definition (SD) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 54 }

tmnxVdoIfStatSDPktLostInSeq40    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatSDPktLostInSeq40 indicates the total number
         of packets within sequences of 31 to 40 consecutive lost packets for
         Standard Definition (SD) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 55 }

tmnxVdoIfStatSDPktLostInSeqMore  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatSDPktLostInSeqMore indicates the total
         number of packets within sequences of 41 or more consecutive lost
         packets for Standard Definition (SD) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 56 }

tmnxVdoIfStatHDPktLostInSeq10    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatHDPktLostInSeq10 indicates the total number
         of packets within sequences of 2 to 10 consecutive lost packets for
         High Definition (HD) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 57 }

tmnxVdoIfStatHDPktLostInSeq20    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatHDPktLostInSeq20 indicates the total number
         of packets within sequences of 11 to 20 consecutive lost packets for
         High Definition (HD) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 58 }

tmnxVdoIfStatHDPktLostInSeq30    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatHDPktLostInSeq30 indicates the total number
         of packets within sequences of 21 to 30 consecutive lost packets for
         High Definition (HD) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 59 }

tmnxVdoIfStatHDPktLostInSeq40    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatHDPktLostInSeq40 indicates the total number
         of packets within sequences of 31 to 40 consecutive lost packets for
         High Definition (HD) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 60 }

tmnxVdoIfStatHDPktLostInSeqMore  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatHDPktLostInSeqMore indicates the total number
         of packets within sequences of 41 or more consecutive lost packets for
         High Definition (HD)  channels on this video interface."
    ::= { tmnxVdoIfStatEntry 61 }

tmnxVdoIfStatPipPktLostInSeq10   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatPipPktLostInSeq10 indicates the total number
         of packets within sequences of 2 to 10 consecutive lost packets for
         Picture-In-Picture (PIP) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 62 }

tmnxVdoIfStatPipPktLostInSeq20   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatPipPktLostInSeq20 indicates the total number
         of packets within sequences of 11 to 20 consecutive lost packets for
         Picture-In-Picture (PIP) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 63 }

tmnxVdoIfStatPipPktLostInSeq30   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatPipPktLostInSeq30 indicates the total number
         of packets within sequences of 21 to 30 consecutive lost packets for
         Picture-In-Picture (PIP) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 64 }

tmnxVdoIfStatPipPktLostInSeq40   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatPipPktLostInSeq40 indicates the total number
         of packets within sequences of 31 to 40 consecutive lost packets for
         Picture-In-Picture (PIP) channels on this video interface."
    ::= { tmnxVdoIfStatEntry 65 }

tmnxVdoIfStatPipPktLostInSeqMore OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatPipPktLostInSeqMore indicates the total number
         of packets within sequences of 41 or more consecutive lost packets for
         Picture-In-Picture (PIP)  channels on this video interface."
    ::= { tmnxVdoIfStatEntry 66 }

tmnxVdoIfStLowTable              OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoIfStLowEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxVdoIfStLowTable contains information and statistics for each
         video interface configured in the system."
    ::= { tmnxVdoObjs 11 }

tmnxVdoIfStLowEntry              OBJECT-TYPE
    SYNTAX      TmnxVdoIfStLowEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoIfStLowTable containing video interface
         statistics.

         The counters in this table are defined as 32-bit entries which hold
         the lower 32 bits of the 64-bit counter values in tmnxVdoIfStatTable."
    AUGMENTS    { tmnxVdoIfAddrEntry }
    ::= { tmnxVdoIfStLowTable 1 }

TmnxVdoIfStLowEntry              ::= SEQUENCE
{
    tmnxVdoIfStLowRTSvrSdRtpPktsReq  Counter32,
    tmnxVdoIfStLowRTSvrHdRtpPktsReq  Counter32,
    tmnxVdoIfStLowRTSvrPipRtpPktsReq Counter32,
    tmnxVdoIfStLowRTSvrRxSdRTReq     Counter32,
    tmnxVdoIfStLowRTSvrRxSdFailedReq Counter32,
    tmnxVdoIfStLowRTSvrRxHdRTReq     Counter32,
    tmnxVdoIfStLowRTSvrRxHdFailedReq Counter32,
    tmnxVdoIfStLowRTSvrRxPipRTReq    Counter32,
    tmnxVdoIfStLowRTSvrRxPipFailedRq Counter32,
    tmnxVdoIfStLowRTSvrTxSdRTReplies Counter32,
    tmnxVdoIfStLowRTSvrTxSdBytes     Counter32,
    tmnxVdoIfStLowRTSvrTxSdPackets   Counter32,
    tmnxVdoIfStLowRTSvrTxHdRTReplies Counter32,
    tmnxVdoIfStLowRTSvrTxHdBytes     Counter32,
    tmnxVdoIfStLowRTSvrTxHdPackets   Counter32,
    tmnxVdoIfStLowRTSvrTxPipRTReplis Counter32,
    tmnxVdoIfStLowRTSvrTxPipBytes    Counter32,
    tmnxVdoIfStLowRTSvrTxPipPackets  Counter32,
    tmnxVdoIfStLowFCCSrRxSdFCCReq    Counter32,
    tmnxVdoIfStLowFCCSrRxSdFailedReq Counter32,
    tmnxVdoIfStLowFCCSrRxHdFCCReq    Counter32,
    tmnxVdoIfStLowFCCSrRxHdFailedReq Counter32,
    tmnxVdoIfStLowFCCSrRxPipFCCReq   Counter32,
    tmnxVdoIfStLowFCCSrRxPipFailedRq Counter32,
    tmnxVdoIfStLowFCCSrTxSdFCCReplis Counter32,
    tmnxVdoIfStLowFCCSrTxSdBytes     Counter32,
    tmnxVdoIfStLowFCCSrTxSdPackets   Counter32,
    tmnxVdoIfStLowFCCSrTxHdFCCReplis Counter32,
    tmnxVdoIfStLowFCCSrTxHdBytes     Counter32,
    tmnxVdoIfStLowFCCSrTxHdPackets   Counter32,
    tmnxVdoIfStLowFCCSrTxPipFCCRplis Counter32,
    tmnxVdoIfStLowFCCSrTxPipBytes    Counter32,
    tmnxVdoIfStLowFCCSrTxPipPackets  Counter32,
    tmnxVdoIfStLowTxFailedPackets    Counter32
}

tmnxVdoIfStLowRTSvrSdRtpPktsReq  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrSdRtpPktsReq indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrSdRtpPktsReq."
    ::= { tmnxVdoIfStLowEntry 1 }

tmnxVdoIfStLowRTSvrHdRtpPktsReq  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrHdRtpPktsReq indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrHdRtpPktsReq."
    ::= { tmnxVdoIfStLowEntry 2 }

tmnxVdoIfStLowRTSvrPipRtpPktsReq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrPipRtpPktsReq indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrPipRtpPktsReq."
    ::= { tmnxVdoIfStLowEntry 3 }

tmnxVdoIfStLowRTSvrRxSdRTReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrRxSdRTReq indicates the lower 32 bits
         of the value of tmnxVdoIfStatRTSvrRxSdRTReq."
    ::= { tmnxVdoIfStLowEntry 4 }

tmnxVdoIfStLowRTSvrRxSdFailedReq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrRxSdFailedReq indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrRxSdFailedReq."
    ::= { tmnxVdoIfStLowEntry 5 }

tmnxVdoIfStLowRTSvrRxHdRTReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrRxHdRTReq indicates the lower 32 bits
         of the value of tmnxVdoIfStatRTSvrRxHdRTReq."
    ::= { tmnxVdoIfStLowEntry 6 }

tmnxVdoIfStLowRTSvrRxHdFailedReq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrRxHdFailedReq indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrRxHdFailedReq."
    ::= { tmnxVdoIfStLowEntry 7 }

tmnxVdoIfStLowRTSvrRxPipRTReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrRxPipRTReq indicates the lower 32 bits
         of the value of tmnxVdoIfStatRTSvrRxPipRTReq."
    ::= { tmnxVdoIfStLowEntry 8 }

tmnxVdoIfStLowRTSvrRxPipFailedRq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrRxPipFailedRq indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrRxPipFailedReq."
    ::= { tmnxVdoIfStLowEntry 9 }

tmnxVdoIfStLowRTSvrTxSdRTReplies OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrTxSdRTReplies indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrTxSdRTReplies."
    ::= { tmnxVdoIfStLowEntry 10 }

tmnxVdoIfStLowRTSvrTxSdBytes     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrTxSdBytes indicates the lower 32 bits
         of the value of tmnxVdoIfStatRTSvrTxSdBytes."
    ::= { tmnxVdoIfStLowEntry 11 }

tmnxVdoIfStLowRTSvrTxSdPackets   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrTxSdPackets indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrTxSdPackets."
    ::= { tmnxVdoIfStLowEntry 12 }

tmnxVdoIfStLowRTSvrTxHdRTReplies OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrTxHdRTReplies indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrTxHdRTReplies."
    ::= { tmnxVdoIfStLowEntry 13 }

tmnxVdoIfStLowRTSvrTxHdBytes     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrTxHdBytes indicates the lower 32 bits
         of the value of tmnxVdoIfStatRTSvrTxHdBytes."
    ::= { tmnxVdoIfStLowEntry 14 }

tmnxVdoIfStLowRTSvrTxHdPackets   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrTxHdPackets indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrTxHdPackets."
    ::= { tmnxVdoIfStLowEntry 15 }

tmnxVdoIfStLowRTSvrTxPipRTReplis OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrTxPipRTReplis indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrTxPipRTReplies."
    ::= { tmnxVdoIfStLowEntry 16 }

tmnxVdoIfStLowRTSvrTxPipBytes    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrTxPipBytes indicates the lower 32 bits
         of the value of tmnxVdoIfStatRTSvrTxPipBytes."
    ::= { tmnxVdoIfStLowEntry 17 }

tmnxVdoIfStLowRTSvrTxPipPackets  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowRTSvrTxPipPackets indicates the lower 32
         bits of the value of tmnxVdoIfStatRTSvrTxPipPackets."
    ::= { tmnxVdoIfStLowEntry 18 }

tmnxVdoIfStLowFCCSrRxSdFCCReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrRxSdFCCReq indicates the lower 32 bits
         of the value of tmnxVdoIfStatFCCSrRxSdFCCReq."
    ::= { tmnxVdoIfStLowEntry 19 }

tmnxVdoIfStLowFCCSrRxSdFailedReq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrRxSdFailedReq indicates the lower 32
         bits of the value of tmnxVdoIfStatFCCSrRxSdFailedReq."
    ::= { tmnxVdoIfStLowEntry 20 }

tmnxVdoIfStLowFCCSrRxHdFCCReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrRxHdFCCReq indicates the lower 32 bits
         of the value of tmnxVdoIfStatFCCSrRxHdFCCReq."
    ::= { tmnxVdoIfStLowEntry 21 }

tmnxVdoIfStLowFCCSrRxHdFailedReq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrRxHdFailedReq indicates the lower 32
         bits of the value of tmnxVdoIfStatFCCSrRxHdFailedReq."
    ::= { tmnxVdoIfStLowEntry 22 }

tmnxVdoIfStLowFCCSrRxPipFCCReq   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrRxPipFCCReq indicates the lower 32
         bits of the value of tmnxVdoIfStatFCCSrRxPipFCCReq."
    ::= { tmnxVdoIfStLowEntry 23 }

tmnxVdoIfStLowFCCSrRxPipFailedRq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrRxPipFailedRq indicates the lower 32
         bits of the value of tmnxVdoIfStatFCCSrRxPipFailedReq."
    ::= { tmnxVdoIfStLowEntry 24 }

tmnxVdoIfStLowFCCSrTxSdFCCReplis OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrTxSdFCCReplis indicates the lower 32
         bits of the value of tmnxVdoIfStatFCCSrTxSdFCCReplies."
    ::= { tmnxVdoIfStLowEntry 25 }

tmnxVdoIfStLowFCCSrTxSdBytes     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrTxSdBytes indicates the lower 32 bits
         of the value of tmnxVdoIfStatFCCSrTxSdBytes."
    ::= { tmnxVdoIfStLowEntry 26 }

tmnxVdoIfStLowFCCSrTxSdPackets   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrTxSdPackets indicates the lower 32
         bits of the value of tmnxVdoIfStatFCCSrTxSdPackets."
    ::= { tmnxVdoIfStLowEntry 27 }

tmnxVdoIfStLowFCCSrTxHdFCCReplis OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrTxHdFCCReplis indicates the lower 32
         bits of the value of tmnxVdoIfStatFCCSrTxHdFCCReplies."
    ::= { tmnxVdoIfStLowEntry 28 }

tmnxVdoIfStLowFCCSrTxHdBytes     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrTxHdBytes indicates the lower 32 bits
         of the value of tmnxVdoIfStatFCCSrTxHdBytes."
    ::= { tmnxVdoIfStLowEntry 29 }

tmnxVdoIfStLowFCCSrTxHdPackets   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrTxHdPackets indicates the lower 32
         bits of the value of tmnxVdoIfStatFCCSrTxHdPackets."
    ::= { tmnxVdoIfStLowEntry 30 }

tmnxVdoIfStLowFCCSrTxPipFCCRplis OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrTxPipFCCRplis indicates the lower 32
         bits of the value of tmnxVdoIfStatFCCSrTxPipFCCRplies."
    ::= { tmnxVdoIfStLowEntry 31 }

tmnxVdoIfStLowFCCSrTxPipBytes    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrTxPipBytes indicates the lower 32 bits
         of the value of tmnxVdoIfStatFCCSrTxPipBytes."
    ::= { tmnxVdoIfStLowEntry 32 }

tmnxVdoIfStLowFCCSrTxPipPackets  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowFCCSrTxPipPackets indicates the lower 32
         bits of the value of tmnxVdoIfStatFCCSrTxPipPackets."
    ::= { tmnxVdoIfStLowEntry 33 }

tmnxVdoIfStLowTxFailedPackets    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStLowTxFailedPackets indicates the lower 32 bits
         of the value of tmnxVdoIfStatTxFailedPackets."
    ::= { tmnxVdoIfStLowEntry 34 }

tmnxVdoIfStHghTable              OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoIfStHghEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxVdoIfStLowTable contains information and statistics for each
         video interface configured in the system."
    ::= { tmnxVdoObjs 12 }

tmnxVdoIfStHghEntry              OBJECT-TYPE
    SYNTAX      TmnxVdoIfStHghEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoIfStLowTable containing video interface
         statistics.

         The counters in this table are defined as 32-bit entries which hold
         the higher 32 bits of the 64-bit counter values in tmnxVdoIfStatTable."
    AUGMENTS    { tmnxVdoIfAddrEntry }
    ::= { tmnxVdoIfStHghTable 1 }

TmnxVdoIfStHghEntry              ::= SEQUENCE
{
    tmnxVdoIfStHghRTSvrSdRtpPktsReq  Counter32,
    tmnxVdoIfStHghRTSvrHdRtpPktsReq  Counter32,
    tmnxVdoIfStHghRTSvrPipRtpPktsReq Counter32,
    tmnxVdoIfStHghRTSvrRxSdRTReq     Counter32,
    tmnxVdoIfStHghRTSvrRxSdFailedReq Counter32,
    tmnxVdoIfStHghRTSvrRxHdRTReq     Counter32,
    tmnxVdoIfStHghRTSvrRxHdFailedReq Counter32,
    tmnxVdoIfStHghRTSvrRxPipRTReq    Counter32,
    tmnxVdoIfStHghRTSvrRxPipFailedRq Counter32,
    tmnxVdoIfStHghRTSvrTxSdRTReplies Counter32,
    tmnxVdoIfStHghRTSvrTxSdBytes     Counter32,
    tmnxVdoIfStHghRTSvrTxSdPackets   Counter32,
    tmnxVdoIfStHghRTSvrTxHdRTReplies Counter32,
    tmnxVdoIfStHghRTSvrTxHdBytes     Counter32,
    tmnxVdoIfStHghRTSvrTxHdPackets   Counter32,
    tmnxVdoIfStHghRTSvrTxPipRTReplis Counter32,
    tmnxVdoIfStHghRTSvrTxPipBytes    Counter32,
    tmnxVdoIfStHghRTSvrTxPipPackets  Counter32,
    tmnxVdoIfStHghFCCSrRxSdFCCReq    Counter32,
    tmnxVdoIfStHghFCCSrRxSdFailedReq Counter32,
    tmnxVdoIfStHghFCCSrRxHdFCCReq    Counter32,
    tmnxVdoIfStHghFCCSrRxHdFailedReq Counter32,
    tmnxVdoIfStHghFCCSrRxPipFCCReq   Counter32,
    tmnxVdoIfStHghFCCSrRxPipFailedRq Counter32,
    tmnxVdoIfStHghFCCSrTxSdFCCReplis Counter32,
    tmnxVdoIfStHghFCCSrTxSdBytes     Counter32,
    tmnxVdoIfStHghFCCSrTxSdPackets   Counter32,
    tmnxVdoIfStHghFCCSrTxHdFCCReplis Counter32,
    tmnxVdoIfStHghFCCSrTxHdBytes     Counter32,
    tmnxVdoIfStHghFCCSrTxHdPackets   Counter32,
    tmnxVdoIfStHghFCCSrTxPipFCCRplis Counter32,
    tmnxVdoIfStHghFCCSrTxPipBytes    Counter32,
    tmnxVdoIfStHghFCCSrTxPipPackets  Counter32,
    tmnxVdoIfStHghTxFailedPackets    Counter32
}

tmnxVdoIfStHghRTSvrSdRtpPktsReq  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrSdRtpPktsReq indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrSdRtpPktsReq."
    ::= { tmnxVdoIfStHghEntry 1 }

tmnxVdoIfStHghRTSvrHdRtpPktsReq  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrHdRtpPktsReq indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrHdRtpPktsReq."
    ::= { tmnxVdoIfStHghEntry 2 }

tmnxVdoIfStHghRTSvrPipRtpPktsReq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrPipRtpPktsReq indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrPipRtpPktsReq."
    ::= { tmnxVdoIfStHghEntry 3 }

tmnxVdoIfStHghRTSvrRxSdRTReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrRxSdRTReq indicates the higher 32 bits
         of the value of tmnxVdoIfStatRTSvrRxSdRTReq."
    ::= { tmnxVdoIfStHghEntry 4 }

tmnxVdoIfStHghRTSvrRxSdFailedReq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrRxSdFailedReq indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrRxSdFailedReq."
    ::= { tmnxVdoIfStHghEntry 5 }

tmnxVdoIfStHghRTSvrRxHdRTReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrRxHdRTReq indicates the higher 32 bits
         of the value of tmnxVdoIfStatRTSvrRxHdRTReq."
    ::= { tmnxVdoIfStHghEntry 6 }

tmnxVdoIfStHghRTSvrRxHdFailedReq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrRxHdFailedReq indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrRxHdFailedReq."
    ::= { tmnxVdoIfStHghEntry 7 }

tmnxVdoIfStHghRTSvrRxPipRTReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrRxPipRTReq indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrRxPipRTReq."
    ::= { tmnxVdoIfStHghEntry 8 }

tmnxVdoIfStHghRTSvrRxPipFailedRq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrRxPipFailedRq indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrRxPipFailedReq."
    ::= { tmnxVdoIfStHghEntry 9 }

tmnxVdoIfStHghRTSvrTxSdRTReplies OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrTxSdRTReplies indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrTxSdRTReplies."
    ::= { tmnxVdoIfStHghEntry 10 }

tmnxVdoIfStHghRTSvrTxSdBytes     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrTxSdBytes indicates the higher 32 bits
         of the value of tmnxVdoIfStatRTSvrTxSdBytes."
    ::= { tmnxVdoIfStHghEntry 11 }

tmnxVdoIfStHghRTSvrTxSdPackets   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrTxSdPackets indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrTxSdPackets."
    ::= { tmnxVdoIfStHghEntry 12 }

tmnxVdoIfStHghRTSvrTxHdRTReplies OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrTxHdRTReplies indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrTxHdRTReplies."
    ::= { tmnxVdoIfStHghEntry 13 }

tmnxVdoIfStHghRTSvrTxHdBytes     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrTxHdBytes indicates the higher 32 bits
         of the value of tmnxVdoIfStatRTSvrTxHdBytes."
    ::= { tmnxVdoIfStHghEntry 14 }

tmnxVdoIfStHghRTSvrTxHdPackets   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrTxHdPackets indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrTxHdPackets."
    ::= { tmnxVdoIfStHghEntry 15 }

tmnxVdoIfStHghRTSvrTxPipRTReplis OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrTxPipRTReplis indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrTxPipRTReplies."
    ::= { tmnxVdoIfStHghEntry 16 }

tmnxVdoIfStHghRTSvrTxPipBytes    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrTxPipBytes indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrTxPipBytes."
    ::= { tmnxVdoIfStHghEntry 17 }

tmnxVdoIfStHghRTSvrTxPipPackets  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghRTSvrTxPipPackets indicates the higher 32
         bits of the value of tmnxVdoIfStatRTSvrTxPipPackets."
    ::= { tmnxVdoIfStHghEntry 18 }

tmnxVdoIfStHghFCCSrRxSdFCCReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrRxSdFCCReq indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrRxSdFCCReq."
    ::= { tmnxVdoIfStHghEntry 19 }

tmnxVdoIfStHghFCCSrRxSdFailedReq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrRxSdFailedReq indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrRxSdFailedReq."
    ::= { tmnxVdoIfStHghEntry 20 }

tmnxVdoIfStHghFCCSrRxHdFCCReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrRxHdFCCReq indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrRxHdFCCReq."
    ::= { tmnxVdoIfStHghEntry 21 }

tmnxVdoIfStHghFCCSrRxHdFailedReq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrRxHdFailedReq indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrRxHdFailedReq."
    ::= { tmnxVdoIfStHghEntry 22 }

tmnxVdoIfStHghFCCSrRxPipFCCReq   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrRxPipFCCReq indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrRxPipFCCReq."
    ::= { tmnxVdoIfStHghEntry 23 }

tmnxVdoIfStHghFCCSrRxPipFailedRq OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrRxPipFailedRq indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrRxPipFailedReq."
    ::= { tmnxVdoIfStHghEntry 24 }

tmnxVdoIfStHghFCCSrTxSdFCCReplis OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrTxSdFCCReplis indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrTxSdFCCReplies."
    ::= { tmnxVdoIfStHghEntry 25 }

tmnxVdoIfStHghFCCSrTxSdBytes     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrTxSdBytes indicates the higher 32 bits
         of the value of tmnxVdoIfStatFCCSrTxSdBytes."
    ::= { tmnxVdoIfStHghEntry 26 }

tmnxVdoIfStHghFCCSrTxSdPackets   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrTxSdPackets indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrTxSdPackets."
    ::= { tmnxVdoIfStHghEntry 27 }

tmnxVdoIfStHghFCCSrTxHdFCCReplis OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrTxHdFCCReplis indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrTxHdFCCReplies."
    ::= { tmnxVdoIfStHghEntry 28 }

tmnxVdoIfStHghFCCSrTxHdBytes     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrTxHdBytes indicates the higher 32 bits
         of the value of tmnxVdoIfStatFCCSrTxHdBytes."
    ::= { tmnxVdoIfStHghEntry 29 }

tmnxVdoIfStHghFCCSrTxHdPackets   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrTxHdPackets indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrTxHdPackets."
    ::= { tmnxVdoIfStHghEntry 30 }

tmnxVdoIfStHghFCCSrTxPipFCCRplis OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrTxPipFCCRplis indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrTxPipFCCRplies."
    ::= { tmnxVdoIfStHghEntry 31 }

tmnxVdoIfStHghFCCSrTxPipBytes    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrTxPipBytes indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrTxPipBytes."
    ::= { tmnxVdoIfStHghEntry 32 }

tmnxVdoIfStHghFCCSrTxPipPackets  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghFCCSrTxPipPackets indicates the higher 32
         bits of the value of tmnxVdoIfStatFCCSrTxPipPackets."
    ::= { tmnxVdoIfStHghEntry 33 }

tmnxVdoIfStHghTxFailedPackets    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStHghTxFailedPackets indicates the higher 32
         bits of the value of tmnxVdoIfStatTxFailedPackets."
    ::= { tmnxVdoIfStHghEntry 34 }

tmnxVdoPIDTable                  OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoPIDEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxVdoPIDTable contains information about the data in the Transport
         Stream."
    ::= { tmnxVdoObjs 13 }

tmnxVdoPIDEntry                  OBJECT-TYPE
    SYNTAX      TmnxVdoPIDEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoPIDTable. Each row entry represents a packet
         identifier used to identify the type of data stored in the packet
         payload."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoGrpSrcGrpAddrType,
        tmnxVdoGrpSrcGroupAddress,
        tmnxVdoGrpSrcSrcAddrType,
        tmnxVdoGrpSrcSourceAddress,
        tmnxVdoPID
    }
    ::= { tmnxVdoPIDTable 1 }

TmnxVdoPIDEntry                  ::= SEQUENCE
{
    tmnxVdoPID                       Unsigned32,
    tmnxVdoPIDType                   TmnxVdoPIDType,
    tmnxVdoPIDMpegStreamType         Unsigned32,
    tmnxVdoPIDLanguage               TNamedItem,
    tmnxVdoPIDCcErrSecs              Unsigned32,
    tmnxVdoPIDTeiErrSecs             Unsigned32,
    tmnxVdoPIDAbsentErrSecs          Unsigned32,
    tmnxVdoPIDBitrate                Unsigned32,
    tmnxVdoPIDIsPCR                  TruthValue
}

tmnxVdoPID                       OBJECT-TYPE
    SYNTAX      Unsigned32 (0..8191)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoPID indicates the 13-bit packet identifier used to
         identify the type of data stored in the packet payload."
    ::= { tmnxVdoPIDEntry 1 }

tmnxVdoPIDType                   OBJECT-TYPE
    SYNTAX      TmnxVdoPIDType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoPIDType indicates the type of the packet
         identifier."
    ::= { tmnxVdoPIDEntry 2 }

tmnxVdoPIDMpegStreamType         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoPIDMpegStreamType indicates the type of MPEG
         stream."
    ::= { tmnxVdoPIDEntry 3 }

tmnxVdoPIDLanguage               OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoPIDLanguage indicates the language of the MPEG
         stream."
    ::= { tmnxVdoPIDEntry 4 }

tmnxVdoPIDCcErrSecs              OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoPIDCcErrSecs indicates the total number of
         continuity counter error seconds for the MPEG stream."
    ::= { tmnxVdoPIDEntry 5 }

tmnxVdoPIDTeiErrSecs             OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoPIDTeiErrSecs indicates the total number of TEI
         (Transport Error Indicator) error seconds for the MPEG stream."
    ::= { tmnxVdoPIDEntry 6 }

tmnxVdoPIDAbsentErrSecs          OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoPIDAbsentErrSecs indicates the total number of
         video or non-video PID (Program Identifier) absent error seconds for
         the MPEG stream based on the PID type. This object has separate
         instances for each PID type within a video stream based on bundle,
         channel and source-override configurations. So for example if we have
         a bundle configured, we can count the absent errors on two different
         PID streams - video and non-video - of the bundle. In this case
         'TIMETRA-MCAST-PATH-MGMT-MIB:: tmnxMcPathBdlVdoVidPIDAbsent' sets the
         time duration in milliseconds, after every lapse of which the video
         PID instance of tmnxVdoPIDAbsentErrSecs updates itself to reflect the
         latest absent error count for the video PIDs for the bundle. Similarly
         we have 'TIMETRA-MCAST-PATH-MGMT-MIB::
         tmnxMcPathBdlVdoNonVidPIDAbsent' which sets the time duration in
         milliseconds, after every lapse of which the non-video PID instance of
         tmnxVdoPIDAbsentErrSecs updates itself to reflect the latest absent
         error count for non-video PIDs in the bundle. The above explanation
         can be extended to apply to channel and source-override video stream.
         Consequently we have 'TIMETRA-MCAST-PATH-MGMT-MIB::
         tmnxMcPathBdlChlVdoVidPIDAbs' and 'TIMETRA-MCAST-PATH-MGMT-MIB::
         tmnxMcPathBdlChlVdoNonVidPIDAbs' which set the time duration in
         milliseconds after every lapse of which the video and non-video PID
         instances of tmnxVdoPIDAbsentErrSecs for channel update themselves to
         reflect their respective latest absent error counts. In case of
         source-override configuration we have 'TIMETRA-MCAST-PATH-MGMT-MIB::
         tmnxMcPathChlSrcVdoVidPIDAbs' and 'TIMETRA-MCAST-PATH-MGMT-MIB::
         tmnxMcPathChlSrcVdoNonVidPIDAbs' which set the time duration in
         milliseconds, after every lapse of which its video and non-video PID
         instances of tmnxVdoPIDAbsentErrSecs for source-override update
         themselves to reflect their latest absent error counts."
    ::= { tmnxVdoPIDEntry 7 }

tmnxVdoPIDBitrate                OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoPIDBitrate indicates the bitrate of the stream."
    ::= { tmnxVdoPIDEntry 8 }

tmnxVdoPIDIsPCR                  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoPIDIsPCR indicates whether or not this is a
         Program Clock Reference(PCR) PID."
    ::= { tmnxVdoPIDEntry 9 }

tmnxVdoIfScte30AdSrvrTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoIfScte30AdSrvrEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The tmnxVdoIfScte30AdSrvrTable has an entry for each ad server IP
         address configured for the video interface in the system.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoObjs 14 }

tmnxVdoIfScte30AdSrvrEntry       OBJECT-TYPE
    SYNTAX      TmnxVdoIfScte30AdSrvrEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Each row entry represents an ad server IP address configured for the
         video interface in the system. Entries can be created and deleted by
         the user.

         This object was obsoleted in the 23.0 release."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoIfScte30AdSrvrAddrType,
        tmnxVdoIfScte30AdSrvrAddr
    }
    ::= { tmnxVdoIfScte30AdSrvrTable 1 }

TmnxVdoIfScte30AdSrvrEntry       ::= SEQUENCE
{
    tmnxVdoIfScte30AdSrvrAddrType    InetAddressType,
    tmnxVdoIfScte30AdSrvrAddr        InetAddress,
    tmnxVdoIfScte30AdSrvrRowStatus   RowStatus
}

tmnxVdoIfScte30AdSrvrAddrType    OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfScte30AdSrvrAddrType specifies the type of
         address represented by tmnxVdoIfScte30AdSrvrAddr.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoIfScte30AdSrvrEntry 1 }

tmnxVdoIfScte30AdSrvrAddr        OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfScte30AdSrvrAddr specifies the IP address of the
         ad server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoIfScte30AdSrvrEntry 2 }

tmnxVdoIfScte30AdSrvrRowStatus   OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoIfScte30AdSrvrRowStatus specifies the row status
         of this row. The row status is used for creation, deletion or control
         of tmnxVdoIfScte30AdSrvrTable entries.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoIfScte30AdSrvrEntry 3 }

tmnxVdoSGAdiStatTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoSGAdiStatEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The tmnxVdoSGAdiStatTable has an entry for each Ad Insert (ADI) server
         on the channel. This table contains ad server information and
         statistics.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoObjs 15 }

tmnxVdoSGAdiStatEntry            OBJECT-TYPE
    SYNTAX      TmnxVdoSGAdiStatEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "An entry in the tmnxVdoSGAdiStatTable. Each entry represents a Ad
         Insert (ADI) server for the corresponding multicast group.

         This object was obsoleted in the 23.0 release."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoGrpSrcGrpAddrType,
        tmnxVdoGrpSrcGroupAddress,
        tmnxVdoGrpSrcSrcAddrType,
        tmnxVdoGrpSrcSourceAddress,
        tmnxVdoSGAdiServerAddrType,
        tmnxVdoSGAdiServerAddr
    }
    ::= { tmnxVdoSGAdiStatTable 1 }

TmnxVdoSGAdiStatEntry            ::= SEQUENCE
{
    tmnxVdoSGAdiServerAddrType       InetAddressType,
    tmnxVdoSGAdiServerAddr           InetAddress,
    tmnxVdoSGAdiServerUptime         Unsigned32,
    tmnxVdoSGAdiInitReq              Counter32,
    tmnxVdoSGAdiSucInitResp          Counter32,
    tmnxVdoSGAdiUnsucInitResp        Counter32,
    tmnxVdoSGAdiAliveReq             Counter32,
    tmnxVdoSGAdiSucAliveResp         Counter32,
    tmnxVdoSGAdiUnSucAliveResp       Counter32,
    tmnxVdoSGAdiCueReq               Counter32,
    tmnxVdoSGAdiSucCueResp           Counter32,
    tmnxVdoSGAdiUnsucCueResp         Counter32,
    tmnxVdoSGAdiAbortReq             Counter32,
    tmnxVdoSGAdiSucAbortResp         Counter32,
    tmnxVdoSGAdiUnsucAbortResp       Counter32,
    tmnxVdoSGAdiUnknownSCTE30Req     Counter32,
    tmnxVdoSGAdiSpliceReq            Counter32,
    tmnxVdoSGAdiSucSpliceResp        Counter32,
    tmnxVdoSGAdiUnsucSpliceResp      Counter32,
    tmnxVdoSGAdiSucSpliceInCompResp  Counter32,
    tmnxVdoSGAdiSucSpliceOutCompResp Counter32,
    tmnxVdoSGAdiUnsucSpliceOutComRes Counter32,
    tmnxVdoSGAdiMinPort              Counter32,
    tmnxVdoSGAdiMaxPort              Counter32,
    tmnxVdoSGAdiChlName              TNamedItem
}

tmnxVdoSGAdiServerAddrType       OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiServerAddrType indicates the type of Ad
         Insert (ADI) server address represented by tmnxVdoSGAdiServerAddr.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 1 }

tmnxVdoSGAdiServerAddr           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiServerAddr indicates the address of Ad Insert
         (ADI) server on this channel.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 2 }

tmnxVdoSGAdiServerUptime         OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiServerUptime indicates the time in seconds
         since the connection with Ad Insert (ADI) server was established.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 3 }

tmnxVdoSGAdiInitReq              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiInitReq indicates the total number of init
         requests received from the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 4 }

tmnxVdoSGAdiSucInitResp          OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiSucInitResp indicates the total number of
         successful init responses sent to the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 5 }

tmnxVdoSGAdiUnsucInitResp        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiUnsucInitResp indicates the total number of
         unsuccessful init responses sent to the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 6 }

tmnxVdoSGAdiAliveReq             OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiAliveReq indicates the total number of alive
         messages received from the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 7 }

tmnxVdoSGAdiSucAliveResp         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiSucAliveResp indicates the total number of
         successful alive messages sent to the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 8 }

tmnxVdoSGAdiUnSucAliveResp       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiUnSucAliveResp indicates the total number of
         unsuccessful alive messages sent to the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 9 }

tmnxVdoSGAdiCueReq               OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiCueReq indicates the total number of total
         number of cue requests sent to the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 10 }

tmnxVdoSGAdiSucCueResp           OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiSucCueResp indicates the total number of
         successful cue responses received from the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 11 }

tmnxVdoSGAdiUnsucCueResp         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiUnsucCueResp indicates the total number of
         unsuccessful cue responses received from the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 12 }

tmnxVdoSGAdiAbortReq             OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiAbortReq indicates the total number of abort
         requests received from the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 13 }

tmnxVdoSGAdiSucAbortResp         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiSucAbortResp indicates the total number of
         successful abort responses sent to the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 14 }

tmnxVdoSGAdiUnsucAbortResp       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiUnsucAbortResp indicates the total number of
         unsuccessful abort responses sent to the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 15 }

tmnxVdoSGAdiUnknownSCTE30Req     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiUnknownSCTE30Req indicates the total number
         of invalid Society of Cable Telecommunications Engineers 30 (SCTE-30)
         requests received from the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 16 }

tmnxVdoSGAdiSpliceReq            OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiSpliceReq indicates the total number of
         splice requests received from the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 17 }

tmnxVdoSGAdiSucSpliceResp        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiSucSpliceResp indicates the total number of
         successful splice responses sent to the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 18 }

tmnxVdoSGAdiUnsucSpliceResp      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiUnsucSpliceResp indicates the total number of
         unsuccessful splice responses sent to the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 19 }

tmnxVdoSGAdiSucSpliceInCompResp  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiSucSpliceInCompResp indicates the total
         number of successful splice-in complete responses sent to the Ad
         Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 20 }

tmnxVdoSGAdiSucSpliceOutCompResp OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiSucSpliceOutCompResp indicates the total
         number of successful splice-out complete responses sent to the Ad
         Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 21 }

tmnxVdoSGAdiUnsucSpliceOutComRes OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiUnsucSpliceOutComRes indicates the total
         number of unsuccessful splice-out complete responses sent to the Ad
         Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 22 }

tmnxVdoSGAdiMinPort              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiMinPort indicates the minimum ip port number
         where the Ad Insert (ADI) server's insertion stream is connected.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 23 }

tmnxVdoSGAdiMaxPort              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiMaxPort indicates the maximum ip port number
         where the Ad Insert (ADI) server's insertion stream is connected.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 24 }

tmnxVdoSGAdiChlName              OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGAdiChlName indicates the channel name associated
         for this multicast group.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGAdiStatEntry 25 }

tmnxVdoSGSpliceStatusTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoSGSpliceStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The tmnxVdoSGSpliceStatusTable has an entry for each splice request
         received by the splicer. This table contains information about the
         splice request.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoObjs 16 }

tmnxVdoSGSpliceStatusEntry       OBJECT-TYPE
    SYNTAX      TmnxVdoSGSpliceStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "An entry in the tmnxVdoSGSpliceStatusEntry. Each entry represents a
         splice request received by the splicer.

         This object was obsoleted in the 23.0 release."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoGrpSrcGrpAddrType,
        tmnxVdoGrpSrcGroupAddress,
        tmnxVdoGrpSrcSrcAddrType,
        tmnxVdoGrpSrcSourceAddress,
        tmnxVdoSGSpliceStartTime
    }
    ::= { tmnxVdoSGSpliceStatusTable 1 }

TmnxVdoSGSpliceStatusEntry       ::= SEQUENCE
{
    tmnxVdoSGSpliceStartTime         Unsigned32,
    tmnxVdoSGSpliceAdServerAddrType  InetAddressType,
    tmnxVdoSGSpliceAdServerAddr      InetAddress,
    tmnxVdoSGSpliceStatus            INTEGER,
    tmnxVdoSGSpliceDurationReq       Unsigned32,
    tmnxVdoSGSpliceDurationPlayed    Unsigned32,
    tmnxVdoSGSpliceRate              Unsigned32,
    tmnxVdoSGSpliceSessionId         Unsigned32,
    tmnxVdoSGSplicePriorSessionId    Unsigned32,
    tmnxVdoSGSpliceAbortReason       INTEGER,
    tmnxVdoSGSpliceSpliceInSeqNum    Unsigned32,
    tmnxVdoSGSpliceSpliceOutSeqNum   Unsigned32,
    tmnxVdoSGSpliceNumBlkFrames      Unsigned32,
    tmnxVdoSGSpliceBlkFramePTS       TmnxVdoPTS,
    tmnxVdoSGSpliceMaxAdPTS          TmnxVdoPTS,
    tmnxVdoSGSpliceMinNwPTS          TmnxVdoPTS
}

tmnxVdoSGSpliceStartTime         OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceStartTime indicates the start time of
         splice in seconds.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 1 }

tmnxVdoSGSpliceAdServerAddrType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceAdServerAddrType indicates the type of Ad
         Insert (ADI) server address represented by
         tmnxVdoSGSpliceAdServerAddr.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 2 }

tmnxVdoSGSpliceAdServerAddr      OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceAdServerAddr indicates the address of the
         Ad Insert (ADI) server that issued the splice request.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 3 }

tmnxVdoSGSpliceStatus            OBJECT-TYPE
    SYNTAX      INTEGER {
        init       (1),
        pending    (2),
        inProgress (3),
        complete   (4)
    }
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceStatus indicates the status of this splice
         request.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 4 }

tmnxVdoSGSpliceDurationReq       OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceDurationReq indicates the splice duration,
         in seconds, of the ad requested by the Ad Insert (ADI) server.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 5 }

tmnxVdoSGSpliceDurationPlayed    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceDurationPlayed indicates the splice
         duration, in seconds, played by the splicer.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 6 }

tmnxVdoSGSpliceRate              OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceRate indicates the rate of the ad stream,
         in kilobits per second (kbps), received by the splicer.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 7 }

tmnxVdoSGSpliceSessionId         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceSessionId indicates the session ID of the
         ad request.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 8 }

tmnxVdoSGSplicePriorSessionId    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSplicePriorSessionId indicates the prior session
         id of the ad. If the value of this object is not equal to 0xFFFFFFFF,
         then this splice is a back-to-back ad insertion.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 9 }

tmnxVdoSGSpliceAbortReason       OBJECT-TYPE
    SYNTAX      INTEGER {
        none              (0),
        unknown           (1),
        adSrvrReq         (2),
        spliceNotFound    (3),
        noPrimaryChannel  (4),
        noInsertChannel   (5),
        tooEarly          (6),
        spliceFailed      (7),
        spliceCollision   (8),
        spliceTooLate     (9),
        spliceQueueFull   (10),
        invalidSessionId  (11),
        sessionIncomplete (12)
    }
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceAbortReason indicates the reason if a
         splice operation has been aborted. If the value of this object is
         equal to 'none', then the splice has not been aborted.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 10 }

tmnxVdoSGSpliceSpliceInSeqNum    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceSpliceInSeqNum indicates the sequence
         number at which the splice-in to the ad occurred.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 11 }

tmnxVdoSGSpliceSpliceOutSeqNum   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceSpliceOutSeqNum indicates the sequence
         number at which the splice-out to the ad occurred.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 12 }

tmnxVdoSGSpliceNumBlkFrames      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceNumBlkFrames indicates the number of black
         frames inserted.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 13 }

tmnxVdoSGSpliceBlkFramePTS       OBJECT-TYPE
    SYNTAX      TmnxVdoPTS
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceBlkFramePTS indicates the Presentation
         Timestamp (PTS) of the first black frame.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 14 }

tmnxVdoSGSpliceMaxAdPTS          OBJECT-TYPE
    SYNTAX      TmnxVdoPTS
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceMaxAdPTS indicates the maximum
         Presentation Timestamp (PTS) value of the last Group of Pictures (GOP)
         of ad stream (non-black frame).

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 15 }

tmnxVdoSGSpliceMinNwPTS          OBJECT-TYPE
    SYNTAX      TmnxVdoPTS
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoSGSpliceMinNwPTS indicates the minimum
         Presentation Timestamp (PTS) value from the first Group of Pictures
         (GOP) of the network stream after the splice out has occurred.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoSGSpliceStatusEntry 16 }

tmnxVdoIfStatExtTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoIfStatExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxVdoIfStatExtTable contains information and statistics for each
         video interface configured in the system."
    ::= { tmnxVdoObjs 17 }

tmnxVdoIfStatExtEntry            OBJECT-TYPE
    SYNTAX      TmnxVdoIfStatExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoIfStatExtTable. Each row entry represents an IP
         address assigned to a video interface."
    AUGMENTS    { tmnxVdoIfAddrEntry }
    ::= { tmnxVdoIfStatExtTable 1 }

TmnxVdoIfStatExtEntry            ::= SEQUENCE
{
    tmnxVdoIfStatExtRxRtcpAppRepSum  Counter64,
    tmnxVdoIfStatExtRxRtcpAppRepSumL Counter32,
    tmnxVdoIfStatExtRxRtcpAppRepSumH Counter32,
    tmnxVdoIfStatExtRxRtcpAppReqSum  Counter64,
    tmnxVdoIfStatExtRxRtcpAppReqSumL Counter32,
    tmnxVdoIfStatExtRxRtcpAppReqSumH Counter32,
    tmnxVdoIfStatExtRxRtcpFbRepSum   Counter64,
    tmnxVdoIfStatExtRxRtcpFbRepSumL  Counter32,
    tmnxVdoIfStatExtRxRtcpFbRepSumH  Counter32,
    tmnxVdoIfStatExtRxRtcpFbReqSum   Counter64,
    tmnxVdoIfStatExtRxRtcpFbReqSumL  Counter32,
    tmnxVdoIfStatExtRxRtcpFbReqSumH  Counter32,
    tmnxVdoIfStatExtRxRudpFbRepSum   Counter64,
    tmnxVdoIfStatExtRxRudpFbRepSumL  Counter32,
    tmnxVdoIfStatExtRxRudpFbRepSumH  Counter32,
    tmnxVdoIfStatExtTxFccPktsSum     Counter64,
    tmnxVdoIfStatExtTxFccPktsSumL    Counter32,
    tmnxVdoIfStatExtTxFccPktsSumH    Counter32,
    tmnxVdoIfStatExtTxFccOctetsSum   Counter64,
    tmnxVdoIfStatExtTxFccOctetsSumL  Counter32,
    tmnxVdoIfStatExtTxFccOctetsSumH  Counter32,
    tmnxVdoIfStatExtTxRetPktsSum     Counter64,
    tmnxVdoIfStatExtTxRetPktsSumL    Counter32,
    tmnxVdoIfStatExtTxRetPktsSumH    Counter32,
    tmnxVdoIfStatExtTxRetOctetsSum   Counter64,
    tmnxVdoIfStatExtTxRetOctetsSumL  Counter32,
    tmnxVdoIfStatExtTxRetOctetsSumH  Counter32,
    tmnxVdoIfStatExtTxRudpPktsSum    Counter64,
    tmnxVdoIfStatExtTxRudpPktsSumL   Counter32,
    tmnxVdoIfStatExtTxRudpPktsSumH   Counter32,
    tmnxVdoIfStatExtTxRudpByteSum    Counter64,
    tmnxVdoIfStatExtTxRudpByteSumL   Counter32,
    tmnxVdoIfStatExtTxRudpByteSumH   Counter32
}

tmnxVdoIfStatExtRxRtcpAppRepSum  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpAppRepSum indicates the total
         number of  Real Time Transport Control Protocol (RTCP) App requests
         processed for currently active sessions for the interface."
    ::= { tmnxVdoIfStatExtEntry 1 }

tmnxVdoIfStatExtRxRtcpAppRepSumL OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpAppRepSumL indicates the lower 32
         bits of the value of tmnxVdoIfStatExtRxRtcpAppRepSum."
    ::= { tmnxVdoIfStatExtEntry 2 }

tmnxVdoIfStatExtRxRtcpAppRepSumH OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpAppRepSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtRxRtcpAppRepSum."
    ::= { tmnxVdoIfStatExtEntry 3 }

tmnxVdoIfStatExtRxRtcpAppReqSum  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpAppReqSum indicates the total
         number of  Real Time Transport Control Protocol (RTCP) App requests
         received for currently active sessions for the interface."
    ::= { tmnxVdoIfStatExtEntry 4 }

tmnxVdoIfStatExtRxRtcpAppReqSumL OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpAppReqSumL indicates the lower 32
         bits of the value of tmnxVdoIfStatExtRxRtcpAppRepSum."
    ::= { tmnxVdoIfStatExtEntry 5 }

tmnxVdoIfStatExtRxRtcpAppReqSumH OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpAppReqSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtRxRtcpAppReqSum."
    ::= { tmnxVdoIfStatExtEntry 6 }

tmnxVdoIfStatExtRxRtcpFbRepSum   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpFbRepSum indicates the total number
         of Real Time Transport Control Protocol (RTCP) feedback (FB) requests
         processed for currently active sessions for the interface."
    ::= { tmnxVdoIfStatExtEntry 7 }

tmnxVdoIfStatExtRxRtcpFbRepSumL  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpFbRepSumL indicates the lower 32
         bits of the value of tmnxVdoIfStatExtRxRtcpFbRepSum."
    ::= { tmnxVdoIfStatExtEntry 8 }

tmnxVdoIfStatExtRxRtcpFbRepSumH  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpFbRepSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtRxRtcpFbRepSum."
    ::= { tmnxVdoIfStatExtEntry 9 }

tmnxVdoIfStatExtRxRtcpFbReqSum   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpFbReqSum indicates the total number
         of Real Time Transport Control Protocol (RTCP) feedback (FB) requests
         received for currently active sessions for the interface."
    ::= { tmnxVdoIfStatExtEntry 10 }

tmnxVdoIfStatExtRxRtcpFbReqSumL  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpFbReqSumL indicates the lower 32
         bits of the value of tmnxVdoIfStatExtRxRtcpFbReqSum."
    ::= { tmnxVdoIfStatExtEntry 11 }

tmnxVdoIfStatExtRxRtcpFbReqSumH  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRtcpFbReqSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtRxRtcpFbReqSum."
    ::= { tmnxVdoIfStatExtEntry 12 }

tmnxVdoIfStatExtRxRudpFbRepSum   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRudpFbRepSum indicates the total number
         of Reliable User Datagram Protocol (RUDP) feedback (FB) messages
         processed for currently active sessions for the interface."
    ::= { tmnxVdoIfStatExtEntry 13 }

tmnxVdoIfStatExtRxRudpFbRepSumL  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRudpFbRepSumL indicates the lower 32
         bits of the value of tmnxVdoIfStatExtRxRudpFbRepSum."
    ::= { tmnxVdoIfStatExtEntry 14 }

tmnxVdoIfStatExtRxRudpFbRepSumH  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtRxRudpFbRepSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtRxRudpFbRepSum."
    ::= { tmnxVdoIfStatExtEntry 15 }

tmnxVdoIfStatExtTxFccPktsSum     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxFccPktsSum indicates the total number
         of data packets sent against Fast Channel Change (FCC) requests for
         the interface for currently active sessions."
    ::= { tmnxVdoIfStatExtEntry 16 }

tmnxVdoIfStatExtTxFccPktsSumL    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxFccPktsSumL indicates the lower 32 bits
         of the value of tmnxVdoIfStatExtTxFccPktsSum."
    ::= { tmnxVdoIfStatExtEntry 17 }

tmnxVdoIfStatExtTxFccPktsSumH    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxFccPktsSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtTxFccPktsSum."
    ::= { tmnxVdoIfStatExtEntry 18 }

tmnxVdoIfStatExtTxFccOctetsSum   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxFccOctetsSum indicates the total number
         of data octets sent against Fast Channel Change (FCC) requests for the
         interface for currently active sessions."
    ::= { tmnxVdoIfStatExtEntry 19 }

tmnxVdoIfStatExtTxFccOctetsSumL  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxFccOctetsSumL indicates the lower 32
         bits of the value of tmnxVdoIfStatExtTxFccOctetsSum."
    ::= { tmnxVdoIfStatExtEntry 20 }

tmnxVdoIfStatExtTxFccOctetsSumH  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxFccOctetsSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtTxFccOctetsSum."
    ::= { tmnxVdoIfStatExtEntry 21 }

tmnxVdoIfStatExtTxRetPktsSum     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRetPktsSum indicates the total number
         of data packets sent against retransmission (Ret) requests for the
         interface for currently active sessions."
    ::= { tmnxVdoIfStatExtEntry 22 }

tmnxVdoIfStatExtTxRetPktsSumL    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRetPktsSumL indicates the lower 32 bits
         of the value of tmnxVdoIfStatExtTxRetPktsSum."
    ::= { tmnxVdoIfStatExtEntry 23 }

tmnxVdoIfStatExtTxRetPktsSumH    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRetPktsSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtTxRetPktsSum."
    ::= { tmnxVdoIfStatExtEntry 24 }

tmnxVdoIfStatExtTxRetOctetsSum   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRetOctetsSum indicates the total number
         of data octets sent against retransmission (Ret) requests for the
         interface for currently active sessions."
    ::= { tmnxVdoIfStatExtEntry 25 }

tmnxVdoIfStatExtTxRetOctetsSumL  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRetOctetsSumL indicates the lower 32
         bits of the value of tmnxVdoIfStatExtTxRetOctetsSum."
    ::= { tmnxVdoIfStatExtEntry 26 }

tmnxVdoIfStatExtTxRetOctetsSumH  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRetOctetsSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtTxRetOctetsSum."
    ::= { tmnxVdoIfStatExtEntry 27 }

tmnxVdoIfStatExtTxRudpPktsSum    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRudpPktsSum indicates the total number
         of data packets sent against Reliable User Datagram Protocol (RUDP)
         retransmission requests for the interface for currently active
         sessions."
    ::= { tmnxVdoIfStatExtEntry 28 }

tmnxVdoIfStatExtTxRudpPktsSumL   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRudpPktsSumL indicates the lower 32
         bits of the value of tmnxVdoIfStatExtTxRudpPktsSum."
    ::= { tmnxVdoIfStatExtEntry 29 }

tmnxVdoIfStatExtTxRudpPktsSumH   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRudpPktsSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtTxRudpPktsSum."
    ::= { tmnxVdoIfStatExtEntry 30 }

tmnxVdoIfStatExtTxRudpByteSum    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRudpByteSum indicates the total number
         of data octets sent against Reliable User Datagram Protocol (RUDP)
         retransmission requests for the interface for currently active
         sessions."
    ::= { tmnxVdoIfStatExtEntry 31 }

tmnxVdoIfStatExtTxRudpByteSumL   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRudpByteSumL indicates the lower 32
         bits of the value of tmnxVdoIfStatExtTxRudpByteSum."
    ::= { tmnxVdoIfStatExtEntry 32 }

tmnxVdoIfStatExtTxRudpByteSumH   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfStatExtTxRudpByteSumH indicates the higher 32
         bits of the value of tmnxVdoIfStatExtTxRudpByteSum."
    ::= { tmnxVdoIfStatExtEntry 33 }

tmnxVdoGrpSrcVqmStatTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoGrpSrcVqmStatEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxVdoGrpSrcVqmStatTable contains VQM (Video Quality Monitoring)
         statistics and heuristics for the multicast video channel."
    ::= { tmnxVdoObjs 18 }

tmnxVdoGrpSrcVqmStatEntry        OBJECT-TYPE
    SYNTAX      TmnxVdoGrpSrcVqmStatEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoGrpSrcVqmStatTable. Each entry represents a
         source address for the corresponding multicast group."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoGrpSrcGrpAddrType,
        tmnxVdoGrpSrcGroupAddress,
        tmnxVdoGrpSrcSrcAddrType,
        tmnxVdoGrpSrcSourceAddress,
        tmnxVdoGrpSrcVqmStatsPeriod,
        tmnxVdoGrpSrcVqmStatsTime
    }
    ::= { tmnxVdoGrpSrcVqmStatTable 1 }

TmnxVdoGrpSrcVqmStatEntry        ::= SEQUENCE
{
    tmnxVdoGrpSrcVqmStatsPeriod      TmnxVdoStatInt,
    tmnxVdoGrpSrcVqmStatsTime        Unsigned32,
    tmnxVdoGrpSrcVqmGoodSecs         Unsigned32,
    tmnxVdoGrpSrcVqmErrSecs          Unsigned32,
    tmnxVdoGrpSrcVqmDegrSecs         Unsigned32,
    tmnxVdoGrpSrcVqmImpairSecs       Unsigned32,
    tmnxVdoGrpSrcVqmPmtRepErrSecs    Unsigned32,
    tmnxVdoGrpSrcVqmPmtRepDegSecs    Unsigned32,
    tmnxVdoGrpSrcVqmPmtRepImpSecs    Unsigned32,
    tmnxVdoGrpSrcVqmPmtSyntxErrSecs  Unsigned32,
    tmnxVdoGrpSrcVqmPatRepErrSecs    Unsigned32,
    tmnxVdoGrpSrcVqmPatRepDegSecs    Unsigned32,
    tmnxVdoGrpSrcVqmPatRepImpSecs    Unsigned32,
    tmnxVdoGrpSrcVqmPatSyntxErrSecs  Unsigned32,
    tmnxVdoGrpSrcVqmPcrRepErrSecs    Unsigned32,
    tmnxVdoGrpSrcVqmPcrRepDegSecs    Unsigned32,
    tmnxVdoGrpSrcVqmPcrRepImpSecs    Unsigned32,
    tmnxVdoGrpSrcVqmSyncByteErrSecs  Unsigned32,
    tmnxVdoGrpSrcVqmSyncLossSecs     Unsigned32,
    tmnxVdoGrpSrcVqmCatErrSecs       Unsigned32,
    tmnxVdoGrpSrcVqmUnrefPidErrSecs  Unsigned32,
    tmnxVdoGrpSrcVqmMDIDelayFactor   Unsigned32,
    tmnxVdoGrpSrcVqmMDILossRate      TmnxMDILossRate,
    tmnxVdoGrpSrcVqmMinGOPLength     Unsigned32,
    tmnxVdoGrpSrcVqmMinFrmPerSec     Unsigned32,
    tmnxVdoGrpSrcVqmAvgGOPLength     Unsigned32,
    tmnxVdoGrpSrcVqmAvgFrmPerSec     Unsigned32,
    tmnxVdoGrpSrcVqmMaxGOPLength     Unsigned32,
    tmnxVdoGrpSrcVqmMaxFrmPerSec     Unsigned32,
    tmnxVdoGrpSrcVqmGoodIFrames      Unsigned32,
    tmnxVdoGrpSrcVqmBadIFrames       Unsigned32,
    tmnxVdoGrpSrcVqmGoodPFrames      Unsigned32,
    tmnxVdoGrpSrcVqmBadPFrames       Unsigned32,
    tmnxVdoGrpSrcVqmGoodBFrames      Unsigned32,
    tmnxVdoGrpSrcVqmBadBFrames       Unsigned32,
    tmnxVdoGrpSrcVqmTrafficLossSecs  Unsigned32,
    tmnxVdoGrpSrcVqmSCTE35ErrSecs    Unsigned32
}

tmnxVdoGrpSrcVqmStatsPeriod      OBJECT-TYPE
    SYNTAX      TmnxVdoStatInt
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmStatsPeriod indicates the period of
         statistics that the user is interested in. The parameter can take a
         value of 'current' which would display to the user all statistics
         within the last second. Alternatively it could a value of 'interval'
         in which case the actual time-duration for which statistics are
         displayed to the user is specified by MIB object
         'tmnxVdoGrpSrcVqmStatsTime'."
    ::= { tmnxVdoGrpSrcVqmStatEntry 1 }

tmnxVdoGrpSrcVqmStatsTime        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmStatsTime is effectively based on the
         value of 'tmnxVdoGrpSrcVqmStatsPeriod'. If
         'tmnxVdoGrpSrcVqmStatsPeriod' has a value of 'current', then this
         object has no functionality and gets assigned a numerical value of
         '0'. If 'tmnxVdoGrpSrcVqmStatsPeriod' has a value of 'interval', then
         this object specifies the duration of the time-interval in minutes for
         which the statistics will be displayed to the user."
    ::= { tmnxVdoGrpSrcVqmStatEntry 2 }

tmnxVdoGrpSrcVqmGoodSecs         OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmGoodSecs indicates the total number of
         good seconds for the stream on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 3 }

tmnxVdoGrpSrcVqmErrSecs          OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmErrSecs indicates the total number of
         errored seconds for the stream on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 4 }

tmnxVdoGrpSrcVqmDegrSecs         OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmDegrSecs indicates the total number of
         degraded seconds for the stream on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 5 }

tmnxVdoGrpSrcVqmImpairSecs       OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmImpairSecs indicates the total number of
         impaired seconds for the stream on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 6 }

tmnxVdoGrpSrcVqmPmtRepErrSecs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPmtRepErrSecs indicates the total number
         of PMT (Program Map Table) repetition error seconds for the stream on
         this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 7 }

tmnxVdoGrpSrcVqmPmtRepDegSecs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPmtRepDegSecs indicates the total number
         of PMT (Program Map Table) repetition degraded seconds for the stream
         on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 8 }

tmnxVdoGrpSrcVqmPmtRepImpSecs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPmtRepImpSecs indicates the total number
         of PMT (Program Map Table) repetition impaired seconds for the stream
         on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 9 }

tmnxVdoGrpSrcVqmPmtSyntxErrSecs  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPmtSyntxErrSecs indicates  the total
         number of PMT syntax error seconds for the stream on this multicast
         channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 10 }

tmnxVdoGrpSrcVqmPatRepErrSecs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPatRepErrSecs indicates the total number
         of PAT (Program Association Table) repetition error seconds for the
         stream on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 11 }

tmnxVdoGrpSrcVqmPatRepDegSecs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPatRepDegSecs indicates the total number
         of PAT (Program Association Table) repetition degraded seconds for the
         stream on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 12 }

tmnxVdoGrpSrcVqmPatRepImpSecs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPatRepImpSecs indicates the total number
         of PAT (Program Association Table) repetition impaired seconds for the
         stream on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 13 }

tmnxVdoGrpSrcVqmPatSyntxErrSecs  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPatSyntxErrSecs indicates  the total
         number of PAT syntax error seconds for the stream on this multicast
         channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 14 }

tmnxVdoGrpSrcVqmPcrRepErrSecs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPcrRepErrSecs indicates the total number
         of PCR (Program Clock Reference) repetition error seconds for the
         video stream with VQM."
    ::= { tmnxVdoGrpSrcVqmStatEntry 15 }

tmnxVdoGrpSrcVqmPcrRepDegSecs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPcrRepDegSecs indicates the total number
         of PCR (Program Clock Reference) repetition degraded seconds for the
         stream on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 16 }

tmnxVdoGrpSrcVqmPcrRepImpSecs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmPcrRepImpSecs indicates the total number
         of PCR (Program Clock Reference) repetition impaired seconds for the
         stream on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 17 }

tmnxVdoGrpSrcVqmSyncByteErrSecs  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmSyncByteErrSecs indicates the total
         number of sync byte error seconds for the stream on this multicast
         channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 18 }

tmnxVdoGrpSrcVqmSyncLossSecs     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmSyncLossSecs indicates the total number
         of sync loss seconds for the stream on this multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 19 }

tmnxVdoGrpSrcVqmCatErrSecs       OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmCatErrSecs indicates the total number of
         CAT (Conditional Access Table) error seconds for the stream on this
         multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 20 }

tmnxVdoGrpSrcVqmUnrefPidErrSecs  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmUnrefPidErrSecs indicates the total
         number of unreferenced PID error seconds for the stream on this
         multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 21 }

tmnxVdoGrpSrcVqmMDIDelayFactor   OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmMDIDelayFactor indicates Media Delivery
         Index (MDI) delay factor. If the value of this object is '4294967295'
         (0xFFFFFFFF) then this indicates there is no media stream."
    REFERENCE
        "RFC-4445, April 2006, Section 3.1"
    ::= { tmnxVdoGrpSrcVqmStatEntry 22 }

tmnxVdoGrpSrcVqmMDILossRate      OBJECT-TYPE
    SYNTAX      TmnxMDILossRate
    UNITS       "TS/sec"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmMDILossRate indicates Media Delivery
         Index (MDI) loss Rate."
    REFERENCE
        "RFC-4445, April 2006, Section 3.2"
    ::= { tmnxVdoGrpSrcVqmStatEntry 23 }

tmnxVdoGrpSrcVqmMinGOPLength     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "pictures"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmMinGOPLength indicates the minimum
         distance in a Group Of Pictures (GOP) between two consecutive I-frames
         within a sequence of frames in that video stream on a multicast
         channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 24 }

tmnxVdoGrpSrcVqmMinFrmPerSec     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "fps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmMinFrmPerSec indicates the minimum number
         of frames per second in a video stream on a multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 25 }

tmnxVdoGrpSrcVqmAvgGOPLength     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "pictures"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmAvgGOPLength indicates the average
         distance in a Group Of Pictures (GOP) between two consecutive I-frames
         within a sequence of frames in that video stream on a multicast
         channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 26 }

tmnxVdoGrpSrcVqmAvgFrmPerSec     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "fps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmAvgFrmPerSec indicates the average number
         of frames per second in a video stream on a multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 27 }

tmnxVdoGrpSrcVqmMaxGOPLength     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "pictures"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmMaxGOPLength indicates the maximum
         distance in a Group Of Pictures (GOP) between two consecutive I-frames
         within a sequence of frames in that video stream on a multicast
         channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 28 }

tmnxVdoGrpSrcVqmMaxFrmPerSec     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "fps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmMaxFrmPerSec indicates the maximum number
         of frames per second in a video stream on a multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 29 }

tmnxVdoGrpSrcVqmGoodIFrames      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmGoodIFrames indicates the number of good
         'I' frames in a video stream on a multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 30 }

tmnxVdoGrpSrcVqmBadIFrames       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmBadIFrames indicates the number of bad
         'I' frames in a video stream on a multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 31 }

tmnxVdoGrpSrcVqmGoodPFrames      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmGoodPFrames indicates the number of good
         'P' frames in a video stream on a multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 32 }

tmnxVdoGrpSrcVqmBadPFrames       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmBadPFrames indicates the number of bad
         'P' frames in a video stream on a multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 33 }

tmnxVdoGrpSrcVqmGoodBFrames      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmGoodBFrames indicates the number of good
         'B' frames in a video stream on a multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 34 }

tmnxVdoGrpSrcVqmBadBFrames       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmBadBFrames indicates the number of bad
         'B' frames in a video stream on a multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 35 }

tmnxVdoGrpSrcVqmTrafficLossSecs  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmTrafficLossSecs indicates loss of traffic
         seconds in a stream on a multicast channel."
    ::= { tmnxVdoGrpSrcVqmStatEntry 36 }

tmnxVdoGrpSrcVqmSCTE35ErrSecs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmSCTE35ErrSecs indicates the total number
         of Society of Cable Telecommunications Engineers (SCTE-35) errors in a
         stream on a multicast channel.

         This object was obsoleted in the 9.0 release."
    ::= { tmnxVdoGrpSrcVqmStatEntry 37 }

tmnxVdoGrpSrcVqmTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoGrpSrcVqmEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxVdoGrpSrcVqmTable contains VQM (Video Quality Monitoring) analyzer
         alarm configured and operational values."
    ::= { tmnxVdoObjs 19 }

tmnxVdoGrpSrcVqmEntry            OBJECT-TYPE
    SYNTAX      TmnxVdoGrpSrcVqmEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoGrpSrcVqmTable. Each entry represents an VQM
         analyzer values for a particular video stream."
    INDEX       {
        svcId,
        tmnxVdoIfName,
        tmnxVdoGrpSrcGrpAddrType,
        tmnxVdoGrpSrcGroupAddress,
        tmnxVdoGrpSrcSrcAddrType,
        tmnxVdoGrpSrcSourceAddress
    }
    ::= { tmnxVdoGrpSrcVqmTable 1 }

TmnxVdoGrpSrcVqmEntry            ::= SEQUENCE
{
    tmnxVdoGrpSrcVqmOperAnalyzerSt   TruthValue,
    tmnxVdoGrpSrcVqmOperCcError      TruthValue,
    tmnxVdoGrpSrcVqmOperPatRepError  TruthValue,
    tmnxVdoGrpSrcVqmOperTncPatRep    Unsigned32,
    tmnxVdoGrpSrcVqmOperQosPatRep    Unsigned32,
    tmnxVdoGrpSrcVqmOperPoaPatRep    Unsigned32,
    tmnxVdoGrpSrcVqmOperPatSyntax    TruthValue,
    tmnxVdoGrpSrcVqmOperPcrRepError  TruthValue,
    tmnxVdoGrpSrcVqmOperTncPcrRep    Unsigned32,
    tmnxVdoGrpSrcVqmOperQosPcrRep    Unsigned32,
    tmnxVdoGrpSrcVqmOperPoaPcrRep    Unsigned32,
    tmnxVdoGrpSrcVqmOperVidPIDAbs    Unsigned32,
    tmnxVdoGrpSrcVqmOperPIDPmtUnref  TruthValue,
    tmnxVdoGrpSrcVqmOperPmtRepError  TruthValue,
    tmnxVdoGrpSrcVqmOperTncPmtRep    Unsigned32,
    tmnxVdoGrpSrcVqmOperQosPmtRep    Unsigned32,
    tmnxVdoGrpSrcVqmOperPoaPmtRep    Unsigned32,
    tmnxVdoGrpSrcVqmOperPmtSyntax    TruthValue,
    tmnxVdoGrpSrcVqmOperSCTE35Error  TruthValue,
    tmnxVdoGrpSrcVqmOperTeiError     TruthValue,
    tmnxVdoGrpSrcVqmOperTsSyncLoss   TruthValue,
    tmnxVdoGrpSrcVqmOperNonVidPIDAbs Unsigned32,
    tmnxVdoGrpSrcVqmOperReportAlarm  TmnxVdoAnalyzerAlarm
}

tmnxVdoGrpSrcVqmOperAnalyzerSt   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperAnalyzerSt indicates whether or not
         the analyzer is enabled for the multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 1 }

tmnxVdoGrpSrcVqmOperCcError      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperCcError indicates whether or not the
         continuity counter error is enabled for the multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 2 }

tmnxVdoGrpSrcVqmOperPatRepError  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperPatRepError indicates whether or not
         PAT (Program Association Table) repetition error is enabled for the
         multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 3 }

tmnxVdoGrpSrcVqmOperTncPatRep    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperTncPatRep indicates the value of TNC
         (Tech Non-Conformant) in milliseconds for PAT repetition and is always
         a multiple of 100."
    ::= { tmnxVdoGrpSrcVqmEntry 4 }

tmnxVdoGrpSrcVqmOperQosPatRep    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperQosPatRep indicates the value of QOS
         (Quality of Service) in milliseconds for PAT repetition and is always
         a multiple of 100."
    ::= { tmnxVdoGrpSrcVqmEntry 5 }

tmnxVdoGrpSrcVqmOperPoaPatRep    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperPoaPatRep indicates the value of TOA
         (Transport Stream off Air) in milliseconds for PAT repetition and is
         always a multiple of 100."
    ::= { tmnxVdoGrpSrcVqmEntry 6 }

tmnxVdoGrpSrcVqmOperPatSyntax    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperPatSyntax indicates whether or not
         PAT syntax error is enabled for the multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 7 }

tmnxVdoGrpSrcVqmOperPcrRepError  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperPcrRepError indicates whether or not
         PCR (Program Clock Reference) repetition error is enabled for the
         multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 8 }

tmnxVdoGrpSrcVqmOperTncPcrRep    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperTncPcrRep indicates the value of TNC
         (Tech Non-Conformant) in milliseconds for PCR repetition and is always
         a multiple of 100."
    ::= { tmnxVdoGrpSrcVqmEntry 9 }

tmnxVdoGrpSrcVqmOperQosPcrRep    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperQosPcrRep indicates the value of QOS
         (Quality of Service) in milliseconds for PCR repetition and is always
         a multiple of 100."
    ::= { tmnxVdoGrpSrcVqmEntry 10 }

tmnxVdoGrpSrcVqmOperPoaPcrRep    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperPoaPcrRep indicates the value of POA
         (Program off Air) in milliseconds for PAT repetition and is always a
         multiple of 100."
    ::= { tmnxVdoGrpSrcVqmEntry 11 }

tmnxVdoGrpSrcVqmOperVidPIDAbs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperVidPIDAbs indicates the counting
         interval for an instance of
         'TIMETRA-VIDEO-MIB::tmnxVdoPIDAbsentErrSecs' which accumulates the
         number of video PID absent errors for the multicast PID stream."
    ::= { tmnxVdoGrpSrcVqmEntry 12 }

tmnxVdoGrpSrcVqmOperPIDPmtUnref  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperPIDPmtUnref indicates whether or not
         unreferenced PID (i.e. PIDs not specified in the PMT) error is enabled
         for the multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 13 }

tmnxVdoGrpSrcVqmOperPmtRepError  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperPmtRepError indicates whether or not
         PMT (Program Map Table) repetition error is enabled for the multicast
         stream."
    ::= { tmnxVdoGrpSrcVqmEntry 14 }

tmnxVdoGrpSrcVqmOperTncPmtRep    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperTncPmtRep indicates the value of TNC
         (Tech Non-Conformance) in milliseconds for PMT repetition and is
         always a multiple of 100."
    ::= { tmnxVdoGrpSrcVqmEntry 15 }

tmnxVdoGrpSrcVqmOperQosPmtRep    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperQosPmtRep indicates the value of QOS
         (Quality of Service) in milliseconds for PMT repetition and is always
         a multiple of 100."
    ::= { tmnxVdoGrpSrcVqmEntry 16 }

tmnxVdoGrpSrcVqmOperPoaPmtRep    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperPoaPmtRep indicates the value of POA
         (Program off Air) in milliseconds for PMT repetition and is always a
         multiple of 100."
    ::= { tmnxVdoGrpSrcVqmEntry 17 }

tmnxVdoGrpSrcVqmOperPmtSyntax    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperPmtSyntax indicates whether or not
         PMT syntax error is enabled for the multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 18 }

tmnxVdoGrpSrcVqmOperSCTE35Error  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperSCTE35Error indicates whether or not
         Society of Cable Telecommunications Engineers (SCTE-35) errors are
         enabled for the multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 19 }

tmnxVdoGrpSrcVqmOperTeiError     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperTeiError indicates whether or not TEI
         (Transport Error Indicator) error is enabled for the multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 20 }

tmnxVdoGrpSrcVqmOperTsSyncLoss   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperTsSyncLoss indicates whether or not
         sync loss error is enabled for the multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 21 }

tmnxVdoGrpSrcVqmOperNonVidPIDAbs OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperNonVidPIDAbs indicates the counting
         interval for an the instance of
         'TIMETRA-VIDEO-MIB::tmnxVdoPIDAbsentErrSecs' which accumulates the
         number of non-video PID absent errors for the multicast PID stream."
    ::= { tmnxVdoGrpSrcVqmEntry 22 }

tmnxVdoGrpSrcVqmOperReportAlarm  OBJECT-TYPE
    SYNTAX      TmnxVdoAnalyzerAlarm
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcVqmOperReportAlarm indicates the severity of
         the analyzer state alarm for the multicast stream."
    ::= { tmnxVdoGrpSrcVqmEntry 23 }

tmnxVdoGrpSrcStatExtTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoGrpSrcStatExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tmnxVdoGrpSrcStatExtTable contains channel information and statistics
         for the multicast groups."
    ::= { tmnxVdoObjs 20 }

tmnxVdoGrpSrcStatExtEntry        OBJECT-TYPE
    SYNTAX      TmnxVdoGrpSrcStatExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tmnxVdoGrpSrcStatExtTable. Each entry represents a
         source address for the corresponding multicast group."
    AUGMENTS    { tmnxVdoGrpSrcStatEntry }
    ::= { tmnxVdoGrpSrcStatExtTable 1 }

TmnxVdoGrpSrcStatExtEntry        ::= SEQUENCE
{
    tmnxVdoGrpSrcExtMaxRtpTsDelta    Counter32,
    tmnxVdoGrpSrcExtMaxTicksDelta    Counter64,
    tmnxVdoGrpSrcExtMaxTicksDeltaL32 Counter32,
    tmnxVdoGrpSrcExtMaxTicksDeltaH32 Counter32,
    tmnxVdoGrpSrcExtCurTsJitter      Counter64,
    tmnxVdoGrpSrcExtCurTsJitterL32   Counter32,
    tmnxVdoGrpSrcExtCurTsJitterH32   Counter32,
    tmnxVdoGrpSrcExtMaxTsJitter      Counter64,
    tmnxVdoGrpSrcExtMaxTsJitterL32   Counter32,
    tmnxVdoGrpSrcExtMaxTsJitterH32   Counter32
}

tmnxVdoGrpSrcExtMaxRtpTsDelta    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcExtMaxRtpTsDelta indicates the maximum Real
         Time Protocol(RTP) Timestamps(Ts) delta recorded up to this point in
         time."
    ::= { tmnxVdoGrpSrcStatExtEntry 1 }

tmnxVdoGrpSrcExtMaxTicksDelta    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcExtMaxTicksDelta indicates the maximum
         arrival Timestamps(Ts) delta recorded up to this point in time."
    ::= { tmnxVdoGrpSrcStatExtEntry 2 }

tmnxVdoGrpSrcExtMaxTicksDeltaL32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcExtMaxTicksDeltaL32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcExtMaxTicksDelta."
    ::= { tmnxVdoGrpSrcStatExtEntry 3 }

tmnxVdoGrpSrcExtMaxTicksDeltaH32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcExtMaxTicksDeltaH32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcExtMaxTicksDelta."
    ::= { tmnxVdoGrpSrcStatExtEntry 4 }

tmnxVdoGrpSrcExtCurTsJitter      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcExtCurTsJitter indicates the difference
         between the current arrival Timestamps(Ts) delta and current Real Time
         Protocol(RTP) Timestamps(Ts) delta."
    ::= { tmnxVdoGrpSrcStatExtEntry 5 }

tmnxVdoGrpSrcExtCurTsJitterL32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcExtCurTsJitterL32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcExtCurTsJitter."
    ::= { tmnxVdoGrpSrcStatExtEntry 6 }

tmnxVdoGrpSrcExtCurTsJitterH32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcExtCurTsJitterH32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcExtCurTsJitter."
    ::= { tmnxVdoGrpSrcStatExtEntry 7 }

tmnxVdoGrpSrcExtMaxTsJitter      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcExtMaxTsJitter indicates the maximum
         difference between the arrival Timestamps(Ts) delta and current Real
         Time Protocol(RTP) Timestamps(Ts) delta."
    ::= { tmnxVdoGrpSrcStatExtEntry 8 }

tmnxVdoGrpSrcExtMaxTsJitterL32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcExtMaxTsJitterL32 indicates the lower 32
         bits of the value of tmnxVdoGrpSrcExtMaxTsJitter."
    ::= { tmnxVdoGrpSrcStatExtEntry 9 }

tmnxVdoGrpSrcExtMaxTsJitterH32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpSrcExtMaxTsJitterH32 indicates the higher 32
         bits of the value of tmnxVdoGrpSrcExtMaxTsJitter."
    ::= { tmnxVdoGrpSrcStatExtEntry 10 }

tmnxVdoGrpEsaObjs                OBJECT IDENTIFIER ::= { tmnxVdoObjs 21 }

tmnxVdoGrpVappTable              OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxVdoGrpVappEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxVdoGrpVappTable contains objects to configure the video ISA
         Group Virtual Application."
    ::= { tmnxVdoGrpEsaObjs 1 }

tmnxVdoGrpVappEntry              OBJECT-TYPE
    SYNTAX      TmnxVdoGrpVappEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each conceptual row represents a video ISA Group Member of a video ISA
         Group.

         Entries in this table can be created or deleted via SNMP operations."
    INDEX       {
        tmnxVdoGrpId,
        tmnxVdoGrpEsaNum,
        tmnxVdoGrpEsaVappNum
    }
    ::= { tmnxVdoGrpVappTable 1 }

TmnxVdoGrpVappEntry              ::= SEQUENCE
{
    tmnxVdoGrpEsaNum                 TmnxEsaNum,
    tmnxVdoGrpEsaVappNum             TmnxEsaVappNum,
    tmnxVdoGrpVappRowStatus          RowStatus,
    tmnxVdoGrpVappAdminState         TmnxAdminState,
    tmnxVdoGrpVappOperState          TmnxOperState,
    tmnxVdoGrpVappUsedMemory         CounterBasedGauge64,
    tmnxVdoGrpVappAvailableMemory    CounterBasedGauge64,
    tmnxVdoGrpVappChannels           Gauge32,
    tmnxVdoGrpVappChannelAllocFails  Counter32,
    tmnxVdoGrpVappMaxBwExceeded      Counter32,
    tmnxVdoGrpVappBwInUse            Gauge32,
    tmnxVdoGrpVappActiveRtcpSessions Gauge32,
    tmnxVdoGrpVappEgressStreamResets Counter32,
    tmnxVdoGrpVappIngrssStreamResets Counter32,
    tmnxVdoGrpVappAdStreamResets     Counter32,
    tmnxVdoGrpVappAdStreamAborts     Counter32,
    tmnxVdoGrpVappSsrcCollisions     Counter32,
    tmnxVdoGrpVappRxDataPackets      Counter64,
    tmnxVdoGrpVappRxDataPacketsLow32 Counter32,
    tmnxVdoGrpVappRxDataPacketsHi32  Counter32,
    tmnxVdoGrpVappRxDataOctets       Counter64,
    tmnxVdoGrpVappRxDataOctetsLow32  Counter32,
    tmnxVdoGrpVappRxDataOctetsHigh32 Counter32,
    tmnxVdoGrpVappRxDataPacketErrors Counter64,
    tmnxVdoGrpVappRxDataPktErrsLow32 Counter32,
    tmnxVdoGrpVappRxDataPktErrsHi32  Counter32,
    tmnxVdoGrpVappTxDataPackets      Counter64,
    tmnxVdoGrpVappTxDataPacketsLow32 Counter32,
    tmnxVdoGrpVappTxDataPacketsHi32  Counter32,
    tmnxVdoGrpVappTxDataOctets       Counter64,
    tmnxVdoGrpVappTxDataOctetsLow32  Counter32,
    tmnxVdoGrpVappTxDataOctetsHigh32 Counter32,
    tmnxVdoGrpVappTxDataPacketErrors Counter64,
    tmnxVdoGrpVappTxDataPktErrsLow32 Counter32,
    tmnxVdoGrpVappTxDataPktErrsHi32  Counter32,
    tmnxVdoGrpVappRtcpParseErrors    Counter32,
    tmnxVdoGrpVappRtcpConfigErrors   Counter32,
    tmnxVdoGrpVappRtcpIpcErrors      Counter32,
    tmnxVdoGrpVappRtcpSgErrors       Counter32,
    tmnxVdoGrpVappRtcpSubErrors      Counter32,
    tmnxVdoGrpVappRtcpIntErrors      Counter32,
    tmnxVdoGrpVappTxLostPackets      Counter32,
    tmnxVdoGrpVappRequestedRtpPkts   Counter32,
    tmnxVdoGrpVappHiPktPoolLimitHit  Counter32,
    tmnxVdoGrpVappMallocFailures     Counter32,
    tmnxVdoGrpVappDentDroppedPkts    Counter32,
    tmnxVdoGrpVappBwPeak             Gauge32,
    tmnxVdoGrpVappCurTotalRetBw      Gauge32,
    tmnxVdoGrpVappPeakRetBw          Gauge32,
    tmnxVdoGrpVappCurFccBw           Gauge32,
    tmnxVdoGrpVappFccDropCntReq      Gauge32,
    tmnxVdoGrpVappMcRtcp             Counter64,
    tmnxVdoGrpVappMcRtcpLow32        Counter32,
    tmnxVdoGrpVappMcRtcpHigh32       Counter32,
    tmnxVdoGrpVappMcRudp             Counter64,
    tmnxVdoGrpVappMcRudpLow32        Counter32,
    tmnxVdoGrpVappMcRudpHigh32       Counter32,
    tmnxVdoGrpVappMcRetReqCrt        Counter64,
    tmnxVdoGrpVappMcRetReqCrtLow32   Counter32,
    tmnxVdoGrpVappMcRetReqCrtHigh32  Counter32,
    tmnxVdoGrpVappRetReqQnc          Counter64,
    tmnxVdoGrpVappRetReqQncLow32     Counter32,
    tmnxVdoGrpVappRetReqQncHigh32    Counter32,
    tmnxVdoGrpVappPktsLostInSeq10    Counter32,
    tmnxVdoGrpVappPktsLostInSeq20    Counter32,
    tmnxVdoGrpVappPktsLostInSeq30    Counter32,
    tmnxVdoGrpVappPktsLostInSeq40    Counter32,
    tmnxVdoGrpVappPktsLostInSeqMore  Counter32,
    tmnxVdoGrpVappPeakFccBw          Gauge32,
    tmnxVdoGrpVappPeakFccBwTime      TimeStamp,
    tmnxVdoGrpVappPeakAbsRetBw       Gauge32,
    tmnxVdoGrpVappPeakAbsRetBwTime   TimeStamp,
    tmnxVdoGrpVappPeakFccSession     Gauge32,
    tmnxVdoGrpVappPeakFccSessionTime TimeStamp,
    tmnxVdoGrpVappPeakRetSession     Gauge32,
    tmnxVdoGrpVappPeakRetSessionTime TimeStamp,
    tmnxVdoGrpVappPeakFccRetTotBw    Gauge32,
    tmnxVdoGrpVappPkFccRetTotBwTime  TimeStamp,
    tmnxVdoGrpVappPeakFccRetTotSess  Gauge32,
    tmnxVdoGrpVappPkFccRetTotSeTime  TimeStamp,
    tmnxVdoGrpVappCurAbsRetBw        Gauge32,
    tmnxVdoGrpVappCurFccRetTotalBw   Gauge32,
    tmnxVdoGrpVappActFccSess         Gauge32,
    tmnxVdoGrpVappActRetSess         Gauge32,
    tmnxVdoGrpVappActFccRetTotalSess Gauge32,
    tmnxVdoGrpVappLhPkFccBw          Gauge32,
    tmnxVdoGrpVappLhPkFccBwTime      TimeStamp,
    tmnxVdoGrpVappLhPkAbsRetBw       Gauge32,
    tmnxVdoGrpVappLhPkAbsRetBwTime   TimeStamp,
    tmnxVdoGrpVappLhPkFccSession     Gauge32,
    tmnxVdoGrpVappLhPkFccSessionTime TimeStamp,
    tmnxVdoGrpVappLhPkRetSession     Gauge32,
    tmnxVdoGrpVappLhPkRetSessionTime TimeStamp,
    tmnxVdoGrpVappLhPkFccRetTotBw    Gauge32,
    tmnxVdoGrpVappLPFccRetTotBwTime  TimeStamp,
    tmnxVdoGrpVappLhPkFccRetTotSess  Gauge32,
    tmnxVdoGrpVappLPFccRetTotSeTime  TimeStamp,
    tmnxVdoGrpVappChPkFccBw          Gauge32,
    tmnxVdoGrpVappChPkFccBwTime      TimeStamp,
    tmnxVdoGrpVappChPkAbsRetBw       Gauge32,
    tmnxVdoGrpVappChPkAbsRetBwTime   TimeStamp,
    tmnxVdoGrpVappChPkFccSession     Gauge32,
    tmnxVdoGrpVappChPkFccSessionTime TimeStamp,
    tmnxVdoGrpVappChPkRetSession     Gauge32,
    tmnxVdoGrpVappChPkRetSessionTime TimeStamp,
    tmnxVdoGrpVappChPkFccRetTotBw    Gauge32,
    tmnxVdoGrpVappCPFccRetTotBwTime  TimeStamp,
    tmnxVdoGrpVappChPkFccRetTotSess  Gauge32,
    tmnxVdoGrpVappCPFccRetTotSeTime  TimeStamp
}

tmnxVdoGrpEsaNum                 OBJECT-TYPE
    SYNTAX      TmnxEsaNum (1..16)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpEsaNum indicates the number of the Extended
         Service Appliance where the member is located."
    ::= { tmnxVdoGrpVappEntry 1 }

tmnxVdoGrpEsaVappNum             OBJECT-TYPE
    SYNTAX      TmnxEsaVappNum (1..4)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpEsaVappNum indicates the number of the Virtual
         Machine within an Extended Service Appliance where the member is
         located."
    ::= { tmnxVdoGrpVappEntry 2 }

tmnxVdoGrpVappRowStatus          OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRowStatus specifies the row status of this
         row."
    ::= { tmnxVdoGrpVappEntry 3 }

tmnxVdoGrpVappAdminState         OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappAdminState indicates the administrative
         state of the video group on this virtual application."
    ::= { tmnxVdoGrpVappEntry 5 }

tmnxVdoGrpVappOperState          OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappOperState indicates the current operational
         state of the video group on this virtual application."
    ::= { tmnxVdoGrpVappEntry 6 }

tmnxVdoGrpVappUsedMemory         OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappUsedMemory indicates the amount of cache
         being used by the video group for storing the video stream."
    ::= { tmnxVdoGrpVappEntry 7 }

tmnxVdoGrpVappAvailableMemory    OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappAvailableMemory indicates the amount of
         cache available on the virtual application for storing the video
         stream."
    ::= { tmnxVdoGrpVappEntry 8 }

tmnxVdoGrpVappChannels           OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChannels indicates the number of channels
         being served on this virtual application."
    ::= { tmnxVdoGrpVappEntry 9 }

tmnxVdoGrpVappChannelAllocFails  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChannelAllocFails indicates the number of
         failed channel allocations on this virtual application."
    ::= { tmnxVdoGrpVappEntry 10 }

tmnxVdoGrpVappMaxBwExceeded      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMaxBwExceeded indicates the number of times
         maximum allowed bandwidth has been exceeded for each egress stream."
    ::= { tmnxVdoGrpVappEntry 11 }

tmnxVdoGrpVappBwInUse            OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappBwInUse indicates the total aggregate
         bandwidth of the currently running egress streams."
    ::= { tmnxVdoGrpVappEntry 12 }

tmnxVdoGrpVappActiveRtcpSessions OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappActiveRtcpSessions indicates the number of
         active Real Time Transport Control Protocol (RTCP) sessions on this
         virtual application."
    ::= { tmnxVdoGrpVappEntry 13 }

tmnxVdoGrpVappEgressStreamResets OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappEgressStreamResets indicates the number of
         egress stream resets on this virtual application. An egress stream
         reset occurs when there are no packets to transmit on the virtual
         application."
    ::= { tmnxVdoGrpVappEntry 14 }

tmnxVdoGrpVappIngrssStreamResets OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappIngrssStreamResets indicates the number of
         ingress stream resets on this virtual application. An ingress stream
         reset occurs when the ingress stream stopped coming in for more than
         one second."
    ::= { tmnxVdoGrpVappEntry 15 }

tmnxVdoGrpVappAdStreamResets     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpVappAdStreamResets indicates the number of ad
         stream resets on this virtual application. An ad stream reset occurs
         when the ingress ad stream stops.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpVappEntry 16 }

tmnxVdoGrpVappAdStreamAborts     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxVdoGrpVappAdStreamAborts indicates the number of ad
         stream aborts on this virtual application. An ad stream abort could
         happen when an egress reset happens.

         This object was obsoleted in the 23.0 release."
    ::= { tmnxVdoGrpVappEntry 17 }

tmnxVdoGrpVappSsrcCollisions     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappSsrcCollisions indicates the number of
         synchronization source (SSRC) id collisions on this virtual
         application."
    ::= { tmnxVdoGrpVappEntry 18 }

tmnxVdoGrpVappRxDataPackets      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRxDataPackets indicates the number of data
         packets received on this virtual application."
    ::= { tmnxVdoGrpVappEntry 19 }

tmnxVdoGrpVappRxDataPacketsLow32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRxDataPacketsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpVappRxDataPackets."
    ::= { tmnxVdoGrpVappEntry 20 }

tmnxVdoGrpVappRxDataPacketsHi32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRxDataPacketsHi32 indicates the higher 32
         bits of the value of tmnxVdoGrpVappRxDataPackets."
    ::= { tmnxVdoGrpVappEntry 21 }

tmnxVdoGrpVappRxDataOctets       OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRxDataOctets indicates the number of data
         octets received on this virtual application."
    ::= { tmnxVdoGrpVappEntry 22 }

tmnxVdoGrpVappRxDataOctetsLow32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRxDataOctetsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpVappRxDataOctets."
    ::= { tmnxVdoGrpVappEntry 23 }

tmnxVdoGrpVappRxDataOctetsHigh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRxDataOctetsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpVappRxDataOctets."
    ::= { tmnxVdoGrpVappEntry 24 }

tmnxVdoGrpVappRxDataPacketErrors OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRxDataPacketErrors indicates the number of
         malformed or non-RTP (Real Time Transport Protocol) packets received
         on this virtual application."
    ::= { tmnxVdoGrpVappEntry 25 }

tmnxVdoGrpVappRxDataPktErrsLow32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRxDataPktErrsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpVappRxDataPacketErrors."
    ::= { tmnxVdoGrpVappEntry 26 }

tmnxVdoGrpVappRxDataPktErrsHi32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRxDataPktErrsHi32 indicates the higher 32
         bits of the value of tmnxVdoGrpVappRxDataPacketErrors."
    ::= { tmnxVdoGrpVappEntry 27 }

tmnxVdoGrpVappTxDataPackets      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappTxDataPackets indicates the number of data
         packets transmitted on this virtual application."
    ::= { tmnxVdoGrpVappEntry 28 }

tmnxVdoGrpVappTxDataPacketsLow32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappTxDataPacketsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpVappTxDataPackets."
    ::= { tmnxVdoGrpVappEntry 29 }

tmnxVdoGrpVappTxDataPacketsHi32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappTxDataPacketsHi32 indicates the higher 32
         bits of the value of tmnxVdoGrpVappTxDataPackets."
    ::= { tmnxVdoGrpVappEntry 30 }

tmnxVdoGrpVappTxDataOctets       OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappTxDataOctets indicates the number of data
         octets transmitted on this virtual application."
    ::= { tmnxVdoGrpVappEntry 31 }

tmnxVdoGrpVappTxDataOctetsLow32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappTxDataOctetsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpVappTxDataOctets."
    ::= { tmnxVdoGrpVappEntry 32 }

tmnxVdoGrpVappTxDataOctetsHigh32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappTxDataOctetsHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpVappTxDataOctets."
    ::= { tmnxVdoGrpVappEntry 33 }

tmnxVdoGrpVappTxDataPacketErrors OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappTxDataPacketErrors indicates the number of
         failed data packets due to lack of resources to be transmitted on this
         virtual application."
    ::= { tmnxVdoGrpVappEntry 34 }

tmnxVdoGrpVappTxDataPktErrsLow32 OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappTxDataPktErrsLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpVappTxDataPacketErrors."
    ::= { tmnxVdoGrpVappEntry 35 }

tmnxVdoGrpVappTxDataPktErrsHi32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappTxDataPktErrsHi32 indicates the higher 32
         bits of the value of tmnxVdoGrpVappTxDataPacketErrors."
    ::= { tmnxVdoGrpVappEntry 36 }

tmnxVdoGrpVappRtcpParseErrors    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRtcpParseErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) packet parsing errors on
         this virtual application."
    ::= { tmnxVdoGrpVappEntry 37 }

tmnxVdoGrpVappRtcpConfigErrors   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRtcpConfigErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) config errors on this
         virtual application. These errors occur when there is inconsistency
         between the RTCP values and the configured values."
    ::= { tmnxVdoGrpVappEntry 38 }

tmnxVdoGrpVappRtcpIpcErrors      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRtcpIpcErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) inter-process
         communication message processing errors on this virtual application."
    ::= { tmnxVdoGrpVappEntry 39 }

tmnxVdoGrpVappRtcpSgErrors       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRtcpSgErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) channel errors on this
         virtual application. These errors occur when a channel is not found
         for a given interface to process RTCP packets."
    ::= { tmnxVdoGrpVappEntry 40 }

tmnxVdoGrpVappRtcpSubErrors      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRtcpSubErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) subscriber parameter
         errors on this virtual application. These errors occur when the
         subscriber calculations exceed the maximum allowed bandwidth."
    ::= { tmnxVdoGrpVappEntry 41 }

tmnxVdoGrpVappRtcpIntErrors      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRtcpIntErrors indicates the number of
         Real-time Transport Control Protocol (RTCP) interface related errors
         on this virtual application."
    ::= { tmnxVdoGrpVappEntry 42 }

tmnxVdoGrpVappTxLostPackets      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappTxLostPackets indicates the number of
         packets not found in the video virtual application buffer for
         retransmission. When a retransmission request arrives, packets are
         checked in the buffer and if they are not found, the value of this
         object is incremented."
    ::= { tmnxVdoGrpVappEntry 43 }

tmnxVdoGrpVappRequestedRtpPkts   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRequestedRtpPkts indicates the number of
         Real-time Transport Protocol (RTP) packets requested in the Real-time
         Transport Control Protocol (RTCP) feedback (FB) messages received on
         this virtual application."
    ::= { tmnxVdoGrpVappEntry 44 }

tmnxVdoGrpVappHiPktPoolLimitHit  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappHiPktPoolLimitHit indicates the number of
         times the high packet pool limit has been hit. A high value of this
         object indicates potential failure in ingress packet storage."
    ::= { tmnxVdoGrpVappEntry 45 }

tmnxVdoGrpVappMallocFailures     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMallocFailures indicates the number of
         memory allocation failures on the management core of the video virtual
         application."
    ::= { tmnxVdoGrpVappEntry 46 }

tmnxVdoGrpVappDentDroppedPkts    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappDentDroppedPkts indicates the number of
         packets dropped by the video virtual application due to denting."
    ::= { tmnxVdoGrpVappEntry 47 }

tmnxVdoGrpVappBwPeak             OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappBwPeak indicates the maximum bandwidth of
         the currently running egress streams since the last clear event."
    ::= { tmnxVdoGrpVappEntry 48 }

tmnxVdoGrpVappCurTotalRetBw      OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappCurTotalRetBw indicates the current total
         Retransmission (RET) bandwidth in use."
    ::= { tmnxVdoGrpVappEntry 49 }

tmnxVdoGrpVappPeakRetBw          OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakRetBw indicates the maximum
         Retransmission (RET) bandwidth used since the last clear event."
    ::= { tmnxVdoGrpVappEntry 50 }

tmnxVdoGrpVappCurFccBw           OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappCurFccBw indicates the current Fast Channel
         Change (FCC) bandwidth in use."
    ::= { tmnxVdoGrpVappEntry 51 }

tmnxVdoGrpVappFccDropCntReq      OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappFccDropCntReq indicates the drop count for
         the Fast Channel Change (FCC) requests due to reserved Retransmission
         (RET) bandwidth."
    ::= { tmnxVdoGrpVappEntry 52 }

tmnxVdoGrpVappMcRtcp             OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMcRtcp indicates the number of multicast
         retransmissions done in response to Real Time Transport Control
         Protocol (RTCP) requests."
    ::= { tmnxVdoGrpVappEntry 53 }

tmnxVdoGrpVappMcRtcpLow32        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMcRtcpLow32 indicates the lower 32 bits of
         the value of tmnxVdoGrpVappMcRtcp."
    ::= { tmnxVdoGrpVappEntry 54 }

tmnxVdoGrpVappMcRtcpHigh32       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMcRtcpHigh32 indicates the higher 32 bits
         of the value of tmnxVdoGrpVappMcRtcp."
    ::= { tmnxVdoGrpVappEntry 55 }

tmnxVdoGrpVappMcRudp             OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMcRudp indicates the number of multicast
         retransmissions done in response to Reliable User Datagram Protocol
         (RUDP) requests."
    ::= { tmnxVdoGrpVappEntry 56 }

tmnxVdoGrpVappMcRudpLow32        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMcRudpLow32 indicates the lower 32 bits of
         the value of tmnxVdoGrpVappMcRudp."
    ::= { tmnxVdoGrpVappEntry 57 }

tmnxVdoGrpVappMcRudpHigh32       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMcRudpHigh32 indicates the higher 32 bits
         of the value of tmnxVdoGrpVappMcRudp."
    ::= { tmnxVdoGrpVappEntry 58 }

tmnxVdoGrpVappMcRetReqCrt        OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMcRetReqCrt indicates the total number of
         mcast retransmission requests created in response to the unicast
         retransmission requests."
    ::= { tmnxVdoGrpVappEntry 59 }

tmnxVdoGrpVappMcRetReqCrtLow32   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMcRetReqCrtLow32 indicates the lower 32
         bits of the value of tmnxVdoGrpVappMcRetReqCrt."
    ::= { tmnxVdoGrpVappEntry 60 }

tmnxVdoGrpVappMcRetReqCrtHigh32  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappMcRetReqCrtHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpVappMcRetReqCrt."
    ::= { tmnxVdoGrpVappEntry 61 }

tmnxVdoGrpVappRetReqQnc          OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRetReqQnc indicates the total number of
         unicast retransmission requests quenched with the multicast
         retransmission."
    ::= { tmnxVdoGrpVappEntry 62 }

tmnxVdoGrpVappRetReqQncLow32     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRetReqQncLow32 indicates the lower 32 bits
         of the value of tmnxVdoGrpVappRetReqQnc."
    ::= { tmnxVdoGrpVappEntry 63 }

tmnxVdoGrpVappRetReqQncHigh32    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappRetReqQncHigh32 indicates the higher 32
         bits of the value of tmnxVdoGrpVappRetReqQnc."
    ::= { tmnxVdoGrpVappEntry 64 }

tmnxVdoGrpVappPktsLostInSeq10    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPktsLostInSeq10 indicates the total number
         of packets within sequences of 2 to 10 consecutive lost packets of the
         video group on this virtual application."
    ::= { tmnxVdoGrpVappEntry 65 }

tmnxVdoGrpVappPktsLostInSeq20    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPktsLostInSeq20 indicates the total number
         of packets within sequences of 11 to 20 consecutive lost packets of
         the video group on this virtual application."
    ::= { tmnxVdoGrpVappEntry 66 }

tmnxVdoGrpVappPktsLostInSeq30    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPktsLostInSeq30 indicates the total number
         of packets within sequences of 21 to 30 consecutive lost packets of
         the video group on this virtual application."
    ::= { tmnxVdoGrpVappEntry 67 }

tmnxVdoGrpVappPktsLostInSeq40    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPktsLostInSeq40 indicates the total number
         of packets within sequences of 31 to 40 consecutive lost packets of
         the video group on this virtual application."
    ::= { tmnxVdoGrpVappEntry 68 }

tmnxVdoGrpVappPktsLostInSeqMore  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPktsLostInSeqMore indicates the total
         number of packets within sequences of 41 or more consecutive lost
         packets of the video group on this virtual application."
    ::= { tmnxVdoGrpVappEntry 69 }

tmnxVdoGrpVappPeakFccBw          OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakFccBw indicates the peak value of
         bandwidth for Fast Channel Change (FCC) requests since the last
         reboot/clear."
    ::= { tmnxVdoGrpVappEntry 70 }

tmnxVdoGrpVappPeakFccBwTime      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakFccBwTime indicates the time
         (timestamp) when tmnxVdoGrpVappPeakFccBw occurred since the last
         reboot/clear."
    ::= { tmnxVdoGrpVappEntry 71 }

tmnxVdoGrpVappPeakAbsRetBw       OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakAbsRetBw indicates the absolute peak
         value of bandwidth for Retransmission requests (RET) since the last
         reboot/clear."
    ::= { tmnxVdoGrpVappEntry 72 }

tmnxVdoGrpVappPeakAbsRetBwTime   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakAbsRetBwTime indicates the time
         (timestamp) when tmnxVdoGrpVappPeakAbsRetBw occurred since the last
         reboot/clear.."
    ::= { tmnxVdoGrpVappEntry 73 }

tmnxVdoGrpVappPeakFccSession     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakFccSession indicates the peak number of
         Fast Channel Change (FCC) sessions since the last reboot/clear."
    ::= { tmnxVdoGrpVappEntry 74 }

tmnxVdoGrpVappPeakFccSessionTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakFccSessionTime indicates the time
         (timestamp) when tmnxVdoGrpVappPeakFccSession occurred since the last
         reboot/clear."
    ::= { tmnxVdoGrpVappEntry 75 }

tmnxVdoGrpVappPeakRetSession     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakRetSession indicates the peak number of
         Retransmission (RET) sessions since the last reboot/clear."
    ::= { tmnxVdoGrpVappEntry 76 }

tmnxVdoGrpVappPeakRetSessionTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakRetSessionTime indicates the time
         (timestamp) when tmnxVdoGrpVappPeakRetSession occurred since the last
         reboot/clear."
    ::= { tmnxVdoGrpVappEntry 77 }

tmnxVdoGrpVappPeakFccRetTotBw    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakFccRetTotBw indicates the total peak
         value of bandwidth for Channel Change (FCC) and Retransmission (RET)
         requests since the last reboot/clear."
    ::= { tmnxVdoGrpVappEntry 78 }

tmnxVdoGrpVappPkFccRetTotBwTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPkFccRetTotBwTime indicates the time
         (timestamp) when tmnxVdoGrpVappPeakFccRetTotBw occurred since the last
         reboot/clear."
    ::= { tmnxVdoGrpVappEntry 79 }

tmnxVdoGrpVappPeakFccRetTotSess  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPeakFccRetTotSess indicates the total peak
         number of sessions for Fast Channel Change (FCC) and Retransmission
         (RET) since the last reboot/clear."
    ::= { tmnxVdoGrpVappEntry 80 }

tmnxVdoGrpVappPkFccRetTotSeTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappPkFccRetTotSeTime indicates the time
         (timestamp) when tmnxVdoGrpVappPeakFccRetTotSess occurred since the
         last reboot/clear."
    ::= { tmnxVdoGrpVappEntry 81 }

tmnxVdoGrpVappCurAbsRetBw        OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappCurAbsRetBw indicates the current
         Retransmission (RET) bandwidth in use."
    ::= { tmnxVdoGrpVappEntry 82 }

tmnxVdoGrpVappCurFccRetTotalBw   OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappCurFccRetTotalBw indicates the current total
         Fast Channel Change (FCC) and  Retransmission (RET) bandwidth in use."
    ::= { tmnxVdoGrpVappEntry 83 }

tmnxVdoGrpVappActFccSess         OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappActFccSess indicates the number of active
         Real Time Transport Control Protocol (RTCP) sessions allocated for
         Fast Channel Change (FCC) on this virtual application."
    ::= { tmnxVdoGrpVappEntry 84 }

tmnxVdoGrpVappActRetSess         OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappActRetSess indicates the number of active
         Real Time Transport Control Protocol (RTCP) sessions allocated for
         Retransmission (RET) on this virtual application."
    ::= { tmnxVdoGrpVappEntry 85 }

tmnxVdoGrpVappActFccRetTotalSess OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappActFccRetTotalSess indicates the number of
         active Real Time Transport Control Protocol (RTCP) sessions allocated
         for Fast Channel Change (FCC) and Retransmission (RET) on this virtual
         application."
    ::= { tmnxVdoGrpVappEntry 86 }

tmnxVdoGrpVappLhPkFccBw          OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLhPkFccBw indicates the peak value of
         bandwidth for Fast Channel Change (FCC) requests since the last hour."
    ::= { tmnxVdoGrpVappEntry 87 }

tmnxVdoGrpVappLhPkFccBwTime      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLhPkFccBwTime indicates the time
         (timestamp) when tmnxVdoGrpVappLhPkFccBw occurred in the last hour."
    ::= { tmnxVdoGrpVappEntry 88 }

tmnxVdoGrpVappLhPkAbsRetBw       OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLhPkAbsRetBw indicates the absolute peak
         value of bandwidth for Retransmission requests (RET) in the last hour."
    ::= { tmnxVdoGrpVappEntry 89 }

tmnxVdoGrpVappLhPkAbsRetBwTime   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLhPkAbsRetBwTime indicates the time
         (timestamp) when tmnxVdoGrpVappLhPkAbsRetBw occurred in the last
         hour.."
    ::= { tmnxVdoGrpVappEntry 90 }

tmnxVdoGrpVappLhPkFccSession     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLhPkFccSession indicates the peak number of
         Fast Channel Change (FCC) sessions in the last hour."
    ::= { tmnxVdoGrpVappEntry 91 }

tmnxVdoGrpVappLhPkFccSessionTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLhPkFccSessionTime indicates the time
         (timestamp) when tmnxVdoGrpVappLhPkFccSession occurred in the last
         hour."
    ::= { tmnxVdoGrpVappEntry 92 }

tmnxVdoGrpVappLhPkRetSession     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLhPkRetSession indicates the peak number of
         Retransmission (RET) sessions in the last hour."
    ::= { tmnxVdoGrpVappEntry 93 }

tmnxVdoGrpVappLhPkRetSessionTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLhPkRetSessionTime indicates the time
         (timestamp) when tmnxVdoGrpVappLhPkRetSession occurred in the last
         hour."
    ::= { tmnxVdoGrpVappEntry 94 }

tmnxVdoGrpVappLhPkFccRetTotBw    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLhPkFccRetTotBw indicates the total peak
         value of bandwidth for Channel Change (FCC) and Retransmission (RET)
         requests in the last hour."
    ::= { tmnxVdoGrpVappEntry 95 }

tmnxVdoGrpVappLPFccRetTotBwTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLPFccRetTotBwTime indicates the time
         (timestamp) when tmnxVdoGrpVappLhPkFccRetTotBw occurred in the last
         hour."
    ::= { tmnxVdoGrpVappEntry 96 }

tmnxVdoGrpVappLhPkFccRetTotSess  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLhPkFccRetTotSess indicates the total peak
         number of sessions for Fast Channel Change (FCC) and Retransmission
         (RET) since the last hour."
    ::= { tmnxVdoGrpVappEntry 97 }

tmnxVdoGrpVappLPFccRetTotSeTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappLPFccRetTotSeTime indicates the time
         (timestamp) when tmnxVdoGrpVappLhPkFccRetTotSess occurred in the last
         hour."
    ::= { tmnxVdoGrpVappEntry 98 }

tmnxVdoGrpVappChPkFccBw          OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChPkFccBw indicates the peak value of
         bandwidth for Fast Channel Change (FCC) requests since the last hour."
    ::= { tmnxVdoGrpVappEntry 99 }

tmnxVdoGrpVappChPkFccBwTime      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChPkFccBwTime indicates the time
         (timestamp) when tmnxVdoGrpVappChPkFccBw occurred in the current hour."
    ::= { tmnxVdoGrpVappEntry 100 }

tmnxVdoGrpVappChPkAbsRetBw       OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChPkAbsRetBw indicates the absolute peak
         value of bandwidth for Retransmission requests (RET) in the current
         hour."
    ::= { tmnxVdoGrpVappEntry 101 }

tmnxVdoGrpVappChPkAbsRetBwTime   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChPkAbsRetBwTime indicates the time
         (timestamp) when tmnxVdoGrpVappChPkAbsRetBw occurred in the current
         hour."
    ::= { tmnxVdoGrpVappEntry 102 }

tmnxVdoGrpVappChPkFccSession     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChPkFccSession indicates the peak number of
         Fast Channel Change (FCC) sessions in the current hour."
    ::= { tmnxVdoGrpVappEntry 103 }

tmnxVdoGrpVappChPkFccSessionTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChPkFccSessionTime indicates the time
         (timestamp) when tmnxVdoGrpVappChPkFccSession occurred in the current
         hour."
    ::= { tmnxVdoGrpVappEntry 104 }

tmnxVdoGrpVappChPkRetSession     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChPkRetSession indicates the peak number of
         Retransmission (RET) sessions in the current hour."
    ::= { tmnxVdoGrpVappEntry 105 }

tmnxVdoGrpVappChPkRetSessionTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChPkRetSessionTime indicates the time
         (timestamp) when tmnxVdoGrpVappChPkRetSession occurred in the current
         hour."
    ::= { tmnxVdoGrpVappEntry 106 }

tmnxVdoGrpVappChPkFccRetTotBw    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChPkFccRetTotBw indicates the total peak
         value of bandwidth for Channel Change (FCC) and Retransmission (RET)
         requests in the current hour."
    ::= { tmnxVdoGrpVappEntry 107 }

tmnxVdoGrpVappCPFccRetTotBwTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappCPFccRetTotBwTime indicates the time
         (timestamp) when tmnxVdoGrpVappChPkFccRetTotBw occurred in the current
         hour."
    ::= { tmnxVdoGrpVappEntry 108 }

tmnxVdoGrpVappChPkFccRetTotSess  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappChPkFccRetTotSess indicates the total peak
         number of sessions for Fast Channel Change (FCC) and Retransmission
         (RET) since the last hour."
    ::= { tmnxVdoGrpVappEntry 109 }

tmnxVdoGrpVappCPFccRetTotSeTime  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpVappCPFccRetTotSeTime indicates the time
         (timestamp) when tmnxVdoGrpVappChPkFccRetTotSess occurred in the
         current hour."
    ::= { tmnxVdoGrpVappEntry 110 }

tmnxVdoGlobalObjs                OBJECT IDENTIFIER ::= { tmnxVdo 2 }

tmnxVdoIfTableLastChanged        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfTableLastChanged indicates the sysUpTime at the
         time of the last modification to tmnxVdoIfTable by adding, deleting an
         entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxVdoGlobalObjs 1 }

tmnxVdoIfAddrTableLastChanged    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfAddrTableLastChanged indicates the sysUpTime at
         the time of the last modification to tmnxVdoIfAddrTable by adding,
         deleting an entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxVdoGlobalObjs 2 }

tmnxVdoGrpTableLastChanged       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpTableLastChanged indicates the sysUpTime at the
         time of the last modification to tmnxVdoGrpTable by adding, deleting
         an entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxVdoGlobalObjs 3 }

tmnxVdoGrpMDATableLastChanged    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoGrpMDATableLastChanged indicates the sysUpTime at
         the time of the last modification to tmnxVdoGrpMDATable by adding,
         deleting an entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxVdoGlobalObjs 4 }

tmnxVdoAdiChlTableLastChanged    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiChlTableLastChanged indicates the sysUpTime at
         the time of the last modification to tmnxVdoAdiChlTable by adding,
         deleting an entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxVdoGlobalObjs 5 }

tmnxVdoAdiZoneChlTableLastChngd  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoAdiZoneChlTableLastChngd indicates the sysUpTime
         at the time of the last modification to tmnxVdoAdiZoneChlTable by
         adding, deleting an entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxVdoGlobalObjs 6 }

tmnxVdoIfScte30AdSrvrTblLstChngd OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoIfScte30AdSrvrTblLstChngd indicates the sysUpTime
         at the time of the last modification to tmnxVdoIfScte30AdSrvrTable by
         adding, deleting an entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tmnxVdoGlobalObjs 7 }

tmnxVdoGrpVappTableLastChanged   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tmnxVdoGrpVappTableLastChanged indicates the
         value of sysUpTime at the time of the last modification of an entry in
         the tmnxVdoGrpVappTable."
    ::= { tmnxVdoGlobalObjs 8 }

tmnxVdoNotificationObjs          OBJECT IDENTIFIER ::= { tmnxVdo 3 }

tmnxVdoNotifysvcId               OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifysvcId indicates the Service identifier."
    ::= { tmnxVdoNotificationObjs 1 }

tmnxVdoNotifyIfName              OBJECT-TYPE
    SYNTAX      TmnxVdoIfName
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifyIfName indicates the administrative name of
         a video interface."
    ::= { tmnxVdoNotificationObjs 2 }

tmnxVdoNotifyGrpAddrType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifyGrpAddrType indicates the type of IP
         multicast group address represented by tmnxVdoNotifyGroupAddress."
    ::= { tmnxVdoNotificationObjs 3 }

tmnxVdoNotifyGroupAddress        OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifyGroupAddress indicates the IP multicast
         group address of a channel."
    ::= { tmnxVdoNotificationObjs 4 }

tmnxVdoNotifySrcAddrType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifySrcAddrType indicates the type of source
         address represented by tmnxVdoNotifySourceAddress."
    ::= { tmnxVdoNotificationObjs 5 }

tmnxVdoNotifySourceAddress       OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifySourceAddress indicates the source address
         of a channel."
    ::= { tmnxVdoNotificationObjs 6 }

tmnxVdoNotifyAdSpliceSessionId   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifyAdSpliceSessionId indicates the session id
         of an ad splice operation."
    ::= { tmnxVdoNotificationObjs 7 }

tmnxVdoNotifyAdSpliceAbortTime   OBJECT-TYPE
    SYNTAX      DateAndTime (SIZE (11))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifyAdSpliceAbortTime indicates the date and
         time (in UTC) when the ad splice was aborted."
    ::= { tmnxVdoNotificationObjs 8 }

tmnxVdoNotifyAdSpliceDuration    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifyAdSpliceDuration indicates the number of
         seconds ads were played before the slice was aborted."
    ::= { tmnxVdoNotificationObjs 9 }

tmnxVdoNotifyClientAddrType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifyClientAddrType indicates the type of client
         address represented by tmnxVdoNotifyClientAddress."
    ::= { tmnxVdoNotificationObjs 10 }

tmnxVdoNotifyClientAddress       OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifyClientAddress indicates the client address
         of a Real Time Transport Control Protocol (RTCP) stream."
    ::= { tmnxVdoNotificationObjs 11 }

tmnxVdoNotifyAnalyzerState       OBJECT-TYPE
    SYNTAX      TmnxVdoAnalyzerAlarmStates
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxVdoNotifyAnalyzerState indicates the analyzer state
         for the past 10 seconds of the video analyzer alarm."
    ::= { tmnxVdoNotificationObjs 12 }

tmnxVdoConformance               OBJECT IDENTIFIER ::= { tmnxSRConfs 61 }

tmnxVdoCompliances               OBJECT IDENTIFIER ::= { tmnxVdoConformance 1 }

tmnxVdoV7v0Compliance            MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of video features on version
         7.0 of the Nokia SROS series systems."
    MODULE
        MANDATORY-GROUPS {
            tmnxVdoGlobalV7v0Group,
            tmnxVdoIfV7v0Group,
            tmnxVdoGrpV7v0Group,
            tmnxVdoAdiV7v0Group,
            tmnxVdoStatsV7v0Group,
            tmnxVdoGrpSrcV7v0Group,
            tmnxVdoNotificationsV7v0Group
        }
    ::= { tmnxVdoCompliances 1 }

tmnxVdoV8v0Compliance            MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of video features on version
         8.0 of the Nokia SROS series systems."
    MODULE
        MANDATORY-GROUPS {
            tmnxVdoGlobalV7v0Group,
            tmnxVdoIfV7v0Group,
            tmnxVdoGrpV7v0Group,
            tmnxVdoAdiV7v0Group,
            tmnxVdoStatsV7v0Group,
            tmnxVdoStatsV8v0Group,
            tmnxVdoNotificationsV7v0Group,
            tmnxVdoGrpSrcV7v0Group,
            tmnxVdoGrpV8v0Group,
            tmnxVdoIfV8v0Group,
            tmnxVdoNotificationsV8v0Group
        }
    ::= { tmnxVdoCompliances 2 }

tmnxVdoV9v0Compliance            MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of video features on version
         9.0 of the Nokia SROS series systems."
    MODULE
        MANDATORY-GROUPS {
            tmnxVdoGlobalV7v0Group,
            tmnxVdoIfV7v0Group,
            tmnxVdoGrpV7v0Group,
            tmnxVdoAdiV7v0Group,
            tmnxVdoStatsV7v0Group,
            tmnxVdoStatsV9v0Group,
            tmnxVdoNotificationsV7v0Group,
            tmnxVdoGrpSrcV7v0Group,
            tmnxVdoGrpV8v0Group,
            tmnxVdoIfV8v0Group,
            tmnxVdoNotificationsV8v0Group
        }
    ::= { tmnxVdoCompliances 3 }

tmnxVdoV13v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of video features on version
         13.0 of the Nokia SROS series systems."
    MODULE
        MANDATORY-GROUPS {
            tmnxVdoGrpV13v0Group
        }
    ::= { tmnxVdoCompliances 4 }

tmnxVdoV15v0Compliance           MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of video features on version
         15.0 of the Nokia SROS series systems."
    MODULE
        MANDATORY-GROUPS {
            tmnxVdoGrpV15v0Group,
            tmnxVdoNotificationsV15v0Group
        }
    ::= { tmnxVdoCompliances 5 }

tmnxVdoV21v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of video features on version
         21.0 of the Nokia SROS series systems."
    MODULE
        MANDATORY-GROUPS {
            tmnxVdoGrpEsaV21v0Group,
            tmnxVdoNotificationsV21v0Group,
            tmnxVdoGrpV21v0Group
        }
    ::= { tmnxVdoCompliances 6 }

tmnxVdoV23v0Compliance           MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of video features on version
         23.0 of the Nokia SROS series systems."
    MODULE
        MANDATORY-GROUPS {
            tmnxVdoGlobalV7v0Group,
            tmnxVdoAdiV7v0Group,
            tmnxVdoStatsV9v0Group,
            tmnxVdoNotificationsV7v0Group,
            tmnxVdoGrpSrcV7v0Group,
            tmnxVdoGrpV8v0Group,
            tmnxVdoIfV8v0Group,
            tmnxVdoNotificationsV8v0Group,
            tmnxVdoIfV23v0Group,
            tmnxVdoStatsV23v0Group,
            tmnxVdoGrpV23v0Group,
            tmnxVdoGrpEsaV23v0Group,
            tmnxVdoNotificationsV21v0Group,
            tmnxVdoGrpV21v0Group
        }
    ::= { tmnxVdoCompliances 7 }

tmnxVdoGroups                    OBJECT IDENTIFIER ::= { tmnxVdoConformance 2 }

tmnxVdoGlobalV7v0Group           OBJECT-GROUP
    OBJECTS     {
        tmnxVdoIfTableLastChanged,
        tmnxVdoGrpTableLastChanged,
        tmnxVdoGrpMDATableLastChanged,
        tmnxVdoIfAddrTableLastChanged,
        tmnxVdoAdiChlTableLastChanged,
        tmnxVdoAdiZoneChlTableLastChngd,
        tmnxVdoIfScte30AdSrvrTblLstChngd
    }
    STATUS      current
    DESCRIPTION
        "The group of global objects supporting management of the video
         features on version 7.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 1 }

tmnxVdoIfV7v0Group               OBJECT-GROUP
    OBJECTS     {
        tmnxVdoIfRowStatus,
        tmnxVdoIfLastChanged,
        tmnxVdoIfAdminState,
        tmnxVdoIfOperState,
        tmnxVdoIfDescription,
        tmnxVdoIfVdoGrpId,
        tmnxVdoIfVrtrIfIndex,
        tmnxVdoIfIngressQosPolicyId,
        tmnxVdoIfEgressQosPolicyId,
        tmnxVdoIfAddrRowStatus,
        tmnxVdoIfAdi,
        tmnxVdoIfRTClientAddrType,
        tmnxVdoIfRTClientAddr,
        tmnxVdoIfGatewayAddrType,
        tmnxVdoIfGatewayAddr,
        tmnxVdoIfMcastSvcId,
        tmnxVdoIfIngressIpFilterId,
        tmnxVdoIfIngressMacFilterId,
        tmnxVdoIfEgressIpFilterId,
        tmnxVdoIfEgressMacFilterId,
        tmnxVdoIfScte30ControlAddrType,
        tmnxVdoIfScte30ControlAddr,
        tmnxVdoIfScte30DataAddrType,
        tmnxVdoIfScte30DataAddr,
        tmnxVdoIfSapId,
        tmnxVdoIfMcastProtocol,
        tmnxVdoIfSessions,
        tmnxVdoIfCpmProtectPolicyId,
        tmnxVdoIfScte30AdSrvrRowStatus
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of video interfaces on
         version 7.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 2 }

tmnxVdoGrpV7v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpDescription,
        tmnxVdoGrpAdminState,
        tmnxVdoGrpOperState,
        tmnxVdoGrpLocalRTServerState,
        tmnxVdoGrpFCCServerState,
        tmnxVdoGrpADIServerState,
        tmnxVdoGrpRowStatus,
        tmnxVdoGrpLastChanged,
        tmnxVdoGrpMdaRowStatus,
        tmnxVdoGrpMdaAdminState,
        tmnxVdoGrpMdaOperState,
        tmnxVdoGrpMdaUsedMemory,
        tmnxVdoGrpMdaAvailableMemory,
        tmnxVdoGrpMdaChannels,
        tmnxVdoGrpMdaChannelAllocFails,
        tmnxVdoGrpMdaMaxBwExceeded,
        tmnxVdoGrpMdaBwInUse,
        tmnxVdoGrpMdaActiveRtcpSessions,
        tmnxVdoGrpMdaEgressStreamResets,
        tmnxVdoGrpMdaIngressStreamResets,
        tmnxVdoGrpMdaAdStreamResets,
        tmnxVdoGrpMdaAdStreamAborts,
        tmnxVdoGrpMdaSsrcCollisions,
        tmnxVdoGrpMdaRxDataPackets,
        tmnxVdoGrpMdaRxDataPacketsLow32,
        tmnxVdoGrpMdaRxDataPacketsHigh32,
        tmnxVdoGrpMdaRxDataOctets,
        tmnxVdoGrpMdaRxDataOctetsLow32,
        tmnxVdoGrpMdaRxDataOctetsHigh32,
        tmnxVdoGrpMdaRxDataPacketErrors,
        tmnxVdoGrpMdaRxDataPktErrsLow32,
        tmnxVdoGrpMdaRxDataPktErrsHigh32,
        tmnxVdoGrpMdaTxDataPackets,
        tmnxVdoGrpMdaTxDataPacketsLow32,
        tmnxVdoGrpMdaTxDataPacketsHigh32,
        tmnxVdoGrpMdaTxDataOctets,
        tmnxVdoGrpMdaTxDataOctetsLow32,
        tmnxVdoGrpMdaTxDataOctetsHigh32,
        tmnxVdoGrpMdaTxDataPacketErrors,
        tmnxVdoGrpMdaTxDataPktErrsLow32,
        tmnxVdoGrpMdaTxDataPktErrsHigh32,
        tmnxVdoGrpMdaRtcpParseErrors,
        tmnxVdoGrpMdaRtcpConfigErrors,
        tmnxVdoGrpMdaRtcpIpcErrors,
        tmnxVdoGrpMdaRtcpSgErrors,
        tmnxVdoGrpMdaRtcpSubErrors,
        tmnxVdoGrpMdaRtcpIntErrors,
        tmnxVdoGrpMdaTxLostPackets,
        tmnxVdoGrpMdaRequestedRtpPkts,
        tmnxVdoGrpMdaHighPktPoolLimitHit,
        tmnxVdoGrpMdaMallocFailures,
        tmnxVdoGrpMdaDentDroppedPkts
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of video groups on version
         7.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 3 }

tmnxVdoAdiV7v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxVdoAdiChlRowStatus,
        tmnxVdoAdiChlName,
        tmnxVdoAdiChlDescription,
        tmnxVdoAdiZoneChlRowStatus,
        tmnxVdoAdiZoneChlName,
        tmnxVdoAdiChlForwardScte35
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of Ad-Insertion (ADI)
         feature on version 7.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 4 }

tmnxVdoStatsV7v0Group            OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpSrcStreamType,
        tmnxVdoGrpSrcVdoGrpId,
        tmnxVdoGrpSrcAdminRTBufferSize,
        tmnxVdoGrpSrcSSRCId,
        tmnxVdoGrpSrcUDPSrcPort,
        tmnxVdoGrpSrcUDPDestPort,
        tmnxVdoGrpSrcUptime,
        tmnxVdoGrpSrcAdminBW,
        tmnxVdoGrpSrcBufferSize,
        tmnxVdoGrpSrcRxBytes,
        tmnxVdoGrpSrcRxPackets,
        tmnxVdoGrpSrcRxInvalidPackets,
        tmnxVdoGrpSrcTxBytes,
        tmnxVdoGrpSrcTxPackets,
        tmnxVdoGrpSrcTxFailedPackets,
        tmnxVdoGrpSrcRTClientAdminState,
        tmnxVdoGrpSrcRTClntRTSvrAddrType,
        tmnxVdoGrpSrcRTClntRTSvrAddr,
        tmnxVdoGrpSrcRTClientRTSrvrPort,
        tmnxVdoGrpSrcRTClientRxReTxBytes,
        tmnxVdoGrpSrcRTClientRxReTxPkts,
        tmnxVdoGrpSrcRTClientTxRTReq,
        tmnxVdoGrpSrcRTClientTxRTReqReTx,
        tmnxVdoGrpSrcRTClientGapsDetectd,
        tmnxVdoGrpSrcRTClientFailedReq,
        tmnxVdoGrpSrcRTSrvrAdminState,
        tmnxVdoGrpSrcRTSrvrRtpPktsReq,
        tmnxVdoGrpSrcRTSrvrRxRTReq,
        tmnxVdoGrpSrcRTSrvrRxFailedReq,
        tmnxVdoGrpSrcRTSrvrTxRTReplies,
        tmnxVdoGrpSrcRTSrvrTxBytes,
        tmnxVdoGrpSrcRTSrvrTxPackets,
        tmnxVdoGrpSrcFCCSrvrAdminState,
        tmnxVdoGrpSrcFCCSrvrChnlType,
        tmnxVdoGrpSrcFCCSrvrRxFCCReq,
        tmnxVdoGrpSrcFCCSrvrRxFailedReq,
        tmnxVdoGrpSrcFCCSrvrTxFCCReplies,
        tmnxVdoGrpSrcFCCSrvrTxBytes,
        tmnxVdoGrpSrcFCCSrvrTxPackets,
        tmnxVdoGrpSrcADIAdminState,
        tmnxVdoGrpSrcADICurrentState,
        tmnxVdoGrpSrcADIPATVersion,
        tmnxVdoGrpSrcADIPMTVersion,
        tmnxVdoGrpSrcADIPATChanges,
        tmnxVdoGrpSrcADIPMTChanges,
        tmnxVdoGrpSrcADIRxPackets,
        tmnxVdoGrpSrcADITxPackets,
        tmnxVdoGrpSrcADIRxSCTE35Msgs,
        tmnxVdoGrpSrcADIRxSCTE35MsgEnc,
        tmnxVdoGrpSrcADIRxSCTE35MsgUnsup,
        tmnxVdoGrpSrcADIRxSCTE35MsgDisc,
        tmnxVdoGrpSrcADIUnsuppTSLenPkts,
        tmnxVdoGrpSrcRTClientPort,
        tmnxVdoGrpSrcDupSeqNumber,
        tmnxVdoSGV1RxBytesLow32,
        tmnxVdoSGV1RxBytesHigh32,
        tmnxVdoSGV1RxPacketsLow32,
        tmnxVdoSGV1RxPacketsHigh32,
        tmnxVdoSGV1RxInvalidPacketsLow32,
        tmnxVdoSGV1RxInvalidPacketsHgh32,
        tmnxVdoSGV1TxBytesLow32,
        tmnxVdoSGV1TxBytesHigh32,
        tmnxVdoSGV1TxPacketsLow32,
        tmnxVdoSGV1TxPacketsHigh32,
        tmnxVdoSGV1TxFailedPacketsLow32,
        tmnxVdoSGV1TxFailedPacketsHigh32,
        tmnxVdoSGV1RTClntRxReTxBytsLow32,
        tmnxVdoSGV1RTClntRxReTxBytsHgh32,
        tmnxVdoSGV1RTClntRxReTxPktsLow32,
        tmnxVdoSGV1RTClntRxReTxPktsHgh32,
        tmnxVdoSGV1RTSrvrTxBytesLow32,
        tmnxVdoSGV1RTSrvrTxBytesHigh32,
        tmnxVdoSGV1RTSrvrTxPacketsLow32,
        tmnxVdoSGV1RTSrvrTxPacketsHigh32,
        tmnxVdoSGV1FCCSrvrTxBytesLow32,
        tmnxVdoSGV1FCCSrvrTxBytesHigh32,
        tmnxVdoSGV1FCCSrvrTxPacketsLow32,
        tmnxVdoSGV1FCCSrvrTxPacketsHgh32,
        tmnxVdoSGV1ADIRxPacketsLow32,
        tmnxVdoSGV1ADIRxPacketsHigh32,
        tmnxVdoSGV1ADITxPacketsLow32,
        tmnxVdoSGV1ADITxPacketsHigh32,
        tmnxVdoSessionSSRCId,
        tmnxVdoSessionUpTime,
        tmnxVdoSessionExpireTime,
        tmnxVdoSessionCName,
        tmnxVdoSessionDestAddrType,
        tmnxVdoSessionDestAddr,
        tmnxVdoSessionRxFCCRequests,
        tmnxVdoSessionTxFCCReplies,
        tmnxVdoSessionTxFCCPackets,
        tmnxVdoSessionTxFCCOctets,
        tmnxVdoSessionTxFCCFailedPackets,
        tmnxVdoSessionRxRTRequests,
        tmnxVdoSessionTxRTReplies,
        tmnxVdoSessionTxRTPackets,
        tmnxVdoSessionTxRTOctets,
        tmnxVdoSessionTxRTFailedPackets,
        tmnxVdoSessionRequestedRtpPkts,
        tmnxVdoIfStatHdRTServerState,
        tmnxVdoIfStatSdRTServerState,
        tmnxVdoIfStatPipRTServerState,
        tmnxVdoIfStatRTSvrSdRtpPktsReq,
        tmnxVdoIfStatRTSvrHdRtpPktsReq,
        tmnxVdoIfStatRTSvrPipRtpPktsReq,
        tmnxVdoIfStatRTSvrRxSdRTReq,
        tmnxVdoIfStatRTSvrRxSdFailedReq,
        tmnxVdoIfStatRTSvrRxHdRTReq,
        tmnxVdoIfStatRTSvrRxHdFailedReq,
        tmnxVdoIfStatRTSvrRxPipRTReq,
        tmnxVdoIfStatRTSvrRxPipFailedReq,
        tmnxVdoIfStatRTSvrTxSdRTReplies,
        tmnxVdoIfStatRTSvrTxSdBytes,
        tmnxVdoIfStatRTSvrTxSdPackets,
        tmnxVdoIfStatRTSvrTxHdRTReplies,
        tmnxVdoIfStatRTSvrTxHdBytes,
        tmnxVdoIfStatRTSvrTxHdPackets,
        tmnxVdoIfStatRTSvrTxPipRTReplies,
        tmnxVdoIfStatRTSvrTxPipBytes,
        tmnxVdoIfStatRTSvrTxPipPackets,
        tmnxVdoIfStatHdFCCServerMode,
        tmnxVdoIfStatSdFCCServerMode,
        tmnxVdoIfStatPipFCCServerMode,
        tmnxVdoIfStatFCCSrRxSdFCCReq,
        tmnxVdoIfStatFCCSrRxSdFailedReq,
        tmnxVdoIfStatFCCSrRxHdFCCReq,
        tmnxVdoIfStatFCCSrRxHdFailedReq,
        tmnxVdoIfStatFCCSrRxPipFCCReq,
        tmnxVdoIfStatFCCSrRxPipFailedReq,
        tmnxVdoIfStatFCCSrTxSdFCCReplies,
        tmnxVdoIfStatFCCSrTxSdBytes,
        tmnxVdoIfStatFCCSrTxSdPackets,
        tmnxVdoIfStatFCCSrTxHdFCCReplies,
        tmnxVdoIfStatFCCSrTxHdBytes,
        tmnxVdoIfStatFCCSrTxHdPackets,
        tmnxVdoIfStatFCCSrTxPipFCCRplies,
        tmnxVdoIfStatFCCSrTxPipBytes,
        tmnxVdoIfStatFCCSrTxPipPackets,
        tmnxVdoIfStatTxFailedPackets,
        tmnxVdoIfScte30TcpSessions,
        tmnxVdoIfScte30InitSessions,
        tmnxVdoIfStLowRTSvrSdRtpPktsReq,
        tmnxVdoIfStLowRTSvrHdRtpPktsReq,
        tmnxVdoIfStLowRTSvrPipRtpPktsReq,
        tmnxVdoIfStLowRTSvrRxSdRTReq,
        tmnxVdoIfStLowRTSvrRxSdFailedReq,
        tmnxVdoIfStLowRTSvrRxHdRTReq,
        tmnxVdoIfStLowRTSvrRxHdFailedReq,
        tmnxVdoIfStLowRTSvrRxPipRTReq,
        tmnxVdoIfStLowRTSvrRxPipFailedRq,
        tmnxVdoIfStLowRTSvrTxSdRTReplies,
        tmnxVdoIfStLowRTSvrTxSdBytes,
        tmnxVdoIfStLowRTSvrTxSdPackets,
        tmnxVdoIfStLowRTSvrTxHdRTReplies,
        tmnxVdoIfStLowRTSvrTxHdBytes,
        tmnxVdoIfStLowRTSvrTxHdPackets,
        tmnxVdoIfStLowRTSvrTxPipRTReplis,
        tmnxVdoIfStLowRTSvrTxPipBytes,
        tmnxVdoIfStLowRTSvrTxPipPackets,
        tmnxVdoIfStLowFCCSrRxSdFCCReq,
        tmnxVdoIfStLowFCCSrRxSdFailedReq,
        tmnxVdoIfStLowFCCSrRxHdFCCReq,
        tmnxVdoIfStLowFCCSrRxHdFailedReq,
        tmnxVdoIfStLowFCCSrRxPipFCCReq,
        tmnxVdoIfStLowFCCSrRxPipFailedRq,
        tmnxVdoIfStLowFCCSrTxSdFCCReplis,
        tmnxVdoIfStLowFCCSrTxSdBytes,
        tmnxVdoIfStLowFCCSrTxSdPackets,
        tmnxVdoIfStLowFCCSrTxHdFCCReplis,
        tmnxVdoIfStLowFCCSrTxHdBytes,
        tmnxVdoIfStLowFCCSrTxHdPackets,
        tmnxVdoIfStLowFCCSrTxPipFCCRplis,
        tmnxVdoIfStLowFCCSrTxPipBytes,
        tmnxVdoIfStLowFCCSrTxPipPackets,
        tmnxVdoIfStLowTxFailedPackets,
        tmnxVdoIfStHghRTSvrSdRtpPktsReq,
        tmnxVdoIfStHghRTSvrHdRtpPktsReq,
        tmnxVdoIfStHghRTSvrPipRtpPktsReq,
        tmnxVdoIfStHghRTSvrRxSdRTReq,
        tmnxVdoIfStHghRTSvrRxSdFailedReq,
        tmnxVdoIfStHghRTSvrRxHdRTReq,
        tmnxVdoIfStHghRTSvrRxHdFailedReq,
        tmnxVdoIfStHghRTSvrRxPipRTReq,
        tmnxVdoIfStHghRTSvrRxPipFailedRq,
        tmnxVdoIfStHghRTSvrTxSdRTReplies,
        tmnxVdoIfStHghRTSvrTxSdBytes,
        tmnxVdoIfStHghRTSvrTxSdPackets,
        tmnxVdoIfStHghRTSvrTxHdRTReplies,
        tmnxVdoIfStHghRTSvrTxHdBytes,
        tmnxVdoIfStHghRTSvrTxHdPackets,
        tmnxVdoIfStHghRTSvrTxPipRTReplis,
        tmnxVdoIfStHghRTSvrTxPipBytes,
        tmnxVdoIfStHghRTSvrTxPipPackets,
        tmnxVdoIfStHghFCCSrRxSdFCCReq,
        tmnxVdoIfStHghFCCSrRxSdFailedReq,
        tmnxVdoIfStHghFCCSrRxHdFCCReq,
        tmnxVdoIfStHghFCCSrRxHdFailedReq,
        tmnxVdoIfStHghFCCSrRxPipFCCReq,
        tmnxVdoIfStHghFCCSrRxPipFailedRq,
        tmnxVdoIfStHghFCCSrTxSdFCCReplis,
        tmnxVdoIfStHghFCCSrTxSdBytes,
        tmnxVdoIfStHghFCCSrTxSdPackets,
        tmnxVdoIfStHghFCCSrTxHdFCCReplis,
        tmnxVdoIfStHghFCCSrTxHdBytes,
        tmnxVdoIfStHghFCCSrTxHdPackets,
        tmnxVdoIfStHghFCCSrTxPipFCCRplis,
        tmnxVdoIfStHghFCCSrTxPipBytes,
        tmnxVdoIfStHghFCCSrTxPipPackets,
        tmnxVdoIfStHghTxFailedPackets,
        tmnxVdoPIDType,
        tmnxVdoPIDMpegStreamType,
        tmnxVdoPIDLanguage,
        tmnxVdoSGAdiServerUptime,
        tmnxVdoSGAdiInitReq,
        tmnxVdoSGAdiSucInitResp,
        tmnxVdoSGAdiUnsucInitResp,
        tmnxVdoSGAdiAliveReq,
        tmnxVdoSGAdiSucAliveResp,
        tmnxVdoSGAdiUnSucAliveResp,
        tmnxVdoSGAdiCueReq,
        tmnxVdoSGAdiSucCueResp,
        tmnxVdoSGAdiUnsucCueResp,
        tmnxVdoSGAdiAbortReq,
        tmnxVdoSGAdiSucAbortResp,
        tmnxVdoSGAdiUnsucAbortResp,
        tmnxVdoSGAdiUnknownSCTE30Req,
        tmnxVdoSGAdiSpliceReq,
        tmnxVdoSGAdiSucSpliceResp,
        tmnxVdoSGAdiUnsucSpliceResp,
        tmnxVdoSGAdiSucSpliceInCompResp,
        tmnxVdoSGAdiSucSpliceOutCompResp,
        tmnxVdoSGAdiUnsucSpliceOutComRes,
        tmnxVdoSGSpliceAdServerAddrType,
        tmnxVdoSGSpliceAdServerAddr,
        tmnxVdoSGSpliceStatus,
        tmnxVdoSGSpliceDurationReq,
        tmnxVdoSGSpliceDurationPlayed,
        tmnxVdoSGSpliceRate,
        tmnxVdoSGSpliceSessionId,
        tmnxVdoSGSplicePriorSessionId,
        tmnxVdoSGSpliceAbortReason,
        tmnxVdoSGSpliceSpliceInSeqNum,
        tmnxVdoSGSpliceSpliceOutSeqNum,
        tmnxVdoSGSpliceNumBlkFrames,
        tmnxVdoSGSpliceBlkFramePTS,
        tmnxVdoSGSpliceMaxAdPTS,
        tmnxVdoSGSpliceMinNwPTS,
        tmnxVdoSGAdiMinPort,
        tmnxVdoSGAdiMaxPort,
        tmnxVdoSGAdiChlName
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting FCC or RD or ADI statistics on version
         7.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 5 }

tmnxVdoNotifyObjsV7v0Group       OBJECT-GROUP
    OBJECTS     {
        tmnxVdoNotifysvcId,
        tmnxVdoNotifyIfName,
        tmnxVdoNotifyGrpAddrType,
        tmnxVdoNotifyGroupAddress,
        tmnxVdoNotifySrcAddrType,
        tmnxVdoNotifySourceAddress,
        tmnxVdoNotifyAdSpliceSessionId,
        tmnxVdoNotifyAdSpliceAbortTime,
        tmnxVdoNotifyAdSpliceDuration,
        tmnxVdoNotifyClientAddrType,
        tmnxVdoNotifyClientAddress
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting video notifications on version 7.0 of
         the Nokia SROS series systems."
    ::= { tmnxVdoGroups 6 }

tmnxVdoNotificationsV7v0Group    NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxVdoDuplicateSsrcId,
        tmnxVdoMdaSessionsLimitExceeded,
        tmnxVdoMdaSGLimitExceeded,
        tmnxVdoMdaSessionsLimitCleared,
        tmnxVdoMdaSGLimitCleared,
        tmnxVdoAdSpliceAbort,
        tmnxVdoClientSessionsLmtExceeded,
        tmnxVdoClientSessionsLmtCleared
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting management of video features on
         version 7.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 7 }

tmnxVdoGrpV8v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpMdaBwPeak,
        tmnxVdoGrpResvRet,
        tmnxVdoGrpAnalyzerState,
        tmnxVdoGrpStreamSelectionState,
        tmnxVdoGrpMdaCurTotalRetBw,
        tmnxVdoGrpMdaPeakRetBw,
        tmnxVdoGrpMdaCurFccBw,
        tmnxVdoGrpMdaFccDropCntReq,
        tmnxVdoGrpMdaMcRtcp,
        tmnxVdoGrpMdaMcRtcpLow32,
        tmnxVdoGrpMdaMcRtcpHigh32,
        tmnxVdoGrpMdaMcRudp,
        tmnxVdoGrpMdaMcRudpLow32,
        tmnxVdoGrpMdaMcRudpHigh32,
        tmnxVdoGrpMdaMcRetReqCrt,
        tmnxVdoGrpMdaMcRetReqCrtLow32,
        tmnxVdoGrpMdaMcRetReqCrtHigh32,
        tmnxVdoGrpMdaRetReqQnc,
        tmnxVdoGrpMdaRetReqQncLow32,
        tmnxVdoGrpMdaRetReqQncHigh32,
        tmnxVdoGrpMdaPktsLostInSeq10,
        tmnxVdoGrpMdaPktsLostInSeq20,
        tmnxVdoGrpMdaPktsLostInSeq30,
        tmnxVdoGrpMdaPktsLostInSeq40,
        tmnxVdoGrpMdaPktsLostInSeqMore
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of video groups on version
         8.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 8 }

tmnxVdoIfV8v0Group               OBJECT-GROUP
    OBJECTS     {
        tmnxVdoIfRTMcastReply,
        tmnxVdoIfRTCount,
        tmnxVdoIfRTInterval,
        tmnxVdoIfRTHoldTime,
        tmnxVdoIfAcctPolicyId,
        tmnxVdoIfOutputFormat
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of video interfaces on
         version 8.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 9 }

tmnxVdoStatsV8v0Group            OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpSrcRTSTxMcRetPkts,
        tmnxVdoGrpSrcRTSTxMcRetPktsL32,
        tmnxVdoGrpSrcRTSTxMcRetPktsH32,
        tmnxVdoGrpSrcRTSTxMcRetBytes,
        tmnxVdoGrpSrcRTSTxMcRetBytesL32,
        tmnxVdoGrpSrcRTSTxMcRetBytesH32,
        tmnxVdoGrpSrcRTSTxMcRetErrs,
        tmnxVdoGrpSrcRTSTxMcRetErrsL32,
        tmnxVdoGrpSrcRTSTxMcRetErrsH32,
        tmnxVdoGrpSrcRTSRetReqQnc,
        tmnxVdoGrpSrcRTSRetReqQncL32,
        tmnxVdoGrpSrcRTSRetReqQncH32,
        tmnxVdoGrpSrcRTSRetReqCrt,
        tmnxVdoGrpSrcRTSRetReqCrtL32,
        tmnxVdoGrpSrcRTSRetReqCrtH32,
        tmnxVdoGrpSrcFccMinDuration,
        tmnxVdoGrpSrcAudioReorder,
        tmnxVdoGrpSrcRxBytesSaved,
        tmnxVdoGrpSrcRxBytesSavedL32,
        tmnxVdoGrpSrcRxBytesSavedH32,
        tmnxVdoGrpSrcRxPacketsSaved,
        tmnxVdoGrpSrcRxPacketsSavedL32,
        tmnxVdoGrpSrcRxPacketsSavedH32,
        tmnxVdoGrpSrcStatOperBW,
        tmnxVdoGrpSrcRouterIfName,
        tmnxVdoIfStatRTSSdMcRdPktsReq,
        tmnxVdoIfStatRTSSdMcRdPktsReqL32,
        tmnxVdoIfStatRTSSdMcRdPktsReqH32,
        tmnxVdoIfStatRTSHDMcRdPktsReq,
        tmnxVdoIfStatRTSHDMcRdPktsReqL32,
        tmnxVdoIfStatRTSHDMcRdPktsReqH32,
        tmnxVdoIfStatRTSPipMcRdPktReq,
        tmnxVdoIfStatRTSPipMcRdPktReqL32,
        tmnxVdoIfStatRTSPipMcRdPktReqH32,
        tmnxVdoSessionRTReqQuenched,
        tmnxVdoSessionRTMcastReqCreated,
        tmnxVdoSessionPktsLostInSeq10,
        tmnxVdoSessionPktsLostInSeq20,
        tmnxVdoSessionPktsLostInSeq30,
        tmnxVdoSessionPktsLostInSeq40,
        tmnxVdoSessionPktsLostInSeqMore,
        tmnxVdoIfStatSDPktLostInSeq10,
        tmnxVdoIfStatSDPktLostInSeq20,
        tmnxVdoIfStatSDPktLostInSeq30,
        tmnxVdoIfStatSDPktLostInSeq40,
        tmnxVdoIfStatSDPktLostInSeqMore,
        tmnxVdoIfStatHDPktLostInSeq10,
        tmnxVdoIfStatHDPktLostInSeq20,
        tmnxVdoIfStatHDPktLostInSeq30,
        tmnxVdoIfStatHDPktLostInSeq40,
        tmnxVdoIfStatHDPktLostInSeqMore,
        tmnxVdoIfStatPipPktLostInSeq10,
        tmnxVdoIfStatPipPktLostInSeq20,
        tmnxVdoIfStatPipPktLostInSeq30,
        tmnxVdoIfStatPipPktLostInSeq40,
        tmnxVdoIfStatPipPktLostInSeqMore,
        tmnxVdoIfStatExtRxRtcpAppRepSum,
        tmnxVdoIfStatExtRxRtcpAppRepSumL,
        tmnxVdoIfStatExtRxRtcpAppRepSumH,
        tmnxVdoIfStatExtRxRtcpAppReqSum,
        tmnxVdoIfStatExtRxRtcpAppReqSumL,
        tmnxVdoIfStatExtRxRtcpAppReqSumH,
        tmnxVdoIfStatExtRxRtcpFbRepSum,
        tmnxVdoIfStatExtRxRtcpFbRepSumL,
        tmnxVdoIfStatExtRxRtcpFbRepSumH,
        tmnxVdoIfStatExtRxRtcpFbReqSum,
        tmnxVdoIfStatExtRxRtcpFbReqSumL,
        tmnxVdoIfStatExtRxRtcpFbReqSumH,
        tmnxVdoIfStatExtRxRudpFbRepSum,
        tmnxVdoIfStatExtRxRudpFbRepSumL,
        tmnxVdoIfStatExtRxRudpFbRepSumH,
        tmnxVdoIfStatExtTxFccPktsSum,
        tmnxVdoIfStatExtTxFccPktsSumL,
        tmnxVdoIfStatExtTxFccPktsSumH,
        tmnxVdoIfStatExtTxFccOctetsSum,
        tmnxVdoIfStatExtTxFccOctetsSumL,
        tmnxVdoIfStatExtTxFccOctetsSumH,
        tmnxVdoIfStatExtTxRetPktsSum,
        tmnxVdoIfStatExtTxRetPktsSumL,
        tmnxVdoIfStatExtTxRetPktsSumH,
        tmnxVdoIfStatExtTxRetOctetsSum,
        tmnxVdoIfStatExtTxRetOctetsSumL,
        tmnxVdoIfStatExtTxRetOctetsSumH,
        tmnxVdoIfStatExtTxRudpPktsSum,
        tmnxVdoIfStatExtTxRudpPktsSumL,
        tmnxVdoIfStatExtTxRudpPktsSumH,
        tmnxVdoIfStatExtTxRudpByteSum,
        tmnxVdoIfStatExtTxRudpByteSumL,
        tmnxVdoIfStatExtTxRudpByteSumH,
        tmnxVdoGrpSrcVqmGoodSecs,
        tmnxVdoGrpSrcVqmErrSecs,
        tmnxVdoGrpSrcVqmDegrSecs,
        tmnxVdoGrpSrcVqmImpairSecs,
        tmnxVdoGrpSrcVqmPmtRepErrSecs,
        tmnxVdoGrpSrcVqmPmtRepDegSecs,
        tmnxVdoGrpSrcVqmPmtRepImpSecs,
        tmnxVdoGrpSrcVqmPmtSyntxErrSecs,
        tmnxVdoGrpSrcVqmPatRepErrSecs,
        tmnxVdoGrpSrcVqmPatRepDegSecs,
        tmnxVdoGrpSrcVqmPatRepImpSecs,
        tmnxVdoGrpSrcVqmPatSyntxErrSecs,
        tmnxVdoGrpSrcVqmPcrRepErrSecs,
        tmnxVdoGrpSrcVqmPcrRepDegSecs,
        tmnxVdoGrpSrcVqmPcrRepImpSecs,
        tmnxVdoGrpSrcVqmSyncByteErrSecs,
        tmnxVdoGrpSrcVqmSyncLossSecs,
        tmnxVdoGrpSrcVqmCatErrSecs,
        tmnxVdoGrpSrcVqmUnrefPidErrSecs,
        tmnxVdoGrpSrcVqmMDIDelayFactor,
        tmnxVdoGrpSrcVqmMDILossRate,
        tmnxVdoGrpSrcVqmMinGOPLength,
        tmnxVdoGrpSrcVqmMinFrmPerSec,
        tmnxVdoGrpSrcVqmAvgGOPLength,
        tmnxVdoGrpSrcVqmAvgFrmPerSec,
        tmnxVdoGrpSrcVqmMaxGOPLength,
        tmnxVdoGrpSrcVqmMaxFrmPerSec,
        tmnxVdoGrpSrcVqmGoodIFrames,
        tmnxVdoGrpSrcVqmBadIFrames,
        tmnxVdoGrpSrcVqmGoodPFrames,
        tmnxVdoGrpSrcVqmBadPFrames,
        tmnxVdoGrpSrcVqmGoodBFrames,
        tmnxVdoGrpSrcVqmBadBFrames,
        tmnxVdoGrpSrcVqmTrafficLossSecs,
        tmnxVdoGrpSrcVqmSCTE35ErrSecs,
        tmnxVdoGrpSrcVqmOperAnalyzerSt,
        tmnxVdoGrpSrcVqmOperCcError,
        tmnxVdoGrpSrcVqmOperPatRepError,
        tmnxVdoGrpSrcVqmOperTncPatRep,
        tmnxVdoGrpSrcVqmOperQosPatRep,
        tmnxVdoGrpSrcVqmOperPoaPatRep,
        tmnxVdoGrpSrcVqmOperPatSyntax,
        tmnxVdoGrpSrcVqmOperPcrRepError,
        tmnxVdoGrpSrcVqmOperTncPcrRep,
        tmnxVdoGrpSrcVqmOperQosPcrRep,
        tmnxVdoGrpSrcVqmOperPoaPcrRep,
        tmnxVdoGrpSrcVqmOperVidPIDAbs,
        tmnxVdoGrpSrcVqmOperPIDPmtUnref,
        tmnxVdoGrpSrcVqmOperPmtRepError,
        tmnxVdoGrpSrcVqmOperTncPmtRep,
        tmnxVdoGrpSrcVqmOperQosPmtRep,
        tmnxVdoGrpSrcVqmOperPoaPmtRep,
        tmnxVdoGrpSrcVqmOperPmtSyntax,
        tmnxVdoGrpSrcVqmOperSCTE35Error,
        tmnxVdoGrpSrcVqmOperTeiError,
        tmnxVdoGrpSrcVqmOperTsSyncLoss,
        tmnxVdoGrpSrcVqmOperNonVidPIDAbs,
        tmnxVdoGrpSrcVqmOperReportAlarm,
        tmnxVdoPIDCcErrSecs,
        tmnxVdoPIDTeiErrSecs,
        tmnxVdoPIDAbsentErrSecs,
        tmnxVdoPIDBitrate,
        tmnxVdoPIDIsPCR,
        tmnxVdoGrpSrcExtMaxRtpTsDelta,
        tmnxVdoGrpSrcExtMaxTicksDelta,
        tmnxVdoGrpSrcExtMaxTicksDeltaL32,
        tmnxVdoGrpSrcExtMaxTicksDeltaH32,
        tmnxVdoGrpSrcExtCurTsJitter,
        tmnxVdoGrpSrcExtCurTsJitterL32,
        tmnxVdoGrpSrcExtCurTsJitterH32,
        tmnxVdoGrpSrcExtMaxTsJitter,
        tmnxVdoGrpSrcExtMaxTsJitterL32,
        tmnxVdoGrpSrcExtMaxTsJitterH32,
        tmnxVdoGrpSrcNumFccDentedPkts
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting Fast Channel Change (FCC) or Reliable
         Delivery (RD) or Ad Insert (ADI) statistics on version 8.0 of the
         Nokia SROS series systems."
    ::= { tmnxVdoGroups 10 }

tmnxVdoGrpSrcV7v0Group           OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpSrcRxDupSsrcDrops,
        tmnxVdoGrpSrcDupSsrc
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting multicast group statistics on version
         7.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 11 }

tmnxVdoNotifyObjsV8v0Group       OBJECT-GROUP
    OBJECTS     {
        tmnxVdoNotifyAnalyzerState
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting video notifications on version 8.0 of
         the Nokia SROS series systems."
    ::= { tmnxVdoGroups 12 }

tmnxVdoNotificationsV8v0Group    NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxVdoGrpSrcAnlyzrErrState,
        tmnxVdoGrpSrcAnlyzrStClear
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting management of video features on
         version 8.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 13 }

tmnxVdoStatsV9v0Group            OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpSrcRTSTxMcRetPkts,
        tmnxVdoGrpSrcRTSTxMcRetPktsL32,
        tmnxVdoGrpSrcRTSTxMcRetPktsH32,
        tmnxVdoGrpSrcRTSTxMcRetBytes,
        tmnxVdoGrpSrcRTSTxMcRetBytesL32,
        tmnxVdoGrpSrcRTSTxMcRetBytesH32,
        tmnxVdoGrpSrcRTSTxMcRetErrs,
        tmnxVdoGrpSrcRTSTxMcRetErrsL32,
        tmnxVdoGrpSrcRTSTxMcRetErrsH32,
        tmnxVdoGrpSrcRTSRetReqQnc,
        tmnxVdoGrpSrcRTSRetReqQncL32,
        tmnxVdoGrpSrcRTSRetReqQncH32,
        tmnxVdoGrpSrcRTSRetReqCrt,
        tmnxVdoGrpSrcRTSRetReqCrtL32,
        tmnxVdoGrpSrcRTSRetReqCrtH32,
        tmnxVdoGrpSrcFccMinDuration,
        tmnxVdoGrpSrcAudioReorder,
        tmnxVdoGrpSrcRxBytesSaved,
        tmnxVdoGrpSrcRxBytesSavedL32,
        tmnxVdoGrpSrcRxBytesSavedH32,
        tmnxVdoGrpSrcRxPacketsSaved,
        tmnxVdoGrpSrcRxPacketsSavedL32,
        tmnxVdoGrpSrcRxPacketsSavedH32,
        tmnxVdoGrpSrcStatOperBW,
        tmnxVdoGrpSrcRouterIfName,
        tmnxVdoIfStatRTSSdMcRdPktsReq,
        tmnxVdoIfStatRTSSdMcRdPktsReqL32,
        tmnxVdoIfStatRTSSdMcRdPktsReqH32,
        tmnxVdoIfStatRTSHDMcRdPktsReq,
        tmnxVdoIfStatRTSHDMcRdPktsReqL32,
        tmnxVdoIfStatRTSHDMcRdPktsReqH32,
        tmnxVdoIfStatRTSPipMcRdPktReq,
        tmnxVdoIfStatRTSPipMcRdPktReqL32,
        tmnxVdoIfStatRTSPipMcRdPktReqH32,
        tmnxVdoSessionRTReqQuenched,
        tmnxVdoSessionRTMcastReqCreated,
        tmnxVdoSessionPktsLostInSeq10,
        tmnxVdoSessionPktsLostInSeq20,
        tmnxVdoSessionPktsLostInSeq30,
        tmnxVdoSessionPktsLostInSeq40,
        tmnxVdoSessionPktsLostInSeqMore,
        tmnxVdoIfStatSDPktLostInSeq10,
        tmnxVdoIfStatSDPktLostInSeq20,
        tmnxVdoIfStatSDPktLostInSeq30,
        tmnxVdoIfStatSDPktLostInSeq40,
        tmnxVdoIfStatSDPktLostInSeqMore,
        tmnxVdoIfStatHDPktLostInSeq10,
        tmnxVdoIfStatHDPktLostInSeq20,
        tmnxVdoIfStatHDPktLostInSeq30,
        tmnxVdoIfStatHDPktLostInSeq40,
        tmnxVdoIfStatHDPktLostInSeqMore,
        tmnxVdoIfStatPipPktLostInSeq10,
        tmnxVdoIfStatPipPktLostInSeq20,
        tmnxVdoIfStatPipPktLostInSeq30,
        tmnxVdoIfStatPipPktLostInSeq40,
        tmnxVdoIfStatPipPktLostInSeqMore,
        tmnxVdoIfStatExtRxRtcpAppRepSum,
        tmnxVdoIfStatExtRxRtcpAppRepSumL,
        tmnxVdoIfStatExtRxRtcpAppRepSumH,
        tmnxVdoIfStatExtRxRtcpAppReqSum,
        tmnxVdoIfStatExtRxRtcpAppReqSumL,
        tmnxVdoIfStatExtRxRtcpAppReqSumH,
        tmnxVdoIfStatExtRxRtcpFbRepSum,
        tmnxVdoIfStatExtRxRtcpFbRepSumL,
        tmnxVdoIfStatExtRxRtcpFbRepSumH,
        tmnxVdoIfStatExtRxRtcpFbReqSum,
        tmnxVdoIfStatExtRxRtcpFbReqSumL,
        tmnxVdoIfStatExtRxRtcpFbReqSumH,
        tmnxVdoIfStatExtRxRudpFbRepSum,
        tmnxVdoIfStatExtRxRudpFbRepSumL,
        tmnxVdoIfStatExtRxRudpFbRepSumH,
        tmnxVdoIfStatExtTxFccPktsSum,
        tmnxVdoIfStatExtTxFccPktsSumL,
        tmnxVdoIfStatExtTxFccPktsSumH,
        tmnxVdoIfStatExtTxFccOctetsSum,
        tmnxVdoIfStatExtTxFccOctetsSumL,
        tmnxVdoIfStatExtTxFccOctetsSumH,
        tmnxVdoIfStatExtTxRetPktsSum,
        tmnxVdoIfStatExtTxRetPktsSumL,
        tmnxVdoIfStatExtTxRetPktsSumH,
        tmnxVdoIfStatExtTxRetOctetsSum,
        tmnxVdoIfStatExtTxRetOctetsSumL,
        tmnxVdoIfStatExtTxRetOctetsSumH,
        tmnxVdoIfStatExtTxRudpPktsSum,
        tmnxVdoIfStatExtTxRudpPktsSumL,
        tmnxVdoIfStatExtTxRudpPktsSumH,
        tmnxVdoIfStatExtTxRudpByteSum,
        tmnxVdoIfStatExtTxRudpByteSumL,
        tmnxVdoIfStatExtTxRudpByteSumH,
        tmnxVdoGrpSrcVqmGoodSecs,
        tmnxVdoGrpSrcVqmErrSecs,
        tmnxVdoGrpSrcVqmDegrSecs,
        tmnxVdoGrpSrcVqmImpairSecs,
        tmnxVdoGrpSrcVqmPmtRepErrSecs,
        tmnxVdoGrpSrcVqmPmtRepDegSecs,
        tmnxVdoGrpSrcVqmPmtRepImpSecs,
        tmnxVdoGrpSrcVqmPmtSyntxErrSecs,
        tmnxVdoGrpSrcVqmPatRepErrSecs,
        tmnxVdoGrpSrcVqmPatRepDegSecs,
        tmnxVdoGrpSrcVqmPatRepImpSecs,
        tmnxVdoGrpSrcVqmPatSyntxErrSecs,
        tmnxVdoGrpSrcVqmPcrRepErrSecs,
        tmnxVdoGrpSrcVqmPcrRepDegSecs,
        tmnxVdoGrpSrcVqmPcrRepImpSecs,
        tmnxVdoGrpSrcVqmSyncByteErrSecs,
        tmnxVdoGrpSrcVqmSyncLossSecs,
        tmnxVdoGrpSrcVqmCatErrSecs,
        tmnxVdoGrpSrcVqmUnrefPidErrSecs,
        tmnxVdoGrpSrcVqmMDIDelayFactor,
        tmnxVdoGrpSrcVqmMDILossRate,
        tmnxVdoGrpSrcVqmMinGOPLength,
        tmnxVdoGrpSrcVqmMinFrmPerSec,
        tmnxVdoGrpSrcVqmAvgGOPLength,
        tmnxVdoGrpSrcVqmAvgFrmPerSec,
        tmnxVdoGrpSrcVqmMaxGOPLength,
        tmnxVdoGrpSrcVqmMaxFrmPerSec,
        tmnxVdoGrpSrcVqmGoodIFrames,
        tmnxVdoGrpSrcVqmBadIFrames,
        tmnxVdoGrpSrcVqmGoodPFrames,
        tmnxVdoGrpSrcVqmBadPFrames,
        tmnxVdoGrpSrcVqmGoodBFrames,
        tmnxVdoGrpSrcVqmBadBFrames,
        tmnxVdoGrpSrcVqmTrafficLossSecs,
        tmnxVdoGrpSrcVqmOperAnalyzerSt,
        tmnxVdoGrpSrcVqmOperCcError,
        tmnxVdoGrpSrcVqmOperPatRepError,
        tmnxVdoGrpSrcVqmOperTncPatRep,
        tmnxVdoGrpSrcVqmOperQosPatRep,
        tmnxVdoGrpSrcVqmOperPoaPatRep,
        tmnxVdoGrpSrcVqmOperPatSyntax,
        tmnxVdoGrpSrcVqmOperPcrRepError,
        tmnxVdoGrpSrcVqmOperTncPcrRep,
        tmnxVdoGrpSrcVqmOperQosPcrRep,
        tmnxVdoGrpSrcVqmOperPoaPcrRep,
        tmnxVdoGrpSrcVqmOperVidPIDAbs,
        tmnxVdoGrpSrcVqmOperPIDPmtUnref,
        tmnxVdoGrpSrcVqmOperPmtRepError,
        tmnxVdoGrpSrcVqmOperTncPmtRep,
        tmnxVdoGrpSrcVqmOperQosPmtRep,
        tmnxVdoGrpSrcVqmOperPoaPmtRep,
        tmnxVdoGrpSrcVqmOperPmtSyntax,
        tmnxVdoGrpSrcVqmOperSCTE35Error,
        tmnxVdoGrpSrcVqmOperTeiError,
        tmnxVdoGrpSrcVqmOperTsSyncLoss,
        tmnxVdoGrpSrcVqmOperNonVidPIDAbs,
        tmnxVdoGrpSrcVqmOperReportAlarm,
        tmnxVdoPIDCcErrSecs,
        tmnxVdoPIDTeiErrSecs,
        tmnxVdoPIDAbsentErrSecs,
        tmnxVdoPIDBitrate,
        tmnxVdoPIDIsPCR,
        tmnxVdoGrpSrcExtMaxRtpTsDelta,
        tmnxVdoGrpSrcExtMaxTicksDelta,
        tmnxVdoGrpSrcExtMaxTicksDeltaL32,
        tmnxVdoGrpSrcExtMaxTicksDeltaH32,
        tmnxVdoGrpSrcExtCurTsJitter,
        tmnxVdoGrpSrcExtCurTsJitterL32,
        tmnxVdoGrpSrcExtCurTsJitterH32,
        tmnxVdoGrpSrcExtMaxTsJitter,
        tmnxVdoGrpSrcExtMaxTsJitterL32,
        tmnxVdoGrpSrcExtMaxTsJitterH32,
        tmnxVdoGrpSrcNumFccDentedPkts
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting Fast Channel Change (FCC) or Reliable
         Delivery (RD) or Ad Insert (ADI) statistics on version 9.0 of the
         Nokia SROS series systems."
    ::= { tmnxVdoGroups 14 }

tmnxVdoObsoletedV9v0Group        OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpSrcVqmSCTE35ErrSecs
    }
    STATUS      current
    DESCRIPTION
        "The group of objects obsoleted on version 9.0 of the Nokia SROS series
         systems."
    ::= { tmnxVdoGroups 15 }

tmnxVdoGrpV13v0Group             OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpEnableRtClient
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of video features on
         version 13.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 16 }

tmnxVdoGrpV15v0Group             OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpMdaPeakFccBw,
        tmnxVdoGrpMdaPeakFccBwTime,
        tmnxVdoGrpMdaPeakAbsRetBw,
        tmnxVdoGrpMdaPeakAbsRetBwTime,
        tmnxVdoGrpMdaPeakFccSession,
        tmnxVdoGrpMdaPeakFccSessionTime,
        tmnxVdoGrpMdaPeakRetSession,
        tmnxVdoGrpMdaPeakRetSessionTime,
        tmnxVdoGrpMdaPeakFccRetTotBw,
        tmnxVdoGrpMdaPeakFccRetTotBwTime,
        tmnxVdoGrpMdaPeakFccRetTotSess,
        tmnxVdoGrpMdaPeakFccRetTotSeTime,
        tmnxVdoGrpWmBwFcc,
        tmnxVdoGrpWmBwRet,
        tmnxVdoGrpWmBwTotal,
        tmnxVdoGrpWmSesFcc,
        tmnxVdoGrpWmSesRet,
        tmnxVdoGrpWmSesTotal,
        tmnxVdoGrpMdaCurAbsRetBw,
        tmnxVdoGrpMdaCurFccRetTotalBw,
        tmnxVdoGrpMdaActFccSess,
        tmnxVdoGrpMdaActRetSess,
        tmnxVdoGrpMdaActFccRetTotalSess
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of video groups on version
         15.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 17 }

tmnxVdoNotificationsV15v0Group   NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxVdoMdaFccBwLimitExceeded,
        tmnxVdoMdaFccBwLimitCleared,
        tmnxVdoMdaRetBwLimitExceeded,
        tmnxVdoMdaRetBwLimitCleared,
        tmnxVdoMdaFccRetTotBwLmtExceeded,
        tmnxVdoMdaFccRetTotBwLmtCleared,
        tmnxVdoMdaFccSesLimitExceeded,
        tmnxVdoMdaFccSesLimitCleared,
        tmnxVdoMdaRetSesLimitExceeded,
        tmnxVdoMdaRetSesLimitCleared,
        tmnxVdoMdaFccRetTotSeLmtExceeded,
        tmnxVdoMdaFccRetTotSeLmtCleared
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting management of video features on
         version 15.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 18 }

tmnxVdoGrpEsaV21v0Group          OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpVappTableLastChanged,
        tmnxVdoGrpVappRowStatus,
        tmnxVdoGrpVappAdminState,
        tmnxVdoGrpVappOperState,
        tmnxVdoGrpVappUsedMemory,
        tmnxVdoGrpVappAvailableMemory,
        tmnxVdoGrpVappChannels,
        tmnxVdoGrpVappChannelAllocFails,
        tmnxVdoGrpVappMaxBwExceeded,
        tmnxVdoGrpVappBwInUse,
        tmnxVdoGrpVappActiveRtcpSessions,
        tmnxVdoGrpVappEgressStreamResets,
        tmnxVdoGrpVappIngrssStreamResets,
        tmnxVdoGrpVappAdStreamResets,
        tmnxVdoGrpVappAdStreamAborts,
        tmnxVdoGrpVappSsrcCollisions,
        tmnxVdoGrpVappRxDataPackets,
        tmnxVdoGrpVappRxDataPacketsLow32,
        tmnxVdoGrpVappRxDataPacketsHi32,
        tmnxVdoGrpVappRxDataOctets,
        tmnxVdoGrpVappRxDataOctetsLow32,
        tmnxVdoGrpVappRxDataOctetsHigh32,
        tmnxVdoGrpVappRxDataPacketErrors,
        tmnxVdoGrpVappRxDataPktErrsLow32,
        tmnxVdoGrpVappRxDataPktErrsHi32,
        tmnxVdoGrpVappTxDataPackets,
        tmnxVdoGrpVappTxDataPacketsLow32,
        tmnxVdoGrpVappTxDataPacketsHi32,
        tmnxVdoGrpVappTxDataOctets,
        tmnxVdoGrpVappTxDataOctetsLow32,
        tmnxVdoGrpVappTxDataOctetsHigh32,
        tmnxVdoGrpVappTxDataPacketErrors,
        tmnxVdoGrpVappTxDataPktErrsLow32,
        tmnxVdoGrpVappTxDataPktErrsHi32,
        tmnxVdoGrpVappRtcpParseErrors,
        tmnxVdoGrpVappRtcpConfigErrors,
        tmnxVdoGrpVappRtcpIpcErrors,
        tmnxVdoGrpVappRtcpSgErrors,
        tmnxVdoGrpVappRtcpSubErrors,
        tmnxVdoGrpVappRtcpIntErrors,
        tmnxVdoGrpVappTxLostPackets,
        tmnxVdoGrpVappRequestedRtpPkts,
        tmnxVdoGrpVappHiPktPoolLimitHit,
        tmnxVdoGrpVappMallocFailures,
        tmnxVdoGrpVappDentDroppedPkts,
        tmnxVdoGrpVappBwPeak,
        tmnxVdoGrpVappCurTotalRetBw,
        tmnxVdoGrpVappPeakRetBw,
        tmnxVdoGrpVappCurFccBw,
        tmnxVdoGrpVappFccDropCntReq,
        tmnxVdoGrpVappMcRtcp,
        tmnxVdoGrpVappMcRtcpLow32,
        tmnxVdoGrpVappMcRtcpHigh32,
        tmnxVdoGrpVappMcRudp,
        tmnxVdoGrpVappMcRudpLow32,
        tmnxVdoGrpVappMcRudpHigh32,
        tmnxVdoGrpVappMcRetReqCrt,
        tmnxVdoGrpVappMcRetReqCrtLow32,
        tmnxVdoGrpVappMcRetReqCrtHigh32,
        tmnxVdoGrpVappRetReqQnc,
        tmnxVdoGrpVappRetReqQncLow32,
        tmnxVdoGrpVappRetReqQncHigh32,
        tmnxVdoGrpVappPktsLostInSeq10,
        tmnxVdoGrpVappPktsLostInSeq20,
        tmnxVdoGrpVappPktsLostInSeq30,
        tmnxVdoGrpVappPktsLostInSeq40,
        tmnxVdoGrpVappPktsLostInSeqMore,
        tmnxVdoGrpVappPeakFccBw,
        tmnxVdoGrpVappPeakFccBwTime,
        tmnxVdoGrpVappPeakAbsRetBw,
        tmnxVdoGrpVappPeakAbsRetBwTime,
        tmnxVdoGrpVappPeakFccSession,
        tmnxVdoGrpVappPeakFccSessionTime,
        tmnxVdoGrpVappPeakRetSession,
        tmnxVdoGrpVappPeakRetSessionTime,
        tmnxVdoGrpVappPeakFccRetTotBw,
        tmnxVdoGrpVappPkFccRetTotBwTime,
        tmnxVdoGrpVappPeakFccRetTotSess,
        tmnxVdoGrpVappPkFccRetTotSeTime,
        tmnxVdoGrpVappCurAbsRetBw,
        tmnxVdoGrpVappCurFccRetTotalBw,
        tmnxVdoGrpVappActFccSess,
        tmnxVdoGrpVappActRetSess,
        tmnxVdoGrpVappActFccRetTotalSess,
        tmnxVdoGrpVappLhPkFccBw,
        tmnxVdoGrpVappLhPkFccBwTime,
        tmnxVdoGrpVappLhPkAbsRetBw,
        tmnxVdoGrpVappLhPkAbsRetBwTime,
        tmnxVdoGrpVappLhPkFccSession,
        tmnxVdoGrpVappLhPkFccSessionTime,
        tmnxVdoGrpVappLhPkRetSession,
        tmnxVdoGrpVappLhPkRetSessionTime,
        tmnxVdoGrpVappLhPkFccRetTotBw,
        tmnxVdoGrpVappLPFccRetTotBwTime,
        tmnxVdoGrpVappLhPkFccRetTotSess,
        tmnxVdoGrpVappLPFccRetTotSeTime,
        tmnxVdoGrpVappChPkFccBw,
        tmnxVdoGrpVappChPkFccBwTime,
        tmnxVdoGrpVappChPkAbsRetBw,
        tmnxVdoGrpVappChPkAbsRetBwTime,
        tmnxVdoGrpVappChPkFccSession,
        tmnxVdoGrpVappChPkFccSessionTime,
        tmnxVdoGrpVappChPkRetSession,
        tmnxVdoGrpVappChPkRetSessionTime,
        tmnxVdoGrpVappChPkFccRetTotBw,
        tmnxVdoGrpVappCPFccRetTotBwTime,
        tmnxVdoGrpVappChPkFccRetTotSess,
        tmnxVdoGrpVappCPFccRetTotSeTime
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects providing configuration of video Extended Service
         Adaptor (ESA) on Nokia SROS series systems release 21.0 or higher."
    ::= { tmnxVdoGroups 19 }

tmnxVdoNotificationsV21v0Group   NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxVdoVappSessionsLimitExceeded,
        tmnxVdoVappSGLimitExceeded,
        tmnxVdoVappSessionsLimitCleared,
        tmnxVdoVappSGLimitCleared,
        tmnxVdoVappFccBwLimitExceeded,
        tmnxVdoVappFccBwLimitCleared,
        tmnxVdoVappRetBwLimitExceeded,
        tmnxVdoVappRetBwLimitCleared,
        tmnxVdoVappFccRetTotBwLmtExceded,
        tmnxVdoVappFccRetTotBwLmtCleared,
        tmnxVdoVappFccSesLimitExceeded,
        tmnxVdoVappFccSesLimitCleared,
        tmnxVdoVappRetSesLimitExceeded,
        tmnxVdoVappRetSesLimitCleared,
        tmnxVdoVappFccRetTotSeLmtExceded,
        tmnxVdoVappFccRetTotSeLmtCleared
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting management of video features on
         version 15.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 20 }

tmnxVdoGrpV21v0Group             OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpMdaLhPkFccBw,
        tmnxVdoGrpMdaLhPkFccBwTime,
        tmnxVdoGrpMdaLhPkAbsRetBw,
        tmnxVdoGrpMdaLhPkAbsRetBwTime,
        tmnxVdoGrpMdaLhPkFccSession,
        tmnxVdoGrpMdaLhPkFccSessionTime,
        tmnxVdoGrpMdaLhPkRetSession,
        tmnxVdoGrpMdaLhPkRetSessionTime,
        tmnxVdoGrpMdaLhPkFccRetTotBw,
        tmnxVdoGrpMdaLPFccRetTotBwTime,
        tmnxVdoGrpMdaLhPkFccRetTotSess,
        tmnxVdoGrpMdaLPFccRetTotSeTime,
        tmnxVdoGrpMdaChPkFccBw,
        tmnxVdoGrpMdaChPkFccBwTime,
        tmnxVdoGrpMdaChPkAbsRetBw,
        tmnxVdoGrpMdaChPkAbsRetBwTime,
        tmnxVdoGrpMdaChPkFccSession,
        tmnxVdoGrpMdaChPkFccSessionTime,
        tmnxVdoGrpMdaChPkRetSession,
        tmnxVdoGrpMdaChPkRetSessionTime,
        tmnxVdoGrpMdaChPkFccRetTotBw,
        tmnxVdoGrpMdaCPFccRetTotBwTime,
        tmnxVdoGrpMdaChPkFccRetTotSess,
        tmnxVdoGrpMdaCPFccRetTotSeTime
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of video groups on version
         21.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 21 }

tmnxVdoIfV23v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxVdoIfRowStatus,
        tmnxVdoIfLastChanged,
        tmnxVdoIfAdminState,
        tmnxVdoIfOperState,
        tmnxVdoIfDescription,
        tmnxVdoIfVdoGrpId,
        tmnxVdoIfVrtrIfIndex,
        tmnxVdoIfIngressQosPolicyId,
        tmnxVdoIfEgressQosPolicyId,
        tmnxVdoIfAddrRowStatus,
        tmnxVdoIfMcastSvcId,
        tmnxVdoIfIngressIpFilterId,
        tmnxVdoIfIngressMacFilterId,
        tmnxVdoIfEgressIpFilterId,
        tmnxVdoIfEgressMacFilterId,
        tmnxVdoIfSapId,
        tmnxVdoIfMcastProtocol,
        tmnxVdoIfSessions,
        tmnxVdoIfCpmProtectPolicyId
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of video interfaces on
         version 7.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 22 }

tmnxVdoIfV23v0ObsoletedGroup     OBJECT-GROUP
    OBJECTS     {
        tmnxVdoIfAdi,
        tmnxVdoIfRTClientAddrType,
        tmnxVdoIfRTClientAddr,
        tmnxVdoIfGatewayAddrType,
        tmnxVdoIfGatewayAddr,
        tmnxVdoIfScte30ControlAddrType,
        tmnxVdoIfScte30ControlAddr,
        tmnxVdoIfScte30DataAddrType,
        tmnxVdoIfScte30DataAddr,
        tmnxVdoIfScte30AdSrvrRowStatus
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted objects on version 23.0 of the Nokia SROS
         series systems."
    ::= { tmnxVdoGroups 23 }

tmnxVdoStatsV23v0Group           OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpSrcStreamType,
        tmnxVdoGrpSrcVdoGrpId,
        tmnxVdoGrpSrcAdminRTBufferSize,
        tmnxVdoGrpSrcSSRCId,
        tmnxVdoGrpSrcUDPSrcPort,
        tmnxVdoGrpSrcUDPDestPort,
        tmnxVdoGrpSrcUptime,
        tmnxVdoGrpSrcAdminBW,
        tmnxVdoGrpSrcBufferSize,
        tmnxVdoGrpSrcRxBytes,
        tmnxVdoGrpSrcRxPackets,
        tmnxVdoGrpSrcRxInvalidPackets,
        tmnxVdoGrpSrcTxBytes,
        tmnxVdoGrpSrcTxPackets,
        tmnxVdoGrpSrcTxFailedPackets,
        tmnxVdoGrpSrcRTSrvrAdminState,
        tmnxVdoGrpSrcRTSrvrRtpPktsReq,
        tmnxVdoGrpSrcRTSrvrRxRTReq,
        tmnxVdoGrpSrcRTSrvrRxFailedReq,
        tmnxVdoGrpSrcRTSrvrTxRTReplies,
        tmnxVdoGrpSrcRTSrvrTxBytes,
        tmnxVdoGrpSrcRTSrvrTxPackets,
        tmnxVdoGrpSrcFCCSrvrAdminState,
        tmnxVdoGrpSrcFCCSrvrChnlType,
        tmnxVdoGrpSrcFCCSrvrRxFCCReq,
        tmnxVdoGrpSrcFCCSrvrRxFailedReq,
        tmnxVdoGrpSrcFCCSrvrTxFCCReplies,
        tmnxVdoGrpSrcFCCSrvrTxBytes,
        tmnxVdoGrpSrcFCCSrvrTxPackets,
        tmnxVdoGrpSrcADIAdminState,
        tmnxVdoGrpSrcADICurrentState,
        tmnxVdoGrpSrcADIPATVersion,
        tmnxVdoGrpSrcADIPMTVersion,
        tmnxVdoGrpSrcADIPATChanges,
        tmnxVdoGrpSrcADIPMTChanges,
        tmnxVdoGrpSrcADIRxPackets,
        tmnxVdoGrpSrcADITxPackets,
        tmnxVdoGrpSrcADIRxSCTE35Msgs,
        tmnxVdoGrpSrcADIRxSCTE35MsgEnc,
        tmnxVdoGrpSrcADIRxSCTE35MsgUnsup,
        tmnxVdoGrpSrcADIRxSCTE35MsgDisc,
        tmnxVdoGrpSrcADIUnsuppTSLenPkts,
        tmnxVdoGrpSrcDupSeqNumber,
        tmnxVdoSGV1RxBytesLow32,
        tmnxVdoSGV1RxBytesHigh32,
        tmnxVdoSGV1RxPacketsLow32,
        tmnxVdoSGV1RxPacketsHigh32,
        tmnxVdoSGV1RxInvalidPacketsLow32,
        tmnxVdoSGV1RxInvalidPacketsHgh32,
        tmnxVdoSGV1TxBytesLow32,
        tmnxVdoSGV1TxBytesHigh32,
        tmnxVdoSGV1TxPacketsLow32,
        tmnxVdoSGV1TxPacketsHigh32,
        tmnxVdoSGV1TxFailedPacketsLow32,
        tmnxVdoSGV1TxFailedPacketsHigh32,
        tmnxVdoSGV1RTClntRxReTxBytsLow32,
        tmnxVdoSGV1RTClntRxReTxBytsHgh32,
        tmnxVdoSGV1RTClntRxReTxPktsLow32,
        tmnxVdoSGV1RTClntRxReTxPktsHgh32,
        tmnxVdoSGV1RTSrvrTxBytesLow32,
        tmnxVdoSGV1RTSrvrTxBytesHigh32,
        tmnxVdoSGV1RTSrvrTxPacketsLow32,
        tmnxVdoSGV1RTSrvrTxPacketsHigh32,
        tmnxVdoSGV1FCCSrvrTxBytesLow32,
        tmnxVdoSGV1FCCSrvrTxBytesHigh32,
        tmnxVdoSGV1FCCSrvrTxPacketsLow32,
        tmnxVdoSGV1FCCSrvrTxPacketsHgh32,
        tmnxVdoSGV1ADIRxPacketsLow32,
        tmnxVdoSGV1ADIRxPacketsHigh32,
        tmnxVdoSGV1ADITxPacketsLow32,
        tmnxVdoSGV1ADITxPacketsHigh32,
        tmnxVdoSessionSSRCId,
        tmnxVdoSessionUpTime,
        tmnxVdoSessionExpireTime,
        tmnxVdoSessionCName,
        tmnxVdoSessionDestAddrType,
        tmnxVdoSessionDestAddr,
        tmnxVdoSessionRxFCCRequests,
        tmnxVdoSessionTxFCCReplies,
        tmnxVdoSessionTxFCCPackets,
        tmnxVdoSessionTxFCCOctets,
        tmnxVdoSessionTxFCCFailedPackets,
        tmnxVdoSessionRxRTRequests,
        tmnxVdoSessionTxRTReplies,
        tmnxVdoSessionTxRTPackets,
        tmnxVdoSessionTxRTOctets,
        tmnxVdoSessionTxRTFailedPackets,
        tmnxVdoSessionRequestedRtpPkts,
        tmnxVdoIfStatHdRTServerState,
        tmnxVdoIfStatSdRTServerState,
        tmnxVdoIfStatPipRTServerState,
        tmnxVdoIfStatRTSvrSdRtpPktsReq,
        tmnxVdoIfStatRTSvrHdRtpPktsReq,
        tmnxVdoIfStatRTSvrPipRtpPktsReq,
        tmnxVdoIfStatRTSvrRxSdRTReq,
        tmnxVdoIfStatRTSvrRxSdFailedReq,
        tmnxVdoIfStatRTSvrRxHdRTReq,
        tmnxVdoIfStatRTSvrRxHdFailedReq,
        tmnxVdoIfStatRTSvrRxPipRTReq,
        tmnxVdoIfStatRTSvrRxPipFailedReq,
        tmnxVdoIfStatRTSvrTxSdRTReplies,
        tmnxVdoIfStatRTSvrTxSdBytes,
        tmnxVdoIfStatRTSvrTxSdPackets,
        tmnxVdoIfStatRTSvrTxHdRTReplies,
        tmnxVdoIfStatRTSvrTxHdBytes,
        tmnxVdoIfStatRTSvrTxHdPackets,
        tmnxVdoIfStatRTSvrTxPipRTReplies,
        tmnxVdoIfStatRTSvrTxPipBytes,
        tmnxVdoIfStatRTSvrTxPipPackets,
        tmnxVdoIfStatHdFCCServerMode,
        tmnxVdoIfStatSdFCCServerMode,
        tmnxVdoIfStatPipFCCServerMode,
        tmnxVdoIfStatFCCSrRxSdFCCReq,
        tmnxVdoIfStatFCCSrRxSdFailedReq,
        tmnxVdoIfStatFCCSrRxHdFCCReq,
        tmnxVdoIfStatFCCSrRxHdFailedReq,
        tmnxVdoIfStatFCCSrRxPipFCCReq,
        tmnxVdoIfStatFCCSrRxPipFailedReq,
        tmnxVdoIfStatFCCSrTxSdFCCReplies,
        tmnxVdoIfStatFCCSrTxSdBytes,
        tmnxVdoIfStatFCCSrTxSdPackets,
        tmnxVdoIfStatFCCSrTxHdFCCReplies,
        tmnxVdoIfStatFCCSrTxHdBytes,
        tmnxVdoIfStatFCCSrTxHdPackets,
        tmnxVdoIfStatFCCSrTxPipFCCRplies,
        tmnxVdoIfStatFCCSrTxPipBytes,
        tmnxVdoIfStatFCCSrTxPipPackets,
        tmnxVdoIfStatTxFailedPackets,
        tmnxVdoIfStLowRTSvrSdRtpPktsReq,
        tmnxVdoIfStLowRTSvrHdRtpPktsReq,
        tmnxVdoIfStLowRTSvrPipRtpPktsReq,
        tmnxVdoIfStLowRTSvrRxSdRTReq,
        tmnxVdoIfStLowRTSvrRxSdFailedReq,
        tmnxVdoIfStLowRTSvrRxHdRTReq,
        tmnxVdoIfStLowRTSvrRxHdFailedReq,
        tmnxVdoIfStLowRTSvrRxPipRTReq,
        tmnxVdoIfStLowRTSvrRxPipFailedRq,
        tmnxVdoIfStLowRTSvrTxSdRTReplies,
        tmnxVdoIfStLowRTSvrTxSdBytes,
        tmnxVdoIfStLowRTSvrTxSdPackets,
        tmnxVdoIfStLowRTSvrTxHdRTReplies,
        tmnxVdoIfStLowRTSvrTxHdBytes,
        tmnxVdoIfStLowRTSvrTxHdPackets,
        tmnxVdoIfStLowRTSvrTxPipRTReplis,
        tmnxVdoIfStLowRTSvrTxPipBytes,
        tmnxVdoIfStLowRTSvrTxPipPackets,
        tmnxVdoIfStLowFCCSrRxSdFCCReq,
        tmnxVdoIfStLowFCCSrRxSdFailedReq,
        tmnxVdoIfStLowFCCSrRxHdFCCReq,
        tmnxVdoIfStLowFCCSrRxHdFailedReq,
        tmnxVdoIfStLowFCCSrRxPipFCCReq,
        tmnxVdoIfStLowFCCSrRxPipFailedRq,
        tmnxVdoIfStLowFCCSrTxSdFCCReplis,
        tmnxVdoIfStLowFCCSrTxSdBytes,
        tmnxVdoIfStLowFCCSrTxSdPackets,
        tmnxVdoIfStLowFCCSrTxHdFCCReplis,
        tmnxVdoIfStLowFCCSrTxHdBytes,
        tmnxVdoIfStLowFCCSrTxHdPackets,
        tmnxVdoIfStLowFCCSrTxPipFCCRplis,
        tmnxVdoIfStLowFCCSrTxPipBytes,
        tmnxVdoIfStLowFCCSrTxPipPackets,
        tmnxVdoIfStLowTxFailedPackets,
        tmnxVdoIfStHghRTSvrSdRtpPktsReq,
        tmnxVdoIfStHghRTSvrHdRtpPktsReq,
        tmnxVdoIfStHghRTSvrPipRtpPktsReq,
        tmnxVdoIfStHghRTSvrRxSdRTReq,
        tmnxVdoIfStHghRTSvrRxSdFailedReq,
        tmnxVdoIfStHghRTSvrRxHdRTReq,
        tmnxVdoIfStHghRTSvrRxHdFailedReq,
        tmnxVdoIfStHghRTSvrRxPipRTReq,
        tmnxVdoIfStHghRTSvrRxPipFailedRq,
        tmnxVdoIfStHghRTSvrTxSdRTReplies,
        tmnxVdoIfStHghRTSvrTxSdBytes,
        tmnxVdoIfStHghRTSvrTxSdPackets,
        tmnxVdoIfStHghRTSvrTxHdRTReplies,
        tmnxVdoIfStHghRTSvrTxHdBytes,
        tmnxVdoIfStHghRTSvrTxHdPackets,
        tmnxVdoIfStHghRTSvrTxPipRTReplis,
        tmnxVdoIfStHghRTSvrTxPipBytes,
        tmnxVdoIfStHghRTSvrTxPipPackets,
        tmnxVdoIfStHghFCCSrRxSdFCCReq,
        tmnxVdoIfStHghFCCSrRxSdFailedReq,
        tmnxVdoIfStHghFCCSrRxHdFCCReq,
        tmnxVdoIfStHghFCCSrRxHdFailedReq,
        tmnxVdoIfStHghFCCSrRxPipFCCReq,
        tmnxVdoIfStHghFCCSrRxPipFailedRq,
        tmnxVdoIfStHghFCCSrTxSdFCCReplis,
        tmnxVdoIfStHghFCCSrTxSdBytes,
        tmnxVdoIfStHghFCCSrTxSdPackets,
        tmnxVdoIfStHghFCCSrTxHdFCCReplis,
        tmnxVdoIfStHghFCCSrTxHdBytes,
        tmnxVdoIfStHghFCCSrTxHdPackets,
        tmnxVdoIfStHghFCCSrTxPipFCCRplis,
        tmnxVdoIfStHghFCCSrTxPipBytes,
        tmnxVdoIfStHghFCCSrTxPipPackets,
        tmnxVdoIfStHghTxFailedPackets,
        tmnxVdoPIDType,
        tmnxVdoPIDMpegStreamType,
        tmnxVdoPIDLanguage
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting FCC or RD statistics on version 23.0
         of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 24 }

tmnxVdoStatsV23v0ObsoletedGroup  OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpSrcRTClientAdminState,
        tmnxVdoGrpSrcRTClntRTSvrAddrType,
        tmnxVdoGrpSrcRTClntRTSvrAddr,
        tmnxVdoGrpSrcRTClientRTSrvrPort,
        tmnxVdoGrpSrcRTClientRxReTxBytes,
        tmnxVdoGrpSrcRTClientRxReTxPkts,
        tmnxVdoGrpSrcRTClientTxRTReq,
        tmnxVdoGrpSrcRTClientTxRTReqReTx,
        tmnxVdoGrpSrcRTClientGapsDetectd,
        tmnxVdoGrpSrcRTClientFailedReq,
        tmnxVdoGrpSrcRTClientPort,
        tmnxVdoIfScte30TcpSessions,
        tmnxVdoIfScte30InitSessions,
        tmnxVdoSGSpliceAdServerAddrType,
        tmnxVdoSGSpliceAdServerAddr,
        tmnxVdoSGSpliceStatus,
        tmnxVdoSGSpliceDurationReq,
        tmnxVdoSGSpliceDurationPlayed,
        tmnxVdoSGSpliceRate,
        tmnxVdoSGSpliceSessionId,
        tmnxVdoSGSplicePriorSessionId,
        tmnxVdoSGSpliceAbortReason,
        tmnxVdoSGSpliceSpliceInSeqNum,
        tmnxVdoSGSpliceSpliceOutSeqNum,
        tmnxVdoSGSpliceNumBlkFrames,
        tmnxVdoSGSpliceBlkFramePTS,
        tmnxVdoSGSpliceMaxAdPTS,
        tmnxVdoSGSpliceMinNwPTS,
        tmnxVdoSGAdiServerUptime,
        tmnxVdoSGAdiInitReq,
        tmnxVdoSGAdiSucInitResp,
        tmnxVdoSGAdiUnsucInitResp,
        tmnxVdoSGAdiAliveReq,
        tmnxVdoSGAdiSucAliveResp,
        tmnxVdoSGAdiUnSucAliveResp,
        tmnxVdoSGAdiCueReq,
        tmnxVdoSGAdiSucCueResp,
        tmnxVdoSGAdiUnsucCueResp,
        tmnxVdoSGAdiAbortReq,
        tmnxVdoSGAdiSucAbortResp,
        tmnxVdoSGAdiUnsucAbortResp,
        tmnxVdoSGAdiUnknownSCTE30Req,
        tmnxVdoSGAdiSpliceReq,
        tmnxVdoSGAdiSucSpliceResp,
        tmnxVdoSGAdiUnsucSpliceResp,
        tmnxVdoSGAdiSucSpliceInCompResp,
        tmnxVdoSGAdiSucSpliceOutCompResp,
        tmnxVdoSGAdiUnsucSpliceOutComRes,
        tmnxVdoSGAdiMinPort,
        tmnxVdoSGAdiMaxPort,
        tmnxVdoSGAdiChlName
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted objects for FCC or RD or ADI statistics on
         version 23.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 25 }

tmnxVdoGrpV23v0Group             OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpDescription,
        tmnxVdoGrpAdminState,
        tmnxVdoGrpOperState,
        tmnxVdoGrpLocalRTServerState,
        tmnxVdoGrpFCCServerState,
        tmnxVdoGrpRowStatus,
        tmnxVdoGrpLastChanged,
        tmnxVdoGrpMdaRowStatus,
        tmnxVdoGrpMdaAdminState,
        tmnxVdoGrpMdaOperState,
        tmnxVdoGrpMdaUsedMemory,
        tmnxVdoGrpMdaAvailableMemory,
        tmnxVdoGrpMdaChannels,
        tmnxVdoGrpMdaChannelAllocFails,
        tmnxVdoGrpMdaMaxBwExceeded,
        tmnxVdoGrpMdaBwInUse,
        tmnxVdoGrpMdaActiveRtcpSessions,
        tmnxVdoGrpMdaEgressStreamResets,
        tmnxVdoGrpMdaIngressStreamResets,
        tmnxVdoGrpMdaSsrcCollisions,
        tmnxVdoGrpMdaRxDataPackets,
        tmnxVdoGrpMdaRxDataPacketsLow32,
        tmnxVdoGrpMdaRxDataPacketsHigh32,
        tmnxVdoGrpMdaRxDataOctets,
        tmnxVdoGrpMdaRxDataOctetsLow32,
        tmnxVdoGrpMdaRxDataOctetsHigh32,
        tmnxVdoGrpMdaRxDataPacketErrors,
        tmnxVdoGrpMdaRxDataPktErrsLow32,
        tmnxVdoGrpMdaRxDataPktErrsHigh32,
        tmnxVdoGrpMdaTxDataPackets,
        tmnxVdoGrpMdaTxDataPacketsLow32,
        tmnxVdoGrpMdaTxDataPacketsHigh32,
        tmnxVdoGrpMdaTxDataOctets,
        tmnxVdoGrpMdaTxDataOctetsLow32,
        tmnxVdoGrpMdaTxDataOctetsHigh32,
        tmnxVdoGrpMdaTxDataPacketErrors,
        tmnxVdoGrpMdaTxDataPktErrsLow32,
        tmnxVdoGrpMdaTxDataPktErrsHigh32,
        tmnxVdoGrpMdaRtcpParseErrors,
        tmnxVdoGrpMdaRtcpConfigErrors,
        tmnxVdoGrpMdaRtcpIpcErrors,
        tmnxVdoGrpMdaRtcpSgErrors,
        tmnxVdoGrpMdaRtcpSubErrors,
        tmnxVdoGrpMdaRtcpIntErrors,
        tmnxVdoGrpMdaTxLostPackets,
        tmnxVdoGrpMdaRequestedRtpPkts,
        tmnxVdoGrpMdaHighPktPoolLimitHit,
        tmnxVdoGrpMdaMallocFailures,
        tmnxVdoGrpMdaDentDroppedPkts
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of video groups on version
         23.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 26 }

tmnxVdoGrpV23v0ObsoletedGroup    OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpADIServerState,
        tmnxVdoGrpEnableRtClient,
        tmnxVdoGrpMdaAdStreamResets,
        tmnxVdoGrpMdaAdStreamAborts
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted objects in management of video groups on
         version 23.0 of the Nokia SROS series systems."
    ::= { tmnxVdoGroups 27 }

tmnxVdoGrpEsaV23v0Group          OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpVappTableLastChanged,
        tmnxVdoGrpVappRowStatus,
        tmnxVdoGrpVappAdminState,
        tmnxVdoGrpVappOperState,
        tmnxVdoGrpVappUsedMemory,
        tmnxVdoGrpVappAvailableMemory,
        tmnxVdoGrpVappChannels,
        tmnxVdoGrpVappChannelAllocFails,
        tmnxVdoGrpVappMaxBwExceeded,
        tmnxVdoGrpVappBwInUse,
        tmnxVdoGrpVappActiveRtcpSessions,
        tmnxVdoGrpVappEgressStreamResets,
        tmnxVdoGrpVappIngrssStreamResets,
        tmnxVdoGrpVappSsrcCollisions,
        tmnxVdoGrpVappRxDataPackets,
        tmnxVdoGrpVappRxDataPacketsLow32,
        tmnxVdoGrpVappRxDataPacketsHi32,
        tmnxVdoGrpVappRxDataOctets,
        tmnxVdoGrpVappRxDataOctetsLow32,
        tmnxVdoGrpVappRxDataOctetsHigh32,
        tmnxVdoGrpVappRxDataPacketErrors,
        tmnxVdoGrpVappRxDataPktErrsLow32,
        tmnxVdoGrpVappRxDataPktErrsHi32,
        tmnxVdoGrpVappTxDataPackets,
        tmnxVdoGrpVappTxDataPacketsLow32,
        tmnxVdoGrpVappTxDataPacketsHi32,
        tmnxVdoGrpVappTxDataOctets,
        tmnxVdoGrpVappTxDataOctetsLow32,
        tmnxVdoGrpVappTxDataOctetsHigh32,
        tmnxVdoGrpVappTxDataPacketErrors,
        tmnxVdoGrpVappTxDataPktErrsLow32,
        tmnxVdoGrpVappTxDataPktErrsHi32,
        tmnxVdoGrpVappRtcpParseErrors,
        tmnxVdoGrpVappRtcpConfigErrors,
        tmnxVdoGrpVappRtcpIpcErrors,
        tmnxVdoGrpVappRtcpSgErrors,
        tmnxVdoGrpVappRtcpSubErrors,
        tmnxVdoGrpVappRtcpIntErrors,
        tmnxVdoGrpVappTxLostPackets,
        tmnxVdoGrpVappRequestedRtpPkts,
        tmnxVdoGrpVappHiPktPoolLimitHit,
        tmnxVdoGrpVappMallocFailures,
        tmnxVdoGrpVappDentDroppedPkts,
        tmnxVdoGrpVappBwPeak,
        tmnxVdoGrpVappCurTotalRetBw,
        tmnxVdoGrpVappPeakRetBw,
        tmnxVdoGrpVappCurFccBw,
        tmnxVdoGrpVappFccDropCntReq,
        tmnxVdoGrpVappMcRtcp,
        tmnxVdoGrpVappMcRtcpLow32,
        tmnxVdoGrpVappMcRtcpHigh32,
        tmnxVdoGrpVappMcRudp,
        tmnxVdoGrpVappMcRudpLow32,
        tmnxVdoGrpVappMcRudpHigh32,
        tmnxVdoGrpVappMcRetReqCrt,
        tmnxVdoGrpVappMcRetReqCrtLow32,
        tmnxVdoGrpVappMcRetReqCrtHigh32,
        tmnxVdoGrpVappRetReqQnc,
        tmnxVdoGrpVappRetReqQncLow32,
        tmnxVdoGrpVappRetReqQncHigh32,
        tmnxVdoGrpVappPktsLostInSeq10,
        tmnxVdoGrpVappPktsLostInSeq20,
        tmnxVdoGrpVappPktsLostInSeq30,
        tmnxVdoGrpVappPktsLostInSeq40,
        tmnxVdoGrpVappPktsLostInSeqMore,
        tmnxVdoGrpVappPeakFccBw,
        tmnxVdoGrpVappPeakFccBwTime,
        tmnxVdoGrpVappPeakAbsRetBw,
        tmnxVdoGrpVappPeakAbsRetBwTime,
        tmnxVdoGrpVappPeakFccSession,
        tmnxVdoGrpVappPeakFccSessionTime,
        tmnxVdoGrpVappPeakRetSession,
        tmnxVdoGrpVappPeakRetSessionTime,
        tmnxVdoGrpVappPeakFccRetTotBw,
        tmnxVdoGrpVappPkFccRetTotBwTime,
        tmnxVdoGrpVappPeakFccRetTotSess,
        tmnxVdoGrpVappPkFccRetTotSeTime,
        tmnxVdoGrpVappCurAbsRetBw,
        tmnxVdoGrpVappCurFccRetTotalBw,
        tmnxVdoGrpVappActFccSess,
        tmnxVdoGrpVappActRetSess,
        tmnxVdoGrpVappActFccRetTotalSess,
        tmnxVdoGrpVappLhPkFccBw,
        tmnxVdoGrpVappLhPkFccBwTime,
        tmnxVdoGrpVappLhPkAbsRetBw,
        tmnxVdoGrpVappLhPkAbsRetBwTime,
        tmnxVdoGrpVappLhPkFccSession,
        tmnxVdoGrpVappLhPkFccSessionTime,
        tmnxVdoGrpVappLhPkRetSession,
        tmnxVdoGrpVappLhPkRetSessionTime,
        tmnxVdoGrpVappLhPkFccRetTotBw,
        tmnxVdoGrpVappLPFccRetTotBwTime,
        tmnxVdoGrpVappLhPkFccRetTotSess,
        tmnxVdoGrpVappLPFccRetTotSeTime,
        tmnxVdoGrpVappChPkFccBw,
        tmnxVdoGrpVappChPkFccBwTime,
        tmnxVdoGrpVappChPkAbsRetBw,
        tmnxVdoGrpVappChPkAbsRetBwTime,
        tmnxVdoGrpVappChPkFccSession,
        tmnxVdoGrpVappChPkFccSessionTime,
        tmnxVdoGrpVappChPkRetSession,
        tmnxVdoGrpVappChPkRetSessionTime,
        tmnxVdoGrpVappChPkFccRetTotBw,
        tmnxVdoGrpVappCPFccRetTotBwTime,
        tmnxVdoGrpVappChPkFccRetTotSess,
        tmnxVdoGrpVappCPFccRetTotSeTime
    }
    STATUS      current
    DESCRIPTION
        "The group of objects providing configuration of video Extended Service
         Adaptor (ESA) on Nokia SROS series systems release 23.0 or higher."
    ::= { tmnxVdoGroups 28 }

tmnxVdoGrpEsaV23v0ObsoletedGroup OBJECT-GROUP
    OBJECTS     {
        tmnxVdoGrpVappAdStreamResets,
        tmnxVdoGrpVappAdStreamAborts
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted objects providing configuration of video
         Extended Service Adaptor (ESA) on Nokia SROS series systems release
         23.0 or higher."
    ::= { tmnxVdoGroups 29 }

tmnxVdoNotifyPrefix              OBJECT IDENTIFIER ::= { tmnxSRNotifyPrefix 61 }

tmnxVdoNotifications             OBJECT IDENTIFIER ::= { tmnxVdoNotifyPrefix 0 }

tmnxVdoDuplicateSsrcId           NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpSrcSSRCId
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoDuplicateSsrcId notification is generated for a video channel
         if it has a synchronization source (SSRC) identifier that conflicts
         with another channel's SSRC identifier."
    ::= { tmnxVdoNotifications 1 }

tmnxVdoMdaSessionsLimitExceeded  NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaActiveRtcpSessions
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaSessionsLimitExceeded notification is generated when the
         configuration exceeds the maximum number of Real Time Transport
         Control Protocol (RTCP) sessions supported by a video Media Dependent
         Adapter (MDA)."
    ::= { tmnxVdoNotifications 2 }

tmnxVdoMdaSGLimitExceeded        NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaChannels
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaSGLimitExceeded notification is generated when the
         configuration exceeds the maximum number of channels supported by a
         video Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 3 }

tmnxVdoMdaSessionsLimitCleared   NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaActiveRtcpSessions
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaSessionsLimitCleared notification is generated after a
         tmnxVdoMdaSessionsLimitExceeded notification when the number of Real
         Time Transport Control Protocol (RTCP) sessions goes back down to the
         limit supported by a video Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 4 }

tmnxVdoMdaSGLimitCleared         NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaChannels
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaSGLimitCleared notification is generated after a
         tmnxVdoMdaSGLimitExceeded notification when the number of channels
         goes back down to the limit supported by a video Media Dependent
         Adapter (MDA)."
    ::= { tmnxVdoNotifications 5 }

tmnxVdoAdSpliceAbort             NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoNotifysvcId,
        tmnxVdoNotifyIfName,
        tmnxVdoNotifyGrpAddrType,
        tmnxVdoNotifyGroupAddress,
        tmnxVdoNotifySrcAddrType,
        tmnxVdoNotifySourceAddress,
        tmnxVdoNotifyAdSpliceSessionId,
        tmnxVdoNotifyAdSpliceAbortTime,
        tmnxVdoNotifyAdSpliceDuration
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoAdSpliceAbort notification is generated when an ad splice is
         aborted."
    ::= { tmnxVdoNotifications 6 }

tmnxVdoClientSessionsLmtExceeded NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoNotifyClientAddrType,
        tmnxVdoNotifyClientAddress
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoClientSessionsLmtExceeded notification is generated when the
         number of Real Time Transport Control Protocol (RTCP) sessions per
         client IP address exceeds the limit supported by a video Media
         Dependent Adapter (MDA).

         The maximum number of RTCP sessions per client IP address supported by
         video MDA is specified by the value of the corresponding
         TIMETRA-MCAST-PATH-MGMT-MIB::tmnxMcPathVdoPlcyMaxClntSessions object."
    ::= { tmnxVdoNotifications 7 }

tmnxVdoClientSessionsLmtCleared  NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoNotifyClientAddrType,
        tmnxVdoNotifyClientAddress
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoClientSessionsLmtCleared notification is generated after a
         tmnxVdoClientSessionsLmtExceeded notification when the number of Real
         Time Transport Control Protocol (RTCP) sessions per client IP address
         goes back down to the limit supported by a video Media Dependent
         Adapter (MDA).

         The maximum number of RTCP sessions per client IP address supported by
         video MDA is specified by the value of the corresponding
         TIMETRA-MCAST-PATH-MGMT-MIB::tmnxMcPathVdoPlcyMaxClntSessions object."
    ::= { tmnxVdoNotifications 8 }

tmnxVdoGrpSrcAnlyzrErrState      NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoNotifysvcId,
        tmnxVdoNotifyIfName,
        tmnxVdoNotifyGrpAddrType,
        tmnxVdoNotifyGroupAddress,
        tmnxVdoNotifySrcAddrType,
        tmnxVdoNotifySourceAddress,
        tmnxVdoNotifyAnalyzerState
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The tmnxVdoGrpSrcAnlyzrErrState notification is raised
         whenever a video channel analyzer's error state changes to one of
         these values - TNC (Tech Non-Conformance), QOS (Quality of Service),
         POA (Program off Air).

         [EFFECT] This trap is informational. No effects are caused by this
         trap.

         [RECOVERY] No recovery mechanism is required."
    ::= { tmnxVdoNotifications 9 }

tmnxVdoGrpSrcAnlyzrStClear       NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoNotifysvcId,
        tmnxVdoNotifyIfName,
        tmnxVdoNotifyGrpAddrType,
        tmnxVdoNotifyGroupAddress,
        tmnxVdoNotifySrcAddrType,
        tmnxVdoNotifySourceAddress
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The tmnxVdoGrpSrcAnlyzrStClear notification is raised whenever
         a video channel analyzer's error state has recovered from past errors
         and is good for the last 10 seconds.

         [EFFECT] This trap is informational. No effects are caused by this
         trap.

         [RECOVERY] No recovery mechanism is required."
    ::= { tmnxVdoNotifications 10 }

tmnxVdoMdaFccBwLimitExceeded     NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaCurFccBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaFccBwLimitExceeded notification is generated when the
         egress bandwidth for FCC (Fast Channel Change) exceeds the high
         watermark level configured for a video Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 11 }

tmnxVdoMdaFccBwLimitCleared      NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaCurFccBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaFccBwLimitCleared notification is generated after a
         tmnxVdoMdaFccBwLimitExceeded notification when the egress FCC (Fast
         Channel Change) bandwidth retreats by 10% from the high watermark
         level configured for a video Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 12 }

tmnxVdoMdaRetBwLimitExceeded     NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaCurAbsRetBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaRetBwLimitExceeded notification is generated when the
         egress bandwidth for RET (Retransmission) exceeds the high watermark
         level configured for a video Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 13 }

tmnxVdoMdaRetBwLimitCleared      NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaCurAbsRetBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaRetBwLimitCleared notification is generated after a
         tmnxVdoMdaRetBwLimitExceeded notification when the egress RET
         (Retransmission) bandwidth retreats by 10% from the high watermark
         level configured for a video Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 14 }

tmnxVdoMdaFccRetTotBwLmtExceeded NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaCurFccRetTotalBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaFccRetTotBwLmtExceeded notification is generated when the
         total egress bandwidth for RET (Retransmission) and FCC (Fast Channel
         Change) exceeds the high watermark level configured for a video Media
         Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 15 }

tmnxVdoMdaFccRetTotBwLmtCleared  NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaCurFccRetTotalBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaFccRetTotBwLmtCleared notification is generated after a
         tmnxVdoMdaFccRetTotBwLmtExceeded notification when the total egress
         bandwidth for RET (Retransmission) and FCC (Fast Channel Change)
         retreats by 10% from the high watermark level configured for a video
         Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 16 }

tmnxVdoMdaFccSesLimitExceeded    NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaActFccSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaFccSesLimitExceeded notification is generated when the
         number of Real Time Transport Control Protocol (RTCP) sessions
         allocated for FCC (Fast Channel Change) exceeds the high watermark
         level configured for a video Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 17 }

tmnxVdoMdaFccSesLimitCleared     NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaActFccSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaFccSesLimitCleared notification is generated after a
         tmnxVdoMdaFccSesLimitExceeded notification when the number of Real
         Time Transport Control Protocol (RTCP) sessions allocated for FCC
         (Fast Channel Change) retreats by 10% from the high watermark level
         configured for a video Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 18 }

tmnxVdoMdaRetSesLimitExceeded    NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaActRetSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaRetSesLimitExceeded notification is generated when the
         number of Real Time Transport Control Protocol (RTCP) sessions
         allocated for RET (Retransmission) exceeds the high watermark level
         configured for a video Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 19 }

tmnxVdoMdaRetSesLimitCleared     NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaActRetSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaRetSesLimitCleared notification is generated after a
         tmnxVdoMdaRetSesLimitExceeded notification when the number of Real
         Time Transport Control Protocol (RTCP) sessions allocated for RET
         (Retransmission) retreats by 10% from the high watermark level
         configured for a video Media Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 20 }

tmnxVdoMdaFccRetTotSeLmtExceeded NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaActFccRetTotalSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaFccRetTotSeLmtExceeded notification is generated when the
         total number of Real Time Transport Control Protocol (RTCP) sessions
         exceeds the high watermark level configured for a video Media
         Dependent Adapter (MDA)."
    ::= { tmnxVdoNotifications 21 }

tmnxVdoMdaFccRetTotSeLmtCleared  NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpMdaActFccRetTotalSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoMdaFccRetTotSeLmtCleared notification is generated after a
         tmnxVdoMdaFccRetTotSeLmtExceeded notification when the number of Real
         Time Transport Control Protocol (RTCP) sessions retreats by 10% from
         the high watermark level configured for a video Media Dependent
         Adapter (MDA)."
    ::= { tmnxVdoNotifications 22 }

tmnxVdoVappSessionsLimitExceeded NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappActiveRtcpSessions
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappSessionsLimitExceeded notification is generated when the
         configuration exceeds the maximum number of Real Time Transport
         Control Protocol (RTCP) sessions supported by a video Virtual
         Application (VAPP)."
    ::= { tmnxVdoNotifications 23 }

tmnxVdoVappSGLimitExceeded       NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappChannels
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappSGLimitExceeded notification is generated when the
         configuration exceeds the maximum number of channels supported by a
         video Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 24 }

tmnxVdoVappSessionsLimitCleared  NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappActiveRtcpSessions
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappSessionsLimitCleared notification is generated after a
         tmnxVdoVappSessionsLimitExceeded notification when the number of Real
         Time Transport Control Protocol (RTCP) sessions goes back down to the
         limit supported by a video Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 25 }

tmnxVdoVappSGLimitCleared        NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappChannels
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappSGLimitCleared notification is generated after a
         tmnxVdoVappSGLimitExceeded notification when the number of channels
         goes back down to the limit supported by a video Virtual Application
         (VAPP)."
    ::= { tmnxVdoNotifications 26 }

tmnxVdoVappFccBwLimitExceeded    NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappCurFccBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappFccBwLimitExceeded notification is generated when the
         egress bandwidth for FCC (Fast Channel Change) exceeds the high
         watermark level configured for a video Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 27 }

tmnxVdoVappFccBwLimitCleared     NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappCurFccBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappFccBwLimitCleared notification is generated after a
         tmnxVdoVappFccBwLimitExceeded notification when the egress FCC (Fast
         Channel Change) bandwidth retreats by 10% from the high watermark
         level configured for a video Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 28 }

tmnxVdoVappRetBwLimitExceeded    NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappCurAbsRetBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappRetBwLimitExceeded notification is generated when the
         egress bandwidth for RET (Retransmission) exceeds the high watermark
         level configured for a video Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 29 }

tmnxVdoVappRetBwLimitCleared     NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappCurAbsRetBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappRetBwLimitCleared notification is generated after a
         tmnxVdoVappRetBwLimitExceeded notification when the egress RET
         (Retransmission) bandwidth retreats by 10% from the high watermark
         level configured for a video Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 30 }

tmnxVdoVappFccRetTotBwLmtExceded NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappCurFccRetTotalBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappFccRetTotBwLmtExceded notification is generated when the
         total egress bandwidth for RET (Retransmission) and FCC (Fast Channel
         Change) exceeds the high watermark level configured for a video
         Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 31 }

tmnxVdoVappFccRetTotBwLmtCleared NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappCurFccRetTotalBw
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappFccRetTotBwLmtCleared notification is generated after a
         tmnxVdoVappFccRetTotBwLmtExceded notification when the total egress
         bandwidth for RET (Retransmission) and FCC (Fast Channel Change)
         retreats by 10% from the high watermark level configured for a video
         Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 32 }

tmnxVdoVappFccSesLimitExceeded   NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappActFccSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappFccSesLimitExceeded notification is generated when the
         number of Real Time Transport Control Protocol (RTCP) sessions
         allocated for FCC (Fast Channel Change) exceeds the high watermark
         level configured for a video Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 33 }

tmnxVdoVappFccSesLimitCleared    NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappActFccSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappFccSesLimitCleared notification is generated after a
         tmnxVdoVappFccSesLimitExceeded notification when the number of Real
         Time Transport Control Protocol (RTCP) sessions allocated for FCC
         (Fast Channel Change) retreats by 10% from the high watermark level
         configured for a video Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 34 }

tmnxVdoVappRetSesLimitExceeded   NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappActRetSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappRetSesLimitExceeded notification is generated when the
         number of Real Time Transport Control Protocol (RTCP) sessions
         allocated for RET (Retransmission) exceeds the high watermark level
         configured for a video Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 35 }

tmnxVdoVappRetSesLimitCleared    NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappActRetSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappRetSesLimitCleared notification is generated after a
         tmnxVdoVappRetSesLimitExceeded notification when the number of Real
         Time Transport Control Protocol (RTCP) sessions allocated for RET
         (Retransmission) retreats by 10% from the high watermark level
         configured for a video Virtual Application (VAPP)."
    ::= { tmnxVdoNotifications 36 }

tmnxVdoVappFccRetTotSeLmtExceded NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappActFccRetTotalSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappFccRetTotSeLmtExceded notification is generated when the
         total number of Real Time Transport Control Protocol (RTCP) sessions
         exceeds the high watermark level configured for a video Virtual
         Application (VAPP)."
    ::= { tmnxVdoNotifications 37 }

tmnxVdoVappFccRetTotSeLmtCleared NOTIFICATION-TYPE
    OBJECTS     {
        tmnxVdoGrpVappActFccRetTotalSess
    }
    STATUS      current
    DESCRIPTION
        "A tmnxVdoVappFccRetTotSeLmtCleared notification is generated after a
         tmnxVdoVappFccRetTotSeLmtExceded notification when the number of Real
         Time Transport Control Protocol (RTCP) sessions retreats by 10% from
         the high watermark level configured for a video Virtual Application
         (VAPP)."
    ::= { tmnxVdoNotifications 38 }

END
