-- Extracted from rfc3593.txt
--
PerfHist-TC-MIB DEFINITIONS ::= BEGIN

   IMPORTS
      MODULE-IDENTITY,
      Gauge32, mib-2
          FROM SNMPv2-SMI
      TEXTUAL-CONVENTION
          FROM SNMPv2-TC;

   perfHistTCMIB MODULE-IDENTITY
        LAST-UPDATED "200308130000Z"
        ORGANIZATION "IETF AToM MIB WG"
        CONTACT-INFO
           "WG charter:
              http://www.ietf.org/html.charters/atommib-charter.html

            Mailing Lists:
              General Discussion: atommib@research.telcordia.com
              To Subscribe: atommib-request@research.telcordia.com

            Editor:  Kaj Tesink
            Postal:  Telcordia Technologies
                     331 Newman Springs Road
                     Red Bank, NJ 07701
                     USA
            Tel:     +1 732 758 5254
            E-mail:  kaj@research.telcordia.com"

        DESCRIPTION
         "This MIB Module provides Textual Conventions
          to be used by systems supporting 15 minute
          based performance history counts.

          Copyright (C) The Internet Society (2003).
          This version of this MIB module is part of
          RFC 3593;  see the RFC itself for full
          legal notices."
        REVISION      "200308130000Z"
        DESCRIPTION
         "Contact information and references updated.
          No technical changes have been applied.
          Published as RFC 3593."
        REVISION      "199811071100Z"
        DESCRIPTION
         "The RFC 2493 version of this MIB module."
        ::= { mib-2 58 }

   -- The Textual Conventions defined below are organized
   -- alphabetically

   -- Use of these TCs assumes the following:
   -- 0  The agent supports 15 minute based history
   --    counters.
   -- 0  The agent is capable of keeping a history of n
   --    intervals of 15 minute performance data.  The
   --    value of n is defined by the specific MIB
   --    module but shall be 0 < n =< 96.
   -- 0  The agent may optionally support performance
   --    data aggregating the history intervals.
   -- 0  The agent will keep separate tables for the
   --    current interval, the history intervals, and
   --    the total aggregates.
   -- 0  The agent will keep the following objects.
   --    If performance data is kept for multiple instances
   --    of a measured entity, then
   --    these objects are applied to each instance of
   --    the measured entity (e.g., interfaces).
   --
   -- xyzTimeElapsed OBJECT-TYPE
   --       SYNTAX  INTEGER (0..899)
   --       MAX-ACCESS  read-only
   --       STATUS  current
   --       DESCRIPTION
   --       "The number of seconds that have elapsed since
   --       the beginning of the current measurement period.
   --       If, for some reason, such as an adjustment in the
   --       system's time-of-day clock, the current interval
   --       exceeds the maximum value, the agent will return
   --       the maximum value."
   --       ::= { xxx }

   -- xyzValidIntervals OBJECT-TYPE
   --       SYNTAX  INTEGER (0..<n>)
   --       MAX-ACCESS  read-only
   --       STATUS  current
   --       DESCRIPTION
   --       "The number of previous near end intervals
   --       for which data was collected.
   --          [ The overall constraint on <n> is 1 =< n =< 96; ]
   --          [ Define any additional constraints on <n> here. ]
   --       The value will be <n> unless the measurement was
   --       (re-)started within the last (<n>*15) minutes, in which
   --       case the value will be the number of complete 15
   --       minute intervals for which the agent has at least
   --       some data.  In certain cases (e.g., in the case
   --       where the agent is a proxy) it is possible that some
   --       intervals are unavailable.  In this case, this
   --       interval is the maximum interval number for
   --       which data is available."
   --       ::= { xxx }

   -- xyzInvalidIntervals OBJECT-TYPE
   --     SYNTAX  INTEGER (0..<n>)
   --     MAX-ACCESS  read-only
   --     STATUS  current
   --     DESCRIPTION
   --       "The number of intervals in the range from
   --        0 to xyzValidIntervals for which no
   --        data is available.  This object will typically
   --        be zero except in cases where the data for some
   --        intervals are not available (e.g., in proxy
   --        situations)."
   --       ::= { xxx }

   PerfCurrentCount ::= TEXTUAL-CONVENTION
         STATUS  current
         DESCRIPTION
            "A counter associated with a
             performance measurement in a current 15
             minute measurement interval.  The value
             of this counter starts from zero and is
             increased when associated events occur,
             until the end of the 15 minute interval.
             At that time the value of the counter is
             stored in the first 15 minute history
             interval, and the CurrentCount is
             restarted at zero.  In the
             case where the agent has no valid data
             available for the current interval the
             corresponding object instance is not
             available and upon a retrieval request
             a corresponding error message shall be
             returned to indicate that this instance
             does not exist (for example, a noSuchName
             error for SNMPv1 and a noSuchInstance for
             SNMPv2 GET operation)."
          SYNTAX  Gauge32

   PerfIntervalCount ::= TEXTUAL-CONVENTION
         STATUS  current
         DESCRIPTION
            "A counter associated with a
             performance measurement in a previous
             15 minute measurement interval.  In the
             case where the agent has no valid data
             available for a particular interval the
             corresponding object instance is not
             available and upon a retrieval request
             a corresponding error message shall be
             returned to indicate that this instance
             does not exist (for example, a noSuchName
             error for SNMPv1 and a noSuchInstance for
             SNMPv2 GET operation).
             In a system supporting
             a history of n intervals with
             IntervalCount(1) and IntervalCount(n) the
             most and least recent intervals
             respectively, the following applies at
             the end of a 15 minute interval:
             - discard the value of IntervalCount(n)
             - the value of IntervalCount(i) becomes that
               of IntervalCount(i-1) for n >= i > 1
             - the value of IntervalCount(1) becomes that
               of CurrentCount
             - the TotalCount, if supported, is adjusted."
          SYNTAX  Gauge32

   PerfTotalCount ::= TEXTUAL-CONVENTION
         STATUS  current
         DESCRIPTION
            "A counter associated with a
             performance measurements aggregating the
             previous valid 15 minute measurement
             intervals.  (Intervals for which no valid
             data was available are not counted)"
          SYNTAX  Gauge32

   END

