TIMETRA-PPPOE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    InterfaceIndexOrZero
                                                         FROM IF-MIB
    InetAddress, InetAddressIPv4,
    InetAddressPrefixLength,
    InetAddressType,
    InetAutonomousSystemNumber
                                                         FROM INET-ADDRESS-MIB
    MODULE-COMPLIANCE, NOTIFICATION-GROUP,
    OBJECT-GROUP
                                                         FROM SNMPv2-CONF
    Counter32, Counter64, Gauge32,
    Integer32, MODULE-IDENTITY,
    NOTIFICATION-TYPE, OBJECT-TYPE,
    TimeTicks, Unsigned32
                                                         FROM SNMPv2-SMI
    DisplayString, MacAddress, RowStatus,
    TEXTUAL-CONVENTION, TimeStamp,
    TruthValue
                                                         FROM SNMPv2-TC
    tmnxCardSlotNum, tmnxChassisIndex,
    tmnxMDASlotNum
                                                         FROM TIMETRA-CHASSIS-MIB
    timetraSRMIBModules, tmnxSRConfs,
    tmnxSRNotifyPrefix, tmnxSRObjs
                                                         FROM TIMETRA-GLOBAL-MIB
    tmnxNatEsaNum, tmnxNatEsaVappNum,
    tmnxNatIsaGrpId
                                                         FROM TIMETRA-NAT-MIB
    sapEncapValue, sapPortId
                                                         FROM TIMETRA-SAP-MIB
    iesIfIndex, svcId
                                                         FROM TIMETRA-SERV-MIB
    tmnxSubPppIndex
                                                         FROM TIMETRA-SUBSCRIBER-MGMT-MIB
    BgpPeeringStatus,
    TBurstSizeBytesOverride,
    TCIRRateOverride, TDirectionIngEgr,
    TItemDescription, TNamedItem,
    TNamedItemOrEmpty, TPIRRateOverride,
    TPolicyStatementNameOrEmpty,
    TQosOverrideType,
    TmnxAccessLoopEncapDataLink,
    TmnxAccessLoopEncaps1,
    TmnxAccessLoopEncaps2,
    TmnxAncpStringOrZero,
    TmnxAppProfileStringOrEmpty,
    TmnxAuthPassword, TmnxDhcpOptionType,
    TmnxManagedRouteStatus,
    TmnxMlpppEpClass, TmnxPppCpState,
    TmnxPppoePadoDelay, TmnxPppoeSessionId,
    TmnxPppoeSessionInfoOrigin,
    TmnxPppoeSessionType, TmnxPppoeUserName,
    TmnxPppoeUserNameOrEmpty, TmnxServId,
    TmnxSlaProfileStringOrEmpty,
    TmnxSubIdentStringOrEmpty,
    TmnxSubMgtIntDestIdOrEmpty,
    TmnxSubProfileStringOrEmpty, TmnxVRtrID,
    TmnxVRtrIDOrZero
                                                         FROM TIMETRA-TC-MIB
    ;

timetraPppoeMIBModule            MODULE-IDENTITY
    LAST-UPDATED "201904010000Z"
    ORGANIZATION "Nokia"
    CONTACT-INFO
        "Nokia SROS Support
         Web: http://www.nokia.com"
    DESCRIPTION
        "This document is the SNMP MIB module to manage and provision the PPP
         over Ethernet (PPPoE) for the Nokia SROS device.

         Copyright 2008-2018 Nokia. All rights reserved. Reproduction of this
         document is authorized on the condition that the foregoing copyright
         notice is included.

         This SNMP MIB module (Specification) embodies Nokia's proprietary
         intellectual property. Nokia retains all title and ownership in the
         Specification, including any revisions.

         Nokia grants all interested parties a non-exclusive license to use and
         distribute an unmodified copy of this Specification in connection with
         management of Nokia products, and without fee, provided this copyright
         notice and license appear on all copies.

         This Specification is supplied 'as is', and Nokia makes no warranty,
         either express or implied, as to the use, operation, condition, or
         performance of the Specification."

    REVISION    "201904010000Z"
    DESCRIPTION
        "Rev 19.0                1 April 2019 00:00
         19.0 release of the TIMETRA-PPPOE-MIB."

    REVISION    "201701010000Z"
    DESCRIPTION
        "Rev 15.0                1 Jan 2017 00:00
         15.0 release of the TIMETRA-PPPOE-MIB."

    REVISION    "201601010000Z"
    DESCRIPTION
        "Rev 14.0                1 Jan 2016 00:00
         14.0 release of the TIMETRA-PPPOE-MIB."

    REVISION    "201501010000Z"
    DESCRIPTION
        "Rev 13.0                1 Jan 2015 00:00
         13.0 release of the TIMETRA-PPPOE-MIB."

    REVISION    "201401010000Z"
    DESCRIPTION
        "Rev 12.0                1 Jan 2014 00:00
         12.0 release of the TIMETRA-PPPOE-MIB."

    REVISION    "201102010000Z"
    DESCRIPTION
        "Rev 7.0                28 Feb 2009 00:00
         7.0 release of the TIMETRA-PPPOE-MIB."

    REVISION    "200902280000Z"
    DESCRIPTION
        "Rev 9.0                 1 Feb 2011 00:00
         9.0 release of the TIMETRA-PPPOE-MIB."

    REVISION    "200807010000Z"
    DESCRIPTION
        "Rev 6.1                01 Jul 2008 00:00
         6.1 release of the TIMETRA-PPPOE-MIB."

    REVISION    "200801010000Z"
    DESCRIPTION
        "Rev 0.1                01 Jan 2008 00:00
         Initial version of the TIMETRA-PPPOE-MIB."

    ::= { timetraSRMIBModules 49 }

TmnxPppoeAdminStatus             ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TmnxPppoeAdminStatus data type is an enumerated integer that
         describes the values used to identify the administrative state."
    SYNTAX      INTEGER {
        enabled  (1),
        disabled (2)
    }

tmnxPppoe                        OBJECT IDENTIFIER ::= { tmnxSRObjs 49 }

tmnxPppoeObjects                 OBJECT IDENTIFIER ::= { tmnxPppoe 1 }

tmnxPppoePlcyTableLastChanged    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyTableLastChanged indicates the sysUpTime at
         the time of the most recent management-initiated change to the
         tmnxPppoePlcyTable."
    ::= { tmnxPppoeObjects 1 }

tmnxPppoePlcyTable               OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoePlcyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxPppoePlcyTable has an entry for each PPP(oE) policy configured
         in the system.

         This table can be used to configure PPP for PPPoE (PPP over Ethernet)
         and PPPoA (PPP over ATM) subscribers."
    ::= { tmnxPppoeObjects 2 }

tmnxPppoePlcyEntry               OBJECT-TYPE
    SYNTAX      TmnxPppoePlcyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a PPP(oE) policy configured in the system.

         Entries can be created and deleted via SNMP SET operations on the
         object tmnxPppoePlcyRowStatus."
    INDEX       { IMPLIED tmnxPppoePlcyName }
    ::= { tmnxPppoePlcyTable 1 }

TmnxPppoePlcyEntry               ::= SEQUENCE
{
    tmnxPppoePlcyName                TNamedItem,
    tmnxPppoePlcyRowStatus           RowStatus,
    tmnxPppoePlcyLastMgmtChange      TimeStamp,
    tmnxPppoePlcyDescription         TItemDescription,
    tmnxPppoePlcyPppMtu              Unsigned32,
    tmnxPppoePlcyLcpKaInterval       Unsigned32,
    tmnxPppoePlcyLcpKaHoldUpMplier   Unsigned32,
    tmnxPppoePlcyDisableAcCookies    TruthValue,
    tmnxPppoePlcyPadoDelay           TmnxPppoePadoDelay,
    tmnxPppoePlcyMaxSessionsPerMac   Unsigned32,
    tmnxPppoePlcyReplyOnPadt         TruthValue,
    tmnxPppoePlcyPppAuthentication   INTEGER,
    tmnxPppoePlcyPppMinChapChallenge Unsigned32,
    tmnxPppoePlcyPppMaxChapChallenge Unsigned32,
    tmnxPppoePlcyPppInitialDelay     Unsigned32,
    tmnxPppoePlcyPppIpcpSubnetNeg    TruthValue,
    tmnxPppoePlcyPadoAcName          DisplayString,
    tmnxPppoePlcyPppMtuForceGt1492   TruthValue,
    tmnxPppoePlcyUniqueSessIdsPerSap INTEGER,
    tmnxPppoePlcyRejectDisabledNcp   TruthValue,
    tmnxPppoePlcyLcpIgnoreMagic      TruthValue,
    tmnxPppoePlcySessionTimeout      Unsigned32,
    tmnxPppoePlcyAllowSameCidForDhcp TruthValue,
    tmnxPppoePlcyReestablishSession  INTEGER,
    tmnxPppoePlcyDefaultUserName     TmnxPppoeUserNameOrEmpty,
    tmnxPppoePlcyDefaultPapPassword  TmnxAuthPassword,
    tmnxPppoePlcySidAllocation       INTEGER,
    tmnxPppoePlcyMaxSessionsPerCid   Unsigned32,
    tmnxPppoePlcyAllowSessionsWoCid  TruthValue,
    tmnxPppoePlcyNcpRenegotiation    INTEGER,
    tmnxPppoePlcyLcpIgnoreIdentifier TruthValue
}

tmnxPppoePlcyName                OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyName specifies the name of the PPP(oE)
         policy."
    ::= { tmnxPppoePlcyEntry 1 }

tmnxPppoePlcyRowStatus           OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyRowStatus controls the creation and deletion
         of rows in this table."
    ::= { tmnxPppoePlcyEntry 2 }

tmnxPppoePlcyLastMgmtChange      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyLastMgmtChange indicates the sysUpTime at
         the time of the most recent management-initiated change to this table
         row."
    ::= { tmnxPppoePlcyEntry 3 }

tmnxPppoePlcyDescription         OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyDescription specifies the user provided
         description of this PPP policy."
    DEFVAL      { "" }
    ::= { tmnxPppoePlcyEntry 4 }

tmnxPppoePlcyPppMtu              OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 512..9212)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyPppMtu specifies the largest IP packet that
         can be sent out without being fragmented over the specific PPPoE
         tunnel.

         A value of 0 indicates the specific MTU is derived from the interface."
    DEFVAL      { 0 }
    ::= { tmnxPppoePlcyEntry 5 }

tmnxPppoePlcyLcpKaInterval       OBJECT-TYPE
    SYNTAX      Unsigned32 (4..300)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyLcpKaInterval specifies the time interval in
         seconds at which LCP echo requests are transmitted."
    DEFVAL      { 30 }
    ::= { tmnxPppoePlcyEntry 6 }

tmnxPppoePlcyLcpKaHoldUpMplier   OBJECT-TYPE
    SYNTAX      Unsigned32 (1..5)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyLcpKaHoldUpMplier specifies how many LCP
         keepalive messages can be missed before the related PPP session is
         brought down."
    DEFVAL      { 3 }
    ::= { tmnxPppoePlcyEntry 7 }

tmnxPppoePlcyDisableAcCookies    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyDisableAcCookies specifies whether the use of
         AC-Cookie tags during the PPPoE discovery phase is disabled."
    DEFVAL      { false }
    ::= { tmnxPppoePlcyEntry 8 }

tmnxPppoePlcyPadoDelay           OBJECT-TYPE
    SYNTAX      TmnxPppoePadoDelay
    UNITS       "deciseconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyPadoDelay specifies the delay timeout before
         sending a PADO (PPPoE Active Discovery Offer)."
    DEFVAL      { 0 }
    ::= { tmnxPppoePlcyEntry 9 }

tmnxPppoePlcyMaxSessionsPerMac   OBJECT-TYPE
    SYNTAX      Unsigned32 (1..8191)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyMaxSessionsPerMac specifies the maximum number
         of PPPoE sessions that can be created per MAC address."
    DEFVAL      { 1 }
    ::= { tmnxPppoePlcyEntry 10 }

tmnxPppoePlcyReplyOnPadt         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyReplyOnPadt specifies whether the system
         replies with a PADT (PPPoE Active Discovery Terminate) packet when a
         PADT packet is received for an existing PPPoE session."
    DEFVAL      { false }
    ::= { tmnxPppoePlcyEntry 11 }

tmnxPppoePlcyPppAuthentication   OBJECT-TYPE
    SYNTAX      INTEGER {
        pap      (1),
        chap     (2),
        prefChap (3),
        prefPap  (4)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyPppAuthentication specifies what PPP
         authentication protocol(s) will be negotiated during the LCP phase.
         This field is only applicable if PAP/CHAP authentication is enabled
         via configuration of a RADIUS authentication policy or a local user
         database.

         If set to 'pap' or 'chap', only PAP respectively CHAP is negotiated.
         If set to 'prefChap', first CHAP is negotiated followed by PAP. If set
         to 'prefPap', first PAP is negotiated followed by CHAP."
    DEFVAL      { prefChap }
    ::= { tmnxPppoePlcyEntry 12 }

tmnxPppoePlcyPppMinChapChallenge OBJECT-TYPE
    SYNTAX      Unsigned32 (8..64)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyPppMinChapChallenge specifies the minimum
         length of the CHAP challenge generated by the system."
    DEFVAL      { 32 }
    ::= { tmnxPppoePlcyEntry 13 }

tmnxPppoePlcyPppMaxChapChallenge OBJECT-TYPE
    SYNTAX      Unsigned32 (8..64)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyPppMaxChapChallenge specifies the maximum
         length of the CHAP challenge generated by the system."
    DEFVAL      { 64 }
    ::= { tmnxPppoePlcyEntry 14 }

tmnxPppoePlcyPppInitialDelay     OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 5)
    UNITS       "centiseconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyPppInitialDelay specifies the delay before
         starting the PPP stack of a PPPoE session."
    DEFVAL      { 0 }
    ::= { tmnxPppoePlcyEntry 15 }

tmnxPppoePlcyPppIpcpSubnetNeg    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyPppIpcpSubnetNeg specifies if IPCP subnet
         negotiation is enabled."
    DEFVAL      { false }
    ::= { tmnxPppoePlcyEntry 20 }

tmnxPppoePlcyPadoAcName          OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..128))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyPadoAcName specifies the AC-name (Access
         Concentrator's name) tag which will be included in the PADO (PPPoE
         Active Discovery Offer).

         If the empty string is specified, the chassis name
         (TIMETRA-CHASSIS-MIB::tmnxChassisName) will be used as AC-name."
    DEFVAL      { "" }
    ::= { tmnxPppoePlcyEntry 21 }

tmnxPppoePlcyPppMtuForceGt1492   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyPppMtuForceGt1492 specifies for PPPoE sessions
         whether a PPP MTU greater than 1492 can be negotiated without
         following the procedure described in RFC 4638."
    DEFVAL      { false }
    ::= { tmnxPppoePlcyEntry 22 }

tmnxPppoePlcyUniqueSessIdsPerSap OBJECT-TYPE
    SYNTAX      INTEGER {
        perCaptureSap (1),
        disabled      (2),
        perMsap       (3)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyUniqueSessIdsPerSap specifies whether each
         PPPoE session on the same SAP gets a unique session-id.

         The value 'disabled' specifies that sessions belonging to the same SAP
         do not get a unique session-id. The session-id gets allocated the
         default way, meaning that the combination MAC address plus session-id
         is unique.

         The value 'perCaptureSap' specifies that sessions created via a
         specific capture SAP get a unique session-id. This limits the total
         number sessions that can get created via a specific capture SAP to
         1023.

         The value 'perMsap' specifies that sessions belonging to the same MSAP
         get a unique session-id. The session-ids are not unique over the
         corresponding capture SAP.

         For plain statically configured SAPs the values 'perCaptureSap' and
         'perMsap' result in the same. Sessions belonging to that SAP get a
         unique session-id."
    DEFVAL      { disabled }
    ::= { tmnxPppoePlcyEntry 23 }

tmnxPppoePlcyRejectDisabledNcp   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyRejectDisabledNcp specifies whether disabled
         NCP's (Network Control Protocol) are rejected or silently ignored.

         When the value of this object is set to 'true(1)' then disabled NCP's
         are explicitly rejected."
    DEFVAL      { false }
    ::= { tmnxPppoePlcyEntry 24 }

tmnxPppoePlcyLcpIgnoreMagic      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyLcpIgnoreMagic specifies if checking the
         Magic-Number field in LCP Echo-Request and Echo-Reply messages is
         skipped.

         If the value of tmnxPppoePlcyLcpIgnoreMagic is equal to 'false',
         checking is performed.

         If the value of tmnxPppoePlcyLcpIgnoreMagic is equal to 'true',
         checking is not performed."
    REFERENCE
        "RFC 1661 PPP section 6.4. Magic-Number."
    DEFVAL      { false }
    ::= { tmnxPppoePlcyEntry 30 }

tmnxPppoePlcySessionTimeout      OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 1..31104000)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcySessionTimeout specifies the session timeout
         period to be used for this PPPOE session. The value '0' has the
         meaning of 'unlimited'"
    DEFVAL      { 0 }
    ::= { tmnxPppoePlcyEntry 31 }

tmnxPppoePlcyAllowSameCidForDhcp OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyAllowSameCidForDhcp specifies whether it is
         allowed to have multiple PPPoE sessions with the same MAC address and
         circuit-id for a specific SAP when using the internal DHCP client to
         retrieve the IP address from a local or remote DHCP server.

         When set to 'true', the PPPoE session ID will be included to select
         the IP address.

         The value of tmnxPppoePlcyAllowSameCidForDhcp is only relevant while
         the value of tmnxPppoePlcyMaxSessionsPerMac is not equal to one."
    DEFVAL      { false }
    ::= { tmnxPppoePlcyEntry 32 }

tmnxPppoePlcyReestablishSession  OBJECT-TYPE
    SYNTAX      INTEGER {
        disabled (1),
        padr     (2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyReestablishSession specifies whether the
         setup of a new PPPoE session triggers the termination of an already
         existing session with the same MAC address.

         The value of tmnxPppoePlcyReestablishSession can only be set different
         from 'disabled' if the value of tmnxPppoePlcyMaxSessionsPerMac is
         equal to one.

         When set to 'disabled', no session will be deleted. When set to
         'padr', the existing session will be deleted upon reception of the
         PADR."
    DEFVAL      { disabled }
    ::= { tmnxPppoePlcyEntry 33 }

tmnxPppoePlcyDefaultUserName     OBJECT-TYPE
    SYNTAX      TmnxPppoeUserNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyDefaultUserName specifies the default PPP
         username.

         A non-empty value of this object is used when the PPP client (the
         'peer') does not provide a PPP username during authentication.

         If the peer does not provide a PPP username during authentication
         while there is no default PPP username specified, the PPP session
         cannot be established."
    DEFVAL      { "" }
    ::= { tmnxPppoePlcyEntry 34 }

tmnxPppoePlcyDefaultPapPassword  OBJECT-TYPE
    SYNTAX      TmnxAuthPassword
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyDefaultPapPassword specifies the default PPP
         password.

         A non-empty value of this object is used when the PPP client (the
         'peer') does not provide a password during Password Authentication
         Protocol (PAP) authentication.

         An SNMP get request for the value of this object will result in a
         response with an empty string."
    DEFVAL      { "" }
    ::= { tmnxPppoePlcyEntry 35 }

tmnxPppoePlcySidAllocation       OBJECT-TYPE
    SYNTAX      INTEGER {
        sequential (0),
        random     (1)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcySidAllocation specifies whether the session id
         will be assigned sequentially or randomly"
    DEFVAL      { sequential }
    ::= { tmnxPppoePlcyEntry 36 }

tmnxPppoePlcyMaxSessionsPerCid   OBJECT-TYPE
    SYNTAX      Unsigned32 (0..8190)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyMaxSessionsPerCid specifies the maximum number
         of PPPoE sessions that can be created per CID."
    DEFVAL      { 0 }
    ::= { tmnxPppoePlcyEntry 37 }

tmnxPppoePlcyAllowSessionsWoCid  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyAllowSessionsWoCid specifies whether it is
         allowed to have PPPoE sessions without a CID.

         When set to 'true', the PPPoE session...

         The value of tmnxPppoePlcyAllowSessionsWoCid is only relevant while
         the value of tmnxPppoePlcyMaxSessionsPerCid is not equal to one."
    DEFVAL      { false }
    ::= { tmnxPppoePlcyEntry 38 }

tmnxPppoePlcyNcpRenegotiation    OBJECT-TYPE
    SYNTAX      INTEGER {
        ignore            (1),
        terminate-session (2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoePlcyNcpRenegotiation specifies whether after
         successful NCP negotiation, the BNG should ignore subsequent
         renegotiation messages or the PPP session should be terminated."
    DEFVAL      { terminate-session }
    ::= { tmnxPppoePlcyEntry 39 }

tmnxPppoePlcyLcpIgnoreIdentifier OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyLcpIgnoreIdentifier specifies whether
         identifier values in LCP Echo Reply packets are ignored. If incorrect
         and not ignored, the PPP session will be terminated."
    DEFVAL      { false }
    ::= { tmnxPppoePlcyEntry 40 }

tmnxPppoePlcyPppOptionTblLstChg  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyPppOptionTblLstChg indicates the sysUpTime
         at the time of the most recent management-initiated change to the
         tmnxPppoePlcyPppOptionTable."
    ::= { tmnxPppoeObjects 3 }

tmnxPppoePlcyPppOptionTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoePlcyPppOptionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxPppoePlcyPppOptionTable has an entry for each PPP option
         configured in the system."
    ::= { tmnxPppoeObjects 4 }

tmnxPppoePlcyPppOptionEntry      OBJECT-TYPE
    SYNTAX      TmnxPppoePlcyPppOptionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a PPP option configured in the system.

         Entries can be created and deleted via SNMP SET operations on the
         object tmnxPppoePlcyOptionRowStatus."
    INDEX       {
        tmnxPppoePlcyName,
        tmnxPppoePlcyOptionProtocol,
        tmnxPppoePlcyOptionNumber
    }
    ::= { tmnxPppoePlcyPppOptionTable 1 }

TmnxPppoePlcyPppOptionEntry      ::= SEQUENCE
{
    tmnxPppoePlcyOptionProtocol      INTEGER,
    tmnxPppoePlcyOptionNumber        Unsigned32,
    tmnxPppoePlcyOptionRowStatus     RowStatus,
    tmnxPppoePlcyOptionLstMgmtChange TimeStamp,
    tmnxPppoePlcyOptionType          TmnxDhcpOptionType,
    tmnxPppoePlcyOptionValue         OCTET STRING
}

tmnxPppoePlcyOptionProtocol      OBJECT-TYPE
    SYNTAX      INTEGER {
        lcp    (1),
        ipcp   (2),
        ipv6cp (3)
    }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyOptionProtocol specifies the PPP protocol
         for this option."
    ::= { tmnxPppoePlcyPppOptionEntry 1 }

tmnxPppoePlcyOptionNumber        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyOptionNumber specifies the number of this
         option."
    ::= { tmnxPppoePlcyPppOptionEntry 2 }

tmnxPppoePlcyOptionRowStatus     OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyOptionRowStatus controls the creation and
         deletion of rows in this table.

         The objects tmnxPppoePlcyOptionType and tmnxPppoePlcyOptionValue must
         be set when creating a new row."
    ::= { tmnxPppoePlcyPppOptionEntry 3 }

tmnxPppoePlcyOptionLstMgmtChange OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyOptionLstMgmtChange indicates the sysUpTime
         at the time of the most recent management-initiated change to this
         table row."
    ::= { tmnxPppoePlcyPppOptionEntry 4 }

tmnxPppoePlcyOptionType          OBJECT-TYPE
    SYNTAX      TmnxDhcpOptionType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyOptionType specifies how the value of this
         option in stored in tmnxPppoePlcyOptionValue.

         This object is mandatory at creation time."
    ::= { tmnxPppoePlcyPppOptionEntry 5 }

tmnxPppoePlcyOptionValue         OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..127))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoePlcyOptionValue specifies the value of this
         option.

         This object is mandatory at creation time. A zero length value is only
         allowed when the value of tmnxPppoePlcyOptionType is 'hex'."
    ::= { tmnxPppoePlcyPppOptionEntry 6 }

tmnxPppoeIesIfInfoTableLastChg   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeIesIfInfoTableLastChg indicates the sysUpTime at
         the time of the most recent management-initiated change to the
         tmnxPppoeIesIfInfoTable."
    ::= { tmnxPppoeObjects 5 }

tmnxPppoeIesIfInfoTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeIesIfInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains IES interface PPPoE configuration information.

         A row is automatically created in the tmnxPppoeIesIfInfoTable for an
         entry in the iesIfTable where either the value of the object iesIfType
         - is equal to 'group (3)' and the value of iesIfGroupInterfaceType is
         equal to 'plain', or
         - equal to 'subscriber (2)' while the value
         of the objects iesIfFwdServId and iesIfFwdSubIf are not equal to zero.

         The first case is referred to as 'group interface' and the second as
         'retailer interface'."
    ::= { tmnxPppoeObjects 6 }

tmnxPppoeIesIfInfoEntry          OBJECT-TYPE
    SYNTAX      TmnxPppoeIesIfInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "PPPoE specific information about an IES interface."
    INDEX       {
        svcId,
        iesIfIndex
    }
    ::= { tmnxPppoeIesIfInfoTable 1 }

TmnxPppoeIesIfInfoEntry          ::= SEQUENCE
{
    tmnxPppoeIesIfLastChg            TimeStamp,
    tmnxPppoeIesIfDescription        TItemDescription,
    tmnxPppoeIesIfAdminState         TmnxPppoeAdminStatus,
    tmnxPppoeIesIfPolicy             TNamedItem,
    tmnxPppoeIesIfSessionLimit       Unsigned32,
    tmnxPppoeIesIfSapSessionLimit    Unsigned32,
    tmnxPppoeIesIfPapChapUserDb      TNamedItemOrEmpty,
    tmnxPppoeIesIfUserDb             TNamedItemOrEmpty,
    tmnxPppoeIesIfDhcpcCcagOriginSap TruthValue,
    tmnxPppoeIesIfAntiSpoofing       INTEGER,
    tmnxPppoeIesIfDhcpcInclOptString DisplayString,
    tmnxPppoeIesIfPythonPolicy       TNamedItemOrEmpty,
    tmnxPppoeIesIfDhcpcInclClientId  INTEGER
}

tmnxPppoeIesIfLastChg            OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeIesIfLastChg indicates the sysUpTime at the time
         of the most recent management-initiated change to this table row."
    ::= { tmnxPppoeIesIfInfoEntry 1 }

tmnxPppoeIesIfDescription        OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of the object tmnxPppoeIesIfDescription specifies a user
         provided description for PPPoE on this IES interface.

         It consists of any printable, seven-bit ASCII characters up to 80
         characters in length."
    DEFVAL      { "" }
    ::= { tmnxPppoeIesIfInfoEntry 2 }

tmnxPppoeIesIfAdminState         OBJECT-TYPE
    SYNTAX      TmnxPppoeAdminStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of the object tmnxPppoeIesIfAdminState specifies the
         administrative state of PPPoE on this IES interface.

         The default value of this object is equal to 'disabled', except for a
         retailer interface, where it is equal to 'enabled'.

         In case of a retailer interface, setting the value of this object (to
         'disabled') is not allowed."
    ::= { tmnxPppoeIesIfInfoEntry 3 }

tmnxPppoeIesIfPolicy             OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeIesIfPolicy specifies the PPPoE policy
         applicable on this IES interface. The corresponding policy is defined
         in tmnxPppoePlcyTable.

         In case of a retailer interface, the value of this object is
         irrelevant and setting it (to a value other than default) is not
         allowed."
    DEFVAL      { "default" }
    ::= { tmnxPppoeIesIfInfoEntry 4 }

tmnxPppoeIesIfSessionLimit       OBJECT-TYPE
    SYNTAX      Unsigned32 (1..333823)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeIesIfSessionLimit specifies the maximum number
         of PPPoE sessions allowed on this IES interface."
    DEFVAL      { 1 }
    ::= { tmnxPppoeIesIfInfoEntry 5 }

tmnxPppoeIesIfSapSessionLimit    OBJECT-TYPE
    SYNTAX      Unsigned32 (1..131071)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeIesIfSapSessionLimit specifies the maximum
         number of PPPoE sessions allowed on each SAP belonging to this IES
         interface.

         In case of a retailer interface, the value of this object is
         irrelevant, and setting it (to a value other than 1) is not allowed."
    DEFVAL      { 1 }
    ::= { tmnxPppoeIesIfInfoEntry 6 }

tmnxPppoeIesIfPapChapUserDb      OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeIesIfPapChapUserDb specifies the local user
         database to use for PPP PAP/CHAP authentication.

         If no PPP authentication is required, the value of this object must be
         set to the empty string."
    DEFVAL      { "" }
    ::= { tmnxPppoeIesIfInfoEntry 7 }

tmnxPppoeIesIfUserDb             OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeIesIfUserDb specifies the local user database to
         use for PPPoE PADI or PPP PAP/CHAP based authentication.

         If no authentication with the local user database is required, the
         value of this object must be set to the empty string.

         In case of a retailer interface, setting the value of this object (to
         a value other than the empty string) is not allowed."
    DEFVAL      { "" }
    ::= { tmnxPppoeIesIfInfoEntry 8 }

tmnxPppoeIesIfDhcpcCcagOriginSap OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "In case this interface is connected to a VPLS via a CCA (Cross Connect
         Adaptor) MDA, the value of tmnxPppoeIesIfDhcpcCcagOriginSap specifies
         whether the system includes the original VPLS SAP in the circuit-id
         option to send to the DHCP server(s).

         In case of a retailer interface, the value of this object is
         irrelevant, and setting it (to a value other than false) is not
         allowed."
    DEFVAL      { false }
    ::= { tmnxPppoeIesIfInfoEntry 9 }

tmnxPppoeIesIfAntiSpoofing       OBJECT-TYPE
    SYNTAX      INTEGER {
        macSid   (1),
        macSidIp (2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeIesIfAntiSpoofing specifies the type of PPPoE
         anti-spoof filtering to use."
    DEFVAL      { macSid }
    ::= { tmnxPppoeIesIfInfoEntry 10 }

tmnxPppoeIesIfDhcpcInclOptString OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeIesIfDhcpcInclOptString specifies the string
         that goes into the Nokia vendor specific sub-option of option 82."
    DEFVAL      { "" }
    ::= { tmnxPppoeIesIfInfoEntry 11 }

tmnxPppoeIesIfPythonPolicy       OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeIesIfPythonPolicy specifies the Python policy
         used for modifying PPPoE packets on this interface.

         A nonzero value must correspond to a row in the
         TIMETRA-PYTHON-MIB::tmnxPythonPolicyTable."
    DEFVAL      { "" }
    ::= { tmnxPppoeIesIfInfoEntry 12 }

tmnxPppoeIesIfDhcpcInclClientId  OBJECT-TYPE
    SYNTAX      INTEGER {
        none              (1),
        macPppoeSessionId (2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeIesIfDhcpcInclClientId specifies whether or not
         to include option61 in messages to the DHCP server, and which layout
         to use.

         For now only 1 layout is defined: mac-address pppoe-session-id."
    DEFVAL      { none }
    ::= { tmnxPppoeIesIfInfoEntry 13 }

tmnxPppoeSapStatsTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeSapStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains statistics on PPPoE per SAP."
    ::= { tmnxPppoeObjects 7 }

tmnxPppoeSapStatsEntry           OBJECT-TYPE
    SYNTAX      TmnxPppoeSapStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "PPPoE statistics about a SAP."
    INDEX       {
        svcId,
        sapPortId,
        sapEncapValue
    }
    ::= { tmnxPppoeSapStatsTable 1 }

TmnxPppoeSapStatsEntry           ::= SEQUENCE
{
    tmnxPppoeSapRxPadi               Counter32,
    tmnxPppoeSapRxPadr               Counter32,
    tmnxPppoeSapRxPadt               Counter32,
    tmnxPppoeSapRxSession            Counter32,
    tmnxPppoeSapRxInvalidVersion     Counter32,
    tmnxPppoeSapRxInvalidType        Counter32,
    tmnxPppoeSapRxInvalidCode        Counter32,
    tmnxPppoeSapRxInvalidSession     Counter32,
    tmnxPppoeSapRxInvalidLen         Counter32,
    tmnxPppoeSapRxInvalidTags        Counter32,
    tmnxPppoeSapRxInvalidAcCookie    Counter32,
    tmnxPppoeSapRxDropped            Counter32,
    tmnxPppoeSapTxPado               Counter32,
    tmnxPppoeSapTxPads               Counter32,
    tmnxPppoeSapTxPadt               Counter32,
    tmnxPppoeSapTxSession            Counter32,
    tmnxPppoeSapRxInvalidMac         Counter32
}

tmnxPppoeSapRxPadi               OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxPadi indicates the number of PADI (PPPoE
         Active Discovery Initiation) packets received on this SAP."
    ::= { tmnxPppoeSapStatsEntry 1 }

tmnxPppoeSapRxPadr               OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxPadr indicates the number of PADR (PPPoE
         Active Discovery Request) packets received on this SAP."
    ::= { tmnxPppoeSapStatsEntry 2 }

tmnxPppoeSapRxPadt               OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxPadt indicates the number of PADT (PPPoE
         Active Discovery Terminate) packets received on this SAP."
    ::= { tmnxPppoeSapStatsEntry 3 }

tmnxPppoeSapRxSession            OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxSession indicates the number packets
         received during the PPP session stage on this SAP."
    ::= { tmnxPppoeSapStatsEntry 4 }

tmnxPppoeSapRxInvalidVersion     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxInvalidVersion indicates the number of
         PPPoE packets received with an invalid version field."
    ::= { tmnxPppoeSapStatsEntry 5 }

tmnxPppoeSapRxInvalidType        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxInvalidType indicates the number of PPPoE
         packets received with an invalid type field."
    ::= { tmnxPppoeSapStatsEntry 6 }

tmnxPppoeSapRxInvalidCode        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxInvalidCode indicates the number of PPPoE
         packets received with an invalid code field."
    ::= { tmnxPppoeSapStatsEntry 7 }

tmnxPppoeSapRxInvalidSession     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxInvalidSession indicates the number of
         PPPoE packets received with an invalid session-id field."
    ::= { tmnxPppoeSapStatsEntry 8 }

tmnxPppoeSapRxInvalidLen         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxInvalidLen indicates the number of PPPoE
         packets received with an invalid length field."
    ::= { tmnxPppoeSapStatsEntry 9 }

tmnxPppoeSapRxInvalidTags        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxInvalidTags indicates the number of PPPoE
         Active Discovery packets received with invalid tags."
    ::= { tmnxPppoeSapStatsEntry 10 }

tmnxPppoeSapRxInvalidAcCookie    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxInvalidAcCookie indicates the number of
         PPPoE Active Discovery packets received with an invalid AC-Cookie tag."
    ::= { tmnxPppoeSapStatsEntry 11 }

tmnxPppoeSapRxDropped            OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxDropped indicates the number of dropped
         PPPoE packets."
    ::= { tmnxPppoeSapStatsEntry 12 }

tmnxPppoeSapTxPado               OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapTxPado indicates the number of PADO (PPPoE
         Active Discovery Offer) packets transmitted on this SAP."
    ::= { tmnxPppoeSapStatsEntry 13 }

tmnxPppoeSapTxPads               OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapTxPads indicates the number of PADS (PPPoE
         Active Discovery Session) packets transmitted on this SAP."
    ::= { tmnxPppoeSapStatsEntry 14 }

tmnxPppoeSapTxPadt               OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapTxPadt indicates the number of PADT (PPPoE
         Active Discovery Terminate) packets transmitted on this SAP."
    ::= { tmnxPppoeSapStatsEntry 15 }

tmnxPppoeSapTxSession            OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapTxSession indicates the number packets
         transmitted during the PPP session stage on this SAP."
    ::= { tmnxPppoeSapStatsEntry 16 }

tmnxPppoeSapRxInvalidMac         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSapRxInvalidMac indicates the number of PPPoE
         packets received with an invalid MAC address."
    ::= { tmnxPppoeSapStatsEntry 17 }

tmnxPppoeSessionTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains PPPoE sessions."
    ::= { tmnxPppoeObjects 8 }

tmnxPppoeSessionEntry            OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a specific PPPoE session.

         In release 9.0 and higher, the actual information is in the
         TIMETRA-SUBSCRIBER-MGMT-MIB::tmnxSubPppTable.

         The corresponding row in that table can be directly retrieved using
         the value of the object tmnxPppoeSessionSubPppIndex."
    INDEX       {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeSessionMac,
        tmnxPppoeSessionId
    }
    ::= { tmnxPppoeSessionTable 1 }

TmnxPppoeSessionEntry            ::= SEQUENCE
{
    tmnxPppoeSessionMac              MacAddress,
    tmnxPppoeSessionId               TmnxPppoeSessionId,
    tmnxPppoeSessionUpTime           TimeTicks,
    tmnxPppoeSessionLcpState         TmnxPppCpState,
    tmnxPppoeSessionIpcpState        TmnxPppCpState,
    tmnxPppoeSessionPppMtu           Unsigned32,
    tmnxPppoeSessionPppAuthProtocol  INTEGER,
    tmnxPppoeSessionPppUserName      TmnxPppoeUserNameOrEmpty,
    tmnxPppoeSessionSubIdent         TmnxSubIdentStringOrEmpty,
    tmnxPppoeSessionOriginSubIdent   TmnxPppoeSessionInfoOrigin,
    tmnxPppoeSessionSubProfString    TmnxSubProfileStringOrEmpty,
    tmnxPppoeSessionSlaProfString    TmnxSlaProfileStringOrEmpty,
    tmnxPppoeSessionAncpString       TmnxAncpStringOrZero,
    tmnxPppoeSessionInterDestId      TmnxSubMgtIntDestIdOrEmpty,
    tmnxPppoeSessionAppProfString    TmnxAppProfileStringOrEmpty,
    tmnxPppoeSessionOriginStrings    TmnxPppoeSessionInfoOrigin,
    tmnxPppoeSessionSessionTimeout   Unsigned32,
    tmnxPppoeSessionIpAddrType       InetAddressType,
    tmnxPppoeSessionIpAddr           InetAddress,
    tmnxPppoeSessionPrimaryDnsType   InetAddressType,
    tmnxPppoeSessionPrimaryDns       InetAddress,
    tmnxPppoeSessionSecondryDnsType  InetAddressType,
    tmnxPppoeSessionSecondryDns      InetAddress,
    tmnxPppoeSessionPrimaryNbnsType  InetAddressType,
    tmnxPppoeSessionPrimaryNbns      InetAddress,
    tmnxPppoeSessionSecondryNbnsType InetAddressType,
    tmnxPppoeSessionSecondryNbns     InetAddress,
    tmnxPppoeSessionOriginIpcpInfo   TmnxPppoeSessionInfoOrigin,
    tmnxPppoeSessionCircuitId        OCTET STRING,
    tmnxPppoeSessionRemoteId         OCTET STRING,
    tmnxPppoeSessionAddressPool      DisplayString,
    tmnxPppoeSessionType             TmnxPppoeSessionType,
    tmnxPppoeSessionRetailerSvcId    TmnxServId,
    tmnxPppoeSessionRetailerIf       InterfaceIndexOrZero,
    tmnxPppoeSessionL2tpVrtrId       TmnxVRtrIDOrZero,
    tmnxPppoeSessionL2tpConnectionId Unsigned32,
    tmnxPppoeSessionServiceName      DisplayString,
    tmnxPppoeSessionCategoryMapName  TNamedItemOrEmpty,
    tmnxPppoeSessionRadiusClassAttr  OCTET STRING,
    tmnxPppoeSessionRadiusUserName   DisplayString,
    tmnxPppoeSessionIpv6cpState      TmnxPppCpState,
    tmnxPppoeSessionInterfaceId      OCTET STRING,
    tmnxPppoeSessionOriginIpv6cpInfo TmnxPppoeSessionInfoOrigin,
    tmnxPppoeSessionIpv6DnsType      InetAddressType,
    tmnxPppoeSessionIpv6Dns1         InetAddress,
    tmnxPppoeSessionIpv6Dns2         InetAddress,
    tmnxPppoeSessionIpv6DelPfxType   InetAddressType,
    tmnxPppoeSessionIpv6DelPfxLen    InetAddressPrefixLength,
    tmnxPppoeSessionIpv6DelPfx       InetAddress,
    tmnxPppoeSessionIpv6PrefixType   InetAddressType,
    tmnxPppoeSessionIpv6PrefixLen    InetAddressPrefixLength,
    tmnxPppoeSessionIpv6Prefix       InetAddress,
    tmnxPppoeSessionSubPppIndex      Unsigned32
}

tmnxPppoeSessionMac              OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSessionMac indicates the MAC address of the
         PPPoE session."
    ::= { tmnxPppoeSessionEntry 1 }

tmnxPppoeSessionId               OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSessionId indicates the session id of the PPPoE
         session."
    ::= { tmnxPppoeSessionEntry 2 }

tmnxPppoeSessionUpTime           OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionUpTime indicates how long (in hundredths
         of a second) that the session already exists in this table."
    ::= { tmnxPppoeSessionEntry 3 }

tmnxPppoeSessionLcpState         OBJECT-TYPE
    SYNTAX      TmnxPppCpState
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionLcpState indicates the obsolete state of
         the PPP Link Control Protocol of the PPPoE session."
    ::= { tmnxPppoeSessionEntry 4 }

tmnxPppoeSessionIpcpState        OBJECT-TYPE
    SYNTAX      TmnxPppCpState
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpcpState indicates the obsolete state of
         the PPP IP Control Protocol of the PPPoE session."
    ::= { tmnxPppoeSessionEntry 5 }

tmnxPppoeSessionPppMtu           OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionPppMtu indicates the PPP MTU of the PPPoE
         session."
    ::= { tmnxPppoeSessionEntry 6 }

tmnxPppoeSessionPppAuthProtocol  OBJECT-TYPE
    SYNTAX      INTEGER {
        none (1),
        pap  (2),
        chap (3)
    }
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionPppAuthProtocol indicates the PPP
         protocol used to authenticate the PPPoE session.

         The value 'none' indicates that no PPP authentication was done. The
         value 'pap' indicates that authentication was done via the Password
         Authentication Protocol. The value 'chap' indicates that
         authentication was done via the Challenge-Handshake Authentication
         Protocol."
    ::= { tmnxPppoeSessionEntry 7 }

tmnxPppoeSessionPppUserName      OBJECT-TYPE
    SYNTAX      TmnxPppoeUserNameOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionPppUserName indicates the user name
         learned during the PPP authentication phase."
    ::= { tmnxPppoeSessionEntry 8 }

tmnxPppoeSessionSubIdent         OBJECT-TYPE
    SYNTAX      TmnxSubIdentStringOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionSubIdent indicates the subscriber
         applicable for this PPPoE session.

         The value of tmnxPppoeSessionOriginSubIdent indicates from what source
         this subscriber identification was received."
    ::= { tmnxPppoeSessionEntry 9 }

tmnxPppoeSessionOriginSubIdent   OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionInfoOrigin
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOriginSubIdent indicates which source
         provided the subscriber."
    ::= { tmnxPppoeSessionEntry 10 }

tmnxPppoeSessionSubProfString    OBJECT-TYPE
    SYNTAX      TmnxSubProfileStringOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionSubProfString indicates the subscriber
         profile string applicable for this PPPoE session.

         The value of tmnxPppoeSessionOriginStrings indicates from what source
         this string was received."
    ::= { tmnxPppoeSessionEntry 11 }

tmnxPppoeSessionSlaProfString    OBJECT-TYPE
    SYNTAX      TmnxSlaProfileStringOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionSlaProfString indicates the SLA profile
         string applicable for this PPPoE session.

         The value of tmnxPppoeSessionOriginStrings indicates from what source
         this string was received."
    ::= { tmnxPppoeSessionEntry 12 }

tmnxPppoeSessionAncpString       OBJECT-TYPE
    SYNTAX      TmnxAncpStringOrZero
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionAncpString indicates the ANCP string
         applicable for this PPPoE session.

         The value of tmnxPppoeSessionOriginStrings indicates from what source
         this string was received."
    ::= { tmnxPppoeSessionEntry 13 }

tmnxPppoeSessionInterDestId      OBJECT-TYPE
    SYNTAX      TmnxSubMgtIntDestIdOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionInterDestId indicates the intermediate
         destination identifier applicable for this PPPoE session.

         The value of tmnxPppoeSessionOriginStrings indicates from what source
         this string was received."
    ::= { tmnxPppoeSessionEntry 14 }

tmnxPppoeSessionAppProfString    OBJECT-TYPE
    SYNTAX      TmnxAppProfileStringOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionAppProfString indicates the application
         profile string applicable for this PPPoE session.

         The value of tmnxPppoeSessionOriginStrings indicates from what source
         this string was received."
    ::= { tmnxPppoeSessionEntry 15 }

tmnxPppoeSessionOriginStrings    OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionInfoOrigin
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOriginStrings indicates which source
         provided the subscriber identification strings (subscriber profile
         string, SLA profile string, ANCP string, intermediate destination
         identifier and application profile string)."
    ::= { tmnxPppoeSessionEntry 16 }

tmnxPppoeSessionSessionTimeout   OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionSessionTimeout indicates the session
         timeout received from the Radius server (if applicable)."
    ::= { tmnxPppoeSessionEntry 17 }

tmnxPppoeSessionIpAddrType       OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpAddrType indicates the address type of
         tmnxPppoeSessionIpAddr."
    ::= { tmnxPppoeSessionEntry 18 }

tmnxPppoeSessionIpAddr           OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpAddr indicates the IP address of the
         PPPoE session.

         The value of tmnxPppoeSessionOriginIpcpInfo indicates from what source
         this IP address was received."
    ::= { tmnxPppoeSessionEntry 19 }

tmnxPppoeSessionPrimaryDnsType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionPrimaryDnsType indicates the address type
         of tmnxPppoeSessionPrimaryDns."
    ::= { tmnxPppoeSessionEntry 20 }

tmnxPppoeSessionPrimaryDns       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionPrimaryDns indicates the primary DNS
         server.

         The value of this object is ''H when not applicable.

         The value of tmnxPppoeSessionOriginIpcpInfo indicates from what source
         this IP address was received."
    ::= { tmnxPppoeSessionEntry 21 }

tmnxPppoeSessionSecondryDnsType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionSecondryDnsType indicates the address
         type of tmnxPppoeSessionSecondryDns."
    ::= { tmnxPppoeSessionEntry 22 }

tmnxPppoeSessionSecondryDns      OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionSecondryDns indicates the secondary DNS
         server.

         The value of this object is ''H when not applicable.

         The value of tmnxPppoeSessionOriginIpcpInfo indicates from what source
         this IP address was received."
    ::= { tmnxPppoeSessionEntry 23 }

tmnxPppoeSessionPrimaryNbnsType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionPrimaryNbnsType indicates the address
         type of tmnxPppoeSessionPrimaryNbns."
    ::= { tmnxPppoeSessionEntry 24 }

tmnxPppoeSessionPrimaryNbns      OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionPrimaryNbns indicates the primary NBNS
         server.

         The value of this object is ''H when not applicable.

         The value of tmnxPppoeSessionOriginIpcpInfo indicates from what source
         this IP address was received."
    ::= { tmnxPppoeSessionEntry 25 }

tmnxPppoeSessionSecondryNbnsType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionSecondryNbnsType indicates the address
         type of tmnxPppoeSessionSecondryNbns."
    ::= { tmnxPppoeSessionEntry 26 }

tmnxPppoeSessionSecondryNbns     OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionSecondryNbns indicates the secondary NBNS
         server.

         The value of this object is ''H when not applicable.

         The value of tmnxPppoeSessionOriginIpcpInfo indicates from what source
         this IP address was received."
    ::= { tmnxPppoeSessionEntry 27 }

tmnxPppoeSessionOriginIpcpInfo   OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionInfoOrigin
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOriginIpcpInfo indicates which source
         provided the IPCP information (IP, DNS and NBNS addresses)."
    ::= { tmnxPppoeSessionEntry 28 }

tmnxPppoeSessionCircuitId        OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..256))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionCircuitId indicates the value of the
         circuit-id sub-option inserted by the PPPoE intermediate agent."
    ::= { tmnxPppoeSessionEntry 29 }

tmnxPppoeSessionRemoteId         OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..256))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRemoteId indicates the value of the
         remote-id sub-option inserted by the PPPoE intermediate agent."
    ::= { tmnxPppoeSessionEntry 30 }

tmnxPppoeSessionAddressPool      OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionAddressPool indicates the IP address pool
         which is used to search for an IP address for this session."
    ::= { tmnxPppoeSessionEntry 31 }

tmnxPppoeSessionType             OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionType indicates the type of this session."
    ::= { tmnxPppoeSessionEntry 32 }

tmnxPppoeSessionRetailerSvcId    OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRetailerSvcId indicates the service ID of
         the retailer VPRN service to which this session belongs. If the value
         of this object is non-zero, the session belongs to a retailer VPRN."
    ::= { tmnxPppoeSessionEntry 33 }

tmnxPppoeSessionRetailerIf       OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRetailerIf indicates the interface index
         of the retailer VPRN interface to which this session belongs. If the
         value of this object is non-zero, the session belongs to a retailer
         VPRN."
    ::= { tmnxPppoeSessionEntry 34 }

tmnxPppoeSessionL2tpVrtrId       OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionL2tpVrtrId indicates the virtual router
         ID of the L2TP session associated with this PPPoE session.

         If there is no L2TP session associated with this PPPoE session, the
         value of this object is equal to zero."
    ::= { tmnxPppoeSessionEntry 35 }

tmnxPppoeSessionL2tpConnectionId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionL2tpConnectionId indicates the connection
         ID of the L2TP session associated with this PPPoE session.

         The values of tmnxPppoeSessionL2tpVrtrId and
         tmnxPppoeSessionL2tpConnectionId are the index in the table
         TIMETRA-L2TP-MIB::tmnxL2tpSeStatusTable of the L2TP session associated
         with this PPPoE session.

         If there is no L2TP session associated with this PPPoE session, the
         value of this object is equal to zero."
    ::= { tmnxPppoeSessionEntry 36 }

tmnxPppoeSessionServiceName      OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSessionServiceName indicates the value of the
         PPPoE service-name tag received in PADI packets."
    ::= { tmnxPppoeSessionEntry 37 }

tmnxPppoeSessionCategoryMapName  OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionCategoryMapName indicates the category
         map name applicable for this PPPoE session.

         The value of tmnxPppoeSessionOriginStrings indicates from what source
         this string was received."
    ::= { tmnxPppoeSessionEntry 38 }

tmnxPppoeSessionRadiusClassAttr  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRadiusClassAttr indicates the Class
         attribute returned by the RADIUS server in an Access-Accept message.

         If no RADIUS authentication is performed for this session, or RADIUS
         did not return this attribute, the value of this object is empty."
    ::= { tmnxPppoeSessionEntry 39 }

tmnxPppoeSessionRadiusUserName   OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRadiusUserName indicates the User-Name
         attribute returned by the RADIUS server in an Access-Accept message.

         If RADIUS did not return this attribute, the value of this object is
         equal to the User-Name attribute sent in the original Access-Request
         message.

         If no RADIUS authentication is performed for this session, the value
         of this object is empty."
    ::= { tmnxPppoeSessionEntry 40 }

tmnxPppoeSessionIpv6cpState      OBJECT-TYPE
    SYNTAX      TmnxPppCpState
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpv6cpState indicates the obsolete state
         of the PPP IPv6 Control Protocol of the PPPoE session."
    ::= { tmnxPppoeSessionEntry 41 }

tmnxPppoeSessionInterfaceId      OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (8))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionInterfaceId indicates the value of the
         remote-id sub-option inserted by the PPPoE intermediate agent."
    ::= { tmnxPppoeSessionEntry 42 }

tmnxPppoeSessionOriginIpv6cpInfo OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionInfoOrigin
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOriginIpv6cpInfo indicates which source
         provided the IPCP information (IP, DNS and NBNS addresses)."
    ::= { tmnxPppoeSessionEntry 43 }

tmnxPppoeSessionIpv6DnsType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpv6DnsType indicates the address type of
         tmnxPppoeSessionIpv6Dns1/2."
    ::= { tmnxPppoeSessionEntry 44 }

tmnxPppoeSessionIpv6Dns1         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|16))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpv6Dns1 indicates the primary DNS
         server.

         The value of this object is ''H when not applicable.

         The value of tmnxPppoeSessionOriginIpv6cpInfo indicates from what
         source this IP address was received."
    ::= { tmnxPppoeSessionEntry 45 }

tmnxPppoeSessionIpv6Dns2         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|16))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpv6Dns2 indicates the secondary DNS
         server.

         The value of this object is ''H when not applicable.

         The value of tmnxPppoeSessionOriginIpv6cpInfo indicates from what
         source this IP address was received."
    ::= { tmnxPppoeSessionEntry 46 }

tmnxPppoeSessionIpv6DelPfxType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpv6DelPfxType indicates the address type
         of tmnxPppoeSessionIpv6DelPfx."
    ::= { tmnxPppoeSessionEntry 47 }

tmnxPppoeSessionIpv6DelPfxLen    OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..128)
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpv6DelPfxLen indicates the length of
         tmnxPppoeSessionIpv6DelPfx."
    ::= { tmnxPppoeSessionEntry 48 }

tmnxPppoeSessionIpv6DelPfx       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|16))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpv6DelPfx indicates the IPv6 prefix used
         for DHCPv6 prefix delegation."
    ::= { tmnxPppoeSessionEntry 49 }

tmnxPppoeSessionIpv6PrefixType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpv6PrefixType indicates the address type
         of tmnxPppoeSessionIpv6Prefix."
    ::= { tmnxPppoeSessionEntry 50 }

tmnxPppoeSessionIpv6PrefixLen    OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..128)
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpv6PrefixLen indicates the length of
         tmnxPppoeSessionIpv6Prefix."
    ::= { tmnxPppoeSessionEntry 51 }

tmnxPppoeSessionIpv6Prefix       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|16))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionIpv6Prefix indicates the IPv6 prefix used
         for stateless address autoconfiguration."
    ::= { tmnxPppoeSessionEntry 52 }

tmnxPppoeSessionSubPppIndex      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeSessionSubPppIndex indicates the local
         identifier of the subscriber PPP session.

         It is the index of the corresponding conceptual row in the
         TIMETRA-SUBSCRIBER-MGMT-MIB::tmnxSubPppTable."
    ::= { tmnxPppoeSessionEntry 53 }

tmnxPppoeSessionModifyTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeSessionModifyEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The tmnxPppoeSessionModifyTable augments the tmnxPppoeSessionTable.
         The table allows the operator to modify attributes of the PPPoE
         session.

         This table is replaced with
         TIMETRA-SUBSCRIBER-MGMT-MIB::tmnxSubPppModTable."
    ::= { tmnxPppoeObjects 9 }

tmnxPppoeSessionModifyEntry      OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionModifyEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Each row entry contains parameters that allow to modify a PPPoE
         session's attributes."
    AUGMENTS    { tmnxPppoeSessionEntry }
    ::= { tmnxPppoeSessionModifyTable 1 }

TmnxPppoeSessionModifyEntry      ::= SEQUENCE
{
    tmnxPppoeSessionModSubIdent      TmnxSubIdentStringOrEmpty,
    tmnxPppoeSessionModSubProfStr    TmnxSubProfileStringOrEmpty,
    tmnxPppoeSessionModSlaProfStr    TmnxSlaProfileStringOrEmpty,
    tmnxPppoeSessionModAncpStr       TmnxAncpStringOrZero,
    tmnxPppoeSessionModInterDestId   TmnxSubMgtIntDestIdOrEmpty,
    tmnxPppoeSessionModAppProfStr    TmnxAppProfileStringOrEmpty,
    tmnxPppoeSessionEvaluateState    TruthValue
}

tmnxPppoeSessionModSubIdent      OBJECT-TYPE
    SYNTAX      TmnxSubIdentStringOrEmpty
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionModSubIdent allows to specify a new
         subscriber name for this session.

         When a SET of this object is done with a non empty string, the system
         will attempt to assign a new subscriber name.

         A SET with an empty string has no effect on the system. (NOOP).

         GETs and GETNEXTs on this variable return an empty string."
    DEFVAL      { "" }
    ::= { tmnxPppoeSessionModifyEntry 1 }

tmnxPppoeSessionModSubProfStr    OBJECT-TYPE
    SYNTAX      TmnxSubProfileStringOrEmpty
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionModSubProfStr allows to specify a new
         subscriber profile string for this session.

         When a SET of this object is done with a non empty string, the system
         will attempt to assign a new subscriber profile string.

         A SET with an empty string has no effect on the system. (NOOP).

         GETs and GETNEXTs on this variable return an empty string."
    DEFVAL      { "" }
    ::= { tmnxPppoeSessionModifyEntry 2 }

tmnxPppoeSessionModSlaProfStr    OBJECT-TYPE
    SYNTAX      TmnxSlaProfileStringOrEmpty
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionModSlaProfStr allows to specify a new SLA
         profile string for this session.

         When a SET of this object is done with a non empty string, the system
         will attempt to assign a new SLA profile string.

         A SET with an empty string has no effect on the system. (NOOP).

         GETs and GETNEXTs on this variable return an empty string."
    DEFVAL      { "" }
    ::= { tmnxPppoeSessionModifyEntry 3 }

tmnxPppoeSessionModAncpStr       OBJECT-TYPE
    SYNTAX      TmnxAncpStringOrZero
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionModAncpStr allows to specify a new
         ANCP-string for this session.

         When a SET of this object is done with a non empty string, the system
         will attempt to assign a new ANCP-string.

         A SET with an empty string has no effect on the system. (NOOP).

         GETs and GETNEXTs on this variable return an empty string."
    DEFVAL      { "" }
    ::= { tmnxPppoeSessionModifyEntry 4 }

tmnxPppoeSessionModInterDestId   OBJECT-TYPE
    SYNTAX      TmnxSubMgtIntDestIdOrEmpty
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionModInterDestId allows to specify a new
         intermediate destination id for this session.

         When a SET of this object is done with a non empty string, the system
         will attempt to assign a new intermediate destination id.

         A SET with an empty string has no effect on the system. (NOOP).

         GETs and GETNEXTs on this variable return an empty string."
    DEFVAL      { "" }
    ::= { tmnxPppoeSessionModifyEntry 5 }

tmnxPppoeSessionModAppProfStr    OBJECT-TYPE
    SYNTAX      TmnxAppProfileStringOrEmpty
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionModAppProfStr specifies a new application
         profile string for this session.

         When a SET of this object is done with a non empty string, the system
         will attempt to assign a new application profile string.

         A SET with an empty string has no effect on the system. (NOOP).

         GETs and GETNEXTs on this variable return an empty string."
    DEFVAL      { "" }
    ::= { tmnxPppoeSessionModifyEntry 6 }

tmnxPppoeSessionEvaluateState    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionEvaluateState allows to cause a
         re-evaluation of the specified session.

         When this object is set to 'true', the system will perform a
         re-evaluation of the session.

         GETs and GETNEXTs on this variable return false.

         It is not possible to simultaneously request for a session
         re-evaluation, and modify any of the strings."
    DEFVAL      { false }
    ::= { tmnxPppoeSessionModifyEntry 7 }

tmnxPppoeSessionStatsTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeSessionStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A table that contains statistics per PPPoE session.

         This table is replaced with
         TIMETRA-SUBSCRIBER-MGMT-MIB::tmnxSubPppStatTable."
    ::= { tmnxPppoeObjects 10 }

tmnxPppoeSessionStatsEntry       OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Statistics about a PPPoE session."
    INDEX       {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeSessionMac,
        tmnxPppoeSessionId
    }
    ::= { tmnxPppoeSessionStatsTable 1 }

TmnxPppoeSessionStatsEntry       ::= SEQUENCE
{
    tmnxPppoeSessionRxUnknownProto   Counter32,
    tmnxPppoeSessionRxLcpConfReq     Counter32,
    tmnxPppoeSessionRxLcpConfAck     Counter32,
    tmnxPppoeSessionRxLcpConfNak     Counter32,
    tmnxPppoeSessionRxLcpConfRej     Counter32,
    tmnxPppoeSessionRxLcpTermReq     Counter32,
    tmnxPppoeSessionRxLcpTermAck     Counter32,
    tmnxPppoeSessionRxLcpCodeRej     Counter32,
    tmnxPppoeSessionRxLcpEchoReq     Counter32,
    tmnxPppoeSessionRxLcpEchoRep     Counter32,
    tmnxPppoeSessionRxLcpProtRej     Counter32,
    tmnxPppoeSessionRxLcpDiscReq     Counter32,
    tmnxPppoeSessionTxLcpConfReq     Counter32,
    tmnxPppoeSessionTxLcpConfAck     Counter32,
    tmnxPppoeSessionTxLcpConfNak     Counter32,
    tmnxPppoeSessionTxLcpConfRej     Counter32,
    tmnxPppoeSessionTxLcpTermReq     Counter32,
    tmnxPppoeSessionTxLcpTermAck     Counter32,
    tmnxPppoeSessionTxLcpCodeRej     Counter32,
    tmnxPppoeSessionTxLcpEchoReq     Counter32,
    tmnxPppoeSessionTxLcpEchoRep     Counter32,
    tmnxPppoeSessionTxLcpProtRej     Counter32,
    tmnxPppoeSessionTxLcpDiscReq     Counter32,
    tmnxPppoeSessionRxPapAuthReq     Counter32,
    tmnxPppoeSessionTxPapAuthAck     Counter32,
    tmnxPppoeSessionTxPapAuthNak     Counter32,
    tmnxPppoeSessionRxChapResponse   Counter32,
    tmnxPppoeSessionTxChapChallenge  Counter32,
    tmnxPppoeSessionTxChapSuccess    Counter32,
    tmnxPppoeSessionTxChapFailure    Counter32,
    tmnxPppoeSessionRxIpcpConfReq    Counter32,
    tmnxPppoeSessionRxIpcpConfAck    Counter32,
    tmnxPppoeSessionRxIpcpConfNak    Counter32,
    tmnxPppoeSessionRxIpcpConfRej    Counter32,
    tmnxPppoeSessionRxIpcpTermReq    Counter32,
    tmnxPppoeSessionRxIpcpTermAck    Counter32,
    tmnxPppoeSessionRxIpcpCodeRej    Counter32,
    tmnxPppoeSessionTxIpcpConfReq    Counter32,
    tmnxPppoeSessionTxIpcpConfAck    Counter32,
    tmnxPppoeSessionTxIpcpConfNak    Counter32,
    tmnxPppoeSessionTxIpcpConfRej    Counter32,
    tmnxPppoeSessionTxIpcpTermReq    Counter32,
    tmnxPppoeSessionTxIpcpTermAck    Counter32,
    tmnxPppoeSessionTxIpcpCodeRej    Counter32,
    tmnxPppoeSessionRxIpv6cpConfReq  Counter32,
    tmnxPppoeSessionRxIpv6cpConfAck  Counter32,
    tmnxPppoeSessionRxIpv6cpConfNak  Counter32,
    tmnxPppoeSessionRxIpv6cpConfRej  Counter32,
    tmnxPppoeSessionRxIpv6cpTermReq  Counter32,
    tmnxPppoeSessionRxIpv6cpTermAck  Counter32,
    tmnxPppoeSessionRxIpv6cpCodeRej  Counter32,
    tmnxPppoeSessionTxIpv6cpConfReq  Counter32,
    tmnxPppoeSessionTxIpv6cpConfAck  Counter32,
    tmnxPppoeSessionTxIpv6cpConfNak  Counter32,
    tmnxPppoeSessionTxIpv6cpConfRej  Counter32,
    tmnxPppoeSessionTxIpv6cpTermReq  Counter32,
    tmnxPppoeSessionTxIpv6cpTermAck  Counter32,
    tmnxPppoeSessionTxIpv6cpCodeRej  Counter32
}

tmnxPppoeSessionRxUnknownProto   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxUnknownProto indicates the number of
         packets with unknown PPP protocol received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 1 }

tmnxPppoeSessionRxLcpConfReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpConfReq indicates the number of LCP
         configure requests received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 2 }

tmnxPppoeSessionRxLcpConfAck     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpConfAck indicates the number of LCP
         configure acknowledgements received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 3 }

tmnxPppoeSessionRxLcpConfNak     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpConfNak indicates the number of
         negative LCP configure acknowledgements received for this PPPoE
         session."
    ::= { tmnxPppoeSessionStatsEntry 4 }

tmnxPppoeSessionRxLcpConfRej     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpConfRej indicates the number of LCP
         configure rejects received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 5 }

tmnxPppoeSessionRxLcpTermReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpTermReq indicates the number of LCP
         terminate requests received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 6 }

tmnxPppoeSessionRxLcpTermAck     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpTermAck indicates the number of LCP
         terminate acknowledgements received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 7 }

tmnxPppoeSessionRxLcpCodeRej     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpCodeRej indicates the number of LCP
         code rejects received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 8 }

tmnxPppoeSessionRxLcpEchoReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpEchoReq indicates the number of LCP
         echo requests received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 9 }

tmnxPppoeSessionRxLcpEchoRep     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpEchoRep indicates the number of LCP
         echo replies received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 10 }

tmnxPppoeSessionRxLcpProtRej     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpProtRej indicates the number of LCP
         protocol rejects received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 11 }

tmnxPppoeSessionRxLcpDiscReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxLcpDiscReq indicates the number of LCP
         discard requests received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 12 }

tmnxPppoeSessionTxLcpConfReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpConfReq indicates the number of LCP
         configure requests transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 13 }

tmnxPppoeSessionTxLcpConfAck     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpConfAck indicates the number of LCP
         configure acknowledgements transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 14 }

tmnxPppoeSessionTxLcpConfNak     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpConfNak indicates the number of
         negative LCP configure acknowledgements transmitted for this PPPoE
         session."
    ::= { tmnxPppoeSessionStatsEntry 15 }

tmnxPppoeSessionTxLcpConfRej     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpConfRej indicates the number of LCP
         configure rejects transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 16 }

tmnxPppoeSessionTxLcpTermReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpTermReq indicates the number of LCP
         terminate requests transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 17 }

tmnxPppoeSessionTxLcpTermAck     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpTermAck indicates the number of LCP
         terminate acknowledgements transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 18 }

tmnxPppoeSessionTxLcpCodeRej     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpCodeRej indicates the number of LCP
         code rejects transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 19 }

tmnxPppoeSessionTxLcpEchoReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpEchoReq indicates the number of LCP
         echo requests transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 20 }

tmnxPppoeSessionTxLcpEchoRep     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpEchoRep indicates the number of LCP
         echo replies transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 21 }

tmnxPppoeSessionTxLcpProtRej     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpProtRej indicates the number of LCP
         protocol rejects transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 22 }

tmnxPppoeSessionTxLcpDiscReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxLcpDiscReq indicates the number of LCP
         discard requests transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 23 }

tmnxPppoeSessionRxPapAuthReq     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxPapAuthReq indicates the number of PAP
         authentication requests received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 24 }

tmnxPppoeSessionTxPapAuthAck     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxPapAuthAck indicates the number of PAP
         authentication acknowledgements transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 25 }

tmnxPppoeSessionTxPapAuthNak     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxPapAuthNak indicates the number of
         negative PAP authentication acknowledgements transmitted for this
         PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 26 }

tmnxPppoeSessionRxChapResponse   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxChapResponse indicates the number of
         CHAP authentication responses received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 27 }

tmnxPppoeSessionTxChapChallenge  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxChapChallenge indicates the number of
         CHAP authentication challenges transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 28 }

tmnxPppoeSessionTxChapSuccess    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxChapSuccess indicates the number of
         CHAP authentication acknowledgements transmitted for this PPPoE
         session."
    ::= { tmnxPppoeSessionStatsEntry 29 }

tmnxPppoeSessionTxChapFailure    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxChapFailure indicates the number of
         negative CHAP authentication acknowledgements transmitted for this
         PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 30 }

tmnxPppoeSessionRxIpcpConfReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpcpConfReq indicates the number of
         IPCP configure requests received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 31 }

tmnxPppoeSessionRxIpcpConfAck    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpcpConfAck indicates the number of
         IPCP configure acknowledgements received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 32 }

tmnxPppoeSessionRxIpcpConfNak    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpcpConfNak indicates the number of
         negative IPCP configure acknowledgements received for this PPPoE
         session."
    ::= { tmnxPppoeSessionStatsEntry 33 }

tmnxPppoeSessionRxIpcpConfRej    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpcpConfRej indicates the number of
         IPCP configure rejects received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 34 }

tmnxPppoeSessionRxIpcpTermReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpcpTermReq indicates the number of
         IPCP terminate requests received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 35 }

tmnxPppoeSessionRxIpcpTermAck    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpcpTermAck indicates the number of
         IPCP terminate acknowledgements received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 36 }

tmnxPppoeSessionRxIpcpCodeRej    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpcpCodeRej indicates the number of
         IPCP code rejects received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 37 }

tmnxPppoeSessionTxIpcpConfReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpcpConfReq indicates the number of
         IPCP configure requests transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 38 }

tmnxPppoeSessionTxIpcpConfAck    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpcpConfAck indicates the number of
         IPCP configure acknowledgements transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 39 }

tmnxPppoeSessionTxIpcpConfNak    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpcpConfNak indicates the number of
         negative IPCP configure acknowledgements transmitted for this PPPoE
         session."
    ::= { tmnxPppoeSessionStatsEntry 40 }

tmnxPppoeSessionTxIpcpConfRej    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpcpConfRej indicates the number of
         IPCP configure rejects transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 41 }

tmnxPppoeSessionTxIpcpTermReq    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpcpTermReq indicates the number of
         IPCP terminate requests transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 42 }

tmnxPppoeSessionTxIpcpTermAck    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpcpTermAck indicates the number of
         IPCP terminate acknowledgements transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 43 }

tmnxPppoeSessionTxIpcpCodeRej    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpcpCodeRej indicates the number of
         IPCP code rejects transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 44 }

tmnxPppoeSessionRxIpv6cpConfReq  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpv6cpConfReq indicates the number of
         IPv6CP configure requests received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 45 }

tmnxPppoeSessionRxIpv6cpConfAck  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpv6cpConfAck indicates the number of
         IPv6CP configure acknowledgements received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 46 }

tmnxPppoeSessionRxIpv6cpConfNak  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpv6cpConfNak indicates the number of
         negative IPv6CP configure acknowledgements received for this PPPoE
         session."
    ::= { tmnxPppoeSessionStatsEntry 47 }

tmnxPppoeSessionRxIpv6cpConfRej  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpv6cpConfRej indicates the number of
         IPv6CP configure rejects received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 48 }

tmnxPppoeSessionRxIpv6cpTermReq  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpv6cpTermReq indicates the number of
         IPv6CP terminate requests received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 49 }

tmnxPppoeSessionRxIpv6cpTermAck  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpv6cpTermAck indicates the number of
         IPv6CP terminate acknowledgements received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 50 }

tmnxPppoeSessionRxIpv6cpCodeRej  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionRxIpv6cpCodeRej indicates the number of
         IPv6CP code rejects received for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 51 }

tmnxPppoeSessionTxIpv6cpConfReq  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpv6cpConfReq indicates the number of
         IPv6CP configure requests transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 52 }

tmnxPppoeSessionTxIpv6cpConfAck  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpv6cpConfAck indicates the number of
         IPv6CP configure acknowledgements transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 53 }

tmnxPppoeSessionTxIpv6cpConfNak  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpv6cpConfNak indicates the number of
         negative IPv6CP configure acknowledgements transmitted for this PPPoE
         session."
    ::= { tmnxPppoeSessionStatsEntry 54 }

tmnxPppoeSessionTxIpv6cpConfRej  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpv6cpConfRej indicates the number of
         IPv6CP configure rejects transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 55 }

tmnxPppoeSessionTxIpv6cpTermReq  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpv6cpTermReq indicates the number of
         IPv6CP terminate requests transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 56 }

tmnxPppoeSessionTxIpv6cpTermAck  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpv6cpTermAck indicates the number of
         IPv6CP terminate acknowledgements transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 57 }

tmnxPppoeSessionTxIpv6cpCodeRej  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionTxIpv6cpCodeRej indicates the number of
         IPv6CP code rejects transmitted for this PPPoE session."
    ::= { tmnxPppoeSessionStatsEntry 58 }

tmnxPppoeManagedRouteTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeManagedRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A table that contains PPPoE managed routes.

         This table is replaced with
         TIMETRA-SUBSCRIBER-MGMT-MIB::tmnxSubPppMRtTable."
    ::= { tmnxPppoeObjects 11 }

tmnxPppoeManagedRouteEntry       OBJECT-TYPE
    SYNTAX      TmnxPppoeManagedRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A specific PPPoE managed route."
    INDEX       {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeSessionMac,
        tmnxPppoeSessionId,
        tmnxPppoeManagedRouteAddrType,
        tmnxPppoeManagedRouteAddr,
        tmnxPppoeManagedRoutePrefixLen
    }
    ::= { tmnxPppoeManagedRouteTable 1 }

TmnxPppoeManagedRouteEntry       ::= SEQUENCE
{
    tmnxPppoeManagedRouteAddrType    InetAddressType,
    tmnxPppoeManagedRouteAddr        InetAddress,
    tmnxPppoeManagedRoutePrefixLen   InetAddressPrefixLength,
    tmnxPppoeManagedRouteStatus      TmnxManagedRouteStatus
}

tmnxPppoeManagedRouteAddrType    OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeManagedRouteAddrType indicates the address type
         of tmnxPppoeManagedRouteAddr."
    ::= { tmnxPppoeManagedRouteEntry 1 }

tmnxPppoeManagedRouteAddr        OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeManagedRouteAddr indicates the IP address of the
         managed route."
    ::= { tmnxPppoeManagedRouteEntry 2 }

tmnxPppoeManagedRoutePrefixLen   OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..32)
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeManagedRoutePrefixLen indicates the prefix
         length of the subnet associated with tmnxPppoeManagedRouteAddr."
    ::= { tmnxPppoeManagedRouteEntry 3 }

tmnxPppoeManagedRouteStatus      OBJECT-TYPE
    SYNTAX      TmnxManagedRouteStatus
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeManagedRouteStatus indicates the state of this
         managed route."
    ::= { tmnxPppoeManagedRouteEntry 4 }

tmnxPppoeSessionBgpTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeSessionBgpEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The tmnxPppoeSessionBgpTable augments the tmnxPppoeSessionTable.

         This table is replaced with
         TIMETRA-SUBSCRIBER-MGMT-MIB::tmnxSubPppBgpTable."
    ::= { tmnxPppoeObjects 12 }

tmnxPppoeSessionBgpEntry         OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionBgpEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A row entry contains parameters used for a BGP peering."
    AUGMENTS    { tmnxPppoeSessionEntry }
    ::= { tmnxPppoeSessionBgpTable 1 }

TmnxPppoeSessionBgpEntry         ::= SEQUENCE
{
    tmnxPppoeSessionBgpPrngPlcyName  TNamedItemOrEmpty,
    tmnxPppoeSessionBgpAuthKeyChain  TNamedItemOrEmpty,
    tmnxPppoeSessionBgpMD5AuthKey    OCTET STRING,
    tmnxPppoeSessionBgpImportPolicy  TPolicyStatementNameOrEmpty,
    tmnxPppoeSessionBgpExportPolicy  TPolicyStatementNameOrEmpty,
    tmnxPppoeSessionBgpPeerAS        InetAutonomousSystemNumber,
    tmnxPppoeSessionBgpPeeringStatus BgpPeeringStatus
}

tmnxPppoeSessionBgpPrngPlcyName  OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionBgpPrngPlcyName indicates the peering
         policy which is used to set up the BGP peer for this pppoe session."
    ::= { tmnxPppoeSessionBgpEntry 1 }

tmnxPppoeSessionBgpAuthKeyChain  OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionBgpAuthKeyChain indicates the keychain
         which is used to sign and/or authenticate the BGP protocol stream."
    ::= { tmnxPppoeSessionBgpEntry 2 }

tmnxPppoeSessionBgpMD5AuthKey    OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionBgpMD5AuthKey indicates the
         authentication key used between BGP peers neighbors before
         establishing sessions. Authentication is done using the MD-5 message
         based digest protocol."
    ::= { tmnxPppoeSessionBgpEntry 3 }

tmnxPppoeSessionBgpImportPolicy  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionBgpImportPolicy indicates the import
         policy."
    ::= { tmnxPppoeSessionBgpEntry 4 }

tmnxPppoeSessionBgpExportPolicy  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionBgpExportPolicy indicates the export
         policy."
    ::= { tmnxPppoeSessionBgpEntry 5 }

tmnxPppoeSessionBgpPeerAS        OBJECT-TYPE
    SYNTAX      InetAutonomousSystemNumber
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionBgpPeerAS indicates the Autonomous System
         number for the remote peer."
    ::= { tmnxPppoeSessionBgpEntry 6 }

tmnxPppoeSessionBgpPeeringStatus OBJECT-TYPE
    SYNTAX      BgpPeeringStatus
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionBgpPeeringStatus indicates the status of
         the BGP peering session."
    ::= { tmnxPppoeSessionBgpEntry 7 }

tmnxPppoeSessionOverridesTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeSessionOverridesEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A table that contains PPPoE session qos overrides.

         This table is replace with
         TIMETRA-SUBSCRIBER-MGMT-MIB::tmnxSubPppOvrTable."
    ::= { tmnxPppoeObjects 13 }

tmnxPppoeSessionOverridesEntry   OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionOverridesEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Information about a specific PPPoE session qos override."
    INDEX       {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeSessionMac,
        tmnxPppoeSessionId,
        tmnxPppoeSessionOvrDirection,
        tmnxPppoeSessionOvrType,
        tmnxPppoeSessionOvrTypeId,
        tmnxPppoeSessionOvrTypeName
    }
    ::= { tmnxPppoeSessionOverridesTable 1 }

TmnxPppoeSessionOverridesEntry   ::= SEQUENCE
{
    tmnxPppoeSessionOvrDirection     TDirectionIngEgr,
    tmnxPppoeSessionOvrType          TQosOverrideType,
    tmnxPppoeSessionOvrTypeId        Integer32,
    tmnxPppoeSessionOvrTypeName      TNamedItemOrEmpty,
    tmnxPppoeSessionOvrPIR           TPIRRateOverride,
    tmnxPppoeSessionOvrCIR           TCIRRateOverride,
    tmnxPppoeSessionOvrCBS           TBurstSizeBytesOverride,
    tmnxPppoeSessionOvrMBS           TBurstSizeBytesOverride
}

tmnxPppoeSessionOvrDirection     OBJECT-TYPE
    SYNTAX      TDirectionIngEgr
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOvrDirection indicates whether this row
         specifies ingress or egress qos override parameters."
    ::= { tmnxPppoeSessionOverridesEntry 1 }

tmnxPppoeSessionOvrType          OBJECT-TYPE
    SYNTAX      TQosOverrideType
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOvrType indicates what field has been
         overwritten by this row."
    ::= { tmnxPppoeSessionOverridesEntry 2 }

tmnxPppoeSessionOvrTypeId        OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOvrTypeId indicates the id of the
         queue/policer that has been overwritten by this row.

         If the value of tmnxPppoeSessionOvrType is not 'queue (1)' or 'policer
         (2)', this field must be set to zero (0)."
    ::= { tmnxPppoeSessionOverridesEntry 3 }

tmnxPppoeSessionOvrTypeName      OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOvrTypeName indicates the name of the
         scheduler/arbiter that has been overwritten by this row.

         If the value of tmnxPppoeSessionOvrType is not 'arbiter (4)' or
         'scheduler (5)', this field must be set to zero (0)."
    ::= { tmnxPppoeSessionOverridesEntry 4 }

tmnxPppoeSessionOvrPIR           OBJECT-TYPE
    SYNTAX      TPIRRateOverride
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOvrPIR indicates the PIR rate in kbps
         allowed for the object overwritten by this row."
    ::= { tmnxPppoeSessionOverridesEntry 5 }

tmnxPppoeSessionOvrCIR           OBJECT-TYPE
    SYNTAX      TCIRRateOverride
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOvrCIR indicates the CIR rate in kbps
         allowed for the object overwritten by this row."
    ::= { tmnxPppoeSessionOverridesEntry 6 }

tmnxPppoeSessionOvrCBS           OBJECT-TYPE
    SYNTAX      TBurstSizeBytesOverride
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOvrCBS indicates the amount of reserved
         buffer space (in bytes) for the object overwritten by this row."
    ::= { tmnxPppoeSessionOverridesEntry 7 }

tmnxPppoeSessionOvrMBS           OBJECT-TYPE
    SYNTAX      TBurstSizeBytesOverride
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionOvrMBS indicates the maximum amount of
         reserved buffer space (in bytes) for the object overwritten by this
         row."
    ::= { tmnxPppoeSessionOverridesEntry 8 }

tmnxPppoeSessionAleTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeSessionAleEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A table that contains PPPoE session Access Loop Encapsulation
         information.

         Entries in this table are created and destroyed by the system.

         This table is a sparse augment of the tmnxPppoeSessionTable: entries
         are created only for PPPoE sessions for which Access Loop
         Encapsulation information is available.

         This table is replaced with
         TIMETRA-SUBSCRIBER-MGMT-MIB::tmnxSubPppAleTable"
    ::= { tmnxPppoeObjects 15 }

tmnxPppoeSessionAleEntry         OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionAleEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Access Loop Encapsulation Information about a specific PPPoE session."
    INDEX       {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeSessionMac,
        tmnxPppoeSessionId
    }
    ::= { tmnxPppoeSessionAleTable 1 }

TmnxPppoeSessionAleEntry         ::= SEQUENCE
{
    tmnxPppoeSessionAleDatalink      TmnxAccessLoopEncapDataLink,
    tmnxPppoeSessionAleEncaps1       TmnxAccessLoopEncaps1,
    tmnxPppoeSessionAleEncaps2       TmnxAccessLoopEncaps2
}

tmnxPppoeSessionAleDatalink      OBJECT-TYPE
    SYNTAX      TmnxAccessLoopEncapDataLink
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionAleDatalink indicates the data link used
         by the subscriber host on the DSL access loop."
    ::= { tmnxPppoeSessionAleEntry 1 }

tmnxPppoeSessionAleEncaps1       OBJECT-TYPE
    SYNTAX      TmnxAccessLoopEncaps1
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionAleEncaps1 indicates the encapsulation
         used by the subscriber host on the DSL access loop."
    ::= { tmnxPppoeSessionAleEntry 2 }

tmnxPppoeSessionAleEncaps2       OBJECT-TYPE
    SYNTAX      TmnxAccessLoopEncaps2
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppoeSessionAleEncaps2 indicates the encapsulation
         used by the subscriber host on the DSL access loop."
    ::= { tmnxPppoeSessionAleEntry 3 }

tmnxPppoeClntPlcyTableLastChg    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyTableLastChg indicates the sysUpTime at
         the time of the most recent management-initiated change to the
         tmnxPppoeClntPlcyTable."
    ::= { tmnxPppoeObjects 16 }

tmnxPppoeClntPlcyTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeClntPlcyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeClntPlcyTable has an entry for each PPP(oE) client policy
         configured in the system.

         This table can be used to configure PPP for PPPoE (PPP over Ethernet)
         clients."
    ::= { tmnxPppoeObjects 17 }

tmnxPppoeClntPlcyEntry           OBJECT-TYPE
    SYNTAX      TmnxPppoeClntPlcyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a PPP(oE) client policy configured in the
         system.

         Entries can be created and deleted via SNMP SET operations on the
         object tmnxPppoeClntPlcyRowStatus."
    INDEX       { IMPLIED tmnxPppoeClntPlcyName }
    ::= { tmnxPppoeClntPlcyTable 1 }

TmnxPppoeClntPlcyEntry           ::= SEQUENCE
{
    tmnxPppoeClntPlcyName            TNamedItem,
    tmnxPppoeClntPlcyRowStatus       RowStatus,
    tmnxPppoeClntPlcyLastMgmtChg     TimeStamp,
    tmnxPppoeClntPlcyDescription     TItemDescription,
    tmnxPppoeClntPlcyKaInterval      Unsigned32,
    tmnxPppoeClntPlcyKaHoldUpM       Unsigned32,
    tmnxPppoeClntPlcyMru             Unsigned32,
    tmnxPppoeClntPlcyMtu             Unsigned32,
    tmnxPppoeClntPlcyStack           BITS,
    tmnxPppoeClntPlcyRestartInit     Unsigned32,
    tmnxPppoeClntPlcyRestartMax      Unsigned32,
    tmnxPppoeClntPlcyPythonPlcy      TNamedItemOrEmpty
}

tmnxPppoeClntPlcyName            OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyName specifies the name of the PPP(oE)
         client policy."
    ::= { tmnxPppoeClntPlcyEntry 1 }

tmnxPppoeClntPlcyRowStatus       OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyRowStatus controls the creation and
         deletion of rows in this table."
    ::= { tmnxPppoeClntPlcyEntry 2 }

tmnxPppoeClntPlcyLastMgmtChg     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyLastMgmtChg indicates the sysUpTime at
         the time of the most recent management-initiated change to this table
         row."
    ::= { tmnxPppoeClntPlcyEntry 3 }

tmnxPppoeClntPlcyDescription     OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyDescription specifies the user provided
         description of this PPP client policy."
    DEFVAL      { "" }
    ::= { tmnxPppoeClntPlcyEntry 4 }

tmnxPppoeClntPlcyKaInterval      OBJECT-TYPE
    SYNTAX      Unsigned32 (10..300)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value tmnxPppoeClntPlcyKaInterval specifies the time interval in
         seconds at which LCP echo requests are transmitted."
    DEFVAL      { 30 }
    ::= { tmnxPppoeClntPlcyEntry 5 }

tmnxPppoeClntPlcyKaHoldUpM       OBJECT-TYPE
    SYNTAX      Unsigned32 (1..5)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyKaHoldUpM specifies how many LCP
         keepalive messages can be missed before the related PPP session is
         brought down."
    DEFVAL      { 3 }
    ::= { tmnxPppoeClntPlcyEntry 6 }

tmnxPppoeClntPlcyMru             OBJECT-TYPE
    SYNTAX      Unsigned32 (512..9154)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyMru specifies the Maximum Receive Unit
         (MRU) value that will be signaled by the PPPoE client."
    DEFVAL      { 1492 }
    ::= { tmnxPppoeClntPlcyEntry 7 }

tmnxPppoeClntPlcyMtu             OBJECT-TYPE
    SYNTAX      Unsigned32 (512..9154)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyMtu specifies the largest IP packet that
         can be sent out without being fragmented over the specific PPPoE
         tunnel."
    DEFVAL      { 1492 }
    ::= { tmnxPppoeClntPlcyEntry 8 }

tmnxPppoeClntPlcyStack           OBJECT-TYPE
    SYNTAX      BITS {
        ipv4      (0),
        ipv6Slaac (1)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyStack specifies which NCP sessions will
         be started in the PPPoE client and how addresses will be retrieved
         within that NCP session.

         'ipv4' indicates that IPCP will be started and will be used to
         retrieve an IPv4 address. 'ipv6Slaac' indicates that IPv6CP will be
         started and SLAAC will be used to retrieve an IPv6 address. At least
         one of the options needs to be specified.

         This value can be overridden by dynamic configuration, for example
         Radius."
    DEFVAL      { {ipv4} }
    ::= { tmnxPppoeClntPlcyEntry 9 }

tmnxPppoeClntPlcyRestartInit     OBJECT-TYPE
    SYNTAX      Unsigned32 (10..3600)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyRestartInit specifies the initial
         backoff time in seconds."
    DEFVAL      { 30 }
    ::= { tmnxPppoeClntPlcyEntry 10 }

tmnxPppoeClntPlcyRestartMax      OBJECT-TYPE
    SYNTAX      Unsigned32 (10..3600)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyRestartMax specifies the maximum backoff
         time in seconds."
    DEFVAL      { 600 }
    ::= { tmnxPppoeClntPlcyEntry 11 }

tmnxPppoeClntPlcyPythonPlcy      OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPlcyPythonPlcy specifies the Python policy
         used for sending an receiving PPPoE packets by this PPPoE client.

         A nonzero value must correspond to a row in the
         TIMETRA-PYTHON-MIB::tmnxPythonPolicyTable."
    DEFVAL      { "" }
    ::= { tmnxPppoeClntPlcyEntry 12 }

tmnxPppoeClientTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeClientEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeClientTable has an entry for each PPPoE client present in
         the system."
    ::= { tmnxPppoeObjects 18 }

tmnxPppoeClientEntry             OBJECT-TYPE
    SYNTAX      TmnxPppoeClientEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a PPPoE client present in the system."
    INDEX       { IMPLIED tmnxPppoeClntIdent }
    ::= { tmnxPppoeClientTable 1 }

TmnxPppoeClientEntry             ::= SEQUENCE
{
    tmnxPppoeClntIdent               DisplayString,
    tmnxPppoeClntSvcId               TmnxServId,
    tmnxPppoeClntMac                 MacAddress,
    tmnxPppoeClntUpTime              TimeTicks,
    tmnxPppoeClntPolicy              TNamedItem,
    tmnxPppoeClntServiceName         DisplayString,
    tmnxPppoeClntSessionId           TmnxPppoeSessionId,
    tmnxPppoeClntAcMac               MacAddress,
    tmnxPppoeClntAcName              DisplayString,
    tmnxPppoeClntLcpState            TmnxPppCpState,
    tmnxPppoeClntIpcpState           TmnxPppCpState,
    tmnxPppoeClntIpv6cpState         TmnxPppCpState,
    tmnxPppoeClntLocalMagicNum       Unsigned32,
    tmnxPppoeClntRemoteMagicNum      Unsigned32,
    tmnxPppoeClntRemoteMru           Unsigned32,
    tmnxPppoeClntPppUserName         TmnxPppoeUserName,
    tmnxPppoeClntPppAuthProtocol     INTEGER,
    tmnxPppoeClntIpcpIpAddrType      InetAddressType,
    tmnxPppoeClntIpcpIpAddr          InetAddress,
    tmnxPppoeClntIpcpPriDnsType      InetAddressType,
    tmnxPppoeClntIpcpPriDns          InetAddress,
    tmnxPppoeClntIpcpSecDnsType      InetAddressType,
    tmnxPppoeClntIpcpSecDns          InetAddress,
    tmnxPppoeClntIpcpPriNbnsType     InetAddressType,
    tmnxPppoeClntIpcpPriNbns         InetAddress,
    tmnxPppoeClntIpcpSecNbnsType     InetAddressType,
    tmnxPppoeClntIpcpSecNbns         InetAddress,
    tmnxPppoeClntIpv6cpInterfaceId   OCTET STRING,
    tmnxPppoeClntSlaacPrefixType     InetAddressType,
    tmnxPppoeClntSlaacPrefix         InetAddress,
    tmnxPppoeClntSlaacPrefixLen      InetAddressPrefixLength,
    tmnxPppoeClntSlaacPrefixTimeout  Unsigned32,
    tmnxPppoeClntSlaacPriDnsType     InetAddressType,
    tmnxPppoeClntSlaacPriDns         InetAddress,
    tmnxPppoeClntSlaacSecDnsType     InetAddressType,
    tmnxPppoeClntSlaacSecDns         InetAddress
}

tmnxPppoeClntIdent               OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (1..64))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIdent indicates an identification string for
         the PPPoE client."
    ::= { tmnxPppoeClientEntry 1 }

tmnxPppoeClntSvcId               OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntSvcId indicates the service ID of the PPPoE
         client."
    ::= { tmnxPppoeClientEntry 2 }

tmnxPppoeClntMac                 OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMac indicates the MAC address of the PPPoE
         client."
    ::= { tmnxPppoeClientEntry 3 }

tmnxPppoeClntUpTime              OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntUpTime indicates how long (in hundredths of
         a second) that the PPPoE client has it's PPP stack in the 'up' state."
    ::= { tmnxPppoeClientEntry 4 }

tmnxPppoeClntPolicy              OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPolicy specifies the policy applicable for
         the PPPoE client. The specific policy can be found in
         TIMETRA-PPPOE-MIB::tmnxPppoeClntPlcyTable."
    ::= { tmnxPppoeClientEntry 5 }

tmnxPppoeClntServiceName         OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..247))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntServiceName indicates the content of the
         Service-Name tag used during the PPPoE discovery phase of the PPPoE
         client."
    ::= { tmnxPppoeClientEntry 6 }

tmnxPppoeClntSessionId           OBJECT-TYPE
    SYNTAX      TmnxPppoeSessionId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntSessionId indicates the session id learned
         during the PPPoE discovery phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 7 }

tmnxPppoeClntAcMac               OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntAcMac indicates the Access Concentrator's
         MAC address learned during the PPPoE discovery phase of the PPPoE
         client."
    ::= { tmnxPppoeClientEntry 8 }

tmnxPppoeClntAcName              OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntAcName indicates the Access Concentrator's
         name learned during the PPPoE discovery phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 9 }

tmnxPppoeClntLcpState            OBJECT-TYPE
    SYNTAX      TmnxPppCpState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntLcpState indicates the current state of the
         PPP Link Control Protocol of the PPPoE client."
    ::= { tmnxPppoeClientEntry 10 }

tmnxPppoeClntIpcpState           OBJECT-TYPE
    SYNTAX      TmnxPppCpState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpState indicates the current state of the
         PPP IP Control Protocol of the PPPoE client."
    ::= { tmnxPppoeClientEntry 11 }

tmnxPppoeClntIpv6cpState         OBJECT-TYPE
    SYNTAX      TmnxPppCpState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpv6cpState indicates the current state of
         the PPP IPv6 Control Protocol of the PPPoE client."
    ::= { tmnxPppoeClientEntry 12 }

tmnxPppoeClntLocalMagicNum       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntLocalMagicNum indicates the local
         Magic-Number negotiated during the PPP LCP phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 13 }

tmnxPppoeClntRemoteMagicNum      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRemoteMagicNum indicates the remote
         Magic-Number negotiated during the PPP LCP phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 14 }

tmnxPppoeClntRemoteMru           OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRemoteMru indicates the remote MRU
         negotiated during the PPP LCP phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 15 }

tmnxPppoeClntPppUserName         OBJECT-TYPE
    SYNTAX      TmnxPppoeUserName
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPppUserName indicates the user name used
         during the PPP authentication phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 16 }

tmnxPppoeClntPppAuthProtocol     OBJECT-TYPE
    SYNTAX      INTEGER {
        none (0),
        pap  (1),
        chap (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntPppAuthProtocol indicates the PPP protocol
         used to authenticate the PPPoE client.

         The value 'none' indicates that no PPP authentication was done. The
         value 'pap' indicates that authentication was done via the Password
         Authentication Protocol. The value 'chap' indicates that
         authentication was done via the Challenge-Handshake Authentication
         Protocol."
    ::= { tmnxPppoeClientEntry 17 }

tmnxPppoeClntIpcpIpAddrType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpIpAddrType indicates the address type of
         tmnxPppoeClntIpcpIpAddr."
    ::= { tmnxPppoeClientEntry 18 }

tmnxPppoeClntIpcpIpAddr          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpIpAddr indicates the IP address learned
         during the PPP IPCP phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 19 }

tmnxPppoeClntIpcpPriDnsType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpPriDnsType indicates the address type of
         tmnxPppoeClntIpcpPriDns."
    ::= { tmnxPppoeClientEntry 20 }

tmnxPppoeClntIpcpPriDns          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpPriDns indicates the primary DNS server
         learned during the PPP IPCP phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 21 }

tmnxPppoeClntIpcpSecDnsType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpSecDnsType indicates the address type of
         tmnxPppoeClntIpcpSecDns."
    ::= { tmnxPppoeClientEntry 22 }

tmnxPppoeClntIpcpSecDns          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpSecDns indicates the secondary DNS
         server learned during the PPP IPCP phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 23 }

tmnxPppoeClntIpcpPriNbnsType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpPriNbnsType indicates the address type
         of tmnxPppoeClntIpcpPriNbns."
    ::= { tmnxPppoeClientEntry 24 }

tmnxPppoeClntIpcpPriNbns         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpPriNbns indicates the primary NBNS
         server learned during the PPP IPCP phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 25 }

tmnxPppoeClntIpcpSecNbnsType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpSecNbnsType indicates the address type
         of tmnxPppoeClntIpcpSecNbns."
    ::= { tmnxPppoeClientEntry 26 }

tmnxPppoeClntIpcpSecNbns         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpcpSecNbns indicates the secondary NBNS
         server learned during the PPP IPCP phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 27 }

tmnxPppoeClntIpv6cpInterfaceId   OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (8))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntIpv6cpInterfaceId indicates the IPv6
         Interface Identifier learned during the PPP IPv6CP phase of the PPPoE
         client."
    ::= { tmnxPppoeClientEntry 28 }

tmnxPppoeClntSlaacPrefixType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntSlaacPrefixType indicates the address type
         of tmnxPppoeClntSlaacPrefix."
    ::= { tmnxPppoeClientEntry 29 }

tmnxPppoeClntSlaacPrefix         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntSlaacPrefix indicates the IPv6 prefix
         learned during the IPv6 SLAAC phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 30 }

tmnxPppoeClntSlaacPrefixLen      OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..128)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntSlaacPrefixLen indicates the length of
         tmnxPppoeClntSlaacPrefix."
    ::= { tmnxPppoeClientEntry 31 }

tmnxPppoeClntSlaacPrefixTimeout  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntSlaacPrefixTimeout indicates the remaining
         time during which tmnxPppoeClntSlaacPrefix is active."
    ::= { tmnxPppoeClientEntry 32 }

tmnxPppoeClntSlaacPriDnsType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntSlaacPriDnsType indicates the address type
         of tmnxPppoeClntSlaacPriDns."
    ::= { tmnxPppoeClientEntry 33 }

tmnxPppoeClntSlaacPriDns         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntSlaacPriDns indicates the primary DNS server
         learned during the IPv6 SLAAC phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 34 }

tmnxPppoeClntSlaacSecDnsType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntSlaacSecDnsType indicates the address type
         of tmnxPppoeClntSlaacSecDns."
    ::= { tmnxPppoeClientEntry 35 }

tmnxPppoeClntSlaacSecDns         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntSlaacSecDns indicates the secondary DNS
         server learned during the IPv6 SLAAC phase of the PPPoE client."
    ::= { tmnxPppoeClientEntry 36 }

tmnxPppoeClntStatsTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeClntStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeClntStatsTable has an entry for each PPPoE client in the
         system."
    ::= { tmnxPppoeObjects 19 }

tmnxPppoeClntStatsEntry          OBJECT-TYPE
    SYNTAX      TmnxPppoeClntStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each conceptual row represents statistics information about a PPPoE
         client.

         Entries in this table are created and destroyed by the system."
    AUGMENTS    { tmnxPppoeClientEntry }
    ::= { tmnxPppoeClntStatsTable 1 }

TmnxPppoeClntStatsEntry          ::= SEQUENCE
{
    tmnxPppoeClntTxPadi              Counter32,
    tmnxPppoeClntTxPadr              Counter32,
    tmnxPppoeClntTxPadt              Counter32,
    tmnxPppoeClntTxSession           Counter32,
    tmnxPppoeClntTxLcpEchoReq        Counter32,
    tmnxPppoeClntTxLcpEchoRep        Counter32,
    tmnxPppoeClntTxV6Rs              Counter32,
    tmnxPppoeClntTxV6DhcpInfo        Counter32,
    tmnxPppoeClntRxPado              Counter32,
    tmnxPppoeClntRxPads              Counter32,
    tmnxPppoeClntRxPadt              Counter32,
    tmnxPppoeClntRxSession           Counter32,
    tmnxPppoeClntRxLcpEchoReq        Counter32,
    tmnxPppoeClntRxLcpEchoRep        Counter32,
    tmnxPppoeClntRxV6Ra              Counter32,
    tmnxPppoeClntRxV6DhcpReply       Counter32,
    tmnxPppoeClntRxDropped           Counter32
}

tmnxPppoeClntTxPadi              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntTxPadi indicates the number of PADI (PPPoE
         Active Discovery Initiation) packets transmitted by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 1 }

tmnxPppoeClntTxPadr              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntTxPadr indicates the number of PADR (PPPoE
         Active Discovery Request) packets transmitted by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 2 }

tmnxPppoeClntTxPadt              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntTxPadt indicates the number of PADT (PPPoE
         Active Discovery Terminate) packets transmitted by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 3 }

tmnxPppoeClntTxSession           OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntTxSession indicates the number of PPP
         session stage packets transmitted by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 4 }

tmnxPppoeClntTxLcpEchoReq        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntTxLcpEchoReq indicates the number of LCP
         echo requests packets transmitted by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 5 }

tmnxPppoeClntTxLcpEchoRep        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntTxLcpEchoRep indicates the number of LCP
         echo replies packets transmitted by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 6 }

tmnxPppoeClntTxV6Rs              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntTxV6Rs indicates the number of IPv6
         Router-Solicit packets transmitted by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 7 }

tmnxPppoeClntTxV6DhcpInfo        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntTxV6DhcpInfo indicates the number of IPv6
         DHCP6 Info-Request packets transmitted by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 8 }

tmnxPppoeClntRxPado              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRxPado indicates the number of PADO (PPPoE
         Active Discovery Offer) packets received by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 9 }

tmnxPppoeClntRxPads              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRxPads indicates the number of PADS (PPPoE
         Active Discovery Session) packets received by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 10 }

tmnxPppoeClntRxPadt              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRxPadt indicates the number of PADT (PPPoE
         Active Discovery Terminate) packets received by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 11 }

tmnxPppoeClntRxSession           OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRxSession indicates the number of PPP
         session stage packets received by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 12 }

tmnxPppoeClntRxLcpEchoReq        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRxLcpEchoReq indicates the number of LCP
         echo requests packets received by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 13 }

tmnxPppoeClntRxLcpEchoRep        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRxLcpEchoRep indicates the number of LCP
         echo replies packets received by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 14 }

tmnxPppoeClntRxV6Ra              OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRxV6Ra indicates the number of IPv6
         Router-Advertisement packets received by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 15 }

tmnxPppoeClntRxV6DhcpReply       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRxV6DhcpReply indicates the number of IPv6
         DHCPv6 Reply packets received by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 16 }

tmnxPppoeClntRxDropped           OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntRxDropped indicates the number of packets
         dropped by this PPPoE client."
    ::= { tmnxPppoeClntStatsEntry 17 }

tmnxPppoeClntMdaStatsTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeClntMdaStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeClntMdaStatsTable contains status and statistics
         information about PPPoE Client traffic processing in ISA Media
         Dependent Adapters (MDA)."
    ::= { tmnxPppoeObjects 20 }

tmnxPppoeClntMdaStatsEntry       OBJECT-TYPE
    SYNTAX      TmnxPppoeClntMdaStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each conceptual row contains contains status and statistics
         information about PPPoE Client traffic processing in a particular ISA
         MDA.

         Conceptual rows in this table are created and removed automatically by
         the system.

         The system creates conceptual rows only for an MDA associated with a
         NAT ISA Group that is referred to by an E-Pipe service by means of a
         row in the TIMETRA-SERV-MIB::svcEpipeNatOutsideTable."
    INDEX       {
        tmnxNatIsaGrpId,
        tmnxChassisIndex,
        tmnxCardSlotNum,
        tmnxMDASlotNum
    }
    ::= { tmnxPppoeClntMdaStatsTable 1 }

TmnxPppoeClntMdaStatsEntry       ::= SEQUENCE
{
    tmnxPppoeClntMdaRxErr            Counter64,
    tmnxPppoeClntMdaRxErrNotPppoe    Counter64,
    tmnxPppoeClntMdaRxErrEchoMagic   Counter64,
    tmnxPppoeClntMdaRxErrNoSession   Counter64,
    tmnxPppoeClntMdaRxDiscovery      Counter64,
    tmnxPppoeClntMdaRxPppControl     Counter64,
    tmnxPppoeClntMdaRxEchoRequest    Counter64,
    tmnxPppoeClntMdaRxEchoReply      Counter64,
    tmnxPppoeClntMdaTxEchoRequest    Counter64,
    tmnxPppoeClntMdaTxEchoReply      Counter64
}

tmnxPppoeClntMdaRxErr            OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMdaRxErr indicates the number of PPPoE
         Client traffic receive errors on this NAT ISA MDA."
    ::= { tmnxPppoeClntMdaStatsEntry 1 }

tmnxPppoeClntMdaRxErrNotPppoe    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMdaRxErrNotPppoe indicates the number of
         non-PPPoE packets received."
    ::= { tmnxPppoeClntMdaStatsEntry 2 }

tmnxPppoeClntMdaRxErrEchoMagic   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMdaRxErrEchoMagic indicates the number of
         PPPoE Echo-Reply or Echo-Request packets received  with an unexpected
         PPP LCP Magic Number."
    ::= { tmnxPppoeClntMdaStatsEntry 4 }

tmnxPppoeClntMdaRxErrNoSession   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMdaRxErrNoSession indicates the number of
         PPPoE Echo or data packets received without an associated session."
    ::= { tmnxPppoeClntMdaStatsEntry 5 }

tmnxPppoeClntMdaRxDiscovery      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMdaRxDiscovery indicates the number of PPPoE
         Discovery packets received."
    ::= { tmnxPppoeClntMdaStatsEntry 6 }

tmnxPppoeClntMdaRxPppControl     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMdaRxPppControl indicates the number of PPP
         control packets received."
    ::= { tmnxPppoeClntMdaStatsEntry 7 }

tmnxPppoeClntMdaRxEchoRequest    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMdaRxEchoRequest indicates the number of LCP
         Echo-Request packets received."
    ::= { tmnxPppoeClntMdaStatsEntry 8 }

tmnxPppoeClntMdaRxEchoReply      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMdaRxEchoReply indicates the number of LCP
         Echo-Reply packets received."
    ::= { tmnxPppoeClntMdaStatsEntry 9 }

tmnxPppoeClntMdaTxEchoRequest    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMdaTxEchoRequest indicates the number of LCP
         Echo-Request packets transmitted."
    ::= { tmnxPppoeClntMdaStatsEntry 10 }

tmnxPppoeClntMdaTxEchoReply      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntMdaTxEchoReply indicates the number of LCP
         Echo-Reply packets transmitted."
    ::= { tmnxPppoeClntMdaStatsEntry 11 }

tmnxPppoeClntVappStatsTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppoeClntVappStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeClntVappStatsTable contains status and statistics
         information about PPPoE Client traffic processing in a NAT Virtual
         Machine within an Extended Service Appliance."
    ::= { tmnxPppoeObjects 21 }

tmnxPppoeClntVappStatsEntry      OBJECT-TYPE
    SYNTAX      TmnxPppoeClntVappStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each conceptual row contains contains status and statistics
         information about PPPoE Client traffic processing in a particular NAT
         Virtual Machine within an Extended Service Appliance.

         Conceptual rows in this table are created and removed automatically by
         the system.

         The system creates conceptual rows only for a Virtual Machine within
         an Extended Service Appliance associated with a NAT ISA Group that is
         referred to by an E-Pipe service by means of a row in the
         TIMETRA-SERV-MIB::svcEpipeNatOutsideTable."
    INDEX       {
        tmnxNatIsaGrpId,
        tmnxNatEsaNum,
        tmnxNatEsaVappNum
    }
    ::= { tmnxPppoeClntVappStatsTable 1 }

TmnxPppoeClntVappStatsEntry      ::= SEQUENCE
{
    tmnxPppoeClntVappRxErr           Counter64,
    tmnxPppoeClntVappRxErrNotPppoe   Counter64,
    tmnxPppoeClntVappRxErrEchoMagic  Counter64,
    tmnxPppoeClntVappRxErrNoSession  Counter64,
    tmnxPppoeClntVappRxDiscovery     Counter64,
    tmnxPppoeClntVappRxPppControl    Counter64,
    tmnxPppoeClntVappRxEchoRequest   Counter64,
    tmnxPppoeClntVappRxEchoReply     Counter64,
    tmnxPppoeClntVappTxEchoRequest   Counter64,
    tmnxPppoeClntVappTxEchoReply     Counter64
}

tmnxPppoeClntVappRxErr           OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntVappRxErr indicates the number of PPPoE
         Client traffic receive errors on this NAT Virtual Machine within an
         Extended Service Appliance."
    ::= { tmnxPppoeClntVappStatsEntry 1 }

tmnxPppoeClntVappRxErrNotPppoe   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntVappRxErrNotPppoe indicates the number of
         non-PPPoE packets received."
    ::= { tmnxPppoeClntVappStatsEntry 2 }

tmnxPppoeClntVappRxErrEchoMagic  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntVappRxErrEchoMagic indicates the number of
         PPPoE Echo-Reply or Echo-Request packets received  with an unexpected
         PPP LCP Magic Number."
    ::= { tmnxPppoeClntVappStatsEntry 4 }

tmnxPppoeClntVappRxErrNoSession  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntVappRxErrNoSession indicates the number of
         PPPoE Echo or data packets received without an associated session."
    ::= { tmnxPppoeClntVappStatsEntry 5 }

tmnxPppoeClntVappRxDiscovery     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntVappRxDiscovery indicates the number of
         PPPoE Discovery packets received."
    ::= { tmnxPppoeClntVappStatsEntry 6 }

tmnxPppoeClntVappRxPppControl    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntVappRxPppControl indicates the number of PPP
         control packets received."
    ::= { tmnxPppoeClntVappStatsEntry 7 }

tmnxPppoeClntVappRxEchoRequest   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntVappRxEchoRequest indicates the number of
         LCP Echo-Request packets received."
    ::= { tmnxPppoeClntVappStatsEntry 8 }

tmnxPppoeClntVappRxEchoReply     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntVappRxEchoReply indicates the number of LCP
         Echo-Reply packets received."
    ::= { tmnxPppoeClntVappStatsEntry 9 }

tmnxPppoeClntVappTxEchoRequest   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntVappTxEchoRequest indicates the number of
         LCP Echo-Request packets transmitted."
    ::= { tmnxPppoeClntVappStatsEntry 10 }

tmnxPppoeClntVappTxEchoReply     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeClntVappTxEchoReply indicates the number of LCP
         Echo-Reply packets transmitted."
    ::= { tmnxPppoeClntVappStatsEntry 11 }

tmnxPppoeNotificationObjs        OBJECT IDENTIFIER ::= { tmnxPppoe 2 }

tmnxPppoeSessionFailureReason    OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The object tmnxPppoeSessionFailureReason indicates the problem
         encountered by the system while trying to create a new PPPoE session
         in the tmnxPppoeSessionTable."
    ::= { tmnxPppoeNotificationObjs 1 }

tmnxPppoeNcpFailureProtocol      OBJECT-TYPE
    SYNTAX      INTEGER {
        ipcp   (1),
        ipv6cp (2)
    }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppoeNcpFailureProtocol indicates the failing NCP
         protocol."
    ::= { tmnxPppoeNotificationObjs 2 }

tmnxPppoeNcpFailureReason        OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The object tmnxPppoeNcpFailureReason indicates the problem encountered
         by the system during NCP phase."
    ::= { tmnxPppoeNotificationObjs 3 }

tmnxPppoeNotifyDescription       OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The object tmnxPppoeNotifyDescription is a printable character string."
    ::= { tmnxPppoeNotificationObjs 4 }

tmnxPppoeLacSteeringFailure      OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The object tmnxPppoeLacSteeringFailure indicates the problem
         encountered by the system while trying to steer a PPPoE/LAC session in
         the tmnxPppoeSessionTable."
    ::= { tmnxPppoeNotificationObjs 5 }

tmnxPppoeLacSteeringSession      OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The object tmnxPppoeLacSteeringSession indicates the session
         (mac,sessionid,username) of a PPPoE/LAC session."
    ::= { tmnxPppoeNotificationObjs 6 }

tmnxPppoeLacSteeringProfile      OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The object tmnxPppoeLacSteeringProfile indicates the steering profile
         used by a PPPoE/LAC session."
    ::= { tmnxPppoeNotificationObjs 7 }

tmnxPppoeMaxSessionsOvrReason    OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The object tmnxPppoeMaxSessionsOvrReason indicates the problem
         encountered by the system while trying to create a new PPPoE session
         in the tmnxPppoeSessionTable."
    ::= { tmnxPppoeNotificationObjs 8 }

tmnxPppoeLacFragVRtrID           OBJECT-TYPE
    SYNTAX      TmnxVRtrID
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The object tmnxPppoeLacFragVRtrID is a number used to identify a
         virtual router instance in the system."
    ::= { tmnxPppoeNotificationObjs 9 }

tmnxPppoeLacFragFpeId            OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 1..64)
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The object tmnxPppoeLacFragFpeId indicates the FPE id used for LAC
         fragmentation for the associated PPPoE session."
    ::= { tmnxPppoeNotificationObjs 10 }

tmnxPppObjects                   OBJECT IDENTIFIER ::= { tmnxPppoe 3 }

tmnxPppIesIfTableLastChg         OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppIesIfTableLastChg indicates the sysUpTime at the
         time of the most recent management-initiated change to the
         tmnxPppIesIfTable."
    ::= { tmnxPppObjects 1 }

tmnxPppIesIfTable                OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppIesIfEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "A table that contains IES interface PPP configuration information.

         A row is automatically created in the tmnxPppIesIfTable for an entry
         in the iesIfTable where the value of the object iesIfType is equal to
         'group (3)'.

         This table is obsoleted in release 23.3 and later."
    ::= { tmnxPppObjects 2 }

tmnxPppIesIfEntry                OBJECT-TYPE
    SYNTAX      TmnxPppIesIfEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "PPP specific information about an IES interface.

         This list is obsoleted in release 23.3 and later."
    INDEX       {
        svcId,
        iesIfIndex
    }
    ::= { tmnxPppIesIfTable 1 }

TmnxPppIesIfEntry                ::= SEQUENCE
{
    tmnxPppIesIfLastChg              TimeStamp,
    tmnxPppIesIfDescription          TItemDescription,
    tmnxPppIesIfAdminState           TmnxPppoeAdminStatus,
    tmnxPppIesIfPolicy               TNamedItem,
    tmnxPppIesIfSessionLimit         Unsigned32,
    tmnxPppIesIfUserDb               TNamedItemOrEmpty
}

tmnxPppIesIfLastChg              OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppIesIfLastChg indicates the sysUpTime at the time
         of the most recent management-initiated change to this table row.

         This object is obsoleted in release 23.3 and later."
    ::= { tmnxPppIesIfEntry 1 }

tmnxPppIesIfDescription          OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tmnxPppIesIfDescription specifies a user
         provided description for PPP on this IES interface.

         This object is obsoleted in release 23.3 and later."
    DEFVAL      { "" }
    ::= { tmnxPppIesIfEntry 2 }

tmnxPppIesIfAdminState           OBJECT-TYPE
    SYNTAX      TmnxPppoeAdminStatus
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tmnxPppIesIfAdminState specifies the
         administrative state of PPP on this IES interface.

         This object is obsoleted in release 23.3 and later."
    DEFVAL      { disabled }
    ::= { tmnxPppIesIfEntry 3 }

tmnxPppIesIfPolicy               OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppIesIfPolicy specifies the PPP policy applicable on
         this IES interface.

         This object is obsoleted in release 23.3 and later."
    DEFVAL      { "default" }
    ::= { tmnxPppIesIfEntry 4 }

tmnxPppIesIfSessionLimit         OBJECT-TYPE
    SYNTAX      Unsigned32 (1..131071)
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppIesIfSessionLimit specifies the maximum number of
         PPP sessions allowed on this IES interface.

         This object is obsoleted in release 23.3 and later."
    DEFVAL      { 1 }
    ::= { tmnxPppIesIfEntry 5 }

tmnxPppIesIfUserDb               OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The value of tmnxPppIesIfUserDb specifies the local user database to
         use for PPP PAP/CHAP based authentication.

         If no authentication with the local user database is required, the
         value of this object must be set to the empty string.

         This object is obsoleted in release 23.3 and later."
    DEFVAL      { "" }
    ::= { tmnxPppIesIfEntry 8 }

tmnxMlpppObjects                 OBJECT IDENTIFIER ::= { tmnxPppObjects 3 }

tmnxMlpppBundleTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxMlpppBundleEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxMlpppBundleTable allows the monitoring of subscriber MLPPP
         (Multi Link PPP) Bundles."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol"
    ::= { tmnxMlpppObjects 1 }

tmnxMlpppBundleEntry             OBJECT-TYPE
    SYNTAX      TmnxMlpppBundleEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each conceptual row represents a subscriber MLPPP Bundle.

         Entries in this table are created and destroyed by the system."
    INDEX       { tmnxMlpppBundleIndex }
    ::= { tmnxMlpppBundleTable 1 }

TmnxMlpppBundleEntry             ::= SEQUENCE
{
    tmnxMlpppBundleIndex             Unsigned32,
    tmnxMlpppBundleLocEpClass        TmnxMlpppEpClass,
    tmnxMlpppBundleLocEpAddress      OCTET STRING,
    tmnxMlpppBundleRemEpClass        TmnxMlpppEpClass,
    tmnxMlpppBundleRemEpAddress      OCTET STRING,
    tmnxMlpppBundleSubPppIndex       Unsigned32,
    tmnxMlpppBundleMaxLinks          Unsigned32,
    tmnxMlpppBundleActualLinks       Gauge32,
    tmnxMlpppBundleRemMrru           Unsigned32,
    tmnxMlpppBundleLocMrru           Unsigned32,
    tmnxMlpppBundleIndicators        BITS,
    tmnxMlpppBundleFragmentSize      Unsigned32,
    tmnxMlpppBundleMaxDelayCfg       Unsigned32,
    tmnxMlpppBundleMaxDelay          Unsigned32,
    tmnxMlpppBundleReassemblyTo      Unsigned32,
    tmnxMlpppBundleEgressRate        Unsigned32
}

tmnxMlpppBundleIndex             OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tmnxMlpppBundleIndex indicates the local
         identifier of the bundle."
    ::= { tmnxMlpppBundleEntry 1 }

tmnxMlpppBundleLocEpClass        OBJECT-TYPE
    SYNTAX      TmnxMlpppEpClass
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleLocEpClass indicates the address class of
         the local endpoint.

         If the value of tmnxMlpppBundleLocEpClass is equal to 'null', the
         address class of the MLPPP Endpoint Discriminator option was not
         present in a received Configure-Request."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.3 Endpoint Discriminator Option."
    ::= { tmnxMlpppBundleEntry 2 }

tmnxMlpppBundleLocEpAddress      OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..20))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleLocEpAddress indicates the address of the
         local MLPPP Endpoint.

         Its interpretation depends on the value of tmnxMlpppBundleLocEpClass."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.3 Endpoint Discriminator Option."
    ::= { tmnxMlpppBundleEntry 3 }

tmnxMlpppBundleRemEpClass        OBJECT-TYPE
    SYNTAX      TmnxMlpppEpClass
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleRemEpClass indicates the address class of
         the local endpoint.

         If the value of tmnxMlpppBundleRemEpClass is equal to 'null', the
         address class of the MLPPP Endpoint Discriminator option was not
         present in a received Configure-Request."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.3 Endpoint Discriminator Option."
    ::= { tmnxMlpppBundleEntry 4 }

tmnxMlpppBundleRemEpAddress      OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..20))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleRemEpAddress indicates the address of the
         local MLPPP Endpoint.

         Its interpretation depends on the value of tmnxMlpppBundleRemEpClass."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.3 Endpoint Discriminator Option."
    ::= { tmnxMlpppBundleEntry 5 }

tmnxMlpppBundleSubPppIndex       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleSubPppIndex indicates the local identifier
         of the subscriber PPP session.

         It is the index of the corresponding conceptual row in the
         TIMETRA-SUBSCRIBER-MGMT-MIB::tmnxSubPppTable."
    ::= { tmnxMlpppBundleEntry 6 }

tmnxMlpppBundleMaxLinks          OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleMaxLinks indicates the maximum number of
         links allowed for this bundle."
    ::= { tmnxMlpppBundleEntry 7 }

tmnxMlpppBundleActualLinks       OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleActualLinks indicates the actual number of
         links of this bundle."
    ::= { tmnxMlpppBundleEntry 8 }

tmnxMlpppBundleRemMrru           OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleRemMrru indicates the Maximum
         Reconstructed Receive Unit (MRRU) for this MLPPP bundle.

         This value is derived from the values proposed by the MLPPP peer for
         the MLPPP links in this bundle."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.1 Multilink MRRU LCP option."
    ::= { tmnxMlpppBundleEntry 9 }

tmnxMlpppBundleLocMrru           OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleLocMrru indicates the Maximum
         Reconstructed Receive Unit (MRRU) for this MLPPP bundle."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.1 Multilink MRRU LCP option."
    ::= { tmnxMlpppBundleEntry 10 }

tmnxMlpppBundleIndicators        OBJECT-TYPE
    SYNTAX      BITS {
        lfiCfg       (0),
        lfi          (1),
        shortSeqNrRx (2),
        shortSeqNrTx (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleIndicators indicates various information
         about this bundle.

         lfiCfg - Link Fragmentation and Interleaving (LFI) configured
                  when this bundle was created;
         lfi - LFI active;
         shortSeqNrRx - Short Sequence Numbers used for incoming messages;
         shortSeqNrTx - Short Sequence Numbers for outgoing messages."
    ::= { tmnxMlpppBundleEntry 11 }

tmnxMlpppBundleFragmentSize      OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleFragmentSize indicates the fragment size
         for this bundle.

         While there is no fragmentation and interleaving on this bundle, the
         value of this object is equal to zero."
    ::= { tmnxMlpppBundleEntry 12 }

tmnxMlpppBundleMaxDelayCfg       OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleMaxDelayCfg indicates the maximum delay
         configured for this bundle when it was created."
    ::= { tmnxMlpppBundleEntry 13 }

tmnxMlpppBundleMaxDelay          OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleMaxDelay indicates the maximum delay for
         this bundle."
    ::= { tmnxMlpppBundleEntry 14 }

tmnxMlpppBundleReassemblyTo      OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleReassemblyTo indicates the reassembly
         timeout configured for this bundle when it was created."
    ::= { tmnxMlpppBundleEntry 15 }

tmnxMlpppBundleEgressRate        OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppBundleEgressRate indicates the nominal egress
         rate for this bundle."
    ::= { tmnxMlpppBundleEntry 16 }

tmnxMlpppLinkTable               OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxMlpppLinkEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxMlpppLinkTable contains the subscriber MLPPP (Multi Link PPP)
         link sessions ordered per bundle."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol"
    ::= { tmnxMlpppObjects 2 }

tmnxMlpppLinkEntry               OBJECT-TYPE
    SYNTAX      TmnxMlpppLinkEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each conceptual row represents a subscriber MLPPP link.

         Entries in this table are created and destroyed by the system."
    INDEX       {
        tmnxMlpppBundleIndex,
        tmnxSubPppIndex
    }
    ::= { tmnxMlpppLinkTable 1 }

TmnxMlpppLinkEntry               ::= SEQUENCE
{ tmnxMlpppLinkRemMrru             Unsigned32 }

tmnxMlpppLinkRemMrru             OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxMlpppLinkRemMrru indicates the Maximum Reconstructed
         Receive Unit (MRRU) proposed by the MLPPP peer for this MLPPP link."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.1 Multilink MRRU LCP option."
    ::= { tmnxMlpppLinkEntry 1 }

tmnxPppPlcyMlpppTableLastCh      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppPlcyMlpppTableLastCh indicates the sysUpTime at
         the time of the most recent management-initiated change to the
         tmnxPppPlcyMlpppTable."
    ::= { tmnxMlpppObjects 3 }

tmnxPppPlcyMlpppTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF TmnxPppPlcyMlpppEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tmnxPppPlcyMlpppTable has an entry for each PPP(oE) policy
         configured in the system.

         This table can be used to configure MLPPP for PPPoE (PPP over
         Ethernet) and PPPoA (PPP over ATM) subscribers."
    ::= { tmnxMlpppObjects 4 }

tmnxPppPlcyMlpppEntry            OBJECT-TYPE
    SYNTAX      TmnxPppPlcyMlpppEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents MLPPP information of a PPP(oE) policy
         configured in the system.

         Conceptual rows are created and destroyed automatically by the system."
    AUGMENTS    { tmnxPppoePlcyEntry }
    ::= { tmnxPppPlcyMlpppTable 1 }

TmnxPppPlcyMlpppEntry            ::= SEQUENCE
{
    tmnxPppPlcyMlpppLastCh           TimeStamp,
    tmnxPppPlcyMlpppAcceptMrru       TruthValue,
    tmnxPppPlcyMlpppEpClass          TmnxMlpppEpClass,
    tmnxPppPlcyMlpppEpIpv4Address    InetAddressIPv4,
    tmnxPppPlcyMlpppEpMacAddress     MacAddress,
    tmnxPppPlcyMlpppShortSeqNumberRx TruthValue
}

tmnxPppPlcyMlpppLastCh           OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppPlcyMlpppLastCh indicates the sysUpTime at the
         time of the most recent management-initiated change to this table row."
    ::= { tmnxPppPlcyMlpppEntry 1 }

tmnxPppPlcyMlpppAcceptMrru       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppPlcyMlpppAcceptMrru specifies if this system will
         accept the Multilink MRRU LCP option for the PPP sessions using this
         policy."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.1.  Multilink MRRU LCP option."
    DEFVAL      { false }
    ::= { tmnxPppPlcyMlpppEntry 2 }

tmnxPppPlcyMlpppEpClass          OBJECT-TYPE
    SYNTAX      TmnxMlpppEpClass { null (0), ipv4Address (2), macAddress (3) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppPlcyMlpppEpClass specifies the type of endpoint.

         If the value of 'tmnxPppPlcyMlpppEpClass' is equal to 'ipv4Address',
         the address for the MLPPP Endpoint Discriminator Option is taken from
         tmnxPppPlcyMlpppEpIpv4Address.

         If the value of 'tmnxPppPlcyMlpppEpClass' is equal to 'macAddress',
         the address for the MLPPP Endpoint Discriminator Option is taken from
         tmnxPppPlcyMlpppEpMacAddress.

         If the value of 'tmnxPppPlcyMlpppEpClass' is equal to 'null', the
         MLPPP Endpoint Discriminator Option must not be transmitted.

         A value other than 'null' is only allowed if this system performs the
         role of LAC with respect to the PPP clients using this policy."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.3 Endpoint Discriminator Option."
    DEFVAL      { null }
    ::= { tmnxPppPlcyMlpppEntry 3 }

tmnxPppPlcyMlpppEpIpv4Address    OBJECT-TYPE
    SYNTAX      InetAddressIPv4
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppPlcyMlpppEpIpv4Address specifies the class 2
         address to use in the MLPPP Endpoint Discriminator Option.

         While the value of tmnxPppPlcyMlpppEpClass is equal to 'ipv4Address',
         a value of all zeroes specifies that the system IP address be used;
         otherwise, it means that no address is specified."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.3 Endpoint Discriminator Option."
    DEFVAL      { '00000000'H }
    ::= { tmnxPppPlcyMlpppEntry 4 }

tmnxPppPlcyMlpppEpMacAddress     OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppPlcyMlpppEpMacAddress specifies the class 3
         address to use in the MLPPP Endpoint Discriminator Option.

         While the value of tmnxPppPlcyMlpppEpClass is equal to 'macAddress', a
         value of all zeroes specifies that the system MAC address be used;
         otherwise, it means that no address is specified."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP),
         section 5.1.3 Endpoint Discriminator Option."
    DEFVAL      { '000000000000'H }
    ::= { tmnxPppPlcyMlpppEntry 5 }

tmnxPppPlcyMlpppShortSeqNumberRx OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tmnxPppPlcyMlpppShortSeqNumberRx specifies if this system
         requests to receive short sequence numbers from the peer.

         If the value of this object is 'true', this system includes the Short
         Sequence Number Header Format Option in its LCP configuration options.

         If the value of this object is 'false', this system does not includes
         the Short Sequence Number Header Format Option in its LCP
         configuration options."
    REFERENCE
        "RFC 1990 The PPP Multilink Protocol (MP)
         section 5.1.2."
    DEFVAL      { false }
    ::= { tmnxPppPlcyMlpppEntry 6 }

tmnxPppoeConformance             OBJECT IDENTIFIER ::= { tmnxSRConfs 49 }

tmnxPppoeCompliances             OBJECT IDENTIFIER ::= { tmnxPppoeConformance 1 }

tmnxPPPoE77x0V6v0MIBCompliance   MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia 7750 SR and
         7710 series systems release R6.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV6v0Group,
            tmnxPPPoEV6v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup
        }
    ::= { tmnxPppoeCompliances 1 }

tmnxPPPoE77x0V6v1MIBCompliance   MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia 7750 SR and
         7710 series systems release R6.1."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV6v1Group,
            tmnxPPPoEV6v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPoEManagedRoutesGroup
        }
    ::= { tmnxPppoeCompliances 2 }

tmnxPPPoE77x0V7v0MIBCompliance   MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia 7750 SR and
         7710 series systems release R7.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV7v0Group,
            tmnxPPPoEV6v0NotifyGroup,
            tmnxPPPoEV6v0NotificationObjGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPoEManagedRoutesGroup,
            tmnxPPPoESessionBGPGroup
        }
    ::= { tmnxPppoeCompliances 3 }

tmnxPPPoE77x0V8v0MIBCompliance   MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia 7750 SR and
         7710 series systems release R8.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV8v0Group,
            tmnxPPPoEV8v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPoEManagedRoutesGroup,
            tmnxPPPoESessionBGPGroup
        }
    ::= { tmnxPppoeCompliances 4 }

tmnxPPPoE77x0V9v0MIBCompliance   MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia 7750 SR and
         7710 series systems release R9.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV8v0Group,
            tmnxPPPoEV9v0Group,
            tmnxPPPoEV8v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPV9v0Group,
            tmnxPPPPlcyAllowSameCidGroup
        }
    ::= { tmnxPppoeCompliances 5 }

tmnxPPPoEV10v0MIBCompliance      MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia SROS release
         10.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV8v0Group,
            tmnxPPPoEV9v0Group,
            tmnxPPPoEV10v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPV9v0Group,
            tmnxPPPMlpppGroup,
            tmnxPPPRejectDisabledNcp,
            tmnxPPPPlcyAllowSameCidGroup
        }
    ::= { tmnxPppoeCompliances 6 }

tmnxPPPoEV11v0MIBCompliance      MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia SROS release
         11.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV8v0Group,
            tmnxPPPoEV9v0Group,
            tmnxPPPoEV10v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPV9v0Group,
            tmnxPPPMlpppGroup,
            tmnxPPPRejectDisabledNcp,
            tmnxPPPLcpIgnoreMagic,
            tmnxPPPPlcyAllowSameCidGroup,
            tmnxPPPoEV11v0Group
        }
    ::= { tmnxPppoeCompliances 7 }

tmnxPPPoEV12v0MIBCompliance      MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia SROS release
         12.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV8v0Group,
            tmnxPPPoEV9v0Group,
            tmnxPPPoEV10v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPV9v0Group,
            tmnxPPPMlpppGroup,
            tmnxPPPRejectDisabledNcp,
            tmnxPPPLcpIgnoreMagic,
            tmnxPPPPlcyAllowSameCidGroup,
            tmnxPPPoEV12v0Group,
            tmnxPPPoEDefaultUsernameGroup
        }
    ::= { tmnxPppoeCompliances 8 }

tmnxPPPoEV14v0MIBCompliance      MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia SROS release
         14.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV8v0Group,
            tmnxPPPoEV9v0Group,
            tmnxPPPoEV10v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPV9v0Group,
            tmnxPPPMlpppGroup,
            tmnxPPPRejectDisabledNcp,
            tmnxPPPLcpIgnoreMagic,
            tmnxPPPPlcyAllowSameCidGroup,
            tmnxPPPoEV12v0Group,
            tmnxPPPoEDefaultUsernameGroup,
            tmnxPPPoEV14v0Group
        }
    ::= { tmnxPppoeCompliances 9 }

tmnxPPPoEV15v0MIBCompliance      MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia SROS release
         15.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV8v0Group,
            tmnxPPPoEV9v0Group,
            tmnxPPPoEV10v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPV9v0Group,
            tmnxPPPMlpppGroup,
            tmnxPPPRejectDisabledNcp,
            tmnxPPPLcpIgnoreMagic,
            tmnxPPPPlcyAllowSameCidGroup,
            tmnxPPPoEV12v0Group,
            tmnxPPPoEDefaultUsernameGroup,
            tmnxPPPoEV14v0Group,
            tmnxPPPoEV15v0Group,
            tmnxPPPoEV15v0NotifyGroup
        }
    ::= { tmnxPppoeCompliances 10 }

tmnxPPPoEV19v0MIBCompliance      MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia SROS release
         19.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV19v0Group,
            tmnxPPPoEV10v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPMlpppGroup,
            tmnxPPPoEV15v0NotifyGroup
        }
    ::= { tmnxPppoeCompliances 11 }

tmnxPPPoEV20v0MIBCompliance      MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia SROS release
         20.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV20v0Group,
            tmnxPPPoEV10v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPMlpppGroup,
            tmnxPPPoEV15v0NotifyGroup
        }
    ::= { tmnxPppoeCompliances 12 }

tmnxPPPoEV21v0MIBCompliance      MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia SROS release
         21.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV21v0Group
        }
    ::= { tmnxPppoeCompliances 13 }

tmnxPPPoEV22v0MIBCompliance      MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia SROS release
         22.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV20v0Group,
            tmnxPPPoEV21v0Group,
            tmnxPPPoEV22v0NotifyGroup,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPMlpppGroup,
            tmnxPPPoEV15v0NotifyGroup
        }
    ::= { tmnxPppoeCompliances 14 }

tmnxPPPoEV25v0MIBCompliance      MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for TIMETRA-PPPOE-MIB on Nokia SROS release
         25.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxPPPoEV20v0Group,
            tmnxPPPoEV21v0Group,
            tmnxPPPoEV6v0BsxGroup,
            tmnxPPPMlpppGroup,
            tmnxPPPoEV15v0NotifyGroup,
            tmnxPPPoEV22v0NotifyGroup,
            tmnxPPPoEV25v0NotifyGroup
        }
    ::= { tmnxPppoeCompliances 15 }

tmnxPppoeGroups                  OBJECT IDENTIFIER ::= { tmnxPppoeConformance 2 }

tmnxPPPoEV6v0Group               OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyTableLastChanged,
        tmnxPppoePlcyRowStatus,
        tmnxPppoePlcyLastMgmtChange,
        tmnxPppoePlcyDescription,
        tmnxPppoePlcyPppMtu,
        tmnxPppoePlcyLcpKaInterval,
        tmnxPppoePlcyLcpKaHoldUpMplier,
        tmnxPppoePlcyDisableAcCookies,
        tmnxPppoePlcyPadoDelay,
        tmnxPppoePlcyMaxSessionsPerMac,
        tmnxPppoePlcyReplyOnPadt,
        tmnxPppoePlcyPppOptionTblLstChg,
        tmnxPppoePlcyOptionRowStatus,
        tmnxPppoePlcyOptionLstMgmtChange,
        tmnxPppoePlcyOptionType,
        tmnxPppoePlcyOptionValue,
        tmnxPppoeIesIfInfoTableLastChg,
        tmnxPppoeIesIfLastChg,
        tmnxPppoeIesIfDescription,
        tmnxPppoeIesIfAdminState,
        tmnxPppoeIesIfPolicy,
        tmnxPppoeIesIfSessionLimit,
        tmnxPppoeIesIfSapSessionLimit,
        tmnxPppoeIesIfPapChapUserDb,
        tmnxPppoeSapRxPadi,
        tmnxPppoeSapRxPadr,
        tmnxPppoeSapRxPadt,
        tmnxPppoeSapRxSession,
        tmnxPppoeSapRxInvalidVersion,
        tmnxPppoeSapRxInvalidType,
        tmnxPppoeSapRxInvalidCode,
        tmnxPppoeSapRxInvalidSession,
        tmnxPppoeSapRxInvalidLen,
        tmnxPppoeSapRxInvalidTags,
        tmnxPppoeSapRxInvalidAcCookie,
        tmnxPppoeSapRxDropped,
        tmnxPppoeSapTxPado,
        tmnxPppoeSapTxPads,
        tmnxPppoeSapTxPadt,
        tmnxPppoeSapTxSession,
        tmnxPppoeSessionUpTime,
        tmnxPppoeSessionLcpState,
        tmnxPppoeSessionIpcpState,
        tmnxPppoeSessionPppMtu,
        tmnxPppoeSessionPppAuthProtocol,
        tmnxPppoeSessionPppUserName,
        tmnxPppoeSessionSubIdent,
        tmnxPppoeSessionOriginSubIdent,
        tmnxPppoeSessionSubProfString,
        tmnxPppoeSessionSlaProfString,
        tmnxPppoeSessionAncpString,
        tmnxPppoeSessionInterDestId,
        tmnxPppoeSessionOriginStrings,
        tmnxPppoeSessionSessionTimeout,
        tmnxPppoeSessionIpAddrType,
        tmnxPppoeSessionIpAddr,
        tmnxPppoeSessionPrimaryDnsType,
        tmnxPppoeSessionPrimaryDns,
        tmnxPppoeSessionSecondryDnsType,
        tmnxPppoeSessionSecondryDns,
        tmnxPppoeSessionPrimaryNbnsType,
        tmnxPppoeSessionPrimaryNbns,
        tmnxPppoeSessionSecondryNbnsType,
        tmnxPppoeSessionSecondryNbns,
        tmnxPppoeSessionOriginIpcpInfo,
        tmnxPppoeSessionCircuitId,
        tmnxPppoeSessionRemoteId,
        tmnxPppoeSessionModSubIdent,
        tmnxPppoeSessionModSubProfStr,
        tmnxPppoeSessionModSlaProfStr,
        tmnxPppoeSessionModAncpStr,
        tmnxPppoeSessionModInterDestId,
        tmnxPppoeSessionEvaluateState,
        tmnxPppoeSessionRxUnknownProto,
        tmnxPppoeSessionRxLcpConfReq,
        tmnxPppoeSessionRxLcpConfAck,
        tmnxPppoeSessionRxLcpConfNak,
        tmnxPppoeSessionRxLcpConfRej,
        tmnxPppoeSessionRxLcpTermReq,
        tmnxPppoeSessionRxLcpTermAck,
        tmnxPppoeSessionRxLcpCodeRej,
        tmnxPppoeSessionRxLcpEchoReq,
        tmnxPppoeSessionRxLcpEchoRep,
        tmnxPppoeSessionRxLcpProtRej,
        tmnxPppoeSessionRxLcpDiscReq,
        tmnxPppoeSessionTxLcpConfReq,
        tmnxPppoeSessionTxLcpConfAck,
        tmnxPppoeSessionTxLcpConfNak,
        tmnxPppoeSessionTxLcpConfRej,
        tmnxPppoeSessionTxLcpTermReq,
        tmnxPppoeSessionTxLcpTermAck,
        tmnxPppoeSessionTxLcpCodeRej,
        tmnxPppoeSessionTxLcpEchoReq,
        tmnxPppoeSessionTxLcpEchoRep,
        tmnxPppoeSessionTxLcpProtRej,
        tmnxPppoeSessionTxLcpDiscReq,
        tmnxPppoeSessionRxPapAuthReq,
        tmnxPppoeSessionTxPapAuthAck,
        tmnxPppoeSessionTxPapAuthNak,
        tmnxPppoeSessionRxChapResponse,
        tmnxPppoeSessionTxChapChallenge,
        tmnxPppoeSessionTxChapSuccess,
        tmnxPppoeSessionTxChapFailure,
        tmnxPppoeSessionRxIpcpConfReq,
        tmnxPppoeSessionRxIpcpConfAck,
        tmnxPppoeSessionRxIpcpConfNak,
        tmnxPppoeSessionRxIpcpConfRej,
        tmnxPppoeSessionRxIpcpTermReq,
        tmnxPppoeSessionRxIpcpTermAck,
        tmnxPppoeSessionRxIpcpCodeRej,
        tmnxPppoeSessionTxIpcpConfReq,
        tmnxPppoeSessionTxIpcpConfAck,
        tmnxPppoeSessionTxIpcpConfNak,
        tmnxPppoeSessionTxIpcpConfRej,
        tmnxPppoeSessionTxIpcpTermReq,
        tmnxPppoeSessionTxIpcpTermAck,
        tmnxPppoeSessionTxIpcpCodeRej
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE on Nokia SROS series systems 6.0
         release."
    ::= { tmnxPppoeGroups 1 }

tmnxPPPoEV6v0NotifyGroup         NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxPppoeSessionFailure
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of notifications generated by the PPPoE feature on Nokia
         SROS series systems 6.0 release."
    ::= { tmnxPppoeGroups 2 }

tmnxPPPoEV6v0NotificationObjGroup OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeSessionFailureReason
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of PPPoE notification
         objects on Nokia SROS series systems 6.0 release."
    ::= { tmnxPppoeGroups 3 }

tmnxPPPoEV6v0BsxGroup            OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeSessionAppProfString,
        tmnxPppoeSessionModAppProfStr
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of PPPoE BSX (Application
         Assurance) objects on Nokia SROS series systems 6.0 release."
    ::= { tmnxPppoeGroups 4 }

tmnxPPPoEManagedRoutesGroup      OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeManagedRouteStatus
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE Managed Routes on Nokia SROS
         series systems."
    ::= { tmnxPppoeGroups 5 }

tmnxPPPoEV6v1Group               OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyTableLastChanged,
        tmnxPppoePlcyRowStatus,
        tmnxPppoePlcyLastMgmtChange,
        tmnxPppoePlcyDescription,
        tmnxPppoePlcyPppMtu,
        tmnxPppoePlcyLcpKaInterval,
        tmnxPppoePlcyLcpKaHoldUpMplier,
        tmnxPppoePlcyDisableAcCookies,
        tmnxPppoePlcyPadoDelay,
        tmnxPppoePlcyMaxSessionsPerMac,
        tmnxPppoePlcyReplyOnPadt,
        tmnxPppoePlcyPppAuthentication,
        tmnxPppoePlcyPppInitialDelay,
        tmnxPppoePlcyPppOptionTblLstChg,
        tmnxPppoePlcyOptionRowStatus,
        tmnxPppoePlcyOptionLstMgmtChange,
        tmnxPppoePlcyOptionType,
        tmnxPppoePlcyOptionValue,
        tmnxPppoeIesIfInfoTableLastChg,
        tmnxPppoeIesIfLastChg,
        tmnxPppoeIesIfDescription,
        tmnxPppoeIesIfAdminState,
        tmnxPppoeIesIfPolicy,
        tmnxPppoeIesIfSessionLimit,
        tmnxPppoeIesIfSapSessionLimit,
        tmnxPppoeIesIfPapChapUserDb,
        tmnxPppoeSapRxPadi,
        tmnxPppoeSapRxPadr,
        tmnxPppoeSapRxPadt,
        tmnxPppoeSapRxSession,
        tmnxPppoeSapRxInvalidVersion,
        tmnxPppoeSapRxInvalidType,
        tmnxPppoeSapRxInvalidCode,
        tmnxPppoeSapRxInvalidSession,
        tmnxPppoeSapRxInvalidLen,
        tmnxPppoeSapRxInvalidTags,
        tmnxPppoeSapRxInvalidAcCookie,
        tmnxPppoeSapRxDropped,
        tmnxPppoeSapTxPado,
        tmnxPppoeSapTxPads,
        tmnxPppoeSapTxPadt,
        tmnxPppoeSapTxSession,
        tmnxPppoeSessionUpTime,
        tmnxPppoeSessionLcpState,
        tmnxPppoeSessionIpcpState,
        tmnxPppoeSessionPppMtu,
        tmnxPppoeSessionPppAuthProtocol,
        tmnxPppoeSessionPppUserName,
        tmnxPppoeSessionSubIdent,
        tmnxPppoeSessionOriginSubIdent,
        tmnxPppoeSessionSubProfString,
        tmnxPppoeSessionSlaProfString,
        tmnxPppoeSessionAncpString,
        tmnxPppoeSessionInterDestId,
        tmnxPppoeSessionOriginStrings,
        tmnxPppoeSessionSessionTimeout,
        tmnxPppoeSessionIpAddrType,
        tmnxPppoeSessionIpAddr,
        tmnxPppoeSessionPrimaryDnsType,
        tmnxPppoeSessionPrimaryDns,
        tmnxPppoeSessionSecondryDnsType,
        tmnxPppoeSessionSecondryDns,
        tmnxPppoeSessionPrimaryNbnsType,
        tmnxPppoeSessionPrimaryNbns,
        tmnxPppoeSessionSecondryNbnsType,
        tmnxPppoeSessionSecondryNbns,
        tmnxPppoeSessionOriginIpcpInfo,
        tmnxPppoeSessionCircuitId,
        tmnxPppoeSessionRemoteId,
        tmnxPppoeSessionAddressPool,
        tmnxPppoeSessionModSubIdent,
        tmnxPppoeSessionModSubProfStr,
        tmnxPppoeSessionModSlaProfStr,
        tmnxPppoeSessionModAncpStr,
        tmnxPppoeSessionModInterDestId,
        tmnxPppoeSessionEvaluateState,
        tmnxPppoeSessionRxUnknownProto,
        tmnxPppoeSessionRxLcpConfReq,
        tmnxPppoeSessionRxLcpConfAck,
        tmnxPppoeSessionRxLcpConfNak,
        tmnxPppoeSessionRxLcpConfRej,
        tmnxPppoeSessionRxLcpTermReq,
        tmnxPppoeSessionRxLcpTermAck,
        tmnxPppoeSessionRxLcpCodeRej,
        tmnxPppoeSessionRxLcpEchoReq,
        tmnxPppoeSessionRxLcpEchoRep,
        tmnxPppoeSessionRxLcpProtRej,
        tmnxPppoeSessionRxLcpDiscReq,
        tmnxPppoeSessionTxLcpConfReq,
        tmnxPppoeSessionTxLcpConfAck,
        tmnxPppoeSessionTxLcpConfNak,
        tmnxPppoeSessionTxLcpConfRej,
        tmnxPppoeSessionTxLcpTermReq,
        tmnxPppoeSessionTxLcpTermAck,
        tmnxPppoeSessionTxLcpCodeRej,
        tmnxPppoeSessionTxLcpEchoReq,
        tmnxPppoeSessionTxLcpEchoRep,
        tmnxPppoeSessionTxLcpProtRej,
        tmnxPppoeSessionTxLcpDiscReq,
        tmnxPppoeSessionRxPapAuthReq,
        tmnxPppoeSessionTxPapAuthAck,
        tmnxPppoeSessionTxPapAuthNak,
        tmnxPppoeSessionRxChapResponse,
        tmnxPppoeSessionTxChapChallenge,
        tmnxPppoeSessionTxChapSuccess,
        tmnxPppoeSessionTxChapFailure,
        tmnxPppoeSessionRxIpcpConfReq,
        tmnxPppoeSessionRxIpcpConfAck,
        tmnxPppoeSessionRxIpcpConfNak,
        tmnxPppoeSessionRxIpcpConfRej,
        tmnxPppoeSessionRxIpcpTermReq,
        tmnxPppoeSessionRxIpcpTermAck,
        tmnxPppoeSessionRxIpcpCodeRej,
        tmnxPppoeSessionTxIpcpConfReq,
        tmnxPppoeSessionTxIpcpConfAck,
        tmnxPppoeSessionTxIpcpConfNak,
        tmnxPppoeSessionTxIpcpConfRej,
        tmnxPppoeSessionTxIpcpTermReq,
        tmnxPppoeSessionTxIpcpTermAck,
        tmnxPppoeSessionTxIpcpCodeRej
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE on Nokia SROS series systems 6.1
         release."
    ::= { tmnxPppoeGroups 6 }

tmnxPPPoEV7v0Group               OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyTableLastChanged,
        tmnxPppoePlcyRowStatus,
        tmnxPppoePlcyLastMgmtChange,
        tmnxPppoePlcyDescription,
        tmnxPppoePlcyPppMtu,
        tmnxPppoePlcyLcpKaInterval,
        tmnxPppoePlcyLcpKaHoldUpMplier,
        tmnxPppoePlcyDisableAcCookies,
        tmnxPppoePlcyPadoDelay,
        tmnxPppoePlcyMaxSessionsPerMac,
        tmnxPppoePlcyReplyOnPadt,
        tmnxPppoePlcyPppAuthentication,
        tmnxPppoePlcyPppInitialDelay,
        tmnxPppoePlcyPppMinChapChallenge,
        tmnxPppoePlcyPppMaxChapChallenge,
        tmnxPppoePlcyPppOptionTblLstChg,
        tmnxPppoePlcyOptionRowStatus,
        tmnxPppoePlcyOptionLstMgmtChange,
        tmnxPppoePlcyOptionType,
        tmnxPppoePlcyOptionValue,
        tmnxPppoeIesIfInfoTableLastChg,
        tmnxPppoeIesIfLastChg,
        tmnxPppoeIesIfDescription,
        tmnxPppoeIesIfAdminState,
        tmnxPppoeIesIfPolicy,
        tmnxPppoeIesIfSessionLimit,
        tmnxPppoeIesIfSapSessionLimit,
        tmnxPppoeIesIfUserDb,
        tmnxPppoeIesIfDhcpcCcagOriginSap,
        tmnxPppoeSapRxPadi,
        tmnxPppoeSapRxPadr,
        tmnxPppoeSapRxPadt,
        tmnxPppoeSapRxSession,
        tmnxPppoeSapRxInvalidVersion,
        tmnxPppoeSapRxInvalidType,
        tmnxPppoeSapRxInvalidCode,
        tmnxPppoeSapRxInvalidSession,
        tmnxPppoeSapRxInvalidLen,
        tmnxPppoeSapRxInvalidTags,
        tmnxPppoeSapRxInvalidAcCookie,
        tmnxPppoeSapRxDropped,
        tmnxPppoeSapTxPado,
        tmnxPppoeSapTxPads,
        tmnxPppoeSapTxPadt,
        tmnxPppoeSapTxSession,
        tmnxPppoeSessionUpTime,
        tmnxPppoeSessionLcpState,
        tmnxPppoeSessionIpcpState,
        tmnxPppoeSessionPppMtu,
        tmnxPppoeSessionPppAuthProtocol,
        tmnxPppoeSessionPppUserName,
        tmnxPppoeSessionSubIdent,
        tmnxPppoeSessionOriginSubIdent,
        tmnxPppoeSessionSubProfString,
        tmnxPppoeSessionSlaProfString,
        tmnxPppoeSessionAncpString,
        tmnxPppoeSessionInterDestId,
        tmnxPppoeSessionOriginStrings,
        tmnxPppoeSessionSessionTimeout,
        tmnxPppoeSessionIpAddrType,
        tmnxPppoeSessionIpAddr,
        tmnxPppoeSessionPrimaryDnsType,
        tmnxPppoeSessionPrimaryDns,
        tmnxPppoeSessionSecondryDnsType,
        tmnxPppoeSessionSecondryDns,
        tmnxPppoeSessionPrimaryNbnsType,
        tmnxPppoeSessionPrimaryNbns,
        tmnxPppoeSessionSecondryNbnsType,
        tmnxPppoeSessionSecondryNbns,
        tmnxPppoeSessionOriginIpcpInfo,
        tmnxPppoeSessionCircuitId,
        tmnxPppoeSessionRemoteId,
        tmnxPppoeSessionAddressPool,
        tmnxPppoeSessionType,
        tmnxPppoeSessionRetailerSvcId,
        tmnxPppoeSessionRetailerIf,
        tmnxPppoeSessionL2tpVrtrId,
        tmnxPppoeSessionL2tpConnectionId,
        tmnxPppoeSessionServiceName,
        tmnxPppoeSessionCategoryMapName,
        tmnxPppoeSessionRadiusClassAttr,
        tmnxPppoeSessionRadiusUserName,
        tmnxPppoeSessionModSubIdent,
        tmnxPppoeSessionModSubProfStr,
        tmnxPppoeSessionModSlaProfStr,
        tmnxPppoeSessionModAncpStr,
        tmnxPppoeSessionModInterDestId,
        tmnxPppoeSessionEvaluateState,
        tmnxPppoeSessionRxUnknownProto,
        tmnxPppoeSessionRxLcpConfReq,
        tmnxPppoeSessionRxLcpConfAck,
        tmnxPppoeSessionRxLcpConfNak,
        tmnxPppoeSessionRxLcpConfRej,
        tmnxPppoeSessionRxLcpTermReq,
        tmnxPppoeSessionRxLcpTermAck,
        tmnxPppoeSessionRxLcpCodeRej,
        tmnxPppoeSessionRxLcpEchoReq,
        tmnxPppoeSessionRxLcpEchoRep,
        tmnxPppoeSessionRxLcpProtRej,
        tmnxPppoeSessionRxLcpDiscReq,
        tmnxPppoeSessionTxLcpConfReq,
        tmnxPppoeSessionTxLcpConfAck,
        tmnxPppoeSessionTxLcpConfNak,
        tmnxPppoeSessionTxLcpConfRej,
        tmnxPppoeSessionTxLcpTermReq,
        tmnxPppoeSessionTxLcpTermAck,
        tmnxPppoeSessionTxLcpCodeRej,
        tmnxPppoeSessionTxLcpEchoReq,
        tmnxPppoeSessionTxLcpEchoRep,
        tmnxPppoeSessionTxLcpProtRej,
        tmnxPppoeSessionTxLcpDiscReq,
        tmnxPppoeSessionRxPapAuthReq,
        tmnxPppoeSessionTxPapAuthAck,
        tmnxPppoeSessionTxPapAuthNak,
        tmnxPppoeSessionRxChapResponse,
        tmnxPppoeSessionTxChapChallenge,
        tmnxPppoeSessionTxChapSuccess,
        tmnxPppoeSessionTxChapFailure,
        tmnxPppoeSessionRxIpcpConfReq,
        tmnxPppoeSessionRxIpcpConfAck,
        tmnxPppoeSessionRxIpcpConfNak,
        tmnxPppoeSessionRxIpcpConfRej,
        tmnxPppoeSessionRxIpcpTermReq,
        tmnxPppoeSessionRxIpcpTermAck,
        tmnxPppoeSessionRxIpcpCodeRej,
        tmnxPppoeSessionTxIpcpConfReq,
        tmnxPppoeSessionTxIpcpConfAck,
        tmnxPppoeSessionTxIpcpConfNak,
        tmnxPppoeSessionTxIpcpConfRej,
        tmnxPppoeSessionTxIpcpTermReq,
        tmnxPppoeSessionTxIpcpTermAck,
        tmnxPppoeSessionTxIpcpCodeRej
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE on Nokia SROS series systems 7.0
         release."
    ::= { tmnxPppoeGroups 7 }

tmnxPPPoESessionBGPGroup         OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeSessionBgpPrngPlcyName,
        tmnxPppoeSessionBgpAuthKeyChain,
        tmnxPppoeSessionBgpMD5AuthKey,
        tmnxPppoeSessionBgpImportPolicy,
        tmnxPppoeSessionBgpExportPolicy,
        tmnxPppoeSessionBgpPeerAS,
        tmnxPppoeSessionBgpPeeringStatus
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE BGP peering on Nokia SROS series
         systems."
    ::= { tmnxPppoeGroups 8 }

tmnxPPPoEV8v0Group               OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyTableLastChanged,
        tmnxPppoePlcyRowStatus,
        tmnxPppoePlcyLastMgmtChange,
        tmnxPppoePlcyDescription,
        tmnxPppoePlcyPppMtu,
        tmnxPppoePlcyLcpKaInterval,
        tmnxPppoePlcyLcpKaHoldUpMplier,
        tmnxPppoePlcyDisableAcCookies,
        tmnxPppoePlcyPadoDelay,
        tmnxPppoePlcyMaxSessionsPerMac,
        tmnxPppoePlcyReplyOnPadt,
        tmnxPppoePlcyPppAuthentication,
        tmnxPppoePlcyPppInitialDelay,
        tmnxPppoePlcyPppMinChapChallenge,
        tmnxPppoePlcyPppMaxChapChallenge,
        tmnxPppoePlcyPppOptionTblLstChg,
        tmnxPppoePlcyOptionRowStatus,
        tmnxPppoePlcyOptionLstMgmtChange,
        tmnxPppoePlcyOptionType,
        tmnxPppoePlcyOptionValue,
        tmnxPppoeIesIfInfoTableLastChg,
        tmnxPppoeIesIfLastChg,
        tmnxPppoeIesIfDescription,
        tmnxPppoeIesIfAdminState,
        tmnxPppoeIesIfPolicy,
        tmnxPppoeIesIfSessionLimit,
        tmnxPppoeIesIfSapSessionLimit,
        tmnxPppoeIesIfUserDb,
        tmnxPppoeIesIfDhcpcCcagOriginSap,
        tmnxPppoeIesIfAntiSpoofing,
        tmnxPppoeSapRxPadi,
        tmnxPppoeSapRxPadr,
        tmnxPppoeSapRxPadt,
        tmnxPppoeSapRxSession,
        tmnxPppoeSapRxInvalidVersion,
        tmnxPppoeSapRxInvalidType,
        tmnxPppoeSapRxInvalidCode,
        tmnxPppoeSapRxInvalidSession,
        tmnxPppoeSapRxInvalidLen,
        tmnxPppoeSapRxInvalidTags,
        tmnxPppoeSapRxInvalidAcCookie,
        tmnxPppoeSapRxDropped,
        tmnxPppoeSapTxPado,
        tmnxPppoeSapTxPads,
        tmnxPppoeSapTxPadt,
        tmnxPppoeSapTxSession,
        tmnxPppoeSessionUpTime,
        tmnxPppoeSessionLcpState,
        tmnxPppoeSessionIpcpState,
        tmnxPppoeSessionPppMtu,
        tmnxPppoeSessionPppAuthProtocol,
        tmnxPppoeSessionPppUserName,
        tmnxPppoeSessionSubIdent,
        tmnxPppoeSessionOriginSubIdent,
        tmnxPppoeSessionSubProfString,
        tmnxPppoeSessionSlaProfString,
        tmnxPppoeSessionAncpString,
        tmnxPppoeSessionInterDestId,
        tmnxPppoeSessionOriginStrings,
        tmnxPppoeSessionSessionTimeout,
        tmnxPppoeSessionIpAddrType,
        tmnxPppoeSessionIpAddr,
        tmnxPppoeSessionPrimaryDnsType,
        tmnxPppoeSessionPrimaryDns,
        tmnxPppoeSessionSecondryDnsType,
        tmnxPppoeSessionSecondryDns,
        tmnxPppoeSessionPrimaryNbnsType,
        tmnxPppoeSessionPrimaryNbns,
        tmnxPppoeSessionSecondryNbnsType,
        tmnxPppoeSessionSecondryNbns,
        tmnxPppoeSessionOriginIpcpInfo,
        tmnxPppoeSessionCircuitId,
        tmnxPppoeSessionRemoteId,
        tmnxPppoeSessionAddressPool,
        tmnxPppoeSessionType,
        tmnxPppoeSessionRetailerSvcId,
        tmnxPppoeSessionRetailerIf,
        tmnxPppoeSessionL2tpVrtrId,
        tmnxPppoeSessionL2tpConnectionId,
        tmnxPppoeSessionServiceName,
        tmnxPppoeSessionCategoryMapName,
        tmnxPppoeSessionRadiusClassAttr,
        tmnxPppoeSessionRadiusUserName,
        tmnxPppoeSessionIpv6cpState,
        tmnxPppoeSessionInterfaceId,
        tmnxPppoeSessionOriginIpv6cpInfo,
        tmnxPppoeSessionIpv6DnsType,
        tmnxPppoeSessionIpv6Dns1,
        tmnxPppoeSessionIpv6Dns2,
        tmnxPppoeSessionIpv6DelPfxType,
        tmnxPppoeSessionIpv6DelPfxLen,
        tmnxPppoeSessionIpv6DelPfx,
        tmnxPppoeSessionIpv6PrefixType,
        tmnxPppoeSessionIpv6PrefixLen,
        tmnxPppoeSessionIpv6Prefix,
        tmnxPppoeSessionModSubIdent,
        tmnxPppoeSessionModSubProfStr,
        tmnxPppoeSessionModSlaProfStr,
        tmnxPppoeSessionModAncpStr,
        tmnxPppoeSessionModInterDestId,
        tmnxPppoeSessionEvaluateState,
        tmnxPppoeSessionRxUnknownProto,
        tmnxPppoeSessionRxLcpConfReq,
        tmnxPppoeSessionRxLcpConfAck,
        tmnxPppoeSessionRxLcpConfNak,
        tmnxPppoeSessionRxLcpConfRej,
        tmnxPppoeSessionRxLcpTermReq,
        tmnxPppoeSessionRxLcpTermAck,
        tmnxPppoeSessionRxLcpCodeRej,
        tmnxPppoeSessionRxLcpEchoReq,
        tmnxPppoeSessionRxLcpEchoRep,
        tmnxPppoeSessionRxLcpProtRej,
        tmnxPppoeSessionRxLcpDiscReq,
        tmnxPppoeSessionTxLcpConfReq,
        tmnxPppoeSessionTxLcpConfAck,
        tmnxPppoeSessionTxLcpConfNak,
        tmnxPppoeSessionTxLcpConfRej,
        tmnxPppoeSessionTxLcpTermReq,
        tmnxPppoeSessionTxLcpTermAck,
        tmnxPppoeSessionTxLcpCodeRej,
        tmnxPppoeSessionTxLcpEchoReq,
        tmnxPppoeSessionTxLcpEchoRep,
        tmnxPppoeSessionTxLcpProtRej,
        tmnxPppoeSessionTxLcpDiscReq,
        tmnxPppoeSessionRxPapAuthReq,
        tmnxPppoeSessionTxPapAuthAck,
        tmnxPppoeSessionTxPapAuthNak,
        tmnxPppoeSessionRxChapResponse,
        tmnxPppoeSessionTxChapChallenge,
        tmnxPppoeSessionTxChapSuccess,
        tmnxPppoeSessionTxChapFailure,
        tmnxPppoeSessionRxIpcpConfReq,
        tmnxPppoeSessionRxIpcpConfAck,
        tmnxPppoeSessionRxIpcpConfNak,
        tmnxPppoeSessionRxIpcpConfRej,
        tmnxPppoeSessionRxIpcpTermReq,
        tmnxPppoeSessionRxIpcpTermAck,
        tmnxPppoeSessionRxIpcpCodeRej,
        tmnxPppoeSessionTxIpcpConfReq,
        tmnxPppoeSessionTxIpcpConfAck,
        tmnxPppoeSessionTxIpcpConfNak,
        tmnxPppoeSessionTxIpcpConfRej,
        tmnxPppoeSessionTxIpcpTermReq,
        tmnxPppoeSessionTxIpcpTermAck,
        tmnxPppoeSessionTxIpcpCodeRej,
        tmnxPppoeSessionRxIpv6cpConfReq,
        tmnxPppoeSessionRxIpv6cpConfAck,
        tmnxPppoeSessionRxIpv6cpConfNak,
        tmnxPppoeSessionRxIpv6cpConfRej,
        tmnxPppoeSessionRxIpv6cpTermReq,
        tmnxPppoeSessionRxIpv6cpTermAck,
        tmnxPppoeSessionRxIpv6cpCodeRej,
        tmnxPppoeSessionTxIpv6cpConfReq,
        tmnxPppoeSessionTxIpv6cpConfAck,
        tmnxPppoeSessionTxIpv6cpConfNak,
        tmnxPppoeSessionTxIpv6cpConfRej,
        tmnxPppoeSessionTxIpv6cpTermReq,
        tmnxPppoeSessionTxIpv6cpTermAck,
        tmnxPppoeSessionTxIpv6cpCodeRej,
        tmnxPppoeSessionOvrPIR,
        tmnxPppoeSessionOvrCIR,
        tmnxPppoeSessionOvrCBS,
        tmnxPppoeSessionOvrMBS,
        tmnxPppoeSessionAleDatalink,
        tmnxPppoeSessionAleEncaps1,
        tmnxPppoeSessionAleEncaps2
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE on Nokia SROS series systems 8.0
         release."
    ::= { tmnxPppoeGroups 10 }

tmnxPPPoEV8v0NotifyGroup         NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxPppoeSessionFailure,
        tmnxPppoeNcpFailure
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of notifications generated by the PPPoE feature on Nokia
         SROS series systems 8.0 release."
    ::= { tmnxPppoeGroups 11 }

tmnxPPPoEV8v0NotifyObjsGroup     OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeSessionFailureReason,
        tmnxPppoeNcpFailureProtocol,
        tmnxPppoeNcpFailureReason
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of PPPoE notification
         objects on Nokia SROS series systems 8.0 release."
    ::= { tmnxPppoeGroups 12 }

tmnxPPPoEV9v0Group               OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyPppIpcpSubnetNeg,
        tmnxPppoePlcyPadoAcName,
        tmnxPppoePlcyPppMtuForceGt1492,
        tmnxPppoePlcyUniqueSessIdsPerSap
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE added in Nokia SROS series
         systems 9.0 release."
    ::= { tmnxPppoeGroups 15 }

tmnxPPPV9v0Group                 OBJECT-GROUP
    OBJECTS     {
        tmnxPppIesIfTableLastChg,
        tmnxPppIesIfLastChg,
        tmnxPppIesIfDescription,
        tmnxPppIesIfAdminState,
        tmnxPppIesIfPolicy,
        tmnxPppIesIfSessionLimit,
        tmnxPppIesIfUserDb,
        tmnxPppoeSessionSubPppIndex
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPP added in Nokia SROS series systems
         9.0 release."
    ::= { tmnxPppoeGroups 16 }

tmnxPPPMlpppGroup                OBJECT-GROUP
    OBJECTS     {
        tmnxMlpppBundleLocEpClass,
        tmnxMlpppBundleLocEpAddress,
        tmnxMlpppBundleRemEpClass,
        tmnxMlpppBundleRemEpAddress,
        tmnxMlpppBundleSubPppIndex,
        tmnxMlpppBundleMaxLinks,
        tmnxMlpppBundleActualLinks,
        tmnxMlpppBundleRemMrru,
        tmnxMlpppBundleLocMrru,
        tmnxMlpppBundleIndicators,
        tmnxMlpppBundleFragmentSize,
        tmnxMlpppBundleMaxDelayCfg,
        tmnxMlpppBundleMaxDelay,
        tmnxMlpppBundleReassemblyTo,
        tmnxMlpppBundleEgressRate,
        tmnxPppPlcyMlpppTableLastCh,
        tmnxMlpppLinkRemMrru,
        tmnxPppPlcyMlpppLastCh,
        tmnxPppPlcyMlpppAcceptMrru,
        tmnxPppPlcyMlpppEpClass,
        tmnxPppPlcyMlpppEpIpv4Address,
        tmnxPppPlcyMlpppEpMacAddress,
        tmnxPppPlcyMlpppShortSeqNumberRx
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting subscriber MLPPP in Nokia SROS series
         systems."
    ::= { tmnxPppoeGroups 20 }

tmnxPPPRejectDisabledNcp         OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyRejectDisabledNcp
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of PPP Policy reject
         disabled NCP's options in Nokia SROS series systems."
    ::= { tmnxPppoeGroups 21 }

tmnxPPPoEV10v0NotifyObjsGroup    OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeSessionFailureReason,
        tmnxPppoeNcpFailureProtocol,
        tmnxPppoeNcpFailureReason,
        tmnxPppoeNotifyDescription
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of PPPoE notification
         objects on Nokia SROS series systems 10.0 release."
    ::= { tmnxPppoeGroups 22 }

tmnxPPPoEV10v0NotifyGroup        NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxPppoeSessionFailure,
        tmnxPppoeNcpFailure,
        tmnxMlpppBundleIndicatorsChange
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of notifications generated by the PPPoE feature on Nokia
         SROS series systems 10.0 release."
    ::= { tmnxPppoeGroups 23 }

tmnxPPPLcpIgnoreMagic            OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyLcpIgnoreMagic
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of PPP Policy
         lcp-ignore-magic-num options in Nokia SROS series systems."
    ::= { tmnxPppoeGroups 25 }

tmnxPPPoEV11v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeSapRxInvalidMac,
        tmnxPppoePlcySessionTimeout,
        tmnxPppoeIesIfDhcpcInclOptString
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE added in Nokia SROS series
         systems 11.0 release."
    ::= { tmnxPppoeGroups 26 }

tmnxPPPPlcyAllowSameCidGroup     OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyAllowSameCidForDhcp
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of multiple PPP sessions
         with the same MAC address in wholesale/retail, in Nokia SROS series
         systems."
    ::= { tmnxPppoeGroups 27 }

tmnxPPPoEV12v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeSapRxInvalidMac,
        tmnxPppoePlcySessionTimeout,
        tmnxPppoePlcyReestablishSession
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE (added) in Nokia SROS series
         systems 12.0 release."
    ::= { tmnxPppoeGroups 30 }

tmnxPPPoEDefaultUsernameGroup    OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyDefaultUserName,
        tmnxPppoePlcyDefaultPapPassword
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE default username configuration."
    ::= { tmnxPppoeGroups 31 }

tmnxPPPoEV14v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeIesIfPythonPolicy
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE (added) in Nokia SROS series
         systems 14.0 release."
    ::= { tmnxPppoeGroups 32 }

tmnxPPPoEV15v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeClntPlcyTableLastChg,
        tmnxPppoeClntPlcyRowStatus,
        tmnxPppoeClntPlcyLastMgmtChg,
        tmnxPppoeClntPlcyDescription,
        tmnxPppoeClntPlcyKaInterval,
        tmnxPppoeClntPlcyKaHoldUpM,
        tmnxPppoeClntPlcyMru,
        tmnxPppoeClntPlcyMtu,
        tmnxPppoeClntPlcyStack,
        tmnxPppoeClntPlcyRestartInit,
        tmnxPppoeClntPlcyRestartMax,
        tmnxPppoeClntPlcyPythonPlcy,
        tmnxPppoeClntSvcId,
        tmnxPppoeClntMac,
        tmnxPppoeClntUpTime,
        tmnxPppoeClntPolicy,
        tmnxPppoeClntServiceName,
        tmnxPppoeClntSessionId,
        tmnxPppoeClntAcMac,
        tmnxPppoeClntAcName,
        tmnxPppoeClntLcpState,
        tmnxPppoeClntIpcpState,
        tmnxPppoeClntIpv6cpState,
        tmnxPppoeClntLocalMagicNum,
        tmnxPppoeClntRemoteMagicNum,
        tmnxPppoeClntRemoteMru,
        tmnxPppoeClntPppUserName,
        tmnxPppoeClntPppAuthProtocol,
        tmnxPppoeClntIpcpIpAddrType,
        tmnxPppoeClntIpcpIpAddr,
        tmnxPppoeClntIpcpPriDnsType,
        tmnxPppoeClntIpcpPriDns,
        tmnxPppoeClntIpcpSecDnsType,
        tmnxPppoeClntIpcpSecDns,
        tmnxPppoeClntIpcpPriNbnsType,
        tmnxPppoeClntIpcpPriNbns,
        tmnxPppoeClntIpcpSecNbnsType,
        tmnxPppoeClntIpcpSecNbns,
        tmnxPppoeClntIpv6cpInterfaceId,
        tmnxPppoeClntSlaacPrefixType,
        tmnxPppoeClntSlaacPrefix,
        tmnxPppoeClntSlaacPrefixLen,
        tmnxPppoeClntSlaacPrefixTimeout,
        tmnxPppoeClntSlaacPriDnsType,
        tmnxPppoeClntSlaacPriDns,
        tmnxPppoeClntSlaacSecDnsType,
        tmnxPppoeClntSlaacSecDns,
        tmnxPppoeClntTxPadi,
        tmnxPppoeClntTxPadr,
        tmnxPppoeClntTxPadt,
        tmnxPppoeClntTxSession,
        tmnxPppoeClntTxLcpEchoReq,
        tmnxPppoeClntTxLcpEchoRep,
        tmnxPppoeClntTxV6Rs,
        tmnxPppoeClntTxV6DhcpInfo,
        tmnxPppoeClntRxPado,
        tmnxPppoeClntRxPads,
        tmnxPppoeClntRxPadt,
        tmnxPppoeClntRxSession,
        tmnxPppoeClntRxLcpEchoReq,
        tmnxPppoeClntRxLcpEchoRep,
        tmnxPppoeClntRxV6Ra,
        tmnxPppoeClntRxV6DhcpReply,
        tmnxPppoeClntRxDropped,
        tmnxPppoeClntMdaRxErr,
        tmnxPppoeClntMdaRxErrNotPppoe,
        tmnxPppoeClntMdaRxErrEchoMagic,
        tmnxPppoeClntMdaRxErrNoSession,
        tmnxPppoeClntMdaRxDiscovery,
        tmnxPppoeClntMdaRxPppControl,
        tmnxPppoeClntMdaRxEchoRequest,
        tmnxPppoeClntMdaRxEchoReply,
        tmnxPppoeClntMdaTxEchoRequest,
        tmnxPppoeClntMdaTxEchoReply
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE added in Nokia SROS series
         systems 15.0 release."
    ::= { tmnxPppoeGroups 33 }

tmnxPPPoEV15v0NotifyObjsGroup    OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeLacSteeringFailure,
        tmnxPppoeLacSteeringProfile,
        tmnxPppoeLacSteeringSession,
        tmnxPppoeClntIdent
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of PPPoE notification
         objects on Nokia SROS series systems 15.0 release."
    ::= { tmnxPppoeGroups 34 }

tmnxPPPoEV15v0NotifyGroup        NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxPppoeLacSteeringActive,
        tmnxPppoeLacSteeringStopped,
        tmnxPppoeLacSteeringFailed,
        tmnxPppoeClientSetupFailure,
        tmnxPppoeClientEchoTimeout,
        tmnxPppoeClientNcpFailure
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications generated by the PPPoE feature on Nokia
         SROS series systems 15.0 release."
    ::= { tmnxPppoeGroups 35 }

tmnxPPPoEV19v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyTableLastChanged,
        tmnxPppoePlcyRowStatus,
        tmnxPppoePlcyLastMgmtChange,
        tmnxPppoePlcyDescription,
        tmnxPppoePlcyPppMtu,
        tmnxPppoePlcyLcpKaInterval,
        tmnxPppoePlcyLcpKaHoldUpMplier,
        tmnxPppoePlcyDisableAcCookies,
        tmnxPppoePlcyPadoDelay,
        tmnxPppoePlcyMaxSessionsPerMac,
        tmnxPppoePlcyReplyOnPadt,
        tmnxPppoePlcyPppAuthentication,
        tmnxPppoePlcyPppInitialDelay,
        tmnxPppoePlcyPppMinChapChallenge,
        tmnxPppoePlcyPppMaxChapChallenge,
        tmnxPppoePlcyPppOptionTblLstChg,
        tmnxPppoePlcyOptionRowStatus,
        tmnxPppoePlcyOptionLstMgmtChange,
        tmnxPppoePlcyOptionType,
        tmnxPppoePlcyOptionValue,
        tmnxPppoeIesIfInfoTableLastChg,
        tmnxPppoeIesIfLastChg,
        tmnxPppoeIesIfDescription,
        tmnxPppoeIesIfAdminState,
        tmnxPppoeIesIfPolicy,
        tmnxPppoeIesIfSessionLimit,
        tmnxPppoeIesIfSapSessionLimit,
        tmnxPppoeIesIfUserDb,
        tmnxPppoeIesIfAntiSpoofing,
        tmnxPppoeSapRxPadi,
        tmnxPppoeSapRxPadr,
        tmnxPppoeSapRxPadt,
        tmnxPppoeSapRxSession,
        tmnxPppoeSapRxInvalidVersion,
        tmnxPppoeSapRxInvalidType,
        tmnxPppoeSapRxInvalidCode,
        tmnxPppoeSapRxInvalidSession,
        tmnxPppoeSapRxInvalidLen,
        tmnxPppoeSapRxInvalidTags,
        tmnxPppoeSapRxInvalidAcCookie,
        tmnxPppoeSapRxDropped,
        tmnxPppoeSapTxPado,
        tmnxPppoeSapTxPads,
        tmnxPppoeSapTxPadt,
        tmnxPppoeSapTxSession,
        tmnxPppoeSessionUpTime,
        tmnxPppoeSessionLcpState,
        tmnxPppoeSessionIpcpState,
        tmnxPppoeSessionPppMtu,
        tmnxPppoeSessionPppAuthProtocol,
        tmnxPppoeSessionPppUserName,
        tmnxPppoeSessionSubIdent,
        tmnxPppoeSessionOriginSubIdent,
        tmnxPppoeSessionSubProfString,
        tmnxPppoeSessionSlaProfString,
        tmnxPppoeSessionAncpString,
        tmnxPppoeSessionInterDestId,
        tmnxPppoeSessionOriginStrings,
        tmnxPppoeSessionSessionTimeout,
        tmnxPppoeSessionIpAddrType,
        tmnxPppoeSessionIpAddr,
        tmnxPppoeSessionPrimaryDnsType,
        tmnxPppoeSessionPrimaryDns,
        tmnxPppoeSessionSecondryDnsType,
        tmnxPppoeSessionSecondryDns,
        tmnxPppoeSessionPrimaryNbnsType,
        tmnxPppoeSessionPrimaryNbns,
        tmnxPppoeSessionSecondryNbnsType,
        tmnxPppoeSessionSecondryNbns,
        tmnxPppoeSessionOriginIpcpInfo,
        tmnxPppoeSessionCircuitId,
        tmnxPppoeSessionRemoteId,
        tmnxPppoeSessionAddressPool,
        tmnxPppoeSessionType,
        tmnxPppoeSessionRetailerSvcId,
        tmnxPppoeSessionRetailerIf,
        tmnxPppoeSessionL2tpVrtrId,
        tmnxPppoeSessionL2tpConnectionId,
        tmnxPppoeSessionServiceName,
        tmnxPppoeSessionCategoryMapName,
        tmnxPppoeSessionRadiusClassAttr,
        tmnxPppoeSessionRadiusUserName,
        tmnxPppoeSessionIpv6cpState,
        tmnxPppoeSessionInterfaceId,
        tmnxPppoeSessionOriginIpv6cpInfo,
        tmnxPppoeSessionIpv6DnsType,
        tmnxPppoeSessionIpv6Dns1,
        tmnxPppoeSessionIpv6Dns2,
        tmnxPppoeSessionIpv6DelPfxType,
        tmnxPppoeSessionIpv6DelPfxLen,
        tmnxPppoeSessionIpv6DelPfx,
        tmnxPppoeSessionIpv6PrefixType,
        tmnxPppoeSessionIpv6PrefixLen,
        tmnxPppoeSessionIpv6Prefix,
        tmnxPppoeSessionModSubIdent,
        tmnxPppoeSessionModSubProfStr,
        tmnxPppoeSessionModSlaProfStr,
        tmnxPppoeSessionModAncpStr,
        tmnxPppoeSessionModInterDestId,
        tmnxPppoeSessionEvaluateState,
        tmnxPppoeSessionRxUnknownProto,
        tmnxPppoeSessionRxLcpConfReq,
        tmnxPppoeSessionRxLcpConfAck,
        tmnxPppoeSessionRxLcpConfNak,
        tmnxPppoeSessionRxLcpConfRej,
        tmnxPppoeSessionRxLcpTermReq,
        tmnxPppoeSessionRxLcpTermAck,
        tmnxPppoeSessionRxLcpCodeRej,
        tmnxPppoeSessionRxLcpEchoReq,
        tmnxPppoeSessionRxLcpEchoRep,
        tmnxPppoeSessionRxLcpProtRej,
        tmnxPppoeSessionRxLcpDiscReq,
        tmnxPppoeSessionTxLcpConfReq,
        tmnxPppoeSessionTxLcpConfAck,
        tmnxPppoeSessionTxLcpConfNak,
        tmnxPppoeSessionTxLcpConfRej,
        tmnxPppoeSessionTxLcpTermReq,
        tmnxPppoeSessionTxLcpTermAck,
        tmnxPppoeSessionTxLcpCodeRej,
        tmnxPppoeSessionTxLcpEchoReq,
        tmnxPppoeSessionTxLcpEchoRep,
        tmnxPppoeSessionTxLcpProtRej,
        tmnxPppoeSessionTxLcpDiscReq,
        tmnxPppoeSessionRxPapAuthReq,
        tmnxPppoeSessionTxPapAuthAck,
        tmnxPppoeSessionTxPapAuthNak,
        tmnxPppoeSessionRxChapResponse,
        tmnxPppoeSessionTxChapChallenge,
        tmnxPppoeSessionTxChapSuccess,
        tmnxPppoeSessionTxChapFailure,
        tmnxPppoeSessionRxIpcpConfReq,
        tmnxPppoeSessionRxIpcpConfAck,
        tmnxPppoeSessionRxIpcpConfNak,
        tmnxPppoeSessionRxIpcpConfRej,
        tmnxPppoeSessionRxIpcpTermReq,
        tmnxPppoeSessionRxIpcpTermAck,
        tmnxPppoeSessionRxIpcpCodeRej,
        tmnxPppoeSessionTxIpcpConfReq,
        tmnxPppoeSessionTxIpcpConfAck,
        tmnxPppoeSessionTxIpcpConfNak,
        tmnxPppoeSessionTxIpcpConfRej,
        tmnxPppoeSessionTxIpcpTermReq,
        tmnxPppoeSessionTxIpcpTermAck,
        tmnxPppoeSessionTxIpcpCodeRej,
        tmnxPppoeSessionRxIpv6cpConfReq,
        tmnxPppoeSessionRxIpv6cpConfAck,
        tmnxPppoeSessionRxIpv6cpConfNak,
        tmnxPppoeSessionRxIpv6cpConfRej,
        tmnxPppoeSessionRxIpv6cpTermReq,
        tmnxPppoeSessionRxIpv6cpTermAck,
        tmnxPppoeSessionRxIpv6cpCodeRej,
        tmnxPppoeSessionTxIpv6cpConfReq,
        tmnxPppoeSessionTxIpv6cpConfAck,
        tmnxPppoeSessionTxIpv6cpConfNak,
        tmnxPppoeSessionTxIpv6cpConfRej,
        tmnxPppoeSessionTxIpv6cpTermReq,
        tmnxPppoeSessionTxIpv6cpTermAck,
        tmnxPppoeSessionTxIpv6cpCodeRej,
        tmnxPppoeSessionOvrPIR,
        tmnxPppoeSessionOvrCIR,
        tmnxPppoeSessionOvrCBS,
        tmnxPppoeSessionOvrMBS,
        tmnxPppoeSessionAleDatalink,
        tmnxPppoeSessionAleEncaps1,
        tmnxPppoeSessionAleEncaps2,
        tmnxPppoePlcyPppIpcpSubnetNeg,
        tmnxPppoePlcyPadoAcName,
        tmnxPppoePlcyPppMtuForceGt1492,
        tmnxPppoePlcyUniqueSessIdsPerSap,
        tmnxPppoePlcySidAllocation,
        tmnxPppIesIfTableLastChg,
        tmnxPppIesIfLastChg,
        tmnxPppIesIfDescription,
        tmnxPppIesIfAdminState,
        tmnxPppIesIfPolicy,
        tmnxPppIesIfSessionLimit,
        tmnxPppIesIfUserDb,
        tmnxPppoeSessionSubPppIndex,
        tmnxPppoePlcyRejectDisabledNcp,
        tmnxPppoePlcyLcpIgnoreMagic,
        tmnxPppoePlcyAllowSameCidForDhcp,
        tmnxPppoeSapRxInvalidMac,
        tmnxPppoePlcySessionTimeout,
        tmnxPppoeIesIfDhcpcInclOptString,
        tmnxPppoePlcyReestablishSession,
        tmnxPppoePlcyDefaultUserName,
        tmnxPppoePlcyDefaultPapPassword,
        tmnxPppoeIesIfPythonPolicy,
        tmnxPppoeClntPlcyTableLastChg,
        tmnxPppoeClntPlcyRowStatus,
        tmnxPppoeClntPlcyLastMgmtChg,
        tmnxPppoeClntPlcyDescription,
        tmnxPppoeClntPlcyKaInterval,
        tmnxPppoeClntPlcyKaHoldUpM,
        tmnxPppoeClntPlcyMru,
        tmnxPppoeClntPlcyMtu,
        tmnxPppoeClntPlcyStack,
        tmnxPppoeClntPlcyRestartInit,
        tmnxPppoeClntPlcyRestartMax,
        tmnxPppoeClntPlcyPythonPlcy,
        tmnxPppoeClntSvcId,
        tmnxPppoeClntMac,
        tmnxPppoeClntUpTime,
        tmnxPppoeClntPolicy,
        tmnxPppoeClntServiceName,
        tmnxPppoeClntSessionId,
        tmnxPppoeClntAcMac,
        tmnxPppoeClntAcName,
        tmnxPppoeClntLcpState,
        tmnxPppoeClntIpcpState,
        tmnxPppoeClntIpv6cpState,
        tmnxPppoeClntLocalMagicNum,
        tmnxPppoeClntRemoteMagicNum,
        tmnxPppoeClntRemoteMru,
        tmnxPppoeClntPppUserName,
        tmnxPppoeClntPppAuthProtocol,
        tmnxPppoeClntIpcpIpAddrType,
        tmnxPppoeClntIpcpIpAddr,
        tmnxPppoeClntIpcpPriDnsType,
        tmnxPppoeClntIpcpPriDns,
        tmnxPppoeClntIpcpSecDnsType,
        tmnxPppoeClntIpcpSecDns,
        tmnxPppoeClntIpcpPriNbnsType,
        tmnxPppoeClntIpcpPriNbns,
        tmnxPppoeClntIpcpSecNbnsType,
        tmnxPppoeClntIpcpSecNbns,
        tmnxPppoeClntIpv6cpInterfaceId,
        tmnxPppoeClntSlaacPrefixType,
        tmnxPppoeClntSlaacPrefix,
        tmnxPppoeClntSlaacPrefixLen,
        tmnxPppoeClntSlaacPrefixTimeout,
        tmnxPppoeClntSlaacPriDnsType,
        tmnxPppoeClntSlaacPriDns,
        tmnxPppoeClntSlaacSecDnsType,
        tmnxPppoeClntSlaacSecDns,
        tmnxPppoeClntTxPadi,
        tmnxPppoeClntTxPadr,
        tmnxPppoeClntTxPadt,
        tmnxPppoeClntTxSession,
        tmnxPppoeClntTxLcpEchoReq,
        tmnxPppoeClntTxLcpEchoRep,
        tmnxPppoeClntTxV6Rs,
        tmnxPppoeClntTxV6DhcpInfo,
        tmnxPppoeClntRxPado,
        tmnxPppoeClntRxPads,
        tmnxPppoeClntRxPadt,
        tmnxPppoeClntRxSession,
        tmnxPppoeClntRxLcpEchoReq,
        tmnxPppoeClntRxLcpEchoRep,
        tmnxPppoeClntRxV6Ra,
        tmnxPppoeClntRxV6DhcpReply,
        tmnxPppoeClntRxDropped,
        tmnxPppoeClntMdaRxErr,
        tmnxPppoeClntMdaRxErrNotPppoe,
        tmnxPppoeClntMdaRxErrEchoMagic,
        tmnxPppoeClntMdaRxErrNoSession,
        tmnxPppoeClntMdaRxDiscovery,
        tmnxPppoeClntMdaRxPppControl,
        tmnxPppoeClntMdaRxEchoRequest,
        tmnxPppoeClntMdaRxEchoReply,
        tmnxPppoeClntMdaTxEchoRequest,
        tmnxPppoeClntMdaTxEchoReply,
        tmnxPppoeIesIfDhcpcInclClientId,
        tmnxPppoeClntVappRxErr,
        tmnxPppoeClntVappRxErrNotPppoe,
        tmnxPppoeClntVappRxErrEchoMagic,
        tmnxPppoeClntVappRxErrNoSession,
        tmnxPppoeClntVappRxDiscovery,
        tmnxPppoeClntVappRxPppControl,
        tmnxPppoeClntVappRxEchoRequest,
        tmnxPppoeClntVappRxEchoReply,
        tmnxPppoeClntVappTxEchoRequest,
        tmnxPppoeClntVappTxEchoReply
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting PPPoE on Nokia SROS series systems
         19.0 release."
    ::= { tmnxPppoeGroups 36 }

tmnxPPPoEV20v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyTableLastChanged,
        tmnxPppoePlcyRowStatus,
        tmnxPppoePlcyLastMgmtChange,
        tmnxPppoePlcyDescription,
        tmnxPppoePlcyPppMtu,
        tmnxPppoePlcyLcpKaInterval,
        tmnxPppoePlcyLcpKaHoldUpMplier,
        tmnxPppoePlcyDisableAcCookies,
        tmnxPppoePlcyPadoDelay,
        tmnxPppoePlcyMaxSessionsPerMac,
        tmnxPppoePlcyReplyOnPadt,
        tmnxPppoePlcyPppAuthentication,
        tmnxPppoePlcyPppInitialDelay,
        tmnxPppoePlcyPppMinChapChallenge,
        tmnxPppoePlcyPppMaxChapChallenge,
        tmnxPppoePlcyPppOptionTblLstChg,
        tmnxPppoePlcyOptionRowStatus,
        tmnxPppoePlcyOptionLstMgmtChange,
        tmnxPppoePlcyOptionType,
        tmnxPppoePlcyOptionValue,
        tmnxPppoeIesIfInfoTableLastChg,
        tmnxPppoeIesIfLastChg,
        tmnxPppoeIesIfDescription,
        tmnxPppoeIesIfAdminState,
        tmnxPppoeIesIfPolicy,
        tmnxPppoeIesIfSessionLimit,
        tmnxPppoeIesIfSapSessionLimit,
        tmnxPppoeIesIfUserDb,
        tmnxPppoeIesIfAntiSpoofing,
        tmnxPppoeSapRxPadi,
        tmnxPppoeSapRxPadr,
        tmnxPppoeSapRxPadt,
        tmnxPppoeSapRxSession,
        tmnxPppoeSapRxInvalidVersion,
        tmnxPppoeSapRxInvalidType,
        tmnxPppoeSapRxInvalidCode,
        tmnxPppoeSapRxInvalidSession,
        tmnxPppoeSapRxInvalidLen,
        tmnxPppoeSapRxInvalidTags,
        tmnxPppoeSapRxInvalidAcCookie,
        tmnxPppoeSapRxDropped,
        tmnxPppoeSapTxPado,
        tmnxPppoeSapTxPads,
        tmnxPppoeSapTxPadt,
        tmnxPppoeSapTxSession,
        tmnxPppoeSessionUpTime,
        tmnxPppoeSessionLcpState,
        tmnxPppoeSessionIpcpState,
        tmnxPppoeSessionPppMtu,
        tmnxPppoeSessionPppAuthProtocol,
        tmnxPppoeSessionPppUserName,
        tmnxPppoeSessionSubIdent,
        tmnxPppoeSessionOriginSubIdent,
        tmnxPppoeSessionSubProfString,
        tmnxPppoeSessionSlaProfString,
        tmnxPppoeSessionAncpString,
        tmnxPppoeSessionInterDestId,
        tmnxPppoeSessionOriginStrings,
        tmnxPppoeSessionSessionTimeout,
        tmnxPppoeSessionIpAddrType,
        tmnxPppoeSessionIpAddr,
        tmnxPppoeSessionPrimaryDnsType,
        tmnxPppoeSessionPrimaryDns,
        tmnxPppoeSessionSecondryDnsType,
        tmnxPppoeSessionSecondryDns,
        tmnxPppoeSessionPrimaryNbnsType,
        tmnxPppoeSessionPrimaryNbns,
        tmnxPppoeSessionSecondryNbnsType,
        tmnxPppoeSessionSecondryNbns,
        tmnxPppoeSessionOriginIpcpInfo,
        tmnxPppoeSessionCircuitId,
        tmnxPppoeSessionRemoteId,
        tmnxPppoeSessionAddressPool,
        tmnxPppoeSessionType,
        tmnxPppoeSessionRetailerSvcId,
        tmnxPppoeSessionRetailerIf,
        tmnxPppoeSessionL2tpVrtrId,
        tmnxPppoeSessionL2tpConnectionId,
        tmnxPppoeSessionServiceName,
        tmnxPppoeSessionCategoryMapName,
        tmnxPppoeSessionRadiusClassAttr,
        tmnxPppoeSessionRadiusUserName,
        tmnxPppoeSessionIpv6cpState,
        tmnxPppoeSessionInterfaceId,
        tmnxPppoeSessionOriginIpv6cpInfo,
        tmnxPppoeSessionIpv6DnsType,
        tmnxPppoeSessionIpv6Dns1,
        tmnxPppoeSessionIpv6Dns2,
        tmnxPppoeSessionIpv6DelPfxType,
        tmnxPppoeSessionIpv6DelPfxLen,
        tmnxPppoeSessionIpv6DelPfx,
        tmnxPppoeSessionIpv6PrefixType,
        tmnxPppoeSessionIpv6PrefixLen,
        tmnxPppoeSessionIpv6Prefix,
        tmnxPppoeSessionModSubIdent,
        tmnxPppoeSessionModSubProfStr,
        tmnxPppoeSessionModSlaProfStr,
        tmnxPppoeSessionModAncpStr,
        tmnxPppoeSessionModInterDestId,
        tmnxPppoeSessionEvaluateState,
        tmnxPppoeSessionRxUnknownProto,
        tmnxPppoeSessionRxLcpConfReq,
        tmnxPppoeSessionRxLcpConfAck,
        tmnxPppoeSessionRxLcpConfNak,
        tmnxPppoeSessionRxLcpConfRej,
        tmnxPppoeSessionRxLcpTermReq,
        tmnxPppoeSessionRxLcpTermAck,
        tmnxPppoeSessionRxLcpCodeRej,
        tmnxPppoeSessionRxLcpEchoReq,
        tmnxPppoeSessionRxLcpEchoRep,
        tmnxPppoeSessionRxLcpProtRej,
        tmnxPppoeSessionRxLcpDiscReq,
        tmnxPppoeSessionTxLcpConfReq,
        tmnxPppoeSessionTxLcpConfAck,
        tmnxPppoeSessionTxLcpConfNak,
        tmnxPppoeSessionTxLcpConfRej,
        tmnxPppoeSessionTxLcpTermReq,
        tmnxPppoeSessionTxLcpTermAck,
        tmnxPppoeSessionTxLcpCodeRej,
        tmnxPppoeSessionTxLcpEchoReq,
        tmnxPppoeSessionTxLcpEchoRep,
        tmnxPppoeSessionTxLcpProtRej,
        tmnxPppoeSessionTxLcpDiscReq,
        tmnxPppoeSessionRxPapAuthReq,
        tmnxPppoeSessionTxPapAuthAck,
        tmnxPppoeSessionTxPapAuthNak,
        tmnxPppoeSessionRxChapResponse,
        tmnxPppoeSessionTxChapChallenge,
        tmnxPppoeSessionTxChapSuccess,
        tmnxPppoeSessionTxChapFailure,
        tmnxPppoeSessionRxIpcpConfReq,
        tmnxPppoeSessionRxIpcpConfAck,
        tmnxPppoeSessionRxIpcpConfNak,
        tmnxPppoeSessionRxIpcpConfRej,
        tmnxPppoeSessionRxIpcpTermReq,
        tmnxPppoeSessionRxIpcpTermAck,
        tmnxPppoeSessionRxIpcpCodeRej,
        tmnxPppoeSessionTxIpcpConfReq,
        tmnxPppoeSessionTxIpcpConfAck,
        tmnxPppoeSessionTxIpcpConfNak,
        tmnxPppoeSessionTxIpcpConfRej,
        tmnxPppoeSessionTxIpcpTermReq,
        tmnxPppoeSessionTxIpcpTermAck,
        tmnxPppoeSessionTxIpcpCodeRej,
        tmnxPppoeSessionRxIpv6cpConfReq,
        tmnxPppoeSessionRxIpv6cpConfAck,
        tmnxPppoeSessionRxIpv6cpConfNak,
        tmnxPppoeSessionRxIpv6cpConfRej,
        tmnxPppoeSessionRxIpv6cpTermReq,
        tmnxPppoeSessionRxIpv6cpTermAck,
        tmnxPppoeSessionRxIpv6cpCodeRej,
        tmnxPppoeSessionTxIpv6cpConfReq,
        tmnxPppoeSessionTxIpv6cpConfAck,
        tmnxPppoeSessionTxIpv6cpConfNak,
        tmnxPppoeSessionTxIpv6cpConfRej,
        tmnxPppoeSessionTxIpv6cpTermReq,
        tmnxPppoeSessionTxIpv6cpTermAck,
        tmnxPppoeSessionTxIpv6cpCodeRej,
        tmnxPppoeSessionOvrPIR,
        tmnxPppoeSessionOvrCIR,
        tmnxPppoeSessionOvrCBS,
        tmnxPppoeSessionOvrMBS,
        tmnxPppoeSessionAleDatalink,
        tmnxPppoeSessionAleEncaps1,
        tmnxPppoeSessionAleEncaps2,
        tmnxPppoePlcyPppIpcpSubnetNeg,
        tmnxPppoePlcyPadoAcName,
        tmnxPppoePlcyPppMtuForceGt1492,
        tmnxPppoePlcyUniqueSessIdsPerSap,
        tmnxPppoePlcySidAllocation,
        tmnxPppIesIfTableLastChg,
        tmnxPppIesIfLastChg,
        tmnxPppIesIfDescription,
        tmnxPppIesIfAdminState,
        tmnxPppIesIfPolicy,
        tmnxPppIesIfSessionLimit,
        tmnxPppIesIfUserDb,
        tmnxPppoeSessionSubPppIndex,
        tmnxPppoePlcyRejectDisabledNcp,
        tmnxPppoePlcyLcpIgnoreMagic,
        tmnxPppoePlcyAllowSameCidForDhcp,
        tmnxPppoeSapRxInvalidMac,
        tmnxPppoePlcySessionTimeout,
        tmnxPppoeIesIfDhcpcInclOptString,
        tmnxPppoePlcyReestablishSession,
        tmnxPppoePlcyDefaultUserName,
        tmnxPppoePlcyDefaultPapPassword,
        tmnxPppoeIesIfPythonPolicy,
        tmnxPppoeClntPlcyTableLastChg,
        tmnxPppoeClntPlcyRowStatus,
        tmnxPppoeClntPlcyLastMgmtChg,
        tmnxPppoeClntPlcyDescription,
        tmnxPppoeClntPlcyKaInterval,
        tmnxPppoeClntPlcyKaHoldUpM,
        tmnxPppoeClntPlcyMru,
        tmnxPppoeClntPlcyMtu,
        tmnxPppoeClntPlcyStack,
        tmnxPppoeClntPlcyRestartInit,
        tmnxPppoeClntPlcyRestartMax,
        tmnxPppoeClntPlcyPythonPlcy,
        tmnxPppoeClntSvcId,
        tmnxPppoeClntMac,
        tmnxPppoeClntUpTime,
        tmnxPppoeClntPolicy,
        tmnxPppoeClntServiceName,
        tmnxPppoeClntSessionId,
        tmnxPppoeClntAcMac,
        tmnxPppoeClntAcName,
        tmnxPppoeClntLcpState,
        tmnxPppoeClntIpcpState,
        tmnxPppoeClntIpv6cpState,
        tmnxPppoeClntLocalMagicNum,
        tmnxPppoeClntRemoteMagicNum,
        tmnxPppoeClntRemoteMru,
        tmnxPppoeClntPppUserName,
        tmnxPppoeClntPppAuthProtocol,
        tmnxPppoeClntIpcpIpAddrType,
        tmnxPppoeClntIpcpIpAddr,
        tmnxPppoeClntIpcpPriDnsType,
        tmnxPppoeClntIpcpPriDns,
        tmnxPppoeClntIpcpSecDnsType,
        tmnxPppoeClntIpcpSecDns,
        tmnxPppoeClntIpcpPriNbnsType,
        tmnxPppoeClntIpcpPriNbns,
        tmnxPppoeClntIpcpSecNbnsType,
        tmnxPppoeClntIpcpSecNbns,
        tmnxPppoeClntIpv6cpInterfaceId,
        tmnxPppoeClntSlaacPrefixType,
        tmnxPppoeClntSlaacPrefix,
        tmnxPppoeClntSlaacPrefixLen,
        tmnxPppoeClntSlaacPrefixTimeout,
        tmnxPppoeClntSlaacPriDnsType,
        tmnxPppoeClntSlaacPriDns,
        tmnxPppoeClntSlaacSecDnsType,
        tmnxPppoeClntSlaacSecDns,
        tmnxPppoeClntTxPadi,
        tmnxPppoeClntTxPadr,
        tmnxPppoeClntTxPadt,
        tmnxPppoeClntTxSession,
        tmnxPppoeClntTxLcpEchoReq,
        tmnxPppoeClntTxLcpEchoRep,
        tmnxPppoeClntTxV6Rs,
        tmnxPppoeClntTxV6DhcpInfo,
        tmnxPppoeClntRxPado,
        tmnxPppoeClntRxPads,
        tmnxPppoeClntRxPadt,
        tmnxPppoeClntRxSession,
        tmnxPppoeClntRxLcpEchoReq,
        tmnxPppoeClntRxLcpEchoRep,
        tmnxPppoeClntRxV6Ra,
        tmnxPppoeClntRxV6DhcpReply,
        tmnxPppoeClntRxDropped,
        tmnxPppoeClntMdaRxErr,
        tmnxPppoeClntMdaRxErrNotPppoe,
        tmnxPppoeClntMdaRxErrEchoMagic,
        tmnxPppoeClntMdaRxErrNoSession,
        tmnxPppoeClntMdaRxDiscovery,
        tmnxPppoeClntMdaRxPppControl,
        tmnxPppoeClntMdaRxEchoRequest,
        tmnxPppoeClntMdaRxEchoReply,
        tmnxPppoeClntMdaTxEchoRequest,
        tmnxPppoeClntMdaTxEchoReply,
        tmnxPppoeIesIfDhcpcInclClientId,
        tmnxPppoeClntVappRxErr,
        tmnxPppoeClntVappRxErrNotPppoe,
        tmnxPppoeClntVappRxErrEchoMagic,
        tmnxPppoeClntVappRxErrNoSession,
        tmnxPppoeClntVappRxDiscovery,
        tmnxPppoeClntVappRxPppControl,
        tmnxPppoeClntVappRxEchoRequest,
        tmnxPppoeClntVappRxEchoReply,
        tmnxPppoeClntVappTxEchoRequest,
        tmnxPppoeClntVappTxEchoReply,
        tmnxPppoePlcyMaxSessionsPerCid,
        tmnxPppoePlcyAllowSessionsWoCid
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting PPPoE on Nokia SROS series systems
         20.0 release."
    ::= { tmnxPppoeGroups 37 }

tmnxPPPoEV21v0Group              OBJECT-GROUP
    OBJECTS     {
        tmnxPppoePlcyNcpRenegotiation,
        tmnxPppoePlcyLcpIgnoreIdentifier
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting PPPoE on Nokia SROS series systems
         21.0 release."
    ::= { tmnxPppoeGroups 38 }

tmnxPPPoEV22v0NotifyGroup        NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxPppoeSessionFailure,
        tmnxPppoeNcpFailure,
        tmnxMlpppBundleIndicatorsChange,
        tmnxPppoeMaxSessionsOvrExceeded
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications generated by the PPPoE feature on Nokia
         SROS series systems 22.0 release."
    ::= { tmnxPppoeGroups 39 }

tmnxPPPoEV22v0NotifyObjsGroup    OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeSessionFailureReason,
        tmnxPppoeNcpFailureProtocol,
        tmnxPppoeNcpFailureReason,
        tmnxPppoeNotifyDescription,
        tmnxPppoeMaxSessionsOvrReason
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of PPPoE notification
         objects on Nokia SROS series systems 22.0 release."
    ::= { tmnxPppoeGroups 40 }

tmnxPPPoEV25v0NotifyGroup        NOTIFICATION-GROUP
    NOTIFICATIONS {
        tmnxPppoeLacFragFailed
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications generated by the PPPoE feature on Nokia
         SROS series systems 25.0 release."
    ::= { tmnxPppoeGroups 41 }

tmnxPPPoEV25v0NotifyObjsGroup    OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeLacFragVRtrID,
        tmnxPppoeLacFragFpeId
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of PPPoE notification
         objects on Nokia SROS series systems 25.0 release."
    ::= { tmnxPppoeGroups 42 }

tmnxPPPoEObsoletedGroup          OBJECT-GROUP
    OBJECTS     {
        tmnxPppoeIesIfPapChapUserDb,
        tmnxPppoeIesIfDhcpcCcagOriginSap,
        tmnxPppoeManagedRouteStatus,
        tmnxPppoeSessionAleDatalink,
        tmnxPppoeSessionAleEncaps1,
        tmnxPppoeSessionAleEncaps2,
        tmnxPppoeSessionBgpAuthKeyChain,
        tmnxPppoeSessionBgpExportPolicy,
        tmnxPppoeSessionBgpImportPolicy,
        tmnxPppoeSessionBgpMD5AuthKey,
        tmnxPppoeSessionBgpPeerAS,
        tmnxPppoeSessionBgpPeeringStatus,
        tmnxPppoeSessionBgpPrngPlcyName,
        tmnxPppoeSessionEvaluateState,
        tmnxPppoeSessionModAncpStr,
        tmnxPppoeSessionModAppProfStr,
        tmnxPppoeSessionModInterDestId,
        tmnxPppoeSessionModSlaProfStr,
        tmnxPppoeSessionModSubIdent,
        tmnxPppoeSessionModSubProfStr,
        tmnxPppoeSessionOvrCBS,
        tmnxPppoeSessionOvrCIR,
        tmnxPppoeSessionOvrMBS,
        tmnxPppoeSessionOvrPIR,
        tmnxPppoeSessionRxChapResponse,
        tmnxPppoeSessionRxIpcpCodeRej,
        tmnxPppoeSessionRxIpcpConfAck,
        tmnxPppoeSessionRxIpcpConfNak,
        tmnxPppoeSessionRxIpcpConfRej,
        tmnxPppoeSessionRxIpcpConfReq,
        tmnxPppoeSessionRxIpcpTermAck,
        tmnxPppoeSessionRxIpcpTermReq,
        tmnxPppoeSessionRxIpv6cpCodeRej,
        tmnxPppoeSessionRxIpv6cpConfAck,
        tmnxPppoeSessionRxIpv6cpConfNak,
        tmnxPppoeSessionRxIpv6cpConfRej,
        tmnxPppoeSessionRxIpv6cpConfReq,
        tmnxPppoeSessionRxIpv6cpTermAck,
        tmnxPppoeSessionRxIpv6cpTermReq,
        tmnxPppoeSessionRxLcpCodeRej,
        tmnxPppoeSessionRxLcpConfAck,
        tmnxPppoeSessionRxLcpConfNak,
        tmnxPppoeSessionRxLcpConfRej,
        tmnxPppoeSessionRxLcpConfReq,
        tmnxPppoeSessionRxLcpDiscReq,
        tmnxPppoeSessionRxLcpEchoRep,
        tmnxPppoeSessionRxLcpEchoReq,
        tmnxPppoeSessionRxLcpProtRej,
        tmnxPppoeSessionRxLcpTermAck,
        tmnxPppoeSessionRxLcpTermReq,
        tmnxPppoeSessionRxPapAuthReq,
        tmnxPppoeSessionRxUnknownProto,
        tmnxPppoeSessionTxChapChallenge,
        tmnxPppoeSessionTxChapFailure,
        tmnxPppoeSessionTxChapSuccess,
        tmnxPppoeSessionTxIpcpCodeRej,
        tmnxPppoeSessionTxIpcpConfAck,
        tmnxPppoeSessionTxIpcpConfNak,
        tmnxPppoeSessionTxIpcpConfRej,
        tmnxPppoeSessionTxIpcpConfReq,
        tmnxPppoeSessionTxIpcpTermAck,
        tmnxPppoeSessionTxIpcpTermReq,
        tmnxPppoeSessionTxIpv6cpCodeRej,
        tmnxPppoeSessionTxIpv6cpConfAck,
        tmnxPppoeSessionTxIpv6cpConfNak,
        tmnxPppoeSessionTxIpv6cpConfRej,
        tmnxPppoeSessionTxIpv6cpConfReq,
        tmnxPppoeSessionTxIpv6cpTermAck,
        tmnxPppoeSessionTxIpv6cpTermReq,
        tmnxPppoeSessionTxLcpCodeRej,
        tmnxPppoeSessionTxLcpConfAck,
        tmnxPppoeSessionTxLcpConfNak,
        tmnxPppoeSessionTxLcpConfRej,
        tmnxPppoeSessionTxLcpConfReq,
        tmnxPppoeSessionTxLcpDiscReq,
        tmnxPppoeSessionTxLcpEchoRep,
        tmnxPppoeSessionTxLcpEchoReq,
        tmnxPppoeSessionTxLcpProtRej,
        tmnxPppoeSessionTxLcpTermAck,
        tmnxPppoeSessionTxLcpTermReq,
        tmnxPppoeSessionTxPapAuthAck,
        tmnxPppoeSessionTxPapAuthNak,
        tmnxPppoeManagedRouteStatus,
        tmnxPppoeSessionAleDatalink,
        tmnxPppoeSessionAleEncaps1,
        tmnxPppoeSessionAleEncaps2,
        tmnxPppoeSessionBgpAuthKeyChain,
        tmnxPppoeSessionBgpExportPolicy,
        tmnxPppoeSessionBgpImportPolicy,
        tmnxPppoeSessionBgpMD5AuthKey,
        tmnxPppoeSessionBgpPeerAS,
        tmnxPppoeSessionBgpPeeringStatus,
        tmnxPppoeSessionBgpPrngPlcyName,
        tmnxPppoeSessionEvaluateState,
        tmnxPppoeSessionModAncpStr,
        tmnxPppoeSessionModAppProfStr,
        tmnxPppoeSessionModInterDestId,
        tmnxPppoeSessionModSlaProfStr,
        tmnxPppoeSessionModSubIdent,
        tmnxPppoeSessionModSubProfStr,
        tmnxPppoeSessionOvrCBS,
        tmnxPppoeSessionOvrCIR,
        tmnxPppoeSessionOvrMBS,
        tmnxPppoeSessionOvrPIR,
        tmnxPppoeSessionUpTime,
        tmnxPppoeSessionLcpState,
        tmnxPppoeSessionIpcpState,
        tmnxPppoeSessionPppMtu,
        tmnxPppoeSessionPppAuthProtocol,
        tmnxPppoeSessionPppUserName,
        tmnxPppoeSessionSubIdent,
        tmnxPppoeSessionOriginSubIdent,
        tmnxPppoeSessionSubProfString,
        tmnxPppoeSessionSlaProfString,
        tmnxPppoeSessionAncpString,
        tmnxPppoeSessionInterDestId,
        tmnxPppoeSessionAppProfString,
        tmnxPppoeSessionOriginStrings,
        tmnxPppoeSessionSessionTimeout,
        tmnxPppoeSessionIpAddrType,
        tmnxPppoeSessionIpAddr,
        tmnxPppoeSessionPrimaryDnsType,
        tmnxPppoeSessionPrimaryDns,
        tmnxPppoeSessionSecondryDnsType,
        tmnxPppoeSessionSecondryDns,
        tmnxPppoeSessionPrimaryNbnsType,
        tmnxPppoeSessionPrimaryNbns,
        tmnxPppoeSessionSecondryNbnsType,
        tmnxPppoeSessionSecondryNbns,
        tmnxPppoeSessionOriginIpcpInfo,
        tmnxPppoeSessionCircuitId,
        tmnxPppoeSessionRemoteId,
        tmnxPppoeSessionAddressPool,
        tmnxPppoeSessionType,
        tmnxPppoeSessionRetailerSvcId,
        tmnxPppoeSessionRetailerIf,
        tmnxPppoeSessionL2tpVrtrId,
        tmnxPppoeSessionL2tpConnectionId,
        tmnxPppoeSessionCategoryMapName,
        tmnxPppoeSessionRadiusClassAttr,
        tmnxPppoeSessionRadiusUserName,
        tmnxPppoeSessionIpv6cpState,
        tmnxPppoeSessionInterfaceId,
        tmnxPppoeSessionOriginIpv6cpInfo,
        tmnxPppoeSessionIpv6DnsType,
        tmnxPppoeSessionIpv6Dns1,
        tmnxPppoeSessionIpv6Dns2,
        tmnxPppoeSessionIpv6DelPfxType,
        tmnxPppoeSessionIpv6DelPfxLen,
        tmnxPppoeSessionIpv6DelPfx,
        tmnxPppoeSessionIpv6PrefixType,
        tmnxPppoeSessionIpv6PrefixLen,
        tmnxPppoeSessionIpv6Prefix,
        tmnxPppoeIesIfDhcpcInclOptString
    }
    STATUS      current
    DESCRIPTION
        "The group of objects obsoleted PPPoE objects."
    ::= { tmnxPppoeGroups 98 }

tmnxPppIesIfObsoletedGroup       OBJECT-GROUP
    OBJECTS     {
        tmnxPppIesIfLastChg,
        tmnxPppIesIfDescription,
        tmnxPppIesIfAdminState,
        tmnxPppIesIfPolicy,
        tmnxPppIesIfSessionLimit,
        tmnxPppIesIfUserDb
    }
    STATUS      current
    DESCRIPTION
        "The group of PPP objects obsoleted in release 23 of the Nokia SROS
         series systems."
    ::= { tmnxPppoeGroups 99 }

tmnxPppoeNotifyPrefix            OBJECT IDENTIFIER ::= { tmnxSRNotifyPrefix 49 }

tmnxPppoeNotifications           OBJECT IDENTIFIER ::= { tmnxPppoeNotifyPrefix 0 }

tmnxPppoeSessionFailure          NOTIFICATION-TYPE
    OBJECTS     {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeSessionFailureReason
    }
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeSessionFailure notification indicates that the system
         could not create a new PPPoE session in the tmnxPppoeSessionTable. The
         problem is described in the object tmnxPppoeSessionFailureReason."
    ::= { tmnxPppoeNotifications 1 }

tmnxPppoeNcpFailure              NOTIFICATION-TYPE
    OBJECTS     {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeNcpFailureProtocol,
        tmnxPppoeNcpFailureReason
    }
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeNcpFailure notification indicates that there is a NCP
         phase setup problem."
    ::= { tmnxPppoeNotifications 2 }

tmnxMlpppBundleIndicatorsChange  NOTIFICATION-TYPE
    OBJECTS     {
        tmnxMlpppBundleIndicators,
        tmnxPppoeNotifyDescription
    }
    STATUS      current
    DESCRIPTION
        "The tmnxMlpppBundleIndicatorsChange notification indicates that the
         value of the object tmnxMlpppBundleIndicatorsChange has changed.

         [CAUSE] The value of the object tmnxMlpppBundleIndicatorsChange has
         changed. A particular change is the change from 'lfi|lfiCfg' to
         'lfiCfg': since interleaving is only supported on bundles with a
         single link, interleaving is disabled when a second link is added to a
         bundle.

         [EFFECT] When the value of the object tmnxMlpppBundleIndicatorsChange
         changes from 'lfi|lfiCfg' to 'lfiCfg', Link Fragmentation and
         Interleaving (LFI) is disabled on the bundle."
    ::= { tmnxPppoeNotifications 3 }

tmnxPppoeLacSteeringActive       NOTIFICATION-TYPE
    OBJECTS     {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeLacSteeringSession,
        tmnxPppoeLacSteeringProfile
    }
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeLacSteeringActive notification indicates that the
         appropriate PPPoE/LAC session is steered."
    ::= { tmnxPppoeNotifications 4 }

tmnxPppoeLacSteeringStopped      NOTIFICATION-TYPE
    OBJECTS     {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeLacSteeringSession,
        tmnxPppoeLacSteeringProfile
    }
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeLacSteeringStopped notification indicates that the
         appropriate steered PPPoE/LAC session has stopped steering. To make
         the session steered again, a COA with the appropriate steering profile
         has to be sent"
    ::= { tmnxPppoeNotifications 5 }

tmnxPppoeLacSteeringFailed       NOTIFICATION-TYPE
    OBJECTS     {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeLacSteeringFailure,
        tmnxPppoeLacSteeringSession,
        tmnxPppoeLacSteeringProfile
    }
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeLacSteeringFailed notification indicates that steering
         has failed. The problem is described in the object
         tmnxPppoeLacSteeringFailure."
    ::= { tmnxPppoeNotifications 6 }

tmnxPppoeMaxSessionsOvrExceeded  NOTIFICATION-TYPE
    OBJECTS     {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeMaxSessionsOvrReason
    }
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeMaxSessionsOvrExceeded notification indicates the
         configured maximum number of sessions has been reached. Detailed
         information is provided in the object tmnxPppoeMaxSessionsOvrReason."
    ::= { tmnxPppoeNotifications 7 }

tmnxPppoeLacFragFailed           NOTIFICATION-TYPE
    OBJECTS     {
        svcId,
        sapPortId,
        sapEncapValue,
        tmnxPppoeLacSteeringSession,
        tmnxPppoeLacFragVRtrID,
        tmnxPppoeLacFragFpeId,
        tmnxPppoeLacSteeringFailure
    }
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeLacFragFailed notification indicates the FPE resources,
         required for LAC fragmentation, are not available or the FPE path is
         not operational. The object tmnxPppoeLacSteeringFailure describes the
         problem."
    ::= { tmnxPppoeNotifications 8 }

tmnxPppoeClntNotifications       OBJECT IDENTIFIER ::= { tmnxPppoeNotifyPrefix 1 }

tmnxPppoeClientSetupFailure      NOTIFICATION-TYPE
    OBJECTS     {
        tmnxPppoeClntIdent
    }
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeClientSetupFailure notification indicates that the
         specified PPPoE client encountered a failure during setup."
    ::= { tmnxPppoeClntNotifications 1 }

tmnxPppoeClientEchoTimeout       NOTIFICATION-TYPE
    OBJECTS     {
        tmnxPppoeClntIdent
    }
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeClientEchoTimeout notification indicates that the
         specified PPPoE client encountered an LCP echo timeout."
    ::= { tmnxPppoeClntNotifications 2 }

tmnxPppoeClientNcpFailure        NOTIFICATION-TYPE
    OBJECTS     {
        tmnxPppoeClntIdent,
        tmnxPppoeNcpFailureProtocol
    }
    STATUS      current
    DESCRIPTION
        "The tmnxPppoeClientNcpFailure notification indicates that the
         specified PPPoE client encountered a NCP phase setup failure."
    ::= { tmnxPppoeClntNotifications 3 }

END
