TIMETRA-LDP-NG-MIB DEFINITIONS ::= BEGIN

IMPORTS
    InterfaceIndexOrZero
                                                         FROM IF-MIB
    InetAddress, InetAddressPrefixLength,
    InetAddressType, InetVersion
                                                         FROM INET-ADDRESS-MIB
    MplsLsrIdentifier
                                                         FROM MPLS-LDP-MIB
    MODULE-COMPLIANCE, NOTIFICATION-GROUP,
    OBJECT-GROUP
                                                         FROM SNMPv2-CONF
    Counter32, Gauge32, Integer32,
    MODULE-IDENTITY, NOTIFICATION-TYPE,
    OBJECT-TYPE, Unsigned32
                                                         FROM SNMPv2-SMI
    DisplayString, RowStatus, TimeInterval,
    TimeStamp, TruthValue
                                                         FROM SNMPv2-TC
    timetraSRMIBModules, tmnxSRConfs,
    tmnxSRNotifyPrefix, tmnxSRObjs
                                                         FROM TIMETRA-GLOBAL-MIB
    TmnxLabelSigStatus, TmnxLabelStatus,
    TmnxLdpAdjacencyType,
    TmnxLdpBackoffTime, TmnxLdpFECFlags,
    TmnxLdpFECPolicy,
    TmnxLdpGenOperDownReasonCode,
    TmnxLdpHelloFactor, TmnxLdpHelloTimeout,
    TmnxLdpInLblWdrawalReasonCode,
    TmnxLdpIntTargOperDownReasonCode,
    TmnxLdpKeepAliveFactor,
    TmnxLdpLabelDistMethod,
    TmnxLdpNewHelloTimeout,
    TmnxLdpNewKeepAliveTimeout, TmnxVpnId
                                                         FROM TIMETRA-LDP-MIB
    SdpId, ServType,
    TdmOptionsCasTrunkFraming,
    TdmOptionsSigPkts
                                                         FROM TIMETRA-SERV-MIB
    TNamedItem, TNamedItemOrEmpty,
    TPolicyStatementNameOrEmpty,
    TmnxAddressAndPrefixAddress,
    TmnxAddressAndPrefixPrefix,
    TmnxAddressAndPrefixType,
    TmnxAdminState, TmnxCBFClasses,
    TmnxEnabledDisabled, TmnxLdpFECType,
    TmnxMplsLdpNgIdType,
    TmnxMplsLdpNgIdentifier,
    TmnxMplsLsrNgIdentifier, TmnxOperState,
    TmnxServId, TmnxVRtrMplsLspID, TmnxVcId,
    TmnxVcIdOrNone, TmnxVcType
                                                         FROM TIMETRA-TC-MIB
    vRtrID
                                                         FROM TIMETRA-VRTR-MIB
    ;

timetraLdpNgMIBModule            MODULE-IDENTITY
    LAST-UPDATED "201701010000Z"
    ORGANIZATION "Nokia"
    CONTACT-INFO
        "Nokia SROS Support
         Web: http://www.nokia.com"
    DESCRIPTION
        "The MIB module to manage and provision the Nokia SROS LDP NG protocol
         features.

         Copyright 2013-2018 Nokia. All rights reserved. Reproduction of this
         document is authorized on the condition that the foregoing copyright
         notice is included.

         This SNMP MIB module (Specification) embodies Nokia's
         proprietary intellectual property.  Nokia retains
         all title and ownership in the Specification, including any
         revisions.

         Nokia grants all interested parties a non-exclusive license to use and
         distribute an unmodified copy of this Specification in connection with
         management of Nokia products, and without fee, provided this copyright
         notice and license appear on all copies.

         This Specification is supplied 'as is', and Nokia makes no warranty,
         either express or implied, as to the use, operation, condition, or
         performance of the Specification."

    REVISION    "201701010000Z"
    DESCRIPTION
        "Rev 15.0                1 Jan 2017 00:00
         15.0 release of the TIMETRA-LDP-NG-MIB."

    REVISION    "201601010000Z"
    DESCRIPTION
        "Rev 14.0                1 Jan 2016 00:00
         14.0 release of the TIMETRA-LDP-NG-MIB."

    REVISION    "201501010000Z"
    DESCRIPTION
        "Rev 13.0                1 Jan 2015 00:00
         13.0 release of the TIMETRA-LDP-NG-MIB."

    REVISION    "201402010000Z"
    DESCRIPTION
        "Rev 0.1                 1 Feb 2014 00:00
         Initial version of the TIMETRA-LDP-NG-MIB."

    ::= { timetraSRMIBModules 91 }

tmnxLdpNgObjs                    OBJECT IDENTIFIER ::= { tmnxSRObjs 91 }

vRtrLdpNgIfTableLstChanged       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfTableLstChanged indicates the last timestamp
         when an entry in the vRtrLdpNgIfTable was last changed."
    ::= { tmnxLdpNgObjs 1 }

vRtrLdpNgIfTable                 OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgIfTable provides an entry for each virtual router
         interface configured to be used with the Label Distribution Protocol
         (LDP)."
    ::= { tmnxLdpNgObjs 2 }

vRtrLdpNgIfEntry                 OBJECT-TYPE
    SYNTAX      VRtrLdpNgIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an interface on this virtual router that
         participates in the LDP protocol.

         Row entries can be created or deleted via SNMP SET requests. A row
         with default attribute values is created by setting
         vRtrLdpNgIfRowStatus to 'createAndGo'. A row entry can be destroyed by
         setting vRtrLdpNgIfRowStatus to 'destroy'."
    INDEX       {
        vRtrID,
        vRtrLdpNgIfIndex
    }
    ::= { vRtrLdpNgIfTable 1 }

VRtrLdpNgIfEntry                 ::= SEQUENCE
{
    vRtrLdpNgIfIndex                 InterfaceIndexOrZero,
    vRtrLdpNgIfRowStatus             RowStatus,
    vRtrLdpNgIfLastChange            TimeStamp,
    vRtrLdpNgIfAdminState            TmnxAdminState,
    vRtrLdpNgIfOperState             TmnxOperState,
    vRtrLdpNgIfOperDownReason        TmnxLdpIntTargOperDownReasonCode,
    vRtrLdpNgIfBfdEnabled            BITS,
    vRtrLdpNgIfLBWeight              Unsigned32
}

vRtrLdpNgIfIndex                 OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfIndex specifies the interface index."
    ::= { vRtrLdpNgIfEntry 1 }

vRtrLdpNgIfRowStatus             OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgIfRowStatus is used to control the creation and deletion of
         rows in the vRtrLdpNgIfTable.

         A row can be created by setting vRtrLdpNgIfRowStatus to 'createAndGo'.
         The agent should assign the default attribute values and change the
         row status to 'active'.

         A row entry can be destroyed by setting vRtrLdpNgIfRowStatus to
         'destroy'."
    ::= { vRtrLdpNgIfEntry 2 }

vRtrLdpNgIfLastChange            OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfLastChange indicates the sysUpTime when this
         row was last modified."
    ::= { vRtrLdpNgIfEntry 3 }

vRtrLdpNgIfAdminState            OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfAdminState specifies the desired
         administrative state for LDP on this interface."
    DEFVAL      { inService }
    ::= { vRtrLdpNgIfEntry 4 }

vRtrLdpNgIfOperState             OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfOperState indicates the current operational
         state of LDP of this interface"
    ::= { vRtrLdpNgIfEntry 5 }

vRtrLdpNgIfOperDownReason        OBJECT-TYPE
    SYNTAX      TmnxLdpIntTargOperDownReasonCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfOperDownReason indicates the reason that the
         LDP interface is operationally down."
    ::= { vRtrLdpNgIfEntry 6 }

vRtrLdpNgIfBfdEnabled            OBJECT-TYPE
    SYNTAX      BITS {
        ipv4 (0),
        ipv6 (1)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfBfdEnabled specifies whether BFD tracking is
         enabled to hello adjacency source address of the peer. When multiple
         links exist to the same LDP peer, a Hello adjacency is established
         over each link and a separate BFD session is enabled on each LDP
         interface. If there are any FEC resolved over this interface, LDP will
         enable BFD tracking to each next hop.

         When this object has a value of 'ipv4', BFD tracking is enabled to
         each resolved ipv4 FEC next hop and or ipv4 hello adjacency over this
         interface. When this object has a value of 'ipv6', BFD tracking is
         enabled to each resolved ipv6 FEC next hop and or ipv6 hello adjacency
         over this interface. In case FEC next hop and hello adjacency source
         address of the peer is same, only one BFD session is used to track
         both. When this object has value of 0, BFD tracking is disabled."
    DEFVAL      { {} }
    ::= { vRtrLdpNgIfEntry 7 }

vRtrLdpNgIfLBWeight              OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object vRtrLdpNgIfLBWeight specifies an explicit
         load-balancing-weight for this interface. This weight overrides IGP
         route next-hop weights if configured."
    DEFVAL      { 0 }
    ::= { vRtrLdpNgIfEntry 8 }

vRtrLdpNgHelloAdjTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgHelloAdjEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgHelloAdjTable is a read-only table which has information
         about Hello Adjacencies for Sessions. A hello adjacency can be
         associated with an LDP interface or with a targeted peer."
    ::= { tmnxLdpNgObjs 3 }

vRtrLdpNgHelloAdjEntry           OBJECT-TYPE
    SYNTAX      VRtrLdpNgHelloAdjEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row represents a single LDP Hello Adjacency. An LDP Session can
         have one or more Hello adjacencies.

         vRtrLdpNgIfIndex and vRtrLdpNgPeerAddress are mutually exclusive
         fields. When vRtrLdpNgIfIndex is non zero, vRtrLdpNgPeerAddressType
         will have value of IPv4 and vRtrLdpNgPeerAddress will be 0.0.0.0. When
         the value of vRtrLdpNgPeerAddress is non zero, vRtrLdpNgIfIndex will
         be 0."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vRtrLdpNgIfIndex,
        vRtrLdpNgIfAddrType,
        vRtrLdpNgPeerAddressType,
        vRtrLdpNgPeerAddress
    }
    ::= { vRtrLdpNgHelloAdjTable 1 }

VRtrLdpNgHelloAdjEntry           ::= SEQUENCE
{
    vRtrLdpNgPeerLdpIdType           TmnxMplsLdpNgIdType,
    vRtrLdpNgPeerLdpId               TmnxMplsLdpNgIdentifier,
    vRtrLdpNgHelloAdjLclLdpIdType    TmnxMplsLdpNgIdType,
    vRtrLdpNgHelloAdjLclLdpId        TmnxMplsLdpNgIdentifier,
    vRtrLdpNgHelloAdjEntityIndex     Unsigned32,
    vRtrLdpNgHelloAdjIndex           Unsigned32,
    vRtrLdpNgHelloAdjHoldTimeRem     Unsigned32,
    vRtrLdpNgHelloAdjType            TmnxLdpAdjacencyType,
    vRtrLdpNgHelloAdjRemConfSeqNum   Unsigned32,
    vRtrLdpNgHelloAdjRemIpAddrType   InetAddressType,
    vRtrLdpNgHelloAdjRemIpAddress    InetAddress,
    vRtrLdpNgHelloAdjUpTime          TimeInterval,
    vRtrLdpNgHelloAdjLclConfSeqNum   Unsigned32,
    vRtrLdpNgHelloAdjLclIpAddrType   InetAddressType,
    vRtrLdpNgHelloAdjLclIpAddress    InetAddress,
    vRtrLdpNgHelloAdjInHelloMsgCnt   Counter32,
    vRtrLdpNgHelloAdjOutHelloMsgCnt  Counter32,
    vRtrLdpNgHelloAdjLclTimeout      TmnxLdpHelloTimeout,
    vRtrLdpNgHelloAdjRemTimeout      TmnxLdpHelloTimeout,
    vRtrLdpNgHelloAdjBfdStatus       INTEGER,
    vRtrLdpNgHelloAdjLclIPv4P2MPCap  TruthValue,
    vRtrLdpNgHelloAdjRemIPv4P2MPCap  TruthValue,
    vRtrLdpNgHelloAdjLclIPv6P2MPCap  TruthValue,
    vRtrLdpNgHelloAdjRemIPv6P2MPCap  TruthValue,
    vRtrLdpNgHelloAdjLclIPv4PfxCap   TruthValue,
    vRtrLdpNgHelloAdjRemIPv4PfxCap   TruthValue,
    vRtrLdpNgHelloAdjLclIPv6PfxCap   TruthValue,
    vRtrLdpNgHelloAdjRemIPv6PfxCap   TruthValue,
    vRtrLdpNgHelloAdjPeerCapRecv     BITS
}

vRtrLdpNgPeerLdpIdType           OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object vRtrLdpNgPeerLdpIdType is an index for the row entry. It
         indicates the LDP identifier type of the peer indicated by
         vRtrLdpNgPeerLdpId."
    ::= { vRtrLdpNgHelloAdjEntry 1 }

vRtrLdpNgPeerLdpId               OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdentifier (SIZE (6|18))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object vRtrLdpNgPeerLdpId is an index for the row entry. It
         indicates the LDP identifier of the peer."
    ::= { vRtrLdpNgHelloAdjEntry 2 }

vRtrLdpNgHelloAdjLclLdpIdType    OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjLclLdpIdType indicates the local LDP
         identifier type for this specific adjacency indicated by
         vRtrLdpNgHelloAdjLclLdpId ."
    ::= { vRtrLdpNgHelloAdjEntry 3 }

vRtrLdpNgHelloAdjLclLdpId        OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdentifier (SIZE (6|18))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjLclLdpId indicates the local LDP
         identifier for this specific adjacency."
    ::= { vRtrLdpNgHelloAdjEntry 4 }

vRtrLdpNgHelloAdjEntityIndex     OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjEntityIndex indicates the Entity index
         which is an index for MPLS-LDP-MIB::mplsLdpHelloAdjacencyEntry."
    ::= { vRtrLdpNgHelloAdjEntry 5 }

vRtrLdpNgHelloAdjIndex           OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjIndex indicates the Hello adjacency
         index which is an index for MPLS-LDP-MIB::mplsLdpHelloAdjacencyEntry."
    ::= { vRtrLdpNgHelloAdjEntry 6 }

vRtrLdpNgHelloAdjHoldTimeRem     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjHoldTimeRem indicates the hold time
         remaining for this Hello Adjacency. This interval will change when the
         next Hello message which corresponds to this Hello Adjacency is
         received."
    ::= { vRtrLdpNgHelloAdjEntry 7 }

vRtrLdpNgHelloAdjType            OBJECT-TYPE
    SYNTAX      TmnxLdpAdjacencyType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjType indicates the type of this Hello
         Adjacency. If this value is 'link' then this adjacency is a result of
         a Link Hello. If this value is 'hello', then the adjacency is a result
         of a Targeted Hello."
    ::= { vRtrLdpNgHelloAdjEntry 8 }

vRtrLdpNgHelloAdjRemConfSeqNum   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjRemConfSeqNum indicates the
         Configuration sequence number that was in the Hello received when this
         adjacency started up. This configuration sequence number changes when
         there is a change of configuration."
    ::= { vRtrLdpNgHelloAdjEntry 9 }

vRtrLdpNgHelloAdjRemIpAddrType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjRemIpAddrType indicates the type of
         address indicated by vRtrLdpNgHelloAdjRemIpAddress."
    ::= { vRtrLdpNgHelloAdjEntry 10 }

vRtrLdpNgHelloAdjRemIpAddress    OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjRemIpAddress indicates the peer IP
         address of the interface/targeted session that sent hellos for this
         specific adjacency."
    ::= { vRtrLdpNgHelloAdjEntry 11 }

vRtrLdpNgHelloAdjUpTime          OBJECT-TYPE
    SYNTAX      TimeInterval
    UNITS       "centiseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjUpTime indicates the time that this
         adjacency has been up."
    ::= { vRtrLdpNgHelloAdjEntry 12 }

vRtrLdpNgHelloAdjLclConfSeqNum   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjLclConfSeqNum indicates the
         Configuration sequence number that was used in the Hello sent when
         this adjacency started up. This configuration sequence number changes
         when there is a change of configuration."
    ::= { vRtrLdpNgHelloAdjEntry 13 }

vRtrLdpNgHelloAdjLclIpAddrType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjLclIpAddrType indicates the type of
         address indicated by vRtrLdpNgHelloAdjLclIpAddress."
    ::= { vRtrLdpNgHelloAdjEntry 14 }

vRtrLdpNgHelloAdjLclIpAddress    OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjLclIpAddress indicates the local IP
         address of the interface/targeted session used in Hellos sent for this
         specific adjacency."
    ::= { vRtrLdpNgHelloAdjEntry 15 }

vRtrLdpNgHelloAdjInHelloMsgCnt   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjInHelloMsgCnt indicates the number of
         Hello messages that have been received for this adjacency."
    ::= { vRtrLdpNgHelloAdjEntry 16 }

vRtrLdpNgHelloAdjOutHelloMsgCnt  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjOutHelloMsgCnt indicates the number of
         Hello messages that have been sent for this adjacency."
    ::= { vRtrLdpNgHelloAdjEntry 17 }

vRtrLdpNgHelloAdjLclTimeout      OBJECT-TYPE
    SYNTAX      TmnxLdpHelloTimeout
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjLclTimeout indicates the hello timeout
         used in the Hellos sent for this specific adjacency."
    ::= { vRtrLdpNgHelloAdjEntry 18 }

vRtrLdpNgHelloAdjRemTimeout      OBJECT-TYPE
    SYNTAX      TmnxLdpHelloTimeout
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjRemTimeout indicates the hello timeout
         used by the remote end that sent Hellos for this specific adjacency."
    ::= { vRtrLdpNgHelloAdjEntry 19 }

vRtrLdpNgHelloAdjBfdStatus       OBJECT-TYPE
    SYNTAX      INTEGER {
        noService    (1),
        inService    (2),
        outOfService (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjBfdStatus indicates the BFD operational
         status for LDP hello adjacency.

         If the value of vRtrLdpNgHelloAdjBfdStatus is 'noService', BFD is not
         enabled for LDP hello adjacency. If the value of the object is
         'outOfService', BFD is enabled but it is down and not running. If the
         value of object is 'inService', BFD is enabled and it is running."
    ::= { vRtrLdpNgHelloAdjEntry 20 }

vRtrLdpNgHelloAdjLclIPv4P2MPCap  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjLclIPv4P2MPCap indicates whether the
         local peer supports traffic exchange for IPv4 P2MP FECs."
    ::= { vRtrLdpNgHelloAdjEntry 21 }

vRtrLdpNgHelloAdjRemIPv4P2MPCap  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjRemIPv4P2MPCap indicates whether the
         remote peer supports traffic exchange for IPv4 P2MP FECs. When the
         'ipv4P2MPFec' bit is not set in object vRtrLdpNgHelloAdjPeerCapRecv,
         this will be 'true'. Otherwise, it will be value sent by the peer LSR."
    ::= { vRtrLdpNgHelloAdjEntry 22 }

vRtrLdpNgHelloAdjLclIPv6P2MPCap  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjLclIPv6P2MPCap indicates whether the
         local peer supports traffic exchange for IPv6 P2MP FECs."
    ::= { vRtrLdpNgHelloAdjEntry 23 }

vRtrLdpNgHelloAdjRemIPv6P2MPCap  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjRemIPv6P2MPCap indicates whether the
         remote peer supports traffic exchange for IPv6 P2MP FECs. When the
         'ipv6P2MPFec' bit is not set in object vRtrLdpNgHelloAdjPeerCapRecv,
         this will be 'true'. Otherwise, it will be value sent by the peer LSR."
    ::= { vRtrLdpNgHelloAdjEntry 24 }

vRtrLdpNgHelloAdjLclIPv4PfxCap   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjLclIPv4PfxCap indicates whether the
         local peer supports traffic exchange for IPv4 Prefix FECs."
    ::= { vRtrLdpNgHelloAdjEntry 25 }

vRtrLdpNgHelloAdjRemIPv4PfxCap   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjRemIPv4PfxCap indicates whether the
         remote peer supports traffic exchange for IPv4 Prefix FECs. When the
         'ipv4PfxFec' bit is not set in object vRtrLdpNgHelloAdjPeerCapRecv,
         this will be 'true'. Otherwise, it will be value sent by the peer LSR."
    ::= { vRtrLdpNgHelloAdjEntry 26 }

vRtrLdpNgHelloAdjLclIPv6PfxCap   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjLclIPv6PfxCap indicates whether the
         local peer supports traffic exchange for IPv6 Prefix FECs."
    ::= { vRtrLdpNgHelloAdjEntry 27 }

vRtrLdpNgHelloAdjRemIPv6PfxCap   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjRemIPv6PfxCap indicates whether the
         remote peer supports traffic exchange for IPv6 Prefix FECs. When the
         'ipv6PfxFec' bit is not set in object vRtrLdpNgHelloAdjPeerCapRecv,
         this will be 'true'. Otherwise, it will be value sent by the peer LSR."
    ::= { vRtrLdpNgHelloAdjEntry 28 }

vRtrLdpNgHelloAdjPeerCapRecv     OBJECT-TYPE
    SYNTAX      BITS {
        ipv4PfxFec  (0),
        ipv6PfxFec  (1),
        ipv4P2MPFec (2),
        ipv6P2MPFec (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjPeerCapRecv indicates various
         capabilities signaled by the peer LSR in a hello message. A particular
         capability bit will be set to 1 when the peer sent capability info in
         at least one of its hello message."
    ::= { vRtrLdpNgHelloAdjEntry 29 }

vRtrLdpNgSessionTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgSessionTable is a read-only table which parallels the
         mplsLdpSessionTable in the MPLS-LDP-MIB. The purpose of this table is
         to keep information about a single session between an LDP entity and
         an LDP Peer."
    ::= { tmnxLdpNgObjs 4 }

vRtrLdpNgSessionEntry            OBJECT-TYPE
    SYNTAX      VRtrLdpNgSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table represents information about a single session
         between an LDP entity and an LDP Peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId
    }
    ::= { vRtrLdpNgSessionTable 1 }

VRtrLdpNgSessionEntry            ::= SEQUENCE
{
    vRtrLdpNgSessLocalLdpIdType      TmnxMplsLdpNgIdType,
    vRtrLdpNgSessLocalLdpId          TmnxMplsLdpNgIdentifier,
    vRtrLdpNgSessEntityIndex         Unsigned32,
    vRtrLdpNgSessLabelDistMethod     TmnxLdpLabelDistMethod,
    vRtrLdpNgSessLoopDetectForPV     INTEGER,
    vRtrLdpNgSessPathVectorLimit     Unsigned32,
    vRtrLdpNgSessState               INTEGER,
    vRtrLdpNgSessAdjacencyType       TmnxLdpAdjacencyType,
    vRtrLdpNgSessProtocolVersion     Unsigned32,
    vRtrLdpNgSessLocalUdpPort        Unsigned32,
    vRtrLdpNgSessPeerUdpPort         Unsigned32,
    vRtrLdpNgSessLocalTcpPort        Unsigned32,
    vRtrLdpNgSessPeerTcpPort         Unsigned32,
    vRtrLdpNgSessLocalAddrType       InetAddressType,
    vRtrLdpNgSessLocalAddress        InetAddress,
    vRtrLdpNgSessPeerAddrType        InetAddressType,
    vRtrLdpNgSessPeerAddress         InetAddress,
    vRtrLdpNgSessKAHoldTimeRemaining TimeInterval,
    vRtrLdpNgSessMaxPduLength        Unsigned32,
    vRtrLdpNgSessUpTime              TimeInterval,
    vRtrLdpNgSessLocalKATimeout      TmnxLdpNewKeepAliveTimeout,
    vRtrLdpNgSessPeerKATimeout       TmnxLdpNewKeepAliveTimeout,
    vRtrLdpNgSessAdvertise           INTEGER,
    vRtrLdpNgSessLclGRHelperState    TruthValue,
    vRtrLdpNgSessPeerGRState         TruthValue,
    vRtrLdpNgSessPeerNumRestart      Counter32,
    vRtrLdpNgSessLastRestartTime     TimeStamp,
    vRtrLdpNgSessLocalFtReconTime    Unsigned32,
    vRtrLdpNgSessPeerFtReconTime     Unsigned32,
    vRtrLdpNgSessLocalFtRecovTime    Unsigned32,
    vRtrLdpNgSessPeerFtRecovTime     Unsigned32,
    vRtrLdpNgSessFtReconTimeRem      Unsigned32,
    vRtrLdpNgSessFtRecovTimeRem      Unsigned32,
    vRtrLdpNgSessBfdStatus           INTEGER,
    vRtrLdpNgSessLocalP2MPCap        TruthValue,
    vRtrLdpNgSessPeerP2MPCap         TruthValue,
    vRtrLdpNgSessLocalMPMBBCap       TruthValue,
    vRtrLdpNgSessPeerMPMBBCap        TruthValue,
    vRtrLdpNgSessLocalDynCap         TruthValue,
    vRtrLdpNgSessPeerDynCap          TruthValue,
    vRtrLdpNgSessLocalOLoadCap       TruthValue,
    vRtrLdpNgSessPeerOLoadCap        TruthValue,
    vRtrLdpNgSessIPv4PfxFecOLoadSent TruthValue,
    vRtrLdpNgSessIPv6PfxFecOLoadSent TruthValue,
    vRtrLdpNgSessIPv4PfxFecOLoadRecv TruthValue,
    vRtrLdpNgSessIPv6PfxFecOLoadRecv TruthValue,
    vRtrLdpNgSessIPv4P2MPFecOLSent   TruthValue,
    vRtrLdpNgSessIPv6P2MPFecOLSent   TruthValue,
    vRtrLdpNgSessIPv4P2MPFecOLRecv   TruthValue,
    vRtrLdpNgSessIPv6P2MPFecOLRecv   TruthValue,
    vRtrLdpNgSessSvcFec128OLoadSent  TruthValue,
    vRtrLdpNgSessSvcFec128OLoadRecv  TruthValue,
    vRtrLdpNgSessSvcFec129OLoadSent  TruthValue,
    vRtrLdpNgSessSvcFec129OLoadRecv  TruthValue,
    vRtrLdpNgSessLocalIPv4PfxFecCap  TruthValue,
    vRtrLdpNgSessPeerIPv4PfxFecCap   TruthValue,
    vRtrLdpNgSessLocalIPv6PfxFecCap  TruthValue,
    vRtrLdpNgSessPeerIPv6PfxFecCap   TruthValue,
    vRtrLdpNgSessLocalSvcFec128Cap   TruthValue,
    vRtrLdpNgSessPeerSvcFec128Cap    TruthValue,
    vRtrLdpNgSessLocalSvcFec129Cap   TruthValue,
    vRtrLdpNgSessPeerSvcFec129Cap    TruthValue,
    vRtrLdpNgSessOperMaxFecThreshold Unsigned32,
    vRtrLdpNgSessPeerCapRecv         BITS,
    vRtrLdpNgSessLocalUnregNotiCap   TruthValue,
    vRtrLdpNgSessPeerUnregNotiCap    TruthValue,
    vRtrLdpNgSessEndOfLibSent        BITS,
    vRtrLdpNgSessEndOfLibRecv        BITS,
    vRtrLdpNgSessCommunity           TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessLsrIdAdvert         TruthValue,
    vRtrLdpNgSessGRState             INTEGER
}

vRtrLdpNgSessLocalLdpIdType      OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalLdpIdType indicates the local LDP
         identifier type for the LDP session indicated by
         vRtrLdpNgSessLocalLdpId."
    ::= { vRtrLdpNgSessionEntry 1 }

vRtrLdpNgSessLocalLdpId          OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdentifier (SIZE (6|18))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalLdpId indicates the local LDP
         identifier for this LDP session."
    ::= { vRtrLdpNgSessionEntry 2 }

vRtrLdpNgSessEntityIndex         OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessEntityIndex indicates the Entity index for
         the LDP entity represented in this session."
    ::= { vRtrLdpNgSessionEntry 3 }

vRtrLdpNgSessLabelDistMethod     OBJECT-TYPE
    SYNTAX      TmnxLdpLabelDistMethod
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLabelDistMethod indicates the label
         distribution method used for this LDP session."
    ::= { vRtrLdpNgSessionEntry 4 }

vRtrLdpNgSessLoopDetectForPV     OBJECT-TYPE
    SYNTAX      INTEGER {
        disabled (0),
        enabled  (1)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLoopDetectForPV indicates whether loop
         detection based on path vectors is disabled or enabled for this LDP
         session.

         If this object has a value of disabled(0), then loop detection
         is disabled.  Otherwise, if this object has a value of enabled(1),
         then loop detection based on path vectors is enabled."
    ::= { vRtrLdpNgSessionEntry 5 }

vRtrLdpNgSessPathVectorLimit     OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "If the value of vRtrLdpNgSessLoopDetectForPV for this entry is
         'enabled', then the value of vRtrLdpNgSessPathVectorLimit represents
         the Path Vector Limit for this LDP Session.

         If the value of vRtrLdpNgSessLoopDetectForPV for this entry is
         'disabled', then the value of vRtrLdpNgSessPathVectorLimit be 0
         (zero)."
    ::= { vRtrLdpNgSessionEntry 6 }

vRtrLdpNgSessState               OBJECT-TYPE
    SYNTAX      INTEGER {
        nonexistent (1),
        initialized (2),
        openrec     (3),
        opensent    (4),
        operational (5)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessState indicates the current state of the LDP
         session. All of the states 1 - 5 are based on the state machine for
         session negotiation behavior."
    ::= { vRtrLdpNgSessionEntry 7 }

vRtrLdpNgSessAdjacencyType       OBJECT-TYPE
    SYNTAX      TmnxLdpAdjacencyType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessAdjacencyType indicates the adjacency
         type(s) supporting this LDP Session."
    ::= { vRtrLdpNgSessionEntry 8 }

vRtrLdpNgSessProtocolVersion     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessProtocolVersion indicates the version of the
         LDP Protocol used by this session."
    ::= { vRtrLdpNgSessionEntry 9 }

vRtrLdpNgSessLocalUdpPort        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalUdpPort indicates the UDP port used
         locally for LDP discovery."
    ::= { vRtrLdpNgSessionEntry 10 }

vRtrLdpNgSessPeerUdpPort         OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerUdpPort indicates the UDP port used on
         the remote end for LDP discovery."
    ::= { vRtrLdpNgSessionEntry 11 }

vRtrLdpNgSessLocalTcpPort        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalTcpPort indicates the TCP port used
         locally for the LDP Session."
    ::= { vRtrLdpNgSessionEntry 12 }

vRtrLdpNgSessPeerTcpPort         OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerTcpPort indicates the TCP port used on
         the remote end for the LDP Session."
    ::= { vRtrLdpNgSessionEntry 13 }

vRtrLdpNgSessLocalAddrType       OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalAddrType indicates the type of address
         indicated by vRtrLdpNgSessLocalAddress."
    ::= { vRtrLdpNgSessionEntry 14 }

vRtrLdpNgSessLocalAddress        OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalAddress indicates the IP address used
         locally for the LDP Session."
    ::= { vRtrLdpNgSessionEntry 15 }

vRtrLdpNgSessPeerAddrType        OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerAddrType indicates the type of address
         indicated by vRtrLdpNgSessPeerAddress."
    ::= { vRtrLdpNgSessionEntry 16 }

vRtrLdpNgSessPeerAddress         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerAddress indicates the IP address used on
         the remote end for the LDP Session."
    ::= { vRtrLdpNgSessionEntry 17 }

vRtrLdpNgSessKAHoldTimeRemaining OBJECT-TYPE
    SYNTAX      TimeInterval
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessKAHoldTimeRemaining indicates the keep alive
         hold time remaining for this LDP session."
    ::= { vRtrLdpNgSessionEntry 18 }

vRtrLdpNgSessMaxPduLength        OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessMaxPduLength indicates the maximum allowable
         length for LDP PDUs for this session. This value may have been
         negotiated during Session Initialization."
    ::= { vRtrLdpNgSessionEntry 19 }

vRtrLdpNgSessUpTime              OBJECT-TYPE
    SYNTAX      TimeInterval
    UNITS       "centiseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessUpTime indicates the time since the session
         was established."
    ::= { vRtrLdpNgSessionEntry 20 }

vRtrLdpNgSessLocalKATimeout      OBJECT-TYPE
    SYNTAX      TmnxLdpNewKeepAliveTimeout
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalKATimeout indicates the keepalive
         timeout used locally for the LDP Session."
    ::= { vRtrLdpNgSessionEntry 21 }

vRtrLdpNgSessPeerKATimeout       OBJECT-TYPE
    SYNTAX      TmnxLdpNewKeepAliveTimeout
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerKATimeout indicates the keepalive
         timeout used at the remote end of the LDP Session."
    ::= { vRtrLdpNgSessionEntry 22 }

vRtrLdpNgSessAdvertise           OBJECT-TYPE
    SYNTAX      INTEGER {
        address           (1),
        service           (2),
        addressAndService (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessAdvertise indicates the type of FECs that
         will be transported by the session."
    ::= { vRtrLdpNgSessionEntry 23 }

vRtrLdpNgSessLclGRHelperState    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLclGRHelperState indicates whether the local
         entity of this session is graceful restart helper capable or not."
    ::= { vRtrLdpNgSessionEntry 24 }

vRtrLdpNgSessPeerGRState         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerGRState indicates whether the peer
         entity of this session is capable of supporting graceful restart."
    ::= { vRtrLdpNgSessionEntry 25 }

vRtrLdpNgSessPeerNumRestart      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerNumRestart indicates the number of times
         graceful restart helper was initiated for this session."
    ::= { vRtrLdpNgSessionEntry 26 }

vRtrLdpNgSessLastRestartTime     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLastRestartTime indicates the last time
         graceful restart helper was initiated."
    ::= { vRtrLdpNgSessionEntry 27 }

vRtrLdpNgSessLocalFtReconTime    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalFtReconTime indicates the session's
         local entity Fault Tolerant(FT) Reconnect Timeout."
    ::= { vRtrLdpNgSessionEntry 28 }

vRtrLdpNgSessPeerFtReconTime     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerFtReconTime indicates the session's peer
         entity Fault Tolerant(FT) Reconnect Timeout."
    ::= { vRtrLdpNgSessionEntry 29 }

vRtrLdpNgSessLocalFtRecovTime    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalFtRecovTime indicates the session's
         local entity Fault Tolerant(FT) recovery timeout."
    ::= { vRtrLdpNgSessionEntry 30 }

vRtrLdpNgSessPeerFtRecovTime     OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerFtRecovTime indicates the session's peer
         entity Fault Tolerant(FT) recovery timeout."
    ::= { vRtrLdpNgSessionEntry 31 }

vRtrLdpNgSessFtReconTimeRem      OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessFtReconTimeRem indicates the amount of time
         left before session's Fault Tolerant(FT) reconnect timeout expires.
         This value is set to lesser of the neighbor advertised FT recovery
         timeout, vRtrLdpNgSessPeerFtRecovTime and the local recovery timeout,
         vRtrLdpNgSessLocalFtRecovTime."
    ::= { vRtrLdpNgSessionEntry 32 }

vRtrLdpNgSessFtRecovTimeRem      OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessFtRecovTimeRem indicates the amount of time
         left before session's Fault Tolerant(FT) recovery timeout expires.
         This value is set to lesser of the neighbor advertised FT recovery
         timeout, vRtrLdpNgSessPeerFtRecovTime and the local recovery timeout,
         vRtrLdpNgSessLocalFtRecovTime."
    ::= { vRtrLdpNgSessionEntry 33 }

vRtrLdpNgSessBfdStatus           OBJECT-TYPE
    SYNTAX      INTEGER {
        noService    (1),
        inService    (2),
        outOfService (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessBfdStatus indicates the BFD operational
         status for the LDP session.

         If the value of vRtrLdpNgSessBfdStatus is 'noService', BFD is not
         enabled for the LDP session. If the value of the object is
         'outOfService', BFD is enabled but it is down and not running. If the
         value of object is 'inService', BFD is enabled and it is running."
    ::= { vRtrLdpNgSessionEntry 34 }

vRtrLdpNgSessLocalP2MPCap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalP2MPCap indicates whether the local
         entity of this session is capable of exchanging P2MP FECs."
    ::= { vRtrLdpNgSessionEntry 35 }

vRtrLdpNgSessPeerP2MPCap         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerP2MPCap indicates whether the peer
         entity of this session is capable of exchanging P2MP FECs."
    ::= { vRtrLdpNgSessionEntry 36 }

vRtrLdpNgSessLocalMPMBBCap       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalMPMBBCap indicates whether the local
         entity of this session is capable of Multipoint MBB."
    ::= { vRtrLdpNgSessionEntry 37 }

vRtrLdpNgSessPeerMPMBBCap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerMPMBBCap indicates whether the peer
         entity of this session is capable of Multipoint MBB."
    ::= { vRtrLdpNgSessionEntry 38 }

vRtrLdpNgSessLocalDynCap         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalDynCap indicates whether the local
         entity of this session supports negotiation of LDP session
         capabilities dynamically."
    ::= { vRtrLdpNgSessionEntry 39 }

vRtrLdpNgSessPeerDynCap          OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerDynCap indicates whether the peer entity
         of this session supports negotiation of LDP session capabilities
         dynamically."
    ::= { vRtrLdpNgSessionEntry 40 }

vRtrLdpNgSessLocalOLoadCap       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalOLoadCap indicates whether the local
         entity of this session is capable of signaling LSR Overload
         Notification."
    ::= { vRtrLdpNgSessionEntry 41 }

vRtrLdpNgSessPeerOLoadCap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerOLoadCap indicates whether the peer
         entity of this session is capable of signaling LSR Overload
         Notification."
    ::= { vRtrLdpNgSessionEntry 42 }

vRtrLdpNgSessIPv4PfxFecOLoadSent OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessIPv4PfxFecOLoadSent indicates whether LSR
         Overload Notification has been sent to the LDP peer for IPv4 Prefix
         FEC Type.

         The value of 'true' indicates that Local LSR has set the LDP session
         as overloaded for IPv4 Prefix FEC type and is not ready to receive new
         Label Mappings for IPv4 Prefix FEC Type. In this state if a Label
         Mapping Message is received from peer for any IPv4 Prefix FEC type
         then the Label is returned with a Label Release Message."
    ::= { vRtrLdpNgSessionEntry 43 }

vRtrLdpNgSessIPv6PfxFecOLoadSent OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessIPv6PfxFecOLoadSent indicates whether LSR
         Overload Notification has been sent to the LDP peer for IPv6 Prefix
         FEC Type.

         The value of 'true' indicates that Local LSR has set the LDP session
         as overloaded for IPv6 Prefix FEC type and is not ready to receive new
         Label Mappings for IPv6 Prefix FEC Type. In this state if a Label
         Mapping Message is received from peer for any IPv6 Prefix FEC type
         then the Label is returned with a Label Release Message."
    ::= { vRtrLdpNgSessionEntry 44 }

vRtrLdpNgSessIPv4PfxFecOLoadRecv OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessIPv4PfxFecOLoadRecv indicates whether LSR
         Overload Notification has been received from the LDP peer for IPv4
         Prefix FEC Type.

         The value of 'true' indicates that Peer LSR has set the LDP session as
         overloaded for IPv4 Prefix FEC type and is not ready to receive new
         Label Mappings for any IPv4 Prefix FEC Type. In this state no new
         Label Mapping Message would be sent to peer for any IPv4 Prefix FEC
         Type."
    ::= { vRtrLdpNgSessionEntry 45 }

vRtrLdpNgSessIPv6PfxFecOLoadRecv OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessIPv6PfxFecOLoadRecv indicates whether LSR
         Overload Notification has been received from the LDP peer for IPv6
         Prefix FEC Type.

         The value of 'true' indicates that Peer LSR has set the LDP session as
         overloaded for IPv6 Prefix FEC type and is not ready to receive new
         Label Mappings for any IPv6 Prefix FEC Type. In this state no new
         Label Mapping Message would be sent to peer for any IPv6 Prefix FEC
         Type."
    ::= { vRtrLdpNgSessionEntry 46 }

vRtrLdpNgSessIPv4P2MPFecOLSent   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessIPv4P2MPFecOLSent indicates whether LSR
         Overload Notification has been sent to the LDP peer for IPv4 P2MP FEC
         Type.

         The value of 'true' indicates that Local LSR has set the LDP session
         as overloaded for IPv4 P2MP FEC type and is not ready to receive new
         Label Mappings for IPv4 P2MP FEC Type. In this state if a Label
         Mapping Message is received from peer for IPv4 P2MP FEC type then the
         Label is returned with a Label Release Message."
    ::= { vRtrLdpNgSessionEntry 47 }

vRtrLdpNgSessIPv6P2MPFecOLSent   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessIPv6P2MPFecOLSent indicates whether LSR
         Overload Notification has been sent to the LDP peer for IPv6 P2MP FEC
         Type.

         The value of 'true' indicates that Local LSR has set the LDP session
         as overloaded for IPv6 P2MP FEC type and is not ready to receive new
         Label Mappings for IPv6 P2MP FEC Type. In this state if a Label
         Mapping Message is received from peer for IPv6 P2MP FEC type then the
         Label is returned with a Label Release Message."
    ::= { vRtrLdpNgSessionEntry 48 }

vRtrLdpNgSessIPv4P2MPFecOLRecv   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessIPv4P2MPFecOLRecv indicates whether LSR
         Overload Notification has been received from the LDP peer for IPv4
         P2MP FEC Type.

         The value of 'true' indicates that Peer LSR has set the LDP session as
         overloaded for IPv4 P2MP FEC type and is not ready to receive new
         Label Mappings for IPv4 P2MP FEC Type. In this state no new Label
         Mapping Message would be sent to peer for IPv4 P2MP FEC Type."
    ::= { vRtrLdpNgSessionEntry 49 }

vRtrLdpNgSessIPv6P2MPFecOLRecv   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessIPv6P2MPFecOLRecv indicates whether LSR
         Overload Notification has been received from the LDP peer for IPv6
         P2MP FEC Type.

         The value of 'true' indicates that Peer LSR has set the LDP session as
         overloaded for IPv6 P2MP FEC type and is not ready to receive new
         Label Mappings for IPv6 P2MP FEC Type. In this state no new Label
         Mapping Message would be sent to peer for IPv6 P2MP FEC Type."
    ::= { vRtrLdpNgSessionEntry 50 }

vRtrLdpNgSessSvcFec128OLoadSent  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessSvcFec128OLoadSent indicates whether LSR
         Overload Notification has been sent to the LDP peer for Service FEC
         128 Type.

         The value of 'true' indicates that Local LSR has set the LDP session
         as overloaded for Service FEC 128 type and is not ready to receive new
         Label Mappings for Service FEC 128 Type. In this state if a Label
         Mapping Message is received from peer for Service FEC 128 type then
         the Label is returned with a Label Release Message."
    ::= { vRtrLdpNgSessionEntry 51 }

vRtrLdpNgSessSvcFec128OLoadRecv  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessSvcFec128OLoadRecv indicates whether LSR
         Overload Notification has been received from the LDP peer for Service
         FEC 128 Type.

         The value of 'true' indicates that Peer LSR has set the LDP session as
         overloaded for Service FEC 128 type and is not ready to receive new
         Label Mappings for Service FEC 128 Type. In this state no new Label
         Mapping Message would be sent to peer for any Service FEC 128 Type."
    ::= { vRtrLdpNgSessionEntry 52 }

vRtrLdpNgSessSvcFec129OLoadSent  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessSvcFec129OLoadSent indicates whether LSR
         Overload Notification has been sent to the LDP peer for Service FEC
         129 Type.

         The value of 'true' indicates that Local LSR has set the LDP session
         as overloaded for Service FEC 129 type and is not ready to receive new
         Label Mappings for any Service FEC 129 Type. In this state if a Label
         Mapping Message is received from peer for Service FEC 129 type then
         the Label is returned with a Label Release Message."
    ::= { vRtrLdpNgSessionEntry 53 }

vRtrLdpNgSessSvcFec129OLoadRecv  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessSvcFec129OLoadRecv indicates whether LSR
         Overload Notification has been received from the LDP peer for Service
         FEC 129 Type.

         The value of 'true' indicates that Peer LSR has set the LDP session as
         overloaded for Service FEC 129 type and is not ready to receive new
         Label Mappings for any Service FEC 129 Type. In this state no new
         Label Mapping Message would be sent to peer for any Service FEC 129
         Type."
    ::= { vRtrLdpNgSessionEntry 54 }

vRtrLdpNgSessLocalIPv4PfxFecCap  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalIPv4PfxFecCap indicates whether the
         local entity of this session is capable of exchanging IPv4 FECs."
    ::= { vRtrLdpNgSessionEntry 55 }

vRtrLdpNgSessPeerIPv4PfxFecCap   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerIPv4PfxFecCap indicates whether the
         peer entity of this session is capable of exchanging IPv4 FECs.
         When the 'ipv4PfxFec' bit is not set in vRtrLdpNgSessPeerCapRecv, this
         will  be 'true'. Otherwise, it will be the value sent by the peer LSR."
    ::= { vRtrLdpNgSessionEntry 56 }

vRtrLdpNgSessLocalIPv6PfxFecCap  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalIPv6PfxFecCap indicates whether the
         local entity of this session is capable of exchanging IPv6 FECs."
    ::= { vRtrLdpNgSessionEntry 57 }

vRtrLdpNgSessPeerIPv6PfxFecCap   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerIPv6PfxFecCap indicates whether the peer
         entity of this session is capable of exchanging IPv6 FECs. When the
         'ipv6PfxFec' bit is not set in vRtrLdpNgSessPeerCapRecv, this will be
         'true'. Otherwise, it will be the value sent by the peer LSR."
    ::= { vRtrLdpNgSessionEntry 58 }

vRtrLdpNgSessLocalSvcFec128Cap   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalSvcFec128Cap indicates whether the
         local entity of this session is capable of exchanging PW ID FECs."
    ::= { vRtrLdpNgSessionEntry 59 }

vRtrLdpNgSessPeerSvcFec128Cap    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerSvcFec128Cap indicates whether the peer
         entity of this session is capable of exchanging PW ID FECs. When the
         'fec128' bit is not set in vRtrLdpNgSessPeerCapRecv, this will be
         'true'. Otherwise, it will be the value sent by the peer LSR."
    ::= { vRtrLdpNgSessionEntry 60 }

vRtrLdpNgSessLocalSvcFec129Cap   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalSvcFec129Cap indicates whether the
         local entity of this session is capable of exchanging General PW ID
         FECs."
    ::= { vRtrLdpNgSessionEntry 61 }

vRtrLdpNgSessPeerSvcFec129Cap    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerSvcFec129Cap indicates whether the peer
         entity of this session is capable of exchanging General PW ID FECs
         over the session. When the 'fec129' bit is not set in
         vRtrLdpNgSessPeerCapRecv, this will be 'true'. Otherwise, it will be
         the value sent by the peer LSR."
    ::= { vRtrLdpNgSessionEntry 62 }

vRtrLdpNgSessOperMaxFecThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        " The value of vRtrLdpNgSessOperMaxFecThreshold indicates the
         operational percentage of vRtrLdpNgSessParamMaxFec. "
    ::= { vRtrLdpNgSessionEntry 63 }

vRtrLdpNgSessPeerCapRecv         OBJECT-TYPE
    SYNTAX      BITS {
        ipv4PfxFec (0),
        ipv6PfxFec (1),
        fec128     (2),
        fec129     (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerCapRecv indicates various capabilities
         signaled by the peer LSR. A particular capability bit will be set to 1
         when there is at least one capability message sent by peer LSR for a
         given capability type."
    ::= { vRtrLdpNgSessionEntry 64 }

vRtrLdpNgSessLocalUnregNotiCap   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLocalUnregNotiCap indicates whether the
         local entity of this session has sent Unrecognized Notification
         capability to peer."
    ::= { vRtrLdpNgSessionEntry 65 }

vRtrLdpNgSessPeerUnregNotiCap    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeerUnregNotiCap indicates whether the peer
         has sent Unrecognized Notification capability."
    ::= { vRtrLdpNgSessionEntry 66 }

vRtrLdpNgSessEndOfLibSent        OBJECT-TYPE
    SYNTAX      BITS {
        ipv4PfxFec  (0),
        ipv6PfxFec  (1),
        ipv4p2mpFec (2),
        ipv6p2mpFec (3),
        fec128      (4),
        fec129      (5)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessEndOfLibSent indicates whether end of Label
         Information Base (LIB) notification has been send to the LDP peer. A
         particular sent bit will be set to 1 when there is at least one LIB
         notification sent to the LDP peer for a given service type."
    ::= { vRtrLdpNgSessionEntry 67 }

vRtrLdpNgSessEndOfLibRecv        OBJECT-TYPE
    SYNTAX      BITS {
        ipv4PfxFec  (0),
        ipv6PfxFec  (1),
        ipv4p2mpFec (2),
        ipv6p2mpFec (3),
        fec128      (4),
        fec129      (5)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessEndOfLibRecv indicates whether end of Label
         Information Base (LIB) notification has been received from the LDP
         peer. A particular received bit will be set to 1 when there is at
         least one LIB notification received from the LDP peer for a given
         service type."
    ::= { vRtrLdpNgSessionEntry 68 }

vRtrLdpNgSessCommunity           OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Contains the FEC community data "
    ::= { vRtrLdpNgSessionEntry 69 }

vRtrLdpNgSessLsrIdAdvert         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessLsrIdAdvert indicates whether or not the
         local router is advertising the local-lsr-id of this session as a FEC
         because of adv-local-lsr-id configuration linked to this session."
    ::= { vRtrLdpNgSessionEntry 70 }

vRtrLdpNgSessGRState             OBJECT-TYPE
    SYNTAX      INTEGER {
        none      (1),
        reconnect (2),
        recovery  (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessGRState indicates the current GR state of
         the LDP session."
    ::= { vRtrLdpNgSessionEntry 71 }

vRtrLdpNgTargPeerTunlLspTblLstCh OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerTunlLspTblLstCh indicates the last
         timestamp when an entry in the vRtrLdpNgTargPeerTunnelLspTable was
         last changed."
    ::= { tmnxLdpNgObjs 5 }

vRtrLdpNgTargPeerTunnelLspTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgTargPeerTunnelLspEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgTargPeerTunnelLspTable keeps the list of LDP-over-RSVP
         LSP ids which are used for the tunneling of unicast FECs.

         Each LSP ID in the list corresponds to the vRtrMplsLspIndex of the
         given MPLS LSP."
    ::= { tmnxLdpNgObjs 6 }

vRtrLdpNgTargPeerTunnelLspEntry  OBJECT-TYPE
    SYNTAX      VRtrLdpNgTargPeerTunnelLspEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table contains the LSP id information about an LDP
         interface or targeted peer.

         Row entry can be only created if there is corresponding targeted peer
         entry in vRtrLdpNgTargPeerTable.

         Row entries can be created or deleted via SNMP SET requests. A row is
         created by setting vRtrLdpNgTargPeerLspRowStatus to 'createAndGo'
         provided the corresponding LSP id exists as an MPLS lsp. A row entry
         can be destroyed by setting vRtrLdpNgTargPeerLspRowStatus to
         'destroy'."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerAddressType,
        vRtrLdpNgPeerAddress,
        vRtrLdpNgTargPeerLspId
    }
    ::= { vRtrLdpNgTargPeerTunnelLspTable 1 }

VRtrLdpNgTargPeerTunnelLspEntry  ::= SEQUENCE
{
    vRtrLdpNgTargPeerLspId           TmnxVRtrMplsLspID,
    vRtrLdpNgTargPeerLspRowStatus    RowStatus
}

vRtrLdpNgTargPeerLspId           OBJECT-TYPE
    SYNTAX      TmnxVRtrMplsLspID (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerLspId specifies the LSP id of the LSP
         associated with the specified interface or targeted peer."
    ::= { vRtrLdpNgTargPeerTunnelLspEntry 1 }

vRtrLdpNgTargPeerLspRowStatus    OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgTargPeerLspRowStatus is used to create, delete or control
         entries in the vRtrLdpNgTargPeerTunnelLspTable.

         An entry is created by setting vRtrLdpNgTargPeerLspRowStatus to
         'createAndGo'.

         An entry is deleted by setting vRtrLdpNgTargPeerLspRowStatus to
         'destroy'."
    ::= { vRtrLdpNgTargPeerTunnelLspEntry 2 }

vRtrLdpNgSessionParamsTableLstCh OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessionParamsTableLstCh indicates the last
         timestamp when an entry in the vRtrLdpNgSessionParamsTable was last
         changed."
    ::= { tmnxLdpNgObjs 7 }

vRtrLdpNgSessionParamsTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgSessionParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgSessionParamsTable is used to configure parameters
         applicable to an LDP session."
    ::= { tmnxLdpNgObjs 8 }

vRtrLdpNgSessionParamsEntry      OBJECT-TYPE
    SYNTAX      VRtrLdpNgSessionParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an LDP session to a far end peer.

         Row entries can be created or deleted via SNMP SET requests. A row
         with default attribute values is created by setting
         vRtrLdpNgSessParamRowStatus to 'createAndGo'. A row entry can be
         destroyed by setting vRtrLdpNgSessParamRowStatus to 'destroy'."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerAddressType,
        vRtrLdpNgPeerAddress
    }
    ::= { vRtrLdpNgSessionParamsTable 1 }

VRtrLdpNgSessionParamsEntry      ::= SEQUENCE
{
    vRtrLdpNgSessParamRowStatus      RowStatus,
    vRtrLdpNgSessParamDODLblDistrib  TruthValue,
    vRtrLdpNgSessParamImportPolicy1  TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamImportPolicy2  TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamImportPolicy3  TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamImportPolicy4  TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamImportPolicy5  TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamExportPolicy1  TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamExportPolicy2  TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamExportPolicy3  TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamExportPolicy4  TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamExportPolicy5  TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessFec129CiscoInterop  TruthValue,
    vRtrLdpNgSessParamAdvAdjAddrOnly TruthValue,
    vRtrLdpNgSessPeIDMacFlushInterop TruthValue,
    vRtrLdpNgSessParamIPv4PfxFecCap  TmnxEnabledDisabled,
    vRtrLdpNgSessParamIPv6PfxFecCap  TmnxEnabledDisabled,
    vRtrLdpNgSessParamP2MPFecCap     TmnxEnabledDisabled,
    vRtrLdpNgSessParamMaxFec         Unsigned32,
    vRtrLdpNgSessParamMaxFecLogOnly  TruthValue,
    vRtrLdpNgSessParamMaxFecThold    Unsigned32,
    vRtrLdpNgSessParamAddrExpPolicy1 TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamAddrExpPolicy2 TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamAddrExpPolicy3 TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamAddrExpPolicy4 TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamAddrExpPolicy5 TPolicyStatementNameOrEmpty,
    vRtrLdpNgSessParamAdvert         TruthValue,
    vRtrLdpNgSessParamCommunity      TPolicyStatementNameOrEmpty
}

vRtrLdpNgSessParamRowStatus      OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgSessParamRowStatus is used to control the creation and
         deletion of rows in the vRtrLdpNgSessionParamsTable.

         A row can be created by setting vRtrLdpNgSessParamRowStatus to
         'createAndGo'. The agent should assign the default attribute values
         and change the row status to 'active'.

         A row entry can be destroyed by setting vRtrLdpNgSessParamRowStatus to
         'destroy'."
    ::= { vRtrLdpNgSessionParamsEntry 1 }

vRtrLdpNgSessParamDODLblDistrib  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamDODLblDistrib specifies whether or not
         Downstream-On-Demand (DOD) has been enabled for the LDP session. When
         the value is set to 'true' DOD is enabled for the LDP session."
    DEFVAL      { false }
    ::= { vRtrLdpNgSessionParamsEntry 4 }

vRtrLdpNgSessParamImportPolicy1  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamImportPolicy1 specifies the first
         import policy used to determine which prefix FECs received from
         specified LDP or TLDP peer should be used for resolution."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 5 }

vRtrLdpNgSessParamImportPolicy2  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamImportPolicy2 specifies the second
         import policy used to determine which prefix FECs received from
         specified LDP or TLDP peer should be used for resolution."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 6 }

vRtrLdpNgSessParamImportPolicy3  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamImportPolicy3 specifies the third
         import policy used to determine which prefix FECs received from
         specified LDP or TLDP peer should be used for resolution."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 7 }

vRtrLdpNgSessParamImportPolicy4  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamImportPolicy4 specifies the fourth
         import policy used to determine which prefix FECs received from
         specified LDP or TLDP peer should be used for resolution."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 8 }

vRtrLdpNgSessParamImportPolicy5  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamImportPolicy5 specifies the fifth
         import policy used to determine which prefix FECs received from
         specified LDP or TLDP peer should be used for resolution."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 9 }

vRtrLdpNgSessParamExportPolicy1  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamExportPolicy1 specifies the first
         export policy used to determine which prefix FECs should be
         distributed to the specified LDP or TLDP peer."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 10 }

vRtrLdpNgSessParamExportPolicy2  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamExportPolicy2 specifies the second
         export policy used to determine which prefix FECs should be
         distributed to the specified LDP or TLDP peer."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 11 }

vRtrLdpNgSessParamExportPolicy3  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamExportPolicy3 specifies the third
         export policy used to determine which prefix FECs should be
         distributed to the specified LDP or TLDP peer."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 12 }

vRtrLdpNgSessParamExportPolicy4  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamExportPolicy4 specifies the fourth
         export policy used to determine which prefix FECs should be
         distributed to the specified LDP or TLDP peer."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 13 }

vRtrLdpNgSessParamExportPolicy5  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamExportPolicy5 specifies the fifth
         export policy used to determine which prefix FECs should be
         distributed to the specified LDP or TLDP peer."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 14 }

vRtrLdpNgSessFec129CiscoInterop  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessFec129CiscoInterop specifies whether LDP
         will provide translation between non-compliant FEC 129 formats of
         Cisco.

         Peer LDP sessions must be manually configured towards the
         non-compliant Cisco PEs.

         When the value of vRtrLdpNgSessFec129CiscoInterop is 'true', Cisco
         non-compliant format will be used to send and interpret received Label
         Release messages i.e. the FEC129 SAII and TAII fields will be
         reversed.

         When the value of vRtrLdpNgSessFec129CiscoInterop is 'false', Cisco
         non-compliant format will not be used or supported."
    DEFVAL      { false }
    ::= { vRtrLdpNgSessionParamsEntry 15 }

vRtrLdpNgSessParamAdvAdjAddrOnly OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamAdvAdjAddrOnly specifies whether to
         only distribute the local addresses used by hello adjacencies with
         this LDP peer.

         When the value is SET to 'true', local addresses that are used by
         hello adjacencies with this LDP peer are only distributed to the peer
         session . When the value is SET to 'false', all known local addresses
         are distributed to the peer session"
    DEFVAL      { false }
    ::= { vRtrLdpNgSessionParamsEntry 16 }

vRtrLdpNgSessPeIDMacFlushInterop OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessPeIDMacFlushInterop specifies whether
         LDP will react to and send the non-standard  PE-ID TLV (type 0x405) in
         an address withdraw message to effect 'flush-all-from-me' behavior. It
         is used to provide interoperability with other vendors that use this
         TLV for the MAC flush mechanism. Only FEC type 128 is currently
         supported.

         Peer LDP sessions must be manually configured towards the PEs
         requiring support for this TLV.

         When the value of vRtrLdpNgSessPeIDMacFlushInterop is set to 'true',
         the receipt of an address withdraw message with empty MAC list
         including the non-standard TLV will trigger 'flush-all-from-me'
         behavior instead of the normal 'flush-all-but-mine'. The TLV will be
         included in any forwarding towards like-configured peers.

         When the value of vRtrLdpNgSessPeIDMacFlushInterop is set to 'false',
         the non-standard TLV will be ignored and will not be included in any
         address withdraw messages sent to the peer."
    DEFVAL      { false }
    ::= { vRtrLdpNgSessionParamsEntry 17 }

vRtrLdpNgSessParamIPv4PfxFecCap  OBJECT-TYPE
    SYNTAX      TmnxEnabledDisabled
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamIPv4PfxFecCap specifies whether IPv4
         prefix FECs can be exchanged over this session"
    DEFVAL      { enabled }
    ::= { vRtrLdpNgSessionParamsEntry 18 }

vRtrLdpNgSessParamIPv6PfxFecCap  OBJECT-TYPE
    SYNTAX      TmnxEnabledDisabled
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamIPv6PfxFecCap specifies whether IPv6
         prefix FECs can be exchanged over this session"
    DEFVAL      { enabled }
    ::= { vRtrLdpNgSessionParamsEntry 19 }

vRtrLdpNgSessParamP2MPFecCap     OBJECT-TYPE
    SYNTAX      TmnxEnabledDisabled
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamP2MPFecCap specifies whether P2MP FECs
         can be exchanged over this session"
    DEFVAL      { enabled }
    ::= { vRtrLdpNgSessionParamsEntry 20 }

vRtrLdpNgSessParamMaxFec         OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 1..4294967295)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        " The value of vRtrLdpNgSessParamMaxFec specifies the maximum number of
         FECs that will be accepted from this peer LSR.

         A value of zero specifies there is no limit to the number of FECs
         accepted from this peer LSR.

         The vRtrLdpNgSessMaxFecThresChanged notification is sent when the
         number of FECs receive from this peer LSR exceeds a percentage of this
         limit as specified by vRtrLdpPeerMaxFecThreshold.

         Furthermore, once the limit is exhausted, following actions are taken
         if vRtrLdpNgSessParamMaxFecLogOnly has value of 'false'.

         (1) If LSR Overload capability is supported, this LSR will follow the
             LSR Overload procedure.

         (2) If LSR Overload capability is not supported, any further Label
             Mapping Message is returned with Label Release Message with LDP
             status code 'No_Label_Resources'. "
    DEFVAL      { 0 }
    ::= { vRtrLdpNgSessionParamsEntry 21 }

vRtrLdpNgSessParamMaxFecLogOnly  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        " The value of vRtrLdpNgSessParamMaxFecLogOnly specifies whether to only
         generate vRtrLdpNgSessMaxFecThresChanged notification or take further
         action when FECs received exceeds vRtrLdpNgSessParamMaxFec limit.

         When this value is set to 'false', trap will be generated and one of
         the following action is taken:

         (1) If LSR Overload capability is supported, this LSR will follow the
             LSR Overload procedure.

         (2) If LSR Overload capability is not supported, any further Label
             Mapping Message is returned with Label Release Message with LDP
             status code 'No_Label_Resources'.

         When this value is set to 'true', trap will be generated only. "
    DEFVAL      { false }
    ::= { vRtrLdpNgSessionParamsEntry 22 }

vRtrLdpNgSessParamMaxFecThold    OBJECT-TYPE
    SYNTAX      Unsigned32 (1..100)
    UNITS       "percent"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        " The value of vRtrLdpNgSessParamMaxFecThold specifies a percentage of
         vRtrLdpNgSessParamMaxFec. "
    DEFVAL      { 90 }
    ::= { vRtrLdpNgSessionParamsEntry 23 }

vRtrLdpNgSessParamAddrExpPolicy1 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamAddrExpPolicy1 specifies the first
         export policy used to determine which local addresses should be
         distributed to this peer."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 24 }

vRtrLdpNgSessParamAddrExpPolicy2 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamAddrExpPolicy2 specifies the second
         export policy used to determine which local addresses should be
         distributed to this peer."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 25 }

vRtrLdpNgSessParamAddrExpPolicy3 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamAddrExpPolicy3 specifies the third
         export policy used to determine which local addresses should be
         distributed to this peer."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 26 }

vRtrLdpNgSessParamAddrExpPolicy4 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamAddrExpPolicy4 specifies the fourth
         export policy used to determine which local addresses should be
         distributed to this peer."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 27 }

vRtrLdpNgSessParamAddrExpPolicy5 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamAddrExpPolicy5 specifies the fifth
         export policy used to determine which local addresses should be
         distributed to this peer."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 28 }

vRtrLdpNgSessParamAdvert         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamAdvert specifies whether or not
         advertisement of a local-LSR ID is sent over a given session"
    DEFVAL      { false }
    ::= { vRtrLdpNgSessionParamsEntry 29 }

vRtrLdpNgSessParamCommunity      OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessParamCommunity defines a community string
         associated with a session to a given peer"
    DEFVAL      { ''H }
    ::= { vRtrLdpNgSessionParamsEntry 30 }

vRtrLdpNgSessionAddrTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgSessionAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgSessionInAddrTable is a read-only table that represents
         all local addresses either sent to or received from an LDP peer for a
         single session between an LDP entity and an LDP Peer."
    ::= { tmnxLdpNgObjs 9 }

vRtrLdpNgSessionAddrEntry        OBJECT-TYPE
    SYNTAX      VRtrLdpNgSessionAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of all local addresses sent to
         or received from an LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId
    }
    ::= { vRtrLdpNgSessionAddrTable 1 }

VRtrLdpNgSessionAddrEntry        ::= SEQUENCE
{
    vRtrLdpNgSessAddrLclLdpIdType    TmnxMplsLdpNgIdType,
    vRtrLdpNgSessionAddrLocalLdpId   TmnxMplsLdpNgIdentifier,
    vRtrLdpNgSessionAddrNumInAddrs   Unsigned32,
    vRtrLdpNgSessionAddrNumOutAddrs  Unsigned32
}

vRtrLdpNgSessAddrLclLdpIdType    OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessAddrLclLdpIdType indicates the local LDP
         identifier type for the LDP session indicated by
         vRtrLdpNgSessionAddrLocalLdpId."
    ::= { vRtrLdpNgSessionAddrEntry 1 }

vRtrLdpNgSessionAddrLocalLdpId   OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdentifier (SIZE (6|18))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessionAddrLocalLdpId indicates the local LDP
         identifier for this LDP session."
    ::= { vRtrLdpNgSessionAddrEntry 2 }

vRtrLdpNgSessionAddrNumInAddrs   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessionAddrNumInAddrs indicates the number of
         local addresses that have been received from the peer for this
         session."
    ::= { vRtrLdpNgSessionAddrEntry 3 }

vRtrLdpNgSessionAddrNumOutAddrs  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessionAddrNumOutAddrs indicates the number of
         local addresses that have been sent to the peer for this session."
    ::= { vRtrLdpNgSessionAddrEntry 4 }

vRtrLdpNgSessionInAddrTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgSessionInAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgSessionInAddrTable is a read-only table that represents
         all local addresses received from an LDP peer for a single session
         between an LDP entity and an LDP Peer."
    ::= { tmnxLdpNgObjs 10 }

vRtrLdpNgSessionInAddrEntry      OBJECT-TYPE
    SYNTAX      VRtrLdpNgSessionInAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a local address received from
         an LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vRtrLdpNgSessionInAddrAddrType,
        vRtrLdpNgSessionInAddrAddress
    }
    ::= { vRtrLdpNgSessionInAddrTable 1 }

VRtrLdpNgSessionInAddrEntry      ::= SEQUENCE
{
    vRtrLdpNgSessionInAddrAddrType   InetAddressType,
    vRtrLdpNgSessionInAddrAddress    InetAddress,
    vRtrLdpNgSessInAddrLclLdpIdType  TmnxMplsLdpNgIdType,
    vRtrLdpNgSessionInAddrLocalLdpId TmnxMplsLdpNgIdentifier
}

vRtrLdpNgSessionInAddrAddrType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessionInAddrAddrType indicates the address type
         of vRtrLdpNgSessionInAddrAddress."
    ::= { vRtrLdpNgSessionInAddrEntry 1 }

vRtrLdpNgSessionInAddrAddress    OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessionInAddrAddress indicates the IP address
         received from the peer for this LDP session."
    ::= { vRtrLdpNgSessionInAddrEntry 2 }

vRtrLdpNgSessInAddrLclLdpIdType  OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessInAddrLclLdpIdType indicates the local LDP
         identifier type for the LDP session indicated by
         vRtrLdpNgSessionInAddrLocalLdpId."
    ::= { vRtrLdpNgSessionInAddrEntry 3 }

vRtrLdpNgSessionInAddrLocalLdpId OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdentifier (SIZE (6|18))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessionInAddrLocalLdpId indicates the local LDP
         identifier for this LDP session."
    ::= { vRtrLdpNgSessionInAddrEntry 4 }

vRtrLdpNgSessionOutAddrTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgSessionOutAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgSessionOutAddrTable is a read-only table that represents
         all local addresses sent to an LDP peer for a single session between
         an LDP entity and an LDP Peer."
    ::= { tmnxLdpNgObjs 11 }

vRtrLdpNgSessionOutAddrEntry     OBJECT-TYPE
    SYNTAX      VRtrLdpNgSessionOutAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a local address sent to an
         LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vRtrLdpNgSessionOutAddrAddrType,
        vRtrLdpNgSessionOutAddrAddress
    }
    ::= { vRtrLdpNgSessionOutAddrTable 1 }

VRtrLdpNgSessionOutAddrEntry     ::= SEQUENCE
{
    vRtrLdpNgSessionOutAddrAddrType  InetAddressType,
    vRtrLdpNgSessionOutAddrAddress   InetAddress,
    vRtrLdpNgSessOutAddrLclLdpIdType TmnxMplsLdpNgIdType,
    vRtrLdpNgSessionOutAddrLclLdpId  TmnxMplsLdpNgIdentifier
}

vRtrLdpNgSessionOutAddrAddrType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessionOutAddrAddrType indicates the address
         type of vRtrLdpNgSessionOutAddrAddress."
    ::= { vRtrLdpNgSessionOutAddrEntry 1 }

vRtrLdpNgSessionOutAddrAddress   OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessionOutAddrAddress indicates the IP address
         sent to the peer for this LDP session."
    ::= { vRtrLdpNgSessionOutAddrEntry 2 }

vRtrLdpNgSessOutAddrLclLdpIdType OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessOutAddrLclLdpIdType indicates the local LDP
         identifier type for the LDP session, indicated by
         vRtrLdpNgSessionOutAddrLclLdpId."
    ::= { vRtrLdpNgSessionOutAddrEntry 3 }

vRtrLdpNgSessionOutAddrLclLdpId  OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdentifier (SIZE (6|18))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessionOutAddrLclLdpId indicates the local LDP
         identifier for this LDP session."
    ::= { vRtrLdpNgSessionOutAddrEntry 4 }

vRtrLdpNgAddrFecTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgAddrFecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgAddrFecTable is a read-only table that represents all
         address FECs either sent to or received from an LDP peer known to the
         Virtual Router."
    ::= { tmnxLdpNgObjs 12 }

vRtrLdpNgAddrFecEntry            OBJECT-TYPE
    SYNTAX      VRtrLdpNgAddrFecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of an address FEC sent to or
         received from an LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgAddrFecFecType,
        vRtrLdpNgAddrFecIpPrefixType,
        vRtrLdpNgAddrFecIpPrefix,
        vRtrLdpNgAddrFecIpPrefixLen,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId
    }
    ::= { vRtrLdpNgAddrFecTable 1 }

VRtrLdpNgAddrFecEntry            ::= SEQUENCE
{
    vRtrLdpNgAddrFecFecType          TmnxLdpFECType,
    vRtrLdpNgAddrFecIpPrefixType     InetAddressType,
    vRtrLdpNgAddrFecIpPrefix         InetAddress,
    vRtrLdpNgAddrFecIpPrefixLen      InetAddressPrefixLength,
    vRtrLdpNgAddrFecFlags            TmnxLdpFECFlags,
    vRtrLdpNgAddrFecNumInLabels      Unsigned32,
    vRtrLdpNgAddrFecNumOutLabels     Unsigned32,
    vRtrLdpNgAddrFecCommunity        TPolicyStatementNameOrEmpty
}

vRtrLdpNgAddrFecFecType          OBJECT-TYPE
    SYNTAX      TmnxLdpFECType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecFecType specifies the FEC type."
    ::= { vRtrLdpNgAddrFecEntry 1 }

vRtrLdpNgAddrFecIpPrefixType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecIpPrefixType indicates the address type
         of vRtrLdpNgAddrFecIpPrefix."
    ::= { vRtrLdpNgAddrFecEntry 2 }

vRtrLdpNgAddrFecIpPrefix         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecIpPrefix specifies the IP Address Prefix
         for this address FEC."
    ::= { vRtrLdpNgAddrFecEntry 3 }

vRtrLdpNgAddrFecIpPrefixLen      OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..128)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecIpPrefixLen indicates the prefix length
         of the subnet associated with vRtrLdpNgAddrFecIpPrefix."
    ::= { vRtrLdpNgAddrFecEntry 4 }

vRtrLdpNgAddrFecFlags            OBJECT-TYPE
    SYNTAX      TmnxLdpFECFlags
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The bit flags of vRtrLdpNgAddrFecFlags indicate the characteristics of
         the FEC."
    ::= { vRtrLdpNgAddrFecEntry 5 }

vRtrLdpNgAddrFecNumInLabels      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecNumInLabels indicates the number of
         labels that have been sent to the peer associated with this FEC."
    ::= { vRtrLdpNgAddrFecEntry 6 }

vRtrLdpNgAddrFecNumOutLabels     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecNumOutLabels indicates the number of
         labels that have been received from the peer associated with this FEC."
    ::= { vRtrLdpNgAddrFecEntry 7 }

vRtrLdpNgAddrFecCommunity        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the community value for a FEC "
    ::= { vRtrLdpNgAddrFecEntry 8 }

vRtrLdpNgAddrFecInLblTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgAddrFecInLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgAddrFecInLblTable is a read-only table that represents
         all address FECs sent to an LDP peer known to the Virtual Router."
    ::= { tmnxLdpNgObjs 13 }

vRtrLdpNgAddrFecInLblEntry       OBJECT-TYPE
    SYNTAX      VRtrLdpNgAddrFecInLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of an address FEC sent to an LDP
         peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgAddrFecFecType,
        vRtrLdpNgAddrFecIpPrefixType,
        vRtrLdpNgAddrFecIpPrefix,
        vRtrLdpNgAddrFecIpPrefixLen,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vRtrLdpNgAddrFecInLblId
    }
    ::= { vRtrLdpNgAddrFecInLblTable 1 }

VRtrLdpNgAddrFecInLblEntry       ::= SEQUENCE
{
    vRtrLdpNgAddrFecInLblId          Unsigned32,
    vRtrLdpNgAddrFecInLbl            Unsigned32,
    vRtrLdpNgAddrFecInLblStatus      TmnxLabelStatus,
    vRtrLdpNgAddrFecInLblIfIndex     InterfaceIndexOrZero
}

vRtrLdpNgAddrFecInLblId          OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecInLblId indicates the label number of the
         ingress label exchanged."
    ::= { vRtrLdpNgAddrFecInLblEntry 1 }

vRtrLdpNgAddrFecInLbl            OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecInLbl indicates the ingress label
         exchanged."
    ::= { vRtrLdpNgAddrFecInLblEntry 2 }

vRtrLdpNgAddrFecInLblStatus      OBJECT-TYPE
    SYNTAX      TmnxLabelStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecInLblStatus indicates the status of the
         ingress label."
    ::= { vRtrLdpNgAddrFecInLblEntry 3 }

vRtrLdpNgAddrFecInLblIfIndex     OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecInLblIfIndex indicates the interface
         index for ingress label."
    ::= { vRtrLdpNgAddrFecInLblEntry 4 }

vRtrLdpNgAddrFecOutLblTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgAddrFecOutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgAddrFecOutLblTable is a read-only table that represents
         all address FECs received from an LDP peer known to the Virtual
         Router."
    ::= { tmnxLdpNgObjs 14 }

vRtrLdpNgAddrFecOutLblEntry      OBJECT-TYPE
    SYNTAX      VRtrLdpNgAddrFecOutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of an address FEC received from
         an LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgAddrFecFecType,
        vRtrLdpNgAddrFecIpPrefixType,
        vRtrLdpNgAddrFecIpPrefix,
        vRtrLdpNgAddrFecIpPrefixLen,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vRtrLdpNgAddrFecOutLblId
    }
    ::= { vRtrLdpNgAddrFecOutLblTable 1 }

VRtrLdpNgAddrFecOutLblEntry      ::= SEQUENCE
{
    vRtrLdpNgAddrFecOutLblId         Unsigned32,
    vRtrLdpNgAddrFecOutLbl           Unsigned32,
    vRtrLdpNgAddrFecOutLblStatus     TmnxLabelStatus,
    vRtrLdpNgAddrFecOutLblIfIndex    InterfaceIndexOrZero,
    vRtrLdpNgAddrFecOutLblNHType     InetAddressType,
    vRtrLdpNgAddrFecOutLblNHAddr     InetAddress,
    vRtrLdpNgAddrFecOutLblMetric     Unsigned32,
    vRtrLdpNgAddrFecOutLblMtu        Unsigned32,
    vRtrLdpNgAddrFecOutLblLspId      Unsigned32
}

vRtrLdpNgAddrFecOutLblId         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecOutLblId indicates the label number of
         the egress label exchanged."
    ::= { vRtrLdpNgAddrFecOutLblEntry 1 }

vRtrLdpNgAddrFecOutLbl           OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecOutLbl indicates the egress label
         exchanged"
    ::= { vRtrLdpNgAddrFecOutLblEntry 2 }

vRtrLdpNgAddrFecOutLblStatus     OBJECT-TYPE
    SYNTAX      TmnxLabelStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecOutLblStatus indicates the status of the
         egress label."
    ::= { vRtrLdpNgAddrFecOutLblEntry 3 }

vRtrLdpNgAddrFecOutLblIfIndex    OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecOutLblIfIndex indicates the interface
         index for egress label."
    ::= { vRtrLdpNgAddrFecOutLblEntry 4 }

vRtrLdpNgAddrFecOutLblNHType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecOutLblNHType indicates the address type
         of vRtrLdpNgAddrFecOutLblNHAddr."
    ::= { vRtrLdpNgAddrFecOutLblEntry 5 }

vRtrLdpNgAddrFecOutLblNHAddr     OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecOutLblNHAddr indicates the IP address of
         the next hop for egress label."
    ::= { vRtrLdpNgAddrFecOutLblEntry 6 }

vRtrLdpNgAddrFecOutLblMetric     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecOutLblMetric indicates the relative cost
         of the tunnel represented by this address FEC egress label."
    ::= { vRtrLdpNgAddrFecOutLblEntry 7 }

vRtrLdpNgAddrFecOutLblMtu        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecOutLblMtu indicates the maximum transfer
         unit for payloads represented by this address FEC egress label."
    ::= { vRtrLdpNgAddrFecOutLblEntry 8 }

vRtrLdpNgAddrFecOutLblLspId      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecOutLblLspId indicates the LSP id
         associated with egress label."
    ::= { vRtrLdpNgAddrFecOutLblEntry 9 }

vRtrLdpNgAddrFecMapTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgAddrFecMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgAddrFecMapTable is a read-only table which maps to the
         vRtrLdpNgAddrFecTable. This table has the same indexes as the
         vRtrLdpNgAddrFecTable but the order in which these indexes are
         specified is different for the two tables."
    ::= { tmnxLdpNgObjs 15 }

vRtrLdpNgAddrFecMapEntry         OBJECT-TYPE
    SYNTAX      VRtrLdpNgAddrFecMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of an address FEC sent to or
         received from an LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vRtrLdpNgAddrFecFecType,
        vRtrLdpNgAddrFecIpPrefixType,
        vRtrLdpNgAddrFecIpPrefix,
        vRtrLdpNgAddrFecIpPrefixLen
    }
    ::= { vRtrLdpNgAddrFecMapTable 1 }

VRtrLdpNgAddrFecMapEntry         ::= SEQUENCE
{
    vRtrLdpNgAddrFecMapFlags         TmnxLdpFECFlags,
    vRtrLdpNgAddrFecMapNumInLabels   Unsigned32,
    vRtrLdpNgAddrFecMapNumOutLabels  Unsigned32
}

vRtrLdpNgAddrFecMapFlags         OBJECT-TYPE
    SYNTAX      TmnxLdpFECFlags
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The bit flags of vRtrLdpNgAddrFecMapFlags indicate the characteristics
         of the FEC."
    ::= { vRtrLdpNgAddrFecMapEntry 1 }

vRtrLdpNgAddrFecMapNumInLabels   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecMapNumInLabels indicates the number of
         labels that have been sent to the peer associated with this FEC."
    ::= { vRtrLdpNgAddrFecMapEntry 2 }

vRtrLdpNgAddrFecMapNumOutLabels  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAddrFecMapNumOutLabels indicates the number of
         labels that have been received from the peer associated with this FEC."
    ::= { vRtrLdpNgAddrFecMapEntry 3 }

vRtrLdpNgExtP2MPFecTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgExtP2MPFecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgExtP2MPFecTable is a read-only table that represents
         operational information of P2MP FECs either sent to or received from
         an LDP peer known to the Virtual Router."
    ::= { tmnxLdpNgObjs 16 }

vRtrLdpNgExtP2MPFecEntry         OBJECT-TYPE
    SYNTAX      VRtrLdpNgExtP2MPFecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of operational information of a
         P2MP FEC sent to or received from an LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgExtP2MPFecRootAddrType,
        vRtrLdpNgExtP2MPFecRootAddress,
        vRtrLdpNgExtP2MPFecOpaqueType,
        vRtrLdpNgExtP2MPFecOpaqueLength,
        vRtrLdpNgExtP2MPFecOpaqueValue,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId
    }
    ::= { vRtrLdpNgExtP2MPFecTable 1 }

VRtrLdpNgExtP2MPFecEntry         ::= SEQUENCE
{
    vRtrLdpNgExtP2MPFecOpaqueType    Unsigned32,
    vRtrLdpNgExtP2MPFecOpaqueLength  Unsigned32,
    vRtrLdpNgExtP2MPFecOpaqueValue   OCTET STRING,
    vRtrLdpNgExtP2MPFecRootAddrType  InetAddressType,
    vRtrLdpNgExtP2MPFecRootAddress   InetAddress,
    vRtrLdpNgExtP2MPFecFlags         TmnxLdpFECFlags,
    vRtrLdpNgExtP2MPFecNumInLabels   Gauge32,
    vRtrLdpNgExtP2MPFecNumOutLabels  Gauge32,
    vRtrLdpNgExtP2MPFecTunnelIfId    Unsigned32,
    vRtrLdpNgExtP2MPFecMetric        Unsigned32,
    vRtrLdpNgExtP2MPFecMTU           Unsigned32
}

vRtrLdpNgExtP2MPFecOpaqueType    OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecOpaqueType indicates the type of a
         Multi-Point Opaque Value Element."
    ::= { vRtrLdpNgExtP2MPFecEntry 1 }

vRtrLdpNgExtP2MPFecOpaqueLength  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecOpaqueLength indicates the length of a
         Multi-Point Opaque Value Element."
    ::= { vRtrLdpNgExtP2MPFecEntry 2 }

vRtrLdpNgExtP2MPFecOpaqueValue   OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..74))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecOpaqueValue indicates the value of a
         Multi-Point Opaque Value Element."
    ::= { vRtrLdpNgExtP2MPFecEntry 3 }

vRtrLdpNgExtP2MPFecRootAddrType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecRootAddrType indicates the type of ip
         address of the root for this P2MP FEC."
    ::= { vRtrLdpNgExtP2MPFecEntry 4 }

vRtrLdpNgExtP2MPFecRootAddress   OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecRootAddress indicates the ip address
         of the root for this P2MP FEC."
    ::= { vRtrLdpNgExtP2MPFecEntry 5 }

vRtrLdpNgExtP2MPFecFlags         OBJECT-TYPE
    SYNTAX      TmnxLdpFECFlags
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The bit flags of vRtrLdpNgExtP2MPFecFlags indicates the
         characteristics of the FEC."
    ::= { vRtrLdpNgExtP2MPFecEntry 6 }

vRtrLdpNgExtP2MPFecNumInLabels   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecNumInLabels indicates the number of
         labels that have been sent to the peer associated with this FEC."
    ::= { vRtrLdpNgExtP2MPFecEntry 7 }

vRtrLdpNgExtP2MPFecNumOutLabels  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecNumOutLabels indicates the number of
         labels that have been received from the peer associated with this FEC."
    ::= { vRtrLdpNgExtP2MPFecEntry 8 }

vRtrLdpNgExtP2MPFecTunnelIfId    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecTunnelIfId indicates the tunnel
         interface identifier for this P2MP FEC."
    ::= { vRtrLdpNgExtP2MPFecEntry 9 }

vRtrLdpNgExtP2MPFecMetric        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecMetric indicates the relative cost of
         the tunnel represented by this P2MP FEC"
    ::= { vRtrLdpNgExtP2MPFecEntry 10 }

vRtrLdpNgExtP2MPFecMTU           OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecMTU indicates the maximum transfer
         unit for payloads represented by this P2MP FEC"
    ::= { vRtrLdpNgExtP2MPFecEntry 11 }

vRtrLdpNgExtP2MPFecInLblTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgExtP2MPFecInLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgExtP2MPFecInLblTable is a read-only table that represents
         all P2MP FECs received from an LDP peer known to the virtual router."
    ::= { tmnxLdpNgObjs 17 }

vRtrLdpNgExtP2MPFecInLblEntry    OBJECT-TYPE
    SYNTAX      VRtrLdpNgExtP2MPFecInLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a P2MP FEC received from an
         LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgExtP2MPFecRootAddrType,
        vRtrLdpNgExtP2MPFecRootAddress,
        vRtrLdpNgExtP2MPFecOpaqueType,
        vRtrLdpNgExtP2MPFecOpaqueLength,
        vRtrLdpNgExtP2MPFecOpaqueValue,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vRtrLdpNgExtP2MPFecInLblId
    }
    ::= { vRtrLdpNgExtP2MPFecInLblTable 1 }

VRtrLdpNgExtP2MPFecInLblEntry    ::= SEQUENCE
{
    vRtrLdpNgExtP2MPFecInLblId       Unsigned32,
    vRtrLdpNgExtP2MPFecInLbl         Unsigned32,
    vRtrLdpNgExtP2MPFecInLblStatus   TmnxLabelStatus
}

vRtrLdpNgExtP2MPFecInLblId       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecInLblId indicates the label number of
         the ingress label exchanged."
    ::= { vRtrLdpNgExtP2MPFecInLblEntry 1 }

vRtrLdpNgExtP2MPFecInLbl         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecInLbl indicates the ingress label
         exchanged."
    ::= { vRtrLdpNgExtP2MPFecInLblEntry 2 }

vRtrLdpNgExtP2MPFecInLblStatus   OBJECT-TYPE
    SYNTAX      TmnxLabelStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecInLblStatus indicates the status of
         the ingress label."
    ::= { vRtrLdpNgExtP2MPFecInLblEntry 3 }

vRtrLdpNgExtP2MPFecOutLblTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgExtP2MPFecOutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgExtP2MPFecTable is a read-only table that represents all
         P2MP FECs sent to an LDP peer known to the Virtual Router."
    ::= { tmnxLdpNgObjs 18 }

vRtrLdpNgExtP2MPFecOutLblEntry   OBJECT-TYPE
    SYNTAX      VRtrLdpNgExtP2MPFecOutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a P2MP FEC sent to a LDP
         peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgExtP2MPFecRootAddrType,
        vRtrLdpNgExtP2MPFecRootAddress,
        vRtrLdpNgExtP2MPFecOpaqueType,
        vRtrLdpNgExtP2MPFecOpaqueLength,
        vRtrLdpNgExtP2MPFecOpaqueValue,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vRtrLdpNgExtP2MPFecOutLblId
    }
    ::= { vRtrLdpNgExtP2MPFecOutLblTable 1 }

VRtrLdpNgExtP2MPFecOutLblEntry   ::= SEQUENCE
{
    vRtrLdpNgExtP2MPFecOutLblId      Unsigned32,
    vRtrLdpNgExtP2MPFecOutLbl        Unsigned32,
    vRtrLdpNgExtP2MPFecOutLblStatus  TmnxLabelStatus,
    vRtrLdpNgExtP2MPFecOutLblNHType  InetAddressType,
    vRtrLdpNgExtP2MPFecOutLblNHAdr   InetAddress,
    vRtrLdpNgExtP2MPFecOutLblIfIndex InterfaceIndexOrZero,
    vRtrLdpNgExtP2MPFecOutLblLspId   Unsigned32
}

vRtrLdpNgExtP2MPFecOutLblId      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecOutLblId indicates the label number of
         the egress label exchanged."
    ::= { vRtrLdpNgExtP2MPFecOutLblEntry 1 }

vRtrLdpNgExtP2MPFecOutLbl        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecOutLbl indicates the egress label
         exchanged."
    ::= { vRtrLdpNgExtP2MPFecOutLblEntry 2 }

vRtrLdpNgExtP2MPFecOutLblStatus  OBJECT-TYPE
    SYNTAX      TmnxLabelStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecOutLblStatus indicates the status of
         the egress label."
    ::= { vRtrLdpNgExtP2MPFecOutLblEntry 3 }

vRtrLdpNgExtP2MPFecOutLblNHType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecOutLblNHType indicates the address
         type of vRtrLdpNgExtP2MPFecOutLblNHAdr."
    ::= { vRtrLdpNgExtP2MPFecOutLblEntry 4 }

vRtrLdpNgExtP2MPFecOutLblNHAdr   OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecOutLblNHAdr indicates the IP address
         of the next hop for egress label."
    ::= { vRtrLdpNgExtP2MPFecOutLblEntry 5 }

vRtrLdpNgExtP2MPFecOutLblIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecOutLblIfIndex indicates the interface
         index for egress label."
    ::= { vRtrLdpNgExtP2MPFecOutLblEntry 6 }

vRtrLdpNgExtP2MPFecOutLblLspId   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecOutLblLspId indicates the LSP id
         associated with egress label."
    ::= { vRtrLdpNgExtP2MPFecOutLblEntry 7 }

vRtrLdpNgExtP2MPFecMapTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgExtP2MPFecMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgExtP2MPFecMapTable is a read-only table which maps to the
         vRtrLdpNgExtP2MPFecTable. This table has the same indexes as the
         vRtrLdpNgExtP2MPFecTable but the order in which these indexes are
         specified is different for the two tables."
    ::= { tmnxLdpNgObjs 19 }

vRtrLdpNgExtP2MPFecMapEntry      OBJECT-TYPE
    SYNTAX      VRtrLdpNgExtP2MPFecMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a P2MP FEC sent to or
         received from an LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vRtrLdpNgExtP2MPFecRootAddrType,
        vRtrLdpNgExtP2MPFecRootAddress,
        vRtrLdpNgExtP2MPFecOpaqueType,
        vRtrLdpNgExtP2MPFecOpaqueLength,
        vRtrLdpNgExtP2MPFecOpaqueValue
    }
    ::= { vRtrLdpNgExtP2MPFecMapTable 1 }

VRtrLdpNgExtP2MPFecMapEntry      ::= SEQUENCE
{
    vRtrLdpNgExtP2MPFecMapFlags      TmnxLdpFECFlags,
    vRtrLdpNgExtP2MPFecMapNumInLbls  Gauge32,
    vRtrLdpNgExtP2MPFecMapNumOutLbls Gauge32,
    vRtrLdpNgExtP2MPFecMapTunnelIfId Unsigned32,
    vRtrLdpNgExtP2MPFecMapMetric     Unsigned32,
    vRtrLdpNgExtP2MPFecMapMTU        Unsigned32
}

vRtrLdpNgExtP2MPFecMapFlags      OBJECT-TYPE
    SYNTAX      TmnxLdpFECFlags
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The bit flags of vRtrLdpNgExtP2MPFecMapFlags indicates the
         characteristics of the FEC."
    ::= { vRtrLdpNgExtP2MPFecMapEntry 1 }

vRtrLdpNgExtP2MPFecMapNumInLbls  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecMapNumInLbls indicates the number of
         labels that have been sent to the peer associated with this FEC."
    ::= { vRtrLdpNgExtP2MPFecMapEntry 2 }

vRtrLdpNgExtP2MPFecMapNumOutLbls OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecMapNumOutLbls indicates the number of
         labels that have been received from the peer associated with this FEC."
    ::= { vRtrLdpNgExtP2MPFecMapEntry 3 }

vRtrLdpNgExtP2MPFecMapTunnelIfId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecMapTunnelIfId indicates the tunnel
         interface identifier for this P2MP FEC."
    ::= { vRtrLdpNgExtP2MPFecMapEntry 4 }

vRtrLdpNgExtP2MPFecMapMetric     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecMapMetric indicates the relative cost
         of the tunnel represented by this P2MP FEC"
    ::= { vRtrLdpNgExtP2MPFecMapEntry 5 }

vRtrLdpNgExtP2MPFecMapMTU        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgExtP2MPFecMapMTU indicates the maximum transfer
         unit for payloads represented by this P2MP FEC"
    ::= { vRtrLdpNgExtP2MPFecMapEntry 6 }

vRtrLdpNgInetIfStatsTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgInetIfStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgInetIfStatsTable is a read-only table. The purpose of
         this table is to keep statistical information about the LDP Interfaces
         for given Inet address family on this LSR.

         Use of AUGMENTS clause implies a one-to-one dependent relationship
         between the base table, vRtrLdpNgInetIfTable, and the augmenting
         table, vRtrLdpNgInetIfStatsTable. This in effect extends the
         vRtrLdpNgInetIfTable with additional columns. Creation or deletion of
         a row in the vRtrLdpNgInetIfTable results in the same fate for the row
         in the vRtrLdpNgInetIfStatsTable."
    ::= { tmnxLdpNgObjs 20 }

vRtrLdpNgInetIfStatsEntry        OBJECT-TYPE
    SYNTAX      VRtrLdpNgInetIfStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table contains statistical information about an LDP
         Interface for given Inet address family.

         Some counters contained in a row are for fatal errors received
         during a former LDP Session associated with this entry. For example,
         an LDP Pdu received on a TCP connection during an LDP Session
         contains a fatal error.  That error is counted here, because the
         session is terminated.

         If the error is NOT fatal (i.e. and the Session remains), then the
         error is counted in the vRtrLdpNgSessionStatsEntry."
    AUGMENTS    { vRtrLdpNgInetIfEntry }
    ::= { vRtrLdpNgInetIfStatsTable 1 }

VRtrLdpNgInetIfStatsEntry        ::= SEQUENCE
{
    vRtrLdpNgInetIfStatsExistingAdj  Gauge32,
    vRtrLdpNgInetIfStatsHelloRecv    Gauge32,
    vRtrLdpNgInetIfStatsHelloSent    Gauge32,
    vRtrLdpNgInetIfStatsBadPduLen    Gauge32,
    vRtrLdpNgInetIfStatsBadMsgLen    Gauge32,
    vRtrLdpNgInetIfStatsMalformedTlv Gauge32,
    vRtrLdpNgInetIfStatsBadProtoVer  Gauge32
}

vRtrLdpNgInetIfStatsExistingAdj  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfStatsExistingAdj indicates a count of the
         total active adjacencies on this LDP interface for given Inet address
         family."
    ::= { vRtrLdpNgInetIfStatsEntry 1 }

vRtrLdpNgInetIfStatsHelloRecv    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfStatsHelloRecv indicates number of Hello
         messages received with this LDP interface."
    ::= { vRtrLdpNgInetIfStatsEntry 2 }

vRtrLdpNgInetIfStatsHelloSent    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfStatsHelloSent indicates the number of
         Hello messages sent with this LDP interface."
    ::= { vRtrLdpNgInetIfStatsEntry 3 }

vRtrLdpNgInetIfStatsBadPduLen    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfStatsBadPduLen indicates the number of bad
         PDU length errors detected with this LDP interface."
    ::= { vRtrLdpNgInetIfStatsEntry 4 }

vRtrLdpNgInetIfStatsBadMsgLen    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfStatsBadMsgLen indicates the number of bad
         message length errors detected with this LDP interface."
    ::= { vRtrLdpNgInetIfStatsEntry 5 }

vRtrLdpNgInetIfStatsMalformedTlv OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfStatsMalformedTlv indicates the number of
         malformed TLV value errors detected with this LDP interface."
    ::= { vRtrLdpNgInetIfStatsEntry 6 }

vRtrLdpNgInetIfStatsBadProtoVer  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfStatsBadProtoVer indicates the number of
         bad protocol version errors detected with this LDP interface."
    ::= { vRtrLdpNgInetIfStatsEntry 7 }

vRtrLdpNgSessionStatsTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgSessionStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgSessionStatsTable is a read-only table. The purpose of
         this table is to keep statistical information about a single session
         between an LDP entity and an LDP Peer.

         Use of AUGMENTS clause implies a one-to-one dependent relationship
         between the base table, vRtrLdpNgSessionTable, and the augmenting
         table, vRtrLdpNgSessionStatsTable. This in effect extends the
         vRtrLdpNgSessionTable with additional columns. Creation or deletion of
         a row in the vRtrLdpNgSessionTable results in the same fate for the
         row in the vRtrLdpNgSessionStatsTable."
    ::= { tmnxLdpNgObjs 21 }

vRtrLdpNgSessionStatsEntry       OBJECT-TYPE
    SYNTAX      VRtrLdpNgSessionStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table represents statistical information about a single
         session between an LDP entity and an LDP Peer."
    AUGMENTS    { vRtrLdpNgSessionEntry }
    ::= { vRtrLdpNgSessionStatsTable 1 }

VRtrLdpNgSessionStatsEntry       ::= SEQUENCE
{
    vRtrLdpNgSessStatsTargAdj        Gauge32,
    vRtrLdpNgSessStatsLinkAdj        Gauge32,
    vRtrLdpNgSessStatsHelloIn        Counter32,
    vRtrLdpNgSessStatsHelloOut       Counter32,
    vRtrLdpNgSessStatsKeepaliveIn    Counter32,
    vRtrLdpNgSessStatsKeepaliveOut   Counter32,
    vRtrLdpNgSessStatsInitIn         Counter32,
    vRtrLdpNgSessStatsInitOut        Counter32,
    vRtrLdpNgSessStatsLblMappingIn   Counter32,
    vRtrLdpNgSessStatsLblMappingOut  Counter32,
    vRtrLdpNgSessStatsLblRequestIn   Counter32,
    vRtrLdpNgSessStatsLblRequestOut  Counter32,
    vRtrLdpNgSessStatsLblReleaseIn   Counter32,
    vRtrLdpNgSessStatsLblReleaseOut  Counter32,
    vRtrLdpNgSessStatsLblWithdrawIn  Counter32,
    vRtrLdpNgSessStatsLblWithdrawOut Counter32,
    vRtrLdpNgSessStatsLblAbortIn     Counter32,
    vRtrLdpNgSessStatsLblAbortOut    Counter32,
    vRtrLdpNgSessStatsAddrIn         Counter32,
    vRtrLdpNgSessStatsAddrOut        Counter32,
    vRtrLdpNgSessStatsAddrWithdrIn   Counter32,
    vRtrLdpNgSessStatsAddrWithdrOut  Counter32,
    vRtrLdpNgSessStatsNotifIn        Counter32,
    vRtrLdpNgSessStatsNotifOut       Counter32,
    vRtrLdpNgSessStatsIPv4PfxFecRcv  Counter32,
    vRtrLdpNgSessStatsIPv6PfxFecRcv  Counter32,
    vRtrLdpNgSessStatsIPv4PfxFecSnt  Counter32,
    vRtrLdpNgSessStatsIPv6PfxFecSnt  Counter32,
    vRtrLdpNgSessStatsIPv4P2MPFecRcv Counter32,
    vRtrLdpNgSessStatsIPv6P2MPFecRcv Counter32,
    vRtrLdpNgSessStatsIPv4P2MPFecSnt Counter32,
    vRtrLdpNgSessStatsIPv6P2MPFecSnt Counter32,
    vRtrLdpNgSessStatsSvcFec128Recv  Counter32,
    vRtrLdpNgSessStatsSvcFec128Sent  Counter32,
    vRtrLdpNgSessStatsSvcFec129Recv  Counter32,
    vRtrLdpNgSessStatsSvcFec129Sent  Counter32,
    vRtrLdpNgSessStatsIPv4AddrRecv   Counter32,
    vRtrLdpNgSessStatsIPv6AddrRecv   Counter32,
    vRtrLdpNgSessStatsIPv4AddrSent   Counter32,
    vRtrLdpNgSessStatsIPv6AddrSent   Counter32,
    vRtrLdpNgSessStatsCapabilityIn   Counter32,
    vRtrLdpNgSessStatsCapabilityOut  Counter32
}

vRtrLdpNgSessStatsTargAdj        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsTargAdj indicates the number of
         targeted adjacencies for this session."
    ::= { vRtrLdpNgSessionStatsEntry 1 }

vRtrLdpNgSessStatsLinkAdj        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLinkAdj indicates the number of link
         adjacencies for this session."
    ::= { vRtrLdpNgSessionStatsEntry 2 }

vRtrLdpNgSessStatsHelloIn        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsHelloIn counts the number of Hello
         Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 3 }

vRtrLdpNgSessStatsHelloOut       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsHelloOut counts the number of Hello
         Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 4 }

vRtrLdpNgSessStatsKeepaliveIn    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsKeepaliveIn counts the number of
         Keepalive Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 5 }

vRtrLdpNgSessStatsKeepaliveOut   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsKeepaliveOut counts the number of
         Keepalive Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 6 }

vRtrLdpNgSessStatsInitIn         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsInitIn counts the number of Init
         Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 7 }

vRtrLdpNgSessStatsInitOut        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsInitOut counts the number of Init
         Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 8 }

vRtrLdpNgSessStatsLblMappingIn   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLblMappingIn counts the number of Label
         Mapping Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 9 }

vRtrLdpNgSessStatsLblMappingOut  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLblMappingOut counts the number of
         Label Mapping Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 10 }

vRtrLdpNgSessStatsLblRequestIn   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLblRequestIn counts the number of Label
         Request Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 11 }

vRtrLdpNgSessStatsLblRequestOut  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLblRequestOut counts the number of
         Label Request Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 12 }

vRtrLdpNgSessStatsLblReleaseIn   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLblReleaseIn counts the number of Label
         Release Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 13 }

vRtrLdpNgSessStatsLblReleaseOut  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLblReleaseOut counts the number of
         Label Release Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 14 }

vRtrLdpNgSessStatsLblWithdrawIn  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLblWithdrawIn counts the number of
         Label Withdraw Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 15 }

vRtrLdpNgSessStatsLblWithdrawOut OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLblWithdrawOut counts the number of
         Label Withdraw Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 16 }

vRtrLdpNgSessStatsLblAbortIn     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLblAbortIn counts the number of Label
         Abort Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 17 }

vRtrLdpNgSessStatsLblAbortOut    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsLblAbortOut counts the number of Label
         Abort Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 18 }

vRtrLdpNgSessStatsAddrIn         OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsAddrIn counts the number of Address
         Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 19 }

vRtrLdpNgSessStatsAddrOut        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsAddrOut counts the number of Address
         Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 20 }

vRtrLdpNgSessStatsAddrWithdrIn   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsAddrWithdrIn counts the number of
         Address Withdraw Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 21 }

vRtrLdpNgSessStatsAddrWithdrOut  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsAddrWithdrOut counts the number of
         Address Withdraw Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 22 }

vRtrLdpNgSessStatsNotifIn        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsNotifIn counts the number of
         Notification Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 23 }

vRtrLdpNgSessStatsNotifOut       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsNotifOut counts the number of
         Notification Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 24 }

vRtrLdpNgSessStatsIPv4PfxFecRcv  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv4PfxFecRcv counts the number of IPv4
         prefix FECs received for this session."
    ::= { vRtrLdpNgSessionStatsEntry 25 }

vRtrLdpNgSessStatsIPv6PfxFecRcv  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv6PfxFecRcv counts the number of IPv6
         prefix FECs received for this session."
    ::= { vRtrLdpNgSessionStatsEntry 26 }

vRtrLdpNgSessStatsIPv4PfxFecSnt  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv4PfxFecSnt counts the number of IPv4
         prefix FECs sent for this session."
    ::= { vRtrLdpNgSessionStatsEntry 27 }

vRtrLdpNgSessStatsIPv6PfxFecSnt  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv6PfxFecSnt counts the number of IPv6
         prefix FECs sent for this session."
    ::= { vRtrLdpNgSessionStatsEntry 28 }

vRtrLdpNgSessStatsIPv4P2MPFecRcv OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv4P2MPFecRcv counts the number of
         IPv4 P2MP FECs received for this session."
    ::= { vRtrLdpNgSessionStatsEntry 29 }

vRtrLdpNgSessStatsIPv6P2MPFecRcv OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv6P2MPFecRcv counts the number of
         IPv6 P2MP FECs received for this session."
    ::= { vRtrLdpNgSessionStatsEntry 30 }

vRtrLdpNgSessStatsIPv4P2MPFecSnt OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv4P2MPFecSnt counts the number of
         IPv4 P2MP FECs sent for this session."
    ::= { vRtrLdpNgSessionStatsEntry 31 }

vRtrLdpNgSessStatsIPv6P2MPFecSnt OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv6P2MPFecSnt counts the number of
         IPv6 P2MP FECs sent for this session."
    ::= { vRtrLdpNgSessionStatsEntry 32 }

vRtrLdpNgSessStatsSvcFec128Recv  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsSvcFec128Recv counts the number of
         service FEC 128 received for this session."
    ::= { vRtrLdpNgSessionStatsEntry 33 }

vRtrLdpNgSessStatsSvcFec128Sent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsSvcFec128Sent counts the number of
         service FEC 128 sent for this session."
    ::= { vRtrLdpNgSessionStatsEntry 34 }

vRtrLdpNgSessStatsSvcFec129Recv  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsSvcFec129Recv counts the number of
         service FEC 129 received for this session."
    ::= { vRtrLdpNgSessionStatsEntry 35 }

vRtrLdpNgSessStatsSvcFec129Sent  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsSvcFec129Sent counts the number of
         service FEC 129 sent for this session."
    ::= { vRtrLdpNgSessionStatsEntry 36 }

vRtrLdpNgSessStatsIPv4AddrRecv   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv4AddrRecv counts the number of IPv4
         local addresses received for this session."
    ::= { vRtrLdpNgSessionStatsEntry 37 }

vRtrLdpNgSessStatsIPv6AddrRecv   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv6AddrRecv counts the number of IPv6
         local addresses received for this session."
    ::= { vRtrLdpNgSessionStatsEntry 38 }

vRtrLdpNgSessStatsIPv4AddrSent   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv4AddrSent counts the number of IPv4
         local addresses sent for this session."
    ::= { vRtrLdpNgSessionStatsEntry 39 }

vRtrLdpNgSessStatsIPv6AddrSent   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsIPv6AddrSent counts the number of IPv6
         local addresses sent for this session."
    ::= { vRtrLdpNgSessionStatsEntry 40 }

vRtrLdpNgSessStatsCapabilityIn   OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsCapabilityIn counts the number of
         Capability Messages that have been received during this session."
    ::= { vRtrLdpNgSessionStatsEntry 41 }

vRtrLdpNgSessStatsCapabilityOut  OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessStatsCapabilityOut counts the number of
         Capability Messages that have been sent during this session."
    ::= { vRtrLdpNgSessionStatsEntry 42 }

vLdpNgSvcFec128Table             OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgSvcFec128Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vLdpNgSvcFec128Table is a read-only table that represents
         operational information of Service FEC 128 either sent to or received
         from an LDP peer known to the Virtual Router."
    ::= { tmnxLdpNgObjs 22 }

vLdpNgSvcFec128Entry             OBJECT-TYPE
    SYNTAX      VLdpNgSvcFec128Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a service FEC 128 sent to or
         received from an LDP peer."
    INDEX       {
        vRtrID,
        vLdpNgFec128FecType,
        vLdpNgFec128VcType,
        vLdpNgFec128VcId,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId
    }
    ::= { vLdpNgSvcFec128Table 1 }

VLdpNgSvcFec128Entry             ::= SEQUENCE
{
    vLdpNgFec128FecType              TmnxLdpFECType,
    vLdpNgFec128VcType               TmnxVcType,
    vLdpNgFec128VcId                 TmnxVcId,
    vLdpNgFec128ServType             ServType,
    vLdpNgFec128ServId               TmnxServId,
    vLdpNgFec128VpnId                TmnxVpnId,
    vLdpNgFec128Flags                TmnxLdpFECFlags,
    vLdpNgFec128NumInLabels          Unsigned32,
    vLdpNgFec128NumOutLabels         Unsigned32,
    vLdpNgFec128SdpId                SdpId,
    vLdpNgFec128MateEndptVcId        TmnxVcIdOrNone,
    vLdpNgFec128MateEndptSdpId       SdpId
}

vLdpNgFec128FecType              OBJECT-TYPE
    SYNTAX      TmnxLdpFECType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128FecType specifies the FEC type associated
         with this service FEC."
    ::= { vLdpNgSvcFec128Entry 1 }

vLdpNgFec128VcType               OBJECT-TYPE
    SYNTAX      TmnxVcType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128VcType specifies the VC type associated with
         this service FEC."
    ::= { vLdpNgSvcFec128Entry 2 }

vLdpNgFec128VcId                 OBJECT-TYPE
    SYNTAX      TmnxVcId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128VcId specifies the VC identifier associated
         with this service FEC."
    ::= { vLdpNgSvcFec128Entry 3 }

vLdpNgFec128ServType             OBJECT-TYPE
    SYNTAX      ServType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128ServType indicates the Service type
         associated with this service FEC."
    ::= { vLdpNgSvcFec128Entry 4 }

vLdpNgFec128ServId               OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128ServId indicates the Service identifier
         associated with this service FEC."
    ::= { vLdpNgSvcFec128Entry 5 }

vLdpNgFec128VpnId                OBJECT-TYPE
    SYNTAX      TmnxVpnId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128VpnId identifies the VPN associated with the
         FEC."
    ::= { vLdpNgSvcFec128Entry 6 }

vLdpNgFec128Flags                OBJECT-TYPE
    SYNTAX      TmnxLdpFECFlags
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The bit flags of vLdpNgFec128Flags indicate the characteristics of the
         FEC."
    ::= { vLdpNgSvcFec128Entry 7 }

vLdpNgFec128NumInLabels          OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128NumInLabels indicates the number of labels
         that have been sent to the peer associated with this FEC."
    ::= { vLdpNgSvcFec128Entry 8 }

vLdpNgFec128NumOutLabels         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128NumOutLabels indicates the number of labels
         that have been received from the peer associated with this FEC."
    ::= { vLdpNgSvcFec128Entry 9 }

vLdpNgFec128SdpId                OBJECT-TYPE
    SYNTAX      SdpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128SdpId identifies the SDP associated with this
         peer."
    ::= { vLdpNgSvcFec128Entry 10 }

vLdpNgFec128MateEndptVcId        OBJECT-TYPE
    SYNTAX      TmnxVcIdOrNone
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128MateEndptVcId indicates the VC identifier
         associated with this service FEC mate endpoint for vc-switching.

         vLdpNgFec128MateEndptVcId is set to zero (0) for non-switching FECs."
    ::= { vLdpNgSvcFec128Entry 11 }

vLdpNgFec128MateEndptSdpId       OBJECT-TYPE
    SYNTAX      SdpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128MateEndptSdpId identifies the SDP associated
         with this service FEC mate endpoint for vc-switching."
    ::= { vLdpNgSvcFec128Entry 12 }

vLdpNgSvcFec128InLblTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgSvcFec128InLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vLdpNgSvcFec128InLblTable is a read-only table that represents all
         service FEC 128 received from an LDP peer known to the Virtual Router."
    ::= { tmnxLdpNgObjs 23 }

vLdpNgSvcFec128InLblEntry        OBJECT-TYPE
    SYNTAX      VLdpNgSvcFec128InLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a service FEC received from
         an LDP peer."
    INDEX       {
        vRtrID,
        vLdpNgFec128FecType,
        vLdpNgFec128VcType,
        vLdpNgFec128VcId,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vLdpNgFec128InLabelId
    }
    ::= { vLdpNgSvcFec128InLblTable 1 }

VLdpNgSvcFec128InLblEntry        ::= SEQUENCE
{
    vLdpNgFec128InLabelId            Unsigned32,
    vLdpNgFec128InLabel              Unsigned32,
    vLdpNgFec128InLabelStatus        TmnxLabelStatus,
    vLdpNgFec128InLabelSigStatus     TmnxLabelSigStatus,
    vLdpNgFec128InLblWdwReason       TmnxLdpInLblWdrawalReasonCode,
    vLdpNgFec128InLblMaxCellConcat   Unsigned32,
    vLdpNgFec128InLblFLTxCap         TruthValue,
    vLdpNgFec128InLblFLRxCap         TruthValue,
    vLdpNgFec128InLblIPv4CeIpAdType  InetAddressType,
    vLdpNgFec128InLblIPv4CeIpAddr    InetAddress,
    vLdpNgFec128InLblIPv4Cap         TruthValue,
    vLdpNgFec128InLblIPv6Cap         TruthValue,
    vLdpNgFec128InLblMTU             Unsigned32,
    vLdpNgFec128InLblVlanTag         Unsigned32,
    vLdpNgFec128InLblVccvCV          BITS,
    vLdpNgFec128InLblVccvCC          BITS,
    vLdpNgFec128InLblPwStatus        TruthValue
}

vLdpNgFec128InLabelId            OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLabelId identifies the ingress label
         exchanged."
    ::= { vLdpNgSvcFec128InLblEntry 1 }

vLdpNgFec128InLabel              OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLabel indicates the ingress label
         exchanged."
    ::= { vLdpNgSvcFec128InLblEntry 2 }

vLdpNgFec128InLabelStatus        OBJECT-TYPE
    SYNTAX      TmnxLabelStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLabelStatus indicates the status of the
         ingress label."
    ::= { vLdpNgSvcFec128InLblEntry 3 }

vLdpNgFec128InLabelSigStatus     OBJECT-TYPE
    SYNTAX      TmnxLabelSigStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLabelSigStatus indicates the signaling
         status for vLdpNgFec128InLabel."
    ::= { vLdpNgSvcFec128InLblEntry 4 }

vLdpNgFec128InLblWdwReason       OBJECT-TYPE
    SYNTAX      TmnxLdpInLblWdrawalReasonCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblWdwReason indicates the reason of
         withdrawal of ingress label value in vLdpNgFec128InLabel."
    ::= { vLdpNgSvcFec128InLblEntry 5 }

vLdpNgFec128InLblMaxCellConcat   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblMaxCellConcat indicates the local
         maximum number of ATM cells to concatenate on a ATM cell-mode VC type
         SDP binding."
    ::= { vLdpNgSvcFec128InLblEntry 6 }

vLdpNgFec128InLblFLTxCap         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblFLTxCap indicates whether or not this
         LDP peer is capable of sending Flow Label in its pseudowire (PW)
         packet.

         The value of vLdpNgFec128InLblFLTxCap is 'true' when this LDP peer is
         capable of sending Flow Label and the value is 'false' when the peer
         is not capable of sending Flow Label in pseudowire packet."
    ::= { vLdpNgSvcFec128InLblEntry 7 }

vLdpNgFec128InLblFLRxCap         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblFLRxCap indicates whether or not this
         LDP peer is capable of receiving Flow Label in its pseudowire packet.

         The value of vLdpNgFec128InLblFLRxCap is 'true' when this LDP peer is
         capable of receiving Flow Label and the value is 'false' when the peer
         is not capable of receiving Flow Label in pseudowire packet."
    ::= { vLdpNgSvcFec128InLblEntry 8 }

vLdpNgFec128InLblIPv4CeIpAdType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblIPv4CeIpAdType indicates the local ipv4
         CE Address type."
    ::= { vLdpNgSvcFec128InLblEntry 9 }

vLdpNgFec128InLblIPv4CeIpAddr    OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblIPv4CeIpAddr indicates the local ipv4 CE
         Address."
    ::= { vLdpNgSvcFec128InLblEntry 10 }

vLdpNgFec128InLblIPv4Cap         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblIPv4Cap indicates whether or not the
         local ipv4 stack capability is supported for this LDP peer.

         The value of vLdpNgFec128InLblIPv4Cap is 'true' when the local ipv4
         stack capability is supported and the value is 'false' when the local
         ipv4 stack capability is not supported."
    ::= { vLdpNgSvcFec128InLblEntry 11 }

vLdpNgFec128InLblIPv6Cap         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblIPv6Cap indicates whether or not the
         local ipv6 stack capability is supported for this LDP peer.

         The value of vLdpNgFec128InLblIPv6Cap is 'true' when the local ipv6
         stack capability is supported and the value is 'false' when the local
         ipv6 stack capability is not supported."
    ::= { vLdpNgSvcFec128InLblEntry 12 }

vLdpNgFec128InLblMTU             OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblMTU indicates the largest service frame
         size (in octets) that can be handled by the local ESR."
    ::= { vLdpNgSvcFec128InLblEntry 13 }

vLdpNgFec128InLblVlanTag         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblVlanTag indicates the local tag on a
         VLAN VC type SDP binding."
    ::= { vLdpNgSvcFec128InLblEntry 14 }

vLdpNgFec128InLblVccvCV          OBJECT-TYPE
    SYNTAX      BITS {
        icmpPing                 (0),
        lspPing                  (1),
        bfdFaultDetect           (2),
        bfdFaultDetectSignalling (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblVccvCV indicates the CV (Connectivity
         Verification) types supported by peer LSR if it supports VCCV (Circuit
         Connectivity Verification) on pseudowire. If VCCV is not supported,
         vLdpNgFec128InLblVccvCV will be set to 0."
    ::= { vLdpNgSvcFec128InLblEntry 15 }

vLdpNgFec128InLblVccvCC          OBJECT-TYPE
    SYNTAX      BITS {
        pwe3ControlWord   (0),
        routerAlertLabel  (1),
        mplsDemuxLabelTL1 (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblVccvCC indicates the CC (Control
         Channel) types supported by peer LSR if it supports VCCV on
         pseudowire. If VCCV is not supported, vLdpNgFec128InLblVccvCC will be
         set to 0."
    ::= { vLdpNgSvcFec128InLblEntry 16 }

vLdpNgFec128InLblPwStatus        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128InLblPwStatus indicates whether the local LSR
         supports pseudowire status signaling."
    ::= { vLdpNgSvcFec128InLblEntry 17 }

vLdpNgSvcFec128OutLblTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgSvcFec128OutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vLdpNgSvcFec128OutLblTable is a read-only table that represents
         all service FEC 128 sent to an LDP peer known to the Virtual Router."
    ::= { tmnxLdpNgObjs 24 }

vLdpNgSvcFec128OutLblEntry       OBJECT-TYPE
    SYNTAX      VLdpNgSvcFec128OutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a service FEC 128 sent to an
         LDP peer."
    INDEX       {
        vRtrID,
        vLdpNgFec128FecType,
        vLdpNgFec128VcType,
        vLdpNgFec128VcId,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vLdpNgFec128OutLabelId
    }
    ::= { vLdpNgSvcFec128OutLblTable 1 }

VLdpNgSvcFec128OutLblEntry       ::= SEQUENCE
{
    vLdpNgFec128OutLabelId           Unsigned32,
    vLdpNgFec128OutLabel             Unsigned32,
    vLdpNgFec128OutLabelStatus       TmnxLabelStatus,
    vLdpNgFec128OutLabelSigStatus    TmnxLabelSigStatus,
    vLdpNgFec128OutLblMaxCellConcat  Unsigned32,
    vLdpNgFec128OutLblFLTxCap        TruthValue,
    vLdpNgFec128OutLblFLRxCap        TruthValue,
    vLdpNgFec128OutLblIPv4CeAddrType InetAddressType,
    vLdpNgFec128OutLblIPv4CeIpAddr   InetAddress,
    vLdpNgFec128OutLblIPv4Cap        TruthValue,
    vLdpNgFec128OutLblIPv6Cap        TruthValue,
    vLdpNgFec128OutLblMTU            Unsigned32,
    vLdpNgFec128OutLblVlanTag        Unsigned32,
    vLdpNgFec128OutLblVccvCV         BITS,
    vLdpNgFec128OutLblVccvCC         BITS,
    vLdpNgFec128OutLblPwStatus       TruthValue
}

vLdpNgFec128OutLabelId           OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLabelId specifies the identifier."
    ::= { vLdpNgSvcFec128OutLblEntry 1 }

vLdpNgFec128OutLabel             OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLabel indicates the egress label
         exchanged."
    ::= { vLdpNgSvcFec128OutLblEntry 2 }

vLdpNgFec128OutLabelStatus       OBJECT-TYPE
    SYNTAX      TmnxLabelStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLabelStatus indicates the status of the
         egress label."
    ::= { vLdpNgSvcFec128OutLblEntry 3 }

vLdpNgFec128OutLabelSigStatus    OBJECT-TYPE
    SYNTAX      TmnxLabelSigStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLabelSigStatus indicates the signaling
         status for vLdpNgFec128OutLabel."
    ::= { vLdpNgSvcFec128OutLblEntry 4 }

vLdpNgFec128OutLblMaxCellConcat  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblMaxCellConcat indicates the remote
         maximum number of ATM cells to concatenate on a ATM cell-mode VC type
         SDP binding."
    ::= { vLdpNgSvcFec128OutLblEntry 5 }

vLdpNgFec128OutLblFLTxCap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblFLTxCap indicates whether or not the
         remote LDP peer is capable of sending Flow Label in its pseudowire
         packet.

         The value of vLdpNgFec128OutLblFLTxCap is 'true' when the remote LDP
         peer is capable of sending Flow Label and the value is 'false' when
         the peer is not capable of sending Flow Label in pseudowire packet."
    ::= { vLdpNgSvcFec128OutLblEntry 6 }

vLdpNgFec128OutLblFLRxCap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblFLRxCap indicates whether or not the
         remote LDP peer is capable of receiving Flow Label in its pseudowire
         packet.

         The value of vLdpNgFec128OutLblFLRxCap is 'true' when the remote LDP
         peer is capable of receiving Flow Label and the value is 'false' when
         the peer is not capable of receiving Flow Label in pseudowire packet."
    ::= { vLdpNgSvcFec128OutLblEntry 7 }

vLdpNgFec128OutLblIPv4CeAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblIPv4CeAddrType indicates the remote
         ipv4 CE Address type."
    ::= { vLdpNgSvcFec128OutLblEntry 8 }

vLdpNgFec128OutLblIPv4CeIpAddr   OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblIPv4CeIpAddr indicates the remote ipv4
         CE Address."
    ::= { vLdpNgSvcFec128OutLblEntry 9 }

vLdpNgFec128OutLblIPv4Cap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblIPv4Cap indicates whether or not the
         remote ipv4 stack capability is supported for this LDP peer.

         The value of vLdpNgFec128OutLblIPv4Cap is 'true' when the remote ipv4
         stack capability is supported and the value is 'false' when the remote
         ipv4 stack capability is not supported."
    ::= { vLdpNgSvcFec128OutLblEntry 10 }

vLdpNgFec128OutLblIPv6Cap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblIPv6Cap indicates whether or not the
         remote ipv6 stack capability is supported for this LDP peer.

         The value of vLdpNgFec128OutLblIPv6Cap is 'true' when the remote ipv6
         stack capability is supported and the value is 'false' when the remote
         ipv6 stack capability is not supported."
    ::= { vLdpNgSvcFec128OutLblEntry 11 }

vLdpNgFec128OutLblMTU            OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblMTU indicates the largest service frame
         size (in octets) that can be handled by the remote ESR."
    ::= { vLdpNgSvcFec128OutLblEntry 12 }

vLdpNgFec128OutLblVlanTag        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblVlanTag indicates the remote tag on a
         VLAN VC type SDP binding."
    ::= { vLdpNgSvcFec128OutLblEntry 13 }

vLdpNgFec128OutLblVccvCV         OBJECT-TYPE
    SYNTAX      BITS {
        icmpPing                 (0),
        lspPing                  (1),
        bfdFaultDetect           (2),
        bfdFaultDetectSignalling (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblVccvCV indicates the CV (Connectivity
         Verification) types supported by local LSR if it supports VCCV
         pseudowire. If VCCV is not supported, vLdpNgFec128OutLblVccvCV will be
         set to 0."
    ::= { vLdpNgSvcFec128OutLblEntry 14 }

vLdpNgFec128OutLblVccvCC         OBJECT-TYPE
    SYNTAX      BITS {
        pwe3ControlWord   (0),
        routerAlertLabel  (1),
        mplsDemuxLabelTL1 (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblVccvCC indicates the CC (Control
         Channel) types supported by local LSR if it supports VCCV on
         pseudowire. If VCCV is not supported, vLdpNgFec128OutLblVccvCC will be
         set to 0."
    ::= { vLdpNgSvcFec128OutLblEntry 15 }

vLdpNgFec128OutLblPwStatus       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec128OutLblPwStatus indicates whether the remote
         LSR supports pseudowire status signaling."
    ::= { vLdpNgSvcFec128OutLblEntry 16 }

vRtrLdpNgHelloAdjMapTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgHelloAdjMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgHelloAdjMapTable is a read-only table which maps to the
         vRtrLdpNgHelloAdjTable. This table has the same indexes as the
         vRtrLdpNgHelloAdjTable but the order in which these indexes are
         specified is different for the two tables."
    ::= { tmnxLdpNgObjs 25 }

vRtrLdpNgHelloAdjMapEntry        OBJECT-TYPE
    SYNTAX      VRtrLdpNgHelloAdjMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row represents a single LDP Hello Adjacency. An LDP Session can
         have one or more Hello adjacencies."
    INDEX       {
        vRtrID,
        vRtrLdpNgIfIndex,
        vRtrLdpNgIfAddrType,
        vRtrLdpNgPeerAddressType,
        vRtrLdpNgPeerAddress,
        vRtrLdpNgHelloAdjMapLdpIdType,
        vRtrLdpNgHelloAdjMapLdpId
    }
    ::= { vRtrLdpNgHelloAdjMapTable 1 }

VRtrLdpNgHelloAdjMapEntry        ::= SEQUENCE
{
    vRtrLdpNgHelloAdjMapLdpIdType    TmnxMplsLdpNgIdType,
    vRtrLdpNgHelloAdjMapLdpId        TmnxMplsLdpNgIdentifier,
    vRtrLdpNgHelloAdjMapIndex        Unsigned32
}

vRtrLdpNgHelloAdjMapLdpIdType    OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgHelloAdjMapLdpIdType is an index for the row entry. It
         indicates the LDP identifier type of the peer, indicated by
         vRtrLdpNgHelloAdjMapLdpId."
    ::= { vRtrLdpNgHelloAdjMapEntry 1 }

vRtrLdpNgHelloAdjMapLdpId        OBJECT-TYPE
    SYNTAX      TmnxMplsLdpNgIdentifier (SIZE (6|18))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgHelloAdjMapLdpId is an index for the row entry. It indicates
         the LDP identifier of the peer."
    ::= { vRtrLdpNgHelloAdjMapEntry 2 }

vRtrLdpNgHelloAdjMapIndex        OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgHelloAdjMapIndex indicates the Hello adjacency
         index which is an index for MPLS-LDP-MIB::mplsLdpHelloAdjacencyEntry."
    ::= { vRtrLdpNgHelloAdjMapEntry 3 }

vLdpNgSvcFec129Table             OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgSvcFec129Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vLdpNgSvcFec129Table is a read-only table that represents all
         service FEC-129s either sent to or received from an LDP peer known to
         the Virtual Router."
    ::= { tmnxLdpNgObjs 26 }

vLdpNgSvcFec129Entry             OBJECT-TYPE
    SYNTAX      VLdpNgSvcFec129Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a service FEC-129 sent to or
         received from an LDP peer."
    INDEX       {
        vRtrID,
        vLdpNgFec128VcType,
        vLdpNgFec129AgiType,
        vLdpNgFec129AgiLen,
        vLdpNgFec129AgiVal,
        vLdpNgFec129SrcAiiType,
        vLdpNgFec129SrcAiiLen,
        vLdpNgFec129SrcAiiVal,
        vLdpNgFec129TgtAiiType,
        vLdpNgFec129TgtAiiLen,
        vLdpNgFec129TgtAiiVal,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId
    }
    ::= { vLdpNgSvcFec129Table 1 }

VLdpNgSvcFec129Entry             ::= SEQUENCE
{
    vLdpNgFec129AgiType              Unsigned32,
    vLdpNgFec129AgiLen               Unsigned32,
    vLdpNgFec129AgiVal               OCTET STRING,
    vLdpNgFec129SrcAiiType           Unsigned32,
    vLdpNgFec129SrcAiiLen            Unsigned32,
    vLdpNgFec129SrcAiiVal            OCTET STRING,
    vLdpNgFec129TgtAiiType           Unsigned32,
    vLdpNgFec129TgtAiiLen            Unsigned32,
    vLdpNgFec129TgtAiiVal            OCTET STRING,
    vLdpNgFec129ServType             ServType,
    vLdpNgFec129ServId               TmnxServId,
    vLdpNgFec129VpnId                TmnxVpnId,
    vLdpNgFec129Flags                TmnxLdpFECFlags,
    vLdpNgFec129NumInLabels          Unsigned32,
    vLdpNgFec129NumOutLabels         Unsigned32,
    vLdpNgFec129SdpId                SdpId,
    vLdpNgFec129MateAgiType          Unsigned32,
    vLdpNgFec129MateAgiLen           Unsigned32,
    vLdpNgFec129MateAgiVal           OCTET STRING,
    vLdpNgFec129MateSrcAiiType       Unsigned32,
    vLdpNgFec129MateSrcAiiLen        Unsigned32,
    vLdpNgFec129MateSrcAiiVal        OCTET STRING,
    vLdpNgFec129MateTgtAiiType       Unsigned32,
    vLdpNgFec129MateTgtAiiLen        Unsigned32,
    vLdpNgFec129MateTgtAiiVal        OCTET STRING,
    vLdpNgFec129MateSdpId            SdpId
}

vLdpNgFec129AgiType              OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129AgiType specifies the type of the Attachment
         Group Identifier TLV associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 1 }

vLdpNgFec129AgiLen               OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129AgiLen specifies the length of the Attachment
         Group Identifier TLV associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 2 }

vLdpNgFec129AgiVal               OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129AgiVal specifies the value of the Attachment
         Group Identifier TLV associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 3 }

vLdpNgFec129SrcAiiType           OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129SrcAiiType specifies the type of the Source
         Attachment Individual Identifier TLV associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 4 }

vLdpNgFec129SrcAiiLen            OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129SrcAiiLen specifies the length of the Source
         Attachment Individual Identifier TLV associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 5 }

vLdpNgFec129SrcAiiVal            OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129SrcAiiVal specifies the value of the Source
         Attachment Individual Identifier TLV associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 6 }

vLdpNgFec129TgtAiiType           OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129TgtAiiType specifies the type of the Target
         Attachment Individual Identifier TLV associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 7 }

vLdpNgFec129TgtAiiLen            OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129TgtAiiLen specifies the length of the Target
         Attachment Individual Identifier TLV associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 8 }

vLdpNgFec129TgtAiiVal            OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129TgtAiiVal specifies the value of the Target
         Attachment Individual Identifier TLV associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 9 }

vLdpNgFec129ServType             OBJECT-TYPE
    SYNTAX      ServType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129ServType indicates the Service type
         associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 10 }

vLdpNgFec129ServId               OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129ServId indicates the Service identifier
         associated with this service FEC."
    ::= { vLdpNgSvcFec129Entry 11 }

vLdpNgFec129VpnId                OBJECT-TYPE
    SYNTAX      TmnxVpnId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129VpnId identifies the VPN associated with the
         FEC."
    ::= { vLdpNgSvcFec129Entry 12 }

vLdpNgFec129Flags                OBJECT-TYPE
    SYNTAX      TmnxLdpFECFlags
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129Flags indicates the characteristics of the
         FEC."
    ::= { vLdpNgSvcFec129Entry 13 }

vLdpNgFec129NumInLabels          OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129NumInLabels indicates the number of labels
         that have been sent to the peer associated with this FEC."
    ::= { vLdpNgSvcFec129Entry 14 }

vLdpNgFec129NumOutLabels         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129NumOutLabels indicates the number of labels
         that have been received from the peer associated with this FEC."
    ::= { vLdpNgSvcFec129Entry 15 }

vLdpNgFec129SdpId                OBJECT-TYPE
    SYNTAX      SdpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129SdpId indicates the SDP associated with this
         peer."
    ::= { vLdpNgSvcFec129Entry 16 }

vLdpNgFec129MateAgiType          OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129MateAgiType indicates the type of the
         Attachment Group Identifier TLV switched with this service FEC."
    ::= { vLdpNgSvcFec129Entry 17 }

vLdpNgFec129MateAgiLen           OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129MateAgiLen indicates the length of the
         Attachment Group Identifier TLV switched with this service FEC."
    ::= { vLdpNgSvcFec129Entry 18 }

vLdpNgFec129MateAgiVal           OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129MateAgiVal indicates the value of the
         Attachment Group Identifier TLV switched with this service FEC."
    ::= { vLdpNgSvcFec129Entry 19 }

vLdpNgFec129MateSrcAiiType       OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129MateSrcAiiType indicates the type of the
         Source Attachment Individual Identifier TLV switched with this service
         FEC."
    ::= { vLdpNgSvcFec129Entry 20 }

vLdpNgFec129MateSrcAiiLen        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129MateSrcAiiLen indicates the length of the
         Source Attachment Individual Identifier TLV switched with this service
         FEC."
    ::= { vLdpNgSvcFec129Entry 21 }

vLdpNgFec129MateSrcAiiVal        OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129MateSrcAiiVal indicates the value of the
         Source Attachment Individual Identifier TLV switched with this service
         FEC."
    ::= { vLdpNgSvcFec129Entry 22 }

vLdpNgFec129MateTgtAiiType       OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129MateTgtAiiType indicates the type of the
         Target Attachment Individual Identifier TLV switched with this service
         FEC."
    ::= { vLdpNgSvcFec129Entry 23 }

vLdpNgFec129MateTgtAiiLen        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129MateTgtAiiLen indicates the length of the
         Target Attachment Individual Identifier TLV switched with this service
         FEC."
    ::= { vLdpNgSvcFec129Entry 24 }

vLdpNgFec129MateTgtAiiVal        OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129MateTgtAiiVal indicates the value of the
         Target Attachment Individual Identifier TLV switched with this service
         FEC."
    ::= { vLdpNgSvcFec129Entry 25 }

vLdpNgFec129MateSdpId            OBJECT-TYPE
    SYNTAX      SdpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129MateSdpId indicates the SDP switched with
         this peer."
    ::= { vLdpNgSvcFec129Entry 26 }

vLdpNgSvcFec129InLblTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgSvcFec129InLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vLdpNgSvcFec129InLblTable is a read-only table that represents all
         service FEC-129s received from an LDP peer known to the Virtual
         Router."
    ::= { tmnxLdpNgObjs 27 }

vLdpNgSvcFec129InLblEntry        OBJECT-TYPE
    SYNTAX      VLdpNgSvcFec129InLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a service FEC-129 received
         from an LDP peer."
    INDEX       {
        vRtrID,
        vLdpNgFec128VcType,
        vLdpNgFec129AgiType,
        vLdpNgFec129AgiLen,
        vLdpNgFec129AgiVal,
        vLdpNgFec129SrcAiiType,
        vLdpNgFec129SrcAiiLen,
        vLdpNgFec129SrcAiiVal,
        vLdpNgFec129TgtAiiType,
        vLdpNgFec129TgtAiiLen,
        vLdpNgFec129TgtAiiVal,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vLdpNgFec129InLblId
    }
    ::= { vLdpNgSvcFec129InLblTable 1 }

VLdpNgSvcFec129InLblEntry        ::= SEQUENCE
{
    vLdpNgFec129InLblId              Unsigned32,
    vLdpNgFec129InLabel              Unsigned32,
    vLdpNgFec129InLabelStatus        TmnxLabelStatus,
    vLdpNgFec129InLblMTU             Unsigned32,
    vLdpNgFec129InLblVlanTag         Unsigned32,
    vLdpNgFec129InLblMaxCellConcat   Unsigned32,
    vLdpNgFec129InLblSigStatus       TmnxLabelSigStatus,
    vLdpNgFec129InLblIPv4Cap         TruthValue,
    vLdpNgFec129InLblIPv6Cap         TruthValue,
    vLdpNgFec129InLblIPv4CeAddrType  InetAddressType,
    vLdpNgFec129InLblIPv4CeIpAddr    InetAddress,
    vLdpNgFec129InLblWdwReason       TmnxLdpInLblWdrawalReasonCode,
    vLdpNgFec129InLblFLTxCap         TruthValue,
    vLdpNgFec129InLblFLRxCap         TruthValue,
    vLdpNgFec129InLblVccvCV          BITS,
    vLdpNgFec129InLblVccvCC          BITS,
    vLdpNgFec129InLblPwStatus        TruthValue
}

vLdpNgFec129InLblId              OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblId indicates the label number of the
         ingress label exchanged."
    ::= { vLdpNgSvcFec129InLblEntry 1 }

vLdpNgFec129InLabel              OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLabel indicates the ingress label
         exchanged."
    ::= { vLdpNgSvcFec129InLblEntry 2 }

vLdpNgFec129InLabelStatus        OBJECT-TYPE
    SYNTAX      TmnxLabelStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLabelStatus indicates the status of the
         ingress label."
    ::= { vLdpNgSvcFec129InLblEntry 3 }

vLdpNgFec129InLblMTU             OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblMTU indicates the largest service frame
         size (in octets) that can be handled by the local ESR."
    ::= { vLdpNgSvcFec129InLblEntry 4 }

vLdpNgFec129InLblVlanTag         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblVlanTag indicates the local tag on a
         VLAN VC type SDP binding."
    ::= { vLdpNgSvcFec129InLblEntry 5 }

vLdpNgFec129InLblMaxCellConcat   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblMaxCellConcat indicates the local
         maximum number of ATM cells to concatenate on a ATM cell-mode VC type
         SDP binding."
    ::= { vLdpNgSvcFec129InLblEntry 6 }

vLdpNgFec129InLblSigStatus       OBJECT-TYPE
    SYNTAX      TmnxLabelSigStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblSigStatus indicates the signaling status
         for vLdpNgFec129InLabel."
    ::= { vLdpNgSvcFec129InLblEntry 7 }

vLdpNgFec129InLblIPv4Cap         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblIPv4Cap indicates whether or not the
         local ipv4 stack capability is supported for this LDP peer.

         The value of vLdpNgFec129InLblIPv4Cap is 'true' when the local ipv4
         stack capability is supported and the value is 'false' when the local
         ipv4 stack capability is not supported."
    ::= { vLdpNgSvcFec129InLblEntry 8 }

vLdpNgFec129InLblIPv6Cap         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblIPv6Cap indicates whether or not the
         local ipv6 stack capability is supported for this LDP peer.

         The value of vLdpNgFec129InLblIPv6Cap is 'true' when the local ipv6
         stack capability is supported and the value is 'false' when the local
         ipv6 stack capability is not supported."
    ::= { vLdpNgSvcFec129InLblEntry 9 }

vLdpNgFec129InLblIPv4CeAddrType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblIPv4CeAddrType indicates the local CE
         Address type of the object indicated by vLdpNgFec129InLblIPv4CeIpAddr."
    ::= { vLdpNgSvcFec129InLblEntry 10 }

vLdpNgFec129InLblIPv4CeIpAddr    OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblIPv4CeIpAddr indicates the local CE
         Address."
    ::= { vLdpNgSvcFec129InLblEntry 11 }

vLdpNgFec129InLblWdwReason       OBJECT-TYPE
    SYNTAX      TmnxLdpInLblWdrawalReasonCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblWdwReason indicates the reason of
         withdrawal of ingress label value in vLdpNgFec129InLabel."
    ::= { vLdpNgSvcFec129InLblEntry 12 }

vLdpNgFec129InLblFLTxCap         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblFLTxCap indicates whether or not this
         LDP peer is capable of sending Flow Label in its pseudowire (PW)
         packet.

         The value of vLdpNgFec129InLblFLTxCap is 'true' when this LDP peer is
         capable of sending Flow Label and the value is 'false' when the peer
         is not capable of sending Flow Label in pseudowire packet."
    ::= { vLdpNgSvcFec129InLblEntry 13 }

vLdpNgFec129InLblFLRxCap         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblFLRxCap indicates whether or not this
         LDP peer is capable of receiving Flow Label in its pseudowire packet.

         The value of vLdpNgFec129InLblFLRxCap is 'true' when this LDP peer is
         capable of receiving Flow Label and the value is 'false' when the peer
         is not capable of receiving Flow Label in pseudowire packet."
    ::= { vLdpNgSvcFec129InLblEntry 14 }

vLdpNgFec129InLblVccvCV          OBJECT-TYPE
    SYNTAX      BITS {
        icmpPing                 (0),
        lspPing                  (1),
        bfdFaultDetect           (2),
        bfdFaultDetectSignalling (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblVccvCV indicates the CV (Connectivity
         Verification) types supported by local LSR if it supports VCCV on
         pseudowire. If VCCV is not supported, vLdpNgFec129InLblVccvCV will be
         set to 0."
    ::= { vLdpNgSvcFec129InLblEntry 15 }

vLdpNgFec129InLblVccvCC          OBJECT-TYPE
    SYNTAX      BITS {
        pwe3ControlWord   (0),
        routerAlertLabel  (1),
        mplsDemuxLabelTL1 (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblVccvCC indicates the CC (Control
         Channel) types supported by local LSR if it supports VCCV on
         pseudowire. If VCCV is not supported, vLdpNgFec129InLblVccvCC will be
         set to 0."
    ::= { vLdpNgSvcFec129InLblEntry 16 }

vLdpNgFec129InLblPwStatus        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129InLblPwStatus indicates whether the local LSR
         supports pseudowire status signaling."
    ::= { vLdpNgSvcFec129InLblEntry 17 }

vLdpNgSvcFec129OutLblTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgSvcFec129OutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vLdpNgSvcFec129OutLblTable is a read-only table that represents
         all service FEC-129s sent to an LDP peer known to the Virtual Router."
    ::= { tmnxLdpNgObjs 28 }

vLdpNgSvcFec129OutLblEntry       OBJECT-TYPE
    SYNTAX      VLdpNgSvcFec129OutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a service FEC-129 sent to an
         LDP peer."
    INDEX       {
        vRtrID,
        vLdpNgFec128VcType,
        vLdpNgFec129AgiType,
        vLdpNgFec129AgiLen,
        vLdpNgFec129AgiVal,
        vLdpNgFec129SrcAiiType,
        vLdpNgFec129SrcAiiLen,
        vLdpNgFec129SrcAiiVal,
        vLdpNgFec129TgtAiiType,
        vLdpNgFec129TgtAiiLen,
        vLdpNgFec129TgtAiiVal,
        vRtrLdpNgPeerLdpIdType,
        vRtrLdpNgPeerLdpId,
        vLdpNgFec129OutLblId
    }
    ::= { vLdpNgSvcFec129OutLblTable 1 }

VLdpNgSvcFec129OutLblEntry       ::= SEQUENCE
{
    vLdpNgFec129OutLblId             Unsigned32,
    vLdpNgFec129OutLabel             Unsigned32,
    vLdpNgFec129OutLabelStatus       TmnxLabelStatus,
    vLdpNgFec129OutLblMTU            Unsigned32,
    vLdpNgFec129OutLblVlanTag        Unsigned32,
    vLdpNgFec129OutLblMaxCellConcat  Unsigned32,
    vLdpNgFec129OutLblSigStatus      TmnxLabelSigStatus,
    vLdpNgFec129OutLblIPv4Cap        TruthValue,
    vLdpNgFec129OutLblIPv6Cap        TruthValue,
    vLdpNgFec129OutLblIPv4CeAddrType InetAddressType,
    vLdpNgFec129OutLblIPv4CeIpAddr   InetAddress,
    vLdpNgFec129OutLblFLTxCap        TruthValue,
    vLdpNgFec129OutLblFLRxCap        TruthValue,
    vLdpNgFec129OutLblVccvCV         BITS,
    vLdpNgFec129OutLblVccvCC         BITS,
    vLdpNgFec129OutLblPwStatus       TruthValue
}

vLdpNgFec129OutLblId             OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblId indicates the label number of the
         egress label exchanged."
    ::= { vLdpNgSvcFec129OutLblEntry 1 }

vLdpNgFec129OutLabel             OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLabel indicates the egress label
         exchanged."
    ::= { vLdpNgSvcFec129OutLblEntry 2 }

vLdpNgFec129OutLabelStatus       OBJECT-TYPE
    SYNTAX      TmnxLabelStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLabelStatus indicates the status of the
         egress label"
    ::= { vLdpNgSvcFec129OutLblEntry 3 }

vLdpNgFec129OutLblMTU            OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblMTU indicates the largest service frame
         size (in octets) that can be handled by the remote ESR."
    ::= { vLdpNgSvcFec129OutLblEntry 4 }

vLdpNgFec129OutLblVlanTag        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblVlanTag indicates the remote tag on a
         VLAN VC type SDP binding."
    ::= { vLdpNgSvcFec129OutLblEntry 5 }

vLdpNgFec129OutLblMaxCellConcat  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblMaxCellConcat indicates the remote
         maximum number of ATM cells to concatenate on a ATM cell-mode VC type
         SDP binding."
    ::= { vLdpNgSvcFec129OutLblEntry 6 }

vLdpNgFec129OutLblSigStatus      OBJECT-TYPE
    SYNTAX      TmnxLabelSigStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblSigStatus indicates the signaling
         status for vLdpNgFec129OutLabel."
    ::= { vLdpNgSvcFec129OutLblEntry 7 }

vLdpNgFec129OutLblIPv4Cap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblIPv4Cap indicates whether or not the
         remote ipv4 stack capability is supported for this LDP peer.

         The value of vLdpNgFec129OutLblIPv4Cap is 'true' when the remote ipv4
         stack capability is supported and the value is 'false' when the remote
         ipv4 stack capability is not supported."
    ::= { vLdpNgSvcFec129OutLblEntry 8 }

vLdpNgFec129OutLblIPv6Cap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblIPv6Cap indicates whether or not the
         remote ipv6 stack capability is supported for this LDP peer.

         The value of vLdpNgFec129OutLblIPv6Cap is 'true' when the remote ipv6
         stack capability is supported and the value is 'false' when the remote
         ipv6 stack capability is not supported."
    ::= { vLdpNgSvcFec129OutLblEntry 9 }

vLdpNgFec129OutLblIPv4CeAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblIPv4CeAddrType indicates the remote CE
         Address type of the object indicated by
         vLdpNgFec129OutLblIPv4CeIpAddr."
    ::= { vLdpNgSvcFec129OutLblEntry 10 }

vLdpNgFec129OutLblIPv4CeIpAddr   OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblIPv4CeIpAddr indicates the remote CE
         Address."
    ::= { vLdpNgSvcFec129OutLblEntry 11 }

vLdpNgFec129OutLblFLTxCap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblFLTxCap indicates whether or not the
         remote LDP peer is capable of sending Flow Label in its pseudowire
         packet.

         The value of vLdpNgFec129OutLblFLTxCap is 'true' when the remote LDP
         peer is capable of sending Flow Label and the value is 'false' when
         the peer is not capable of sending Flow Label in pseudowire packet."
    ::= { vLdpNgSvcFec129OutLblEntry 12 }

vLdpNgFec129OutLblFLRxCap        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblFLRxCap indicates whether or not the
         remote LDP peer is capable of receiving Flow Label in its pseudowire
         packet.

         The value of vLdpNgFec129OutLblFLRxCap is 'true' when the remote LDP
         peer is capable of receiving Flow Label and the value is 'false' when
         the peer is not capable of receiving Flow Label in pseudowire packet."
    ::= { vLdpNgSvcFec129OutLblEntry 13 }

vLdpNgFec129OutLblVccvCV         OBJECT-TYPE
    SYNTAX      BITS {
        icmpPing                 (0),
        lspPing                  (1),
        bfdFaultDetect           (2),
        bfdFaultDetectSignalling (3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblVccvCV indicates the CV (Connectivity
         Verification) types supported by remote LSR if it supports VCCV on
         pseudowire. If VCCV is not supported, vLdpNgFec129OutLblVccvCV will be
         set to 0."
    ::= { vLdpNgSvcFec129OutLblEntry 14 }

vLdpNgFec129OutLblVccvCC         OBJECT-TYPE
    SYNTAX      BITS {
        pwe3ControlWord   (0),
        routerAlertLabel  (1),
        mplsDemuxLabelTL1 (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblVccvCC indicates the CC (Control
         Channel) types supported by remote LSR if it supports VCCV on
         pseudowire. If VCCV is not supported, vLdpNgFec129OutLblVccvCC will be
         set to 0."
    ::= { vLdpNgSvcFec129OutLblEntry 15 }

vLdpNgFec129OutLblPwStatus       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgFec129OutLblPwStatus indicates whether the remote
         LSR supports pseudowire status signaling."
    ::= { vLdpNgSvcFec129OutLblEntry 16 }

vLdpNgCepTdmFec128InLblTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgCepTdmFec128InLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vLdpNgCepTdmFec128InLblTable is a read-only table that represents
         all CEP/TDM FECs received from an LDP peer known to the Virtual
         Router. The CEP/TDM Sub-TLVs are defined in RFC 4446:

         Parameter Id    Description
         0x04            CEP/TDM Payload Bytes
         0x07            CEP/TDM bit-rate
         0x0B            TDM Options."
    ::= { tmnxLdpNgObjs 29 }

vLdpNgCepTdmFec128InLblEntry     OBJECT-TYPE
    SYNTAX      VLdpNgCepTdmFec128InLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a service FEC 128 sent to or
         received from an LDP peer.

         Use of AUGMENTS clause implies a one-to-one dependent relationship
         between the base table, vLdpNgSvcFec128InLblTable, and the augmenting
         table, vLdpNgCepTdmFec128InLblTable.  This in effect extends the
         vLdpNgSvcFec128InLblTable with additional columns.

          Creation or deletion of a row in the vLdpNgSvcFec128InLblTable results
          in the same fate for the row in the vLdpNgCepTdmFec128InLblEntry."
    AUGMENTS    { vLdpNgSvcFec128InLblEntry }
    ::= { vLdpNgCepTdmFec128InLblTable 1 }

VLdpNgCepTdmFec128InLblEntry     ::= SEQUENCE
{
    vLdpNgCepTdmFec128InLblPayldSize Unsigned32,
    vLdpNgCepTdmFec128InLblBitrate   Unsigned32,
    vLdpNgCepTdmFec128InLblRtpHeader TruthValue,
    vLdpNgCepTdmFec128InLblDiffTStmp TruthValue,
    vLdpNgCepTdmFec128InLblSigPkts   TdmOptionsSigPkts,
    vLdpNgCepTdmFec128InLblCasTrunk  TdmOptionsCasTrunkFraming,
    vLdpNgCepTdmFec128InLblTStmpFreq Unsigned32,
    vLdpNgCepTdmFec128InLblPayldType Unsigned32,
    vLdpNgCepTdmFec128InLblSsrcId    Unsigned32
}

vLdpNgCepTdmFec128InLblPayldSize OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128InLblPayldSize indicates the local
         payload size."
    ::= { vLdpNgCepTdmFec128InLblEntry 1 }

vLdpNgCepTdmFec128InLblBitrate   OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "sixty-four kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128InLblBitrate indicates the local
         bitrate."
    ::= { vLdpNgCepTdmFec128InLblEntry 2 }

vLdpNgCepTdmFec128InLblRtpHeader OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128InLblRtpHeader indicates the local RTP
         header usage bit."
    ::= { vLdpNgCepTdmFec128InLblEntry 3 }

vLdpNgCepTdmFec128InLblDiffTStmp OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128InLblDiffTStmp indicates the local
         differential (or dynamic) timestamping mode bit."
    ::= { vLdpNgCepTdmFec128InLblEntry 4 }

vLdpNgCepTdmFec128InLblSigPkts   OBJECT-TYPE
    SYNTAX      TdmOptionsSigPkts
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128InLblSigPkts indicates the local CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec128InLblEntry 5 }

vLdpNgCepTdmFec128InLblCasTrunk  OBJECT-TYPE
    SYNTAX      TdmOptionsCasTrunkFraming
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128InLblCasTrunk indicates the local CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec128InLblEntry 6 }

vLdpNgCepTdmFec128InLblTStmpFreq OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "8 KHz"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128InLblTStmpFreq indicates the local CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec128InLblEntry 7 }

vLdpNgCepTdmFec128InLblPayldType OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128InLblPayldType indicates the local
         payload type."
    ::= { vLdpNgCepTdmFec128InLblEntry 8 }

vLdpNgCepTdmFec128InLblSsrcId    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128InLblSsrcId indicates the local value
         of SSRC ID."
    ::= { vLdpNgCepTdmFec128InLblEntry 9 }

vLdpNgCepTdmFec128OutLblTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgCepTdmFec128OutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vLdpNgCepTdmFec128OutLblTable is a read-only table that represents
         all CEP/TDM FECs sent to an LDP peer known to the Virtual Router. The
         CEP/TDM Sub-TLVs are defined in RFC 4446:

         Parameter Id    Description
         0x04            CEP/TDM Payload Bytes
         0x07            CEP/TDM bit-rate
         0x0B            TDM Options."
    ::= { tmnxLdpNgObjs 30 }

vLdpNgCepTdmFec128OutLblEntry    OBJECT-TYPE
    SYNTAX      VLdpNgCepTdmFec128OutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a service FEC sent to or
         received from an LDP peer.

         Use of AUGMENTS clause implies a one-to-one dependent relationship
         between the base table, vLdpNgSvcFec128OutLblTable, and the augmenting
         table, vLdpNgCepTdmFec128OutLblTable.  This in effect extends the
         vLdpNgSvcFec128OutLblTable with additional columns.

          Creation or deletion of a row in the vLdpNgSvcFec128OutLblTable results
          in the same fate for the row in the vLdpNgCepTdmFec128OutLblEntry."
    AUGMENTS    { vLdpNgSvcFec128OutLblEntry }
    ::= { vLdpNgCepTdmFec128OutLblTable 1 }

VLdpNgCepTdmFec128OutLblEntry    ::= SEQUENCE
{
    vLdpNgCepTdmFec128OutLblPyldSze  Unsigned32,
    vLdpNgCepTdmFec128OutLblBitrate  Unsigned32,
    vLdpNgCepTdmFec128OutLblRtpHdr   TruthValue,
    vLdpNgCepTdmFec128OutLblDfTstmp  TruthValue,
    vLdpNgCepTdmFec128OutLblSigPkts  TdmOptionsSigPkts,
    vLdpNgCepTdmFec128OutLblCasTrnk  TdmOptionsCasTrunkFraming,
    vLdpNgCepTdmFec128OutLblTstmpFq  Unsigned32,
    vLdpNgCepTdmFec128OutLblPyldTyp  Unsigned32,
    vLdpNgCepTdmFec128OutLblSsrcId   Unsigned32
}

vLdpNgCepTdmFec128OutLblPyldSze  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128OutLblPyldSze indicates the remote
         payload size."
    ::= { vLdpNgCepTdmFec128OutLblEntry 1 }

vLdpNgCepTdmFec128OutLblBitrate  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "sixty-four kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128OutLblBitrate indicates the remote
         bitrate."
    ::= { vLdpNgCepTdmFec128OutLblEntry 2 }

vLdpNgCepTdmFec128OutLblRtpHdr   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128OutLblRtpHdr indicates the remote RTP
         header usage bit."
    ::= { vLdpNgCepTdmFec128OutLblEntry 3 }

vLdpNgCepTdmFec128OutLblDfTstmp  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128OutLblDfTstmp indicates the remote
         differential (or dynamic) timestamping mode bit."
    ::= { vLdpNgCepTdmFec128OutLblEntry 4 }

vLdpNgCepTdmFec128OutLblSigPkts  OBJECT-TYPE
    SYNTAX      TdmOptionsSigPkts
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128OutLblSigPkts indicates the remote CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec128OutLblEntry 5 }

vLdpNgCepTdmFec128OutLblCasTrnk  OBJECT-TYPE
    SYNTAX      TdmOptionsCasTrunkFraming
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128OutLblCasTrnk indicates the remote CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec128OutLblEntry 6 }

vLdpNgCepTdmFec128OutLblTstmpFq  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "8 KHz"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128OutLblTstmpFq indicates the remote CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec128OutLblEntry 7 }

vLdpNgCepTdmFec128OutLblPyldTyp  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128OutLblPyldTyp indicates the remote
         payload type."
    ::= { vLdpNgCepTdmFec128OutLblEntry 8 }

vLdpNgCepTdmFec128OutLblSsrcId   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec128OutLblSsrcId indicates the remote value
         of SSRC ID."
    ::= { vLdpNgCepTdmFec128OutLblEntry 9 }

vLdpNgCepTdmFec129InLblTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgCepTdmFec129InLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vLdpNgCepTdmFec129InLblTable is a read-only table that represents
         all CEP/TDM FECs received from an LDP peer known to the Virtual
         Router. The CEP/TDM Sub-TLVs are defined in RFC 4446:

         Parameter Id    Description
         0x04            CEP/TDM Payload Bytes
         0x07            CEP/TDM bit-rate
         0x0B            TDM Options."
    ::= { tmnxLdpNgObjs 31 }

vLdpNgCepTdmFec129InLblEntry     OBJECT-TYPE
    SYNTAX      VLdpNgCepTdmFec129InLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a service FEC received from
         an LDP peer.

         Use of AUGMENTS clause implies a one-to-one dependent relationship
         between the base table, vLdpNgSvcFec129InLblTable, and the augmenting
         table, vLdpNgCepTdmFec129InLblTable.  This in effect extends the
         vLdpNgSvcFec129InLblTable with additional columns.

          Creation or deletion of a row in the vLdpNgSvcFec129InLblTable results
          in the same fate for the row in the VLdpNgCepTdmFec129InLblEntry."
    AUGMENTS    { vLdpNgSvcFec129InLblEntry }
    ::= { vLdpNgCepTdmFec129InLblTable 1 }

VLdpNgCepTdmFec129InLblEntry     ::= SEQUENCE
{
    vLdpNgCepTdmFec129InLblPayldSize Unsigned32,
    vLdpNgCepTdmFec129InLblBitrate   Unsigned32,
    vLdpNgCepTdmFec129InLblRtpHeader TruthValue,
    vLdpNgCepTdmFec129InLblDiffTStmp TruthValue,
    vLdpNgCepTdmFec129InLblSigPkts   TdmOptionsSigPkts,
    vLdpNgCepTdmFec129InLblCasTrunk  TdmOptionsCasTrunkFraming,
    vLdpNgCepTdmFec129InLblTStmpFreq Unsigned32,
    vLdpNgCepTdmFec129InLblPayldType Unsigned32,
    vLdpNgCepTdmFec129InLblSsrcId    Unsigned32
}

vLdpNgCepTdmFec129InLblPayldSize OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129InLblPayldSize indicates the local
         payload size."
    ::= { vLdpNgCepTdmFec129InLblEntry 1 }

vLdpNgCepTdmFec129InLblBitrate   OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "sixty-four kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129InLblBitrate indicates the local
         bitrate."
    ::= { vLdpNgCepTdmFec129InLblEntry 2 }

vLdpNgCepTdmFec129InLblRtpHeader OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129InLblRtpHeader indicates the local RTP
         header usage bit."
    ::= { vLdpNgCepTdmFec129InLblEntry 3 }

vLdpNgCepTdmFec129InLblDiffTStmp OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129InLblDiffTStmp indicates the local
         differential (or dynamic) timestamping mode bit."
    ::= { vLdpNgCepTdmFec129InLblEntry 4 }

vLdpNgCepTdmFec129InLblSigPkts   OBJECT-TYPE
    SYNTAX      TdmOptionsSigPkts
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129InLblSigPkts indicates the local CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec129InLblEntry 5 }

vLdpNgCepTdmFec129InLblCasTrunk  OBJECT-TYPE
    SYNTAX      TdmOptionsCasTrunkFraming
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129InLblCasTrunk indicates the local CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec129InLblEntry 6 }

vLdpNgCepTdmFec129InLblTStmpFreq OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "8 KHz"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129InLblTStmpFreq indicates the local CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec129InLblEntry 7 }

vLdpNgCepTdmFec129InLblPayldType OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129InLblPayldType indicates the local
         payload type."
    ::= { vLdpNgCepTdmFec129InLblEntry 8 }

vLdpNgCepTdmFec129InLblSsrcId    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129InLblSsrcId indicates the local value
         of SSRC ID."
    ::= { vLdpNgCepTdmFec129InLblEntry 9 }

vLdpNgCepTdmFec129OutLblTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgCepTdmFec129OutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vLdpNgCepTdmFec129OutLblTable is a read-only table that represents
         all CEP/TDM FECs sent to an LDP peer known to the Virtual Router. The
         CEP/TDM Sub-TLVs are defined in RFC 4446:

         Parameter Id    Description
         0x04            CEP/TDM Payload Bytes
         0x07            CEP/TDM bit-rate
         0x0B            TDM Options."
    ::= { tmnxLdpNgObjs 32 }

vLdpNgCepTdmFec129OutLblEntry    OBJECT-TYPE
    SYNTAX      VLdpNgCepTdmFec129OutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of a service FEC sent to an LDP
         peer.

         Use of AUGMENTS clause implies a one-to-one dependent relationship
         between the base table, vLdpNgSvcFec129OutLblTable, and the augmenting
         table, vLdpNgCepTdmFec129OutLblTable.  This in effect extends the
         vLdpNgSvcFec129OutLblTable with additional columns.

         Creation or deletion of a row in the vLdpNgSvcFec129OutLblTable
         results in the same fate for the row in the
         VLdpNgCepTdmFec129OutLblEntry."
    AUGMENTS    { vLdpNgSvcFec129OutLblEntry }
    ::= { vLdpNgCepTdmFec129OutLblTable 1 }

VLdpNgCepTdmFec129OutLblEntry    ::= SEQUENCE
{
    vLdpNgCepTdmFec129OutLblPyldSize Unsigned32,
    vLdpNgCepTdmFec129OutLblBitrate  Unsigned32,
    vLdpNgCepTdmFec129OutLblRtpHdr   TruthValue,
    vLdpNgCepTdmFec129OutLblDifTStmp TruthValue,
    vLdpNgCepTdmFec129OutLblSigPkts  TdmOptionsSigPkts,
    vLdpNgCepTdmFec129OutLblCasTrnk  TdmOptionsCasTrunkFraming,
    vLdpNgCepTdmFec129OutLblTStmpFrq Unsigned32,
    vLdpNgCepTdmFec129OutLblPyldType Unsigned32,
    vLdpNgCepTdmFec129OutLblSsrcId   Unsigned32
}

vLdpNgCepTdmFec129OutLblPyldSize OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "bytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129OutLblPyldSize indicates the remote
         payload size."
    ::= { vLdpNgCepTdmFec129OutLblEntry 1 }

vLdpNgCepTdmFec129OutLblBitrate  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "sixty-four kilobps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129OutLblBitrate indicates the remote
         bitrate."
    ::= { vLdpNgCepTdmFec129OutLblEntry 2 }

vLdpNgCepTdmFec129OutLblRtpHdr   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129OutLblRtpHdr indicates the remote RTP
         header usage bit."
    ::= { vLdpNgCepTdmFec129OutLblEntry 3 }

vLdpNgCepTdmFec129OutLblDifTStmp OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129OutLblDifTStmp indicates the remote
         differential (or dynamic) timestamping mode bit."
    ::= { vLdpNgCepTdmFec129OutLblEntry 4 }

vLdpNgCepTdmFec129OutLblSigPkts  OBJECT-TYPE
    SYNTAX      TdmOptionsSigPkts
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129OutLblSigPkts indicates the remote CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec129OutLblEntry 5 }

vLdpNgCepTdmFec129OutLblCasTrnk  OBJECT-TYPE
    SYNTAX      TdmOptionsCasTrunkFraming
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129OutLblCasTrnk indicates the remote CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec129OutLblEntry 6 }

vLdpNgCepTdmFec129OutLblTStmpFrq OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "8 KHz"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129OutLblTStmpFrq indicates the remote CE
         application signalling packets mode."
    ::= { vLdpNgCepTdmFec129OutLblEntry 7 }

vLdpNgCepTdmFec129OutLblPyldType OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129OutLblPyldType indicates the remote
         payload type."
    ::= { vLdpNgCepTdmFec129OutLblEntry 8 }

vLdpNgCepTdmFec129OutLblSsrcId   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgCepTdmFec129OutLblSsrcId indicates the remote value
         of SSRC ID."
    ::= { vLdpNgCepTdmFec129OutLblEntry 9 }

vRtrLdpNgStaticFecTableLstCh     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgStaticFecTableLstCh indicates the last timestamp
         when an entry in the vRtrLdpNgStaticFecTable was last changed."
    ::= { tmnxLdpNgObjs 33 }

vRtrLdpNgStaticFecTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgStaticFecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgStaticFecTable has an entry for each static prefix FEC
         configured on the virtual router."
    ::= { tmnxLdpNgObjs 34 }

vRtrLdpNgStaticFecEntry          OBJECT-TYPE
    SYNTAX      VRtrLdpNgStaticFecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a static prefix FEC configured on the
         virtual router.

         Entries can be created and deleted via SNMP SET operations to
         vRtrLdpNgStaticFecRowStatus.

         An entry is created by setting vRtrLdpNgStaticFecRowStatus to
         'createAndGo'.

         An entry is deleted by setting vRtrLdpNgStaticFecRowStatus to
         'destroy'."
    INDEX       {
        vRtrID,
        vRtrLdpNgStaticFecIpPrefixType,
        vRtrLdpNgStaticFecIpPrefix,
        vRtrLdpNgStaticFecIpPrefixLen
    }
    ::= { vRtrLdpNgStaticFecTable 1 }

VRtrLdpNgStaticFecEntry          ::= SEQUENCE
{
    vRtrLdpNgStaticFecIpPrefixType   InetAddressType,
    vRtrLdpNgStaticFecIpPrefix       InetAddress,
    vRtrLdpNgStaticFecIpPrefixLen    InetAddressPrefixLength,
    vRtrLdpNgStaticFecRowStatus      RowStatus,
    vRtrLdpNgStaticFecNumInLabel     Unsigned32,
    vRtrLdpNgStaticFecNumOutLabel    Unsigned32
}

vRtrLdpNgStaticFecIpPrefixType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgStaticFecIpPrefixType specifies the IP Address
         Prefix type for the static FEC indicated by
         vRtrLdpNgStaticFecIpPrefix."
    ::= { vRtrLdpNgStaticFecEntry 1 }

vRtrLdpNgStaticFecIpPrefix       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgStaticFecIpPrefix specifies the IP Address
         Prefix for this static FEC."
    ::= { vRtrLdpNgStaticFecEntry 2 }

vRtrLdpNgStaticFecIpPrefixLen    OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..128)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgStaticFecIpPrefixLen specifies the IP Address
         Mask length for this static FEC."
    ::= { vRtrLdpNgStaticFecEntry 3 }

vRtrLdpNgStaticFecRowStatus      OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgStaticFecRowStatus is used to create, delete or control
         entries in the vRtrLdpNgStaticFecTable.

         An entry is created by setting vRtrLdpNgStaticFecRowStatus
         'createAndGo'.

         An entry is deleted by setting vRtrLdpNgStaticFecRowStatus to
         'destroy'."
    ::= { vRtrLdpNgStaticFecEntry 4 }

vRtrLdpNgStaticFecNumInLabel     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgStaticFecNumInLabel indicates the number of in
         labels that are associated with the static prefix FEC represented by
         this row entry. This is also the number of row entries configured in
         the vRtrLdpNgStaticFecInLabelTable for this static prefix FEC.

         If the static FEC has no in labels associated with it, this value will
         be 0."
    ::= { vRtrLdpNgStaticFecEntry 5 }

vRtrLdpNgStaticFecNumOutLabel    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgStaticFecNumOutLabel indicates the number of out
         labels that are associated with the static prefix FEC represented by
         this row entry. This is also the number of row entries configured in
         the vRtrLdpNgStaticFecOutLabelTable for this static prefix FEC.

         If the static FEC has no out labels associated with it, this value
         will be 0."
    ::= { vRtrLdpNgStaticFecEntry 6 }

vRtrLdpNgStaticFecInLabelTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgStaticFecInLabelEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgStaticFecInLabelTable has an entry for each static prefix FEC
         in label configured on the virtual router."
    ::= { tmnxLdpNgObjs 35 }

vRtrLdpNgStaticFecInLabelEntry   OBJECT-TYPE
    SYNTAX      VRtrLdpNgStaticFecInLabelEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a static prefix FEC in label configured on
         the virtual router. The static prefix FEC corresponding to a in label
         entry must exist as a row entry in the vRtrLdpNgStaticFecTable.

         Entries can be created and deleted via SNMP SET operations to
         vRtrLdpNgSFecInLabelRowStatus.

         An entry is created by setting vRtrLdpNgSFecInLabelRowStatus to
         'createAndGo'.

         An entry is deleted by setting vRtrLdpNgSFecInLabelRowStatus to
         'destroy'."
    INDEX       {
        vRtrID,
        vRtrLdpNgStaticFecIpPrefixType,
        vRtrLdpNgStaticFecIpPrefix,
        vRtrLdpNgStaticFecIpPrefixLen,
        vRtrLdpNgSFecInLabel
    }
    ::= { vRtrLdpNgStaticFecInLabelTable 1 }

VRtrLdpNgStaticFecInLabelEntry   ::= SEQUENCE
{
    vRtrLdpNgSFecInLabel             Unsigned32,
    vRtrLdpNgSFecInLabelRowStatus    RowStatus,
    vRtrLdpNgSFecOperInLabel         Unsigned32
}

vRtrLdpNgSFecInLabel             OBJECT-TYPE
    SYNTAX      Unsigned32 (32..1048575 | 4294967295)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSFecInLabel indicates the label that is
         advertised to the upstream peer.

         The range of vRtrLdpNgSFecInLabel is dynamic and depends on the value
         of vRtrMplsLabelStaticLabelRange.

         The normal range of vRtrLdpNgSFecInLabel starts at 32 and ends at the
         value of vRtrMplsLabelStaticLabelRange + 31.

         If this variable is set to the value of 4294967295, the ingress label
         will be dynamically assigned by the label manager."
    ::= { vRtrLdpNgStaticFecInLabelEntry 1 }

vRtrLdpNgSFecInLabelRowStatus    OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgSFecInLabelRowStatus is used to create, delete or control
         entries in the vRtrLdpNgStaticFecInLabelTable.

         An entry is created by setting vRtrLdpNgSFecInLabelRowStatus to
         'createAndGo'.

         An entry is deleted by setting vRtrLdpNgSFecInLabelRowStatus to
         'destroy'."
    ::= { vRtrLdpNgStaticFecInLabelEntry 2 }

vRtrLdpNgSFecOperInLabel         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSFecOperInLabel indicates the actual or
         operational value of the label that was advertised to the upstream
         peer."
    ::= { vRtrLdpNgStaticFecInLabelEntry 3 }

vRtrLdpNgStaticFecOutLabelTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgStaticFecOutLabelEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgStaticFecOutLabelTable has an entry for each static prefix
         FEC out label configured on the virtual router."
    ::= { tmnxLdpNgObjs 36 }

vRtrLdpNgStaticFecOutLabelEntry  OBJECT-TYPE
    SYNTAX      VRtrLdpNgStaticFecOutLabelEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a static prefix FEC out label configured on
         the virtual router. The static prefix FEC corresponding to a in label
         entry must exist as a row entry in the vRtrLdpNgStaticFecTable. For
         vRtrLdpNgSFecOutLabelType 'pop' or 'swap' corresponding static FEC
         Prefix row entry must exist in vRtrLdpNgStaticFecInLabelTable

         Entries can be created and deleted via SNMP SET operations to
         vRtrLdpNgSFecOutLabelRowStatus.

         An entry is created by setting vRtrLdpNgSFecOutLabelRowStatus to
         'createAndGo'.

         An entry is deleted by setting vRtrLdpNgSFecOutLabelRowStatus to
         'destroy'."
    INDEX       {
        vRtrID,
        vRtrLdpNgStaticFecIpPrefixType,
        vRtrLdpNgStaticFecIpPrefix,
        vRtrLdpNgStaticFecIpPrefixLen,
        vRtrLdpNgSFecOutLabelType,
        vRtrLdpNgSFecOutLabelIfName,
        vRtrLdpNgSFecOutLabelIpAddrType,
        vRtrLdpNgSFecOutLabelIpAddr
    }
    ::= { vRtrLdpNgStaticFecOutLabelTable 1 }

VRtrLdpNgStaticFecOutLabelEntry  ::= SEQUENCE
{
    vRtrLdpNgSFecOutLabelType        INTEGER,
    vRtrLdpNgSFecOutLabelIfName      DisplayString,
    vRtrLdpNgSFecOutLabelIpAddrType  InetAddressType,
    vRtrLdpNgSFecOutLabelIpAddr      InetAddress,
    vRtrLdpNgSFecOutLabelRowStatus   RowStatus,
    vRtrLdpNgSFecOutLabel            Unsigned32
}

vRtrLdpNgSFecOutLabelType        OBJECT-TYPE
    SYNTAX      INTEGER {
        unknown (0),
        pop     (1),
        push    (2),
        swap    (3)
    }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSFecOutLabelType indicates operation type of
         this FEC."
    ::= { vRtrLdpNgStaticFecOutLabelEntry 1 }

vRtrLdpNgSFecOutLabelIfName      OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "If vRtrLdpNgSFecOutLabelType is set to 'swap' or 'push', the value of
         vRtrLdpNgSFecOutLabelIfName indicates the interface name to use for
         this static fec prefix.

         If vRtrLdpNgSFecOutLabelType is set to 'pop', the value of
         vRtrLdpNgSFecOutLabelIfName will be a null string."
    ::= { vRtrLdpNgStaticFecOutLabelEntry 2 }

vRtrLdpNgSFecOutLabelIpAddrType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSFecOutLabelIpAddrType indicates the IP address
         type for vRtrLdpNgSFecOutLabelIpAddr."
    ::= { vRtrLdpNgStaticFecOutLabelEntry 3 }

vRtrLdpNgSFecOutLabelIpAddr      OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "If vRtrLdpNgSFecOutLabelType is set to 'swap' or 'push', the value of
         vRtrLdpNgSFecOutLabelIpAddr indicates the IP address of the next-hop.

         If vRtrLdpNgSFecOutLabelType is set to 'pop', the value of
         vRtrLdpNgSFecOutLabelIpAddr will be 0.0.0.0"
    ::= { vRtrLdpNgStaticFecOutLabelEntry 4 }

vRtrLdpNgSFecOutLabelRowStatus   OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgSFecOutLabelRowStatus is used to create, delete or control
         entries in the vRtrLdpNgStaticFecOutLabelTable.

         An entry is created by setting vRtrLdpNgSFecOutLabelRowStatus to
         'createAndGo'.

         An entry is deleted by setting vRtrLdpNgSFecOutLabelRowStatus to
         'destroy'."
    ::= { vRtrLdpNgStaticFecOutLabelEntry 5 }

vRtrLdpNgSFecOutLabel            OBJECT-TYPE
    SYNTAX      Unsigned32 (16..1048575 | 4294967295)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSFecOutLabel specifies the egress label
         associated with this next-hop entry. The LSR will swap the incoming
         label with the configured egress label.

         If the value of vRtrLdpNgSFecOutLabel is set to 4294967295, the LSR
         will pop the incoming label."
    DEFVAL      { 4294967295 }
    ::= { vRtrLdpNgStaticFecOutLabelEntry 6 }

vRtrLdpNgTargPeerTableLstCh      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerTableLstCh indicates the last timestamp
         when an entry in the vRtrLdpNgTargPeerTable was last changed."
    ::= { tmnxLdpNgObjs 37 }

vRtrLdpNgTargPeerTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgTargPeerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgTargPeerTable provides an entry for each virtual router
         targeted peer configured to be used with the Label Distribution
         Protocol (LDP)."
    ::= { tmnxLdpNgObjs 38 }

vRtrLdpNgTargPeerEntry           OBJECT-TYPE
    SYNTAX      VRtrLdpNgTargPeerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents a targeted peer on this virtual router that
         participates in the LDP protocol.

         Row entries can be created or deleted via SNMP SET requests. A row
         with default attribute values is created by setting
         vRtrLdpNgTargPeerRowStatus to 'createAndGo'. A row entry can be
         destroyed by setting vRtrLdpNgTargPeerRowStatus to 'destroy'."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerAddressType,
        vRtrLdpNgPeerAddress
    }
    ::= { vRtrLdpNgTargPeerTable 1 }

VRtrLdpNgTargPeerEntry           ::= SEQUENCE
{
    vRtrLdpNgPeerAddressType         InetAddressType,
    vRtrLdpNgPeerAddress             InetAddress,
    vRtrLdpNgTargPeerRowStatus       RowStatus,
    vRtrLdpNgTargPeerLastChange      TimeStamp,
    vRtrLdpNgTargPeerAdminState      TmnxAdminState,
    vRtrLdpNgTargPeerOperState       TmnxOperState,
    vRtrLdpNgTargPeerUpTime          TimeInterval,
    vRtrLdpNgTargPeerOperDownReason  TmnxLdpIntTargOperDownReasonCode,
    vRtrLdpNgTargPeerInheritance     Unsigned32,
    vRtrLdpNgTargPeerKAFactor        TmnxLdpKeepAliveFactor,
    vRtrLdpNgTargPeerKATimeout       TmnxLdpNewKeepAliveTimeout,
    vRtrLdpNgTargPeerHelloFactor     TmnxLdpHelloFactor,
    vRtrLdpNgTargPeerHelloTimeout    TmnxLdpNewHelloTimeout,
    vRtrLdpNgTargPeerOprHelloTimeout TmnxLdpNewHelloTimeout,
    vRtrLdpNgTargPeerHelloReduction  TruthValue,
    vRtrLdpNgTargPeerHelloRdctnFctr  Unsigned32,
    vRtrLdpNgTargPeerBackoffTime     TmnxLdpBackoffTime,
    vRtrLdpNgTargPeerMaxBackoffTime  TmnxLdpBackoffTime,
    vRtrLdpNgTargPeerTunneling       TruthValue,
    vRtrLdpNgTargPeerBfdEnabled      TruthValue,
    vRtrLdpNgTargPeerLsrIfIndex      InterfaceIndexOrZero,
    vRtrLdpNgTargPeerAutoCreate      TruthValue,
    vRtrLdpNgTargPeerCreator         INTEGER,
    vRtrLdpNgTargPeerTemplName       TNamedItemOrEmpty,
    vRtrLdpNgTargPeerLocalIpAddrType InetAddressType,
    vRtrLdpNgTargPeerLocalIpAddress  InetAddress,
    vRtrLdpNgTargPeer32BitLsrFormat  TruthValue,
    vRtrLdpNgTargPeerLsrIdAdvert     TruthValue,
    vRtrLdpNgTargPeerCommunity       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargPeerMcastTunneling  TruthValue
}

vRtrLdpNgPeerAddressType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPeerAddressType specifies the address family
         type for vRtrLdpNgPeerAddress."
    ::= { vRtrLdpNgTargPeerEntry 1 }

vRtrLdpNgPeerAddress             OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgPeerAddress specifies the targeted peer IP address."
    ::= { vRtrLdpNgTargPeerEntry 2 }

vRtrLdpNgTargPeerRowStatus       OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgTargPeerRowStatus is used to control the creation and
         deletion of rows in the vRtrLdpNgTargPeerTable.

         A row can be created by setting vRtrLdpNgTargPeerRowStatus to
         'createAndGo'.  The agent should assign the default attribute values
         and change the row status to 'active'.

         A row entry can be destroyed by setting vRtrLdpNgTargPeerRowStatus to
         'destroy'."
    ::= { vRtrLdpNgTargPeerEntry 3 }

vRtrLdpNgTargPeerLastChange      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerLastChange indicates the sysUpTime when
         this row was last modified."
    ::= { vRtrLdpNgTargPeerEntry 4 }

vRtrLdpNgTargPeerAdminState      OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerAdminState specifies the desired
         administrative state for this LDP targeted peer."
    DEFVAL      { inService }
    ::= { vRtrLdpNgTargPeerEntry 5 }

vRtrLdpNgTargPeerOperState       OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerOperState indicates the current
         operational state of LDP targeted peer."
    ::= { vRtrLdpNgTargPeerEntry 6 }

vRtrLdpNgTargPeerUpTime          OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerUpTime indicates the time, in hundreds
         of seconds, that the targeted peer has been in current operational
         state vRtrLdpNgTargPeerOperState.

         If the value of vRtrLdpNgTargPeerOperState is 'inService (2)', then
         vRtrLdpNgTargPeerUpTime specifies the time that the targeted peer has
         been operationally up.

         If the value of vRtrLdpNgTargPeerOperState is 'outOfService (3)', then
         vRtrLdpNgTargPeerUpTime specifies the time that the targeted peer has
         been operationally down.

         If the value of vRtrLdpNgTargPeerOperState is 'transition (4)', then
         vRtrLdpNgTargPeerUpTime specifies the time that the targeted peer has
         been operationally in transition."
    ::= { vRtrLdpNgTargPeerEntry 7 }

vRtrLdpNgTargPeerOperDownReason  OBJECT-TYPE
    SYNTAX      TmnxLdpIntTargOperDownReasonCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerOperDownReason indicates the operational
         down reason for targeted peer."
    ::= { vRtrLdpNgTargPeerEntry 8 }

vRtrLdpNgTargPeerInheritance     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Some writable object in this row that can be configured to inherit its
         value from its corresponding object in the vRtrLdpNgGeneralTable.
         vRtrLdpNgTargPeerInheritance controls whether to inherit the
         operational value of that object, or to use the administratively set
         value.

         Non mask bits will always have value of zero, and any attempt to
         change the value will be silently discarded.

         When the bit for an object has value of one, then the object's
         administrative and operational value are whatever the DEFVAL or most
         recently SET value. The mask bit(s) will be set to one when SET is
         performed on the inherited object(s). Any attempt to set the mask bit
         to one will be silently discarded.

         When the bit for an object is set to zero, then the object's
         administrative and operational value are inherited from the
         corresponding object in vRtrLdpNgGeneralTable.

         This object is a bit-mask, with the following positions:
         vRtrLdpNgTargPeerKAFactor         0x1
         vRtrLdpNgTargPeerKATimeout        0x2
         vRtrLdpNgTargPeerHelloFactor      0x4
         vRtrLdpNgTargPeerHelloTimeout     0x8
         vRtrLdpNgTargPeerHelloReduction   0x10
         vRtrLdpNgTargPeerHelloRdctnFctr   0x20"
    DEFVAL      { 0 }
    ::= { vRtrLdpNgTargPeerEntry 9 }

vRtrLdpNgTargPeerKAFactor        OBJECT-TYPE
    SYNTAX      TmnxLdpKeepAliveFactor
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerKAFactor specifies the value by which
         the keepalive timeout (vRtrLdpNgTargPeerKATimeout) should be divided
         to give the keepalive time i.e. the time interval, in seconds, between
         LDP keepalive messages. LDP keepalive messages are sent to keep the
         LDP session from timing out when no other LDP traffic is being sent
         between the neighbors."
    DEFVAL      { 4 }
    ::= { vRtrLdpNgTargPeerEntry 10 }

vRtrLdpNgTargPeerKATimeout       OBJECT-TYPE
    SYNTAX      TmnxLdpNewKeepAliveTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerKATimeout specifies the time interval,
         in seconds, that LDP waits before tearing down a session. If no LDP
         messages are exchanged during this time interval, the LDP session is
         torn down. Generally the value of vRtrLdpNgTargPeerKATimeout is
         configured to be 3 times the keepalive time (the time interval between
         successive LDP keepalive messages)."
    DEFVAL      { 40 }
    ::= { vRtrLdpNgTargPeerEntry 11 }

vRtrLdpNgTargPeerHelloFactor     OBJECT-TYPE
    SYNTAX      TmnxLdpHelloFactor
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerHelloFactor specifies the value by which
         the hello timeout (vRtrLdpNgTargPeerHelloTimeout) should be divided to
         give the hello time i.e. the time interval, in seconds, between LDP
         Hello messages. LDP uses hello messages to discover neighbors and to
         detect loss of connectivity with its neighbors."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgTargPeerEntry 12 }

vRtrLdpNgTargPeerHelloTimeout    OBJECT-TYPE
    SYNTAX      TmnxLdpNewHelloTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerHelloTimeout specifies the hello time also
         known as hold time. It is the time interval, in seconds, that LDP waits
         before declaring a neighbor to be down. Hello timeout is local to the
         system and is sent in the hello messages to a neighbor.  Hello timeout
         cannot be set to a value that is less than 3 times the hello time."
    DEFVAL      { 45 }
    ::= { vRtrLdpNgTargPeerEntry 13 }

vRtrLdpNgTargPeerOprHelloTimeout OBJECT-TYPE
    SYNTAX      TmnxLdpNewHelloTimeout (3..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerOprHelloTimeout indicates the
         operational hello time also known as hold time used by the operational
         targeted peer. It is the time interval that LDP waits before declaring
         a neighbor to be down."
    ::= { vRtrLdpNgTargPeerEntry 14 }

vRtrLdpNgTargPeerHelloReduction  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerHelloReduction specifies whether hello
         reduction to this targeted peer is enabled or not. If enabled, the
         sender advertises the dampened vRtrLdpNgTargPeerHelloTimeout, to the
         targeted peer after LDP session is established."
    DEFVAL      { false }
    ::= { vRtrLdpNgTargPeerEntry 15 }

vRtrLdpNgTargPeerHelloRdctnFctr  OBJECT-TYPE
    SYNTAX      Unsigned32 (3..20)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerHelloRdctnFctr specifies the number of
         hello messages that are sent at consistent
         vRtrLdpNgTargPeerHelloTimeout value before advertising further
         dampened vRtrLdpNgTargPeerHelloTimeout.

         An 'inconsistentValue' error is returned if this object is set when
         vRtrLdpNgTargPeerHelloReduction is disabled."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgTargPeerEntry 16 }

vRtrLdpNgTargPeerBackoffTime     OBJECT-TYPE
    SYNTAX      TmnxLdpBackoffTime (1..2592000)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerBackoffTime specifies the initial value
         for the backoff interval.

         The backoff interval is the time, in seconds, that LDP waits after an
         LDP session setup has failed before it attempts to setup the session
         again. After the LDP session startup fails the first time, the backoff
         interval is set to the value of vRtrLdpNgTargPeerBackoffTime.
         Thereafter, if session startup fails again the backoff interval
         increases exponentially."
    ::= { vRtrLdpNgTargPeerEntry 17 }

vRtrLdpNgTargPeerMaxBackoffTime  OBJECT-TYPE
    SYNTAX      TmnxLdpBackoffTime
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerMaxBackoffTime specifies the maximum
         value for the backoff interval.

         For each successive failure of the LDP session startup, the backoff
         interval (the time for which the router waits before retrying)
         increases exponentially. If the backoff interval exceeds
         vRtrLdpNgTargPeerMaxBackoffTime, the router will give up trying to
         establish the LDP session.

         If vRtrLdpNgTargPeerMaxBackoffTime has value of zero (0), then the
         backoff interval does not increase exponentially after the first
         session startup attempt fails. Instead it remains constant and LDP
         will keep retrying to establish a session until it succeeds."
    ::= { vRtrLdpNgTargPeerEntry 18 }

vRtrLdpNgTargPeerTunneling       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerTunneling specifies whether tunneling of
         unicast LDP FECs over tunnels is enabled. When this object has a value
         of 'true', tunneling is enabled. When its value is 'false', tunneling
         is disabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgTargPeerEntry 19 }

vRtrLdpNgTargPeerBfdEnabled      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerBfdEnabled specifies whether BFD
         tracking is enabled to the transport address of this peering session.
         When this object has a value of 'true', BFD tracking is enabled. When
         its value is 'false', BFD tracking is disabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgTargPeerEntry 20 }

vRtrLdpNgTargPeerLsrIfIndex      OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerLsrIfIndex specifies the local interface
         index that is to be used as source LSR-ID to establish targeted hello
         adjacency with a LDP peer."
    DEFVAL      { 0 }
    ::= { vRtrLdpNgTargPeerEntry 21 }

vRtrLdpNgTargPeerAutoCreate      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerAutoCreate indicates whether or not the
         row entry was automatically created."
    ::= { vRtrLdpNgTargPeerEntry 22 }

vRtrLdpNgTargPeerCreator         OBJECT-TYPE
    SYNTAX      INTEGER {
        manual   (1),
        template (2),
        sdp      (3),
        autotx   (4),
        autorx   (5)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerCreator indicates the creator of this
         row.

         A value of 'manual(1)' indicates the entry is created manually by the
         user.

         A value of 'template(2)' indicates the entry is auto created by
         template configuration.

         A value of 'sdp(3)' indicates the entry is auto created by service
         manager.

         A value of 'autotx(4)' indicates the entry is auto created for remote
         LFA.

         A value of 'autorx(5)' indicates the entry is auto created upon
         reception of a targeted Hello message."
    ::= { vRtrLdpNgTargPeerEntry 23 }

vRtrLdpNgTargPeerTemplName       OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerTemplName specifies the template name
         that created this row. This object has valid value when
         vRtrLdpNgTargPeerCreator has value of template."
    ::= { vRtrLdpNgTargPeerEntry 24 }

vRtrLdpNgTargPeerLocalIpAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerLocalIpAddrType indicates the type of
         address indicated by vRtrLdpNgTargPeerLocalIpAddress."
    ::= { vRtrLdpNgTargPeerEntry 25 }

vRtrLdpNgTargPeerLocalIpAddress  OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerLocalIpAddress indicates the local IP
         address used in Hellos sent."
    ::= { vRtrLdpNgTargPeerEntry 26 }

vRtrLdpNgTargPeer32BitLsrFormat  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeer32BitLsrFormat specifies whether to use
         32-bit address as source Label Switch Router identifier (LSR-ID) to
         establish a targeted LDP adjacency with a LDP peer. This value can be
         only be set to true if vRtrLdpNgTargPeerLsrIfIndex is set to non-zero
         value and vRtrLdpNgPeerAddressType is ipv6."
    DEFVAL      { false }
    ::= { vRtrLdpNgTargPeerEntry 28 }

vRtrLdpNgTargPeerLsrIdAdvert     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerLsrIdAdvert is only relevant if
         vRtrLdpNgTargPeerCreator in the same row has the value 'template'. If
         that is the case, the value of vRtrLdpNgTargPeerLsrIdAdvert indicates
         if the targeted-peer template which created this targeted peer is
         configured to advertise the local-lsr-id as a FEC."
    ::= { vRtrLdpNgTargPeerEntry 29 }

vRtrLdpNgTargPeerCommunity       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerCommunity is only relevant if
         vRtrLdpNgTargPeerCreator in the same row has the value 'template'. If
         that is the case, the value of vRtrLdpNgTargPeerCommunity indicates
         the community that has been configured on the targeted-peer template
         associated with this targeted peer."
    ::= { vRtrLdpNgTargPeerEntry 30 }

vRtrLdpNgTargPeerMcastTunneling  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerMcastTunneling specifies whether tunneling
         of multicast LDP FECs over tunnels is enabled.  When this object has a value of
         'true', tunneling is enabled.  When its value is 'false', tunneling is
         disabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgTargPeerEntry 31 }

vRtrLdpNgTargPeerStatsTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgTargPeerStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgTargPeerStatsTable is a read-only table. The purpose of
         this table is to keep statistical information about the Targeted peers
         on the LSR.

         Use of AUGMENTS clause implies a one-to-one dependent relationship
         between the base table, vRtrLdpNgTargPeerTable, and the augmenting
         table, vRtrLdpNgTargPeerStatsTable. This in effect extends the
         vRtrLdpNgTargPeerTable with additional columns. Creation or deletion
         of a row in the vRtrLdpNgTargPeerTable results in the same fate for
         the row in the vRtrLdpNgTargPeerTable."
    ::= { tmnxLdpNgObjs 39 }

vRtrLdpNgTargPeerStatsEntry      OBJECT-TYPE
    SYNTAX      VRtrLdpNgTargPeerStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table contains statistical information about an LDP
         Targeted peer.

         Some counters contained in a row are for fatal errors received
         during a former LDP Session associated with this entry. For example,
         an LDP Pdu received on a TCP connection during an LDP Session
         contains a fatal error.  That error is counted here, because the
         session is terminated.

         If the error is NOT fatal (i.e. and the Session remains), then the
         error is counted in the vRtrLdpNgSessionStatsEntry."
    AUGMENTS    { vRtrLdpNgTargPeerEntry }
    ::= { vRtrLdpNgTargPeerStatsTable 1 }

VRtrLdpNgTargPeerStatsEntry      ::= SEQUENCE
{
    vRtrLdpNgTargPeerStatExistingAdj Gauge32,
    vRtrLdpNgTargPeerStatsHelloRecv  Gauge32,
    vRtrLdpNgTargPeerStatsHelloSent  Gauge32,
    vRtrLdpNgTargPeerStatsBadPduLen  Gauge32,
    vRtrLdpNgTargPeerStatsBadMsgLen  Gauge32,
    vRtrLdpNgTargPeerStatsMalformTlv Gauge32,
    vRtrLdpNgTargPeerStatsBadProtVer Gauge32
}

vRtrLdpNgTargPeerStatExistingAdj OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerStatExistingAdj indicates a count of the
         total active adjacencies with this targeted peer."
    ::= { vRtrLdpNgTargPeerStatsEntry 1 }

vRtrLdpNgTargPeerStatsHelloRecv  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerStatsHelloRecv indicates number of Hello
         messages received with this targeted peer."
    ::= { vRtrLdpNgTargPeerStatsEntry 2 }

vRtrLdpNgTargPeerStatsHelloSent  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerStatsHelloSent indicates the number of
         Hello messages sent with this targeted peer."
    ::= { vRtrLdpNgTargPeerStatsEntry 3 }

vRtrLdpNgTargPeerStatsBadPduLen  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerStatsBadPduLen indicates the number of
         bad PDU length errors detected with this targeted peer."
    ::= { vRtrLdpNgTargPeerStatsEntry 4 }

vRtrLdpNgTargPeerStatsBadMsgLen  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerStatsBadMsgLen indicates the number of
         bad message length errors detected with this targeted peer."
    ::= { vRtrLdpNgTargPeerStatsEntry 5 }

vRtrLdpNgTargPeerStatsMalformTlv OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "value of vRtrLdpNgTargPeerStatsMalformTlv indicates the number of
         malformed TLV value errors detected with this targeted peer."
    ::= { vRtrLdpNgTargPeerStatsEntry 6 }

vRtrLdpNgTargPeerStatsBadProtVer OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerStatsBadProtVer indicates the number of
         bad protocol version errors detected with this targeted peer."
    ::= { vRtrLdpNgTargPeerStatsEntry 7 }

vRtrLdpNgInetIfTableLstCh        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfTableLstCh indicates the last timestamp
         when an entry in the vRtrLdpNgInetIfTable was last changed."
    ::= { tmnxLdpNgObjs 40 }

vRtrLdpNgInetIfTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgInetIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgInetIfTable provides an entry for each virtual router
         interface configuration to be used with the Label Distribution
         Protocol (LDP) for a given Inet address family."
    ::= { tmnxLdpNgObjs 41 }

vRtrLdpNgInetIfEntry             OBJECT-TYPE
    SYNTAX      VRtrLdpNgInetIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an interface on this virtual router that
         participates in the LDP protocol for a given Inet address family.

         Corresponding interface entry must exist in vRtrLdpNgIfTable before
         creating an entry in this table.

         Row entries can be created or deleted via SNMP SET requests.  A row
         with default attribute values is created by setting
         vRtrLdpNgInetIfRowStatus to 'createAndGo'. A row entry can be destroyed
         by setting vRtrLdpNgInetIfRowStatus to 'destroy'."
    INDEX       {
        vRtrID,
        vRtrLdpNgIfIndex,
        vRtrLdpNgIfAddrType
    }
    ::= { vRtrLdpNgInetIfTable 1 }

VRtrLdpNgInetIfEntry             ::= SEQUENCE
{
    vRtrLdpNgIfAddrType              InetVersion,
    vRtrLdpNgInetIfRowStatus         RowStatus,
    vRtrLdpNgInetIfUpTime            TimeInterval,
    vRtrLdpNgInetIfLastChange        TimeStamp,
    vRtrLdpNgInetIfAdminState        TmnxAdminState,
    vRtrLdpNgInetIfOperState         TmnxOperState,
    vRtrLdpNgInetIfOperDownReason    TmnxLdpIntTargOperDownReasonCode,
    vRtrLdpNgInetIfInheritance       Integer32,
    vRtrLdpNgInetIfKAFactor          TmnxLdpKeepAliveFactor,
    vRtrLdpNgInetIfKATimeout         TmnxLdpNewKeepAliveTimeout,
    vRtrLdpNgInetIfHelloFactor       TmnxLdpHelloFactor,
    vRtrLdpNgInetIfHelloTimeout      TmnxLdpNewHelloTimeout,
    vRtrLdpNgInetIfOperHelloTimeout  TmnxLdpNewHelloTimeout,
    vRtrLdpNgInetIfBackoffTime       TmnxLdpBackoffTime,
    vRtrLdpNgInetIfMaxBackoffTime    TmnxLdpBackoffTime,
    vRtrLdpNgInetIfTransAddrType     INTEGER,
    vRtrLdpNgInetIfLsrIfType         INTEGER,
    vRtrLdpNgInetIfLsrIfIndex        InterfaceIndexOrZero,
    vRtrLdpNgInetIfIPv4P2MPFecCap    TmnxEnabledDisabled,
    vRtrLdpNgInetIfIPv6P2MPFecCap    TmnxEnabledDisabled,
    vRtrLdpNgInetIfIPv4PfxFecCap     TmnxEnabledDisabled,
    vRtrLdpNgInetIfIPv6PfxFecCap     TmnxEnabledDisabled,
    vRtrLdpNgInetIfLocalIpAddrType   InetAddressType,
    vRtrLdpNgInetIfLocalIpAddress    InetAddress,
    vRtrLdpNgInetIf32BitLsrFormat    TruthValue
}

vRtrLdpNgIfAddrType              OBJECT-TYPE
    SYNTAX      InetVersion
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgIfAddrType indicates the Inet address family of this
         interface."
    ::= { vRtrLdpNgInetIfEntry 1 }

vRtrLdpNgInetIfRowStatus         OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgInetIfRowStatus is used to control the creation and deletion
         of rows in the vRtrLdpNgInetIfTable.

         A row can be created by setting vRtrLdpNgIfRowStatus to 'createAndGo'.
         The agent should assign the default attribute values and change the
         row status to 'active'. Corresponding interface entry must exit in
         vRtrLdpNgIfTable before creating an entry in this table.

         A row entry can be destroyed by setting vRtrLdpNgInetIfRowStatus to
         'destroy'."
    ::= { vRtrLdpNgInetIfEntry 2 }

vRtrLdpNgInetIfUpTime            OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfUpTime indicates the time, in hundreds of
         seconds, that the LDP interface has been in current operational state
         vRtrLdpNgIfOperState.

         If the value of vRtrLdpNgIfOperState is 'inService (2)', then
         vRtrLdpNgInetIfUpTime specifies the time that the LDP interface has
         been operationally up.

         If the value of vRtrLdpNgIfOperState is 'outOfService (3)', then
         vRtrLdpNgInetIfUpTime specifies the time that the LDP interface has
         been operationally down.

         If the value of vRtrLdpNgIfOperState is 'transition (4)', then
         vRtrLdpNgInetIfUpTime specifies the time that the LDP interface has
         been operationally in transition."
    ::= { vRtrLdpNgInetIfEntry 3 }

vRtrLdpNgInetIfLastChange        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfLastChange indicates the sysUpTime when
         this row was last modified."
    ::= { vRtrLdpNgInetIfEntry 4 }

vRtrLdpNgInetIfAdminState        OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfAdminState specifies the desired
         administrative state for this interface."
    DEFVAL      { inService }
    ::= { vRtrLdpNgInetIfEntry 5 }

vRtrLdpNgInetIfOperState         OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfOperState indicates the current
         operational state of this interface."
    ::= { vRtrLdpNgInetIfEntry 6 }

vRtrLdpNgInetIfOperDownReason    OBJECT-TYPE
    SYNTAX      TmnxLdpIntTargOperDownReasonCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfOperDownReason indicates the reason that
         the LDP interface is operationally down."
    ::= { vRtrLdpNgInetIfEntry 7 }

vRtrLdpNgInetIfInheritance       OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Some writable object in this row that can be configured to inherit its
         value from its corresponding object in the vRtrLdpNgGeneralTable.
         vRtrLdpIfInheritance controls whether to inherit the operational value
         of that object, or use the administratively set value.

         Non mask bits will always have value of zero, and any attempt to
         change the value will be silently discarded.

         When the bit for an object has value of one, then the object's
         administrative and operational value are whatever the DEFVAL or most
         recently SET value. The mask bit(s) will be set to one when set is
         performed on the inherited object(s). Any attempt to set the mask bit
         to one will be silently discarded.

         When the bit for an object is set to zero, then the object's
         administrative and operational value are inherited from the
         corresponding object in vRtrLdpNgGeneralTable.

         This object is a bit-mask, with the following positions:
         vRtrLdpNgInetIfKAFactor        0x1
         vRtrLdpNgInetIfKATimeout       0x2
         vRtrLdpNgInetIfHelloFactor     0x4
         vRtrLdpNgInetIfHelloTimeout    0x8
         vRtrLdpNgInetIfTransAddrType   0x10"
    DEFVAL      { 0 }
    ::= { vRtrLdpNgInetIfEntry 8 }

vRtrLdpNgInetIfKAFactor          OBJECT-TYPE
    SYNTAX      TmnxLdpKeepAliveFactor
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfKAFactor specifies the value by which the
         keepalive timeout (vRtrLdpNgInetIfKATimeout) should be divided to give
         the keepalive time i.e. the time interval, in seconds, between LDP
         keepalive messages. LDP keepalive messages are sent to keep the LDP
         session from timing out when no other LDP traffic is being sent
         between the neighbors."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgInetIfEntry 9 }

vRtrLdpNgInetIfKATimeout         OBJECT-TYPE
    SYNTAX      TmnxLdpNewKeepAliveTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfKATimeout specifies the time interval, in
         seconds, that LDP waits before tearing down a session. If no LDP
         messages are exchanged during this time interval, the LDP session is
         torn down. Generally the value of vRtrLdpNgInetIfKATimeout is
         configured to be 3 times the keepalive time (the time interval between
         successive LDP keepalive messages)."
    DEFVAL      { 30 }
    ::= { vRtrLdpNgInetIfEntry 10 }

vRtrLdpNgInetIfHelloFactor       OBJECT-TYPE
    SYNTAX      TmnxLdpHelloFactor
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfHelloFactor specifies the value by which
         the hello timeout (vRtrLdpNgInetIfHelloTimeout) should be divided to
         give the hello time i.e. the time interval, in seconds, between LDP
         Hello messages. LDP uses hello messages to discover neighbors and to
         detect loss of connectivity with its neighbors."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgInetIfEntry 11 }

vRtrLdpNgInetIfHelloTimeout      OBJECT-TYPE
    SYNTAX      TmnxLdpNewHelloTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfHelloTimeout specifies the hello time also
         known as hold time. It is the time interval, in seconds, that LDP
         waits before declaring a neighbor to be down. Hello timeout is local
         to the system and is sent in the hello messages to a neighbor. Hello
         timeout cannot be set to a value that is less than 3 times the hello
         time."
    DEFVAL      { 15 }
    ::= { vRtrLdpNgInetIfEntry 12 }

vRtrLdpNgInetIfOperHelloTimeout  OBJECT-TYPE
    SYNTAX      TmnxLdpNewHelloTimeout (3..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfOperHelloTimeout indicates the operational
         hello time also known as hold time used by the operational LDP
         interface. It is the time interval that LDP waits before declaring a
         neighbor to be down."
    ::= { vRtrLdpNgInetIfEntry 13 }

vRtrLdpNgInetIfBackoffTime       OBJECT-TYPE
    SYNTAX      TmnxLdpBackoffTime (1..2592000)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfBackoffTime indicates the initial value
         for the backoff interval.

         The backoff interval is the time, in seconds, that LDP waits after an
         LDP session setup has failed before it attempts to setup the session
         again. After the LDP session startup fails the first time, the backoff
         interval is set to the value of vRtrLdpNgInetIfBackoffTime.
         Thereafter, if session startup fails again the backoff interval
         increases exponentially."
    ::= { vRtrLdpNgInetIfEntry 14 }

vRtrLdpNgInetIfMaxBackoffTime    OBJECT-TYPE
    SYNTAX      TmnxLdpBackoffTime
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfMaxBackoffTime specifies the maximum value
         for the backoff interval.

         For each successive failure of the LDP session startup, the backoff
         interval (the time for which the router waits before retrying)
         increases exponentially. If the backoff interval exceeds
         vRtrLdpNgInetIfMaxBackoffTime, the router will give up trying to
         establish the LDP session."
    ::= { vRtrLdpNgInetIfEntry 15 }

vRtrLdpNgInetIfTransAddrType     OBJECT-TYPE
    SYNTAX      INTEGER {
        interface (1),
        system    (2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfTransAddrType specifies the source of the
         transport address to be used when setting up the LDP TCP sessions.

         The interface's IP address is used to setup the LDP session between
         neighbors. If multiple interfaces exist between two neighbors, the
         'interface' mode cannot be used since only one LDP session is actually
         set up between the two neighbors.

         When the value of this object is 'system', the system's IP address is
         used to set up the LDP session between neighbors."
    DEFVAL      { system }
    ::= { vRtrLdpNgInetIfEntry 16 }

vRtrLdpNgInetIfLsrIfType         OBJECT-TYPE
    SYNTAX      INTEGER {
        system    (1),
        interface (2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfLsrIfType specifies whether the local
         interface address or the system interface address should be used as
         source Label Switch Router identifier (LSR-ID) to establish a link LDP
         adjacency with a LDP peer"
    DEFVAL      { system }
    ::= { vRtrLdpNgInetIfEntry 17 }

vRtrLdpNgInetIfLsrIfIndex        OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfLsrIfIndex specifies the local interface
         index that is to be used as source LSR-ID to establish link hello
         adjacency with a LDP peer."
    DEFVAL      { 0 }
    ::= { vRtrLdpNgInetIfEntry 18 }

vRtrLdpNgInetIfIPv4P2MPFecCap    OBJECT-TYPE
    SYNTAX      TmnxEnabledDisabled
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfIPv4P2MPFecCap specifies whether traffic
         exchange for IPv4 P2MP FECs is enabled or disabled on this interface."
    DEFVAL      { enabled }
    ::= { vRtrLdpNgInetIfEntry 19 }

vRtrLdpNgInetIfIPv6P2MPFecCap    OBJECT-TYPE
    SYNTAX      TmnxEnabledDisabled
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfIPv6P2MPFecCap specifies whether traffic
         exchange for IPv6 P2MP FECs is enabled or disabled on this interface."
    DEFVAL      { enabled }
    ::= { vRtrLdpNgInetIfEntry 20 }

vRtrLdpNgInetIfIPv4PfxFecCap     OBJECT-TYPE
    SYNTAX      TmnxEnabledDisabled
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfIPv4PfxFecCap specifies whether traffic
         exchange for IPv4 prefix FECs is enabled or disabled on this
         interface."
    DEFVAL      { enabled }
    ::= { vRtrLdpNgInetIfEntry 21 }

vRtrLdpNgInetIfIPv6PfxFecCap     OBJECT-TYPE
    SYNTAX      TmnxEnabledDisabled
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfIPv6PfxFecCap specifies whether traffic
         exchange for IPv6 prefix FECs is enabled or disabled this interface."
    DEFVAL      { enabled }
    ::= { vRtrLdpNgInetIfEntry 22 }

vRtrLdpNgInetIfLocalIpAddrType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfLocalIpAddrType indicates the type of
         address indicated by vRtrLdpNgInetIfLocalIpAddress."
    ::= { vRtrLdpNgInetIfEntry 23 }

vRtrLdpNgInetIfLocalIpAddress    OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIfLocalIpAddress indicates the local IP
         address used in Hellos sent."
    ::= { vRtrLdpNgInetIfEntry 24 }

vRtrLdpNgInetIf32BitLsrFormat    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInetIf32BitLsrFormat specifies whether to use
         32-bit address as source Label Switch Router identifier (LSR-ID) to
         establish a link LDP adjacency with a LDP peer. This value can be only
         be set to true if vRtrLdpNgInetIfLsrIfType is 'interface' or
         vRtrLdpNgInetIfLsrIfIndex is set to non-zero value and
         vRtrLdpNgIfAddrType is ipv6."
    DEFVAL      { false }
    ::= { vRtrLdpNgInetIfEntry 25 }

vLdpNgStatsTable                 OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vLdpNgStatsTable is a read-only table. The purpose of this table is to
         keep statistical information about an LDP Instance.

         Use of AUGMENTS clause implies a one-to-one dependent
         relationship between the base table, vRtrLdpNgGeneralTable,
         and the augmenting table, vLdpNgStatsTable. This in
         effect extends the vRtrLdpNgGeneralTable with additional
         columns.  Creation or deletion of a row in the
         vRtrLdpNgGeneralTable results in the same fate for the row
         in the vLdpNgStatsTable."
    ::= { tmnxLdpNgObjs 42 }

vLdpNgStatsEntry                 OBJECT-TYPE
    SYNTAX      VLdpNgStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table represents statistical information about an LDP
         instance."
    AUGMENTS    { vRtrLdpNgGeneralEntry }
    ::= { vLdpNgStatsTable 1 }

VLdpNgStatsEntry                 ::= SEQUENCE
{
    vLdpNgStatsIPv4OperDownEvents    Counter32,
    vLdpNgStatsIPv6OperDownEvents    Counter32,
    vLdpNgStatsIPv4ActiveSess        Gauge32,
    vLdpNgStatsIPv6ActiveSess        Gauge32,
    vLdpNgStatsIPv4ActiveLinkAdj     Gauge32,
    vLdpNgStatsIPv6ActiveLinkAdj     Gauge32,
    vLdpNgStatsIPv4ActiveTargAdj     Gauge32,
    vLdpNgStatsIPv6ActiveTargAdj     Gauge32,
    vLdpNgStatsIPv4ActiveIf          Gauge32,
    vLdpNgStatsIPv6ActiveIf          Gauge32,
    vLdpNgStatsIPv4InactiveIf        Gauge32,
    vLdpNgStatsIPv6InactiveIf        Gauge32,
    vLdpNgStatsIPv4ActiveTargPeers   Gauge32,
    vLdpNgStatsIPv6ActiveTargPeers   Gauge32,
    vLdpNgStatsIPv4InactiveTargPeers Gauge32,
    vLdpNgStatsIPv6InactiveTargPeers Gauge32,
    vLdpNgStatsIPv4PfxFecRecv        Gauge32,
    vLdpNgStatsIPv6PfxFecRecv        Gauge32,
    vLdpNgStatsIPv4PfxFecSent        Gauge32,
    vLdpNgStatsIPv6PfxFecSent        Gauge32,
    vLdpNgStatsFec128FecSent         Gauge32,
    vLdpNgStatsFec128FecRecv         Gauge32,
    vLdpNgStatsFec129FecSent         Gauge32,
    vLdpNgStatsFec129FecRecv         Gauge32,
    vLdpNgStatsIPv4AttemptedSessions Counter32,
    vLdpNgStatsIPv6AttemptedSessions Counter32,
    vLdpNgStatsSessRejNoHelloErrs    Counter32,
    vLdpNgStatsSessRejAdvErrors      Counter32,
    vLdpNgStatsSessRejMaxPduErrs     Counter32,
    vLdpNgStatsSessRejLblRngeErrs    Counter32,
    vLdpNgStatsBadLdpIdErrors        Counter32,
    vLdpNgStatsBadPduLengthErrors    Counter32,
    vLdpNgStatsBadMsgLengthErrors    Counter32,
    vLdpNgStatsBadTlvLengthErrors    Counter32,
    vLdpNgStatsMalformedTlvErrors    Counter32,
    vLdpNgStatsKeepAliveExpErrors    Counter32,
    vLdpNgStatsShutdownNotifRecv     Counter32,
    vLdpNgStatsShutdownNotifSent     Counter32,
    vLdpNgStatsIPv4EgrFecPfxCount    Counter32,
    vLdpNgStatsIPv6EgrFecPfxCount    Counter32,
    vLdpNgStatsUnknownTlvErrors      Counter32,
    vLdpNgStatsIPv4P2MPFecSent       Gauge32,
    vLdpNgStatsIPv6P2MPFecSent       Gauge32,
    vLdpNgStatsIPv4P2MPFecRecv       Gauge32,
    vLdpNgStatsIPv6P2MPFecRecv       Gauge32,
    vLdpNgStatsIPv4PfxFecOLSessSent  Gauge32,
    vLdpNgStatsIPv6PfxFecOLSessSent  Gauge32,
    vLdpNgStatsIPv4PfxFecOLSessRecv  Gauge32,
    vLdpNgStatsIPv6PfxFecOLSessRecv  Gauge32,
    vLdpNgStatsIPv4P2MPFecOLSessSent Gauge32,
    vLdpNgStatsIPv6P2MPFecOLSessSent Gauge32,
    vLdpNgStatsIPv4P2MPFecOLSessRecv Gauge32,
    vLdpNgStatsIPv6P2MPFecOLSessRecv Gauge32,
    vLdpNgStatsFec128FecOLSessSent   Gauge32,
    vLdpNgStatsFec128FecOLSessRecv   Gauge32,
    vLdpNgStatsFec129FecOLSessSent   Gauge32,
    vLdpNgStatsFec129FecOLSessRecv   Gauge32,
    vLdpNgStatsIPv4OLoadInterfaces   Gauge32,
    vLdpNgStatsIPv6OLoadInterfaces   Gauge32,
    vLdpNgStatsIPv4OLoadTargPeers    Gauge32,
    vLdpNgStatsIPv6OLoadTargPeers    Gauge32,
    vLdpNgStatsIPv4PfxFecInOLoad     Gauge32,
    vLdpNgStatsIPv6PfxFecInOLoad     Gauge32,
    vLdpNgStatsIPv4P2MPFecInOLoad    Gauge32,
    vLdpNgStatsIPv6P2MPFecInOLoad    Gauge32,
    vLdpNgStatsFec128FecInOLoad      Gauge32,
    vLdpNgStatsFec129FecInOLoad      Gauge32,
    vLdpNgStatsBadProtVersionErrors  Gauge32
}

vLdpNgStatsIPv4OperDownEvents    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4OperDownEvents indicates the number of
         times the IPv4 LDP instance has gone operationally down since the
         instance was created."
    ::= { vLdpNgStatsEntry 1 }

vLdpNgStatsIPv6OperDownEvents    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6OperDownEvents indicates the number of
         times the IPv6 LDP instance has gone operationally down since the
         instance was created."
    ::= { vLdpNgStatsEntry 2 }

vLdpNgStatsIPv4ActiveSess        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4ActiveSess indicates the number of active
         IPv4 sessions (i.e. session in some form of creation) associated with
         the LDP instance."
    ::= { vLdpNgStatsEntry 3 }

vLdpNgStatsIPv6ActiveSess        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6ActiveSess indicates the number of active
         IPv6 sessions (i.e. session in some form of creation) associated with
         the LDP instance."
    ::= { vLdpNgStatsEntry 4 }

vLdpNgStatsIPv4ActiveLinkAdj     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4ActiveLinkAdj indicates the number of
         active IPv4 link adjacencies (i.e. established adjacencies) associated
         with the LDP instance."
    ::= { vLdpNgStatsEntry 5 }

vLdpNgStatsIPv6ActiveLinkAdj     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6ActiveLinkAdj indicates the number of
         active IPv6 link adjacencies (i.e. established adjacencies) associated
         with the LDP instance."
    ::= { vLdpNgStatsEntry 6 }

vLdpNgStatsIPv4ActiveTargAdj     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4ActiveTargAdj indicates the number of
         active IPv4 target adjacencies (i.e. established sessions) associated
         with the LDP instance."
    ::= { vLdpNgStatsEntry 7 }

vLdpNgStatsIPv6ActiveTargAdj     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6ActiveTargAdj indicates the number of
         active IPv6 target adjacencies (i.e. established sessions) associated
         with the LDP instance."
    ::= { vLdpNgStatsEntry 8 }

vLdpNgStatsIPv4ActiveIf          OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4ActiveIf indicates the number of active
         (i.e. operationally up) IPv4 interfaces associated with the LDP
         instance."
    ::= { vLdpNgStatsEntry 9 }

vLdpNgStatsIPv6ActiveIf          OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6ActiveIf indicates the number of active
         (i.e. operationally up) IPv6 interfaces associated with the LDP
         instance."
    ::= { vLdpNgStatsEntry 10 }

vLdpNgStatsIPv4InactiveIf        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4InactiveIf indicates the number of
         inactive (i.e. operationally down) IPv4 interfaces associated with the
         LDP instance."
    ::= { vLdpNgStatsEntry 11 }

vLdpNgStatsIPv6InactiveIf        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6InactiveIf indicates the number of
         inactive (i.e. operationally down) IPv6 interfaces associated with the
         LDP instance."
    ::= { vLdpNgStatsEntry 12 }

vLdpNgStatsIPv4ActiveTargPeers   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4ActiveTargPeers indicates the number of
         configured IPv4 targeted peers that are administratively up in an LDP
         instance."
    ::= { vLdpNgStatsEntry 13 }

vLdpNgStatsIPv6ActiveTargPeers   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6ActiveTargPeers indicates the number of
         configured IPv6 targeted peers that are administratively up in an LDP
         instance."
    ::= { vLdpNgStatsEntry 14 }

vLdpNgStatsIPv4InactiveTargPeers OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4InactiveTargPeers indicates the number of
         inactive (i.e. operationally down) IPv4 targeted sessions associated
         with the LDP instance."
    ::= { vLdpNgStatsEntry 15 }

vLdpNgStatsIPv6InactiveTargPeers OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6InactiveTargPeers indicates the number of
         inactive (i.e. operationally down) IPv6 targeted sessions associated
         with the LDP instance."
    ::= { vLdpNgStatsEntry 16 }

vLdpNgStatsIPv4PfxFecRecv        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4PfxFecRecv indicates the number of IPv4
         Address FECs received by the LDP instance from its neighbors."
    ::= { vLdpNgStatsEntry 17 }

vLdpNgStatsIPv6PfxFecRecv        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6PfxFecRecv indicates the number of IPv6
         Address FECs received by the LDP instance from its neighbors."
    ::= { vLdpNgStatsEntry 18 }

vLdpNgStatsIPv4PfxFecSent        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4PfxFecSent indicates the number of IPv4
         Address FECs sent by the LDP instance to its neighbors."
    ::= { vLdpNgStatsEntry 19 }

vLdpNgStatsIPv6PfxFecSent        OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6PfxFecSent indicates the number of IPv6
         Address FECs sent by the LDP instance to its neighbors."
    ::= { vLdpNgStatsEntry 20 }

vLdpNgStatsFec128FecSent         OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsFec128FecSent indicates the number of Pseudo
         wire ID FECs sent by the LDP instance to its neighbors."
    ::= { vLdpNgStatsEntry 21 }

vLdpNgStatsFec128FecRecv         OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsFec128FecRecv indicates the number of Pseudo
         wire ID FECs received by the LDP instance from its neighbors."
    ::= { vLdpNgStatsEntry 22 }

vLdpNgStatsFec129FecSent         OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsFec129FecSent indicates the number of General
         Pseudo wire ID FECs sent by the LDP instance to its neighbors."
    ::= { vLdpNgStatsEntry 23 }

vLdpNgStatsFec129FecRecv         OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsFec129FecRecv indicates the number of General
         Pseudo wire ID FECs received by the LDP instance from its neighbors."
    ::= { vLdpNgStatsEntry 24 }

vLdpNgStatsIPv4AttemptedSessions OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4AttemptedSessions indicates the total
         number of attempted IPv4 sessions for this LDP instance."
    ::= { vLdpNgStatsEntry 25 }

vLdpNgStatsIPv6AttemptedSessions OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6AttemptedSessions indicates the total
         number of attempted IPv6 sessions for this LDP instance."
    ::= { vLdpNgStatsEntry 26 }

vLdpNgStatsSessRejNoHelloErrs    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsSessRejNoHelloErrs gives the total number of
         Session Rejected/No Hello Error Notification Messages sent or received
         by this LDP instance."
    ::= { vLdpNgStatsEntry 27 }

vLdpNgStatsSessRejAdvErrors      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsSessRejAdvErrors gives the total number of
         Session Rejected/Parameters Advertisement Mode Error Notification
         Messages sent or received by this LDP instance."
    ::= { vLdpNgStatsEntry 28 }

vLdpNgStatsSessRejMaxPduErrs     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsSessRejMaxPduErrs gives the total number of
         Session Rejected/Parameters Max Pdu Length Error Notification Messages
         sent or received by this LDP instance."
    ::= { vLdpNgStatsEntry 29 }

vLdpNgStatsSessRejLblRngeErrs    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsSessRejLblRngeErrs gives the total number of
         Session Rejected/Parameters Label Range Error Notification Messages
         sent or received by this LDP instance."
    ::= { vLdpNgStatsEntry 30 }

vLdpNgStatsBadLdpIdErrors        OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsBadLdpIdErrors gives the number of Bad LDP
         Identifier Fatal Errors detected for sessions associated with this LDP
         instance."
    REFERENCE
        "LDP Specification, Section 3.5.1.2."
    ::= { vLdpNgStatsEntry 31 }

vLdpNgStatsBadPduLengthErrors    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsBadPduLengthErrors gives the number of Bad Pdu
         Length Fatal Errors detected for sessions associated with this LDP
         instance."
    REFERENCE
        "LDP Specification, Section 3.5.1.2."
    ::= { vLdpNgStatsEntry 32 }

vLdpNgStatsBadMsgLengthErrors    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsBadMsgLengthErrors gives the number of Bad
         Message Length Fatal Errors detected for sessions associated with this
         LDP instance."
    REFERENCE
        "LDP Specification, Section 3.5.1.2."
    ::= { vLdpNgStatsEntry 33 }

vLdpNgStatsBadTlvLengthErrors    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsBadTlvLengthErrors gives the number of Bad TLV
         Length Fatal Errors detected for sessions associated with this LDP
         instance."
    REFERENCE
        "LDP Specification, Section 3.5.1.2."
    ::= { vLdpNgStatsEntry 34 }

vLdpNgStatsMalformedTlvErrors    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsMalformedTlvErrors gives the number of
         Malformed TLV Value Fatal Errors detected for sessions associated with
         this LDP instance."
    REFERENCE
        "LDP Specification, Section 3.5.1.2."
    ::= { vLdpNgStatsEntry 35 }

vLdpNgStatsKeepAliveExpErrors    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsKeepAliveExpErrors gives the number of Session
         Keep Alive Timer Expired Errors detected for sessions associated with
         this LDP instance."
    REFERENCE
        "LDP Specification, Section 3.5.1.2."
    ::= { vLdpNgStatsEntry 36 }

vLdpNgStatsShutdownNotifRecv     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsShutdownNotifRecv gives the number of Shutdown
         Notifications received related to sessions associated with this LDP
         instance."
    ::= { vLdpNgStatsEntry 37 }

vLdpNgStatsShutdownNotifSent     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsShutdownNotifSent gives the number of Shutdown
         Notifications sent related to sessions associated with this LDP
         instance."
    ::= { vLdpNgStatsEntry 38 }

vLdpNgStatsIPv4EgrFecPfxCount    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4EgrFecPfxCount indicates the number of
         IPv4 egress FEC prefix statistics configured for this LDP instance."
    ::= { vLdpNgStatsEntry 39 }

vLdpNgStatsIPv6EgrFecPfxCount    OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6EgrFecPfxCount indicates the number of
         IPv6 egress FEC prefix statistics configured for this LDP instance."
    ::= { vLdpNgStatsEntry 40 }

vLdpNgStatsUnknownTlvErrors      OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsUnknownTlvErrors indicates the number of
         Unknown TLV Fatal Errors detected for sessions associated with this
         LDP instance."
    REFERENCE
        "LDP Specification, Section 3.5.1.2."
    ::= { vLdpNgStatsEntry 41 }

vLdpNgStatsIPv4P2MPFecSent       OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4P2MPFecSent indicates the number of IPv4
         P2MP FECs sent by the LDP instance to its neighbors."
    ::= { vLdpNgStatsEntry 42 }

vLdpNgStatsIPv6P2MPFecSent       OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6P2MPFecSent indicates the number of IPv6
         P2MP FECs sent by the LDP instance to its neighbors."
    ::= { vLdpNgStatsEntry 43 }

vLdpNgStatsIPv4P2MPFecRecv       OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4P2MPFecRecv indicates the number of IPv4
         P2MP FECs received by the LDP instance from its neighbors."
    ::= { vLdpNgStatsEntry 44 }

vLdpNgStatsIPv6P2MPFecRecv       OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6P2MPFecRecv indicates the number of IPv6
         P2MP FECs received by the LDP instance from its neighbors."
    ::= { vLdpNgStatsEntry 45 }

vLdpNgStatsIPv4PfxFecOLSessSent  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4PfxFecOLSessSent indicates the number of
         Overload Notifications sent for IPv4 address FEC over sessions in LDP
         instance."
    ::= { vLdpNgStatsEntry 46 }

vLdpNgStatsIPv6PfxFecOLSessSent  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6PfxFecOLSessSent indicates the number of
         Overload Notifications sent for IPv6 address FEC over sessions in LDP
         instance."
    ::= { vLdpNgStatsEntry 47 }

vLdpNgStatsIPv4PfxFecOLSessRecv  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4PfxFecOLSessRecv indicates the number of
         Overload Notifications received for IPv4 address FEC over sessions in
         LDP instance."
    ::= { vLdpNgStatsEntry 48 }

vLdpNgStatsIPv6PfxFecOLSessRecv  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6PfxFecOLSessRecv indicates the number of
         Overload Notifications received for IPv6 address FEC over sessions in
         LDP instance."
    ::= { vLdpNgStatsEntry 49 }

vLdpNgStatsIPv4P2MPFecOLSessSent OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4P2MPFecOLSessSent indicates the number of
         Overload Notifications sent for IPv4 P2MP FEC over sessions in LDP
         instance."
    ::= { vLdpNgStatsEntry 50 }

vLdpNgStatsIPv6P2MPFecOLSessSent OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6P2MPFecOLSessSent indicates the number of
         Overload Notifications sent for IPv6 P2MP FEC over sessions in LDP
         instance."
    ::= { vLdpNgStatsEntry 51 }

vLdpNgStatsIPv4P2MPFecOLSessRecv OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4P2MPFecOLSessRecv indicates the number of
         Overload Notifications received for IPv4 P2MP FEC over sessions in LDP
         instance."
    ::= { vLdpNgStatsEntry 52 }

vLdpNgStatsIPv6P2MPFecOLSessRecv OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6P2MPFecOLSessRecv indicates the number of
         Overload Notifications received for IPv6 P2MP FEC over sessions in LDP
         instance."
    ::= { vLdpNgStatsEntry 53 }

vLdpNgStatsFec128FecOLSessSent   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsFec128FecOLSessSent indicates the number of
         Overload Notifications sent for PW ID FEC over sessions in LDP
         instance."
    ::= { vLdpNgStatsEntry 54 }

vLdpNgStatsFec128FecOLSessRecv   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsFec128FecOLSessRecv indicates the number of
         Overload Notifications received for PW ID FEC over sessions in LDP
         instance."
    ::= { vLdpNgStatsEntry 55 }

vLdpNgStatsFec129FecOLSessSent   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsFec129FecOLSessSent indicates the number of
         Overload Notifications sent for General PW ID FEC over sessions in LDP
         instance."
    ::= { vLdpNgStatsEntry 56 }

vLdpNgStatsFec129FecOLSessRecv   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsFec129FecOLSessRecv indicates the number of
         Overload Notifications received for General PW ID FEC over sessions in
         LDP instance."
    ::= { vLdpNgStatsEntry 57 }

vLdpNgStatsIPv4OLoadInterfaces   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4OLoadInterfaces indicates the number of
         overloaded IPv4 interfaces in LDP instance."
    ::= { vLdpNgStatsEntry 58 }

vLdpNgStatsIPv6OLoadInterfaces   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6OLoadInterfaces indicates the number of
         overloaded IPv6 interfaces in LDP instance."
    ::= { vLdpNgStatsEntry 59 }

vLdpNgStatsIPv4OLoadTargPeers    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4OLoadTargPeers indicates the number of
         overloaded IPv4 targeted peers in LDP instance."
    ::= { vLdpNgStatsEntry 60 }

vLdpNgStatsIPv6OLoadTargPeers    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6OLoadTargPeers indicates the number of
         overloaded IPv6 targeted peers in LDP instance."
    ::= { vLdpNgStatsEntry 61 }

vLdpNgStatsIPv4PfxFecInOLoad     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4PfxFecInOLoad indicates the number IPv4
         Address FEC in overload state in LDP instance."
    ::= { vLdpNgStatsEntry 62 }

vLdpNgStatsIPv6PfxFecInOLoad     OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6PfxFecInOLoad indicates the number IPv6
         Address FEC in overload state in LDP instance."
    ::= { vLdpNgStatsEntry 63 }

vLdpNgStatsIPv4P2MPFecInOLoad    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv4P2MPFecInOLoad indicates the number IPv4
         P2MP FEC in overload state in LDP instance."
    ::= { vLdpNgStatsEntry 64 }

vLdpNgStatsIPv6P2MPFecInOLoad    OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsIPv6P2MPFecInOLoad indicates the number IPv4
         P2MP FEC in overload state in LDP instance."
    ::= { vLdpNgStatsEntry 65 }

vLdpNgStatsFec128FecInOLoad      OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsFec128FecInOLoad indicates the number PW ID
         FEC in overload state in LDP instance."
    ::= { vLdpNgStatsEntry 66 }

vLdpNgStatsFec129FecInOLoad      OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsFec129FecInOLoad indicates the number General
         PW ID FEC in overload state in LDP instance."
    ::= { vLdpNgStatsEntry 67 }

vLdpNgStatsBadProtVersionErrors  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgStatsBadProtVersionErrors indicates the number of
         bad protocol version errors detected for sessions associated with this
         LDP instance."
    ::= { vLdpNgStatsEntry 68 }

vRtrLdpNgCapabilityTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgCapabilityEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgCapabilityTable is a read-only table. The purpose of this
         table is to keep capability information about an LDP Instance.

         Use of AUGMENTS clause implies a one-to-one dependent
         relationship between the base table, vRtrLdpNgGeneralTable,
         and the augmenting table, vRtrLdpNgCapabilityTable. This in
         effect extends the vRtrLdpNgGeneralTable with additional
         columns.  Creation or deletion of a row in the
         vRtrLdpNgGeneralTable results in the same fate for the row
         in the vRtrLdpNgCapabilityTable."
    ::= { tmnxLdpNgObjs 43 }

vRtrLdpNgCapabilityEntry         OBJECT-TYPE
    SYNTAX      VRtrLdpNgCapabilityEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An row in this table contains capability information about an LDP
         instance."
    AUGMENTS    { vRtrLdpNgGeneralEntry }
    ::= { vRtrLdpNgCapabilityTable 1 }

VRtrLdpNgCapabilityEntry         ::= SEQUENCE
{
    vRtrLdpNgGenP2MPCapability       TruthValue,
    vRtrLdpNgGenMPMBBCapability      TruthValue,
    vRtrLdpNgGenDynamicCapability    TruthValue,
    vRtrLdpNgGenOverloadCapability   TruthValue,
    vRtrLdpNgGenFec128Capability     TruthValue,
    vRtrLdpNgGenFec129Capability     TruthValue,
    vRtrLdpNgGenIPv4PfxFecCapability TruthValue,
    vRtrLdpNgGenIPv6PfxFecCapability TruthValue,
    vRtrLdpNgGenUnregNotiCapability  TruthValue
}

vRtrLdpNgGenP2MPCapability       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenP2MPCapability indicates whether
         Point-to-Multipoint (P2MP) FEC capability is supported in the LDP
         instance or not. When the value is 'true', the LDP instance is P2MP
         capable."
    ::= { vRtrLdpNgCapabilityEntry 1 }

vRtrLdpNgGenMPMBBCapability      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenMPMBBCapability indicates whether
         Multipoint(MP) Make-Before-Break (MBB) capability is supported
         in the LDP instance or not.  When the value is 'true', the LDP
         instance is MP MBB capable."
    ::= { vRtrLdpNgCapabilityEntry 2 }

vRtrLdpNgGenDynamicCapability    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenDynamicCapability indicates whether dynamic
         capability negotiation is supported or not in LDP sessions associated
         with the LDP instance.  When 'true', the LDP instance supports dynamic
         capability negotiation."
    ::= { vRtrLdpNgCapabilityEntry 3 }

vRtrLdpNgGenOverloadCapability   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenOverloadCapability indicates whether LSR
         Overload is supported or not in LDP sessions associated with the LDP
         instance. When 'true', the LDP instance is LSR overload capable."
    ::= { vRtrLdpNgCapabilityEntry 4 }

vRtrLdpNgGenFec128Capability     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenFec128Capability indicates whether or not PW
         (Pseudowire) ID FEC capability is supported in LDP instance."
    ::= { vRtrLdpNgCapabilityEntry 5 }

vRtrLdpNgGenFec129Capability     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenFec129Capability indicates whether or not
         General PW ID FEC capability is supported in LDP instance."
    ::= { vRtrLdpNgCapabilityEntry 6 }

vRtrLdpNgGenIPv4PfxFecCapability OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenIPv4PfxFecCapability indicates whether or not
         IPv4 Prefix FEC capability is supported in LDP instance."
    ::= { vRtrLdpNgCapabilityEntry 7 }

vRtrLdpNgGenIPv6PfxFecCapability OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenIPv6PfxFecCapability indicates whether or not
         IPv6 Prefix FEC capability is supported in LDP instance."
    ::= { vRtrLdpNgCapabilityEntry 8 }

vRtrLdpNgGenUnregNotiCapability  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenUnregNotiCapability indicates whether or not
         Unrecognized Notification capability is supported in LDP instance."
    ::= { vRtrLdpNgCapabilityEntry 9 }

vRtrLdpNgTcpSessParamsTableLstCh OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTcpSessParamsTableLstCh indicates the last
         timestamp when an entry in the vRtrLdpNgTcpSessParamsTable was last
         changed."
    ::= { tmnxLdpNgObjs 44 }

vRtrLdpNgTcpSessParamsTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgTcpSessParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgTcpSessParamsTable is used to configure parameters applicable
         to TCP transport session of an LDP session to remote peer."
    ::= { tmnxLdpNgObjs 45 }

vRtrLdpNgTcpSessParamsEntry      OBJECT-TYPE
    SYNTAX      VRtrLdpNgTcpSessParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents information applicable to TCP session to far
         end peer.

         Row entries can be created or deleted via SNMP SET requests. A row
         with default attribute values is created by setting
         vRtrLdpNgTcpSessRowStatus to 'createAndGo'. A row entry can be
         destroyed by setting vRtrLdpNgTcpSessRowStatus to 'destroy'."
    INDEX       {
        vRtrID,
        vRtrLdpNgTcpSessPeerAddrType,
        vRtrLdpNgTcpSessPeerAddr
    }
    ::= { vRtrLdpNgTcpSessParamsTable 1 }

VRtrLdpNgTcpSessParamsEntry      ::= SEQUENCE
{
    vRtrLdpNgTcpSessPeerAddrType     InetAddressType,
    vRtrLdpNgTcpSessPeerAddr         InetAddress,
    vRtrLdpNgTcpSessRowStatus        RowStatus,
    vRtrLdpNgTcpSessAuth             INTEGER,
    vRtrLdpNgTcpSessAuthKey          OCTET STRING,
    vRtrLdpNgTcpSessAuthKeyChain     TNamedItemOrEmpty,
    vRtrLdpNgTcpSessPMTUDiscovery    TruthValue,
    vRtrLdpNgTcpSessMinTTLValue      Unsigned32,
    vRtrLdpNgTcpSessInheritance      Unsigned32
}

vRtrLdpNgTcpSessPeerAddrType     OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTcpSessPeerAddrType specifies the IP address
         type for vRtrLdpNgTcpSessPeerAddr."
    ::= { vRtrLdpNgTcpSessParamsEntry 1 }

vRtrLdpNgTcpSessPeerAddr         OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTcpSessPeerAddr specifies the remote TCP
         transport address to use for an LDP session to a peer. This value
         corresponds to peer address (vRtrLdpNgSessPeerAddress) of LDP session."
    ::= { vRtrLdpNgTcpSessParamsEntry 2 }

vRtrLdpNgTcpSessRowStatus        OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgTcpSessRowStatus is used to control the creation and deletion
         of rows in the vRtrLdpNgTcpSessParamsTable.

         A row can be created by setting vRtrLdpNgTcpSessRowStatus to
         'createAndGo'.  The agent should assign the default attribute values
         and change the row status to 'active'.

         A row entry can be destroyed by setting vRtrLdpNgTcpSessRowStatus to
         'destroy'."
    ::= { vRtrLdpNgTcpSessParamsEntry 3 }

vRtrLdpNgTcpSessAuth             OBJECT-TYPE
    SYNTAX      INTEGER {
        none (1),
        md5  (2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When the value of vRtrLdpNgTcpSessAuth is 'none', no authentication is
         used.

         When the value of this object is 'md5', authentication using MD5
         message based digest protocol is enabled."
    DEFVAL      { none }
    ::= { vRtrLdpNgTcpSessParamsEntry 4 }

vRtrLdpNgTcpSessAuthKey          OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..255))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The string specified in vRtrLdpNgTcpSessAuthKey is the authentication
         key to be used between two LDP neighbors before establishing TCP
         transport session of the LDP protocol stream.  Authentication is done
         using the MD-5 message based digest protocol.  Note that the string may
         NOT contain embedded nulls.

         An SNMP Get request on this object should return an OCTET STRING of
         length 0."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTcpSessParamsEntry 5 }

vRtrLdpNgTcpSessAuthKeyChain     OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTcpSessAuthKeyChain specifies the keychain which
         will be used to sign and/or authenticate TCP transport session of the
         LDP protocol stream.

         The keychain name is defined by tmnxKeyChainName and is the index for
         TIMETRA-SECURITY-MIB::tmnxKeyChainTable"
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTcpSessParamsEntry 6 }

vRtrLdpNgTcpSessPMTUDiscovery    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTcpSessPMTUDiscovery specifies whether path MTU
         discovery is enabled for this TCP transport session.

         When the value is set to 'true', path MTU discovery is enabled for
         this TCP transport session. When the value is set to 'false', path MTU
         discovery is disabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgTcpSessParamsEntry 7 }

vRtrLdpNgTcpSessMinTTLValue      OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 1..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTcpSessMinTTLValue specifies the minimum TTL
         value for an incoming LDP packet.

         If vRtrLdpNgTcpSessMinTTLValue is set to zero (0), the TTL Security
         feature is disabled."
    DEFVAL      { 0 }
    ::= { vRtrLdpNgTcpSessParamsEntry 8 }

vRtrLdpNgTcpSessInheritance      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Some writable object in this row that can be configured to inherit its
         value from its corresponding object in the
         vRtrLdpNgTcpSessParamsGlblTable. vRtrLdpNgTcpSessInheritance controls
         whether to inherit the operational value of that object, or to use the
         administratively set value.

         Non mask bits will always have value of zero, and any attempt to
         change the value will be silently discarded.

         When the bit for an object has value of one, then the object's
         administrative and operational value are whatever the DEFVAL or most
         recently SET value. The mask bit(s) will be set to one when SET is
         performed on the inherited object(s). Any attempt to set the mask bit
         to one will be silently discarded.

         When the bit for an object is set to zero, then the object's
         administrative and operational value are inherited from the
         corresponding object in vRtrLdpNgTcpSessParamsGlblTable.

         This object is a bit-mask, with the following positions:
         vRtrLdpNgTcpSessAuthKeyChain         0x1
         vRtrLdpNgTcpSessAuthKey              0x2"
    DEFVAL      { 0 }
    ::= { vRtrLdpNgTcpSessParamsEntry 9 }

vRtrLdpNgGeneralTableLstCh       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGeneralTableLstCh indicates the last timestamp
         when an entry in the vRtrLdpNgGeneralTable was last changed."
    ::= { tmnxLdpNgObjs 46 }

vRtrLdpNgGeneralTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgGeneralEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgGeneralTable has an entry for each virtual router in the
         system capable of supporting an instance of the Label Distribution
         Protocol (LDP)."
    ::= { tmnxLdpNgObjs 47 }

vRtrLdpNgGeneralEntry            OBJECT-TYPE
    SYNTAX      VRtrLdpNgGeneralEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of the Label Distribution
         Protocol (LDP) for a virtual router in the system.

         An entry in this table is created by the agent when vRtrLdpStatus in
         the vRtrConfTable is set to 'create'. The entry is destroyed when
         vRtrLdpStatus is set to 'delete' but only if vRtrLdpNgGenAdminState
         has a value of 'outOfService'."
    INDEX       { vRtrID }
    ::= { vRtrLdpNgGeneralTable 1 }

VRtrLdpNgGeneralEntry            ::= SEQUENCE
{
    vRtrLdpNgGenCreateTime           TimeStamp,
    vRtrLdpNgGenIPv4UpTime           TimeInterval,
    vRtrLdpNgGenIPv6UpTime           TimeInterval,
    vRtrLdpNgGenLastChange           TimeStamp,
    vRtrLdpNgGenAdminState           TmnxAdminState,
    vRtrLdpNgGenIPv4OperState        TmnxOperState,
    vRtrLdpNgGenIPv6OperState        TmnxOperState,
    vRtrLdpNgGenIPv4OperDownReason   TmnxLdpGenOperDownReasonCode,
    vRtrLdpNgGenIPv6OperDownReason   TmnxLdpGenOperDownReasonCode,
    vRtrLdpNgGenLdpIPv4LsrId         MplsLsrIdentifier,
    vRtrLdpNgGenLdpIPv6LsrId         TmnxMplsLsrNgIdentifier,
    vRtrLdpNgGenProtocolVersion      Unsigned32,
    vRtrLdpNgGenBackoffTime          TmnxLdpBackoffTime,
    vRtrLdpNgGenMaxBackoffTime       TmnxLdpBackoffTime,
    vRtrLdpNgGenTunnelDownDampTime   Unsigned32,
    vRtrLdpNgGenGracefulRestart      TruthValue,
    vRtrLdpNgGenGRNbrLiveTime        Unsigned32,
    vRtrLdpNgGenGRMaxRecoveryTime    Unsigned32,
    vRtrLdpNgGenLabelWithdrawalDelay Unsigned32,
    vRtrLdpNgGenImplicitNull         TruthValue,
    vRtrLdpNgGenShortTTLPropLocal    TruthValue,
    vRtrLdpNgGenShortTTLPropTransit  TruthValue,
    vRtrLdpNgGenMPMBBTime            Unsigned32,
    vRtrLdpNgGenLdpFrr               TruthValue,
    vRtrLdpNgGenMcastUpstreamFrr     TruthValue,
    vRtrLdpNgGenDeaggregateFec       TruthValue,
    vRtrLdpNgGenControlMode          INTEGER,
    vRtrLdpNgGenDistMethod           TmnxLdpLabelDistMethod,
    vRtrLdpNgGenRetentionMode        INTEGER,
    vRtrLdpNgGenPropagatePolicy      TmnxLdpFECPolicy,
    vRtrLdpNgGenLoopDetectCap        INTEGER,
    vRtrLdpNgGenHopLimit             Unsigned32,
    vRtrLdpNgGenPathVectorLimit      Unsigned32,
    vRtrLdpNgGenRoutePreference      Unsigned32,
    vRtrLdpNgGenClassForwarding      TruthValue,
    vRtrLdpNgGenIpv4LsrInterop       TruthValue,
    vRtrLdpNgGenEntropyLblCapability TruthValue,
    vRtrLdpNgGenFrrSRStitch          TruthValue,
    vRtrLdpNgGenMcastUpstrmAsbrFrr   TruthValue,
    vRtrLdpNgGenBasicFecOnly         TmnxEnabledDisabled,
    vRtrLdpNgResolveRootUsing        INTEGER,
    vRtrLdpNgGenWeightedEcmp         TruthValue,
    vRtrLdpNgGenConsiderSysIPInGep   TruthValue,
    vRtrLdpNgGenCBFMode              INTEGER,
    vRtrLdpNgImpPmsiMvpn             TruthValue,
    vRtrLdpNgImpPmsiMvpnNoExpComm    TruthValue,
    vRtrLdpNgMaxEcmpRoutes           Unsigned32,
    vRtrLdpNgOperEcmp                Unsigned32,
    vRtrLdpNgPreferProtocolStitching TruthValue,
    vRtrLdpNgGenTunnelPreference     Unsigned32,
    vRtrLdpNgGenPreferTransportFrr   TruthValue
}

vRtrLdpNgGenCreateTime           OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenCreateTime indicates the sysUpTime when this
         LDP instance was created."
    ::= { vRtrLdpNgGeneralEntry 1 }

vRtrLdpNgGenIPv4UpTime           OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenIPv4UpTime indicates the time, in hundreds of
         seconds, that the IPv4 LDP instance has been in current operational
         state (vRtrLdpNgGenIPv4OperState).

         If the value of vRtrLdpNgGenIPv4OperState is 'inService (2)', then
         vRtrLdpNgGenIPv4UpTime specifies the time that the IPv4 LDP instance
         has been operationally up.

         If the value of vRtrLdpNgGenIPv4OperState is 'outOfService (3)', then
         vRtrLdpNgGenIPv4UpTime specifies the time that the IPv4 LDP instance
         has been operationally down.

         If the value of vRtrLdpNgGenIPv4OperState is 'transition (4)', then
         vRtrLdpNgGenIPv4UpTime specifies the time that the IPv4 LDP instance
         has been operationally in transition."
    ::= { vRtrLdpNgGeneralEntry 2 }

vRtrLdpNgGenIPv6UpTime           OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenIPv6UpTime indicates the time, in hundreds of
         seconds, that the IPv6 LDP instance has been in current operational
         state (vRtrLdpNgGenIPv6OperState).

         If the value of vRtrLdpNgGenIPv6OperState is 'inService (2)', then
         vRtrLdpNgGenIPv6UpTime specifies the time that the IPv6 LDP instance
         has been operationally up.

         If the value of vRtrLdpNgGenIPv6OperState is 'outOfService (3)', then
         vRtrLdpNgGenIPv6UpTime specifies the time that the IPv6 LDP instance
         has been operationally down.

         If the value of vRtrLdpNgGenIPv6OperState is 'transition (4)', then
         vRtrLdpNgGenIPv6UpTime specifies the time that the IPv6 LDP instance
         has been operationally in transition."
    ::= { vRtrLdpNgGeneralEntry 3 }

vRtrLdpNgGenLastChange           OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenLastChange indicates the sysUpTime when this
         row was last modified."
    ::= { vRtrLdpNgGeneralEntry 4 }

vRtrLdpNgGenAdminState           OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenAdminState specifies the desired
         administrative state for this LDP instance."
    DEFVAL      { inService }
    ::= { vRtrLdpNgGeneralEntry 5 }

vRtrLdpNgGenIPv4OperState        OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenIPv4OperState indicates the current
         operational state of this IPv4 LDP instance."
    ::= { vRtrLdpNgGeneralEntry 6 }

vRtrLdpNgGenIPv6OperState        OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenIPv6OperState indicates the current
         operational state of this IPv6 LDP instance."
    ::= { vRtrLdpNgGeneralEntry 7 }

vRtrLdpNgGenIPv4OperDownReason   OBJECT-TYPE
    SYNTAX      TmnxLdpGenOperDownReasonCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenIPv4OperDownReason indicates the reason that
         the IPv4 LDP instance is operationally down."
    ::= { vRtrLdpNgGeneralEntry 8 }

vRtrLdpNgGenIPv6OperDownReason   OBJECT-TYPE
    SYNTAX      TmnxLdpGenOperDownReasonCode
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenIPv6OperDownReason indicates the reason that
         the IPv6 LDP instance is operationally down."
    ::= { vRtrLdpNgGeneralEntry 9 }

vRtrLdpNgGenLdpIPv4LsrId         OBJECT-TYPE
    SYNTAX      MplsLsrIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenLdpIPv4LsrId is the IPv4 Label Switch Router
         (LSR) identifier which is used as the first 4 bytes or the Router Id
         component of the Label Distribution Protocol (LDP) identifier."
    ::= { vRtrLdpNgGeneralEntry 10 }

vRtrLdpNgGenLdpIPv6LsrId         OBJECT-TYPE
    SYNTAX      TmnxMplsLsrNgIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenLdpIPv6LsrId is the IPv6 Label Switch Router
         (LSR) identifier which is used as the first 16 bytes or the Router Id
         component of the Label Distribution Protocol (LDP) identifier."
    ::= { vRtrLdpNgGeneralEntry 11 }

vRtrLdpNgGenProtocolVersion      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of  vRtrLdpNgGenProtocolVersion specifies the
         version of the LDP protocol instance. A value of zero (0)
         indicates that the version of the protocol is unknown."
    ::= { vRtrLdpNgGeneralEntry 12 }

vRtrLdpNgGenBackoffTime          OBJECT-TYPE
    SYNTAX      TmnxLdpBackoffTime (1..2592000)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenBackoffTime specifies the initial value for
         the backoff interval.

         The backoff interval is the time, in seconds, that LDP waits after an
         LDP session setup has failed before it attempts to setup the session
         again. After the LDP session startup fails the first time, the backoff
         interval is set to the value of vRtrLdpNgGenBackoffTime. Thereafter,
         if session startup fails again the backoff interval increases
         exponentially."
    ::= { vRtrLdpNgGeneralEntry 13 }

vRtrLdpNgGenMaxBackoffTime       OBJECT-TYPE
    SYNTAX      TmnxLdpBackoffTime
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenMaxBackoffTime specifies the maximum value
         for the backoff interval.

         For each successive failure of the LDP session startup, the backoff
         interval (the time for which the router waits before retrying)
         increases exponentially. If the backoff interval exceeds
         vRtrLdpNgGenMaxBackoffTime, the router will give up trying to
         establish the LDP session.

         If vRtrLdpNgGenMaxBackoffTime is set to zero (0), then the backoff
         interval does not increase exponentially after the first session
         startup attempt fails. Instead it remains constant and LDP will keep
         retrying to establish a session until it succeeds."
    ::= { vRtrLdpNgGeneralEntry 14 }

vRtrLdpNgGenTunnelDownDampTime   OBJECT-TYPE
    SYNTAX      Unsigned32 (0..20)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenTunnelDownDampTime specifies the time
         interval, in seconds, that LDP waits before posting a tunnel down
         event to the Route Table Manager. If a tunnel up event is generated
         before the damping interval has elapsed, a tunnel modify event will be
         posted to the Route Table Manager (RTM). If this value is set to 0,
         then tunnel down events are not damped."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgGeneralEntry 15 }

vRtrLdpNgGenGracefulRestart      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenGracefulRestart specifies whether graceful
         restart helper is allowed.  When this object has a value of 'true',
         graceful restart helper is enabled.  When its value is 'false',
         graceful restart helper is disabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 16 }

vRtrLdpNgGenGRNbrLiveTime        OBJECT-TYPE
    SYNTAX      Unsigned32 (5..300)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenGRNbrLiveTime specifies the value for neighbor
         liveness timer.  The amount of time the Label Switching Router (LSR)
         keeps its stale label-FEC bindings is set to the lesser of the FT
         Reconnect Timeout, as was advertised by the  neighbor, and this local
         timer, called the Neighbor Liveness Timer.

         The LSR waits for the specified time till a LDP session re-establishes
         itself.  If within that time the LSR still does not establish an LDP
         session with the neighbor, all the stale bindings are deleted.  This
         object has meaning only when vRtrLdpNgGenGracefulRestart is 'true'."
    DEFVAL      { 120 }
    ::= { vRtrLdpNgGeneralEntry 17 }

vRtrLdpNgGenGRMaxRecoveryTime    OBJECT-TYPE
    SYNTAX      Unsigned32 (15..1800)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenGRMaxRecoveryTime specifies the local maximum
         recovery time.

         If the Label Switching Router (LSR)  determines that the neighbor was
         able to preserve its MPLS forwarding state (as was indicated by the
         non-zero Recovery Time advertised by the neighbor), the LSR should
         further keep the stale label-FEC  bindings, received from the
         neighbor, for as long as the lesser of the Recovery Time advertised
         by the neighbor, and a local configurable value, called Maximum
         Recovery Time, allows.  This object has meaning only when
         vRtrLdpNgGenGracefulRestart is 'true'."
    DEFVAL      { 120 }
    ::= { vRtrLdpNgGeneralEntry 18 }

vRtrLdpNgGenLabelWithdrawalDelay OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 3..120)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenLabelWithdrawalDelay specifies the time
         interval, in seconds, LDP will delay for the withdrawal of FEC-label
         binding it distributed to its neighbours when FEC is deactivated. When
         the timer expires, LDP then sends a label withdrawal for the FEC to
         all its neighbours. This is applicable only to LDP transport tunnels
         (ipv4 prefix FECs) and is not applicable to Pseudowires (service
         FECs).

         A value of 0 indicates that vRtrLdpNgGenLabelWithdrawalDelay is
         disabled."
    DEFVAL      { 0 }
    ::= { vRtrLdpNgGeneralEntry 19 }

vRtrLdpNgGenImplicitNull         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenImplicitNull specifies whether or not to
         signal implicit null values for all LDP FECs for which this node is an
         egress Label Edge Router (LER). When the value is true implicit null
         values are signaled."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 20 }

vRtrLdpNgGenShortTTLPropLocal    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenShortTTLPropLocal specifies whether or not
         to enable the propagation of time to live (TTL) from the header of
         IP packet into the header of resulting MPLS packet for all local
         packets forwarded over a LDP shortcut.  When the value is set to
         'true' TTL is propagated from the header of IP packet into the
         header of the resulting MPLS packet for all local packets."
    DEFVAL      { true }
    ::= { vRtrLdpNgGeneralEntry 21 }

vRtrLdpNgGenShortTTLPropTransit  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenShortTTLPropTransit specifies whether or not
         to enable the propagation of time to live (TTL) from the header of
         IP packet into the header of resulting MPLS packet for all transit
         packets forwarded over a LDP shortcut.  When the value is set to
         'true' TTL is propagated from the header of IP packet into the
         header of the resulting MPLS packet for all transit packets."
    DEFVAL      { true }
    ::= { vRtrLdpNgGeneralEntry 22 }

vRtrLdpNgGenMPMBBTime            OBJECT-TYPE
    SYNTAX      Unsigned32 (0..10)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenMPMBBTime specifies the maximum time a Multi
         Point (MP) transit node must wait before switching over to a new path
         if the new node does not send Make Before Break (MBB) Tag Length Value
         (TLV) to inform of the availability of the data plane."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgGeneralEntry 23 }

vRtrLdpNgGenLdpFrr               OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenLdpFrr specifies whether fast reroute of LDP
         tunnel is enabled or disabled.

         When the value of vRtrLdpNgGenLdpFrr is set to 'true' fast reroute of
         LDP tunnel is enabled and when vRtrLdpNgGenLdpFrr is set to 'false'
         fast reroute of LDP tunnel is disabled.

         When disabling vRtrLdpNgGenLdpFrr, the setting for FRR via
         segmented-routing tunnel stitching (vRtrLdpNgGenFrrSRStitch) must also
         be disabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 24 }

vRtrLdpNgGenMcastUpstreamFrr     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenMcastUpstreamFrr specifies whether mLDP fast
         upstream switchover feature is enabled or not for the LDP instance.
         When 'true', the LDP instance supports mLDP fast upstream switchover."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 25 }

vRtrLdpNgGenDeaggregateFec       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When vRtrLdpNgGenDeaggregateFec has a value of 'false', LDP aggregates
         multiple prefixes into a single Forwarding Equivalence Class (FEC) and
         advertises a single label for the FEC. When the value is 'true', LDP
         deaggregates prefixes into multiple FECs."
    ::= { vRtrLdpNgGeneralEntry 26 }

vRtrLdpNgGenControlMode          OBJECT-TYPE
    SYNTAX      INTEGER {
        ordered     (1),
        independent (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenControlMode specifies the mode used for
         distributing labels in response to label binding requests.

         When vRtrLdpNgGenControlMode has a value of 'ordered', label bindings
         are not distributed in response to a label request until a label
         binding has been received from the next hop for the destination.

         When vRtrLdpNgGenControlMode has a value of 'independent', label
         bindings are distributed immediately in response to a label request
         even if a label binding has not yet been received from the next hop
         for the destination."
    ::= { vRtrLdpNgGeneralEntry 27 }

vRtrLdpNgGenDistMethod           OBJECT-TYPE
    SYNTAX      TmnxLdpLabelDistMethod
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenDistMethod specifies the label distribution
         method used.

         When vRtrLdpNgGenDistMethod has a value of 'downstreamOnDemand', label
         bindings are distributed to the upstream LSR, for each FEC, without
         requiring a request message for the FEC from the upstream LSR.

         When vRtrLdpNgGenDistMethod has a value of 'downstreamUnsolicited',
         label bindings are distributed to the upstream LSR only when a label
         request message is received."
    ::= { vRtrLdpNgGeneralEntry 28 }

vRtrLdpNgGenRetentionMode        OBJECT-TYPE
    SYNTAX      INTEGER {
        conservative (1),
        liberal      (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenRetentionMode specifies the label retention
         mode used.

         If the value of this object is 'conservative', then advertised
         label mappings are retained only if they will be used to forward
         packets, i.e. if the label came from a valid next hop.  Label
         bindings received from non-nexthops for each FEC are discarded.

         If the value of this object is 'liberal', then all advertised
         label mappings are retained whether they are from a valid next
         hop or not.  When vRtrLdpNgGenDistMethod has a value of
         'downstreamUnsolicited', a LSR may receive label bindings for
         the same destination for all its neighbors.  Labels for the
         non-nexthops for the FECs are retained in the software but not
         used.  When a network topology change occurs where a non-nexthop
         becomes a true next hop, the label received earlier is then used."
    ::= { vRtrLdpNgGeneralEntry 29 }

vRtrLdpNgGenPropagatePolicy      OBJECT-TYPE
    SYNTAX      TmnxLdpFECPolicy
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenPropagatePolicy determines whether the LSR
         should generate FECs and which FECs it should generate.

         When the value of this object is 'system', LDP will distribute label
         bindings only for the router's system IP address

         When the value of this object is 'interface', LDP will distribute
         label bindings for all LDP interfaces

         When the value of this object is 'all', LDP will distribute label
         bindings for all prefixes in the routing table

         When the value of this object is 'none', LDP will not distribute any
         label bindings."
    ::= { vRtrLdpNgGeneralEntry 30 }

vRtrLdpNgGenLoopDetectCap        OBJECT-TYPE
    SYNTAX      INTEGER {
        none                  (1),
        other                 (2),
        hopCount              (3),
        pathVector            (4),
        hopCountAndPathVector (5)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenLoopDetectCap indicates whether this LSR
         supports loop detection and if so, what type of loop detection is
         supported.

         When the value is 'none' loop detection is not supported on this LSR.

         When the value is 'other' Loop Detection is supported but by a method
         other than those listed below.

         When the value is 'hopCount' Loop Detection is supported by Hop Count
         only.

         When the value is 'pathVector' Loop Detection is supported by Path
         Vector only.

         When the value is 'hopCountAndPathVector' Loop Detection is supported
         by both Hop Count and Path Vector.

         Since Loop Detection is determined during Session Initialization, an
         individual session may not be running with loop detection. This object
         simply gives an indication of whether or not the LSR has the ability
         to support Loop Detection and which types."
    ::= { vRtrLdpNgGeneralEntry 31 }

vRtrLdpNgGenHopLimit             OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenHopLimit specifies the maximum
         allowable value for the hop count.  The value of this object
         is valid and used only if vRtrLdpNgGenLoopDetectCap has
         a value of either 'hopCount' or 'hopCountAndPathVector'."
    ::= { vRtrLdpNgGeneralEntry 32 }

vRtrLdpNgGenPathVectorLimit      OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenPathVectorLimit specifies the maximum
         allowable value for the path vector count.  The value of this
         object is valid and used only if vRtrLdpNgGenLoopDetectCap
         has a value of either 'pathVector' or 'hopCountAndPathVector'."
    ::= { vRtrLdpNgGeneralEntry 33 }

vRtrLdpNgGenRoutePreference      OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenRoutePreference specifies the route
         preference assigned to LDP routes. When multiple routes are available
         to a destination, the route with the lowest preference will be used."
    ::= { vRtrLdpNgGeneralEntry 34 }

vRtrLdpNgGenClassForwarding      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenClassForwarding indicates whether class
         forwarding is enabled or not for LDP-over-RSVP."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 35 }

vRtrLdpNgGenIpv4LsrInterop       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenIpv4LsrInterop specifies if interoperability
         with legacy IPv4 LSR implementations which do not comply to the
         processing of Hello TLVs with the U-bit set is allowed."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 36 }

vRtrLdpNgGenEntropyLblCapability OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenEntropyLblCapability specifies whether
         entropy label capability is enabled or not on the LDP node. When the
         value of vRtrLdpNgGenEntropyLblCapability is set to 'true', the egress
         LER will advertise that it is capable of receiving and processing the
         entropy label."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 37 }

vRtrLdpNgGenFrrSRStitch          OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenFrrSRStitch specifies whether fast reroute of
         LDP tunnel via a segmented-routing tunnel is enabled or disabled.

         When the value of vRtrLdpNgGenFrrSRStitch is set to 'true' fast
         reroute of LDP tunnel via SR tunnel is enabled and when
         vRtrLdpNgGenFrrSRStitch is set to 'false' fast reroute of LDP tunnel
         via SR tunnel is disabled.

         Regular LDP FRR must be enabled via vRtrLdpNgGenLdpFrr in order to
         enable FRR via segmented-routing tunnel stitching."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 38 }

vRtrLdpNgGenMcastUpstrmAsbrFrr   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenMcastUpstrmAsbrFrr specifies whether the
         local leaf will do MOFRR to the multiple ASBRs or not.

         When the value of vRtrLdpNgGenMcastUpstrmAsbrFrr is set to 'false'
         only IGP MOFRR in the local AS is allowed."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 39 }

vRtrLdpNgGenBasicFecOnly         OBJECT-TYPE
    SYNTAX      TmnxEnabledDisabled
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenBasicFecOnly specifies whether the root node
         will generate a non recursive FEC even if the root node is resolved
         via BGP.

         When the value of vRtrLdpNgGenBasicFecOnly is set to 'enabled', a
         non-recursive FEC will be generated towards the root node.

         When the value of vRtrLdpNgGenBasicFecOnly is set to 'disabled', a
         recursive FEC will be generated towards the root node.

         This configuration is applicable to FECs whose root address is in the
         GRT and that have a generic LSP identifier as the opaque type."
    DEFVAL      { disabled }
    ::= { vRtrLdpNgGeneralEntry 40 }

vRtrLdpNgResolveRootUsing        OBJECT-TYPE
    SYNTAX      INTEGER {
        ucastRtm (1),
        mcastRtm (2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgResolveRootUsing specifies whether multicast
         FECs will use the unicast route table or the multicast route table
         for resolution."
    DEFVAL      { ucastRtm }
    ::= { vRtrLdpNgGeneralEntry 41 }

vRtrLdpNgGenWeightedEcmp         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenWeightedEcmp specifies
         whether or not LDP will use weighted-ECMP when programming
         LDP prefix FECs.  Weighting information must be available
         for the relevant route in order for weighted-ECMP to be used."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 42 }

vRtrLdpNgGenConsiderSysIPInGep   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenConsiderSysIPInGep specifies whether or not
         creation of system IP FECs is affected by the LDP global export
         policy. When enabled, the global export policy is consulted when
         determining whether or not to create a FEC for the system IP
         address(es). When disabled, FECs are unconditionally created for the
         system IP address(es)."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 43 }

vRtrLdpNgGenCBFMode              OBJECT-TYPE
    SYNTAX      INTEGER {
        lsr         (1),
        ler         (2),
        lsr-and-ler (3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenCBFMode indicates whether class forwarding is
         enabled for LER, LSR or both. It has no effect unless
         vRtrLdpNgGenClassForwarding is enabled."
    DEFVAL      { lsr }
    ::= { vRtrLdpNgGeneralEntry 44 }

vRtrLdpNgImpPmsiMvpn             OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgImpPmsiMvpn specifies  whether LDP will import
         BGP MVPN inter-AS routes."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 46 }

vRtrLdpNgImpPmsiMvpnNoExpComm    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgImpPmsiMvpnNoExpComm specifies  whether LDP will
         import BGP MVPN intra-AS routes."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 47 }

vRtrLdpNgMaxEcmpRoutes           OBJECT-TYPE
    SYNTAX      Unsigned32 (1..64)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgMaxEcmpRoutes specifies the maximum ECMP value
         for LDP. LDP uses the smaller value of this configured value and the
         ECMP value configured under router as the operational  ECMP value."
    DEFVAL      { 32 }
    ::= { vRtrLdpNgGeneralEntry 49 }

vRtrLdpNgOperEcmp                OBJECT-TYPE
    SYNTAX      Unsigned32 (1..64)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgOperEcmp specifies the operational ECMP  value.
         This value is the smaller of the configured router ECMP  value and the
         configured LDP max ECMP routes value."
    ::= { vRtrLdpNgGeneralEntry 50 }

vRtrLdpNgPreferProtocolStitching OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPreferProtocolStitching indicates whether
         stitching to another protocol is preferred over route  resolution. If
         the value is 'true', then protocol stitching is preferred. If value is
         'false', then route resolution is preferred."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 51 }

vRtrLdpNgGenTunnelPreference     OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenTunnelPreference specifies the tunnel
         preference assigned to LDP tunnels for address FECs."
    DEFVAL      { 9 }
    ::= { vRtrLdpNgGeneralEntry 52 }

vRtrLdpNgGenPreferTransportFrr   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgGenPreferTransportFrr indicates whether the FRR
         of the outer protocol is preferred or not. If the value  is 'true'
         then the FRR of outer protocol is preferred. If value  is 'false' then
         LDP FRR is preferred."
    DEFVAL      { false }
    ::= { vRtrLdpNgGeneralEntry 53 }

vRtrLdpNgPolicyTableLstCh        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolicyTableLstCh indicates the last timestamp
         when an entry in the vRtrLdpNgPolicyTable was last changed."
    ::= { tmnxLdpNgObjs 48 }

vRtrLdpNgPolicyTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgGeneralTable keeps information about LDP policies.

         Use of AUGMENTS clause implies a one-to-one dependent relationship
         between the base table, vRtrLdpNgGeneralTable, and the augmenting table,
         vRtrLdpTargTable. This in effect extends the vRtrLdpNgGeneralTable with
         additional columns.  Creation or deletion of a row in the
         vRtrLdpNgGeneralTable results in the same fate for the row in the
         vRtrLdpTargTable."
    ::= { tmnxLdpNgObjs 49 }

vRtrLdpNgPolicyEntry             OBJECT-TYPE
    SYNTAX      VRtrLdpNgPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table represents information about the policy
         configuration in LDP"
    AUGMENTS    { vRtrLdpNgGeneralEntry }
    ::= { vRtrLdpNgPolicyTable 1 }

VRtrLdpNgPolicyEntry             ::= SEQUENCE
{
    vRtrLdpNgPolRowLastCh            TimeStamp,
    vRtrLdpNgPolImportPolicy1        TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolImportPolicy2        TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolImportPolicy3        TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolImportPolicy4        TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolImportPolicy5        TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolExportPolicy1        TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolExportPolicy2        TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolExportPolicy3        TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolExportPolicy4        TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolExportPolicy5        TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolTunlTblExportPolicy1 TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolTunlTblExportPolicy2 TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolTunlTblExportPolicy3 TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolTunlTblExportPolicy4 TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolTunlTblExportPolicy5 TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolTunlTblImportPolicy1 TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolTunlTblImportPolicy2 TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolTunlTblImportPolicy3 TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolTunlTblImportPolicy4 TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolTunlTblImportPolicy5 TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolImportMcastPolicy1   TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolImportMcastPolicy2   TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolImportMcastPolicy3   TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolImportMcastPolicy4   TPolicyStatementNameOrEmpty,
    vRtrLdpNgPolImportMcastPolicy5   TPolicyStatementNameOrEmpty
}

vRtrLdpNgPolRowLastCh            OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolRowLastCh indicates the timestamp when this
         row was last modified."
    ::= { vRtrLdpNgPolicyEntry 1 }

vRtrLdpNgPolImportPolicy1        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolImportPolicy1 specifies the first import
         policy used to filter LDP label bindings received from LDP peers."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 2 }

vRtrLdpNgPolImportPolicy2        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolImportPolicy2 specifies the second import
         policy used to filter LDP label bindings received from LDP peers."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 3 }

vRtrLdpNgPolImportPolicy3        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolImportPolicy3 specifies the third import
         policy used to filter LDP label bindings received from LDP peers."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 4 }

vRtrLdpNgPolImportPolicy4        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolImportPolicy4 specifies the fourth import
         policy used to filter LDP label bindings received from LDP peers."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 5 }

vRtrLdpNgPolImportPolicy5        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolImportPolicy5 specifies the fifth import
         policy used to filter LDP label bindings received from LDP peers."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 6 }

vRtrLdpNgPolExportPolicy1        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolExportPolicy1 specifies the first export
         policy used to filter interface addresses that are exported as label
         bindings."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 7 }

vRtrLdpNgPolExportPolicy2        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolExportPolicy2 specifies the second export
         policy used to filter interface addresses that are exported as label
         bindings."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 8 }

vRtrLdpNgPolExportPolicy3        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolExportPolicy3 specifies the third export
         policy used to filter interface addresses that are exported as label
         bindings."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 9 }

vRtrLdpNgPolExportPolicy4        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolExportPolicy4 specifies the fourth export
         policy used to filter interface addresses that are exported as label
         bindings."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 10 }

vRtrLdpNgPolExportPolicy5        OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolExportPolicy5 specifies the fifth export
         policy used to filter interface addresses that are exported as label
         bindings."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 11 }

vRtrLdpNgPolTunlTblExportPolicy1 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolTunlTblExportPolicy1 specifies the first
         tunnel table export policy used for exporting tunneled routes from the
         CPM tunnel table as LDP FEC."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 12 }

vRtrLdpNgPolTunlTblExportPolicy2 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolTunlTblExportPolicy2 specifies the second
         tunnel table export policy used for exporting tunneled routes from the
         CPM tunnel table as LDP FEC."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 13 }

vRtrLdpNgPolTunlTblExportPolicy3 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolTunlTblExportPolicy3 specifies the third
         tunnel table export policy used for exporting tunneled routes from the
         CPM tunnel table as LDP FEC."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 14 }

vRtrLdpNgPolTunlTblExportPolicy4 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolTunlTblExportPolicy4 specifies the fourth
         tunnel table export policy used for exporting tunneled routes from the
         CPM tunnel table as LDP FEC."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 15 }

vRtrLdpNgPolTunlTblExportPolicy5 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolTunlTblExportPolicy5 specifies the fifth
         tunnel table export policy used for exporting tunneled routes from the
         CPM tunnel table as LDP FEC."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 16 }

vRtrLdpNgPolTunlTblImportPolicy1 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolTunlTblImportPolicy1 specifies the first
         tunnel table import policy used for controlling the insertion of
         non-host prefixes resolved by LDP into the CPM tunnel table."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 17 }

vRtrLdpNgPolTunlTblImportPolicy2 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolTunlTblImportPolicy2 specifies the second
         tunnel table import policy used for controlling the insertion of
         non-host prefixes resolved by LDP into the CPM tunnel table."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 18 }

vRtrLdpNgPolTunlTblImportPolicy3 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolTunlTblImportPolicy3 specifies the third
         tunnel table import policy used for controlling the insertion of
         non-host prefixes resolved by LDP into the CPM tunnel table."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 19 }

vRtrLdpNgPolTunlTblImportPolicy4 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolTunlTblImportPolicy4 specifies the fourth
         tunnel table import policy used for controlling the insertion of
         non-host prefixes resolved by LDP into the CPM tunnel table."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 20 }

vRtrLdpNgPolTunlTblImportPolicy5 OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolTunlTblImportPolicy5 specifies the fifth
         tunnel table import policy used for controlling the insertion of
         non-host prefixes resolved by LDP into the CPM tunnel table."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 21 }

vRtrLdpNgPolImportMcastPolicy1   OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolImportMcastPolicy1 specifies the first import
         multicast policy used for controlling which multicast FECs are
         accepted  from downstream peers for resolution."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 22 }

vRtrLdpNgPolImportMcastPolicy2   OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolImportMcastPolicy2 specifies the second
         import multicast policy used for controlling which multicast FECs are
         accepted  from downstream peers for resolution."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 23 }

vRtrLdpNgPolImportMcastPolicy3   OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolImportMcastPolicy3 specifies the third import
         multicast policy used for controlling which multicast FECs are
         accepted  from downstream peers for resolution."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 24 }

vRtrLdpNgPolImportMcastPolicy4   OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolImportMcastPolicy4 specifies the fourth
         import multicast policy used for controlling which multicast FECs are
         accepted  from downstream peers for resolution."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 25 }

vRtrLdpNgPolImportMcastPolicy5   OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgPolImportMcastPolicy5 specifies the fifth import
         multicast policy used for controlling which multicast FECs are
         accepted  from downstream peers for resolution."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgPolicyEntry 26 }

vRtrLdpNgIfParamsTableLstCh      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamsTableLstCh indicates the last timestamp
         when an entry in the vRtrLdpNgIfParamsTable was last changed."
    ::= { tmnxLdpNgObjs 50 }

vRtrLdpNgIfParamsTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgIfParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgIfParamsTable keeps information applicable to the interfaces
         in LDP.

         Use of AUGMENTS clause implies a one-to-one dependent relationship
         between the base table, vRtrLdpNgGeneralTable, and the augmenting
         table, vRtrLdpNgIfParamsTable. This in effect extends the
         vRtrLdpNgGeneralTable with additional columns.  Creation or deletion
         of a row in the vRtrLdpNgGeneralTable results in the same fate for the
         row in the vRtrLdpNgIfParamsTable."
    ::= { tmnxLdpNgObjs 51 }

vRtrLdpNgIfParamsEntry           OBJECT-TYPE
    SYNTAX      VRtrLdpNgIfParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table represents information applicable to the
         interfaces in LDP."
    AUGMENTS    { vRtrLdpNgGeneralEntry }
    ::= { vRtrLdpNgIfParamsTable 1 }

VRtrLdpNgIfParamsEntry           ::= SEQUENCE
{
    vRtrLdpNgIfParamRowLastCh        TimeStamp,
    vRtrLdpNgIfParamIPv4KAFactor     TmnxLdpKeepAliveFactor,
    vRtrLdpNgIfParamIPv6KAFactor     TmnxLdpKeepAliveFactor,
    vRtrLdpNgIfParamIPv4KATimeout    TmnxLdpNewKeepAliveTimeout,
    vRtrLdpNgIfParamIPv6KATimeout    TmnxLdpNewKeepAliveTimeout,
    vRtrLdpNgIfParamIPv4HelloFactor  TmnxLdpHelloFactor,
    vRtrLdpNgIfParamIPv6HelloFactor  TmnxLdpHelloFactor,
    vRtrLdpNgIfParamIPv4HelloTimeout TmnxLdpNewHelloTimeout,
    vRtrLdpNgIfParamIPv6HelloTimeout TmnxLdpNewHelloTimeout,
    vRtrLdpNgIfParamIPv4TransAddrTyp INTEGER,
    vRtrLdpNgIfParamIPv6TransAddrTyp INTEGER
}

vRtrLdpNgIfParamRowLastCh        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamRowLastCh indicates the timestamp when
         this row was last modified."
    ::= { vRtrLdpNgIfParamsEntry 1 }

vRtrLdpNgIfParamIPv4KAFactor     OBJECT-TYPE
    SYNTAX      TmnxLdpKeepAliveFactor
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamIPv4KAFactor specifies the value by which
         the keepalive timeout (vRtrLdpNgIfParamKeepAliveTimeout) should be
         divided to give the keepalive time i.e. the time interval, in seconds,
         between LDP keepalive messages. LDP keepalive messages are sent to
         keep the LDP session from timing out when no other LDP traffic is
         being sent between the neighbors.

         This value is only applicable to LDP IPv4 interfaces."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgIfParamsEntry 2 }

vRtrLdpNgIfParamIPv6KAFactor     OBJECT-TYPE
    SYNTAX      TmnxLdpKeepAliveFactor
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamIPv6KAFactor specifies the value by which
         the keepalive timeout (vRtrLdpNgIfParamKeepAliveTimeout) should be
         divided to give the keepalive time i.e. the time interval, in seconds,
         between LDP keepalive messages. LDP keepalive messages are sent to
         keep the LDP session from timing out when no other LDP traffic is
         being sent between the neighbors.

         This value is only applicable to LDP IPv6 interfaces."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgIfParamsEntry 3 }

vRtrLdpNgIfParamIPv4KATimeout    OBJECT-TYPE
    SYNTAX      TmnxLdpNewKeepAliveTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamIPv4KATimeout specifies the time
         interval, in seconds, that LDP waits before tearing down a session. If
         no LDP messages are exchanged during this time interval, the LDP
         session is torn down. Generally the value of
         vRtrLdpNgIfParamIPv4KATimeout is configured to be 3 times the
         keepalive time (the time interval between successive LDP keepalive
         messages).

         This value is only applicable to LDP IPv4 interfaces."
    DEFVAL      { 30 }
    ::= { vRtrLdpNgIfParamsEntry 4 }

vRtrLdpNgIfParamIPv6KATimeout    OBJECT-TYPE
    SYNTAX      TmnxLdpNewKeepAliveTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamIPv6KATimeout specifies the time
         interval, in seconds, that LDP waits before tearing down a session. If
         no LDP messages are exchanged during this time interval, the LDP
         session is torn down. Generally the value of
         vRtrLdpNgIfParamIPv6KATimeout is configured to be 3 times the
         keepalive time (the time interval between successive LDP keepalive
         messages).

         This value is only applicable to LDP IPv6 interfaces."
    DEFVAL      { 30 }
    ::= { vRtrLdpNgIfParamsEntry 5 }

vRtrLdpNgIfParamIPv4HelloFactor  OBJECT-TYPE
    SYNTAX      TmnxLdpHelloFactor
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamIPv4HelloFactor specifies the value by
         which the hello timeout (vRtrLdpNgIfParamIPv4HelloTimeout) should be
         divided to give the hello time i.e. the time interval, in seconds,
         between LDP Hello messages. LDP uses hello messages to discover
         neighbors and to detect loss of connectivity with its neighbors.

         This value is only applicable to LDP IPv4 interfaces."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgIfParamsEntry 6 }

vRtrLdpNgIfParamIPv6HelloFactor  OBJECT-TYPE
    SYNTAX      TmnxLdpHelloFactor
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamIPv6HelloFactor specifies the value by
         which the hello timeout (vRtrLdpNgIfParamIPv6HelloTimeout) should be
         divided to give the hello time i.e. the time interval, in seconds,
         between LDP Hello messages. LDP uses hello messages to discover
         neighbors and to detect loss of connectivity with its neighbors.

         This value is only applicable to LDP IPv6 interfaces."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgIfParamsEntry 7 }

vRtrLdpNgIfParamIPv4HelloTimeout OBJECT-TYPE
    SYNTAX      TmnxLdpNewHelloTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamIPv4HelloTimeout specifies the hello time
         also known as hold time. It is the time interval, in seconds, that LDP
         waits before declaring a neighbor to be down. Hello timeout is local
         to the system and is sent in the hello messages to a neighbor. Hello
         timeout cannot be set to a value that is less than 3 times the hello
         time.

         This value is only applicable to LDP IPv4 interfaces."
    DEFVAL      { 15 }
    ::= { vRtrLdpNgIfParamsEntry 8 }

vRtrLdpNgIfParamIPv6HelloTimeout OBJECT-TYPE
    SYNTAX      TmnxLdpNewHelloTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamIPv6HelloTimeout specifies the hello time
         also known as hold time. It is the time interval, in seconds, that LDP
         waits before declaring a neighbor to be down. Hello timeout is local
         to the system and is sent in the hello messages to a neighbor. Hello
         timeout cannot be set to a value that is less than 3 times the hello
         time.

         This value is only applicable to LDP IPv6 interfaces."
    DEFVAL      { 15 }
    ::= { vRtrLdpNgIfParamsEntry 9 }

vRtrLdpNgIfParamIPv4TransAddrTyp OBJECT-TYPE
    SYNTAX      INTEGER {
        interface (1),
        system    (2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamIPv4TransAddrTyp specifies the source
         of the transport address to be used when setting up the LDP TCP
         sessions.  The transport address can be configured globally
         (applied to all interfaces) or per interface.

         When the value of this object is 'interface', the interface's IP
         address is used to setup the LDP session between neighbors. If
         multiple interfaces exist between two neighbors, the 'interface' mode
         cannot be used since only one LDP session is actually set up between
         the two neighbors.

         When the value of this object is 'system', the system's IP address is
         used to set up the LDP session between neighbors.

         This value is only applicable to LDP IPv4 interfaces."
    DEFVAL      { system }
    ::= { vRtrLdpNgIfParamsEntry 10 }

vRtrLdpNgIfParamIPv6TransAddrTyp OBJECT-TYPE
    SYNTAX      INTEGER {
        interface (1),
        system    (2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgIfParamIPv6TransAddrTyp specifies the source
         of the transport address to be used when setting up the LDP TCP
         sessions.  The transport address can be configured globally
         (applied to all interfaces) or per interface.

         When the value of this object is 'interface', the interface's IP
         address is used to setup the LDP session between neighbors. If
         multiple interfaces exist between two neighbors, the 'interface' mode
         cannot be used since only one LDP session is actually set up between
         the two neighbors.

         When the value of this object is 'system', the system's IP address is
         used to set up the LDP session between neighbors.

         This value is only applicable to LDP IPv6 interfaces."
    DEFVAL      { system }
    ::= { vRtrLdpNgIfParamsEntry 11 }

vRtrLdpNgTargTableLstCh          OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargTableLstCh indicates the last timestamp when
         an entry in the vRtrLdpNgTargTable was last changed."
    ::= { tmnxLdpNgObjs 52 }

vRtrLdpNgTargTable               OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgTargEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgTargTable keeps information applicable to the LDP targeted
         peers.

         Use of AUGMENTS clause implies a one-to-one dependent relationship
         between the base table, vRtrLdpNgGeneralTable, and the augmenting
         table, vRtrLdpNgTargTable. This in effect extends the
         vRtrLdpNgGeneralTable with additional columns.  Creation or deletion
         of a row in the vRtrLdpNgGeneralTable results in the same fate for the
         row in the vRtrLdpNgTargTable."
    ::= { tmnxLdpNgObjs 53 }

vRtrLdpNgTargEntry               OBJECT-TYPE
    SYNTAX      VRtrLdpNgTargEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table represents information applicable to the LDP
         targeted peers in virtual router instance."
    AUGMENTS    { vRtrLdpNgGeneralEntry }
    ::= { vRtrLdpNgTargTable 1 }

VRtrLdpNgTargEntry               ::= SEQUENCE
{
    vRtrLdpNgTargRowLastCh           TimeStamp,
    vRtrLdpNgTargImportPolicy1       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargImportPolicy2       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargImportPolicy3       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargImportPolicy4       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargImportPolicy5       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargExportPolicy1       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargExportPolicy2       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargExportPolicy3       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargExportPolicy4       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargExportPolicy5       TPolicyStatementNameOrEmpty,
    vRtrLdpNgTargTunnelPreference    TruthValue,
    vRtrLdpNgTargetedSessions        TruthValue,
    vRtrLdpNgTargIPv4KAFactor        TmnxLdpKeepAliveFactor,
    vRtrLdpNgTargIPv6KAFactor        TmnxLdpKeepAliveFactor,
    vRtrLdpNgTargIPv4KATimeout       TmnxLdpNewKeepAliveTimeout,
    vRtrLdpNgTargIPv6KATimeout       TmnxLdpNewKeepAliveTimeout,
    vRtrLdpNgTargIPv4HelloFactor     TmnxLdpHelloFactor,
    vRtrLdpNgTargIPv6HelloFactor     TmnxLdpHelloFactor,
    vRtrLdpNgTargIPv4HelloTimeout    TmnxLdpNewHelloTimeout,
    vRtrLdpNgTargIPv6HelloTimeout    TmnxLdpNewHelloTimeout,
    vRtrLdpNgTargIPv4HelloReduction  TruthValue,
    vRtrLdpNgTargIPv6HelloReduction  TruthValue,
    vRtrLdpNgTargIPv4HelloReduceFctr Unsigned32,
    vRtrLdpNgTargIPv6HelloReduceFctr Unsigned32,
    vRtrLdpNgTargTunnelMcastPrefer   TruthValue,
    vRtrLdpNgTargAutoTxV4AdminState  TmnxAdminState,
    vRtrLdpNgTargAutoTxV4Tunneling   TruthValue,
    vRtrLdpNgTargAutoRxV4AdminState  TmnxAdminState,
    vRtrLdpNgTargAutoRxV4Tunneling   TruthValue,
    vRtrLdpNgTargResV6PfxOvrShortcut TruthValue
}

vRtrLdpNgTargRowLastCh           OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargRowLastCh indicates the timestamp when this
         row was last modified."
    ::= { vRtrLdpNgTargEntry 1 }

vRtrLdpNgTargImportPolicy1       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargImportPolicy1 specifies the import policy to
         determine which prefix FECs are accepted from targeted peers for
         resolution. A maximum of 5 policies can be specified.
         vRtrLdpNgTargImportPolicy1 specifies the first policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTargEntry 2 }

vRtrLdpNgTargImportPolicy2       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargImportPolicy2 specifies the import policy to
         determine which prefix FECs are accepted from targeted peers for
         resolution. A maximum of 5 policies can be specified.
         vRtrLdpNgTargImportPolicy2 specifies the second policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTargEntry 3 }

vRtrLdpNgTargImportPolicy3       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargImportPolicy3 specifies the import policy to
         determine which prefix FECs are accepted from targeted peers for
         resolution. A maximum of 5 policies can be specified.
         vRtrLdpNgTargImportPolicy3 specifies the third policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTargEntry 4 }

vRtrLdpNgTargImportPolicy4       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargImportPolicy4 specifies the import policy to
         determine which prefix FECs are accepted from targeted peers for
         resolution. A maximum of 5 policies can be specified.
         vRtrLdpNgTargImportPolicy4 specifies the fourth policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTargEntry 5 }

vRtrLdpNgTargImportPolicy5       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargImportPolicy5 specifies the import policy to
         determine which prefix FECs are accepted from targeted peers for
         resolution. A maximum of 5 policies can be specified.
         vRtrLdpNgTargImportPolicy5 specifies the fifth policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTargEntry 6 }

vRtrLdpNgTargExportPolicy1       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargExportPolicy1 specifies the export policy
         used to determine which prefix FECs are exported to all targeted
         sessions. A maximum of 5 policies can be specified.
         vRtrLdpNgTargExportPolicy1 specifies the first policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTargEntry 7 }

vRtrLdpNgTargExportPolicy2       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargExportPolicy2 specifies the export policy
         used to determine which prefix FECs are exported to all targeted
         sessions. A maximum of 5 policies can be specified.
         vRtrLdpNgTargExportPolicy2 specifies the second policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTargEntry 8 }

vRtrLdpNgTargExportPolicy3       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargExportPolicy3 specifies the export policy
         used to determine which prefix FECs are exported to all targeted
         sessions. A maximum of 5 policies can be specified.
         vRtrLdpNgTargExportPolicy3 specifies the third policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTargEntry 9 }

vRtrLdpNgTargExportPolicy4       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargExportPolicy4 specifies the export policy
         used to determine which prefix FECs are exported to all targeted
         sessions. A maximum of 5 policies can be specified.
         vRtrLdpNgTargExportPolicy4 specifies the fourth policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTargEntry 10 }

vRtrLdpNgTargExportPolicy5       OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargExportPolicy5 specifies the export policy
         used to determine which prefix FECs are exported to all targeted
         sessions. A maximum of 5 policies can be specified.
         vRtrLdpNgTargExportPolicy5 specifies the fifth policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTargEntry 11 }

vRtrLdpNgTargTunnelPreference    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargTunnelPreference indicates whether LDP over
         tunnel is preferred when link-level LDP bindings are also available.
         If this value is 'true', then LDP tunnels are preferred and if the
         value is 'false' then LDP over tunnel is preferred.

         By default LDP tunnels are preferred."
    DEFVAL      { true }
    ::= { vRtrLdpNgTargEntry 12 }

vRtrLdpNgTargetedSessions        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargetedSessions specifies whether or
         not targeted sessions are allowed.  Targeted sessions are LDP
         sessions between indirectly connected peers.  The discovery
         messages for an indirect LDP session are addressed to the
         specified peer instead of to the multicast address.  When this
         object has a value of 'true', targeted sessions are enabled.
         When its value is 'false', targeted sessions are disabled."
    DEFVAL      { true }
    ::= { vRtrLdpNgTargEntry 13 }

vRtrLdpNgTargIPv4KAFactor        OBJECT-TYPE
    SYNTAX      TmnxLdpKeepAliveFactor
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv4KAFactor specifies the value by which
         the keepalive timeout (vRtrLdpNgTargKATimeout) should be divided to
         give the keepalive time i.e. the time interval, in seconds, between
         LDP keepalive messages. LDP keepalive messages are sent to keep the
         LDP session from timing out when no other LDP traffic is being sent
         between the neighbors.

         This value is only applicable to IPv4 targeted LDP peer."
    DEFVAL      { 4 }
    ::= { vRtrLdpNgTargEntry 14 }

vRtrLdpNgTargIPv6KAFactor        OBJECT-TYPE
    SYNTAX      TmnxLdpKeepAliveFactor
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv6KAFactor specifies the value by which
         the keepalive timeout (vRtrLdpNgTargKATimeout) should be divided to
         give the keepalive time i.e. the time interval, in seconds, between
         LDP keepalive messages. LDP keepalive messages are sent to keep the
         LDP session from timing out when no other LDP traffic is being sent
         between the neighbors.

         This value is only applicable to IPv6 targeted LDP peer."
    DEFVAL      { 4 }
    ::= { vRtrLdpNgTargEntry 15 }

vRtrLdpNgTargIPv4KATimeout       OBJECT-TYPE
    SYNTAX      TmnxLdpNewKeepAliveTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv4KATimeout specifies the time interval,
         in seconds, that LDP waits before tearing down a session. If no LDP
         messages are exchanged during this time interval, the LDP session is
         torn down. Generally the value of vRtrLdpNgTargIPv4KATimeout is
         configured to be 3 times the keepalive time (the time interval between
         successive LDP keepalive messages).

         This value is only applicable to IPv4 LDP targeted peer."
    DEFVAL      { 40 }
    ::= { vRtrLdpNgTargEntry 16 }

vRtrLdpNgTargIPv6KATimeout       OBJECT-TYPE
    SYNTAX      TmnxLdpNewKeepAliveTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv6KATimeout specifies the time interval,
         in seconds, that LDP waits before tearing down a session. If no LDP
         messages are exchanged during this time interval, the LDP session is
         torn down. Generally the value of vRtrLdpNgTargIPv6KATimeout is
         configured to be 3 times the keepalive time (the time interval between
         successive LDP keepalive messages).

         This value is only applicable to IPv6 LDP targeted peer."
    DEFVAL      { 40 }
    ::= { vRtrLdpNgTargEntry 17 }

vRtrLdpNgTargIPv4HelloFactor     OBJECT-TYPE
    SYNTAX      TmnxLdpHelloFactor
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv4HelloFactor specifies the value by which
         the hello timeout (vRtrLdpNgTargIPv4HelloTimeout) should be divided to
         give the hello time i.e. the time interval, in seconds, between LDP
         Hello messages. LDP uses hello messages to discover neighbors and to
         detect loss of connectivity with its neighbors.

         This value is only applicable to IPv4 LDP targeted peer."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgTargEntry 18 }

vRtrLdpNgTargIPv6HelloFactor     OBJECT-TYPE
    SYNTAX      TmnxLdpHelloFactor
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv6HelloFactor specifies the value by which
         the hello timeout (vRtrLdpNgTargIPv6HelloTimeout) should be divided to
         give the hello time i.e. the time interval, in seconds, between LDP
         Hello messages. LDP uses hello messages to discover neighbors and to
         detect loss of connectivity with its neighbors.

         This value is only applicable to IPv6 LDP targeted peer."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgTargEntry 19 }

vRtrLdpNgTargIPv4HelloTimeout    OBJECT-TYPE
    SYNTAX      TmnxLdpNewHelloTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv4HelloTimeout specifies the hello time
         also known as hold time. It is the time interval, in seconds, that LDP
         waits before declaring a neighbor to be down. Hello timeout is local
         to the system and is sent in the hello messages to a neighbor. Hello
         timeout cannot be set to a value that is less than 3 times the hello
         time.

         This value is only applicable to IPv4 LDP targeted peer."
    DEFVAL      { 45 }
    ::= { vRtrLdpNgTargEntry 20 }

vRtrLdpNgTargIPv6HelloTimeout    OBJECT-TYPE
    SYNTAX      TmnxLdpNewHelloTimeout
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv6HelloTimeout specifies the hello time
         also known as hold time. It is the time interval, in seconds, that LDP
         waits before declaring a neighbor to be down. Hello timeout is local
         to the system and is sent in the hello messages to a neighbor. Hello
         timeout cannot be set to a value that is less than 3 times the hello
         time.

         This value is only applicable to IPv6 LDP targeted peer."
    DEFVAL      { 45 }
    ::= { vRtrLdpNgTargEntry 21 }

vRtrLdpNgTargIPv4HelloReduction  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv4HelloReduction specifies whether hello
         reduction to this targeted peer is enabled or not. If enabled, the
         sender advertises further dampened vRtrLdpNgTargIPv4HelloTimeout, to
         the targeted peer after LDP session is established.

         The value of 'true' means targeted hello reduction is enabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgTargEntry 22 }

vRtrLdpNgTargIPv6HelloReduction  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv6HelloReduction specifies whether hello
         reduction to this targeted peer is enabled or not. If enabled, the
         sender advertises further dampened vRtrLdpNgTargIPv6HelloTimeout, to
         the targeted peer after LDP session is established.

         The value of 'true' means targeted hello reduction is enabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgTargEntry 23 }

vRtrLdpNgTargIPv4HelloReduceFctr OBJECT-TYPE
    SYNTAX      Unsigned32 (3..20)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv4HelloReduceFctr specifies the number of
         hello messages that are sent at consistent
         vRtrLdpNgTargIPv4HelloTimeout, before advertising further dampened
         vRtrLdpNgTargIPv4HelloTimeout.

         An 'inconsistentValue' error is returned if this object is set when
         vRtrLdpNgTargIPv4HelloReduction is disabled."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgTargEntry 24 }

vRtrLdpNgTargIPv6HelloReduceFctr OBJECT-TYPE
    SYNTAX      Unsigned32 (3..20)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargIPv6HelloReduceFctr specifies the number of
         hello messages that are sent at consistent
         vRtrLdpNgTargIPv6HelloTimeout, before advertising further dampened
         vRtrLdpNgTargIPv6HelloTimeout.

         An 'inconsistentValue' error is returned if this object is set when
         vRtrLdpNgTargIPv6HelloReduction is disabled."
    DEFVAL      { 3 }
    ::= { vRtrLdpNgTargEntry 25 }

vRtrLdpNgTargTunnelMcastPrefer   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargTunnelMcastPrefer indicates the preference
         of targeted LDP session over a link LDP session for both the upstream
         and downstream resolution of a multicast FEC. If this value is 'true',
         then link session is preferred for upstream FEC resolution and regular
         next-hop is preferred for downstream FEC resolution. If the value is
         'false' then targeted session is preferred for upstream FEC resolution
         and tunneled next-hop is preferred for downstream FEC resolution."
    DEFVAL      { true }
    ::= { vRtrLdpNgTargEntry 26 }

vRtrLdpNgTargAutoTxV4AdminState  OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargAutoTxV4AdminState specifies whether
         automatic IPv4 TX targeted sessions are created or not. When this
         object is administratively up, automatic targeted sessions are created
         to the PQ router ID of each route that contains remote LFA
         information. When this object is administratively down, automatic
         targeted sessions are not created to the PQ router IDs."
    DEFVAL      { outOfService }
    ::= { vRtrLdpNgTargEntry 27 }

vRtrLdpNgTargAutoTxV4Tunneling   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargAutoTxV4Tunneling specifies whether
         tunneling of unicast LDP FECs over tunnels is enabled for the
         automatic IPv4 TX targeted sessions. When this object has a value of
         'true', tunneling is enabled. When its value is 'false', tunneling is
         disabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgTargEntry 28 }

vRtrLdpNgTargAutoRxV4AdminState  OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargAutoRxV4AdminState specifies whether
         automatic IPv4 RX targeted sessions are created or not. When this
         object is administratively up, the reception of an unhandled IPv4
         targeted hello message causes the creation of automatic targeted
         session to the source peer of the hello message. When this object is
         administratively down, automatic targeted sessions are not created for
         unhandled IPv4 targeted hello messages."
    DEFVAL      { outOfService }
    ::= { vRtrLdpNgTargEntry 29 }

vRtrLdpNgTargAutoRxV4Tunneling   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargAutoRxV4Tunneling specifies whether
         tunneling of unicast LDP FECs over tunnels is enabled for the
         automatic IPv4 RX targeted sessions. When this object has a value of
         'true', tunneling is enabled. When its value is 'false', tunneling is
         disabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgTargEntry 30 }

vRtrLdpNgTargResV6PfxOvrShortcut OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargResV6PfxOvrShortcut indicates whether an
         IPv6 prefix FEC is resolved over an IGP shortcut. If the value is
         'true', then  resolution is allowed. If value is 'false', then
         resolution is not allowed."
    DEFVAL      { false }
    ::= { vRtrLdpNgTargEntry 31 }

vRtrLdpNgAggrPreMatchTableLstCh  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAggrPreMatchTableLstCh indicates the last
         timestamp when an entry in the vRtrLdpNgAggrPreMatchTable was last
         changed."
    ::= { tmnxLdpNgObjs 54 }

vRtrLdpNgAggrPreMatchTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgAggrPreMatchEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgAggrPreMatchTable keeps information about aggregate prefix
         match procedures.

         Use of AUGMENTS clause implies a one-to-one dependent
         relationship between the base table, vRtrLdpNgGeneralTable,
         and the augmenting table, vRtrLdpNgAggrPreMatchTable. This in
         effect extends the vRtrLdpNgGeneralTable with additional
         columns.  Creation or deletion of a row in the
         vRtrLdpNgGeneralTable results in the same fate for the row
         in the vRtrLdpNgAggrPreMatchTable."
    REFERENCE
        "RFC5283 LDP Extension for Inter-Area Label Switched Paths (LSPs)"
    ::= { tmnxLdpNgObjs 55 }

vRtrLdpNgAggrPreMatchEntry       OBJECT-TYPE
    SYNTAX      VRtrLdpNgAggrPreMatchEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table represents information about the aggregate prefix
         match procedures."
    AUGMENTS    { vRtrLdpNgGeneralEntry }
    ::= { vRtrLdpNgAggrPreMatchTable 1 }

VRtrLdpNgAggrPreMatchEntry       ::= SEQUENCE
{
    vRtrLdpNgAggrPreMatchRowLastCh   TimeStamp,
    vRtrLdpNgAggrPreMatchEnabled     TruthValue,
    vRtrLdpNgAggrPreMatchExcPolicy1  TPolicyStatementNameOrEmpty,
    vRtrLdpNgAggrPreMatchExcPolicy2  TPolicyStatementNameOrEmpty,
    vRtrLdpNgAggrPreMatchExcPolicy3  TPolicyStatementNameOrEmpty,
    vRtrLdpNgAggrPreMatchExcPolicy4  TPolicyStatementNameOrEmpty,
    vRtrLdpNgAggrPreMatchExcPolicy5  TPolicyStatementNameOrEmpty,
    vRtrLdpNgAggrPreMatchAdminState  TmnxAdminState
}

vRtrLdpNgAggrPreMatchRowLastCh   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAggrPreMatchRowLastCh indicates the timestamp
         when this row was last modified."
    ::= { vRtrLdpNgAggrPreMatchEntry 1 }

vRtrLdpNgAggrPreMatchEnabled     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAggrPreMatchEnabled specifies whether aggregate
         prefix match procedures are enabled."
    DEFVAL      { false }
    ::= { vRtrLdpNgAggrPreMatchEntry 2 }

vRtrLdpNgAggrPreMatchExcPolicy1  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAggrPreMatchExcPolicy1 specifies the policy name
         containing the prefixes to be excluded from the aggregate prefix match
         procedures. A maximum of 5 policies can be specified.
         vRtrLdpNgAggrPreMatchExcPolicy1 specifies the first policy."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgAggrPreMatchEntry 3 }

vRtrLdpNgAggrPreMatchExcPolicy2  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAggrPreMatchExcPolicy2 specifies the second
         policy name containing the prefixes to be excluded from the aggregate
         prefix match procedures."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgAggrPreMatchEntry 4 }

vRtrLdpNgAggrPreMatchExcPolicy3  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAggrPreMatchExcPolicy3 specifies the third
         policy name containing the prefixes to be excluded from the aggregate
         prefix match procedures."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgAggrPreMatchEntry 5 }

vRtrLdpNgAggrPreMatchExcPolicy4  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAggrPreMatchExcPolicy4 specifies the fourth
         policy name containing the prefixes to be excluded from the aggregate
         prefix match procedures."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgAggrPreMatchEntry 6 }

vRtrLdpNgAggrPreMatchExcPolicy5  OBJECT-TYPE
    SYNTAX      TPolicyStatementNameOrEmpty
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAggrPreMatchExcPolicy5 specifies the fifth
         policy name containing the prefixes to be excluded from the aggregate
         prefix match procedures."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgAggrPreMatchEntry 7 }

vRtrLdpNgAggrPreMatchAdminState  OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgAggrPreMatchAdminState specifies whether the
         aggregate prefix procedures will be used by LDP."
    DEFVAL      { outOfService }
    ::= { vRtrLdpNgAggrPreMatchEntry 8 }

tmnxLdpNgNotificationObjects     OBJECT IDENTIFIER ::= { tmnxLdpNgObjs 56 }

vRtrLdpNgSessOperThresLevel      OBJECT-TYPE
    SYNTAX      INTEGER {
        up   (0),
        down (1)
    }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessOperThresLevel indicates whether the number
         of fec-bindings has exceeded or is below the configured fec threshold."
    ::= { tmnxLdpNgNotificationObjects 1 }

vRtrLdpNgInstNotifyReasonCode    OBJECT-TYPE
    SYNTAX      INTEGER {
        adminUp   (1),
        adminDown (2),
        operUp    (3),
        operDown  (4)
    }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgInstNotifyReasonCode indicates the reason for
         the LDP instance state change."
    ::= { tmnxLdpNgNotificationObjects 2 }

vRtrLdpNgSessOverloadState       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessOverloadState indicates if session is
         overload or not."
    ::= { tmnxLdpNgNotificationObjects 3 }

vRtrLdpNgSessOverloadDirection   OBJECT-TYPE
    SYNTAX      INTEGER {
        sent     (1),
        received (2)
    }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessOverloadDirection indicates if the LDP
         Overload Notification message is sent to or received from the peer."
    ::= { tmnxLdpNgNotificationObjects 4 }

vRtrLdpNgSessOverloadFecType     OBJECT-TYPE
    SYNTAX      INTEGER {
        prefixes  (1),
        p2mp      (2),
        svcFec128 (3),
        svcFec129 (4)
    }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessOverloadFecType indicates the overloaded FEC
         type."
    ::= { tmnxLdpNgNotificationObjects 5 }

vRtrLdpNgSessOvldFecTypeSubTyp   OBJECT-TYPE
    SYNTAX      INTEGER {
        ipv4      (1),
        ipv6      (2),
        allVcType (3)
    }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgSessOvldFecTypeSubTyp indicates the sub type for
         overloaded FEC type."
    ::= { tmnxLdpNgNotificationObjects 6 }

vLdpNgAddrActiveFecTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgAddrActiveFecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vLdpNgAddrActiveFecTable is a read-only table that represents all
         active in data plane address FECs either sent to or received from an
         LDP peer known to the Virtual Router."
    ::= { tmnxLdpNgObjs 57 }

vLdpNgAddrActiveFecEntry         OBJECT-TYPE
    SYNTAX      VLdpNgAddrActiveFecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of an active in data plane
         address FEC sent to or received from an LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgAddrFecFecType,
        vRtrLdpNgAddrFecIpPrefixType,
        vRtrLdpNgAddrFecIpPrefix,
        vRtrLdpNgAddrFecIpPrefixLen,
        vLdpNgAddrActiveFecOpType
    }
    ::= { vLdpNgAddrActiveFecTable 1 }

VLdpNgAddrActiveFecEntry         ::= SEQUENCE
{
    vLdpNgAddrActiveFecOpType        INTEGER,
    vLdpNgAddrActiveFecFecFlags      TmnxLdpFECFlags,
    vLdpNgAddrActiveFecNumInLbls     Unsigned32,
    vLdpNgAddrActiveFecNumOutLbls    Unsigned32
}

vLdpNgAddrActiveFecOpType        OBJECT-TYPE
    SYNTAX      INTEGER {
        pop  (1),
        push (2),
        swap (3)
    }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOpType indicates operation type of
         this FEC."
    ::= { vLdpNgAddrActiveFecEntry 1 }

vLdpNgAddrActiveFecFecFlags      OBJECT-TYPE
    SYNTAX      TmnxLdpFECFlags
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The bit flags of vLdpNgAddrActiveFecFecFlags indicates the
         characteristics of the FEC."
    ::= { vLdpNgAddrActiveFecEntry 2 }

vLdpNgAddrActiveFecNumInLbls     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecNumInLbls indicates the number of
         labels that have been sent to the peer associated with this FEC."
    ::= { vLdpNgAddrActiveFecEntry 3 }

vLdpNgAddrActiveFecNumOutLbls    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecNumOutLbls indicates the number of
         labels that have been received from the peer associated with this FEC."
    ::= { vLdpNgAddrActiveFecEntry 4 }

vLdpNgAddrActiveFecInLblTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgAddrActiveFecInLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vLdpNgAddrActiveFecInLblTable is a read-only table that represents all
         active in data plane address FECs received from an LDP peer known to
         the Virtual Router."
    ::= { tmnxLdpNgObjs 58 }

vLdpNgAddrActiveFecInLblEntry    OBJECT-TYPE
    SYNTAX      VLdpNgAddrActiveFecInLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of an active in data plane
         address FEC received from an LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgAddrFecFecType,
        vRtrLdpNgAddrFecIpPrefixType,
        vRtrLdpNgAddrFecIpPrefix,
        vRtrLdpNgAddrFecIpPrefixLen,
        vLdpNgAddrActiveFecOpType,
        vLdpNgAddrActiveFecInLblId
    }
    ::= { vLdpNgAddrActiveFecInLblTable 1 }

VLdpNgAddrActiveFecInLblEntry    ::= SEQUENCE
{
    vLdpNgAddrActiveFecInLblId       Unsigned32,
    vLdpNgAddrActiveFecInLbl         Unsigned32,
    vLdpNgAddrActiveFecInLblIfIndex  InterfaceIndexOrZero
}

vLdpNgAddrActiveFecInLblId       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecInLblId indicates the label number of
         the ingress label exchanged."
    ::= { vLdpNgAddrActiveFecInLblEntry 1 }

vLdpNgAddrActiveFecInLbl         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecInLbl indicates the ingress label
         exchanged."
    ::= { vLdpNgAddrActiveFecInLblEntry 2 }

vLdpNgAddrActiveFecInLblIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecInLblIfIndex indicates the interface
         index for ingress label."
    ::= { vLdpNgAddrActiveFecInLblEntry 3 }

vLdpNgAddrActiveFecOutLblTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF VLdpNgAddrActiveFecOutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vLdpNgAddrActiveFecOutLblTable is a read-only table that represents
         all active in data plane address FECs received from an LDP peer known
         to the Virtual Router."
    ::= { tmnxLdpNgObjs 59 }

vLdpNgAddrActiveFecOutLblEntry   OBJECT-TYPE
    SYNTAX      VLdpNgAddrActiveFecOutLblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of an active in data plane
         address FEC received from an LDP peer."
    INDEX       {
        vRtrID,
        vRtrLdpNgAddrFecFecType,
        vRtrLdpNgAddrFecIpPrefixType,
        vRtrLdpNgAddrFecIpPrefix,
        vRtrLdpNgAddrFecIpPrefixLen,
        vLdpNgAddrActiveFecOpType,
        vLdpNgAddrActiveFecOutLblId
    }
    ::= { vLdpNgAddrActiveFecOutLblTable 1 }

VLdpNgAddrActiveFecOutLblEntry   ::= SEQUENCE
{
    vLdpNgAddrActiveFecOutLblId      Unsigned32,
    vLdpNgAddrActiveFecOutLbl        Unsigned32,
    vLdpNgAddrActiveFecOutLblStatus  TmnxLabelStatus,
    vLdpNgAddrActiveFecOutLblIfIdx   InterfaceIndexOrZero,
    vLdpNgAddrActiveFecOutLblNHType  InetAddressType,
    vLdpNgAddrActiveFecOutLblNHAddr  InetAddress,
    vLdpNgAddrActiveFecOutLblMetric  Unsigned32,
    vLdpNgAddrActiveFecOutLblMtu     Unsigned32,
    vLdpNgAddrActiveFecOutLblLspId   Unsigned32,
    vLdpNgAddrActiveFecOutLblCBF     TmnxCBFClasses
}

vLdpNgAddrActiveFecOutLblId      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOutLblId indicates the label number of
         the egress label exchanged."
    ::= { vLdpNgAddrActiveFecOutLblEntry 1 }

vLdpNgAddrActiveFecOutLbl        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOutLbl indicates the egress label
         exchanged"
    ::= { vLdpNgAddrActiveFecOutLblEntry 2 }

vLdpNgAddrActiveFecOutLblStatus  OBJECT-TYPE
    SYNTAX      TmnxLabelStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOutLblStatus indicates the status of
         the egress label."
    ::= { vLdpNgAddrActiveFecOutLblEntry 3 }

vLdpNgAddrActiveFecOutLblIfIdx   OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOutLblIfIdx indicates the interface
         index for egress label."
    ::= { vLdpNgAddrActiveFecOutLblEntry 4 }

vLdpNgAddrActiveFecOutLblNHType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOutLblNHType indicates the address
         type of vLdpNgAddrActiveFecOutLblNHAddr."
    ::= { vLdpNgAddrActiveFecOutLblEntry 5 }

vLdpNgAddrActiveFecOutLblNHAddr  OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOutLblNHAddr indicates the IP address
         of the next hop for egress label."
    ::= { vLdpNgAddrActiveFecOutLblEntry 6 }

vLdpNgAddrActiveFecOutLblMetric  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOutLblMetric indicates the relative
         cost of the tunnel represented by this address FEC egress label."
    ::= { vLdpNgAddrActiveFecOutLblEntry 7 }

vLdpNgAddrActiveFecOutLblMtu     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOutLblMtu indicates the maximum
         transfer unit for payloads represented by this address FEC egress
         label."
    ::= { vLdpNgAddrActiveFecOutLblEntry 8 }

vLdpNgAddrActiveFecOutLblLspId   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOutLblLspId indicates the LSP id
         associated with egress label."
    ::= { vLdpNgAddrActiveFecOutLblEntry 9 }

vLdpNgAddrActiveFecOutLblCBF     OBJECT-TYPE
    SYNTAX      TmnxCBFClasses
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vLdpNgAddrActiveFecOutLblCBF indicates (if
         vRtrLdpNgAddrFecOutLblLspId is non-zero) the forwarding classes
         installed for the RSVP tunnel used by LDP in LDP over RSVP associated
         with egress label.

         If bit is set to 8, it indicates if the LSP for the RSVP tunnel used
         by LDP in LDP over RSVP associated with egress label is used as the
         class-based-forwarding default."
    ::= { vLdpNgAddrActiveFecOutLblEntry 10 }

vRtrLdpNgBfdOnLspPfxListTabLastC OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListTabLastC indicates the elapsed
         time (since system startup) of the most recent change to
         vRtrLdpNgBfdOnLspPfxListTable.  If there has been no change to
         vRtrLdpNgBfdOnLspPfxListTable since system startup, 0 is returned."
    ::= { tmnxLdpNgObjs 60 }

vRtrLdpNgBfdOnLspPfxListTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgBfdOnLspPfxListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgBfdOnLspPfxListTable contains configuration information for
         Bidirectional Forwarding Detection (BFD) on LDP LSPs."
    REFERENCE
        "RFC 5884, 'Bidirectional Forwarding Detection (BFD) for MPLS Label
         Switched Paths (LSPs)', June 2010."
    ::= { tmnxLdpNgObjs 61 }

vRtrLdpNgBfdOnLspPfxListEntry    OBJECT-TYPE
    SYNTAX      VRtrLdpNgBfdOnLspPfxListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgBfdOnLspPfxListEntry contains configuration information for
         BFD on LDP LSPs, as configured against a virtual router identifier and
         a router policy prefix list.

         Rows are created and destroyed using vRtrLdpNgBfdOnLspPfxListRowStat.
         At most 16 rows are supported per virtual router identifier."
    INDEX       {
        vRtrID,
        vRtrLdpNgBfdOnLspPfxListName
    }
    ::= { vRtrLdpNgBfdOnLspPfxListTable 1 }

VRtrLdpNgBfdOnLspPfxListEntry    ::= SEQUENCE
{
    vRtrLdpNgBfdOnLspPfxListName     TNamedItem,
    vRtrLdpNgBfdOnLspPfxListRowStat  RowStatus,
    vRtrLdpNgBfdOnLspPfxListLastChgd TimeStamp,
    vRtrLdpNgBfdOnLspPfxListTmplName TNamedItemOrEmpty,
    vRtrLdpNgBfdOnLspPfxListEnable   TruthValue,
    vRtrLdpNgBfdOnLspPfxListPingIntv Unsigned32,
    vRtrLdpNgBfdOnLspPfxListSrcAddrT InetAddressType,
    vRtrLdpNgBfdOnLspPfxListSrcAddr  InetAddress,
    vRtrLdpNgBfdOnLspPfxListFailAct  INTEGER,
    vRtrLdpNgBfdOnLspPfxListPriority Unsigned32
}

vRtrLdpNgBfdOnLspPfxListName     OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListName specifies the prefix list
         name index of the row.

         The prefix list name should match a router policy prefix list name
         created using TIMETRA-ROUTE-POLICY-MIB::tRPOperPfxListNameRowStatus.

         When this prefix list name does not match a router policy prefix list
         name, this row is ignored."
    ::= { vRtrLdpNgBfdOnLspPfxListEntry 1 }

vRtrLdpNgBfdOnLspPfxListRowStat  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListRowStat specifies the status of
         this row."
    ::= { vRtrLdpNgBfdOnLspPfxListEntry 2 }

vRtrLdpNgBfdOnLspPfxListLastChgd OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListLastChgd indicates the elapsed
         time (since system startup) of the most recent change to this row.  If
         there has been no change to this row since system startup, 0 is
         returned."
    ::= { vRtrLdpNgBfdOnLspPfxListEntry 3 }

vRtrLdpNgBfdOnLspPfxListTmplName OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListTmplName specifies the BFD
         template to be used by BFD sessions configured using this row.  The
         template name must match a template name created using
         TIMETRA-BFD-MIB::tmnxBfdOperTemplateRowStatus."
    DEFVAL      { "" }
    ::= { vRtrLdpNgBfdOnLspPfxListEntry 4 }

vRtrLdpNgBfdOnLspPfxListEnable   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListEnable specifies whether or not
         to enable BFD sessions configured using this row."
    DEFVAL      { false }
    ::= { vRtrLdpNgBfdOnLspPfxListEntry 5 }

vRtrLdpNgBfdOnLspPfxListPingIntv OBJECT-TYPE
    SYNTAX      Unsigned32 (0 | 60..300)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListPingIntv specifies the transmit
         interval of LSP ping packets used for periodic verification.  When this
         object is set to zero, transmission is disabled."
    DEFVAL      { 60 }
    ::= { vRtrLdpNgBfdOnLspPfxListEntry 6 }

vRtrLdpNgBfdOnLspPfxListSrcAddrT OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListSrcAddrT specifies the address
         type of vRtrLdpNgBfdOnLspPfxListSrcAddr."
    DEFVAL      { unknown }
    ::= { vRtrLdpNgBfdOnLspPfxListEntry 7 }

vRtrLdpNgBfdOnLspPfxListSrcAddr  OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListSrcAddr specifies the source
         address to be used in LSP ping packets and BFD control packets
         transmitted for BFD sessions configured using this row.

         When vRtrLdpNgBfdOnLspPfxListSrcAddrT and
         vRtrLdpNgBfdOnLspPfxListSrcAddr are default, the system IP address is
         transmitted."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgBfdOnLspPfxListEntry 8 }

vRtrLdpNgBfdOnLspPfxListFailAct  OBJECT-TYPE
    SYNTAX      INTEGER {
        none (0),
        down (1)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListFailAct specifies the action to
         be taken when a BFD session configured using this row fails.

         When vRtrLdpNgBfdOnLspPfxListFailAct is set to 'down(1)', a BFD
         session failure marks its LSP as no longer available as a transport
         for user traffic."
    DEFVAL      { none }
    ::= { vRtrLdpNgBfdOnLspPfxListEntry 9 }

vRtrLdpNgBfdOnLspPfxListPriority OBJECT-TYPE
    SYNTAX      Unsigned32 (1..99)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPfxListPriority specifies the priority of
         the prefix list specified by the indices.  The priority is used when
         searching the set of configured prefix lists for a prefix.  For
         example, a prefix list with priority 1 is searched before a prefix list
         with priority 2."
    DEFVAL      { 1 }
    ::= { vRtrLdpNgBfdOnLspPfxListEntry 10 }

vRtrLdpNgP2MPFecStitchTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgP2MPFecStitchEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgP2MPFecStitchTable is a read-only table that represents
         the stitch relationship of a lower FEC and its upper FECs"
    ::= { tmnxLdpNgObjs 62 }

vRtrLdpNgP2MPFecStitchEntry      OBJECT-TYPE
    SYNTAX      VRtrLdpNgP2MPFecStitchEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents either the lower P2MP FEC if it is stitched,
         or the stitched upper P2MP FEC."
    INDEX       {
        vRtrID,
        vRtrLdpNgExtP2MPFecRootAddrType,
        vRtrLdpNgExtP2MPFecRootAddress,
        vRtrLdpNgExtP2MPFecOpaqueType,
        vRtrLdpNgExtP2MPFecOpaqueLength,
        vRtrLdpNgExtP2MPFecOpaqueValue,
        vRtrLdpNgP2MPFecStitchType
    }
    ::= { vRtrLdpNgP2MPFecStitchTable 1 }

VRtrLdpNgP2MPFecStitchEntry      ::= SEQUENCE
{
    vRtrLdpNgP2MPFecStitchType       INTEGER,
    vRtrLdpNgP2MPStitchRootAddrType  InetAddressType,
    vRtrLdpNgP2MPStitchRootAddress   InetAddress,
    vRtrLdpNgP2MPFecStitchOpaqueTyp  Unsigned32,
    vRtrLdpNgP2MPFecStitchOpaqueLen  Unsigned32,
    vRtrLdpNgP2MPFecStitchOpaqueVal  OCTET STRING
}

vRtrLdpNgP2MPFecStitchType       OBJECT-TYPE
    SYNTAX      INTEGER {
        lowerFec     (1),
        primUpperFec (2),
        mbbUpperFec  (3),
        bkpUpperFec  (4)
    }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgP2MPFecStitchType indicates the stitching
         relationship between the lower and upper FEC."
    ::= { vRtrLdpNgP2MPFecStitchEntry 1 }

vRtrLdpNgP2MPStitchRootAddrType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgP2MPStitchRootAddrType indicates the type of ip
         address of the root for the P2MP FEC."
    ::= { vRtrLdpNgP2MPFecStitchEntry 2 }

vRtrLdpNgP2MPStitchRootAddress   OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgP2MPStitchRootAddress indicates the ip address
         of the root for the P2MP FEC."
    ::= { vRtrLdpNgP2MPFecStitchEntry 3 }

vRtrLdpNgP2MPFecStitchOpaqueTyp  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgP2MPFecStitchOpaqueTyp indicates the type of a
         Multi-Point Opaque Value Element."
    ::= { vRtrLdpNgP2MPFecStitchEntry 4 }

vRtrLdpNgP2MPFecStitchOpaqueLen  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgP2MPFecStitchOpaqueLen indicates the length of a
         Multi-Point Opaque Value Element."
    ::= { vRtrLdpNgP2MPFecStitchEntry 5 }

vRtrLdpNgP2MPFecStitchOpaqueVal  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..74))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgP2MPFecStitchOpaqueVal indicates the value of a
         Multi-Point Opaque Value Element."
    ::= { vRtrLdpNgP2MPFecStitchEntry 6 }

vRtrLdpNgBfdOnLspPrefixTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgBfdOnLspPrefixEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgBfdOnLspPrefixTable contains operational information for IP
         prefixes used with Bidirectional Forwarding Detection (BFD) on LDP
         LSPs."
    REFERENCE
        "RFC 5884, 'Bidirectional Forwarding Detection (BFD) for MPLS Label
         Switched Paths (LSPs)', June 2010."
    ::= { tmnxLdpNgObjs 63 }

vRtrLdpNgBfdOnLspPrefixEntry     OBJECT-TYPE
    SYNTAX      VRtrLdpNgBfdOnLspPrefixEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgBfdOnLspPrefixEntry contains operational information for an
         IP prefix used with BFD on LDP LSPs.

         A row is created/destroyed by the system when a prefix becomes
         available/unavailable for use with BFD on an LDP LSP."
    INDEX       {
        vRtrID,
        vRtrLdpNgBfdOnLspPfxListName,
        vRtrLdpNgBfdOnLspPrefixType,
        vRtrLdpNgBfdOnLspPrefix,
        vRtrLdpNgBfdOnLspPrefixLen
    }
    ::= { vRtrLdpNgBfdOnLspPrefixTable 1 }

VRtrLdpNgBfdOnLspPrefixEntry     ::= SEQUENCE
{
    vRtrLdpNgBfdOnLspPrefixType      TmnxAddressAndPrefixType,
    vRtrLdpNgBfdOnLspPrefix          TmnxAddressAndPrefixAddress,
    vRtrLdpNgBfdOnLspPrefixLen       TmnxAddressAndPrefixPrefix,
    vRtrLdpNgBfdOnLspPrefixOperState INTEGER
}

vRtrLdpNgBfdOnLspPrefixType      OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPrefixType specifies the address type of
         vRtrLdpNgBfdOnLspPrefix."
    ::= { vRtrLdpNgBfdOnLspPrefixEntry 1 }

vRtrLdpNgBfdOnLspPrefix          OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPrefix (in conjunction with
         vRtrLdpNgBfdOnLspPrefixType and vRtrLdpNgBfdOnLspPrefixLen) specifies
         the IP prefix to be read."
    ::= { vRtrLdpNgBfdOnLspPrefixEntry 2 }

vRtrLdpNgBfdOnLspPrefixLen       OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixPrefix (0..128)
    UNITS       "bits"
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPrefixLen specifies the number of
         significant bits in vRtrLdpNgBfdOnLspPrefix."
    ::= { vRtrLdpNgBfdOnLspPrefixEntry 3 }

vRtrLdpNgBfdOnLspPrefixOperState OBJECT-TYPE
    SYNTAX      INTEGER {
        invalid         (0),
        noMatch         (1),
        disabled        (2),
        srcAddrMissing  (3),
        srcAddrMismatch (4),
        up              (5),
        down            (6),
        downTrapOnly    (7),
        srcDstAddrSame  (8)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgBfdOnLspPrefixOperState indicates the
         operational state of the prefix for use by BFD on LDP LSPs.

         Code points:
         invalid         - Invalid state (unexpected).
         noMatch         - The prefix has not been matched to a prefix list.
         disabled        - The LSP BFD configuration is not enabled, or there
                           is no tunnel for the prefix.
         srcAddrMissing  - There is no LDP LSRID for the address family.
         srcAddrMismatch - The address family of the prefix doesn't match the
                           address family of the source address configured in
                           the matched LSP-BFD prefix list.
         up              - LSP BFD is operationally up for the prefix.
         down            - LSP BFD is operationally down for the prefix, and the
                           configured failure-action (i.e.
                           vRtrLdpNgBfdOnLspPfxListFailAct) is 'down(1)'.
         downTrapOnly    - LSP BFD is operationally down for the prefix, and the
                           configured failure-action (i.e.
                           vRtrLdpNgBfdOnLspPfxListFailAct) is 'none(0)'.
         srcDstAddrSame  - The address of the prefix is the same as the source
                           address."
    ::= { vRtrLdpNgBfdOnLspPrefixEntry 4 }

vRtrLdpNgTargPeerMcTuLspTblLstCh OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerMcTuLspTblLstCh indicates the last
         timestamp when an entry in the vRtrLdpNgTargPeerMcTunnLspTable was
         last changed."
    ::= { tmnxLdpNgObjs 64 }

vRtrLdpNgTargPeerMcTunnLspTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgTargPeerMcTunnLspEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The vRtrLdpNgTargPeerMcTunnLspTable keeps the list of LDP-over-RSVP
         LSP ids which are used for the tunneling of multicast FECs.

         Each LSP ID in the list corresponds to the vRtrMplsLspIndex of the
         given MPLS LSP."
    ::= { tmnxLdpNgObjs 65 }

vRtrLdpNgTargPeerMcTunnLspEntry  OBJECT-TYPE
    SYNTAX      VRtrLdpNgTargPeerMcTunnLspEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table contains the LSP id information about an LDP
         interface or targeted peer.

         Row entry can be only created if there is corresponding targeted peer
         entry in vRtrLdpNgTargPeerTable.

         Row entries can be created or deleted via SNMP SET requests. A row is
         created by setting vRtrLdpNgTargPeerMcTunLspRowStat to 'createAndGo'
         provided the corresponding LSP id exists as an MPLS lsp. A row entry
         can be destroyed by setting vRtrLdpNgTargPeerMcTunLspRowStat to
         'destroy'."
    INDEX       {
        vRtrID,
        vRtrLdpNgPeerAddressType,
        vRtrLdpNgPeerAddress,
        vRtrLdpNgTargPeerMcTunnlLspId
    }
    ::= { vRtrLdpNgTargPeerMcTunnLspTable 1 }

VRtrLdpNgTargPeerMcTunnLspEntry  ::= SEQUENCE
{
    vRtrLdpNgTargPeerMcTunnlLspId    TmnxVRtrMplsLspID,
    vRtrLdpNgTargPeerMcTunLspRowStat RowStatus
}

vRtrLdpNgTargPeerMcTunnlLspId    OBJECT-TYPE
    SYNTAX      TmnxVRtrMplsLspID (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTargPeerMcTunnlLspId specifies the LSP id of the
         LSP associated with the specified interface or targeted peer."
    ::= { vRtrLdpNgTargPeerMcTunnLspEntry 1 }

vRtrLdpNgTargPeerMcTunLspRowStat OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgTargPeerMcTunLspRowStat is used to create, delete or control
         entries in the vRtrLdpNgTargPeerMcTunnLspTable.

         An entry is created by setting vRtrLdpNgTargPeerMcTunLspRowStat to
         'createAndGo'.

         An entry is deleted by setting vRtrLdpNgTargPeerMcTunLspRowStat to
         'destroy'."
    ::= { vRtrLdpNgTargPeerMcTunnLspEntry 2 }

vRtrLdpNgTcpSessParamsGlTblLstCh OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTcpSessParamsGlTblLstCh indicates the last
         timestamp when an entry in the vRtrLdpNgTcpSessParamsGlblTable was
         last changed"
    ::= { tmnxLdpNgObjs 66 }

vRtrLdpNgTcpSessParamsGlblTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF VRtrLdpNgTcpSessParamsGlblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "vRtrLdpNgTcpSessParamsGlblTable is used to configure global TCP
         parameters to be used by all peers.

         Use of AUGMENTS clause implies a one-to-one dependent
         relationship between the base table, vRtrLdpNgGeneralTable,
         and the augmenting table, vRtrLdpNgTcpSessParamsGlblTable. This in
         effect extends the vRtrLdpNgGeneralTable with additional
         columns.  Creation or deletion of a row in the
         vRtrLdpNgGeneralTable results in the same fate for the row
         in the vRtrLdpNgTcpSessParamsGlblTable."
    ::= { tmnxLdpNgObjs 67 }

vRtrLdpNgTcpSessParamsGlblEntry  OBJECT-TYPE
    SYNTAX      VRtrLdpNgTcpSessParamsGlblEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table represents the configuration of global TCP peer
         parameters."
    AUGMENTS    { vRtrLdpNgGeneralEntry }
    ::= { vRtrLdpNgTcpSessParamsGlblTable 1 }

VRtrLdpNgTcpSessParamsGlblEntry  ::= SEQUENCE
{
    vRtrLdpNgTcpSessParamsGlblKeyChn TNamedItemOrEmpty,
    vRtrLdpNgTcpSessParmGlblAuthType INTEGER,
    vRtrLdpNgTcpSessParmGlblAuthKey  OCTET STRING
}

vRtrLdpNgTcpSessParamsGlblKeyChn OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of vRtrLdpNgTcpSessParamsGlblKeyChn specifies the keychain
         which will be used to sign and/or authenticate TCP transport session
         of the LDP protocol stream.

         The keychain name is defined by tmnxKeyChainName and is the index for
         TIMETRA-SECURITY-MIB::tmnxKeyChainTable"
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTcpSessParamsGlblEntry 1 }

vRtrLdpNgTcpSessParmGlblAuthType OBJECT-TYPE
    SYNTAX      INTEGER {
        none (1),
        md5  (2)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When the value of vRtrLdpNgTcpSessParmGlblAuthType is 'none', no
         authentication is used.

         When the value of this object is 'md5', authentication using MD5
         message based digest protocol is enabled."
    DEFVAL      { none }
    ::= { vRtrLdpNgTcpSessParamsGlblEntry 2 }

vRtrLdpNgTcpSessParmGlblAuthKey  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..255))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The string specified in vRtrLdpNgTcpSessParmGlblAuthKey is the authentication
         key to be used between two LDP neighbors before establishing TCP
         transport session of the LDP protocol stream.  Authentication is done
         using the MD-5 message based digest protocol.  Note that the string may
         NOT contain embedded nulls.

         An SNMP Get request on this object should return an OCTET STRING of
         length 0."
    DEFVAL      { ''H }
    ::= { vRtrLdpNgTcpSessParamsGlblEntry 3 }

tmnxLdpNgConformance             OBJECT IDENTIFIER ::= { tmnxSRConfs 91 }

tmnxLdpNgCompliances             OBJECT IDENTIFIER ::= { tmnxLdpNgConformance 1 }

tmnxLdpNgV12v0Compliance         MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of extended LDP on Nokia SROS
         series systems 12.0 release."
    MODULE
        MANDATORY-GROUPS {
            tmnxLdpNgIfV12v0Group,
            tmnxLdpNgAdjV12v0Group,
            tmnxLdpNgSessionV12v0Group,
            tmnxLdpNgPeerParamsV12v0Group,
            tmnxLdpNgAddrFecV12v0Group,
            tmnxLdpNgP2MPFecV12v0Group,
            tmnxLdpNgServFecV12v0Group,
            tmnxLdpNgFec129V12v0Group,
            tmnxLdpNgCepTdmFecV12v0Group,
            tmnxLdpNgStaticFecV12v0Group,
            tmnxLdpNgSessionStatsV12v0Group,
            tmnxLdpNgTargPeerV12v0Group,
            tmnxLdpNgInetIfV12v0Group,
            tmnxLdpNgStatsV12v0Group,
            tmnxLdpNgCapabilityV12v0Group,
            tmnxLdpNgTcpSessParamsV12v0Group,
            tmnxLdpNgGeneralV12v0Group,
            tmnxLdpNgPolicyV12v0Group,
            tmnxLdpNgIfParamsV12v0Group,
            tmnxLdpNgTargetedPeerV12v0Group,
            tmnxLdpNgAggrPreMatchV12v0Group
        }
    ::= { tmnxLdpNgCompliances 1 }

tmnxLdpNgV13v0Compliance         MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of extended LDP on Nokia SROS
         series systems 13.0 release."
    MODULE
        MANDATORY-GROUPS {
            tmnxLdpNgIfV12v0Group,
            tmnxLdpNgAdjV12v0Group,
            tmnxLdpNgSessionV12v0Group,
            tmnxLdpNgPeerParamsV12v0Group,
            tmnxLdpNgAddrFecV12v0Group,
            tmnxLdpNgP2MPFecV12v0Group,
            tmnxLdpNgServFecV12v0Group,
            tmnxLdpNgFec129V12v0Group,
            tmnxLdpNgCepTdmFecV12v0Group,
            tmnxLdpNgStaticFecV12v0Group,
            tmnxLdpNgSessionStatsV12v0Group,
            tmnxLdpNgTargPeerV12v0Group,
            tmnxLdpNgInetIfV12v0Group,
            tmnxLdpNgStatsV12v0Group,
            tmnxLdpNgCapabilityV12v0Group,
            tmnxLdpNgTcpSessParamsV12v0Group,
            tmnxLdpNgGeneralV12v0Group,
            tmnxLdpNgPolicyV12v0Group,
            tmnxLdpNgIfParamsV12v0Group,
            tmnxLdpNgTargetedPeerV12v0Group,
            tmnxLdpNgAggrPreMatchV12v0Group,
            tmnxLdpNgFecLimPerPeerV13v0Group,
            tmnxLdpNgNotificationGroup,
            tmnxLdpNgSessParamPeerV13v0Group,
            tmnxLdpNgTcpSessParamsV13v0Group,
            tmnxLdpNgNotifyObjs,
            tmnxLdpNgHelloAdjV13v0Group,
            tmnxLdpNgTargPeerV13v0Group,
            tmnxLdpNgInetIfV13v0Group,
            tmnxLdpNgAddrActiveFecV13v0Group,
            tmnxLdpNgGeneralV13v0Group,
            tmnxLdpNgRecvFecCapV13v0Group
        }
    ::= { tmnxLdpNgCompliances 2 }

tmnxLdpNgV14v0Compliance         MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of extended LDP on Nokia SROS
         series systems 14.0 release."
    MODULE
        MANDATORY-GROUPS {
            tmnxLdpNgGeneralEliV14v0Group,
            tmnxLdpNgIfV14v0Group,
            tmnxLdpNgTargPeerV14v0Group,
            tmnxLdpNgGeneralFrrV14v0Group,
            tmnxLdpNgSessV14v0Group,
            tmnxLdpNgLegacyInteropGrp
        }
    ::= { tmnxLdpNgCompliances 3 }

tmnxLdpNgV15v0Compliance         MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of extended LDP on Nokia SROS
         series systems release 15.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxLdpNgBfdOnLspGroup,
            tmnxLdpNgNonRecFecGroup,
            tmnxLdpNgIpV632BitLsridGroup,
            tmnxLdpNgSessParamAdvertGroup,
            tmnxLdpNgSessParamCommunityGroup,
            tmnxLdpNgMcastUpstrmAsbrFrrGroup
        }
    ::= { tmnxLdpNgCompliances 4 }

tmnxLdpNgV16v0Compliance         MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of extended LDP on Nokia SROS
         series systems release 16.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxLdpNgResolveRootUsingGroup,
            tmnxLdpNgWeightedEcmpGroup,
            tmnxLdpNgSysIpFecPolicyGroup,
            tmnxLdpNgPolicyV16v0Group,
            tmnxLdpNgCBFV16v0Group
        }
    ::= { tmnxLdpNgCompliances 5 }

tmnxLdpNgV19v0Compliance         MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of extended LDP on Nokia SROS
         series systems release 19.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxLdpNgImportPmsiRoutesGroup,
            tmnxLdpNgPolicyV19v0Group,
            tmnxLdpNgIntfWeightedEcmpGroup,
            tmnxLdpNgEcmpGroup
        }
    ::= { tmnxLdpNgCompliances 6 }

tmnxLdpNgV20v0Compliance         MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of extended LDP on Nokia SROS
         series systems release 20.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxLdpNgAddrFecStitchPrefGroup,
            tmnxLdpNgMldpOverRsvpV20v0Group,
            tmnxLdpNgTargPeerV20v0Group,
            tmnxLdpNgPeerParamsV20v0Group,
            tmnxLdpTargAutoTldpV20v0Group
        }
    ::= { tmnxLdpNgCompliances 7 }

tmnxLdpNgV21v0Compliance         MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of extended LDP on Nokia SROS
         series systems release 21.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxLdpNgTcpSeParGlblV21v0Group,
            tmnxLdpNgAddrFecTunlPrefGroup,
            tmnxLdpNgPreferTransFrrGroup
        }
    ::= { tmnxLdpNgCompliances 8 }

tmnxLdpNgV22v0Compliance         MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of extended LDP on Nokia SROS
         series systems release 22.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxLdpTargResV6PfxOvrIgpShGroup
        }
    ::= { tmnxLdpNgCompliances 9 }

tmnxLdpNgV24v0Compliance         MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of extended LDP on Nokia SROS
         series systems release 24.0."
    MODULE
        MANDATORY-GROUPS {
            tmnxLdpNgSessionGRGroup
        }
    ::= { tmnxLdpNgCompliances 10 }

tmnxLdpNgGroups                  OBJECT IDENTIFIER ::= { tmnxLdpNgConformance 2 }

tmnxLdpNgIfV12v0Group            OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgIfTableLstChanged,
        vRtrLdpNgIfRowStatus,
        vRtrLdpNgIfLastChange,
        vRtrLdpNgIfAdminState,
        vRtrLdpNgIfOperState,
        vRtrLdpNgIfOperDownReason,
        vRtrLdpNgIfBfdEnabled,
        vRtrLdpNgInetIfStatsExistingAdj
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of extended LDP
         interfaces on Nokia SROS series systems 12.0 release."
    ::= { tmnxLdpNgGroups 1 }

tmnxLdpNgAdjV12v0Group           OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgHelloAdjLclLdpIdType,
        vRtrLdpNgHelloAdjLclLdpId,
        vRtrLdpNgHelloAdjEntityIndex,
        vRtrLdpNgHelloAdjIndex,
        vRtrLdpNgHelloAdjHoldTimeRem,
        vRtrLdpNgHelloAdjType,
        vRtrLdpNgHelloAdjRemConfSeqNum,
        vRtrLdpNgHelloAdjRemIpAddrType,
        vRtrLdpNgHelloAdjRemIpAddress,
        vRtrLdpNgHelloAdjUpTime,
        vRtrLdpNgHelloAdjLclConfSeqNum,
        vRtrLdpNgHelloAdjLclIpAddrType,
        vRtrLdpNgHelloAdjLclIpAddress,
        vRtrLdpNgHelloAdjInHelloMsgCnt,
        vRtrLdpNgHelloAdjOutHelloMsgCnt,
        vRtrLdpNgHelloAdjLclTimeout,
        vRtrLdpNgHelloAdjRemTimeout,
        vRtrLdpNgHelloAdjBfdStatus,
        vRtrLdpNgHelloAdjMapIndex
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP Adjacencies
         for LDP sessions on Nokia SROS series systems 12.0 Release."
    ::= { tmnxLdpNgGroups 2 }

tmnxLdpNgSessionV12v0Group       OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgSessLocalLdpIdType,
        vRtrLdpNgSessLocalLdpId,
        vRtrLdpNgSessEntityIndex,
        vRtrLdpNgSessLabelDistMethod,
        vRtrLdpNgSessLoopDetectForPV,
        vRtrLdpNgSessPathVectorLimit,
        vRtrLdpNgSessState,
        vRtrLdpNgSessAdjacencyType,
        vRtrLdpNgSessProtocolVersion,
        vRtrLdpNgSessLocalUdpPort,
        vRtrLdpNgSessPeerUdpPort,
        vRtrLdpNgSessLocalTcpPort,
        vRtrLdpNgSessPeerTcpPort,
        vRtrLdpNgSessLocalAddrType,
        vRtrLdpNgSessLocalAddress,
        vRtrLdpNgSessPeerAddrType,
        vRtrLdpNgSessPeerAddress,
        vRtrLdpNgSessKAHoldTimeRemaining,
        vRtrLdpNgSessMaxPduLength,
        vRtrLdpNgSessUpTime,
        vRtrLdpNgSessLocalKATimeout,
        vRtrLdpNgSessPeerKATimeout,
        vRtrLdpNgSessAdvertise,
        vRtrLdpNgSessLclGRHelperState,
        vRtrLdpNgSessPeerGRState,
        vRtrLdpNgSessPeerNumRestart,
        vRtrLdpNgSessLastRestartTime,
        vRtrLdpNgSessLocalFtReconTime,
        vRtrLdpNgSessPeerFtReconTime,
        vRtrLdpNgSessLocalFtRecovTime,
        vRtrLdpNgSessPeerFtRecovTime,
        vRtrLdpNgSessFtReconTimeRem,
        vRtrLdpNgSessFtRecovTimeRem,
        vRtrLdpNgSessBfdStatus,
        vRtrLdpNgSessLocalP2MPCap,
        vRtrLdpNgSessPeerP2MPCap,
        vRtrLdpNgSessLocalMPMBBCap,
        vRtrLdpNgSessPeerMPMBBCap,
        vRtrLdpNgSessLocalDynCap,
        vRtrLdpNgSessPeerDynCap,
        vRtrLdpNgSessLocalOLoadCap,
        vRtrLdpNgSessPeerOLoadCap,
        vRtrLdpNgSessIPv4PfxFecOLoadSent,
        vRtrLdpNgSessIPv6PfxFecOLoadSent,
        vRtrLdpNgSessIPv4PfxFecOLoadRecv,
        vRtrLdpNgSessIPv6PfxFecOLoadRecv,
        vRtrLdpNgSessIPv4P2MPFecOLSent,
        vRtrLdpNgSessIPv6P2MPFecOLSent,
        vRtrLdpNgSessIPv4P2MPFecOLRecv,
        vRtrLdpNgSessIPv6P2MPFecOLRecv,
        vRtrLdpNgSessSvcFec128OLoadSent,
        vRtrLdpNgSessSvcFec128OLoadRecv,
        vRtrLdpNgSessSvcFec129OLoadSent,
        vRtrLdpNgSessSvcFec129OLoadRecv,
        vRtrLdpNgSessLocalIPv4PfxFecCap,
        vRtrLdpNgSessPeerIPv4PfxFecCap,
        vRtrLdpNgSessLocalIPv6PfxFecCap,
        vRtrLdpNgSessPeerIPv6PfxFecCap,
        vRtrLdpNgSessLocalSvcFec128Cap,
        vRtrLdpNgSessPeerSvcFec128Cap,
        vRtrLdpNgSessLocalSvcFec129Cap,
        vRtrLdpNgSessPeerSvcFec129Cap
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP Sessions on
         Nokia SROS series systems 12.0 Release."
    ::= { tmnxLdpNgGroups 3 }

tmnxLdpNgSessionStatsV12v0Group  OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgSessStatsTargAdj,
        vRtrLdpNgSessStatsLinkAdj,
        vRtrLdpNgSessStatsHelloIn,
        vRtrLdpNgSessStatsHelloOut,
        vRtrLdpNgSessStatsKeepaliveIn,
        vRtrLdpNgSessStatsKeepaliveOut,
        vRtrLdpNgSessStatsInitIn,
        vRtrLdpNgSessStatsInitOut,
        vRtrLdpNgSessStatsLblMappingIn,
        vRtrLdpNgSessStatsLblMappingOut,
        vRtrLdpNgSessStatsLblRequestIn,
        vRtrLdpNgSessStatsLblRequestOut,
        vRtrLdpNgSessStatsLblReleaseIn,
        vRtrLdpNgSessStatsLblReleaseOut,
        vRtrLdpNgSessStatsLblWithdrawIn,
        vRtrLdpNgSessStatsLblWithdrawOut,
        vRtrLdpNgSessStatsLblAbortIn,
        vRtrLdpNgSessStatsLblAbortOut,
        vRtrLdpNgSessStatsAddrIn,
        vRtrLdpNgSessStatsAddrOut,
        vRtrLdpNgSessStatsAddrWithdrIn,
        vRtrLdpNgSessStatsAddrWithdrOut,
        vRtrLdpNgSessStatsNotifIn,
        vRtrLdpNgSessStatsNotifOut,
        vRtrLdpNgSessStatsIPv4PfxFecRcv,
        vRtrLdpNgSessStatsIPv6PfxFecRcv,
        vRtrLdpNgSessStatsIPv4PfxFecSnt,
        vRtrLdpNgSessStatsIPv6PfxFecSnt,
        vRtrLdpNgSessStatsIPv4P2MPFecRcv,
        vRtrLdpNgSessStatsIPv6P2MPFecRcv,
        vRtrLdpNgSessStatsIPv4P2MPFecSnt,
        vRtrLdpNgSessStatsIPv6P2MPFecSnt,
        vRtrLdpNgSessStatsSvcFec128Recv,
        vRtrLdpNgSessStatsSvcFec128Sent,
        vRtrLdpNgSessStatsSvcFec129Recv,
        vRtrLdpNgSessStatsSvcFec129Sent,
        vRtrLdpNgSessStatsIPv4AddrRecv,
        vRtrLdpNgSessStatsIPv6AddrRecv,
        vRtrLdpNgSessStatsIPv4AddrSent,
        vRtrLdpNgSessStatsIPv6AddrSent,
        vRtrLdpNgSessStatsCapabilityIn,
        vRtrLdpNgSessStatsCapabilityOut
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP Session
         statistics on Nokia SROS series systems 12.0 Release."
    ::= { tmnxLdpNgGroups 4 }

tmnxLdpNgPeerParamsV12v0Group    OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargPeerLspRowStatus,
        vRtrLdpNgSessParamRowStatus,
        vRtrLdpNgSessParamDODLblDistrib,
        vRtrLdpNgSessParamImportPolicy1,
        vRtrLdpNgSessParamImportPolicy2,
        vRtrLdpNgSessParamImportPolicy3,
        vRtrLdpNgSessParamImportPolicy4,
        vRtrLdpNgSessParamImportPolicy5,
        vRtrLdpNgSessParamExportPolicy1,
        vRtrLdpNgSessParamExportPolicy2,
        vRtrLdpNgSessParamExportPolicy3,
        vRtrLdpNgSessParamExportPolicy4,
        vRtrLdpNgSessParamExportPolicy5,
        vRtrLdpNgSessFec129CiscoInterop,
        vRtrLdpNgSessParamAdvAdjAddrOnly,
        vRtrLdpNgSessAddrLclLdpIdType,
        vRtrLdpNgSessionAddrLocalLdpId,
        vRtrLdpNgSessionAddrNumInAddrs,
        vRtrLdpNgSessionAddrNumOutAddrs,
        vRtrLdpNgSessInAddrLclLdpIdType,
        vRtrLdpNgSessionInAddrLocalLdpId,
        vRtrLdpNgSessOutAddrLclLdpIdType,
        vRtrLdpNgSessionOutAddrLclLdpId,
        vRtrLdpNgTargPeerTunlLspTblLstCh,
        vRtrLdpNgSessionParamsTableLstCh,
        vRtrLdpNgSessPeIDMacFlushInterop,
        vRtrLdpNgSessParamIPv4PfxFecCap,
        vRtrLdpNgSessParamIPv6PfxFecCap,
        vRtrLdpNgSessParamP2MPFecCap
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP interfaces
         and targeted peers on Nokia SROS series systems 12.0 release."
    ::= { tmnxLdpNgGroups 5 }

tmnxLdpNgAddrFecV12v0Group       OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgAddrFecFlags,
        vRtrLdpNgAddrFecNumInLabels,
        vRtrLdpNgAddrFecNumOutLabels,
        vRtrLdpNgAddrFecInLbl,
        vRtrLdpNgAddrFecInLblStatus,
        vRtrLdpNgAddrFecInLblIfIndex,
        vRtrLdpNgAddrFecOutLbl,
        vRtrLdpNgAddrFecOutLblStatus,
        vRtrLdpNgAddrFecOutLblIfIndex,
        vRtrLdpNgAddrFecOutLblNHType,
        vRtrLdpNgAddrFecOutLblNHAddr,
        vRtrLdpNgAddrFecOutLblMetric,
        vRtrLdpNgAddrFecOutLblMtu,
        vRtrLdpNgAddrFecOutLblLspId,
        vRtrLdpNgAddrFecMapFlags,
        vRtrLdpNgAddrFecMapNumInLabels,
        vRtrLdpNgAddrFecMapNumOutLabels
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting Address FECs on Nokia SROS series
         systems 12.0 Release."
    ::= { tmnxLdpNgGroups 6 }

tmnxLdpNgP2MPFecV12v0Group       OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgExtP2MPFecFlags,
        vRtrLdpNgExtP2MPFecNumInLabels,
        vRtrLdpNgExtP2MPFecNumOutLabels,
        vRtrLdpNgExtP2MPFecTunnelIfId,
        vRtrLdpNgExtP2MPFecMetric,
        vRtrLdpNgExtP2MPFecMTU,
        vRtrLdpNgExtP2MPFecInLbl,
        vRtrLdpNgExtP2MPFecInLblStatus,
        vRtrLdpNgExtP2MPFecOutLbl,
        vRtrLdpNgExtP2MPFecOutLblStatus,
        vRtrLdpNgExtP2MPFecOutLblNHType,
        vRtrLdpNgExtP2MPFecOutLblNHAdr,
        vRtrLdpNgExtP2MPFecOutLblIfIndex,
        vRtrLdpNgExtP2MPFecOutLblLspId,
        vRtrLdpNgExtP2MPFecMapFlags,
        vRtrLdpNgExtP2MPFecMapNumInLbls,
        vRtrLdpNgExtP2MPFecMapNumOutLbls,
        vRtrLdpNgExtP2MPFecMapTunnelIfId,
        vRtrLdpNgExtP2MPFecMapMetric,
        vRtrLdpNgExtP2MPFecMapMTU
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting P2MP FECs on Nokia SROS series systems
         12.0 Release."
    ::= { tmnxLdpNgGroups 7 }

tmnxLdpNgServFecV12v0Group       OBJECT-GROUP
    OBJECTS     {
        vLdpNgFec128ServType,
        vLdpNgFec128ServId,
        vLdpNgFec128VpnId,
        vLdpNgFec128Flags,
        vLdpNgFec128NumInLabels,
        vLdpNgFec128NumOutLabels,
        vLdpNgFec128SdpId,
        vLdpNgFec128MateEndptVcId,
        vLdpNgFec128MateEndptSdpId,
        vLdpNgFec128InLabel,
        vLdpNgFec128InLabelStatus,
        vLdpNgFec128InLabelSigStatus,
        vLdpNgFec128InLblWdwReason,
        vLdpNgFec128InLblMaxCellConcat,
        vLdpNgFec128InLblFLTxCap,
        vLdpNgFec128InLblFLRxCap,
        vLdpNgFec128InLblIPv4CeIpAdType,
        vLdpNgFec128InLblIPv4CeIpAddr,
        vLdpNgFec128InLblIPv4Cap,
        vLdpNgFec128InLblIPv6Cap,
        vLdpNgFec128InLblMTU,
        vLdpNgFec128InLblVlanTag,
        vLdpNgFec128InLblVccvCV,
        vLdpNgFec128InLblVccvCC,
        vLdpNgFec128InLblPwStatus,
        vLdpNgFec128OutLabel,
        vLdpNgFec128OutLabelStatus,
        vLdpNgFec128OutLabelSigStatus,
        vLdpNgFec128OutLblMaxCellConcat,
        vLdpNgFec128OutLblFLTxCap,
        vLdpNgFec128OutLblFLRxCap,
        vLdpNgFec128OutLblIPv4CeAddrType,
        vLdpNgFec128OutLblIPv4CeIpAddr,
        vLdpNgFec128OutLblIPv4Cap,
        vLdpNgFec128OutLblIPv6Cap,
        vLdpNgFec128OutLblMTU,
        vLdpNgFec128OutLblVlanTag,
        vLdpNgFec128OutLblVccvCV,
        vLdpNgFec128OutLblVccvCC,
        vLdpNgFec128OutLblPwStatus
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP service
         FECs sent to or received from an LDP peer on Nokia SROS series systems
         release 12.0."
    ::= { tmnxLdpNgGroups 8 }

tmnxLdpNgFec129V12v0Group        OBJECT-GROUP
    OBJECTS     {
        vLdpNgFec129ServType,
        vLdpNgFec129ServId,
        vLdpNgFec129VpnId,
        vLdpNgFec129Flags,
        vLdpNgFec129NumInLabels,
        vLdpNgFec129NumOutLabels,
        vLdpNgFec129SdpId,
        vLdpNgFec129MateAgiType,
        vLdpNgFec129MateAgiLen,
        vLdpNgFec129MateAgiVal,
        vLdpNgFec129MateSrcAiiType,
        vLdpNgFec129MateSrcAiiLen,
        vLdpNgFec129MateSrcAiiVal,
        vLdpNgFec129MateTgtAiiType,
        vLdpNgFec129MateTgtAiiLen,
        vLdpNgFec129MateTgtAiiVal,
        vLdpNgFec129MateSdpId,
        vLdpNgFec129InLabel,
        vLdpNgFec129InLabelStatus,
        vLdpNgFec129InLblMTU,
        vLdpNgFec129InLblVlanTag,
        vLdpNgFec129InLblMaxCellConcat,
        vLdpNgFec129InLblSigStatus,
        vLdpNgFec129InLblIPv4Cap,
        vLdpNgFec129InLblIPv6Cap,
        vLdpNgFec129InLblIPv4CeAddrType,
        vLdpNgFec129InLblIPv4CeIpAddr,
        vLdpNgFec129InLblWdwReason,
        vLdpNgFec129InLblFLTxCap,
        vLdpNgFec129InLblFLRxCap,
        vLdpNgFec129InLblVccvCV,
        vLdpNgFec129InLblVccvCC,
        vLdpNgFec129InLblPwStatus,
        vLdpNgFec129OutLabel,
        vLdpNgFec129OutLabelStatus,
        vLdpNgFec129OutLblMTU,
        vLdpNgFec129OutLblVlanTag,
        vLdpNgFec129OutLblMaxCellConcat,
        vLdpNgFec129OutLblSigStatus,
        vLdpNgFec129OutLblIPv4Cap,
        vLdpNgFec129OutLblIPv6Cap,
        vLdpNgFec129OutLblIPv4CeAddrType,
        vLdpNgFec129OutLblIPv4CeIpAddr,
        vLdpNgFec129OutLblFLTxCap,
        vLdpNgFec129OutLblFLRxCap,
        vLdpNgFec129OutLblVccvCV,
        vLdpNgFec129OutLblVccvCC,
        vLdpNgFec129OutLblPwStatus
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of LDP FEC-129s sent to or
         received from an LDP peer on Nokia SROS series systems release 12.0."
    ::= { tmnxLdpNgGroups 9 }

tmnxLdpNgCepTdmFecV12v0Group     OBJECT-GROUP
    OBJECTS     {
        vLdpNgCepTdmFec128InLblPayldSize,
        vLdpNgCepTdmFec128InLblBitrate,
        vLdpNgCepTdmFec128InLblRtpHeader,
        vLdpNgCepTdmFec128InLblDiffTStmp,
        vLdpNgCepTdmFec128InLblSigPkts,
        vLdpNgCepTdmFec128InLblCasTrunk,
        vLdpNgCepTdmFec128InLblTStmpFreq,
        vLdpNgCepTdmFec128InLblPayldType,
        vLdpNgCepTdmFec128InLblSsrcId,
        vLdpNgCepTdmFec128OutLblPyldSze,
        vLdpNgCepTdmFec128OutLblBitrate,
        vLdpNgCepTdmFec128OutLblRtpHdr,
        vLdpNgCepTdmFec128OutLblDfTstmp,
        vLdpNgCepTdmFec128OutLblSigPkts,
        vLdpNgCepTdmFec128OutLblCasTrnk,
        vLdpNgCepTdmFec128OutLblTstmpFq,
        vLdpNgCepTdmFec128OutLblPyldTyp,
        vLdpNgCepTdmFec128OutLblSsrcId,
        vLdpNgCepTdmFec129InLblPayldSize,
        vLdpNgCepTdmFec129InLblBitrate,
        vLdpNgCepTdmFec129InLblRtpHeader,
        vLdpNgCepTdmFec129InLblDiffTStmp,
        vLdpNgCepTdmFec129InLblSigPkts,
        vLdpNgCepTdmFec129InLblCasTrunk,
        vLdpNgCepTdmFec129InLblTStmpFreq,
        vLdpNgCepTdmFec129InLblPayldType,
        vLdpNgCepTdmFec129InLblSsrcId,
        vLdpNgCepTdmFec129OutLblPyldSize,
        vLdpNgCepTdmFec129OutLblBitrate,
        vLdpNgCepTdmFec129OutLblRtpHdr,
        vLdpNgCepTdmFec129OutLblDifTStmp,
        vLdpNgCepTdmFec129OutLblSigPkts,
        vLdpNgCepTdmFec129OutLblCasTrnk,
        vLdpNgCepTdmFec129OutLblTStmpFrq,
        vLdpNgCepTdmFec129OutLblPyldType,
        vLdpNgCepTdmFec129OutLblSsrcId
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP CEP/TDM
         FECs sent to or received from an LDP peer on Nokia SROS series systems
         release 12.0."
    ::= { tmnxLdpNgGroups 10 }

tmnxLdpNgStaticFecV12v0Group     OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgStaticFecTableLstCh,
        vRtrLdpNgStaticFecRowStatus,
        vRtrLdpNgStaticFecNumInLabel,
        vRtrLdpNgStaticFecNumOutLabel,
        vRtrLdpNgSFecInLabelRowStatus,
        vRtrLdpNgSFecOperInLabel,
        vRtrLdpNgSFecOutLabelRowStatus,
        vRtrLdpNgSFecOutLabel
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of LDP Static FECs on Nokia
         SROS series systems 12.0 release."
    ::= { tmnxLdpNgGroups 11 }

tmnxLdpNgTargPeerV12v0Group      OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargPeerTableLstCh,
        vRtrLdpNgTargPeerRowStatus,
        vRtrLdpNgTargPeerLastChange,
        vRtrLdpNgTargPeerAdminState,
        vRtrLdpNgTargPeerOperState,
        vRtrLdpNgTargPeerUpTime,
        vRtrLdpNgTargPeerOperDownReason,
        vRtrLdpNgTargPeerInheritance,
        vRtrLdpNgTargPeerKAFactor,
        vRtrLdpNgTargPeerKATimeout,
        vRtrLdpNgTargPeerHelloFactor,
        vRtrLdpNgTargPeerHelloTimeout,
        vRtrLdpNgTargPeerOprHelloTimeout,
        vRtrLdpNgTargPeerHelloReduction,
        vRtrLdpNgTargPeerHelloRdctnFctr,
        vRtrLdpNgTargPeerBackoffTime,
        vRtrLdpNgTargPeerMaxBackoffTime,
        vRtrLdpNgTargPeerTunneling,
        vRtrLdpNgTargPeerBfdEnabled,
        vRtrLdpNgTargPeerLsrIfIndex,
        vRtrLdpNgTargPeerAutoCreate,
        vRtrLdpNgTargPeerCreator,
        vRtrLdpNgTargPeerTemplName,
        vRtrLdpNgTargPeerStatExistingAdj
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP targeted
         peer on Nokia SROS series systems release 12.0."
    ::= { tmnxLdpNgGroups 14 }

tmnxLdpNgInetIfV12v0Group        OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgInetIfTableLstCh,
        vRtrLdpNgInetIfRowStatus,
        vRtrLdpNgInetIfUpTime,
        vRtrLdpNgInetIfLastChange,
        vRtrLdpNgInetIfAdminState,
        vRtrLdpNgInetIfOperState,
        vRtrLdpNgInetIfOperDownReason,
        vRtrLdpNgInetIfInheritance,
        vRtrLdpNgInetIfKAFactor,
        vRtrLdpNgInetIfKATimeout,
        vRtrLdpNgInetIfHelloFactor,
        vRtrLdpNgInetIfHelloTimeout,
        vRtrLdpNgInetIfOperHelloTimeout,
        vRtrLdpNgInetIfBackoffTime,
        vRtrLdpNgInetIfMaxBackoffTime,
        vRtrLdpNgInetIfTransAddrType,
        vRtrLdpNgInetIfLsrIfType,
        vRtrLdpNgInetIfLsrIfIndex,
        vRtrLdpNgInetIfIPv4P2MPFecCap,
        vRtrLdpNgInetIfIPv6P2MPFecCap,
        vRtrLdpNgInetIfIPv4PfxFecCap,
        vRtrLdpNgInetIfIPv6PfxFecCap
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP Inet family
         interfaces on Nokia SROS series systems release 12.0."
    ::= { tmnxLdpNgGroups 15 }

tmnxLdpNgStatsV12v0Group         OBJECT-GROUP
    OBJECTS     {
        vLdpNgStatsIPv4OperDownEvents,
        vLdpNgStatsIPv6OperDownEvents,
        vLdpNgStatsIPv4ActiveSess,
        vLdpNgStatsIPv6ActiveSess,
        vLdpNgStatsIPv4ActiveLinkAdj,
        vLdpNgStatsIPv6ActiveLinkAdj,
        vLdpNgStatsIPv4ActiveTargAdj,
        vLdpNgStatsIPv6ActiveTargAdj,
        vLdpNgStatsIPv4ActiveIf,
        vLdpNgStatsIPv6ActiveIf,
        vLdpNgStatsIPv4InactiveIf,
        vLdpNgStatsIPv6InactiveIf,
        vLdpNgStatsIPv4ActiveTargPeers,
        vLdpNgStatsIPv6ActiveTargPeers,
        vLdpNgStatsIPv4InactiveTargPeers,
        vLdpNgStatsIPv6InactiveTargPeers,
        vLdpNgStatsIPv4PfxFecRecv,
        vLdpNgStatsIPv6PfxFecRecv,
        vLdpNgStatsIPv4PfxFecSent,
        vLdpNgStatsIPv6PfxFecSent,
        vLdpNgStatsFec128FecSent,
        vLdpNgStatsFec128FecRecv,
        vLdpNgStatsFec129FecSent,
        vLdpNgStatsFec129FecRecv,
        vLdpNgStatsIPv4AttemptedSessions,
        vLdpNgStatsIPv6AttemptedSessions,
        vLdpNgStatsSessRejNoHelloErrs,
        vLdpNgStatsSessRejAdvErrors,
        vLdpNgStatsSessRejMaxPduErrs,
        vLdpNgStatsSessRejLblRngeErrs,
        vLdpNgStatsBadLdpIdErrors,
        vLdpNgStatsBadPduLengthErrors,
        vLdpNgStatsBadMsgLengthErrors,
        vLdpNgStatsBadTlvLengthErrors,
        vLdpNgStatsMalformedTlvErrors,
        vLdpNgStatsKeepAliveExpErrors,
        vLdpNgStatsShutdownNotifRecv,
        vLdpNgStatsShutdownNotifSent,
        vLdpNgStatsIPv4EgrFecPfxCount,
        vLdpNgStatsIPv6EgrFecPfxCount,
        vLdpNgStatsUnknownTlvErrors,
        vLdpNgStatsIPv4P2MPFecSent,
        vLdpNgStatsIPv6P2MPFecSent,
        vLdpNgStatsIPv4P2MPFecRecv,
        vLdpNgStatsIPv6P2MPFecRecv,
        vLdpNgStatsIPv4PfxFecOLSessSent,
        vLdpNgStatsIPv6PfxFecOLSessSent,
        vLdpNgStatsIPv4PfxFecOLSessRecv,
        vLdpNgStatsIPv6PfxFecOLSessRecv,
        vLdpNgStatsIPv4P2MPFecOLSessSent,
        vLdpNgStatsIPv6P2MPFecOLSessSent,
        vLdpNgStatsIPv4P2MPFecOLSessRecv,
        vLdpNgStatsIPv6P2MPFecOLSessRecv,
        vLdpNgStatsFec128FecOLSessSent,
        vLdpNgStatsFec128FecOLSessRecv,
        vLdpNgStatsFec129FecOLSessSent,
        vLdpNgStatsFec129FecOLSessRecv,
        vLdpNgStatsIPv4OLoadInterfaces,
        vLdpNgStatsIPv6OLoadInterfaces,
        vLdpNgStatsIPv4OLoadTargPeers,
        vLdpNgStatsIPv6OLoadTargPeers,
        vLdpNgStatsIPv4PfxFecInOLoad,
        vLdpNgStatsIPv6PfxFecInOLoad,
        vLdpNgStatsIPv4P2MPFecInOLoad,
        vLdpNgStatsIPv6P2MPFecInOLoad,
        vLdpNgStatsFec128FecInOLoad,
        vLdpNgStatsFec129FecInOLoad,
        vLdpNgStatsBadProtVersionErrors
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP statistics
         on Nokia SROS series systems release 12.0."
    ::= { tmnxLdpNgGroups 16 }

tmnxLdpNgCapabilityV12v0Group    OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenP2MPCapability,
        vRtrLdpNgGenMPMBBCapability,
        vRtrLdpNgGenDynamicCapability,
        vRtrLdpNgGenOverloadCapability,
        vRtrLdpNgGenFec128Capability,
        vRtrLdpNgGenFec129Capability,
        vRtrLdpNgGenIPv4PfxFecCapability,
        vRtrLdpNgGenIPv6PfxFecCapability
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP
         capabilities on Nokia SROS series systems release 12.0."
    ::= { tmnxLdpNgGroups 17 }

tmnxLdpNgTcpSessParamsV12v0Group OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTcpSessParamsTableLstCh,
        vRtrLdpNgTcpSessRowStatus,
        vRtrLdpNgTcpSessAuth,
        vRtrLdpNgTcpSessAuthKey,
        vRtrLdpNgTcpSessAuthKeyChain,
        vRtrLdpNgTcpSessPMTUDiscovery
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP TCP session
         parameters on Nokia SROS series systems release 12.0."
    ::= { tmnxLdpNgGroups 18 }

tmnxLdpNgGeneralV12v0Group       OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGeneralTableLstCh,
        vRtrLdpNgGenCreateTime,
        vRtrLdpNgGenIPv4UpTime,
        vRtrLdpNgGenIPv6UpTime,
        vRtrLdpNgGenLastChange,
        vRtrLdpNgGenAdminState,
        vRtrLdpNgGenIPv4OperState,
        vRtrLdpNgGenIPv6OperState,
        vRtrLdpNgGenIPv4OperDownReason,
        vRtrLdpNgGenIPv6OperDownReason,
        vRtrLdpNgGenLdpIPv4LsrId,
        vRtrLdpNgGenLdpIPv6LsrId,
        vRtrLdpNgGenProtocolVersion,
        vRtrLdpNgGenBackoffTime,
        vRtrLdpNgGenMaxBackoffTime,
        vRtrLdpNgGenTunnelDownDampTime,
        vRtrLdpNgGenGracefulRestart,
        vRtrLdpNgGenGRNbrLiveTime,
        vRtrLdpNgGenGRMaxRecoveryTime,
        vRtrLdpNgGenLabelWithdrawalDelay,
        vRtrLdpNgGenImplicitNull,
        vRtrLdpNgGenShortTTLPropLocal,
        vRtrLdpNgGenShortTTLPropTransit,
        vRtrLdpNgGenMPMBBTime,
        vRtrLdpNgGenLdpFrr,
        vRtrLdpNgGenMcastUpstreamFrr,
        vRtrLdpNgGenDeaggregateFec,
        vRtrLdpNgGenControlMode,
        vRtrLdpNgGenDistMethod,
        vRtrLdpNgGenRetentionMode,
        vRtrLdpNgGenPropagatePolicy,
        vRtrLdpNgGenLoopDetectCap,
        vRtrLdpNgGenHopLimit,
        vRtrLdpNgGenPathVectorLimit,
        vRtrLdpNgGenRoutePreference
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of extended LDP on
         Nokia SROS series systems 12.0 release."
    ::= { tmnxLdpNgGroups 19 }

tmnxLdpNgPolicyV12v0Group        OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgPolicyTableLstCh,
        vRtrLdpNgPolRowLastCh,
        vRtrLdpNgPolImportPolicy1,
        vRtrLdpNgPolImportPolicy2,
        vRtrLdpNgPolImportPolicy3,
        vRtrLdpNgPolImportPolicy4,
        vRtrLdpNgPolImportPolicy5,
        vRtrLdpNgPolExportPolicy1,
        vRtrLdpNgPolExportPolicy2,
        vRtrLdpNgPolExportPolicy3,
        vRtrLdpNgPolExportPolicy4,
        vRtrLdpNgPolExportPolicy5,
        vRtrLdpNgPolTunlTblExportPolicy1,
        vRtrLdpNgPolTunlTblExportPolicy2,
        vRtrLdpNgPolTunlTblExportPolicy3,
        vRtrLdpNgPolTunlTblExportPolicy4,
        vRtrLdpNgPolTunlTblExportPolicy5
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting policies of extended LDP protocol on
         Nokia SROS series systems 12.0 release."
    ::= { tmnxLdpNgGroups 20 }

tmnxLdpNgIfParamsV12v0Group      OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgIfParamsTableLstCh,
        vRtrLdpNgIfParamRowLastCh,
        vRtrLdpNgIfParamIPv4KAFactor,
        vRtrLdpNgIfParamIPv6KAFactor,
        vRtrLdpNgIfParamIPv4KATimeout,
        vRtrLdpNgIfParamIPv6KATimeout,
        vRtrLdpNgIfParamIPv4HelloFactor,
        vRtrLdpNgIfParamIPv6HelloFactor,
        vRtrLdpNgIfParamIPv4HelloTimeout,
        vRtrLdpNgIfParamIPv6HelloTimeout,
        vRtrLdpNgIfParamIPv4TransAddrTyp,
        vRtrLdpNgIfParamIPv6TransAddrTyp
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting interface parameters of extended LDP
         on Nokia SROS series systems 12.0 release."
    ::= { tmnxLdpNgGroups 21 }

tmnxLdpNgTargetedPeerV12v0Group  OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargTableLstCh,
        vRtrLdpNgTargRowLastCh,
        vRtrLdpNgTargImportPolicy1,
        vRtrLdpNgTargImportPolicy2,
        vRtrLdpNgTargImportPolicy3,
        vRtrLdpNgTargImportPolicy4,
        vRtrLdpNgTargImportPolicy5,
        vRtrLdpNgTargExportPolicy1,
        vRtrLdpNgTargExportPolicy2,
        vRtrLdpNgTargExportPolicy3,
        vRtrLdpNgTargExportPolicy4,
        vRtrLdpNgTargExportPolicy5,
        vRtrLdpNgTargTunnelPreference,
        vRtrLdpNgTargetedSessions,
        vRtrLdpNgTargIPv4KAFactor,
        vRtrLdpNgTargIPv6KAFactor,
        vRtrLdpNgTargIPv4KATimeout,
        vRtrLdpNgTargIPv6KATimeout,
        vRtrLdpNgTargIPv4HelloFactor,
        vRtrLdpNgTargIPv6HelloFactor,
        vRtrLdpNgTargIPv4HelloTimeout,
        vRtrLdpNgTargIPv6HelloTimeout,
        vRtrLdpNgTargIPv4HelloReduction,
        vRtrLdpNgTargIPv6HelloReduction,
        vRtrLdpNgTargIPv4HelloReduceFctr,
        vRtrLdpNgTargIPv6HelloReduceFctr
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting Targeted Peers of extended LDP on
         Nokia SROS series systems 12.0 release."
    ::= { tmnxLdpNgGroups 22 }

tmnxLdpNgAggrPreMatchV12v0Group  OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgAggrPreMatchTableLstCh,
        vRtrLdpNgAggrPreMatchRowLastCh,
        vRtrLdpNgAggrPreMatchEnabled,
        vRtrLdpNgAggrPreMatchExcPolicy1,
        vRtrLdpNgAggrPreMatchExcPolicy2,
        vRtrLdpNgAggrPreMatchExcPolicy3,
        vRtrLdpNgAggrPreMatchExcPolicy4,
        vRtrLdpNgAggrPreMatchExcPolicy5,
        vRtrLdpNgAggrPreMatchAdminState
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting Aggregate Prefix Match policies of
         extended LDP on Nokia SROS series systems 12.0 release."
    ::= { tmnxLdpNgGroups 23 }

tmnxLdpNgFecLimPerPeerV13v0Group OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgSessParamMaxFec,
        vRtrLdpNgSessParamMaxFecLogOnly,
        vRtrLdpNgSessParamMaxFecThold,
        vRtrLdpNgSessOperMaxFecThreshold
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting LSR FEC limit per LDP peer
         feature on Nokia SROS series systems."
    ::= { tmnxLdpNgGroups 24 }

tmnxLdpNgNotificationGroup       NOTIFICATION-GROUP
    NOTIFICATIONS {
        vRtrLdpNgSessMaxFecThresChanged,
        vRtrLdpNgSessMaxFecLimitReached,
        vRtrLdpNgIfStateChange,
        vRtrLdpNgInetIfStateChange,
        vRtrLdpNgIpv4InstStateChange,
        vRtrLdpNgIpv6InstStateChange,
        vRtrLdpNgSessionStateChange,
        vRtrLdpNgTargPeerStateChange,
        vRtrLdpNgResourceExhaustion,
        vRtrLdpNgAddrFecCommMismatch
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting LSR FEC limit per LDP peer
         feature on Nokia SROS series systems."
    ::= { tmnxLdpNgGroups 25 }

tmnxLdpNgSessParamPeerV13v0Group OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgSessParamAddrExpPolicy1,
        vRtrLdpNgSessParamAddrExpPolicy2,
        vRtrLdpNgSessParamAddrExpPolicy3,
        vRtrLdpNgSessParamAddrExpPolicy4,
        vRtrLdpNgSessParamAddrExpPolicy5
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP interfaces
         and targeted peers on Nokia SROS series systems 13.0 release."
    ::= { tmnxLdpNgGroups 26 }

tmnxLdpNgTcpSessParamsV13v0Group OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTcpSessMinTTLValue
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP TCP session
         parameters on Nokia SROS series systems release 13.0."
    ::= { tmnxLdpNgGroups 27 }

tmnxLdpNgNotifyObjs              OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgSessOperThresLevel,
        vRtrLdpNgInstNotifyReasonCode,
        vRtrLdpNgSessOverloadState,
        vRtrLdpNgSessOverloadDirection,
        vRtrLdpNgSessOverloadFecType,
        vRtrLdpNgSessOvldFecTypeSubTyp
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting LDP fec-limit notification on Nokia
         SROS series systems."
    ::= { tmnxLdpNgGroups 28 }

tmnxLdpNgHelloAdjV13v0Group      OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgHelloAdjLclIPv4P2MPCap,
        vRtrLdpNgHelloAdjRemIPv4P2MPCap,
        vRtrLdpNgHelloAdjLclIPv6P2MPCap,
        vRtrLdpNgHelloAdjRemIPv6P2MPCap,
        vRtrLdpNgHelloAdjLclIPv4PfxCap,
        vRtrLdpNgHelloAdjRemIPv4PfxCap,
        vRtrLdpNgHelloAdjLclIPv6PfxCap,
        vRtrLdpNgHelloAdjRemIPv6PfxCap
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP Hello
         Adjacencies on Nokia SROS series systems release 13.0."
    ::= { tmnxLdpNgGroups 29 }

tmnxLdpNgTargPeerV13v0Group      OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargPeerLocalIpAddrType,
        vRtrLdpNgTargPeerLocalIpAddress
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP targeted
         peer on Nokia SROS series systems release 13.0."
    ::= { tmnxLdpNgGroups 30 }

tmnxLdpNgInetIfV13v0Group        OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgInetIfLocalIpAddrType,
        vRtrLdpNgInetIfLocalIpAddress
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP Inet family
         interfaces on Nokia SROS series systems release 13.0."
    ::= { tmnxLdpNgGroups 31 }

tmnxLdpNgAddrActiveFecV13v0Group OBJECT-GROUP
    OBJECTS     {
        vLdpNgAddrActiveFecFecFlags,
        vLdpNgAddrActiveFecNumInLbls,
        vLdpNgAddrActiveFecNumOutLbls,
        vLdpNgAddrActiveFecInLbl,
        vLdpNgAddrActiveFecInLblIfIndex,
        vLdpNgAddrActiveFecOutLbl,
        vLdpNgAddrActiveFecOutLblStatus,
        vLdpNgAddrActiveFecOutLblIfIdx,
        vLdpNgAddrActiveFecOutLblNHType,
        vLdpNgAddrActiveFecOutLblNHAddr,
        vLdpNgAddrActiveFecOutLblMetric,
        vLdpNgAddrActiveFecOutLblMtu,
        vLdpNgAddrActiveFecOutLblLspId
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting Active Address FECs on Nokia SROS
         series systems 13.0."
    ::= { tmnxLdpNgGroups 32 }

tmnxLdpNgGeneralV13v0Group       OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenClassForwarding,
        vLdpNgAddrActiveFecOutLblCBF
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of extended LDP on
         Nokia SROS series systems 13.0 release."
    ::= { tmnxLdpNgGroups 33 }

tmnxLdpNgRecvFecCapV13v0Group    OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgSessPeerCapRecv,
        vRtrLdpNgHelloAdjPeerCapRecv
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting Active Address FECs on Nokia SROS
         series systems 13.0."
    ::= { tmnxLdpNgGroups 34 }

tmnxLdpNgGeneralEliV14v0Group    OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenEntropyLblCapability
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of extended LDP on
         Nokia SROS series systems 14.0 release."
    ::= { tmnxLdpNgGroups 35 }

tmnxLdpNgTargPeerV14v0Group      OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargPeerStatsHelloRecv,
        vRtrLdpNgTargPeerStatsHelloSent,
        vRtrLdpNgTargPeerStatsBadPduLen,
        vRtrLdpNgTargPeerStatsBadMsgLen,
        vRtrLdpNgTargPeerStatsMalformTlv,
        vRtrLdpNgTargPeerStatsBadProtVer
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP targeted
         peer on Nokia SROS series systems release 14.0."
    ::= { tmnxLdpNgGroups 36 }

tmnxLdpNgIfV14v0Group            OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgInetIfStatsHelloRecv,
        vRtrLdpNgInetIfStatsHelloSent,
        vRtrLdpNgInetIfStatsBadPduLen,
        vRtrLdpNgInetIfStatsBadMsgLen,
        vRtrLdpNgInetIfStatsMalformedTlv,
        vRtrLdpNgInetIfStatsBadProtoVer
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of extended LDP
         interfaces on Nokia SROS series systems 14.0 release."
    ::= { tmnxLdpNgGroups 37 }

tmnxLdpNgGeneralFrrV14v0Group    OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenFrrSRStitch
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of extended LDP
         fast reroute on Nokia SROS series systems 14.0 release."
    ::= { tmnxLdpNgGroups 38 }

tmnxLdpNgSessV14v0Group          OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgSessLocalUnregNotiCap,
        vRtrLdpNgSessPeerUnregNotiCap,
        vRtrLdpNgSessEndOfLibSent,
        vRtrLdpNgSessEndOfLibRecv,
        vRtrLdpNgGenUnregNotiCapability
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of End of Label
         Information Base Notifications on Nokia SROS series systems 14.0
         release."
    ::= { tmnxLdpNgGroups 40 }

tmnxLdpNgLegacyInteropGrp        OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenIpv4LsrInterop
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting general management of interoperability
         with legacy IPv4 LSR implementations on Nokia SROS series systems 14.0
         release."
    ::= { tmnxLdpNgGroups 41 }

tmnxLdpNgIpV632BitLsridGroup     OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargPeer32BitLsrFormat,
        vRtrLdpNgInetIf32BitLsrFormat
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting LDP IPv6 32-bit LSR-ID
         interoperability with Cisco and implementations not supporting 128-bit
         LSR-ID systems release 15.0."
    ::= { tmnxLdpNgGroups 43 }

tmnxLdpNgMcastUpstrmAsbrFrrGroup OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenMcastUpstrmAsbrFrr,
        vRtrLdpNgP2MPStitchRootAddrType,
        vRtrLdpNgP2MPStitchRootAddress,
        vRtrLdpNgP2MPFecStitchOpaqueTyp,
        vRtrLdpNgP2MPFecStitchOpaqueLen,
        vRtrLdpNgP2MPFecStitchOpaqueVal
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of multicast E2E P2mp
         protection for MLDP feature on Nokia SROS series systems release 15.0."
    ::= { tmnxLdpNgGroups 45 }

tmnxLdpNgBfdOnLspGroup           OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgBfdOnLspPfxListEnable,
        vRtrLdpNgBfdOnLspPfxListFailAct,
        vRtrLdpNgBfdOnLspPfxListLastChgd,
        vRtrLdpNgBfdOnLspPfxListPingIntv,
        vRtrLdpNgBfdOnLspPfxListPriority,
        vRtrLdpNgBfdOnLspPfxListRowStat,
        vRtrLdpNgBfdOnLspPfxListSrcAddr,
        vRtrLdpNgBfdOnLspPfxListSrcAddrT,
        vRtrLdpNgBfdOnLspPfxListTabLastC,
        vRtrLdpNgBfdOnLspPfxListTmplName,
        vRtrLdpNgBfdOnLspPrefixOperState
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting BFD on LDP LSPs, added in SROS series
         systems, release 15.0."
    ::= { tmnxLdpNgGroups 46 }

tmnxLdpNgNonRecFecGroup          OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenBasicFecOnly
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting non recursive FEC for option C feature
         on Nokia SROS series systems release 15.0."
    ::= { tmnxLdpNgGroups 47 }

tmnxLdpNgSessParamAdvertGroup    OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgSessParamAdvert,
        vRtrLdpNgSessLsrIdAdvert,
        vRtrLdpNgTargPeerLsrIdAdvert
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP session
         parameter on Nokia SROS series systems release 15.0."
    ::= { tmnxLdpNgGroups 48 }

tmnxLdpNgSessParamCommunityGroup OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgSessParamCommunity,
        vRtrLdpNgAddrFecCommunity,
        vRtrLdpNgSessCommunity,
        vRtrLdpNgTargPeerCommunity
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP session
         parameter on Nokia SROS series systems release 15.0."
    ::= { tmnxLdpNgGroups 49 }

tmnxLdpNgResolveRootUsingGroup   OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgResolveRootUsing
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting resolution via multicast route  table
         feature on Nokia SROS series systems release 16.0."
    ::= { tmnxLdpNgGroups 50 }

tmnxLdpNgWeightedEcmpGroup       OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenWeightedEcmp
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting control of weighted-ECMP in LDP on
         Nokia SROS series systems release 16.0."
    ::= { tmnxLdpNgGroups 51 }

tmnxLdpNgSysIpFecPolicyGroup     OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenConsiderSysIPInGep
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting control of system IP address FEC
         generation by policy feature feature on Nokia SROS series systems
         release 16.0."
    ::= { tmnxLdpNgGroups 52 }

tmnxLdpNgPolicyV16v0Group        OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgPolTunlTblImportPolicy1,
        vRtrLdpNgPolTunlTblImportPolicy2,
        vRtrLdpNgPolTunlTblImportPolicy3,
        vRtrLdpNgPolTunlTblImportPolicy4,
        vRtrLdpNgPolTunlTblImportPolicy5
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting policies of extended LDP protocol on
         Nokia SROS series systems 16.0 release."
    ::= { tmnxLdpNgGroups 53 }

tmnxLdpNgCBFV16v0Group           OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenCBFMode
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting class-based-forwarding of extended LDP
         protocol on Nokia SROS series systems 16.0 release."
    ::= { tmnxLdpNgGroups 54 }

tmnxLdpNgImportPmsiRoutesGroup   OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgImpPmsiMvpn,
        vRtrLdpNgImpPmsiMvpnNoExpComm
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting import of BGP PMSI routes feature on
         Nokia SROS series systems release 19.0."
    ::= { tmnxLdpNgGroups 56 }

tmnxLdpNgPolicyV19v0Group        OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgPolImportMcastPolicy1,
        vRtrLdpNgPolImportMcastPolicy2,
        vRtrLdpNgPolImportMcastPolicy3,
        vRtrLdpNgPolImportMcastPolicy4,
        vRtrLdpNgPolImportMcastPolicy5
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting policies of extended LDP  protocol on
         Nokia SROS series systems release 19.0."
    ::= { tmnxLdpNgGroups 57 }

tmnxLdpNgIntfWeightedEcmpGroup   OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgIfLBWeight
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting non-IGP-shortcut weighted ECMP for LDP
         prefix FECs on Nokia SROS series systems release 19.0."
    ::= { tmnxLdpNgGroups 58 }

tmnxLdpNgEcmpGroup               OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgMaxEcmpRoutes,
        vRtrLdpNgOperEcmp
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the LDP ECMP on Nokia SROS series
         systems release 19.0."
    ::= { tmnxLdpNgGroups 59 }

tmnxLdpNgAddrFecStitchPrefGroup  OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgPreferProtocolStitching
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the LDP address FEC stitch  preference
         on Nokia SROS series systems release 20.0."
    ::= { tmnxLdpNgGroups 60 }

tmnxLdpNgMldpOverRsvpV20v0Group  OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargTunnelMcastPrefer
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting mLDP over RSVP on Nokia SROS series
         systems 20.0 release."
    ::= { tmnxLdpNgGroups 61 }

tmnxLdpNgTargPeerV20v0Group      OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargPeerMcastTunneling
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP targeted
         peer on Nokia SROS series systems release 20.0."
    ::= { tmnxLdpNgGroups 62 }

tmnxLdpNgPeerParamsV20v0Group    OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargPeerMcTuLspTblLstCh,
        vRtrLdpNgTargPeerMcTunLspRowStat
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP interfaces
         and targeted peers on Nokia SROS series systems 20.0 release."
    ::= { tmnxLdpNgGroups 63 }

tmnxLdpTargAutoTldpV20v0Group    OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargAutoTxV4AdminState,
        vRtrLdpNgTargAutoTxV4Tunneling,
        vRtrLdpNgTargAutoRxV4AdminState,
        vRtrLdpNgTargAutoRxV4Tunneling
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of automatic T-LDP
         (Targeted Label Distribution Protocol) on Nokia SROS series systems
         20.0 release."
    ::= { tmnxLdpNgGroups 64 }

tmnxLdpNgTcpSeParGlblV21v0Group  OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTcpSessParamsGlTblLstCh,
        vRtrLdpNgTcpSessParamsGlblKeyChn,
        vRtrLdpNgTcpSessParmGlblAuthType,
        vRtrLdpNgTcpSessParmGlblAuthKey,
        vRtrLdpNgTcpSessInheritance
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of global TCP parameters
         for LDP peers on Nokia SROS series systems 21.0 release."
    ::= { tmnxLdpNgGroups 65 }

tmnxLdpNgAddrFecTunlPrefGroup    OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenTunnelPreference
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the LDP address FEC tunnel  preference
         on Nokia SROS series systems release 21.0."
    ::= { tmnxLdpNgGroups 66 }

tmnxLdpNgPreferTransFrrGroup     OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgGenPreferTransportFrr
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the LDP preference for transport FRR
         on Nokia SROS series systems  release 21.0."
    ::= { tmnxLdpNgGroups 67 }

tmnxLdpTargResV6PfxOvrIgpShGroup OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgTargResV6PfxOvrShortcut
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the LDP IPv6 prefix FEC resolution
         over IGP shortcut on Nokia SROS series  systems release 22.0."
    ::= { tmnxLdpNgGroups 68 }

tmnxLdpNgSessionGRGroup          OBJECT-GROUP
    OBJECTS     {
        vRtrLdpNgSessGRState
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of extended LDP Sessions on
         Nokia SROS series systems 24.0 Release."
    ::= { tmnxLdpNgGroups 69 }

tmnxLdpNgNotifyPrefix            OBJECT IDENTIFIER ::= { tmnxSRNotifyPrefix 91 }

tmnxLdpNgNotifications           OBJECT IDENTIFIER ::= { tmnxLdpNgNotifyPrefix 0 }

vRtrLdpNgIpv4InstStateChange     NOTIFICATION-TYPE
    OBJECTS     {
        vRtrLdpNgGenAdminState,
        vRtrLdpNgGenIPv4OperState,
        vRtrLdpNgInstNotifyReasonCode,
        vRtrLdpNgGenIPv4OperDownReason
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrLdpNgIpv4InstStateChange is generated when the IPv4
         LDP instance changes state operationally as specified by
         vRtrLdpNgGenIPv4OperState.

         [EFFECT] Based on the vRtrLdpNgGenIPv4OperDownReason reason code, the
         system may not be able to accept new requests from peers.

         [RECOVERY] Based on the vRtrLdpNgGenIPv4OperDownReason reason code,
         appropriate configuration changes in LDP may be required."
    ::= { tmnxLdpNgNotifications 1 }

vRtrLdpNgIpv6InstStateChange     NOTIFICATION-TYPE
    OBJECTS     {
        vRtrLdpNgGenAdminState,
        vRtrLdpNgGenIPv6OperState,
        vRtrLdpNgInstNotifyReasonCode,
        vRtrLdpNgGenIPv6OperDownReason
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrLdpNgIpv6InstStateChange is generated when the IPv6
         LDP instance changes state operationally as specified by
         vRtrLdpNgGenIPv6OperState.

         [EFFECT] Based on the vRtrLdpNgGenIPv6OperDownReason reason code, the
         system may not be able to accept new requests from peers.

         [RECOVERY] Based on the vRtrLdpNgGenIPv6OperDownReason reason code,
         appropriate configuration changes in LDP may be required."
    ::= { tmnxLdpNgNotifications 2 }

vRtrLdpNgIfStateChange           NOTIFICATION-TYPE
    OBJECTS     {
        vRtrLdpNgIfAdminState,
        vRtrLdpNgIfOperState,
        vRtrLdpNgIfOperDownReason
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrLdpNgIfStateChange notification is generated when the
         LDP interface changes state either administratively or operationally.

         [EFFECT] Based on the vRtrLdpNgIfOperDownReason reason code, the
         system may not be able to accept new requests from peers over this
         interface.

         [RECOVERY] Based on the vRtrLdpNgIfOperDownReason reason code,
         appropriate configuration changes in LDP may be required."
    ::= { tmnxLdpNgNotifications 3 }

vRtrLdpNgInetIfStateChange       NOTIFICATION-TYPE
    OBJECTS     {
        vRtrLdpNgInetIfAdminState,
        vRtrLdpNgInetIfOperState,
        vRtrLdpNgInetIfOperDownReason
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrLdpNgInetIfStateChange notification is generated when
         the LDP sub-interface changes state either administratively or
         operationally.

         [EFFECT] Based on the vRtrLdpNgInetIfOperDownReason reason code, the
         system may not be able to accept new requests over this interface.

         [RECOVERY] Based on the vRtrLdpNgInetIfOperDownReason reason code,
         appropriate configuration changes in LDP may be required."
    ::= { tmnxLdpNgNotifications 4 }

vRtrLdpNgTargPeerStateChange     NOTIFICATION-TYPE
    OBJECTS     {
        vRtrLdpNgTargPeerAdminState,
        vRtrLdpNgTargPeerOperState,
        vRtrLdpNgTargPeerOperDownReason
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrLdpNgTargPeerStateChange notification is generated
         when the LDP peer changes state either administratively or
         operationally.

         [EFFECT] Based on the vRtrLdpNgTargPeerOperDownReason reason code, the
         system may not be able to accept new requests from this peer.

         [RECOVERY] Based on the vRtrLdpNgTargPeerOperDownReason reason code,
         appropriate configuration changes in LDP may be required."
    ::= { tmnxLdpNgNotifications 5 }

vRtrLdpNgSessionStateChange      NOTIFICATION-TYPE
    OBJECTS     {
        vRtrLdpNgSessState,
        vRtrLdpNgSessOverloadState,
        vRtrLdpNgSessOverloadDirection,
        vRtrLdpNgSessOverloadFecType,
        vRtrLdpNgSessOvldFecTypeSubTyp
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrLdpNgSessionStateChange notification is generated when
         the LDP Overload Notification message is sent to or received from the
         peer vRtrLdpNgPeerLdpId for the combination of
         vRtrLdpNgSessOverloadFecType and vRtrLdpNgSessOvldFecTypeSubTyp while
         vRtrLdpNgSessState remains 'operational'.

         [EFFECT] Once the Local LSR has sent the LDP Overload Notification
         message to the peer vRtrLdpNgPeerLdpId for fec and sub type fec
         indicated by vRtrLdpNgSessOverloadFecType and
         vRtrLdpNgSessOvldFecTypeSubTyp and vRtrLdpNgSessOverloadState has the
         value of 'true', then new Label Mapping Messages received for this
         peer for the given combination of fec and sub type fec is returned
         with a Label Release Message.

         If the Local LSR has received an LDP Overload Notification message
         from the peer vRtrLdpNgPeerLdpId for fec and sub type fec indicated by
         vRtrLdpNgSessOverloadFecType and vRtrLdpNgSessOvldFecTypeSubTyp and
         vRtrLdpNgSessOverloadState has the value of 'true', no new Label
         Mapping Message for the given combination of fec and sub type fec will
         be sent to this peer.

         If the Local LSR has received an LDP Overload Notification message
         from the peer vRtrLdpNgPeerLdpId for fec and sub type fec indicated by
         vRtrLdpNgSessOverloadFecType and vRtrLdpNgSessOvldFecTypeSubTyp and
         vRtrLdpNgSessOverloadState has the value of 'false', then the Local
         LSR will send all pending and any new Label Mapping Message for the
         given combination of fec and sub type fec to this peer.

         [RECOVERY] In case the Local LSR sent the LDP Overload Notification
         message to the peer vRtrLdpNgPeerLdpId and vRtrLdpNgSessOverloadState
         has the value of 'true' for fec and sub type fec indicated by
         vRtrLdpNgSessOverloadFecType and vRtrLdpNgSessOvldFecTypeSubTyp, then
         appropriate LDP configuration changes may be required on the Local
         and/or Remote LSR.

         Once the Local LSR is not overloaded anymore, an LDP Overload
         Notification message is sent to the peer vRtrLdpNgPeerLdpId and
         vRtrLdpNgSessOverloadState has the value of 'false' for given fec and
         sub type fec."
    ::= { tmnxLdpNgNotifications 6 }

vRtrLdpNgSessMaxFecThresChanged  NOTIFICATION-TYPE
    OBJECTS     {
        vRtrLdpNgSessParamMaxFec,
        vRtrLdpNgSessOperThresLevel,
        vRtrLdpNgSessOperMaxFecThreshold
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] A vRtrLdpNgSessMaxFecThresChanged notification is generated
         when the number of FECs accepted from the peer has exceeded or drops
         below vRtrLdpNgSessOperMaxFecThreshold percent of the value specified
         by vRtrLdpNgSessParamMaxFec.

         New notification will not be generated if multiple internal change
         events occur for the same level indicated by
         vRtrLdpNgSessOperThresLevel during a 2 minute interval.

         If any parameter in FEC limit configuration changes then we would
         always raise this trap if current number of FECs are above the
         configured threshold or has crossed the threshold downwards. If we
         remain on or below the configured threshold before and after the
         configuration changes then no trap would be generated.

         [EFFECT] No direct effect but if the peer LSR continues to send
         further Label Mapping Message, then the number of FECs may exceed the
         configured maximum (vRtrLdpNgSessParamMaxFec) resulting in the
         generation of vRtrLdpNgSessMaxFecLimitReached notification.

         [RECOVERY] Appropriate Configuration changes in local or peer LSR will
         be required."
    ::= { tmnxLdpNgNotifications 7 }

vRtrLdpNgSessMaxFecLimitReached  NOTIFICATION-TYPE
    OBJECTS     {
        vRtrLdpNgSessParamMaxFec,
        vRtrLdpNgSessOperMaxFecThreshold
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] A vRtrLdpNgSessMaxFecLimitReached notification is generated
         when the number of FECs accepted from the peer has reached the value
         specified by vRtrLdpNgSessParamMaxFec.

         If the current number of FECs go below the limit but higher than the
         configured threshold and again start to increase and hit the limit a
         second time, we will raise a trap if 2 or more minutes have elapsed
         since the first vRtrLdpNgSessMaxFecLimitReached trap was sent.

         If any parameter in FEC limit configuration changes and the current
         number of FECs are equal to or higher than the limit specified by
         vRtrLdpPeerMaxFec, then we would always raise the
         vRtrLdpNgSessMaxFecLimitReached trap.

         [EFFECT] When the number of FECs exceed the configured maximum
         (vRtrLdpNgSessParamMaxFec) it results in any of the following:

         (1) If vRtrLdpNgSessParamMaxFecLogOnly is set to 'false' and LSR
         Overload Capability is supported, then Overload procedure will take
         place.

         (2) If vRtrLdpNgSessParamMaxFecLogOnly is set to 'false' and LSR
         Overload Capability is not supported, Label Mapping Message will be
         returned with Label Release Message.

         (3) If vRtrLdpNgSessParamMaxFecLogOnly is set to 'true', no action
         will be taken.

         [RECOVERY] Appropriate Configuration changes in local or peer LSR will
         be required."
    ::= { tmnxLdpNgNotifications 8 }

vRtrLdpNgResourceExhaustion      NOTIFICATION-TYPE
    OBJECTS     {
        vRtrID
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] The vRtrLdpNgResourceExhaustion notification is generated when
         CPM or data path resource required for FEC resolution is exhausted.The
         new notification will not be generated if multiple internal change
         events occur during a 10 minute interval.

         [EFFECT] The system may not be able to accept new request from peers.

         [RECOVERY] Appropriate configuration changes in LDP may be required."
    ::= { tmnxLdpNgNotifications 9 }

vRtrLdpNgAddrFecCommMismatch     NOTIFICATION-TYPE
    OBJECTS     {
        vRtrID,
        vRtrLdpNgAddrFecCommunity
    }
    STATUS      current
    DESCRIPTION
        "[CAUSE] A vRtrLdpNgAddrFecCommMismatch notification is generated when
         two or more peer routers advertising labels for the given address FEC
         have been assigned differing communities, or some have been assigned
         communities and some have not.  It will also be generated if multiple
         LDP peer routers have been configured to advertise their local LSR-ID
         as a FEC, and those peer routers have been assigned differing communities.
         This notification is rate-limited to at most one notification every 60 seconds.

         [EFFECT] This condition indicates that the network is misconfigured,
         and it is likely that the affected address FEC is not being advertised
         to the routers which the operator intends.

         [RECOVERY] Analyze, check and fix the community configuration for all
         LDP session-parameters and LDP targeted-session peer-templates in the
         network to find the error.  Start with the configuration on the router
         generating the notification, and if this is correct, look next at the
         routers advertising the labels to see if their configuration is correct."
    ::= { tmnxLdpNgNotifications 11 }

END
