TIMETRA-FILTER-MIB DEFINITIONS ::= BEGIN

IMPORTS
    InterfaceIndexOrZero
                                                         FROM IF-MIB
    InetAddress, InetAddressIPv4,
    InetAddressIPv6,
    InetAddressPrefixLength, InetAddressType
                                                         FROM INET-ADDRESS-MIB
    MODULE-COMPLIANCE, NOTIFICATION-GROUP,
    OBJECT-GROUP
                                                         FROM SNMPv2-CONF
    Counter32, Counter64, Gauge32,
    Integer32, IpAddress, MODULE-IDENTITY,
    NOTIFICATION-TYPE, OBJECT-TYPE, Opaque,
    TimeTicks, Unsigned32
                                                         FROM SNMPv2-SMI
    DisplayString, MacAddress, RowPointer,
    RowStatus, TEXTUAL-CONVENTION,
    TimeStamp, TruthValue
                                                         FROM SNMPv2-TC
    timetraSRMIBModules, tmnxSRConfs,
    tmnxSRNotifyPrefix, tmnxSRObjs
                                                         FROM TIMETRA-GLOBAL-MIB
    TmnxPortEncapType
                                                         FROM TIMETRA-PORT-MIB
    ClassIndexOrNone, Dot1PPriority,
    IPv6FlowLabel, IPv6FlowLabelMask,
    IpAddressPrefixLength, QTagFullRange,
    QTagFullRangeOrNone, QTagOrNone,
    SdpBindId, ServiceAccessPoint, SvcISID,
    TDSCPFilterActionValue,
    TDSCPNameOrEmpty, TFCTypeOrNone,
    TFrameType, TIcmpCodeOrNone,
    TIcmpTypeOrNone, TIpOption, TIpProtocol,
    TIpProtocolNumber, TItemDescription,
    TLNamedItem, TLNamedItemOrEmpty,
    TMacFilterType, TNamedItem,
    TNamedItemOrEmpty, TOperator,
    TPolicerBurstSizeBytes,
    TRegularExpression, TTcpUdpPort,
    TmnxAddressAndPrefixAddress,
    TmnxAddressAndPrefixPrefix,
    TmnxAddressAndPrefixType,
    TmnxAdminState,
    TmnxAdminStateTruthValue, TmnxEncapVal,
    TmnxHttpRedirectUrl,
    TmnxNatSubscriberType,
    TmnxNatSubscriberTypeOrNone,
    TmnxOperState, TmnxPortID, TmnxServId,
    TmnxSubBondingConnIdOrEmpty, TmnxVRtrID,
    TmnxVRtrIDOrZero, TmnxVRtrMplsLspID
                                                         FROM TIMETRA-TC-MIB
    ;

timetraFilterMIBModule           MODULE-IDENTITY
    LAST-UPDATED "201701010000Z"
    ORGANIZATION "Nokia"
    CONTACT-INFO
        "Nokia SROS Support
         Web: http://www.nokia.com"
    DESCRIPTION
        "This document is the SNMP MIB module to manage and provision Filter
         features on Nokia SROS systems.

         Copyright 2003-2018 Nokia. All rights reserved. Reproduction of this
         document is authorized on the condition that the foregoing copyright
         notice is included.

         This SNMP MIB module (Specification) embodies Nokia's
         proprietary intellectual property.  Nokia retains
         all title and ownership in the Specification, including any
         revisions.

         Nokia grants all interested parties a non-exclusive license to use and
         distribute an unmodified copy of this Specification in connection with
         management of Nokia products, and without fee, provided this copyright
         notice and license appear on all copies.

         This Specification is supplied 'as is', and Nokia makes no warranty,
         either express or implied, as to the use, operation, condition, or
         performance of the Specification."

    REVISION    "201701010000Z"
    DESCRIPTION
        "Rev 15.0                1 Jan 2017 00:00
         15.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "201601010000Z"
    DESCRIPTION
        "Rev 14.0                1 Jan 2016 00:00
         14.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "201501010000Z"
    DESCRIPTION
        "Rev 13.0                1 Jan 2015 00:00
         13.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "201401010000Z"
    DESCRIPTION
        "Rev 12.0                1 Jan 2014 00:00
         12.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "201208010000Z"
    DESCRIPTION
        "Rev 11.0                1 Aug 2012 00:00
         11.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "201102010000Z"
    DESCRIPTION
        "Rev 9.0                01 Feb 2011 00:00
         9.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "200907010000Z"
    DESCRIPTION
        "Rev 8.0                01 Jul 2009 00:00
         8.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "200807010000Z"
    DESCRIPTION
        "Rev 6.1                01 Jul 2008 00:00
         6.1 release of the TIMETRA-FILTER-MIB."

    REVISION    "200801010000Z"
    DESCRIPTION
        "Rev 6.0                01 Jan 2008 00:00
         6.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "200701010000Z"
    DESCRIPTION
        "Rev 5.0                01 Jan 2007 00:00
         5.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "200602280000Z"
    DESCRIPTION
        "Rev 4.0                28 Feb 2006 00:00
         4.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "200508310000Z"
    DESCRIPTION
        "Rev 3.0                31 Aug 2005 00:00
         3.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "200501240000Z"
    DESCRIPTION
        "Rev 2.1                24 Jan 2005 00:00
         2.1 release of the TIMETRA-FILTER-MIB."

    REVISION    "200401150000Z"
    DESCRIPTION
        "Rev 2.0                15 Jan 2004 00:00
         2.0 release of the TIMETRA-FILTER-MIB."

    REVISION    "200308150000Z"
    DESCRIPTION
        "Rev 1.2                15 Aug 2003 00:00
         1.2 release of the TIMETRA-FILTER-MIB."

    REVISION    "200301290000Z"
    DESCRIPTION
        "Rev 0.1                29 Jan 2003 00:00
         Initial version of the TIMETRA-FILTER-MIB."

    ::= { timetraSRMIBModules 21 }

TFilterID                        ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The identification number of a filter. 0 indicates an invalid
         filter-id."
    SYNTAX      Unsigned32 (0..65535)

TFilterFlowspecGroupId           ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The identification number of a flowspec group. 65535 indicates an
         invalid group id (when used in embedding it means embed rules from all
         groups)"
    SYNTAX      Unsigned32 (0..16383 | 65535)

TIPFilterIdOrEmpty               ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The identification number of an IP filter."
    SYNTAX      Integer32 (-1 | 0..65535)

TVsdFilterID                     ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The identification number of a filter managed by a VSD controller.

         The value of the upper 16 bits is always equal to 0x0400.

         The value of the lower 16 bits corresponds to the last segment of the
         name used for the filter in CLI (_tmnx_vsd_<lower_16_bits>)."
    SYNTAX      Unsigned32 (67108865..67174399)

TConfigOrVsdFilterID             ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The identification number of a filter. Any value greater than
         0x0000FFFF (65535) indicates a filter that was dynamically created
         (auto-generated) by the system and as such cannot be used as part of
         any SNMP SET operation.

         - The range 0x00000001 .. 0x0000FFFF (1 .. 65535)
           indicates a regular configuration originated filter.

         - The range 0x04000001 .. 0x0400FFFF (67108865 .. 67174399)
           indicates a filter managed by a VSD controller. In this case
           the last 16 bits indicate the ID of the VSD filter.

         - The value 0 indicates an invalid filter-id (e.g. no filter applied
           on a particular endpoint)."
    SYNTAX      Unsigned32 (0..65535 | 67108865..67174399)

TAnyFilterID                     ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Represents a filter Id. Any value greater than 65535 indicates a
         filter that was created (auto-generated) by the system.

         - The range 0x01000000 through 0x0100FFFF indicates a filter used for
           BGP Flow-Spec. In this case, the last 15 bits indicate the value of
           the vRtrID where the filter is active. Values higher than 0x01008000
           represent flowspec group filters.

         - The range 0x03000000 through 0x0300FFFF indicates a filter used for
           Open-Flow.

         - The range 0x20000000 .. 0x3FFFFFFF is used for handling filter rules
           (received from RADIUS) that are to be shared between users. The Id
           is encoded as follows:
           - the highest 3 bits (0b001) indicate that it is an auto-generated
             shared filter
           - the subsequent 13 bits indicate which combination of filter rules
             are inserted; this corresponds to the second number in the filter
             Id as displayed in CLI: the '1' in the example '9:1'
           - the subsequent 16 bits indicate the base filter Id; this
             corresponds to the first number ('9') in  '9:1'

         - The range 0x10000000 .. 0x1FFFFFFF is used for handling filter
           flow-rules (received from DIAMETER) that are to be shared between
           users. The Id is encoded as follows:
           - the highest 4 bits (0b0001) indicate that it is an auto-generated
             flow-rule filter
           - the subsequent 12 bits indicate which combination of flow-rules are
             inserted; this corresponds to the second number in the filter Id as
             displayed in CLI: the '2' in the example '9:P2'
           - the subsequent 16 bits indicate the base filter Id; this
             corresponds to the first number ('9') in the example '9:P2'

         - The range 0x04000001 .. 0x0400FFFF (67108865..67174399)
           indicates a filter managed by a VSD controller. In this case
           the last 16 bits indicate the ID of the VSD filter.
           "
    SYNTAX      Unsigned32

TFilterScope                     ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "This textual convention determines some aspects of an item's behavior
         regarding creation and use, unused entry garbage collection, and
         automated promulgation by Element Management System to other systems
         in the service domain.

         TFilterScope is an extension of the textual convention TItemScope.

         exclusive:

            When the scope of an item is defined as exclusive, the item can
            only be applied once, for example to a single SAP.  Attempting
            to assign the policy to a second SAP is not allowed and will
            result in an error.  If the item is removed from the exclusive
            SAP, it will become available for assignment to another
            exclusive SAP.

            A non-applied exclusive scope policy is a candidate to be removed
            from the system by a TBD garbage collection command.

            The system default policies cannot be put into the exclusive scope.
            An error will be generated if scope exclusive is executed in
            any policies with a policy-id equal to 1.

         template:

            When the scope of an item is defined as template, the item can be
            applied any number of times.  Policies with template scope
            will not be considered for deletion by a TBD garbage collection
            command; all items of scope 'template' must be deleted explicitly.

            The system default policies will always be scope template.
            An error will occur if a policy-id 1 is attempted to be
            set to scope exclusive.

         embedded:

            When the scope of a filter is defined as embedded, this indicates
            that the filter may be embedded in other non-embedded filters.
            An embedded filter may not be applied anywhere in the system.
            Attempting to set scope to embedded for a filter which is
            already applied will be rejected by the system.

         system:

            When the scope of a filter policy is defined as system, the filter
            policy can be used as a common system filter policy only.

            The policy cannot be applied directly anywhere in the system.
            In order to activate the policy it must be configured as the active
            system filter policy in tFilterSystemFilterTable.

            All other 'exclusive' and 'template' IP / IPv6 filter policies may
            be chained to the active system policy by setting the
            tIPFilterChainToSystemFilter or tIPv6FilterChainToSystemFilter
            object to 'true(1)'.

            When an IP / IPv6 filter policy is chained to the system filter
            policy, system filter policy's rules are executed first before
            any rules of the activating filter policy are executed.

            The scope of a filter policy can be set to/from this value only
            when the policy does not contain any entry.

         cpm:

            When the scope of a filter is defined as cpm, this indicates
            that the filter can be used as cpm filter only.

            Cpm filter cannot be applied directly anywhere in the system.
            In order to activate the cpm-filter it must be configured as the active
            cpm filter policy in tmnxCpmHwFilterObjs."
    SYNTAX      INTEGER {
        exclusive (1),
        template  (2),
        embedded  (3),
        system    (4),
        cpm       (5)
    }

TItemMatch                       ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "when set to off, the item is not matched. when set to false, packets
         without the item match the filter. when set to true, packets with the
         item match the filter."
    SYNTAX      INTEGER {
        off   (1),
        false (2),
        true  (3)
    }

TFragmentMatch                   ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "when set to off, the item is not matched. when set to false, packets
         without the item match the filter entry. when set to true, packets
         with the item match the filter entry. when set to first-only, packets
         with first fragment match the filter entry. when set to
         non-first-only, packets with non-first fragment match the filter
         entry."
    SYNTAX      INTEGER {
        off            (1),
        false          (2),
        true           (3),
        first-only     (4),
        non-first-only (5)
    }

TAnyEntryId                      ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Uniquely identifies an entry in a policy or filter table."
    SYNTAX      Unsigned32

TEntryIdOrZero                   ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Uniquely identifies an entry in a policy or filter table.
         To facilitate insertion of entries in the tables, we recommend
         assigning entry IDs by 10s:  10, 20, 30, etc.
         The value 0, means that the object does not refer to a filter
         entry at this time."
    SYNTAX      TAnyEntryId (0..2097151)

TEntryId                         ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Uniquely identifies an entry in a policy or filter table.
         To facilitate insertion of entries in the tables, we recommend
         assigning entry IDs by 10s:  10, 20, 30, etc."
    SYNTAX      TEntryIdOrZero (1..2097151)

TLimitedEntryId                  ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Uniquely identifies an entry in a policy or filter table.
         To facilitate insertion of entries in the tables, we recommend
         assigning entry IDs by 10s:  10, 20, 30, etc."
    SYNTAX      TEntryId (1..65535)

TDhcpEntryId                     ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        ""
    SYNTAX      TLimitedEntryId

TEntryBlockSize                  ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Defines size of block used for filter entries insertion."
    SYNTAX      TEntryIdOrZero (0..65535)

TFilterAction                    ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Action to take on a packet:
         - drop        (1): packets matching the filter entry are dropped.
         - forward     (2): packets matching the filter entry are forwarded.
         - httpRedirect(4): packets matching the filter entry are redirected.
         - nat         (5): packets matching the filter entry are forwarded to
                            the NAT function in the system.
         - reassemble  (6): packets matching the filter entry are forwarded to
                            the packet REASSEMBLE function in the system.
         - gtpLclBrkout(7): packets matching the filter entry are broken out
                            locally from a GTP tunnel (and thereby bypass the
                            mobile packet core). For packets that are not sent
                            in the context of a GTP tunnel, this action is
                            equivalent to 'forward'.
         - forwardEsiL2(8): packets matching the filter entry are forwarded to
                            ESI identified first appliance in Nuage service
                            chain using EVPN-resolved VXLAN tunnel in
                            the specified VPLS service.
         - forwardEsiL3(9): packets matching the filter entry are forwarded to
                            ESI/SF-IP identified first appliance in Nuage
                            service chain using EVPN-resolved VXLAN tunnel over
                            the configured VAS interface in the specified VPRN
                            service.
         - unrecognized(11): Tables tMacFilterParamsTable, tIPFilterParamsTable,
                            tIPv6FilterParamsTable and their augment tables can
                            only be used to configure actions which were
                            available before introducing
                            tMacFltrEntryActionTable and
                            tIPvXFltrEntryActionTable. All actions (including
                            action related functionality) can be configured via
                            tables tMacFltrEntryActionTable and
                            tIPvXFltrEntryActionTable. The value 'unrecognized'
                            indicates that the currently configured action was
                            added after introduction of tMacFltrEntryActionTable
                            and tIPvXFltrEntryActionTable and can't be
                            interpreted in the tables tMacFilterParamsTable,
                            tIPFilterParamsTable, tIPv6FilterParamsTable and
                            their augment tables.
                            "
    SYNTAX      INTEGER {
        drop         (1),
        forward      (2),
        httpRedirect (4),
        nat          (5),
        reassemble   (6),
        gtpLclBrkout (7),
        forwardEsiL2 (8),
        forwardEsiL3 (9),
        unrecognized (11)
    }

TFilterPbrDownActionOvr          ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The textual convention TFilterPbrDownActionOvr specifies an override of
         default PBR down action:
         - none                  (0): default PBR down action is applied to
                                      packets matching the filter entry.
                                      Default PBR down action is either drop
                                      or forward based on PBR action type.
         - drop                  (1): packets matching the filter entry are
                                      dropped.
         - forward               (2): packets matching the filter entry are
                                      forwarded.
         - filterDefaultAction   (3): packets matching the filter entry are
                                      handled according to filter default action
                                      configured using tIPFilterDefaultAction
                                      for IP filter, tIPv6FilterDefaultAction
                                      for IPv6 filter and
                                      tMacFilterDefaultAction for MAC filter."
    SYNTAX      INTEGER {
        none                (0),
        drop                (1),
        forward             (2),
        filterDefaultAction (3)
    }

TFilterActionOrDefault           ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Action to take on a packet:
         - drop        (1): packets matching the filter entry are dropped.
         - forward     (2): packets matching the filter entry are forwarded.
         - default     (3): packets matching the filter entry get the applicable
                            default behavior. Note: the value 'default' is
                            currently not supported.
         - httpRedirect(4): packets matching the filter entry are redirected.
         - nat         (5): packets matching the filter entry are forwarded to
                            the NAT function in the system.
         - reassemble  (6): packets matching the filter entry are forwarded to
                            the packet REASSEMBLE function in the system.
         - gtpLclBrkout(7): packets matching the filter entry are broken out
                            locally from a GTP tunnel (and thereby bypass the
                            mobile packet core). For packets that are not sent
                            in the context of a GTP tunnel, this action is
                            equivalent to 'forward'.
         - forwardEsiL2(8): packets matching the filter entry are forwarded to
                            ESI identified first appliance in Nuage service
                            chain using EVPN-resolved VXLAN tunnel in
                            the specified VPLS service.
         - forwardEsiL3(9): packets matching the filter entry are forwarded to
                            ESI/SF-IP identified first appliance in Nuage
                            service chain using EVPN-resolved VXLAN tunnel over
                            the configured VAS interface in the specified VPRN
                            service.
         - unrecognized(11): Tables tMacFilterParamsTable, tIPFilterParamsTable,
                            tIPv6FilterParamsTable and their augment tables can
                            only be used to configure actions which were
                            available before introducing
                            tMacFltrEntryActionTable and
                            tIPvXFltrEntryActionTable. All actions (including
                            action related functionality) can be configured via
                            tables tMacFltrEntryActionTable and
                            tIPvXFltrEntryActionTable. The value 'unrecognized'
                            indicates that the currently configured action was
                            added after introduction of tMacFltrEntryActionTable
                            and tIPvXFltrEntryActionTable and can't be
                            interpreted in the tables tMacFilterParamsTable,
                            tIPFilterParamsTable, tIPv6FilterParamsTable and
                            their augment tables.
         - ignoreMatch(30): Match criteria are skipped.
                            "
    SYNTAX      INTEGER {
        drop         (1),
        forward      (2),
        default      (3),
        httpRedirect (4),
        nat          (5),
        reassemble   (6),
        gtpLclBrkout (7),
        forwardEsiL2 (8),
        forwardEsiL3 (9),
        unrecognized (11),
        ignoreMatch  (30)
    }

TIPvXFilterEntryAction           ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Action to take on a packet:
         - drop                (1): A packet matching the entry will be dropped.
         - forward             (2): A packet matching the entry will be
                                    forwarded using regular routing.
         - httpRedirect        (4): An HTTP GET packet matching the entry is
                                    forwarded to CPM for HTTP captive portal
                                    processing.
         - nat                 (5): A packet matching the entry will be
                                    forwarded to NAT.
         - reassemble          (6): Packets matching the entry are forwarded to
                                    the packet REASSEMBLE function in the
                                    system.
         - gtpLclBrkout        (7): A packet matching the entry is broken out
                                    locally from a GTP tunnel (and thereby
                                    bypass the mobile packet core). For packets
                                    that are not sent in the context of a GTP
                                    tunnel, this action is equivalent to
                                    forward.
         - forwardEsiL2        (8): A packet matching the entry will be
                                    forwarded to ESI identified first appliance
                                    in Nuage service chain using EVPN-resolved
                                    VXLAN tunnel in the specified VPLS service.
         - forwardEsiL3        (9): A packet matching the entry will be
                                    forwarded to ESI/SF-IP identified first
                                    appliance in Nuage service chain using
                                    EVPN-resolved VXLAN tunnel over the
                                    configured VAS interface in the specified
                                    VPRN service.
         - ofPacketIn         (10): Packets are sent to controller configured
                                    for this H-OFS instance on a dedicated
                                    packet-in channel part of the main or
                                    auxiliary connection.
         - dropTtl            (12): A packet matching the entry will be dropped
                                    only if 'Time-to-live' field of packet's
                                    IPv4 header or 'Hop-Limit' field of packet's
                                    IPv6 header meets the configured condition.
         - dropPktLen         (13): A packet matching the entry will be dropped
                                    only if 'Total Length' field of packet's
                                    IPv4 header or 'Payload Length' field of
                                    packet's IPv6 header field meets the
                                    configured condition.
         - forwardRtr         (14): A packet matching the entry will be
                                    forwarded in the configured routing context.
         - forwardNextHop     (15): A packet matching the entry will be
                                    forwarded in the routing context of the
                                    incoming interface using direct or indirect
                                    IP address in the routing lookup.
         - forwardNextHopRtr  (16): A packet matching the entry will be
                                    forwarded in the configured routing context
                                    using direct or indirect IP address in the
                                    routing lookup.
         - forwardNHInterface (17): A packet matching the entry will be
                                    forwarded using the configured local
                                    interface. This value was obsoleted in
                                    release 24.3.
         - forwardLsp         (18): A packet matching the entry will be
                                    forwarded using the specified LSP.
         - forwardSdp         (19): A packet matching the entry will be
                                    forwarded using the configured SDP.
         - forwardSap         (20): A packet matching the entry will be
                                    forwarded using the configured SAP.
         - forwardRPlcy       (21): A packet matching the entry will be
                                    forwarded using forward next-hop or forward
                                    next-hop router and the IP address of
                                    destination selected by the configured
                                    redirect policy.  If no destination is
                                    selected packets are subject to action
                                    forward.
         - rateLimit          (22): Traffic matching the entry will be limited
                                    to the value specified by the object
                                    tIPvXFltrEntryActRateLimit.
         - tcpMssAdjust       (23): The value of TCP Maximum Segment Size (MSS)
                                    option of packets matching the entry will be
                                    set to the value specified by
                                    TIMETRA-VRTR-MIB.mib::tmnxVrtrMssAdjSegmentSize
                                    if the value of the option exceeds that
                                    value or the option is not present at all.
         - remarkDscp         (24): DSCP value of packets matching the entry
                                    will be remarked.
         - rateLimitPktLen    (25): Packet rate of packets matching the entry
                                    and having value of 'Total Length' field of
                                    packet's IPv4 header or value of 'Payload
                                    Length' field of packet's IPv6 header
                                    meeting the configured condition is limited
                                    to value specified by
                                    tIPvXFltrEntryActRateLimit.
         - rateLimitTtl       (26): Packet rate of packets matching the entry
                                    and having value of 'Time-to-live' field of
                                    packet's IPv4 header or value of 'Hop-Limit'
                                    field of packet's IPv6 header
                                    meeting the configured condition is limited
                                    to value specified by
                                    tIPvXFltrEntryActRateLimit.
         - dropExtractedTraffic (27): Traffic extracted to CPM will be dropped.
         - forwardVprnTarget   (28): A packet matching the filter entry will be
                                    forwarded using specified tunnel.
         - forwardBondingConnection (29):In a bonding context indicates the packet should be
                                         forwarded over the given connection if that
                                         connection is available. Outside a bonding context
                                         this is equivalent to an unqualified forward action.
         - ignoreMatch        (30): Match criteria are skipped.
         - forwardGreTunnel         (31):A packet matching the entry will be
                                         encapsulated in GRE an transported to a locations
                                         defined in GRE tunnel template.
         - dropPattern              (32):A packet matching the entry and containing
                                         the specified pattern will be dropped.
         - rateLimitPattern         (33):Packet rate of packets matching the entry
                                         and containing the specified pattern is limited
                                         to value specified by tIPvXFltrEntryActRateLimit.
         - forwardPattern              (34):A packet matching the entry and containing
                                         the specified pattern will be forwarded.
         - forwardMplsPlcyEndpt   (35): A packet matching the entry will be forwarded
                                           using a tunnel associated with the MPLS forwarding policy endpoint.
         - forwardSrtePlcyEndptColor (36): A packet matching the entry will be forwarded
                                           using a tunnel associated with the SR-TE policy endpoint and color.
         - rateLimitExtractedTraffic (38): Packet rate of packets extracted to CPM and
                                           matching the entry is limited to a value specified by
                                           tIPvXFltrEntryActRateLimit.
         - forwardSrv6Plcy           (39): A packet matching the entry will be forwarded
                                           using a tunnel associated with the SRv6 policy.
         - rateLimitPolicer          (40): Traffic matching the entry will be limited
                                           to the values specified in the tFltrPolicerTable entry
                                           with tFltrPolicerName equal to tIPvXFltrEntryActRateLimitPlcr."
    SYNTAX      INTEGER {
        drop                      (1),
        forward                   (2),
        httpRedirect              (4),
        nat                       (5),
        reassemble                (6),
        gtpLclBrkout              (7),
        forwardEsiL2              (8),
        forwardEsiL3              (9),
        ofPacketIn                (10),
        dropTtl                   (12),
        dropPktLen                (13),
        forwardRtr                (14),
        forwardNextHop            (15),
        forwardNextHopRtr         (16),
        forwardNHInterface        (17),
        forwardLsp                (18),
        forwardSdp                (19),
        forwardSap                (20),
        forwardRPlcy              (21),
        rateLimit                 (22),
        tcpMssAdjust              (23),
        remarkDscp                (24),
        rateLimitPktLen           (25),
        rateLimitTtl              (26),
        dropExtractedTraffic      (27),
        forwardVprnTarget         (28),
        forwardBondingConnection  (29),
        ignoreMatch               (30),
        forwardGreTunnel          (31),
        dropPattern               (32),
        rateLimitPattern          (33),
        forwardPattern            (34),
        forwardMplsPlcyEndpt      (35),
        forwardSrtePlcyEndptColor (36),
        httpRedirectCpf           (37),
        rateLimitExtractedTraffic (38),
        forwardSrv6Plcy           (39),
        rateLimitPolicer          (40)
    }

TFilterPbrTargetStatus           ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Status of PBR target :
         - unknown           (0): Status of PBR target is not tracked
         - doesNotExist      (1): The system does not know the PBR target.
         - up                (2): PBR target is known by the system and can be
                                  used for forwarding the traffic.
         - down              (3): PBR target is known by the system but can't be
                                  used for forwarding the traffic.
         - routerSpecific    (4): PBR target status depends on service where
                                  filter is applied."
    SYNTAX      INTEGER {
        unknown        (0),
        doesNotExist   (1),
        up             (2),
        down           (3),
        routerSpecific (4)
    }

TFilterDownloadedAction          ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Filter action downloaded to IOM:
         - none          (1): No filter entry action is downloaded to IOM.
                              Entry is inactive or filter is not applied.
         - primary       (2): Primary filter entry action is downloaded to IOM.
         - secondary     (3): Secondary filter entry action is downloaded to
                              IOM.
         - forward       (4): Neither primary nor secondary action is downloaded
                              to IOM. Action forward is downloaded to IOM.
         - drop          (5): Neither primary nor secondary action is downloaded
                              to IOM. Action drop is downloaded to IOM.
         - notDisplayed  (6): Field is not supported for configured action."
    SYNTAX      INTEGER {
        none         (1),
        primary      (2),
        secondary    (3),
        forward      (4),
        drop         (5),
        notDisplayed (6)
    }

TFilterEntryActionId             ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The textual convention TFilterEntryActionId specifies the unique
         identifier and also the priority of the action within the filter
         entry."
    SYNTAX      INTEGER {
        primary   (1),
        secondary (2)
    }

TMacFilterEntryAction            ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Action to take on a packet matching the filter entry:
         - drop              (1) : A packet matching the entry will be dropped.
         - forward           (2) : A packet matching the entry will be
                                   forwarded
                                   using regular routing.
         - httpRedirect      (4):  An HTTP GET packet matching the entry is
                                   forwarded to CPM for HTTP captive portal
                                   processing.
         - forwardEsiL2      (8):  A packet matching the entry will be forwarded
                                   to ESI identified first appliance in Nuage
                                   service chain using EVPN-resolved VXLAN
                                   tunnel in the specified VPLS service.
         - forwardSdp        (19): A packet matching the entry will be forwarded
                                   using the configured SDP.
         - forwardSap        (20): A packet matching the entry will be forwarded
                                   using the configured SAP.
         - rateLimit         (22): Traffic matching the entry will be limited to
                                   the value specified by the object
                                   tIPvXFltrEntryActRateLimit.
         - ignoreMatch       (30): Match criteria are skipped.
                                   "
    SYNTAX      INTEGER {
        drop         (1),
        forward      (2),
        httpRedirect (4),
        forwardEsiL2 (8),
        forwardSdp   (19),
        forwardSap   (20),
        rateLimit    (22),
        ignoreMatch  (30)
    }

TIPvXFilterEntryActionExt        ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Action to take on a packet:
         - none              (0) : This value indicates that no action
                                   is specified.
         - remarkDscp        (24): DSCP value of packets will be remarked.
                                   "
    SYNTAX      INTEGER {
        none       (0),
        remarkDscp (24)
    }

TFilterLogId                     ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Uniquely identifies an entry in the filter log table. 0 indicates an
         invalid log-id."
    SYNTAX      Unsigned32 (0 | 101..199)

TFilterLogDestination            ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Determines the location where filtered packets are logged."
    SYNTAX      INTEGER {
        memory (1),
        syslog (2),
        file   (3)
    }

TTimeRangeState                  ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The textual convention TTimeRangeState is used to indicate the state
         of an object that is controlled by a time range.
         - timeRangeNotApplic:
           no time range is applicable for this entry.
         - timeRangeNotActive:
           A time range is defined but is not active at this moment.
         - timeRangeActive.
           A time range is defined, and is activated successfully.
         - timeRangeActiveDownloadFailed:
           A time range is defined and is activated, but the corresponding
           object could not be installed due to resource problems."
    SYNTAX      INTEGER {
        timeRangeNotApplic            (0),
        timeRangeNotActive            (1),
        timeRangeActive               (2),
        timeRangeActiveDownloadFailed (3)
    }

TFilterLogSummaryCriterium       ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Indicates the field on which log summarization will be done.
         - when set to srcAddr, received log packets are summarized
           based on the src ip/mac-addr
         - when set to dstAddr, received log packets are summarized
           based on the dst ip/mac-addr"
    SYNTAX      INTEGER {
        srcAddr (0),
        dstAddr (1)
    }

TFilterType                      ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Type of filter."
    SYNTAX      INTEGER {
        fltrtypeselNone   (0),
        fltrtypeselIp     (1),
        fltrtypeselMac    (2),
        fltrtypeselCpm    (3),
        fltrtypeselIpv6   (4),
        fltrtypeselCpm6   (5),
        fltrtypeselCpmMac (6)
    }

TFilterSubInsSpaceOwner          ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Owner of a range of filter entries related to subscribers in an
         existing filter"
    SYNTAX      INTEGER {
        radius           (1),
        creditControl    (2),
        radiusSharedHost (6),
        pccRule          (8)
    }

TFltrGrpInsrtdEntriesApplication ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Application capable of inserting filter entries into an existing
         filter that supports regrouping of inserted entries"
    SYNTAX      INTEGER {
        none          (0),
        radius        (1),
        creditControl (2)
    }

TDHCPFilterID                    ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The identification number of a DHCP filter."
    SYNTAX      TFilterID

TDhcpFilterAction                ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Action to take on DHCP host creation when the filter entry matches.

         When set to none(1), host creation proceeds as normal.

         When set to bypass-host-creation(2), host creation is bypassed.

         When set to drop(3), the DHCP message is dropped. "
    SYNTAX      INTEGER {
        none                 (1),
        bypass-host-creation (2),
        drop                 (3)
    }

TDhcpFilterMatch                 ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Match condition for a DHCP option in a DHCP filter entry

         When set to present(1) the related DHCP option must be present, when
         set to absent(2) the related DHCP option must be absent.

         When set to string(3) the option must (partially) match a specified
         ASCII string, setting string-exact(4) requires an exact match, setting
         string-invert(5) requires the option not to (partially) match, setting
         string-exact-invert(6) requires the option not to match exact.

         Setting hex(7), hex-exact(8), hex-invert(9) or hex-exact-invert(10)
         will use a hex octet string for the matching."
    SYNTAX      INTEGER {
        present             (1),
        absent              (2),
        string              (3),
        string-exact        (4),
        string-invert       (5),
        string-exact-invert (6),
        hex                 (7),
        hex-exact           (8),
        hex-invert          (9),
        hex-exact-invert    (10)
    }

TFltrPrefixListType              ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The type TFltrPrefixListType enumerates all possible prefix list
         types."
    SYNTAX      INTEGER {
        ipv4 (1),
        ipv6 (2)
    }

TFltrPktLenListType              ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The type TFltrPktLenListType enumerates all possible packet length
         list types."
    SYNTAX      INTEGER {
        ipv4 (1),
        ipv6 (2)
    }

TFltrPolicerScope                ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The type TFltrPolicerScope enumerates all possible policer scope
         types."
    SYNTAX      INTEGER {
        system (1),
        filter (2)
    }

TmnxEmbeddedFltrOperState        ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TmnxEmbeddedFltrOperState data type is an enumerated integer that
         describes the current operational state of a filter embedding request."
    SYNTAX      INTEGER {
        embedFailedNoResources (-1),
        inactive               (0),
        active                 (1)
    }

TmnxEmbeddedFltrAdminState       ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TmnxEmbeddedFltrAdminState data type is an enumerated integer that
         describes the current administrative state of a filter embedding
         request."
    SYNTAX      INTEGER {
        inactive (0),
        active   (1)
    }

TmnxFltrEmbeddedEntryState       ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TmnxFltrEmbeddedEntryState data type is an enumerated integer that
         describes the current operational state of an embedded filter entry."
    SYNTAX      INTEGER {
        inserted            (1),
        overruled           (2),
        inactiveAdminDown   (3),
        inactiveNoResources (4)
    }

TmnxFilterApplyPathSource        ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TmnxFilterApplyPathSource data type is an enumerated integer that
         describes the source of the apply-path imported prefixes"
    SYNTAX      INTEGER {
        unknown   (0),
        bgp-peers (1)
    }

TFltrPortSelector                ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "This textual convention specifies how the source port and
         destination port filter objects are combined to form the filter match
         criterion.
         - If the selector takes the value and-port(0) then the source port
           and destination port objects (if set) are combined into 1 filter
           condition that fires if both conditions are met (i.e. a logical
           and-operation of both is done). If one of them is not set (default
           values) then only the other one is taken into account for the match
           condition.
         - If the selector takes the value or-port(1) then the source port
           objects are used as match condition for either source port or
           destination port (i.e. a logical or-operation is done). In this case,
           non-default values must be set for the source port objects. In this
           case the destination port objects are (silently) copied from the
           source port objects by the system; any other values set by the user
           are overwritten by the system."
    SYNTAX      INTEGER {
        and-port (0),
        or-port  (1)
    }

TFltrMatchIpSelector             ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "This textual convention specifies how the source ip and
         destination ip filter objects are combined to form the filter match
         criterion.
         - If the selector takes the value and-ip(0) then the source address
           and destination address objects (if set) are combined into 1 filter
           condition that fires if both conditions are met (i.e. a logical
           and-operation of both is done). If one of them is not set (default
           values) then only the other one is taken into account for the match
           condition.
         - If the selector takes the value or-ip(1) then the source ip
           objects are used as match condition for either source ip or
           destination ip (i.e. a logical or-operation is done). In this case,
           non-default values must be set for the source address objects. In this
           case the destination address objects are (silently) copied from the
           source address objects by the system; any other values set by the user
           are overwritten by the system."
    SYNTAX      INTEGER {
        and-ip (0),
        or-ip  (1)
    }

TFilterRPBindingOperator         ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "This textual convention specifies how the destinations in filter
         redirect policy binding are combined to form the operational state of
         the whole binding."
    SYNTAX      INTEGER {
        and (0),
        or  (1)
    }

TFilterPacketLength              ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TFilterPacketLength textual convention is used to specify the
         'Total Length' value of packet's IPv4 header or the 'Payload Length'
         value of packet's IPv6 header."
    SYNTAX      Unsigned32 (0..65535)

TFilterIpv6MatchPacketLength     ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TFilterPacketLength textual convention is used to specify the
         total length value of a packet"
    SYNTAX      Unsigned32 (0 | 40..65575)

TIPvXFilterPktLen                ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TIPvXFilterPktLen textual convention is used to specify the total
         length value of a packet as specified in packet length lists"
    SYNTAX      Unsigned32 (0..65575)

TFilterTTL                       ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TFilterTTL textual convention is used to specify a Time To Live
         (IPv4) or Hop Limit (IPv6) value."
    SYNTAX      Unsigned32 (0..255)

TmnxFilterRPlcyTestLastAction    ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TmnxFilterRPlcyTestLastAction textual convention is used to
         indicate the last impact of a test assigned to a destination of a
         redirect policy on an operational state of the destination.

         Value 'enable' indicates the operational state of the destination has
         been set to 'inService'.

         Value 'disable' indicates the operational state of the destination has
         been set to 'outOfService'.

         Value 'none' indicates the operational state of the destination has
         not been changed yet."
    SYNTAX      INTEGER {
        enable  (1),
        disable (2),
        none    (3)
    }

TmnxFilterRPlcyTestRespAction    ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The TmnxFilterRPlcyTestRespAction textual convention is used to
         indicate the action of a test assigned to a destination of a redirect
         policy on a operational priority of the destination.

         Value 'increase' indicates that if the response passes the test the
         operational priority of the destination will be increased.

         Value 'decrease' indicates that if the response passes the test the
         operational priority of the destination will be decreased.

         Value 'disable' indicates the test wont have impact on the operational
         priority of the destination."
    SYNTAX      INTEGER {
        increase (1),
        decrease (2),
        disable  (3)
    }

TFilterEgressPBR                 ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "disable         - 0: policy based routing has no effect when applied
                              on egress
         enable          - 1: egress policy based routing is allowed and default
                              load-balancing based on hash of source/destination
                              address of the packet is applied
         enableWithL4LB  - 2: egress policy based routing is allowed and
                              l4-load-balancing is applied (if available include
                              TCP/UDP port in hash."
    SYNTAX      INTEGER {
        disable        (0),
        enable         (1),
        enableWithL4LB (2)
    }

TFilterEsi                       ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Ethernet Segment Identifier (ESI) as defined in IETF draft
         BGP MPLS Based Ethernet VPN. ESI is a unique non-zero identifier that
         identifies an Ethernet Segment. ESI is encoded as a ten octets integer
         in line format with the most significant octet sent first.
         The following two ESI values are reserved:
             - ESI 0 denotes a single-homed CE.
             - ESI 0xFF repeated 10 times is known as MAX-ESI.

         In a network with managed and not-managed CEs, the ESI has the
         following format:

                      +---+---+---+---+---+---+---+---+---+---+
                      | T |          ESI Value                |
                      +---+---+---+---+---+---+---+---+---+---+

          Where:
          T (ESI Type) is a 1-octet field (most significant octet) that
          specifies the format of the remaining nine octets (ESI Value).
          ESI type can be one of the values 0x00-0x05."
    SYNTAX      OCTET STRING (SIZE (10))

TFilterEntryActionRateLimit      ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "A limiting rate in kilobits per second for traffic matching the filter
         entry. The value -1 means max rate."
    SYNTAX      Integer32 (-1 | 0..2000000000)

TFilterEntryActionRateLimitPps   ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "A limiting rate in packets per second for traffic matching the filter
         entry. The value -1 means max rate. The value -2 is a default value
         and means that a leaf of this type is not used."
    SYNTAX      Integer32 (-2 | -1 | 0..100000000)

TFilterPolicerPIR                ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "A limiting rate in kilobits per second for traffic matching the filter
         entry. The value -1 means that a leaf of this  type is not used."
    SYNTAX      Integer32 (-1 | 0..2000000000)

TFilterPolicerPPSPIR             ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "A limiting rate in packets per second for traffic matching the filter
         entry. The value -1 means that a leaf of this  type is not used."
    SYNTAX      Integer32 (-1 | 0..100000000)

TFilterEmbedOffset               ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Insertion offset of entries of an embedded filter into an embedding
         filter. An entry at position x in the embedded filter is inserted at
         position x + offset in the embedding filter."
    SYNTAX      Unsigned32 (0..2097151)

TIPvXFilterType                  ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Specifies the set of available match criteria for a filter policy.

         - normal                  (0): Allows all match criteria except:
                                        - Source MAC, Packet Length and Destination class.
         - srcMac                  (1): Allows matching Source MAC and all match criteria for type normal except:
                                        - Source IP, DSCP and all IP Options in IPv4 filters.
                                        - Source IP in IPv6 filters.
         - pktLen                  (2): Allows matching Packet length and all match criteria for type normal except:
                                        - DSCP and all IP Options in IPv4 filters.
                                        - Flow Label in IPv6 filters.
         - destClass               (3): Allows matching Destination class and all match criteria for type normal except:
                                        - DSCP and all IP Options in IPv4 filters.
                                        - Flow Label in IPv6 filters."
    SYNTAX      INTEGER {
        normal    (0),
        srcMac    (1),
        pktLen    (2),
        destClass (3)
    }

TmnxFilterCflowdSampleProfileId  ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Specifies a unique number that identifies a row in the
         tmnxCflowdSampleProfileEntry. Default value 0 means that no sample
         profile is applied with the given filter entry."
    SYNTAX      Unsigned32 (0 | 1..5)

tFilterObjects                   OBJECT IDENTIFIER ::= { tmnxSRObjs 21 }

tIPFilterTable                   OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIPFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Contains a List of all ip filters configured on this system."
    ::= { tFilterObjects 1 }

tIPFilterEntry                   OBJECT-TYPE
    SYNTAX      TIPFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular IP Filter entry. Entries are
         created/deleted  by user. Entries have a presumed StorageType of
         nonVolatile."
    INDEX       { tIPFilterId }
    ::= { tIPFilterTable 1 }

TIPFilterEntry                   ::= SEQUENCE
{
    tIPFilterId                      TAnyFilterID,
    tIPFilterRowStatus               RowStatus,
    tIPFilterScope                   TFilterScope,
    tIPFilterDescription             TItemDescription,
    tIPFilterDefaultAction           TFilterAction,
    tIPFilterRadiusInsertPt          TEntryIdOrZero,
    tIPFilterRadiusInsertSize        TEntryBlockSize,
    tIPFilterCreditCntrlInsertPt     TEntryIdOrZero,
    tIPFilterCreditCntrlInsertSize   TEntryBlockSize,
    tIPFilterSubInsertHighWmark      Integer32,
    tIPFilterSubInsertLowWmark       Integer32,
    tIpFilterCreditCntrlNbrInsertd   Unsigned32,
    tIpFilterRadiusNbrInsertd        Unsigned32,
    tIpFilterName                    TLNamedItemOrEmpty,
    tIPFilterHostSharedInsertPt      TEntryIdOrZero,
    tIPFilterHostSharedInsertSize    TEntryBlockSize,
    tIpFilterHostSharedNbrInsertd    Unsigned32,
    tIPFilterHostSharedHighWmark     Integer32,
    tIPFilterHostSharedLowWmark      Integer32,
    tIPFilterNbrHostSharedFltrs      Unsigned32,
    tIPFilterSharedPccRuleInsrtPt    TEntryIdOrZero,
    tIPFilterSharedPccRuleInsrtSize  TEntryBlockSize,
    tIPFilterSharedPccRuleNbrInsrtd  Unsigned32,
    tIPFilterChainToSystemFilter     TruthValue,
    tIPFilterType                    TIPvXFilterType,
    tIPFilterSharedPolicer           TruthValue
}

tIPFilterId                      OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterId uniquely identifies an ip filter.
         User-configured filters have values between (1..65535). Other values
         are reserved for filters that are created (auto-generated) by the
         system. Refer to the description of the textual convention
         TAnyFilterID for more details."
    ::= { tIPFilterEntry 1 }

tIPFilterRowStatus               OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted in the
         tIPFilterTable."
    ::= { tIPFilterEntry 2 }

tIPFilterScope                   OBJECT-TYPE
    SYNTAX      TFilterScope
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object specifies the scope of this filter definition."
    DEFVAL      { template }
    ::= { tIPFilterEntry 3 }

tIPFilterDescription             OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "User-provided description for this filter."
    DEFVAL      { ''H }
    ::= { tIPFilterEntry 4 }

tIPFilterDefaultAction           OBJECT-TYPE
    SYNTAX      TFilterAction
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The action to take for packets that do not match any filter entries.
         The only allowed values for this field are drop(1) and forward(2)."
    DEFVAL      { drop }
    ::= { tIPFilterEntry 5 }

tIPFilterRadiusInsertPt          OBJECT-TYPE
    SYNTAX      TEntryIdOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterRadiusInsertPt specifies at what place the host
         specific filter entries received from Radius will be inserted in the
         filter.

         The area defined here will be dedicated to those entries, no other
         entries will be allowed.

         The value 0 means that no Radius provided host specific filter entries
         can be inserted in the filter.

         If tIPFilterRadiusInsertSize is set to 0, then this object will be put
         to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPFilterEntry 6 }

tIPFilterRadiusInsertSize        OBJECT-TYPE
    SYNTAX      TEntryBlockSize
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterRadiusInsertSize specifies how many host
         specific filter entries received from Radius for subscriber hosts can
         be inserted in the filter.

         If tIPFilterRadiusInsertPt is set to 0, then this object will be put
         to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPFilterEntry 7 }

tIPFilterCreditCntrlInsertPt     OBJECT-TYPE
    SYNTAX      TEntryIdOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterCreditCntrlInsertPt specifies at what place the
         filter entries received from Credit Control for a particular
         subscriber host will be inserted in the filter.

         The area defined here will be dedicated to those entries, no other
         entries will be allowed.

         The value 0 means that no Credit Control provided filter entries can
         be inserted in the filter.

         If tIPFilterCreditCntrlInsertSize is set to 0, then this object will
         be put to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPFilterEntry 8 }

tIPFilterCreditCntrlInsertSize   OBJECT-TYPE
    SYNTAX      TEntryBlockSize
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterCreditCntrlInsertSize specifies how many filter
         entries received from Credit Control can be inserted in the filter.

         If tIPFilterCreditCntrlInsertPt is set to 0, then this object will be
         put to 0 as well. Any change attempts will result in error"
    DEFVAL      { 0 }
    ::= { tIPFilterEntry 9 }

tIPFilterSubInsertHighWmark      OBJECT-TYPE
    SYNTAX      Integer32 (0..100)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterSubInsertHighWmark specifies the
         utilization of the filter ranges for filter entry insertion, at which
         a table full alarm will be raised by the agent. The value 0 indicates
         that no alarm will be generated."
    DEFVAL      { 95 }
    ::= { tIPFilterEntry 10 }

tIPFilterSubInsertLowWmark       OBJECT-TYPE
    SYNTAX      Integer32 (0..100)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterSubInsertLowWmark specifies the
         utilization of the filter ranges for filter entry insertion, at which
         a table full alarm will be cleared by the agent."
    DEFVAL      { 90 }
    ::= { tIPFilterEntry 11 }

tIpFilterCreditCntrlNbrInsertd   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIpFilterCreditCntrlNbrInsertd indicates how
         many filter entries are currently inserted in the filter on request of
         credit control."
    ::= { tIPFilterEntry 12 }

tIpFilterRadiusNbrInsertd        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIpFilterRadiusNbrInsertd indicates how many
         host specific filter entries are currently inserted in the filter on
         request of RADIUS."
    ::= { tIPFilterEntry 13 }

tIpFilterName                    OBJECT-TYPE
    SYNTAX      TLNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIpFilterName specifies the name to associate with this
         filter."
    DEFVAL      { ''H }
    ::= { tIPFilterEntry 14 }

tIPFilterHostSharedInsertPt      OBJECT-TYPE
    SYNTAX      TEntryIdOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterHostSharedInsertPt specifies at what place the
         filter entries received from Radius that are shared between several
         hosts (host common rules) will be inserted in the filter.

         The area defined here will be dedicated to those entries, no other
         entries will be allowed.

         The value 0 means that no Radius provided host common filter entries
         can be inserted in the filter.

         If tIPFilterHostSharedInsertSize is set to 0, then this object will be
         put to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPFilterEntry 15 }

tIPFilterHostSharedInsertSize    OBJECT-TYPE
    SYNTAX      TEntryBlockSize
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterHostSharedInsertSize specifies how many host
         common filter entries received from Radius for subscriber hosts can be
         inserted in the filter.

         If tIPFilterHostSharedInsertPt is set to 0, then this object will be
         put to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPFilterEntry 16 }

tIpFilterHostSharedNbrInsertd    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIpFilterHostSharedNbrInsertd indicates how
         many Radius Shared Filter rules are inserted in the filter."
    ::= { tIPFilterEntry 17 }

tIPFilterHostSharedHighWmark     OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 1..8000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterHostSharedHighWmark specifies the
         number of Radius Shared Filters that can be dynamically created in the
         system before an high watermark notification is generated by the
         system. The value -1 specifies that no notifications are sent. If any
         of the watermarks (high or low) is set to -1, both watermarks will be
         set to -1 by the system."
    DEFVAL      { -1 }
    ::= { tIPFilterEntry 18 }

tIPFilterHostSharedLowWmark      OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..8000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterHostSharedLowWmark specifies the
         number of Radius Shared Filters that are still dynamically created in
         the system before an high watermark notification is cleared by the
         system. The value -1 specifies that no notifications are sent. If any
         of the watermarks (high or low) is set to -1, both watermarks will be
         set to -1 by the system."
    DEFVAL      { -1 }
    ::= { tIPFilterEntry 19 }

tIPFilterNbrHostSharedFltrs      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterNbrHostSharedFltrs indicates how many
         filters are currently created by Radius or Diameter based on this
         filter. (Both host shared or flow-rule filters.)"
    ::= { tIPFilterEntry 20 }

tIPFilterSharedPccRuleInsrtPt    OBJECT-TYPE
    SYNTAX      TEntryIdOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterSharedPccRuleInsrtPt specifies at what place the
         flow-rule filter entries that are received from Diameter and that are
         shared across several hosts will be inserted in the filter.

         The range defined here will be reserved for those entries; no other
         entries will be allowed in this range.

         The value 0 means that no flow-rule filter entries can be inserted in
         the filter by Diameter.

         If tIPFilterSharedPccRuleInsrtSize is set to 0 then
         tIPFilterSharedPccRuleInsrtPt is also set to 0 by the system.

         Note that the range reserved for shared flow-rule entries must not
         overlap with that of either
         tIPFilterRadiusInsertPt/tIPFilterRadiusInsertSize,
         tIPFilterCreditCntrlInsertPt/tIPFilterCreditCntrlInsertSize, or
         tIPFilterHostSharedInsertPt/tIPFilterHostSharedInsertSize"
    DEFVAL      { 0 }
    ::= { tIPFilterEntry 21 }

tIPFilterSharedPccRuleInsrtSize  OBJECT-TYPE
    SYNTAX      TEntryBlockSize
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterSharedPccRuleInsrtSize specifies how many
         flow-rule filter entries that are received from Diameter and that are
         shared across several hosts can be inserted in the filter.

         The range defined here will be reserved for those entries; no other
         entries will be allowed in this range.

         The value 0 means that no flow-rule filter entries can be inserted in
         the filter by Diameter.

         If tIPFilterSharedPccRuleInsrtPt is set to 0 then
         tIPFilterSharedPccRuleInsrtSize is also set to 0 by the system.

         Note that the range reserved for shared flow-rule entries must not
         overlap with that of either
         tIPFilterRadiusInsertPt/tIPFilterRadiusInsertSize,
         tIPFilterCreditCntrlInsertPt/tIPFilterCreditCntrlInsertSize, or
         tIPFilterHostSharedInsertPt/tIPFilterHostSharedInsertSize"
    DEFVAL      { 0 }
    ::= { tIPFilterEntry 22 }

tIPFilterSharedPccRuleNbrInsrtd  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterSharedPccRuleNbrInsrtd indicates how
         many flow-rule filter entries received from Diameter have been
         inserted in this filter"
    ::= { tIPFilterEntry 23 }

tIPFilterChainToSystemFilter     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterChainToSystemFilter specifies whether
         this filter policy is chained to the active IP system filter policy.

         The active IP system filter policy is defined as a row in
         tFilterSystemFilterTable that have the value of the object
         tFilterSystemFilterType set to 'fltrtypeselIp(1)'.

         The value 'true(1)' means this filter policy is chained to the active
         IP system filter policy. The system filter policy's rules are executed
         first before any rules of this filter policy are executed.

         The value of this object can be set to 'true(1)' only when the scope
         of this policy (value of the object tIPFilterScope) is 'exclusive(1)'
         or 'template(2)'.

         The value 'false(2)' means this filter policy is not chained to the
         active IP system filter policy."
    DEFVAL      { false }
    ::= { tIPFilterEntry 24 }

tIPFilterType                    OBJECT-TYPE
    SYNTAX      TIPvXFilterType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterType specifies the type of IP filter."
    DEFVAL      { normal }
    ::= { tIPFilterEntry 25 }

tIPFilterSharedPolicer           OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterSharedPolicer specifies whether the
         value of tIPvXFltrEntryActRateLimit will be shared among LAG active
         ports.

         When the value is 'true' and the filter policy is applied to a single
         LAG interface or multiple LAG interfaces then Filter Entry Rate Limit
         Value per FP = ((tIPvXFltrEntryActRateLimit) / (Nb Active Ports in the
         LAG)) * (Nb active ports in the LAG for this FP)

         When the value is 'false' then Filter Entry Rate Limit Value per FP =
         tIPvXFltrEntryActRateLimit."
    DEFVAL      { false }
    ::= { tIPFilterEntry 26 }

tIPFilterParamsTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIPFilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of all IP filter match entries for all IP filters."
    ::= { tFilterObjects 2 }

tIPFilterParamsEntry             OBJECT-TYPE
    SYNTAX      TIPFilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular IP Filter entry. Every IP Filter can
         have zero or more IP Filter match entries.

         A filter entry with no match criteria set will match every packet, and
         the entry action will be taken.

         Entries are created/deleted by user.

         Additional parameters can be found in tIPFilterParamsExtTable.

         There is no StorageType object, entries have a presumed StorageType of
         nonVolatile."
    INDEX       {
        tIPFilterId,
        tIPFilterParamsIndex
    }
    ::= { tIPFilterParamsTable 1 }

TIPFilterParamsEntry             ::= SEQUENCE
{
    tIPFilterParamsIndex             TEntryId,
    tIPFilterParamsRowStatus         RowStatus,
    tIPFilterParamsLogId             TFilterLogId,
    tIPFilterParamsDescription       TItemDescription,
    tIPFilterParamsAction            TFilterActionOrDefault,
    tIPFilterParamsForwardNH         IpAddress,
    tIPFilterParamsForwardNHIndirect TruthValue,
    tIPFilterParamsRemarkDSCP        TDSCPFilterActionValue,
    tIPFilterParamsRemarkDSCPMask    TDSCPFilterActionValue,
    tIPFilterParamsRemarkDot1p       Dot1PPriority,
    tIPFilterParamsSourceIpAddr      IpAddress,
    tIPFilterParamsSourceIpMask      IpAddressPrefixLength,
    tIPFilterParamsDestinationIpAddr IpAddress,
    tIPFilterParamsDestinationIpMask IpAddressPrefixLength,
    tIPFilterParamsProtocol          TIpProtocol,
    tIPFilterParamsSourcePortValue1  TTcpUdpPort,
    tIPFilterParamsSourcePortValue2  TTcpUdpPort,
    tIPFilterParamsSourcePortOperator TOperator,
    tIPFilterParamsDestPortValue1    TTcpUdpPort,
    tIPFilterParamsDestPortValue2    TTcpUdpPort,
    tIPFilterParamsDestPortOperator  TOperator,
    tIPFilterParamsDSCP              TDSCPNameOrEmpty,
    tIPFilterParamsFragment          TFragmentMatch,
    tIPFilterParamsOptionPresent     TItemMatch,
    tIPFilterParamsIpOptionValue     TIpOption,
    tIPFilterParamsIpOptionMask      TIpOption,
    tIPFilterParamsMultipleOption    TItemMatch,
    tIPFilterParamsTcpSyn            TItemMatch,
    tIPFilterParamsTcpAck            TItemMatch,
    tIPFilterParamsIcmpCode          TIcmpCodeOrNone,
    tIPFilterParamsIcmpType          TIcmpTypeOrNone,
    tIPFilterParamsCflowdSample      TruthValue,
    tIPFilterParamsCflowdIfSample    TruthValue,
    tIPFilterParamsForwardNHInterface DisplayString,
    tIPFilterParamsIngressHitCount   Counter64,
    tIPFilterParamsEgressHitCount    Counter64,
    tIPFilterParamsLogInstantiated   TruthValue,
    tIPFilterParamsForwardRedPlcy    TNamedItemOrEmpty,
    tIPFilterParamsActiveDest        IpAddress,
    tIPFilterParamsFwdSvcId          TmnxServId,
    tIPFilterParamsFwdSapPortId      TmnxPortID,
    tIPFilterParamsFwdSapEncapVal    TmnxEncapVal,
    tIPFilterParamsFwdSdpBind        SdpBindId,
    tIPFilterParamsTimeRangeName     TNamedItemOrEmpty,
    tIPFilterParamsTimeRangeState    TTimeRangeState,
    tIPFilterParamsRedirectURL       TmnxHttpRedirectUrl,
    tIPFilterParamsSrcIpFullMask     IpAddress,
    tIPFilterParamsDestIpFullMask    IpAddress,
    tIPFilterParamsIngrHitByteCount  Counter64,
    tIPFilterParamsEgrHitByteCount   Counter64,
    tIPFilterParamsFwdRtrId          TmnxVRtrIDOrZero,
    tIPFilterParamsSrcRouteOption    TItemMatch,
    tIPFilterParamsSrcIpPrefixList   TNamedItemOrEmpty,
    tIPFilterParamsDstIpPrefixList   TNamedItemOrEmpty,
    tIPFilterParamsPortSelector      TFltrPortSelector,
    tIPFilterParamsSrcPortList       TNamedItemOrEmpty,
    tIPFilterParamsDstPortList       TNamedItemOrEmpty,
    tIPFilterParamsRdirAllwRadOvrd   TruthValue,
    tIPFilterParamsNatPolicyName     TNamedItemOrEmpty,
    tIPFilterParamsFwdLsp            TmnxVRtrMplsLspID,
    tIPFilterParamsFwdLspRtrId       TmnxVRtrIDOrZero,
    tIPFilterParamsIpSelector        TFltrMatchIpSelector
}

tIPFilterParamsIndex             OBJECT-TYPE
    SYNTAX      TEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This is the secondary index for the entry. Every ip filter can have
         multiple entries, therefore every ip filter entry is identified by the
         tIPFilterId and tIPFilterParamsIndex."
    ::= { tIPFilterParamsEntry 1 }

tIPFilterParamsRowStatus         OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted in the
         tIPFilterParamsTable."
    ::= { tIPFilterParamsEntry 2 }

tIPFilterParamsLogId             OBJECT-TYPE
    SYNTAX      TFilterLogId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object specifies the log to use for packets that match this
         entry. The value zero indicates that logging is disabled."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 3 }

tIPFilterParamsDescription       OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "User-provided description for this filter entry."
    DEFVAL      { ''H }
    ::= { tIPFilterParamsEntry 4 }

tIPFilterParamsAction            OBJECT-TYPE
    SYNTAX      TFilterActionOrDefault
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The action to take for packets that match this filter entry. The value
         default(3) specifies this entry to inherit the behavior defined as the
         default for the filter.

         Setting the values 'forwardEsiL2' and 'forwardEsiL3' explicitly is
         ignored by the system. The values 'forwardEsiL2'(8) and
         'forwardEsiL3'(9) can be set only implicitly by specifying non default
         values of objects specifying parameters for these actions. In such
         case the value of tIPFilterParamsAction will be set to
         'forwardEsiL2'(8) or 'forwardEsiL3'(9) automatically by system.

         The object tIPFilterParamsAction supports only subset of filter
         actions. The object tIPvXFltrEntryActAction supports all actions. It's
         recommended to use tIPvXFltrEntryActAction instead of
         tIPFilterParamsAction."
    DEFVAL      { ignoreMatch }
    ::= { tIPFilterParamsEntry 5 }

tIPFilterParamsForwardNH         OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The IP address of the nexthop to which the packet should be forwarded
         if it hits this filter entry. The action of this entry should be
         'forward' in such a case.

         Note that the value of tIPFilterParamsForwardNH is silently cleared by
         the system if tIPFilterParamsAction is set to value other than
         'forward'(2), or any object related to 'forward' other than
         tIPFilterParamsForwardNH, tIPFilterParamsForwardNHIndirect or
         tIPFilterParamsFwdRtrId is set."
    DEFVAL      { '00000000'H }
    ::= { tIPFilterParamsEntry 6 }

tIPFilterParamsForwardNHIndirect OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPFilterParamsForwardNHIndirect specifies if the nexthop is directly/
         indirectly reachable.

         Note that the value of tIPFilterParamsForwardNHIndirect is silently
         cleared by the system if tIPFilterParamsAction is set to value other
         than 'forward'(2), or any object related to 'forward' other than
         tIPFilterParamsForwardNH, tIPFilterParamsForwardNHIndirect or
         tIPFilterParamsFwdRtrId is set."
    DEFVAL      { false }
    ::= { tIPFilterParamsEntry 7 }

tIPFilterParamsRemarkDSCP        OBJECT-TYPE
    SYNTAX      TDSCPFilterActionValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The DSCP value that should be remarked in case a packet hits this
         filter entry."
    DEFVAL      { -1 }
    ::= { tIPFilterParamsEntry 8 }

tIPFilterParamsRemarkDSCPMask    OBJECT-TYPE
    SYNTAX      TDSCPFilterActionValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPFilterParamsRemarkDSCPMask specifies the care bits while remarking
         with the DSCP value."
    DEFVAL      { 255 }
    ::= { tIPFilterParamsEntry 9 }

tIPFilterParamsRemarkDot1p       OBJECT-TYPE
    SYNTAX      Dot1PPriority
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPFilterParamsRemarkDot1p specifies the Dot1p value that needs to be
         remarked on the packet if it hits this filter entry."
    DEFVAL      { -1 }
    ::= { tIPFilterParamsEntry 10 }

tIPFilterParamsSourceIpAddr      OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "IP address to match the source IP address of the packet."
    DEFVAL      { '00000000'H }
    ::= { tIPFilterParamsEntry 11 }

tIPFilterParamsSourceIpMask      OBJECT-TYPE
    SYNTAX      IpAddressPrefixLength
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the object tIPFilterParamsSourceIpMask specifies
         the IP Mask value for this policy IP Filter entry. The mask is ANDed
         with the received source IP address to match the
         tIPFilterParamsSourceIpAddr.

         If the value of tIPFilterParamsSourceIpMask is 0, and the value of
         tIPFilterParamsSrcIpFullMask is non zero then the value of
         tIPFilterParamsSrcIpFullMask is used as mask.

         If the value of tIPFilterParamsSourceIpMask is non zero, it will be
         equal to the mask expressed the object tIPFilterParamsSrcIpFullMask.

         If both tIPFilterParamsSourceIpMask and tIPFilterParamsSrcIpFullMask
         are set to 0, no matching is done on the source IP address.

         If a value is specified for this object, then the value of the object
         tIPFilterParamsSrcIpFullMask will be set to reflect this same mask."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 12 }

tIPFilterParamsDestinationIpAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "IP address to match the destination IP address of the packet."
    DEFVAL      { '00000000'H }
    ::= { tIPFilterParamsEntry 13 }

tIPFilterParamsDestinationIpMask OBJECT-TYPE
    SYNTAX      IpAddressPrefixLength
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the object tIPFilterParamsDestinationIpMask
         specifies the IP Mask value for this policy IP Filter entry. The mask
         is ANDed with the received Destination IP address to match the
         tIPFilterParamsDestinationIpAddr.

         If the value of tIPFilterParamsDestinationIpMask is 0, and the value
         of tIPFilterParamsDestIpFullMask is non zero then the value of
         tIPFilterParamsDestIpFullMask is used as mask.

         If the value of tIPFilterParamsDestinationIpMask is non zero, it will
         be equal to the mask expressed the object
         tIPFilterParamsDestIpFullMask.

         If both tIPFilterParamsDestinationIpMask and
         tIPFilterParamsDestIpFullMask are set to 0, no matching is done on the
         Destination IP address.

         If a value is specified for this object, then the value of the object
         tIPFilterParamsDestIpFullMask will be set to reflect this same mask."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 14 }

tIPFilterParamsProtocol          OBJECT-TYPE
    SYNTAX      TIpProtocol
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "IP protocol to match. Set to -1 to disable matching IP protocol."
    DEFVAL      { -1 }
    ::= { tIPFilterParamsEntry 15 }

tIPFilterParamsSourcePortValue1  OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "TCP/UDP port value1. The value of this object is used as per the
         description for tIPFilterParamsSourcePortOperator."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 16 }

tIPFilterParamsSourcePortValue2  OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "TCP/UDP port value2. The value of this object is used as per the
         description for tIPFilterParamsSourcePortOperator."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 17 }

tIPFilterParamsSourcePortOperator OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The operator specifies the manner in which
         tIPFilterParamsSourcePortValue1 and tIPFilterParamsSourcePortValue2
         are to be used. The value of these latter 2 objects and
         tIPFilterParamsSourcePortOperator is used as described in
         TTcpUdpPortOperator."
    DEFVAL      { none }
    ::= { tIPFilterParamsEntry 18 }

tIPFilterParamsDestPortValue1    OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "TCP/UDP port value1. The value of this object is used as per the
         description for tIPFilterParamsDestPortOperator."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 19 }

tIPFilterParamsDestPortValue2    OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "TCP/UDP port value2.

         The value of this object is used as per the description for
         tIPFilterParamsDestPortOperator."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 20 }

tIPFilterParamsDestPortOperator  OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The operator specifies the manner in which
         tIPFilterParamsDestPortValue1 and tIPFilterParamsDestPortValue2 are to
         be used. The value of these latter 2 objects and
         tIPFilterParamsDestPortOperator is used as described in
         TTcpUdpPortOperator."
    DEFVAL      { none }
    ::= { tIPFilterParamsEntry 21 }

tIPFilterParamsDSCP              OBJECT-TYPE
    SYNTAX      TDSCPNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "DSCP to be matched on the packet."
    DEFVAL      { ''H }
    ::= { tIPFilterParamsEntry 22 }

tIPFilterParamsFragment          OBJECT-TYPE
    SYNTAX      TFragmentMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If enabled, this object matches fragmented/unfragmented packets as per
         the value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsEntry 24 }

tIPFilterParamsOptionPresent     OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If enabled, this object matches packets if they have options present
         or not as per the value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsEntry 25 }

tIPFilterParamsIpOptionValue     OBJECT-TYPE
    SYNTAX      TIpOption
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the specific IP option to match."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 26 }

tIPFilterParamsIpOptionMask      OBJECT-TYPE
    SYNTAX      TIpOption
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Mask is ANDed with the IP option before being compared to
         tIPFilterParamsIpOptionValue."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 27 }

tIPFilterParamsMultipleOption    OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If enabled, matches multiple options as per the value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsEntry 28 }

tIPFilterParamsTcpSyn            OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Syn as per value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsEntry 29 }

tIPFilterParamsTcpAck            OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Ack as per value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsEntry 30 }

tIPFilterParamsIcmpCode          OBJECT-TYPE
    SYNTAX      TIcmpCodeOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "ICMP code to be matched.

         The value -1 means ICMP code matching is not enabled."
    DEFVAL      { -1 }
    ::= { tIPFilterParamsEntry 31 }

tIPFilterParamsIcmpType          OBJECT-TYPE
    SYNTAX      TIcmpTypeOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "ICMP type to be matched.

         The value -1 means ICMP type matching is not enabled."
    DEFVAL      { -1 }
    ::= { tIPFilterParamsEntry 32 }

tIPFilterParamsCflowdSample      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When tIPFilterParamsCflowdSample has a value of 'true',  Cflowd
         sampling and analysis is performed on those packet streams where this
         filter has been applied.  Only packets matching this IP filter entry
         are subjected to Cflowd sampling and analysis.  A Cflowd profile
         controls the sampling and analysis of data flows through the router."
    DEFVAL      { false }
    ::= { tIPFilterParamsEntry 33 }

tIPFilterParamsCflowdIfSample    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When tIPFilterParamsCflowdIfSample has a value of 'true', Cflowd
         sampling and analysis is performed on those packet streams where this
         filter has been applied.  Only packets matching this IP filter entry
         are subjected to Cflowd sampling and analysis.  A Cflowd profile
         controls the sampling and analysis of data flows through the router."
    DEFVAL      { true }
    ::= { tIPFilterParamsEntry 34 }

tIPFilterParamsForwardNHInterface OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The interface name for the nexthop to which the packet should be
         forwarded if it hits this filter entry. The action of this entry
         should be 'forward' in such a case.

         Note that the value of tIPFilterParamsForwardNHInterface is silently
         cleared  by the system if tIPFilterParamsAction is set to value other
         than 'forward'(2) or any object related to 'forward' other than
         this one is set."
    DEFVAL      { ''H }
    ::= { tIPFilterParamsEntry 35 }

tIPFilterParamsIngressHitCount   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the number of times an ingress packet matched
         this entry."
    ::= { tIPFilterParamsEntry 36 }

tIPFilterParamsEgressHitCount    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the number of times an egress packet matched
         this entry."
    ::= { tIPFilterParamsEntry 37 }

tIPFilterParamsLogInstantiated   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tIPFilterParamsLogInstantiated indicates if the filter log for this
         filter entry has been instantiated or not."
    ::= { tIPFilterParamsEntry 38 }

tIPFilterParamsForwardRedPlcy    OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPFilterParamsForwardRedPlcy specifies the redirect policy to be used
         to determine the nexthop.

         Note that the value of tIPFilterParamsForwardRedPlcy is silently
         cleared  by the system if tIPFilterParamsAction is set to value other
         than 'forward'(2) or any object related to 'forward' other than
         this one is set."
    DEFVAL      { ''H }
    ::= { tIPFilterParamsEntry 39 }

tIPFilterParamsActiveDest        OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tIPFilterParamsActiveDest indicates the IP address of the active
         destination for this IP filter. A value of 0 indicates that there is
         currently no active destination."
    ::= { tIPFilterParamsEntry 40 }

tIPFilterParamsFwdSvcId          OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tIPFilterParamsFwdSvcId indicates the service id of the destination
         for this IP filter entry. A value of 0 indicates that there is
         currently no active SAP or SDP destination."
    ::= { tIPFilterParamsEntry 41 }

tIPFilterParamsFwdSapPortId      OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPFilterParamsFwdSapPortId specifies the sap port identity of the
         destination for this IP filter entry.

         A value of 0 indicates that there is currently no SAP destination
         defined. A value different from 0 can only be specified if the value
         of the tIPFilterParamsAction object of this entry is 'forward'. In
         addition a non-zero value can only be given if the object
         tIPFilterParamsFwdSdpBind has a zero value.

         Note that the value of tIPFilterParamsFwdSapPortId is silently cleared
         by the system if tIPFilterParamsAction is set to value other than
         'forward'(2) or any object related to 'forward' other than
         tIPFilterParamsFwdSapPortId, tIPFilterParamsFwdSapEncapVal is set."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 42 }

tIPFilterParamsFwdSapEncapVal    OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPFilterParamsFwdSapEncapVal specifies the sap port encap value of
         the destination SAP for this IP filter entry.

         A value different from 0 can only be specified if the value of the
         tIPFilterParamsAction object of this entry is 'forward'.  In addition
         a non-zero value can only be given if the object
         tIPFilterParamsFwdSdpBind has a zero value. A value of 0 indicates
         that either
         1) the sap encapsulation value is not specified when
            tIPFilterParamsFwdSapPortId and tIPFilterParamsFwdSvcId
            have valid values; or
         2) that there is no SAP destination.

         Note that the value of tIPFilterParamsFwdSapEncapVal is silently
         cleared  by the system if tIPFilterParamsAction is set to value other
         than 'forward'(2) or any object related to 'forward' other than
         tIPFilterParamsFwdSapPortId or tIPFilterParamsFwdSapEncapVal is set."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 43 }

tIPFilterParamsFwdSdpBind        OBJECT-TYPE
    SYNTAX      SdpBindId
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPFilterParamsFwdSdpBind specifies the sdp bind identity of the
         destination for this IP filter entry.

         A value of 0 indicates that there is currently no SDP binding defined.
         A value different from 0 can only be specified if the value of the
         tIPFilterParamsAction object of this entry is 'forward'. In addition a
         non-zero value can only be given if the objects
         tIPFilterParamsFwdSapPortId and tIPFilterParamsFwdSapEncapVal have a
         zero value.

         Note that the value of tIPFilterParamsFwdSdpBind is silently cleared
         by the system if tIPFilterParamsAction is set to value other than
         'forward'(2) or any object related to 'forward' other than this one is
         set."
    DEFVAL      { '0000000000000000'H }
    ::= { tIPFilterParamsEntry 44 }

tIPFilterParamsTimeRangeName     OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPFilterParamsTimeRangeName specifies the tmnxTimeRangeEntry to be
         associated with this filter entry.

         A value for this object can only be specified during row creation, and
         cannot be altered later on. Also, a value is accepted only if the
         tmnxTimeRangeEntry is defined in the
         TIMETRA-SCHEDULER-MIB::tmnxTimeRangeTable.tTimeRangeName.

         This object is obsoleted in release 14.0."
    DEFVAL      { ''H }
    ::= { tIPFilterParamsEntry 45 }

tIPFilterParamsTimeRangeState    OBJECT-TYPE
    SYNTAX      TTimeRangeState
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tIPFilterParamsTimeRangeState indicates whether or not the entry
         is currently in effect.
         - timeRangeNotApplic:
           no time range is applicable for this entry.
         - timeRangeNotActive:
           A time range is defined in tIPFilterParamsTimeRangeName, but is not
           active at this moment. Consequently the filter entry is not
           installed.
         - timeRangeActive.
           A time range is defined in tIPFilterParamsTimeRangeName, and is
           activated successfully.
         - timeRangeActiveDownloadFailed:
           A time range is defined in tIPFilterParamsTimeRangeName, and is
           activated, but the corresponding filter entry could not be
           installed due to resource problems.

         This object is obsoleted in release 14.0."
    ::= { tIPFilterParamsEntry 46 }

tIPFilterParamsRedirectURL       OBJECT-TYPE
    SYNTAX      TmnxHttpRedirectUrl
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tIPFilterParamsRedirectURL specifies the URL to redirect
         to, when the value of tIPFilterParamsAction is 'httpRedirect'.

         The following macro substitutions are applicable in this context:
         $URL, $MAC, $IP, $SUB, $SAP, $SAPDESC, $CID, and $RID.

         Note that the value of tIPFilterParamsRedirectURL is silently cleared
         by the system if tIPFilterParamsAction is set to any value other than
         httpRedirect."
    DEFVAL      { ''H }
    ::= { tIPFilterParamsEntry 47 }

tIPFilterParamsSrcIpFullMask     OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the object tIPFilterParamsSrcIpFullMask specifies
         the IP Mask value for this policy IP Filter entry. The mask is ANDed
         with the received Source IP address to match the
         tIPFilterParamsSourceIpAddr.

         If the value of tIPFilterParamsSourceIpMask is non zero, it will be
         equal to the mask expressed the object tIPFilterParamsSrcIpFullMask.

         If both tIPFilterParamsSourceIpMask and tIPFilterParamsSrcIpFullMask
         are set to 0, no matching is done on the Source IP address.

         This object should contain consecutive ones and zeros. Both a regular
         and an inverse mask is allowed (i.e. the sequence of consecutive ones
         can appear at the front or at the end of the mask).

         If a regular mask is specified for tIPFilterParamsSrcIpFullMask then
         the value of tIPFilterParamsSourceIpMask will be changed to reflect
         this value. If an inverse is specified, the value of
         tIPFilterParamsSourceIpMask will be set to 0."
    DEFVAL      { '0000'H }
    ::= { tIPFilterParamsEntry 48 }

tIPFilterParamsDestIpFullMask    OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the object tIPFilterParamsDestIpFullMask
         specifies the IP Mask value for this policy IP Filter entry. The mask
         is ANDed with the received Destination IP address to match the
         tIPFilterParamsDestinationIpAddr.

         If the value of tIPFilterParamsDestinationIpMask is non zero, it will
         be equal to the mask expressed the object
         tIPFilterParamsDestIpFullMask.

         If both tIPFilterParamsDestinationIpMask and
         tIPFilterParamsDestIpFullMask are set to 0, no matching is done on the
         Destination IP address.

         This object should contain consecutive ones and zeros. Both a regular
         and an inverse mask is allowed (i.e. the sequence of consecutive ones
         can appear at the front or at the end of the mask).

         If a regular mask is specified for tIPFilterParamsDestIpFullMask then
         the value of tIPFilterParamsDestinationIpMask will be changed to
         reflect this value. If an inverse is specified, the value of
         tIPFilterParamsDestinationIpMask will be set to 0."
    DEFVAL      { '0000'H }
    ::= { tIPFilterParamsEntry 49 }

tIPFilterParamsIngrHitByteCount  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterParamsIngrHitByteCount indicates the number of
         bytes of all ingress packets that matched this entry."
    ::= { tIPFilterParamsEntry 50 }

tIPFilterParamsEgrHitByteCount   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterParamsEgrHitByteCount indicates the number of
         bytes of all egress packets that matched this entry."
    ::= { tIPFilterParamsEntry 51 }

tIPFilterParamsFwdRtrId          OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPFilterParamsFwdRtrId specifies, if different from '0', the router
         id into which the packet should be forwarded if it hits this filter
         entry.

         The action of this entry should be 'forward' in such a case.

         Note that the value of tIPFilterParamsFwdRtrId is silently cleared by
         the system if tIPFilterParamsAction is set to value other than
         'forward'(2) or any object related to 'forward' other than
         tIPFilterParamsFwdRtrId, tIPFilterParamsForwardNH or
         tIPFilterParamsForwardNHIndirect is set."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 52 }

tIPFilterParamsSrcRouteOption    OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "tIPFilterParamsSrcRouteOption specifies, when enabled, that this
         filter should match if a (strict or loose) source route option is
         present/not present at any location within the IP header, as per the
         value of this object."
    DEFVAL      { off }
    ::= { tIPFilterParamsEntry 53 }

tIPFilterParamsSrcIpPrefixList   OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the IP prefix list used as match
         criterion for the source IP address.

         The value specified for this object must correspond to a prefix list
         defined in tFilterPrefixListTable.

         If the value of this object is empty then the values of the objects
         tIPFilterParamsSourceIpAddr and tIPFilterParamsSourceIpMask are used
         as source IP address match criterion.

         When this object is set to a non-empty value then the objects
         tIPFilterParamsSourceIpAddr and tIPFilterParamsSourceIpMask are reset
         to their default values by the system.

         Vice versa, when a new (non-default) value is provided for the objects
         tIPFilterParamsSourceIpAddr and tIPFilterParamsSourceIpMask then this
         object is reset to its default (empty) value by the system.

         An attempt to set tIPFilterParamsSrcIpPrefixList to a non-default
         value in combination with setting any of tIPFilterParamsSourceIpAddr
         or tIPFilterParamsSourceIpMask to (a) non-default value(s) is rejected
         by the system"
    DEFVAL      { ''H }
    ::= { tIPFilterParamsEntry 54 }

tIPFilterParamsDstIpPrefixList   OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the IP prefix list used as match
         criterion for the destination IP address.

         The value specified for this object must correspond to a prefix list
         defined in tFilterPrefixListTable.

         If the value of this object is empty then the values of the objects
         tIPFilterParamsDestinationIpAddr and tIPFilterParamsDestinationIpMask
         are used as destination IP address match criterion.

         When this object is set to a non-empty value then the objects
         tIPFilterParamsDestinationIpAddr and tIPFilterParamsDestinationIpMask
         are reset to their default values by the system.

         Vice versa, when a new (non-default) value is provided for the objects
         tIPFilterParamsDestinationIpAddr and tIPFilterParamsDestinationIpMask
         then this object is reset to its default (empty) value by the system.

         An attempt to set tIPFilterParamsDstIpPrefixList to a non-default
         value in combination with setting any of
         tIPFilterParamsDestinationIpAddr or tIPFilterParamsDestinationIpMask
         to (a) non-default value(s) is rejected by the system"
    DEFVAL      { ''H }
    ::= { tIPFilterParamsEntry 55 }

tIPFilterParamsPortSelector      OBJECT-TYPE
    SYNTAX      TFltrPortSelector
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object specifies how the source port objects
         (tIPFilterParamsSourcePortValue1, tIPFilterParamsSourcePortValue2,
         tIPFilterParamsSourcePortOperator, tIPFilterParamsSrcPortList) and
         destination port objects (tIPFilterParamsDestPortValue1,
         tIPFilterParamsDestPortValue2, tIPFilterParamsDestPortOperator,
         tIPFilterParamsDstPortList) are combined to form the filter match
         criterion. See description of TFltrPortSelector."
    DEFVAL      { and-port }
    ::= { tIPFilterParamsEntry 56 }

tIPFilterParamsSrcPortList       OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the port-list used as match
         criterion for the source port.

         The value specified for this object must correspond to a port-list
         defined in tFilterPortListTable.

         If the value of this object is empty then the values of the objects
         tIPFilterParamsSourcePortValue1, tIPFilterParamsSourcePortValue2, and
         tIPFilterParamsSourcePortOperator are used as source port match
         criterion.

         When this object is set to a non-empty value then the objects
         tIPFilterParamsSourcePortValue1, tIPFilterParamsSourcePortValue2, and
         tIPFilterParamsSourcePortOperator are reset to their default values by
         the system.

         Vice versa, when a new (non-default) value is provided for one of the
         objects tIPFilterParamsSourcePortValue1,
         tIPFilterParamsSourcePortValue2, or tIPFilterParamsSourcePortOperator
         then tIPFilterParamsSrcPortList is reset to its default (empty) value
         by the system.

         Setting any one of the objects tIPFilterParamsSourcePortValue1,
         tIPFilterParamsSourcePortValue2, or tIPFilterParamsSourcePortOperator
         to a non-default value in combination with a non-default value for the
         object tIPFilterParamsSrcPortList is rejected by the system."
    DEFVAL      { ''H }
    ::= { tIPFilterParamsEntry 57 }

tIPFilterParamsDstPortList       OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the port-list used as match
         criterion for the destination port.

         The value specified for this object must correspond to a port-list
         defined in tFilterPortListTable.

         If the value of this object is empty then the values of the objects
         tIPFilterParamsDestPortValue1, tIPFilterParamsDestPortValue2, and
         tIPFilterParamsDestPortOperator are used as destination port match
         criterion.

         When this object is set to a non-empty value then the objects
         tIPFilterParamsDestPortValue1, tIPFilterParamsDestPortValue2, and
         tIPFilterParamsDestPortOperator are reset to their default values by
         the system.

         Vice versa, when a new (non-default) value is provided for one of the
         objects tIPFilterParamsDestPortValue1, tIPFilterParamsDestPortValue2,
         or tIPFilterParamsDestPortOperator then tIPFilterParamsDstPortList is
         reset to its default (empty) value by the system.

         Setting any one of the objects tIPFilterParamsDestPortValue1,
         tIPFilterParamsDestPortValue2, or tIPFilterParamsDestPortOperator to a
         non-default value in combination with a non-default value for the
         object tIPFilterParamsDstPortList is rejected by the system."
    DEFVAL      { ''H }
    ::= { tIPFilterParamsEntry 58 }

tIPFilterParamsRdirAllwRadOvrd   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of this object specifies whether or not the value of
         tIPFilterParamsRedirectURL can be overridden by a Radius VSA. The
         default value is false (i.e. the URL cannot be overridden by Radius).
         The value of tIPFilterParamsRdirAllwRadOvrd is relevant only if the
         value of tIPFilterParamsAction is httpRedirect.

         Setting the value of tIPFilterParamsRdirAllwRadOvrd to true is ignored
         by the system if the value of tIPFilterParamsAction is not
         httpRedirect. Furthermore, the value of tIPFilterParamsRdirAllwRadOvrd
         is silently reset to false by the system if tIPFilterParamsAction is
         set to any value other than httpRedirect."
    DEFVAL      { false }
    ::= { tIPFilterParamsEntry 59 }

tIPFilterParamsNatPolicyName     OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of this object specifies the name of the NAT policy to be
         used when the value of tIPFilterParamsAction is nat. If the value is
         empty then a default policy is used. If the value is non-empty then it
         must correspond to a policy defined in tmnxNatPlcyTable.

         The value of tIPFilterParamsNatPolicyName is relevant only if the
         value of tIPFilterParamsAction is nat. Setting the value of
         tIPFilterParamsNatPolicyName to a non-empty string is ignored by the
         system if the value of tIPFilterParamsAction is not nat.

         Furthermore, the value of tIPFilterParamsNatPolicyName is silently
         reset to an empty string by the system if tIPFilterParamsAction is set
         to any value other than nat."
    DEFVAL      { "" }
    ::= { tIPFilterParamsEntry 60 }

tIPFilterParamsFwdLsp            OBJECT-TYPE
    SYNTAX      TmnxVRtrMplsLspID
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "If different from zero the value of the object tIPFilterParamsFwdLsp
         together with the value of the object tIPFilterParamsFwdLspRtrId
         specifies the LSP into which a packet should be forwarded if it hits
         this filter entry.

         The value of the object tIPFilterParamsAction of this entry must be
         'forward' in such case. Otherwise the value of the object
         tIPFilterParamsFwdLsp is ignored by the system.

         Note that the value of tIPFilterParamsFwdLsp is reset to '0' by the
         system if tIPFilterParamsAction is set to value other than
         'forward'(2) or any object related to 'forward' other than
         tIPFilterParamsFwdLsp or tIPFilterParamsFwdLspRtrId is set.

         The value of the object tIPFilterParamsFwdLsp cannot be set to a
         non-zero value if other destinations are already specified.

         The value has to be '0' if the value of the object
         tIPFilterParamsFwdLspRtrId is not set (i.e. is '0').

         If a non-zero value is set, the value of the object
         tIPFilterParamsFwdLspRtrId has to be set as well."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 61 }

tIPFilterParamsFwdLspRtrId       OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsFwdLspRtrId specifies the
         router ID that the LSP ID defined by the value of the object
         tIPFilterParamsFwdLsp belongs to.

         The value of the object tIPFilterParamsAction of this entry must be
         'forward' in such case. Otherwise the value of the object
         tIPFilterParamsFwdLspRtrId is ignored by the system.

         Note that the value of tIPFilterParamsFwdLspRtrId is reset to '0' by
         the system if tIPFilterParamsAction is set to value other than
         'forward'(2) or any object related to 'forward' other than
         tIPFilterParamsFwdLsp or tIPFilterParamsFwdLspRtrId is set.

         The value of this object cannot be set to a non-zero value if other
         destinations are already specified.

         The value has to be '0' if the value of the object
         tIPFilterParamsFwdLsp is not set (i.e. is '0').

         If a non-zero value is set, the value of the object
         tIPFilterParamsFwdLsp has to be set as well.

         The ID of the base router or '0' are the only allowed value with this
         version of the product."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsEntry 62 }

tIPFilterParamsIpSelector        OBJECT-TYPE
    SYNTAX      TFltrMatchIpSelector
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsIpSelector specifies how the
         source address objects (tIPFilterParamsSourceIpAddr,
         tIPFilterParamsSourceIpMask, tIPFilterParamsSrcIpFullMask,
         tIPFilterParamsSrcIpPrefixList) and destination address objects
         (tIPFilterParamsDestinationIpAddr, tIPFilterParamsDestinationIpMask,
         tIPFilterParamsDestIpFullMask, tIPFilterParamsDstIpPrefixList) are
         combined to form the filter match criterion. See description of
         TFltrMatchIpSelector."
    DEFVAL      { and-ip }
    ::= { tIPFilterParamsEntry 63 }

tMacFilterTable                  OBJECT-TYPE
    SYNTAX      SEQUENCE OF TMacFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Contains a List of all mac filters configured on this system."
    ::= { tFilterObjects 3 }

tMacFilterEntry                  OBJECT-TYPE
    SYNTAX      TMacFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular MAC Filter. Entries are created/deleted
         by user. Entries have a presumed StorageType of nonVolatile."
    INDEX       { tMacFilterId }
    ::= { tMacFilterTable 1 }

TMacFilterEntry                  ::= SEQUENCE
{
    tMacFilterId                     TAnyFilterID,
    tMacFilterRowStatus              RowStatus,
    tMacFilterScope                  TFilterScope,
    tMacFilterDescription            TItemDescription,
    tMacFilterDefaultAction          TFilterAction,
    tMacFilterType                   TMacFilterType,
    tMacFilterName                   TLNamedItemOrEmpty
}

tMacFilterId                     OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Uniquely identifies a mac filter as configures on this system.

         Values outside of range 1..65535 are reserved for entries dynamically
         created by the system and cannot be used in any SNMP SET operation."
    ::= { tMacFilterEntry 1 }

tMacFilterRowStatus              OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted in the
         tMacFilterTable."
    ::= { tMacFilterEntry 2 }

tMacFilterScope                  OBJECT-TYPE
    SYNTAX      TFilterScope
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object specifies the scope of this filter definition.

         The value 'system(4)' is not supported."
    DEFVAL      { template }
    ::= { tMacFilterEntry 3 }

tMacFilterDescription            OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "User-provided description for this filter."
    DEFVAL      { ''H }
    ::= { tMacFilterEntry 4 }

tMacFilterDefaultAction          OBJECT-TYPE
    SYNTAX      TFilterAction
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The action to take for packets that do not match any filter entries.
         The only allowed values for this field are drop(1) and forward(2)."
    DEFVAL      { drop }
    ::= { tMacFilterEntry 5 }

tMacFilterType                   OBJECT-TYPE
    SYNTAX      TMacFilterType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "tMacFilterType specifies which type of entries this mac filter can
         contain.

         If tMacFilterType is set to 'normal(1)', all match criteria are
         accepted except the criteria mentioned below that belong to type
         isid(2) and vid(3).

         If tMacFilterType is set to 'isid(2)' the only accepted match
         criteria for the filter entries are:
         - tMacFilterParamsLowISID
         - tMacFilterParamsHighISID

         If tMacFilterType is set to vid(3) the only accepted match
         criteria for the filter entries are:
         - tMacFilterParamsInnerTagValue
         - tMacFilterParamsInnerTagMask
         - tMacFilterParamsOuterTagValue
         - tMacFilterParamsOuterTagMask

         tMacFilterType can only be changed if the filter is not applied and
         has no entries."
    DEFVAL      { normal }
    ::= { tMacFilterEntry 6 }

tMacFilterName                   OBJECT-TYPE
    SYNTAX      TLNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterName specifies the name to associate with this
         filter."
    DEFVAL      { ''H }
    ::= { tMacFilterEntry 7 }

tMacFilterParamsTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF TMacFilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of all MAC filter match entries for all MAC filters."
    ::= { tFilterObjects 4 }

tMacFilterParamsEntry            OBJECT-TYPE
    SYNTAX      TMacFilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular MAC Filter entry. Every MAC Filter can
         have zero or more MAC Filter match entries.

         A filter entry with no match criteria set will match every packet, and
         the entry action will be taken.

         Entries are created/deleted by user.

         There is no StorageType object, entries have a presumed StorageType of
         nonVolatile."
    INDEX       {
        tMacFilterId,
        tMacFilterParamsIndex
    }
    ::= { tMacFilterParamsTable 1 }

TMacFilterParamsEntry            ::= SEQUENCE
{
    tMacFilterParamsIndex            TEntryId,
    tMacFilterParamsRowStatus        RowStatus,
    tMacFilterParamsLogId            TFilterLogId,
    tMacFilterParamsDescription      TItemDescription,
    tMacFilterParamsAction           TFilterActionOrDefault,
    tMacFilterParamsFrameType        TFrameType,
    tMacFilterParamsSrcMAC           MacAddress,
    tMacFilterParamsSrcMACMask       MacAddress,
    tMacFilterParamsDstMAC           MacAddress,
    tMacFilterParamsDstMACMask       MacAddress,
    tMacFilterParamsDot1pValue       Dot1PPriority,
    tMacFilterParamsDot1pMask        Dot1PPriority,
    tMacFilterParamsEtherType        Integer32,
    tMacFilterParamsDsap             ServiceAccessPoint,
    tMacFilterParamsDsapMask         ServiceAccessPoint,
    tMacFilterParamsSsap             ServiceAccessPoint,
    tMacFilterParamsSsapMask         ServiceAccessPoint,
    tMacFilterParamsSnapPid          Integer32,
    tMacFilterParamsSnapOui          INTEGER,
    tMacFilterParamsIngressHitCount  Counter64,
    tMacFilterParamsEgressHitCount   Counter64,
    tMacFilterParamsLogInstantiated  TruthValue,
    tMacFilterParamsFwdSvcId         TmnxServId,
    tMacFilterParamsFwdSapPortId     TmnxPortID,
    tMacFilterParamsFwdSapEncapVal   TmnxEncapVal,
    tMacFilterParamsFwdSdpBind       SdpBindId,
    tMacFilterParamsTimeRangeName    TNamedItemOrEmpty,
    tMacFilterParamsTimeRangeState   TTimeRangeState,
    tMacFilterParamsRedirectURL      TmnxHttpRedirectUrl,
    tMacFilterParamsIngrHitByteCount Counter64,
    tMacFilterParamsEgrHitByteCount  Counter64,
    tMacFilterParamsLowISID          SvcISID,
    tMacFilterParamsHighISID         SvcISID,
    tMacFilterParamsInnerTagValue    QTagFullRangeOrNone,
    tMacFilterParamsInnerTagMask     QTagFullRange,
    tMacFilterParamsOuterTagValue    QTagFullRangeOrNone,
    tMacFilterParamsOuterTagMask     QTagFullRange,
    tMacFilterParamsEsi              TFilterEsi,
    tMacFilterParamsFwdEsiSvcId      TmnxServId,
    tMacFilterParamsPbrDwnActOvr     TFilterPbrDownActionOvr,
    tMacFilterParamsStickyDst        Integer32,
    tMacFilterParamsHoldRemain       Integer32,
    tMacFilterParamsDownloadAct      TFilterDownloadedAction,
    tMacFilterParamsCollectStats     TruthValue
}

tMacFilterParamsIndex            OBJECT-TYPE
    SYNTAX      TEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This is the secondary index for the entry. Every mac filter can have
         multiple entries, therefore every mac filter entry is identified by
         the tMacFilterId and tMacFilterParamsIndex."
    ::= { tMacFilterParamsEntry 1 }

tMacFilterParamsRowStatus        OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted in the
         tMacFilterParamsTable."
    ::= { tMacFilterParamsEntry 2 }

tMacFilterParamsLogId            OBJECT-TYPE
    SYNTAX      TFilterLogId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object specifies the log to use for packets that match this
         entry. The value zero indicates that logging is disabled."
    DEFVAL      { 0 }
    ::= { tMacFilterParamsEntry 3 }

tMacFilterParamsDescription      OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "User-provided description for this filter entry."
    DEFVAL      { ''H }
    ::= { tMacFilterParamsEntry 4 }

tMacFilterParamsAction           OBJECT-TYPE
    SYNTAX      TFilterActionOrDefault
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The action to take for packets that match this filter entry. The value
         default(3) specifies this entry to inherit the behavior defined as the
         default for the filter. The values nat(5), reassemble(6),
         gtpLclBrkout(7) and forwardEsiL3(9) are not allowed.

         The object tMacFilterParamsAction supports only subset of filter
         actions. The object tMacFltrEntryActAction supports all actions. It's
         recommended to use tMacFltrEntryActAction instead of
         tMacFilterParamsAction."
    DEFVAL      { ignoreMatch }
    ::= { tMacFilterParamsEntry 5 }

tMacFilterParamsFrameType        OBJECT-TYPE
    SYNTAX      TFrameType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The type of mac frame for which we are defining this match criteria.

         For filter entries in a MAC filter of type tMacFilterType = dot1q or
         tMacFilterType qinq the default value for this object is set to
         ethernetII (3), and no changes are allowed. In all other cases the
         default value is set to e802dot3 (0) "
    DEFVAL      { e802dot3 }
    ::= { tMacFilterParamsEntry 6 }

tMacFilterParamsSrcMAC           OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Source MAC to match for this policy MAC filter entry."
    DEFVAL      { '000000000000'H }
    ::= { tMacFilterParamsEntry 8 }

tMacFilterParamsSrcMACMask       OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Source MAC mask value for this policy MAC filter entry. The mask is
         ANDed with the MAC to match tMacFilterParamsSrcMAC. A cleared bit
         means ignore this bit, do not match. A set bit means match this bit
         with tMacFilterParamsSrcMAC. Use the value 00-00-00-00-00-00 to
         disable this filter criteria."
    DEFVAL      { '000000000000'H }
    ::= { tMacFilterParamsEntry 9 }

tMacFilterParamsDstMAC           OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Destination MAC mask value for this policy MAC filter entry."
    DEFVAL      { '000000000000'H }
    ::= { tMacFilterParamsEntry 10 }

tMacFilterParamsDstMACMask       OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Destination MAC mask value for this policy MAC filter entry. The mask
         is ANDed with the MAC to match tMacFilterParamsDstMAC. A cleared bit
         means ignore this bit, do not match. A set bit means match this bit
         with tMacFilterParamsDstMAC. Use the value 00-00-00-00-00-00 to
         disable this filter criteria."
    DEFVAL      { '000000000000'H }
    ::= { tMacFilterParamsEntry 11 }

tMacFilterParamsDot1pValue       OBJECT-TYPE
    SYNTAX      Dot1PPriority
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "IEEE 802.1p priority value for this policy MAC filter entry. Use -1 to
         disable matching this filter criteria."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 12 }

tMacFilterParamsDot1pMask        OBJECT-TYPE
    SYNTAX      Dot1PPriority (0..7)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "IEEE 802.1p priority mask value for this policy MAC filter entry. Use
         zero to disable matching, use 7 to match everything."
    DEFVAL      { 0 }
    ::= { tMacFilterParamsEntry 13 }

tMacFilterParamsEtherType        OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 1536..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Ethertype for this policy MAC filter entry. Use -1 to disable matching
         by this criteria. This object has no significance if the object
         tMacFilterParamsFrameType is not set to Ethernet_II."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 14 }

tMacFilterParamsDsap             OBJECT-TYPE
    SYNTAX      ServiceAccessPoint
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "MAC DSAP to match for this policy MAC filter entry. This object has no
         significance if the object tMacFilterParamsFrameType is not set to
         802dot2LLC. In order to reset the value to the default value, both
         objects tMacFilterParamsDsap and tMacFilterParamsDsapMask need to be
         modified together to the default value."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 15 }

tMacFilterParamsDsapMask         OBJECT-TYPE
    SYNTAX      ServiceAccessPoint
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "MAC DSAP mask for this policy MAC filter entry. Use 0 to disable
         matching by this criteria. This object has no significance if the
         object tMacFilterParamsFrameType is not set to 802dot2LLC. In order to
         reset the value to the default value, both objects
         tMacFilterParamsDsap and tMacFilterParamsDsapMask need to be modified
         together to the default value."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 16 }

tMacFilterParamsSsap             OBJECT-TYPE
    SYNTAX      ServiceAccessPoint
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "MAC SSAP to match for this policy MAC filter entry. This object has no
         significance if the object tMacFilterParamsFrameType is not set to
         802dot2LLC. In order to reset the value to the default value, both
         objects tMacFilterParamsSsap and tMacFilterParamsSsapMask need to be
         modified together to the default value."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 17 }

tMacFilterParamsSsapMask         OBJECT-TYPE
    SYNTAX      ServiceAccessPoint
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "MAC SSAP mask for this policy MAC filter entry. Use 0 to disable
         matching by this criteria. This object has no significance if the
         object tMacFilterParamsFrameType is not set to 802dot2LLC. In order to
         reset the value to the default value, both objects
         tMacFilterParamsSsap and tMacFilterParamsSsapMask need to be modified
         together to the default value."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 18 }

tMacFilterParamsSnapPid          OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "MAC SNAP PID to match for this policy MAC filter entry.  Use -1 to
         disable matching by this criteria. This object has no significance if
         object tMacFilterParamsFrameType is not set to 802dot2SNAP."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 19 }

tMacFilterParamsSnapOui          OBJECT-TYPE
    SYNTAX      INTEGER {
        off     (1),
        zero    (2),
        nonZero (3)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "MAC SNAP OUI to match. The values zero(2) and nonZero(3) specify what
         to match. Matching can be disabled by the use of the value off(1).
         This object has no significance if the object
         tMacFilterParamsFrameType is not set to 802dot2SNAP."
    DEFVAL      { off }
    ::= { tMacFilterParamsEntry 20 }

tMacFilterParamsIngressHitCount  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the number of times an ingress packet matched
         this entry."
    ::= { tMacFilterParamsEntry 21 }

tMacFilterParamsEgressHitCount   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the number of times an egress packet matched
         this entry."
    ::= { tMacFilterParamsEntry 22 }

tMacFilterParamsLogInstantiated  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tMacFilterParamsLogInstantiated indicates if the filter log for this
         filter entry has been instantiated or not."
    ::= { tMacFilterParamsEntry 23 }

tMacFilterParamsFwdSvcId         OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tMacFilterParamsFwdSvcId indicates the service id of the destination
         for this MAC filter entry. A value of 0 indicates that there is
         currently no active SAP or SDP destination."
    ::= { tMacFilterParamsEntry 24 }

tMacFilterParamsFwdSapPortId     OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tMacFilterParamsFwdSapPortId specifies the sap port identity of the
         destination for this MAC filter entry. A value of 0 indicates that
         there is currently no SAP destination defined. A value different from
         0 can only be specified if the value of the tMacFilterParamsAction
         object of this entry is 'forward'. In addition a non-zero value can
         only be given if the object tMacFilterParamsFwdSdpBind has a zero
         value.

         Note that the value of tMacFilterParamsFwdSapPortId is silently
         cleared by the system if tMacFilterParamsAction is set to value other
         than 'forward'(2), or any object related to 'forward' other than
         tMacFilterParamsFwdSvcId, tMacFilterParamsFwdSapPortId or
         tMacFilterParamsFwdSapEncapVal is set."
    DEFVAL      { 0 }
    ::= { tMacFilterParamsEntry 25 }

tMacFilterParamsFwdSapEncapVal   OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tMacFilterParamsFwdSapEncapVal specifies the sap port encap value
         of the destination SAP for this MAC filter entry.
         A value different from 0 can only be specified if
         the tMacFilterParamsFwdSapPortId object has a non zero value,
         and if the value of the tMacFilterParamsAction object of this entry
         is 'forward'. In addition a non-zero value can only be given if
         the object tMacFilterParamsFwdSdpBind has a zero value.
         A value of 0 indicates that either
         1) the sap encapsulation value is not specified when
            tMacFilterParamsFwdSapPortId and tMacFilterParamsFwdSvcId
            have valid values; or
         2) that there is no SAP destination.

         Note that the value of tMacFilterParamsFwdSapEncapVal is silently
         cleared by the system if tMacFilterParamsAction is set to value other
         than 'forward'(2), or any object related to 'forward' other than
         tMacFilterParamsFwdSvcId, tMacFilterParamsFwdSapPortId or
         tMacFilterParamsFwdSapEncapVal is set."
    DEFVAL      { 0 }
    ::= { tMacFilterParamsEntry 26 }

tMacFilterParamsFwdSdpBind       OBJECT-TYPE
    SYNTAX      SdpBindId
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tMacFilterParamsFwdSdpBind specifies the sdp bind identity of the
         destination for this MAC filter entry. A value of 0 indicates that
         there is currently no SDP binding defined. A value different from 0
         can only be specified if the value of the tMacFilterParamsAction
         object of this entry is 'forward'. In addition a non-zero value can
         only be given if the objects tMacFilterParamsFwdSapPortId and
         tMacFilterParamsFwdSapEncapVal have a zero value.

         Note that the value of tMacFilterParamsFwdSdpBind is silently cleared
         by the system if tMacFilterParamsAction is set to value other than
         'forward'(2), or any object related to 'forward' other than
         tMacFilterParamsFwdSvcId or tMacFilterParamsFwdSdpBind is set."
    DEFVAL      { '0000000000000000'H }
    ::= { tMacFilterParamsEntry 27 }

tMacFilterParamsTimeRangeName    OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tMacFilterParamsTimeRangeName specifies the tmnxTimeRangeEntry to be
         associated with this filter entry.

         A value for this object can only be specified during row creation, and
         cannot be altered later on. Also, a value is accepted only if the
         tmnxTimeRangeEntry is defined in the
         TIMETRA-SCHEDULER-MIB::tmnxTimeRangeTable.tTimeRangeName.

         This object is obsoleted in release 14.0."
    DEFVAL      { ''H }
    ::= { tMacFilterParamsEntry 28 }

tMacFilterParamsTimeRangeState   OBJECT-TYPE
    SYNTAX      TTimeRangeState
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tMacFilterParamsTimeRangeState indicates whether or not the entry
         is currently in effect.
         - timeRangeNotApplic:
           no time range is applicable for this entry.
         - timeRangeNotActive:
           A time range is defined in tMacFilterParamsTimeRangeName, but is not
           active at this moment. Consequently the filter entry is not
           installed.
         - timeRangeActive.
           A time range is defined in tMacFilterParamsTimeRangeName, and is
           activated successfully.
         - timeRangeActiveDownloadFailed:
           A time range is defined in tMacFilterParamsTimeRangeName, and is
           activated, but the corresponding filter entry could not be
           installed due to resource problems.

         This object is obsoleted in release 14.0."
    ::= { tMacFilterParamsEntry 29 }

tMacFilterParamsRedirectURL      OBJECT-TYPE
    SYNTAX      TmnxHttpRedirectUrl
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tMacFilterParamsRedirectURL specifies the URL to redirect
         to, when the value of tMacFilterParamsAction is 'httpRedirect'.

         Note that the value of tMacFilterParamsRedirectURL is silently cleared
         by the system if tMacFilterParamsAction is set to any value other than
         'httpRedirect'."
    DEFVAL      { ''H }
    ::= { tMacFilterParamsEntry 30 }

tMacFilterParamsIngrHitByteCount OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterParamsIngrHitByteCount indicates the number of
         bytes of all ingress packets that matched this entry."
    ::= { tMacFilterParamsEntry 31 }

tMacFilterParamsEgrHitByteCount  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterParamsEgrHitByteCount indicates the number of
         bytes of all egress packets that matched this entry."
    ::= { tMacFilterParamsEntry 32 }

tMacFilterParamsLowISID          OBJECT-TYPE
    SYNTAX      SvcISID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterParamsLowISID specifies the lowest value of the
         24 bit (0..16777215) service instance identifier for this service that
         matches this entry.

         The default value of -1 indicates no ISID matching will be performed.

         The value of this field can be equal to but not lower than the value
         of the tMacFilterParamsHighISID field.

         Changing the value of this field might also change the value of
         tMacFilterParamsHighISID: A value of -1 will change the value of
         tMacFilterParamsHighISID to -1. Changing the value of this field from
         -1 to any other value will change the value of
         tMacFilterParamsHighISID to this same value.

         Note that tMacFilterParamsLowISID and tMacFilterParamsHighISID can
         only be set if tMacFilterType is set to 'isid(1)'."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 33 }

tMacFilterParamsHighISID         OBJECT-TYPE
    SYNTAX      SvcISID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterParamsHighISID specifies the highest value of
         the 24 bit (0..16777215) service instance identifier for this service
         that matches this entry.

         The default value of -1 indicates no ISID matching will be performed.

         The value of this field can be equal to but not higher than the value
         of the tMacFilterParamsLowISID field.

         Changing the value of this field might also change the value of
         tMacFilterParamsLowISID: A value of -1 will change the value of
         tMacFilterParamsLowISID to -1. Changing the value of this field from
         -1 to any other value will change the value of tMacFilterParamsLowISID
         to this same value.

         Note that tMacFilterParamsLowISID and tMacFilterParamsHighISID can
         only be set if tMacFilterType is set to 'isid(1)'."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 34 }

tMacFilterParamsInnerTagValue    OBJECT-TYPE
    SYNTAX      QTagFullRangeOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterParamsInnerTagValue specifies the value to
         match against the VID of the second VLAN tag in the packet that is
         carried transparently through the service (the second vlan tag after
         the service delimiting tags).

         This object can only be set if tMacFilterType is set to 'vid(3)'.

         The (default) value of '-1' indicates no inner VLAN tag matching will
         be performed."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 35 }

tMacFilterParamsInnerTagMask     OBJECT-TYPE
    SYNTAX      QTagFullRange (1..4095)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterParamsInnerTagMask is applied as a mask to VID
         of the inner VLAN tag of the packet prior to comparing it
         with tMacFilterParamsInnerTagValue.  The inner tag is the second tag in
         the packet that is carried transparently through the service
         (the second tag after the service delimiting tags).

         This object can only be set if tMacFilterType is set to 'vid(3)'."
    DEFVAL      { 4095 }
    ::= { tMacFilterParamsEntry 36 }

tMacFilterParamsOuterTagValue    OBJECT-TYPE
    SYNTAX      QTagFullRangeOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterParamsOuterTagValue specifies the value to
         match against the VID of the first VLAN tag in the packet that is
         carried transparently through the service (the first vlan tag after
         the service delimiting tags).

         This object can only be set if tMacFilterType is set to 'vid(3)'.

         The (default) value of '-1' indicates no outer VLAN tag matching will
         be performed."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 37 }

tMacFilterParamsOuterTagMask     OBJECT-TYPE
    SYNTAX      QTagFullRange (1..4095)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterParamsOuterTagMask is applied as a mask to VID
         of the outer VLAN tag of the packet prior to comparing it
         with tMacFilterParamsOuterTagValue.  The outer tag is the first tag in
         the packet that is carried transparently through the service
         (the first tag after the service delimiting tags).

         This object can only be set if tMacFilterType is set to 'vid(3)'."
    DEFVAL      { 4095 }
    ::= { tMacFilterParamsEntry 38 }

tMacFilterParamsEsi              OBJECT-TYPE
    SYNTAX      TFilterEsi
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tMacFilterParamsEsi specifies the ethernet
         segment identifier (ESI) of the first ESI identified appliance in
         Nuage service chain. When the value of tMacFilterParamsAction is
         'forwardEsiL2' packets matching the filter entry are forwarded to the
         appliance using EVPN-resolved VXLAN tunnel in the specified VPLS
         service (tMacFilterParamsFwdEsiSvcId).

         The value '0' indicates that there is no ESI specified. The value of
         tMacFilterParamsEsi is ignored by the system if the value of
         tMacFilterParamsAction is different from 'forwardEsiL2'. The value of
         tMacFilterParamsAction can be set to 'forwardEsiL2' only if
         tMacFilterParamsEsi and tMacFilterParamsFwdEsiSvcId are set to non
         zero values."
    DEFVAL      { '00000000000000000000'H }
    ::= { tMacFilterParamsEntry 39 }

tMacFilterParamsFwdEsiSvcId      OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tMacFilterParamsFwdEsiSvcId specifies the
         identifier of the VPLS used for VPN/DC connectivity.

         The value '0' indicates that no VPLS identifier is specified. The
         value of tMacFilterParamsFwdEsiSvcId is ignored by the system if the
         value of tMacFilterParamsAction is different from 'forwardEsiL2'. The
         value of tMacFilterParamsAction can be set to 'forwardEsiL2' only if
         tMacFilterParamsEsi and tMacFilterParamsFwdEsiSvcId are set to non
         zero values."
    DEFVAL      { 0 }
    ::= { tMacFilterParamsEntry 40 }

tMacFilterParamsPbrDwnActOvr     OBJECT-TYPE
    SYNTAX      TFilterPbrDownActionOvr
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFilterParamsPbrDwnActOvr specifies the
         filter action which will be performed when the PBR/PBF target for this
         entry is not available.

         If the value of tMacFltrEntryActAction is not one of the following
         values then tMacFilterParamsPbrDwnActOvr must be set to the value
         'none':
         - forwardEsiL2
         - forwardSap
         - forwardSdp

         If the value of tMacFilterParamsPbrDwnActOvr is different from 'none'
         then PBF destination availability checking for an entry is turned on.
         There is a limit to the number of filter entries with the destination
         availability checking turned on. Entries with the value of
         tMacFltrEntryActAction equal to 'forwardEsiL2' are not counted against
         this limit.

         Refer to the description of the textual convention
         TFilterPbrDownActionOvr for more details."
    DEFVAL      { none }
    ::= { tMacFilterParamsEntry 41 }

tMacFilterParamsStickyDst        OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFilterParamsStickyDst specifies how long
         the system will wait (in seconds) until it activates the best action
         (action with available PBF destination and the highest priority).
         Until then the action specified by tMacFilterParamsPbrDwnActOvr will
         be taken on a packet matching the filter entry. After the value of the
         active destination is fixed it will remain unchanged until the active
         PBF destination becomes unreachable.

         The value of -1 indicates that the property of PBF destination
         stickiness is turned off. When the property of stickiness is turned
         off the active PBF destination is always the one which is available
         and has the highest priority.

         The countdown starts when there was no PBR/PBF destination reachable
         and any PBR/PBF destination becomes reachable.

         tMacFilterParamsStickyDst can be set to value other than -1 only if
         the value of tMacFltrEntryActAction is 'forwardSap' or 'forwardSdp'."
    DEFVAL      { -1 }
    ::= { tMacFilterParamsEntry 42 }

tMacFilterParamsHoldRemain       OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFilterParamsHoldRemain indicates the
         remaining time in seconds, until the best action will become active
         and will be fixed.

         Best action is:
         - primary action if PBR target status of primary action is up.
         - secondary action if PBR target status of secondary action is up
           and PBR target status of primary action is down.
         - none if both PBR targets are down"
    ::= { tMacFilterParamsEntry 43 }

tMacFilterParamsDownloadAct      OBJECT-TYPE
    SYNTAX      TFilterDownloadedAction
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFilterParamsDownloadAct indicates the
         filter entry action downloaded to IOM.

         Refer to the description of the textual convention
         TFilterDownloadedAction for more information."
    ::= { tMacFilterParamsEntry 44 }

tMacFilterParamsCollectStats     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterParamsCollectStats specifies whether or not the
         collection of statistical data for the filter entry is enabled.

         tMacFilterParamsCollectStats is supported only on IXR J2 platforms."
    DEFVAL      { false }
    ::= { tMacFilterParamsEntry 45 }

tFilterLogTable                  OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterLogEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of all filter logs."
    ::= { tFilterObjects 5 }

tFilterLogEntry                  OBJECT-TYPE
    SYNTAX      TFilterLogEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular Filter Log entry."
    INDEX       { tFilterLogId }
    ::= { tFilterLogTable 1 }

TFilterLogEntry                  ::= SEQUENCE
{
    tFilterLogId                     TFilterLogId,
    tFilterLogRowStatus              RowStatus,
    tFilterLogDestination            TFilterLogDestination,
    tFilterLogDescription            TItemDescription,
    tFilterLogMaxNumEntries          Unsigned32,
    tFilterLogSysLogId               Unsigned32,
    tFilterLogFileId                 Unsigned32,
    tFilterLogStopOnFull             TruthValue,
    tFilterLogEnabled                TmnxAdminStateTruthValue,
    tFilterLogSummaryEnabled         TmnxAdminStateTruthValue,
    tFilterLogSummaryCrit1           TFilterLogSummaryCriterium
}

tFilterLogId                     OBJECT-TYPE
    SYNTAX      TFilterLogId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This is the index for the entry. An entry cannot be created with an id
         of 0."
    ::= { tFilterLogEntry 1 }

tFilterLogRowStatus              OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted in the
         tFilterLogTable."
    ::= { tFilterLogEntry 2 }

tFilterLogDestination            OBJECT-TYPE
    SYNTAX      TFilterLogDestination
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object specifies the destination of the log."
    DEFVAL      { memory }
    ::= { tFilterLogEntry 3 }

tFilterLogDescription            OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "User-provided description for this filter log entry."
    DEFVAL      { ''H }
    ::= { tFilterLogEntry 4 }

tFilterLogMaxNumEntries          OBJECT-TYPE
    SYNTAX      Unsigned32 (0..50000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterLogMaxNumEntries specifies the maximum number of
         entries that the log can store.

         The value of tFilterLogMaxNumEntries can be set to any value other
         than zero only if tFilterLogDestination is 'memory'."
    DEFVAL      { 1000 }
    ::= { tFilterLogEntry 5 }

tFilterLogSysLogId               OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterLogSysLogId specifies the syslog Id to be used as
         destination.

         The value of tFilterLogSysLogId can be set to any value other than
         zero only if tFilterLogDestination is 'syslog'."
    DEFVAL      { 0 }
    ::= { tFilterLogEntry 6 }

tFilterLogFileId                 OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterLogFileId specifies the File Id to be used as
         destination.

         The value of tFilterLogFileId can be set to any value other than zero
         only if tFilterLogDestination is 'file'."
    DEFVAL      { 0 }
    ::= { tFilterLogEntry 7 }

tFilterLogStopOnFull             OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterLogStopOnFull specifies what should
         happen when tFilterLogMaxNumEntries is reached. The value true,
         specifies that logging will stop. The value false specifies that
         wrap-around will be used."
    DEFVAL      { false }
    ::= { tFilterLogEntry 8 }

tFilterLogEnabled                OBJECT-TYPE
    SYNTAX      TmnxAdminStateTruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterLogEnabled specifies whether the
         logging is enabled or disabled"
    DEFVAL      { true }
    ::= { tFilterLogEntry 9 }

tFilterLogSummaryEnabled         OBJECT-TYPE
    SYNTAX      TmnxAdminStateTruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tFilterLogSummaryEnabled specifies whether or not
         summarization of filter log entries is performed. Summarization is
         only allowed in case tFilterLogDestination is set to syslog."
    DEFVAL      { false }
    ::= { tFilterLogEntry 10 }

tFilterLogSummaryCrit1           OBJECT-TYPE
    SYNTAX      TFilterLogSummaryCriterium
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tFilterLogSummaryCrit1 specifies how filter log entries
         will be summarized.

         This field is only meaningful if the object tFilterLogSummaryEnabled
         is set to true."
    DEFVAL      { srcAddr }
    ::= { tFilterLogEntry 11 }

tFilterLogScalars                OBJECT IDENTIFIER ::= { tFilterObjects 6 }

tFilterLogMaxInstances           OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tFilterLogMaxInstances maintains the maximum allowed instances of
         filter logs allowed on the system"
    ::= { tFilterLogScalars 1 }

tFilterLogInstances              OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tFilterLogInstances maintains the instances of filter logs presently
         existing on the system"
    ::= { tFilterLogScalars 2 }

tFilterLogBindings               OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tFilterLogBindings maintains the count of the configured filter log
         bindings presently existing on the system. The bindings get
         instantiated when the filter is instantiated"
    ::= { tFilterLogScalars 3 }

tFilterNotificationObjects       OBJECT IDENTIFIER ::= { tFilterObjects 8 }

tFilterPBRDropReason             OBJECT-TYPE
    SYNTAX      INTEGER {
        invalidInterface (0),
        interfaceDown    (1)
    }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "Used by tIPFilterPBRPacketsDrop to report the failure reason code."
    ::= { tFilterNotificationObjects 1 }

tFilterParmRow                   OBJECT-TYPE
    SYNTAX      RowPointer
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterParmRow indicates the OID of the row
         status of the applicable filter parameter table. This can be a row from
         either one of the following tables:
         - tIPFilterParamsTable;
         - tMacFilterParamsTable; or
         - tIPv6FilterParamsTable"
    ::= { tFilterNotificationObjects 2 }

tFilterAlarmDescription          OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterAlarmDescription is a printable
         character string which contains information about the cause of the
         problem."
    ::= { tFilterNotificationObjects 3 }

tFilterId                        OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterId, together with the object
         tFilterType uniquely defines the filter for which this notification is
         generated."
    ::= { tFilterNotificationObjects 4 }

tFilterType                      OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterType, together with the object
         tFilterId uniquely defines the filter for which this notification is
         generated."
    ::= { tFilterNotificationObjects 5 }

tFilterSubInsSpaceOwner          OBJECT-TYPE
    SYNTAX      TFilterSubInsSpaceOwner
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterSubInsSpaceOwner, specifies for which
         application, capable of inserting filter entries, this notification is
         generated."
    ::= { tFilterNotificationObjects 6 }

tFilterThresholdReached          OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterThresholdReached, specifies the
         threshold reached at the moment this notification was generated."
    ::= { tFilterNotificationObjects 7 }

tFltrFlowSpecProblem             OBJECT-TYPE
    SYNTAX      INTEGER {
        nlriDecodeProblem            (0),
        maxNbrFlowSpecEntriesReached (1),
        fltrResourceProblem          (2),
        other                        (3)
    }
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrFlowSpecProblem, indicates which problem
         has occurred while processing a BGP flowspec NLRI in the filter
         module."
    ::= { tFilterNotificationObjects 8 }

tFltrFlowSpecProblemDescription  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrFlowSpecProblemDescription may contain a
         more detailed problem description then as given by
         tFltrFlowSpecProblem."
    ::= { tFilterNotificationObjects 9 }

tFltrFLowSpecNLRI                OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrFLowSpecNLRI contains at most the first
         30 octets of the NLRI causing the problem."
    ::= { tFilterNotificationObjects 10 }

tFltrFlowSpecVrtrId              OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrFlowSpecVrtrId indicates the virtual
         router Id to which the NLRI belongs."
    ::= { tFilterNotificationObjects 11 }

tFltrPrefixListType              OBJECT-TYPE
    SYNTAX      TFltrPrefixListType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPrefixListType indicates the type of
         prefix list."
    ::= { tFilterNotificationObjects 12 }

tFltrPrefixListName              OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPrefixListName indicates the name of the
         prefix list."
    ::= { tFilterNotificationObjects 13 }

tFltrApplyPathSource             OBJECT-TYPE
    SYNTAX      TmnxFilterApplyPathSource
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tFltrApplyPathSource indicates the source of the
         apply-path rule."
    ::= { tFilterNotificationObjects 14 }

tFltrApplyPathIndex              OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of tFltrApplyPathIndex indicates the index of the apply-path
         rule."
    ::= { tFilterNotificationObjects 15 }

tFltrNotifDescription            OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrNotifDescription may contain a
         description text."
    ::= { tFilterNotificationObjects 16 }

tFltrMdaId                       OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrMdaId contains the MDA-id of the mda on
         which an filter event is being reported."
    ::= { tFilterNotificationObjects 17 }

tFilterTimeStampObjects          OBJECT IDENTIFIER ::= { tFilterObjects 9 }

tFilterDomainLastChanged         OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "timestamp of last change to tFilterObjects."
    ::= { tFilterTimeStampObjects 1 }

tFilterRedirectPolicyTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRedirectPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Contains a List of all redirect policies configured on this system."
    ::= { tFilterObjects 10 }

tFilterRedirectPolicyEntry       OBJECT-TYPE
    SYNTAX      TFilterRedirectPolicyEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular redirect policy. Entries are
         created/deleted by user."
    INDEX       { tFilterRedirectPolicy }
    ::= { tFilterRedirectPolicyTable 1 }

TFilterRedirectPolicyEntry       ::= SEQUENCE
{
    tFilterRedirectPolicy            TNamedItem,
    tFilterRPRowStatus               RowStatus,
    tFilterRPDescription             TItemDescription,
    tFilterRPAdminState              TmnxAdminState,
    tFilterRPActiveDest              IpAddress,
    tFilterRPVrtrId                  TmnxVRtrIDOrZero,
    tFilterRPActiveDestAddrType      InetAddressType,
    tFilterRPActiveDestAddr          InetAddress,
    tFilterRPDstStickiness           Integer32,
    tFilterRPBestDstAddrType         InetAddressType,
    tFilterRPBestDstAddr             InetAddress,
    tFilterRPStickinessHoldRemain    Integer32,
    tFilterRPNotifyDestChange        TruthValue
}

tFilterRedirectPolicy            OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "tFilterRedirectPolicy uniquely identifies each redirect policy
         configured on this system."
    ::= { tFilterRedirectPolicyEntry 1 }

tFilterRPRowStatus               OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "tFilterRPRowStatus allows entries to be created and deleted in the
         tFilterRedirectPolicyTable."
    ::= { tFilterRedirectPolicyEntry 2 }

tFilterRPDescription             OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "User-provided description for this redirect policy is maintained in
         the object tFilterRPDescription."
    DEFVAL      { ''H }
    ::= { tFilterRedirectPolicyEntry 3 }

tFilterRPAdminState              OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "tFilterRPAdminState holds the admin state of the policy. If the admin
         state is 'outOfService', the tests will not be conducted."
    DEFVAL      { outOfService }
    ::= { tFilterRedirectPolicyEntry 4 }

tFilterRPActiveDest              OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tFilterRPActiveDest indicates the IP address of the active
         destination. A value of 0 indicates that there is currently no active
         destination.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectPolicyEntry 5 }

tFilterRPVrtrId                  OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPVrtrId specifies the target routing
         instance as part of the redirect policy. When the target routing
         instance is configured (not equal to 0), the following applies:

         - Ping and unicast-reachability tests configured in a redirect policy
           are now executed in the routing instance specified by the redirect
           policy regardless of what routing instance is the filter using this
           redirect policy deployed in.

         - When packets are routed to a destination configured in a redirect
           policy with router instance specified (as result of filter match),
           routing is executed in the router instance context configured in
           the redirect policy regardless of the routing context for the
           interface on which the packet arrived.
           Note that if all destinations are down, the forward action is still
           executed in the routing instance of the incoming interface and not
           the routing instance of the redirect policy.
           If PBR specifies action forward router, then deploying the policy
           on card not supporting such action will result in action forward
           using incoming interface routing context.

         - If the H/W does not support the next-hop router PBR action, action
           forward is executed (even if the router instance in the action is the
           same as the router instance of the incoming interface).

         If the target routing instance is not configured (equal to 0), the
         following applies:

         - Redirect policy can be deployed in any VPRN or GRT routing context
           but a test will only run in GRT context regardless of where the policy
           is deployed.

         - The PBR will execute in the routing context of the ingress interface.

         SNMP and URL tests can be configured only if the target routing
         instance is not configured."
    DEFVAL      { 0 }
    ::= { tFilterRedirectPolicyEntry 6 }

tFilterRPActiveDestAddrType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPActiveDestAddrType indicates the
         context in which the values of the objects tFilterRPActiveDestAddr are
         interpreted.

         Only following values are supported:
            unknown(0)
            ipv4(1)
            ipv6(2)"
    DEFVAL      { unknown }
    ::= { tFilterRedirectPolicyEntry 7 }

tFilterRPActiveDestAddr          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPActiveDestAddr indicates the IP
         address of the active destination. A value of 0 indicates that there
         is currently no active destination.

         The value must be consistent with the IP version value of the
         associated tFilterRPActiveDestAddrType object."
    DEFVAL      { ''H }
    ::= { tFilterRedirectPolicyEntry 8 }

tFilterRPDstStickiness           OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPDstStickiness specifies the time in
         seconds, how long the system will wait until it sets and fixes the
         current best destination as active destination.  After the value of
         active destination is fixed it will remain unchanged until the active
         destination becomes unreachable.

         When the value of tFilterRPDstStickiness is -1 the property of
         destination stickiness is turned off. That means that active
         destination is always the best one.

         The countdown starts when there was no destination reachable and any
         destination becomes reachable."
    DEFVAL      { -1 }
    ::= { tFilterRedirectPolicyEntry 9 }

tFilterRPBestDstAddrType         OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPBestDstAddrType indicates the context
         in which the values of the objects tFilterRPActiveDestAddr are
         interpreted.

         Only following values are supported:
            unknown(0)
            ipv4(1)
            ipv6(2)"
    DEFVAL      { unknown }
    ::= { tFilterRedirectPolicyEntry 10 }

tFilterRPBestDstAddr             OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPBestDstAddr indicates the IP address
         of the available destination with the highest priority.  A value of
         0 indicates that currently there is no reachable destination.

         The value must be consistent with the IP version value of the
         associated tFilterRPActiveDestAddrType object."
    DEFVAL      { ''H }
    ::= { tFilterRedirectPolicyEntry 11 }

tFilterRPStickinessHoldRemain    OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPStickinessHoldRemain indicates the
         remaining time in seconds, until the best destination becomes the
         active destination and will become fixed."
    DEFVAL      { 0 }
    ::= { tFilterRedirectPolicyEntry 12 }

tFilterRPNotifyDestChange        OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPNotifyDestChange indicates whether to
         send tFilterRPActiveDestChangeEvent notification for this redirect
         policy active destination changes."
    DEFVAL      { false }
    ::= { tFilterRedirectPolicyEntry 13 }

tFilterRedirectDestTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRedirectDestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Contains a List of all redirect destinations configured on this
         system.

         This table is obsoleted in release 13.0 and replaced by
         tFilterRPlcyDstTable."
    ::= { tFilterObjects 11 }

tFilterRedirectDestEntry         OBJECT-TYPE
    SYNTAX      TFilterRedirectDestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Information about a particular Redirect destination. Entries are
         created/deleted by user.

         This object is obsoleted in release 13.0."
    INDEX       {
        tFilterRedirectPolicy,
        tFilterRedirectDest
    }
    ::= { tFilterRedirectDestTable 1 }

TFilterRedirectDestEntry         ::= SEQUENCE
{
    tFilterRedirectDest              IpAddress,
    tFilterRDRowStatus               RowStatus,
    tFilterRDDescription             TItemDescription,
    tFilterRDAdminPriority           Unsigned32,
    tFilterRDOperPriority            Unsigned32,
    tFilterRDAdminState              TmnxAdminState,
    tFilterRDOperState               TmnxOperState
}

tFilterRedirectDest              OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "tFilterRedirectDest holds the IP address of the destination entry.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectDestEntry 1 }

tFilterRDRowStatus               OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRDRowStatus allows entries to be created and deleted in the
         tFilterRedirectDestTable.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectDestEntry 2 }

tFilterRDDescription             OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "User-provided description for this destination is maintained in the
         object tFilterRDDescription.

         This object is obsoleted in release 13.0."
    DEFVAL      { ''H }
    ::= { tFilterRedirectDestEntry 3 }

tFilterRDAdminPriority           OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRDAdminPriority holds the configured base priority for the
         destination.

         This object is obsoleted in release 13.0."
    DEFVAL      { 100 }
    ::= { tFilterRedirectDestEntry 4 }

tFilterRDOperPriority            OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tFilterRDAdminPriority maintains the operational value of the priority
         for this destination. The highest operational priority across multiple
         destinations is used as the preferred destination.

         A value of '0' is maintained if the destination if tFilterRDOperState
         is 'outOfService'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectDestEntry 5 }

tFilterRDAdminState              OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRDAdminState maintains the configured state of the destination.
         If the admin state is 'outOfService', the tests for this destination
         will not be conducted.

         This object is obsoleted in release 13.0."
    DEFVAL      { outOfService }
    ::= { tFilterRedirectDestEntry 6 }

tFilterRDOperState               OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRDOperState indicates the operational state of the
         destination.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectDestEntry 7 }

tFilterRedirectSNMPTestTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRedirectSNMPTestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Contains a List of all redirect SNMP tests configured on this system.

         This table is obsoleted in release 13.0 and replaced by
         tFilterRPlcySNMPTestTable."
    ::= { tFilterObjects 12 }

tFilterRedirectSNMPTestEntry     OBJECT-TYPE
    SYNTAX      TFilterRedirectSNMPTestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Information about a specific SNMP test configured for a destination.
         Entries are created/deleted  by user.

         This object is obsoleted in release 13.0."
    INDEX       {
        tFilterRedirectPolicy,
        tFilterRedirectDest,
        tFilterRedirectSNMPTest
    }
    ::= { tFilterRedirectSNMPTestTable 1 }

TFilterRedirectSNMPTestEntry     ::= SEQUENCE
{
    tFilterRedirectSNMPTest          TNamedItem,
    tFilterRSTRowStatus              RowStatus,
    tFilterRSTOID                    OBJECT IDENTIFIER,
    tFilterRSTCommunity              DisplayString,
    tFilterRSTSNMPVersion            INTEGER,
    tFilterRSTInterval               Unsigned32,
    tFilterRSTTimeout                Unsigned32,
    tFilterRSTDropCount              Unsigned32,
    tFilterRSTHoldDown               Unsigned32,
    tFilterRSTHoldDownRemain         Unsigned32,
    tFilterRSTLastActionTime         TimeStamp,
    tFilterRSTLastOID                OBJECT IDENTIFIER,
    tFilterRSTLastType               INTEGER,
    tFilterRSTLastCounter32Val       Counter32,
    tFilterRSTLastUnsigned32Val      Unsigned32,
    tFilterRSTLastTimeTicksVal       TimeTicks,
    tFilterRSTLastInt32Val           Integer32,
    tFilterRSTLastOctetStringVal     OCTET STRING,
    tFilterRSTLastIpAddressVal       IpAddress,
    tFilterRSTLastOidVal             OBJECT IDENTIFIER,
    tFilterRSTLastCounter64Val       Counter64,
    tFilterRSTLastOpaqueVal          Opaque,
    tFilterRSTLastAction             INTEGER,
    tFilterRSTLastPrioChange         Integer32,
    tFilterRSTNextRespIndex          Integer32
}

tFilterRedirectSNMPTest          OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "tFilterRedirectSNMPTest specifies the name of the SNMP test.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 1 }

tFilterRSTRowStatus              OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRSTRowStatus allows tests to be created and deleted in the
         tFilterRedirectSNMPTestTable.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 2 }

tFilterRSTOID                    OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRSTOID stores the OID of the object to be fetched from the
         destination. The value of this object can only be changed if the
         object tFilterRSTCommunity is changed at the same time.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 3 }

tFilterRSTCommunity              OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRSTCommunity is the SNMPv1 or SNMPv2c Community
         String or the SNMPv3 Context Name used to conduct this SNMP test as
         described in RFC2571 and RFC2737.

         When the value of tFilterRSTSNMPVersion is 'snmpv1' or 'snmpv2c'
         this object represents a community string.  When the value of
         tFilterRSTSNMPVersion is 'snmpv3' this object represents a SNMPv3
         context name.
         The value of this object can only be changed if the object
         tFilterRSTOID is changed at the same time.

         This object is obsoleted in release 13.0."
    DEFVAL      { ''H }
    ::= { tFilterRedirectSNMPTestEntry 4 }

tFilterRSTSNMPVersion            OBJECT-TYPE
    SYNTAX      INTEGER {
        snmpv1  (1),
        snmpv2c (2),
        snmpv3  (3)
    }
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRSTSNMPVersion specifies the SNMP PDU format to be used while
         conducting the test. Currently only snmpv2c is supported.

         This object is obsoleted in release 13.0."
    DEFVAL      { snmpv2c }
    ::= { tFilterRedirectSNMPTestEntry 5 }

tFilterRSTInterval               OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRSTInterval specifies the amount of time in
         seconds between consecutive requests sent to the far end host.

         This object is obsoleted in release 13.0."
    DEFVAL      { 1 }
    ::= { tFilterRedirectSNMPTestEntry 6 }

tFilterRSTTimeout                OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRSTTimeout specifies the amount of time in seconds
         that is allowed for receiving a response from the far end host. If a
         reply is not received within this time the far end host is considered
         unresponsive.

         This object is obsoleted in release 13.0."
    DEFVAL      { 1 }
    ::= { tFilterRedirectSNMPTestEntry 7 }

tFilterRSTDropCount              OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRSTDropCount specifies the number of consecutive
         requests that must fail for the destination to declared unreachable.

         This object is obsoleted in release 13.0."
    DEFVAL      { 3 }
    ::= { tFilterRedirectSNMPTestEntry 8 }

tFilterRSTHoldDown               OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRSTHoldDown specifies the amount of time in
         seconds that the system should be held down if any of the test has
         marked it unreachable.

         This object is obsoleted in release 13.0."
    DEFVAL      { 0 }
    ::= { tFilterRedirectSNMPTestEntry 9 }

tFilterRSTHoldDownRemain         OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRSTHoldDownRemain indicates the amount of time in
         seconds that the system will remain in held down state before being
         used again.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 10 }

tFilterRSTLastActionTime         OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tFilterRSTLastActionTime maintains the time stamp when this test
         received a response for a probe sent out.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 11 }

tFilterRSTLastOID                OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The object tFilterRSTLastOID holds the OID received in the response.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 12 }

tFilterRSTLastType               OBJECT-TYPE
    SYNTAX      INTEGER {
        none        (0),
        counter32   (1),
        unsigned32  (2),
        timeTicks   (3),
        integer32   (4),
        ipAddress   (5),
        octetString (6),
        objectId    (7),
        counter64   (8),
        opaque      (9)
    }
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tFilterRSTLastType maintains the type of the value received. A value
         of none(0) indicated that no value has been received.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 13 }

tFilterRSTLastCounter32Val       OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTLastType is 'counter32'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 14 }

tFilterRSTLastUnsigned32Val      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTLastType is 'unsigned32'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 15 }

tFilterRSTLastTimeTicksVal       OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTLastType is 'timeTicks'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 16 }

tFilterRSTLastInt32Val           OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTLastType is 'integer32'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 17 }

tFilterRSTLastOctetStringVal     OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTLastType is 'octetString'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 18 }

tFilterRSTLastIpAddressVal       OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTLastType is 'ipAddress'. Although this seems to be
         unfriendly for IPv6, we have to recognize that there are a number of
         older MIBs that do contain an IPv4 format address, known as IpAddress.

         IPv6 addresses are represented using TAddress or InetAddress, and so
         the underlying datatype is OCTET STRING, and their value would be
         stored in the tFilterRSTLastOctetStringVal column.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 19 }

tFilterRSTLastOidVal             OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTLastType is 'objectId'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 20 }

tFilterRSTLastCounter64Val       OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTLastType is 'counter64'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 21 }

tFilterRSTLastOpaqueVal          OBJECT-TYPE
    SYNTAX      Opaque
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTLastType is 'opaque'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 22 }

tFilterRSTLastAction             OBJECT-TYPE
    SYNTAX      INTEGER {
        enable  (1),
        disable (2),
        none    (3)
    }
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tFilterRSTLastAction maintains impact that the last test probe made on
         the operational status of the destination as maintained in
         tFilterRDOperState.

         If the last action was 'disable', the destination may not be used for
         tFilterRSTHoldDown seconds.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 23 }

tFilterRSTLastPrioChange         OBJECT-TYPE
    SYNTAX      Integer32 (-255..255)
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "If the last action on the operational state of the destination i.e.
         tFilterRSTLastAction is 'enable', tFilterRSTLastPrioChange maintains
         the impact that the last test probe made on the operational priority
         of the destination.

         In other cases, this object has no significance and hence should be
         holding the value '0'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 24 }

tFilterRSTNextRespIndex          OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 1..2147483647)
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRSTNextRespIndex indicates the next response index
         to be used while creating a row in the tFilterRedirectSNMPRespTable.

         The value of '-1' means that the maximum number of return values for
         this OID are already configured.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPTestEntry 25 }

tFilterRedirectSNMPRespTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRedirectSNMPRespEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Each row in this table holds the effect of the test on the destination
         for a specific return value.

         Each row is created once and cannot be modified after creation. Any
         change attempts will be silently discarded.

         This table is obsoleted in release 13.0 and replaced by
         tFilterRPlcySNMPRespTable."
    ::= { tFilterObjects 13 }

tFilterRedirectSNMPRespEntry     OBJECT-TYPE
    SYNTAX      TFilterRedirectSNMPRespEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Information about action to be taken for a specific destination when a
         specific response is received.

         Each row is created once and cannot be modified after creation. Any
         change attempts will be silently discarded.

         This object is obsoleted in release 13.0."
    INDEX       {
        tFilterRedirectPolicy,
        tFilterRedirectDest,
        tFilterRedirectSNMPTest,
        tFilterRSTRespId
    }
    ::= { tFilterRedirectSNMPRespTable 1 }

TFilterRedirectSNMPRespEntry     ::= SEQUENCE
{
    tFilterRSTRespId                 Integer32,
    tFilterRSTRespRowStatus          RowStatus,
    tFilterRSTRespAction             INTEGER,
    tFilterRSTRespPrioChange         Unsigned32,
    tFilterRSTRespOID                OBJECT IDENTIFIER,
    tFilterRSTRespType               INTEGER,
    tFilterRSTCounter32Val           Counter32,
    tFilterRSTUnsigned32Val          Unsigned32,
    tFilterRSTTimeTicksVal           TimeTicks,
    tFilterRSTInt32Val               Integer32,
    tFilterRSTOctetStringVal         OCTET STRING,
    tFilterRSTIpAddressVal           IpAddress,
    tFilterRSTOidVal                 OBJECT IDENTIFIER,
    tFilterRSTCounter64Val           Counter64,
    tFilterRSTOpaqueVal              Opaque
}

tFilterRSTRespId                 OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "tFilterRSTRespId holds the response value received from the
         destination.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 1 }

tFilterRSTRespRowStatus          OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "This object allows response strings to be specified for a specific
         test and the change it will cause to the priority of the destination.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 2 }

tFilterRSTRespAction             OBJECT-TYPE
    SYNTAX      INTEGER {
        increase (1),
        decrease (2),
        disable  (3)
    }
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRSTRespAction specifies the type of change that should be made
         to the destination priority tFilterRDOperPriority, if the return value
         is same as tFilterRSTRespId. If tFilterRSTRespPrioChange is 0 this
         field will be set to 'disable'.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded.

         This object is obsoleted in release 13.0."
    DEFVAL      { disable }
    ::= { tFilterRedirectSNMPRespEntry 3 }

tFilterRSTRespPrioChange         OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRSTRespPrioChange specifies the amount of change to be made to
         the priority of the destination if the tFilterRSTRespAction is either
         'increase' or 'decrease'. If tFilterRSTRespAction is 'disable', this
         field will be set to 0.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded.

         This object is obsoleted in release 13.0."
    DEFVAL      { 0 }
    ::= { tFilterRedirectSNMPRespEntry 4 }

tFilterRSTRespOID                OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The object tFilterRSTRespOID holds the OID to be received in the
         response.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 5 }

tFilterRSTRespType               OBJECT-TYPE
    SYNTAX      INTEGER {
        counter32   (1),
        unsigned32  (2),
        timeTicks   (3),
        integer32   (4),
        ipAddress   (5),
        octetString (6),
        objectId    (7),
        counter64   (8),
        opaque      (9)
    }
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRSTRespType maintains the type of the value to be received.

         Note: types 'objectId' and 'counter64' are not supported for now, and
         will be rejected when used.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 6 }

tFilterRSTCounter32Val           OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTRespType is 'counter32'. This field cannot be
         modified after creation. Any change attempts will be silently
         discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 7 }

tFilterRSTUnsigned32Val          OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTRespType is 'unsigned32'. This field cannot be
         modified after creation. Any change attempts will be silently
         discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 8 }

tFilterRSTTimeTicksVal           OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTRespType is 'timeTicks'. This field cannot be
         modified after creation. Any change attempts will be silently
         discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 9 }

tFilterRSTInt32Val               OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTRespType is 'integer32'. This field cannot be
         modified after creation. Any change attempts will be silently
         discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 10 }

tFilterRSTOctetStringVal         OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTRespType is 'octetString'. This field cannot be
         modified after creation. Any change attempts will be silently
         discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 11 }

tFilterRSTIpAddressVal           OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTRespType is 'ipAddress'. Although this seems to be
         unfriendly for IPv6, we have to recognize that there are a number of
         older MIBs that do contain an IPv4 format address, known as IpAddress.

         IPv6 addresses are represented using TAddress or InetAddress, and so
         the underlying datatype is OCTET STRING, and their value would be
         stored in the tFilterRSTOctetStringVal column.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 12 }

tFilterRSTOidVal                 OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The response value if tFilterRSTRespType is set to 'objectId'. This
         field cannot be modified after creation. Any change attempts will be
         silently discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 13 }

tFilterRSTCounter64Val           OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The response value if tFilterRSTRespType is set to 'counter64'. This
         field cannot be modified after creation. Any change attempts will be
         silently discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 14 }

tFilterRSTOpaqueVal              OBJECT-TYPE
    SYNTAX      Opaque
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value tFilterRSTRespType is 'opaque'. This field cannot be
         modified after creation. Any change attempts will be silently
         discarded.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectSNMPRespEntry 15 }

tFilterRedirectURLTestTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRedirectURLTestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Contains a List of all redirect snmp tests configured on this system.

         This table is obsoleted in release 13.0 and replaced by
         tFilterRPlcyURLTestTable."
    ::= { tFilterObjects 14 }

tFilterRedirectURLTestEntry      OBJECT-TYPE
    SYNTAX      TFilterRedirectURLTestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Information about a specific URL test configured for a destination.
         Entries are created/deleted  by user. Entries have a presumed
         StorageType of nonVolatile.

         This object is obsoleted in release 13.0."
    INDEX       {
        tFilterRedirectPolicy,
        tFilterRedirectDest,
        tFilterRedirectURLTest
    }
    ::= { tFilterRedirectURLTestTable 1 }

TFilterRedirectURLTestEntry      ::= SEQUENCE
{
    tFilterRedirectURLTest           TNamedItem,
    tFilterRUTRowStatus              RowStatus,
    tFilterRUTURL                    DisplayString,
    tFilterRUTHTTPVersion            DisplayString,
    tFilterRUTInterval               Unsigned32,
    tFilterRUTTimeout                Unsigned32,
    tFilterRUTDropCount              Unsigned32,
    tFilterRUTHoldDown               Unsigned32,
    tFilterRUTHoldDownRemain         Unsigned32,
    tFilterRUTLastActionTime         TimeStamp,
    tFilterRUTLastRetCode            Unsigned32,
    tFilterRUTLastAction             INTEGER,
    tFilterRUTLastPrioChange         Integer32
}

tFilterRedirectURLTest           OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "tFilterRedirectURLTest holds the name of the URL test.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectURLTestEntry 1 }

tFilterRUTRowStatus              OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRUTRowStatus allows tests to be created and deleted in the
         tFilterRedirectURLTestTable.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectURLTestEntry 2 }

tFilterRUTURL                    OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "This object holds the URL to be probed.

         This object is obsoleted in release 13.0."
    DEFVAL      { ''H }
    ::= { tFilterRedirectURLTestEntry 3 }

tFilterRUTHTTPVersion            OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The HTTP Version to be used while performing the URL test. The system
         by default uses HTTP Version 1.1 until explicitly specified.

         This object is obsoleted in release 13.0."
    DEFVAL      { ''H }
    ::= { tFilterRedirectURLTestEntry 4 }

tFilterRUTInterval               OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRUTInterval specifies the amount of time in
         seconds between consecutive requests sent to the far end host.

         This object is obsoleted in release 13.0."
    DEFVAL      { 1 }
    ::= { tFilterRedirectURLTestEntry 5 }

tFilterRUTTimeout                OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRUTTimeout specifies the amount of time in seconds
         that is allowed for receiving a response from the far end host. If a
         reply is not received within this time the far end host is considered
         unresponsive.

         This object is obsoleted in release 13.0."
    DEFVAL      { 1 }
    ::= { tFilterRedirectURLTestEntry 6 }

tFilterRUTDropCount              OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRUTDropCount specifies the number of consecutive
         requests that must fail for the destination to declared unreachable.

         This object is obsoleted in release 13.0."
    DEFVAL      { 3 }
    ::= { tFilterRedirectURLTestEntry 7 }

tFilterRUTHoldDown               OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRUTHoldDown specifies the amount of time in
         seconds that the system should be held down if any of the test has
         marked it unreachable.

         This object is obsoleted in release 13.0."
    DEFVAL      { 0 }
    ::= { tFilterRedirectURLTestEntry 8 }

tFilterRUTHoldDownRemain         OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRUTHoldDownRemain indicates the amount of time in
         seconds that the system will remain in held down state before being
         used again.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectURLTestEntry 9 }

tFilterRUTLastActionTime         OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tFilterRUTLastActionTime maintains the time stamp when this test
         received a response for a probe sent out.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectURLTestEntry 10 }

tFilterRUTLastRetCode            OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tFilterRUTLastRetCode holds the return code received in the last
         response.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectURLTestEntry 11 }

tFilterRUTLastAction             OBJECT-TYPE
    SYNTAX      INTEGER {
        enable  (1),
        disable (2),
        none    (3)
    }
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tFilterRUTLastAction maintains impact that the last test probe made on
         the operational status of the destination as maintained in
         tFilterRDOperState.

         If the last action was 'disable', the destination may not be used for
         tFilterRUTHoldDown seconds.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectURLTestEntry 12 }

tFilterRUTLastPrioChange         OBJECT-TYPE
    SYNTAX      Integer32 (-255..255)
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "If the last action on the operational state of the destination i.e.
         tFilterRUTLastAction is 'enable', tFilterRUTLastPrioChange maintains
         the impact that the last test probe made on the operational priority
         of the destination.

         In other cases, this object has no significance and hence should be
         holding the value '0'.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectURLTestEntry 13 }

tFilterRedirectURLRespTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRedirectURLRespEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Each row in this table holds the effect of the test on the destination
         for a range of return values.

         This table is obsoleted in release 13.0 and replaced by
         tFilterRPlcyURLRespTable."
    ::= { tFilterObjects 15 }

tFilterRedirectURLRespEntry      OBJECT-TYPE
    SYNTAX      TFilterRedirectURLRespEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Information about action to be taken for a specific destination when a
         return value within the range specified between
         tFilterRedirectURLLowRespCode and tFilterRedirectURLHighRespCode is
         received.

         This object is obsoleted in release 13.0."
    INDEX       {
        tFilterRedirectPolicy,
        tFilterRedirectDest,
        tFilterRedirectURLTest,
        tFilterRedirectURLLowRespCode,
        tFilterRedirectURLHighRespCode
    }
    ::= { tFilterRedirectURLRespTable 1 }

TFilterRedirectURLRespEntry      ::= SEQUENCE
{
    tFilterRedirectURLLowRespCode    Unsigned32,
    tFilterRedirectURLHighRespCode   Unsigned32,
    tFilterRUTRespRowStatus          RowStatus,
    tFilterRUTRespAction             INTEGER,
    tFilterRUTRespPrioChange         Unsigned32
}

tFilterRedirectURLLowRespCode    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "tFilterRedirectURLLowRespCode specifies the lower return code of the
         range specified by this entry.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectURLRespEntry 1 }

tFilterRedirectURLHighRespCode   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "tFilterRedirectURLHighRespCode specifies the higher return code of the
         range specified by this entry.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectURLRespEntry 2 }

tFilterRUTRespRowStatus          OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRUTRespRowStatus allows the mapping of a range of return codes
         returned from a specific test to the change it will cause to the
         priority of the destination.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectURLRespEntry 3 }

tFilterRUTRespAction             OBJECT-TYPE
    SYNTAX      INTEGER {
        increase (1),
        decrease (2),
        disable  (3)
    }
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "If the tFilterRUTRespAction is either 'increase(1)' or 'decrease(2)'
         tFilterRUTRespPrioChange specifies the offset to be applied to the
         destination base priority (tFilterRDAdminPriority) in order to compute
         the tFilterRDOperPriority as a result of this test.

         If the tFilterRUTRespAction is set to 'disable(3)', on the reception
         of the specified response, the destination will be deemed unusable and
         the tFilterRDOperPriority will be set to '0'.

         The value of tFilterRUTRespAction will be forced by the system to the
         value 'disable(3)' if the tFilterRUTRespPrioChange has the value '0'.
         Any change attempts will be silently discarded in this case.

         This object is obsoleted in release 13.0."
    DEFVAL      { disable }
    ::= { tFilterRedirectURLRespEntry 4 }

tFilterRUTRespPrioChange         OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tFilterRUTRespPrioChange specifies the amount of change to be made to
         the priority of the destination if the tFilterRUTRespAction is either
         'increase' or 'decrease'.

         If tFilterRUTRespAction is 'disable', tFilterRUTRespPrioChange will be
         forced to 0. Any change to tFilterRUTRespPrioChange will be silently
         discarded in this case.

         Setting the object tFilterRUTRespPrioChange to 0 will cause the value
         of tFilterRUTRespAction to be set to 'disable'.

         This object is obsoleted in release 13.0."
    DEFVAL      { 0 }
    ::= { tFilterRedirectURLRespEntry 5 }

tFilterRedirectPingTestTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRedirectPingTestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Contains a List of all redirect Ping tests configured on this system.

         This table is obsoleted in release 13.0 and replaced by
         tFilterRPlcyPingTestTable."
    ::= { tFilterObjects 16 }

tFilterRedirectPingTestEntry     OBJECT-TYPE
    SYNTAX      TFilterRedirectPingTestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Information about a specific Ping test configured for a destination.
         Entries are created/deleted  by user. Entries have a presumed
         StorageType of nonVolatile.

         This object is obsoleted in release 13.0."
    INDEX       {
        tFilterRedirectPolicy,
        tFilterRedirectDest
    }
    ::= { tFilterRedirectPingTestTable 1 }

TFilterRedirectPingTestEntry     ::= SEQUENCE
{
    tFilterRPTRowStatus              RowStatus,
    tFilterRPTInterval               Unsigned32,
    tFilterRPTTimeout                Unsigned32,
    tFilterRPTDropCount              Unsigned32,
    tFilterRPTHoldDown               Unsigned32,
    tFilterRPTHoldDownRemain         Unsigned32,
    tFilterRPTLastActionTime         TimeStamp,
    tFilterRPTLastAction             INTEGER
}

tFilterRPTRowStatus              OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "This object allows tests to be created and deleted in the
         tFilterRedirectPingTestTable.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectPingTestEntry 1 }

tFilterRPTInterval               OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRPTInterval specifies the amount of time in
         seconds between consecutive requests sent to the far end host.

         Note that the value of tFilterRPTInterval can only be modified if the
         value of the corresponding tFilterRPAdminState and/or
         tFilterRDAdminState object is outOfService.

         This object is obsoleted in release 13.0."
    DEFVAL      { 1 }
    ::= { tFilterRedirectPingTestEntry 2 }

tFilterRPTTimeout                OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRPTTimeout specifies the amount of time in seconds
         that is allowed for receiving a response from the far end host. If a
         reply is not received within this time the far end host is considered
         unresponsive.

         Note that the value of tFilterRPTTimeout can only be modified if the
         value of the corresponding tFilterRPAdminState and/or
         tFilterRDAdminState object is outOfService.

         This object is obsoleted in release 13.0."
    DEFVAL      { 1 }
    ::= { tFilterRedirectPingTestEntry 3 }

tFilterRPTDropCount              OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRPTDropCount specifies the number of consecutive
         requests that must fail for the destination to declared unreachable.

         This object is obsoleted in release 13.0."
    DEFVAL      { 3 }
    ::= { tFilterRedirectPingTestEntry 4 }

tFilterRPTHoldDown               OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRPTHoldDown specifies the amount of time in
         seconds that the system should be held down if any of the test has
         marked it unreachable.

         This object is obsoleted in release 13.0."
    DEFVAL      { 0 }
    ::= { tFilterRedirectPingTestEntry 5 }

tFilterRPTHoldDownRemain         OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tFilterRPTHoldDownRemain indicates the amount of time in
         seconds that the system will remain in held down state before being
         used again.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectPingTestEntry 6 }

tFilterRPTLastActionTime         OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tFilterRPTLastActionTime maintains the time stamp when this test
         received a response for a probe sent out.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectPingTestEntry 7 }

tFilterRPTLastAction             OBJECT-TYPE
    SYNTAX      INTEGER {
        enable  (1),
        disable (2),
        none    (3)
    }
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tFilterRPTLastAction maintains impact that the last test probe made on
         the operational status of the destination as maintained in
         tFilterRDOperState.

         If the last action was 'disable', the destination may not be used for
         tFilterRPTHoldDown seconds.

         This object is obsoleted in release 13.0."
    ::= { tFilterRedirectPingTestEntry 8 }

tAutoIPFilterEntryTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF TAutoIPFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Defines the Nokia SROS series automatic IP filters for providing, via
         SNMP, the capability of gathering information regarding the same.

         tAutoIPFilterEntryTable holds a list of all automatic filter entries
         being used for filtering.

         This table is obsoleted in release 3.0."
    ::= { tFilterObjects 17 }

tAutoIPFilterEntry               OBJECT-TYPE
    SYNTAX      TAutoIPFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Defines an entry in the tAutoIPFilterEntryTable.

         Entries are created and deleted in this table by the system.

         Each entry provides information about a single active automatic filter
         entry.

         This entry is obsoleted in release 3.0."
    INDEX       {
        tAutoIPFilterId,
        tAutoIPFilterEntrySourceIpAddr
    }
    ::= { tAutoIPFilterEntryTable 1 }

TAutoIPFilterEntry               ::= SEQUENCE
{
    tAutoIPFilterId                  TFilterID,
    tAutoIPFilterEntrySourceIpAddr   IpAddress,
    tAutoIPFilterEntrySourceIpMask   IpAddressPrefixLength
}

tAutoIPFilterId                  OBJECT-TYPE
    SYNTAX      TFilterID (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "tAutoIPFilterId serves as a primary index and uniquely identifies an
         application point such as a routed interface or a SAP.

         This object is obsoleted in release 3.0."
    ::= { tAutoIPFilterEntry 1 }

tAutoIPFilterEntrySourceIpAddr   OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "tAutoIPFilterEntrySourceIpAddr specifies the source IP address and
         also serves as the secondary index to this table.

         This object is obsoleted in release 3.0."
    ::= { tAutoIPFilterEntry 2 }

tAutoIPFilterEntrySourceIpMask   OBJECT-TYPE
    SYNTAX      IpAddressPrefixLength
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of tAutoIPFilterEntrySourceIpMask indicates the number of
         bits to be matched in the source IP address.

         This object is obsoleted in release 3.0."
    ::= { tAutoIPFilterEntry 3 }

tIPv6FilterTable                 OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIPv6FilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Contains a List of all IPv6 filters configured on this system."
    ::= { tFilterObjects 18 }

tIPv6FilterEntry                 OBJECT-TYPE
    SYNTAX      TIPv6FilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular IPv6 Filter entry. Entries are
         created/deleted  by user. Entries have a presumed StorageType of
         nonVolatile."
    INDEX       { tIPv6FilterId }
    ::= { tIPv6FilterTable 1 }

TIPv6FilterEntry                 ::= SEQUENCE
{
    tIPv6FilterId                    TAnyFilterID,
    tIPv6FilterRowStatus             RowStatus,
    tIPv6FilterScope                 TFilterScope,
    tIPv6FilterDescription           TItemDescription,
    tIPv6FilterDefaultAction         TFilterAction,
    tIPv6FilterRadiusInsertPt        TEntryIdOrZero,
    tIPv6FilterRadiusInsertSize      TEntryBlockSize,
    tIPv6FilterCreditCntrlInsertPt   TEntryIdOrZero,
    tIPv6FilterCreditCntrlInsertSize TEntryBlockSize,
    tIPv6FilterSubInsertHighWmark    Integer32,
    tIPv6FilterSubInsertLowWmark     Integer32,
    tIpv6FilterCreditCntrlNbrInsertd Unsigned32,
    tIpv6FilterRadiusNbrInsertd      Unsigned32,
    tIpv6FilterName                  TLNamedItemOrEmpty,
    tIPv6FilterHostSharedInsertPt    TEntryIdOrZero,
    tIPv6FilterHostSharedInsertSize  TEntryBlockSize,
    tIpv6FilterHostSharedNbrInsertd  Unsigned32,
    tIPv6FilterHostSharedHighWmark   Integer32,
    tIPv6FilterHostSharedLowWmark    Integer32,
    tIPv6FilterNbrHostSharedFltrs    Unsigned32,
    tIPv6FilterSharedPccRuleInsrtPt  TEntryIdOrZero,
    tIPv6FilterSharedPccRuleInsrtSiz TEntryBlockSize,
    tIPv6FilterSharedPccRuleNbrInsrt Unsigned32,
    tIPv6FilterChainToSystemFilter   TruthValue,
    tIPv6FilterType                  TIPvXFilterType,
    tIPv6FilterSharedPolicer         TruthValue
}

tIPv6FilterId                    OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterId uniquely identifies an ip
         filter. User-configured filters have values between (1..65535). Other
         values are reserved for filters that are created (auto-generated) by
         the system. Refer to the description of the textual convention
         TAnyFilterID for more details."
    ::= { tIPv6FilterEntry 1 }

tIPv6FilterRowStatus             OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterRowStatus specifies the status of
         the IPv6 filter. The object allows entries to be created and deleted
         in the tIPv6FilterTable."
    ::= { tIPv6FilterEntry 2 }

tIPv6FilterScope                 OBJECT-TYPE
    SYNTAX      TFilterScope
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterScope specifies the scope of this
         filter definition."
    DEFVAL      { template }
    ::= { tIPv6FilterEntry 3 }

tIPv6FilterDescription           OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterDescription specifies a
         user-provided description for this filter."
    DEFVAL      { ''H }
    ::= { tIPv6FilterEntry 4 }

tIPv6FilterDefaultAction         OBJECT-TYPE
    SYNTAX      TFilterAction
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterDefaultAction specifies the action
         to be taken for packets that do not match any of the filter entries.
         The only allowed values for this field are drop(1) and forward(2)."
    DEFVAL      { drop }
    ::= { tIPv6FilterEntry 5 }

tIPv6FilterRadiusInsertPt        OBJECT-TYPE
    SYNTAX      TEntryIdOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterRadiusInsertPt specifies at what place the
         host specific filter entries received from Radius will be inserted in
         the filter.

         The area defined here will be dedicated to those entries, no other
         entries will be allowed.

         The value 0 means that no Radius provided host specific filter entries
         can be inserted in the filter.

         If tIPv6FilterRadiusInsertSize is set to 0, then this object will be
         put to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPv6FilterEntry 6 }

tIPv6FilterRadiusInsertSize      OBJECT-TYPE
    SYNTAX      TEntryBlockSize
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterRadiusInsertSize specifies how many host
         specific filter entries received from Radius for subscriber hosts can
         be inserted in the filter.

         If tIPv6FilterRadiusInsertPt is set to 0, then this object will be put
         to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPv6FilterEntry 7 }

tIPv6FilterCreditCntrlInsertPt   OBJECT-TYPE
    SYNTAX      TEntryIdOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterCreditCntrlInsertPt specifies at what place
         the filter entries received from Credit Control for a particular
         subscriber host will be inserted in the filter.

         The area defined here will be dedicated to those entries, no other
         entries will be allowed.

         The value 0 means that no Credit Control provided filter entries can
         be inserted in the filter.

         If tIPv6FilterCreditCntrlInsertSize is set to 0, then this object will
         be put to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPv6FilterEntry 8 }

tIPv6FilterCreditCntrlInsertSize OBJECT-TYPE
    SYNTAX      TEntryBlockSize
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterCreditCntrlInsertSize specifies how many
         filter entries received from Credit Control can be inserted in the
         filter.

         If tIPv6FilterCreditCntrlInsertPt is set to 0, then this object will
         be put to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPv6FilterEntry 9 }

tIPv6FilterSubInsertHighWmark    OBJECT-TYPE
    SYNTAX      Integer32 (0..100)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterSubInsertHighWmark specifies the
         utilization of the filter ranges for filter entry insertion, at which
         a table full alarm will be raised by the agent. The value 0 indicates
         that no alarm will be generated."
    DEFVAL      { 95 }
    ::= { tIPv6FilterEntry 10 }

tIPv6FilterSubInsertLowWmark     OBJECT-TYPE
    SYNTAX      Integer32 (0..100)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterSubInsertLowWmark specifies the
         utilization of the filter ranges for filter entry insertion, at which
         a table full alarm will be cleared by the agent."
    DEFVAL      { 90 }
    ::= { tIPv6FilterEntry 11 }

tIpv6FilterCreditCntrlNbrInsertd OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIpv6FilterCreditCntrlNbrInsertd indicates how
         many filter entries are currently inserted in the filter on request of
         credit control."
    ::= { tIPv6FilterEntry 12 }

tIpv6FilterRadiusNbrInsertd      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIpv6FilterRadiusNbrInsertd indicates how many
         host specific filter entries are currently inserted in the filter on
         request of RADIUS."
    ::= { tIPv6FilterEntry 13 }

tIpv6FilterName                  OBJECT-TYPE
    SYNTAX      TLNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIpv6FilterName specifies the name to associate with this
         filter."
    DEFVAL      { ''H }
    ::= { tIPv6FilterEntry 14 }

tIPv6FilterHostSharedInsertPt    OBJECT-TYPE
    SYNTAX      TEntryIdOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterHostSharedInsertPt specifies at what place the
         filter entries received from Radius that are shared between several
         hosts (host common rules) will be inserted in the filter.

         The area defined here will be dedicated to those entries, no other
         entries will be allowed.

         The value 0 means that no Radius provided host common filter entries
         can be inserted in the filter.

         If tIPv6FilterHostSharedInsertSize is set to 0, then this object will
         be put to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPv6FilterEntry 15 }

tIPv6FilterHostSharedInsertSize  OBJECT-TYPE
    SYNTAX      TEntryBlockSize
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterHostSharedInsertSize specifies how many host
         common filter entries received from Radius for subscriber hosts can be
         inserted in the filter.

         If tIPv6FilterHostSharedInsertPt is set to 0, then this object will be
         put to 0 as well. Any change attempts will result in error."
    DEFVAL      { 0 }
    ::= { tIPv6FilterEntry 16 }

tIpv6FilterHostSharedNbrInsertd  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIpv6FilterHostSharedNbrInsertd indicates how
         many host common filter entries are currently inserted in the filter
         on request of Radius."
    ::= { tIPv6FilterEntry 17 }

tIPv6FilterHostSharedHighWmark   OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 1..8000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterHostSharedHighWmark specifies the
         number of Radius Shared Filters that can be dynamically created in the
         system before an high watermark notification is generated by the
         system. The value -1 specifies that no notifications are sent. If any
         of the watermarks (high or low) is set to -1, both watermarks will be
         set to -1 by the system."
    DEFVAL      { -1 }
    ::= { tIPv6FilterEntry 18 }

tIPv6FilterHostSharedLowWmark    OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..8000)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterHostSharedLowWmark specifies the
         number of Radius Shared Filters that are still dynamically created in
         the system before an high watermark notification is cleared by the
         system. The value -1 specifies that no notifications are sent. If any
         of the watermarks (high or low) is set to -1, both watermarks will be
         set to -1 by the system."
    DEFVAL      { -1 }
    ::= { tIPv6FilterEntry 19 }

tIPv6FilterNbrHostSharedFltrs    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterNbrHostSharedFltrs indicates how
         many filters are currently created by Radius or Diameter based on this
         filter. (Both host shared or flow-rule filters.)"
    ::= { tIPv6FilterEntry 20 }

tIPv6FilterSharedPccRuleInsrtPt  OBJECT-TYPE
    SYNTAX      TEntryIdOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterSharedPccRuleInsrtPt specifies at what place
         the flow-rule filter entries that are received from Diameter and that
         are shared across several hosts will be inserted in the filter.

         The range defined here will be reserved for those entries; no other
         entries will be allowed in this range.

         The value 0 means that no flow-rule filter entries can be inserted in
         the filter by Diameter.

         If tIPv6FilterSharedPccRuleInsrtSiz is set to 0 then
         tIPv6FilterSharedPccRuleInsrtPt is also set to 0 by the system.

         Note that the range reserved for shared flow-rule entries must not
         overlap with that of either
         tIPv6FilterRadiusInsertPt/tIPv6FilterRadiusInsertSize,
         tIPv6FilterCreditCntrlInsertPt/tIPv6FilterCreditCntrlInsertSize, or
         tIPv6FilterHostSharedInsertPt/tIPv6FilterHostSharedInsertSize"
    DEFVAL      { 0 }
    ::= { tIPv6FilterEntry 21 }

tIPv6FilterSharedPccRuleInsrtSiz OBJECT-TYPE
    SYNTAX      TEntryBlockSize
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterSharedPccRuleInsrtSiz specifies how many
         flow-rule filter entries that are received from Diameter and that are
         shared across several hosts can be inserted in the filter.

         The range defined here will be reserved for those entries; no other
         entries will be allowed in this range.

         The value 0 means that no flow-rule filter entries can be inserted in
         the filter by Diameter.

         If tIPv6FilterSharedPccRuleInsrtPt is set to 0 then
         tIPv6FilterSharedPccRuleInsrtSiz is also set to 0 by the system.

         Note that the range reserved for shared flow-rule entries must not
         overlap with that of either
         tIPv6FilterRadiusInsertPt/tIPv6FilterRadiusInsertSize,
         tIPv6FilterCreditCntrlInsertPt/tIPv6FilterCreditCntrlInsertSize, or
         tIPv6FilterHostSharedInsertPt/tIPv6FilterHostSharedInsertSize"
    DEFVAL      { 0 }
    ::= { tIPv6FilterEntry 22 }

tIPv6FilterSharedPccRuleNbrInsrt OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterSharedPccRuleNbrInsrt indicates how
         many flow-rule filter entries received from Diameter have been
         inserted in this filter"
    ::= { tIPv6FilterEntry 23 }

tIPv6FilterChainToSystemFilter   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterChainToSystemFilter specifies
         whether this filter policy is chained to the active IPv6 system filter
         policy.

         The active IPv6 system filter policy is defined as a row in
         tFilterSystemFilterTable that have the value of the object
         tFilterSystemFilterType set to 'fltrtypeselIpv6(4)'.

         The value 'true(1)' means this filter policy is chained to the active
         IPv6 system filter policy. The system filter policy's rules are
         executed first before any rules of this filter policy are executed.

         The value of this object can be set to 'true(1)' only when the scope
         of this policy (value of the object tIPv6FilterScope) is
         'exclusive(1)' or 'template(2)'.

         The value 'false(2)' means this filter policy is not chained to the
         system filter policy."
    DEFVAL      { false }
    ::= { tIPv6FilterEntry 24 }

tIPv6FilterType                  OBJECT-TYPE
    SYNTAX      TIPvXFilterType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterType specifies the type of IPv6
         filter."
    DEFVAL      { normal }
    ::= { tIPv6FilterEntry 25 }

tIPv6FilterSharedPolicer         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterSharedPolicer specifies whether the
         value of tIPvXFltrEntryActRateLimit will be shared among LAG active
         ports.

         When the value is 'true' and the filter policy is applied to a single
         LAG interface or multiple LAG interfaces then Filter Entry Rate Limit
         Value per FP = ((tIPvXFltrEntryActRateLimit) / (Nb Active Ports in the
         LAG)) * (Nb active ports in the LAG for this FP)

         When the value is 'false' then Filter Entry Rate Limit Value per FP =
         tIPvXFltrEntryActRateLimit."
    DEFVAL      { false }
    ::= { tIPv6FilterEntry 26 }

tIPv6FilterParamsTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIPv6FilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of all IPv6 filter match entries for all IPv6 filters"
    ::= { tFilterObjects 19 }

tIPv6FilterParamsEntry           OBJECT-TYPE
    SYNTAX      TIPv6FilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular IPv6 Filter entry. Every IPv6 Filter
         can have zero or more IPv6 Filter match entries.

         A filter entry with no match criteria set will match every packet, and
         the entry action will be taken.

         Entries are created/deleted by user.

         Additional match criteria can be found in tIPv6FilterParamsExtTable.

         There is no StorageType object, entries have a presumed StorageType of
         nonVolatile."
    INDEX       {
        tIPv6FilterId,
        tIPv6FilterParamsIndex
    }
    ::= { tIPv6FilterParamsTable 1 }

TIPv6FilterParamsEntry           ::= SEQUENCE
{
    tIPv6FilterParamsIndex           TEntryId,
    tIPv6FilterParamsRowStatus       RowStatus,
    tIPv6FilterParamsLogId           TFilterLogId,
    tIPv6FilterParamsDescription     TItemDescription,
    tIPv6FilterParamsAction          TFilterActionOrDefault,
    tIPv6FilterParamsForwardNH       InetAddressIPv6,
    tIPv6FilterParamsForwardNHIndirect TruthValue,
    tIPv6FilterParamsRemarkDSCP      TDSCPFilterActionValue,
    tIPv6FilterParamsRemarkDSCPMask  TDSCPFilterActionValue,
    tIPv6FilterParamsRemarkDot1p     Dot1PPriority,
    tIPv6FilterParamsSourceIpAddr    InetAddressIPv6,
    tIPv6FilterParamsSourceIpMask    InetAddressPrefixLength,
    tIPv6FilterParamsDestinationIpAddr InetAddressIPv6,
    tIPv6FilterParamsDestinationIpMask InetAddressPrefixLength,
    tIPv6FilterParamsNextHeader      TIpProtocol,
    tIPv6FilterParamsSourcePortValue1 TTcpUdpPort,
    tIPv6FilterParamsSourcePortValue2 TTcpUdpPort,
    tIPv6FilterParamsSourcePortOperator TOperator,
    tIPv6FilterParamsDestPortValue1  TTcpUdpPort,
    tIPv6FilterParamsDestPortValue2  TTcpUdpPort,
    tIPv6FilterParamsDestPortOperator TOperator,
    tIPv6FilterParamsDSCP            TDSCPNameOrEmpty,
    tIPv6FilterParamsTcpSyn          TItemMatch,
    tIPv6FilterParamsTcpAck          TItemMatch,
    tIPv6FilterParamsIcmpCode        TIcmpCodeOrNone,
    tIPv6FilterParamsIcmpType        TIcmpTypeOrNone,
    tIPv6FilterParamsCflowdSample    TruthValue,
    tIPv6FilterParamsCflowdIfSample  TruthValue,
    tIPv6FilterParamsForwardNHInterface DisplayString,
    tIPv6FilterParamsIngressHitCount Counter64,
    tIPv6FilterParamsEgressHitCount  Counter64,
    tIPv6FilterParamsLogInstantiated TruthValue,
    tIPv6FilterParamsForwardRedPlcy  TNamedItemOrEmpty,
    tIPv6FilterParamsActiveDest      InetAddressIPv6,
    tIPv6FilterParamsTimeRangeName   TNamedItemOrEmpty,
    tIPv6FilterParamsTimeRangeState  TTimeRangeState,
    tIPv6FilterParamsIngrHitByteCount Counter64,
    tIPv6FilterParamsEgrHitByteCount Counter64,
    tIPv6FilterParamsFwdSvcId        TmnxServId,
    tIPv6FilterParamsFwdSapPortId    TmnxPortID,
    tIPv6FilterParamsFwdSapEncapVal  TmnxEncapVal,
    tIPv6FilterParamsFwdSdpBind      SdpBindId,
    tIPv6FilterParamsRedirectURL     TmnxHttpRedirectUrl,
    tIPv6FilterParamsSrcIpPrefixList TNamedItemOrEmpty,
    tIPv6FilterParamsDstIpPrefixList TNamedItemOrEmpty,
    tIPv6FilterParamsFragment        TFragmentMatch,
    tIPv6FilterParamsHopByHopOpt     TItemMatch,
    tIPv6FilterParamsRoutingType0    TItemMatch,
    tIPv6FilterParamsPortSelector    TFltrPortSelector,
    tIPv6FilterParamsSrcPortList     TNamedItemOrEmpty,
    tIPv6FilterParamsDstPortList     TNamedItemOrEmpty,
    tIPv6FilterParamsRdirAllwRadOvrd TruthValue,
    tIPv6FilterParamsFwdRtrId        TmnxVRtrIDOrZero,
    tIPv6FilterParamsSrcIpFullMask   InetAddressIPv6,
    tIPv6FilterParamsDstIpFullMask   InetAddressIPv6,
    tIPv6FilterParamsNatPolicyName   TNamedItemOrEmpty,
    tIPv6FilterParamsFlowLabel       IPv6FlowLabel,
    tIPv6FilterParamsFlowLabelMask   IPv6FlowLabelMask,
    tIPv6FilterParamsFwdLsp          TmnxVRtrMplsLspID,
    tIPv6FilterParamsFwdLspRtrId     TmnxVRtrIDOrZero,
    tIPv6FilterParamsIpSelector      TFltrMatchIpSelector
}

tIPv6FilterParamsIndex           OBJECT-TYPE
    SYNTAX      TEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This is the secondary index for the entry. Every IPv6 filter can have
         multiple entries, therefore every IPv6 filter entry is identified by
         the tIPv6FilterId and tIPv6FilterParamsIndex."
    ::= { tIPv6FilterParamsEntry 1 }

tIPv6FilterParamsRowStatus       OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted in the
         tIPv6FilterParamsTable."
    ::= { tIPv6FilterParamsEntry 2 }

tIPv6FilterParamsLogId           OBJECT-TYPE
    SYNTAX      TFilterLogId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object specifies the log to use for packets that match this
         entry. The value zero indicates that logging is disabled."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 3 }

tIPv6FilterParamsDescription     OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "User-provided description for this filter entry."
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsEntry 4 }

tIPv6FilterParamsAction          OBJECT-TYPE
    SYNTAX      TFilterActionOrDefault
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The action to take for packets that match this filter entry. The value
         default(3) specifies this entry to inherit the behavior defined as the
         default for the filter.

         Setting the values 'forwardEsiL2' and 'forwardEsiL3' explicitly is
         ignored by the system. The values 'forwardEsiL2'(8) and
         'forwardEsiL3'(9) can be set only implicitly by specifying non default
         values of objects specifying parameters for these actions. In such
         case the value of tIPFilterParamsAction will be set to
         'forwardEsiL2'(8) or 'forwardEsiL3'(9) automatically by system.


         The object tIPv6FilterParamsAction supports only subset of filter
         actions. The object tIPvXFltrEntryActAction supports all actions. It's
         recommended to use tIPvXFltrEntryActAction instead of
         tIPv6FilterParamsAction.

         The following value(s) is(are) not supported:
         - reassemble"
    DEFVAL      { ignoreMatch }
    ::= { tIPv6FilterParamsEntry 5 }

tIPv6FilterParamsForwardNH       OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The IPv6 address of the nexthop to which the packet should be
         forwarded if it hits this filter entry. The action of this entry
         should be 'forward' in such a case.

         Note that the value of tIPv6FilterParamsForwardNH is silently cleared
         by the system if tIPv6FilterParamsAction is set to value other than
         'forward'(2), or any object related to 'forward' other than
         tIPv6FilterParamsForwardNH or tIPv6FilterParamsForwardNHIndirect or
         tIPv6FilterParamsFwdRtrId is set."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPv6FilterParamsEntry 6 }

tIPv6FilterParamsForwardNHIndirect OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPv6FilterParamsForwardNHIndirect specifies if the nexthop is
         directly or indirectly reachable.

         Note that the value of tIPv6FilterParamsForwardNHIndirect is silently
         cleared by the system if tIPv6FilterParamsAction is set to value other
         than 'forward'(2), or any object related to 'forward' other than
         tIPv6FilterParamsForwardNH, tIPv6FilterParamsForwardNHIndirect or
         tIPv6FilterParamsFwdRtrId is set."
    DEFVAL      { false }
    ::= { tIPv6FilterParamsEntry 7 }

tIPv6FilterParamsRemarkDSCP      OBJECT-TYPE
    SYNTAX      TDSCPFilterActionValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The DSCP value that should be remarked in case a packet hits this
         filter entry."
    DEFVAL      { -1 }
    ::= { tIPv6FilterParamsEntry 8 }

tIPv6FilterParamsRemarkDSCPMask  OBJECT-TYPE
    SYNTAX      TDSCPFilterActionValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPv6FilterParamsRemarkDSCPMask specifies the care bits while
         remarking with the DSCP value."
    DEFVAL      { 255 }
    ::= { tIPv6FilterParamsEntry 9 }

tIPv6FilterParamsRemarkDot1p     OBJECT-TYPE
    SYNTAX      Dot1PPriority
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPv6FilterParamsRemarkDot1p specifies the Dot1p value that needs to
         be remarked on the packet if it hits this filter entry."
    DEFVAL      { -1 }
    ::= { tIPv6FilterParamsEntry 10 }

tIPv6FilterParamsSourceIpAddr    OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "IPv6 address to match the source IPv6 address of the packet."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPv6FilterParamsEntry 11 }

tIPv6FilterParamsSourceIpMask    OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..128)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the object tIPv6FilterParamsSourceIpMask
         specifies the IPv6 prefix length value for this policy IPv6 Filter
         entry. The mask generated from the prefix length value is ANDed with
         the received source IPv6 address to match the
         tIPv6FilterParamsSourceIpAddr.

         If the value of tIPv6FilterParamsSourceIpMask is 0, and the value of
         tIPv6FilterParamsSrcIpFullMask is non zero then the value of
         tIPv6FilterParamsSrcIpFullMask is used as a mask.

         If the value of tIPv6FilterParamsSourceIpMask is non zero, it will be
         equal to the mask expressed in the object
         tIPv6FilterParamsSrcIpFullMask.

         If both tIPv6FilterParamsSourceIpMask and
         tIPv6FilterParamsSrcIpFullMask are set to 0, no matching is done on
         the source IPv6 address.

         If a value is specified for this object, then the value of the object
         tIPv6FilterParamsSrcIpFullMask will be set to reflect this same mask."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 12 }

tIPv6FilterParamsDestinationIpAddr OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "IPv6 address to match the destination IPv6 address of the packet."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPv6FilterParamsEntry 13 }

tIPv6FilterParamsDestinationIpMask OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..128)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the object tIPv6FilterParamsDestinationIpMask
         specifies the IPv6 prefix length value for this policy IPv6 Filter
         entry. The mask generated from the prefix length value is ANDed with
         the received destination IPv6 address to match the
         tIPv6FilterParamsDestinationIpAddr.

         If the value of tIPv6FilterParamsDestinationIpMask is 0, and the value
         of tIPv6FilterParamsDstIpFullMask is non zero then the value of
         tIPv6FilterParamsDstIpFullMask is used as a mask.

         If the value of tIPv6FilterParamsDestinationIpMask is non zero, it
         will be equal to the mask expressed in the object
         tIPv6FilterParamsDstIpFullMask.

         If both tIPv6FilterParamsDestinationIpMask and
         tIPv6FilterParamsDstIpFullMask are set to 0, no matching is done on
         the destination IPv6 address.

         If a value is specified for this object, then the value of the object
         tIPv6FilterParamsDstIpFullMask will be set to reflect this same mask."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 14 }

tIPv6FilterParamsNextHeader      OBJECT-TYPE
    SYNTAX      TIpProtocol
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "IPv6 next header to match. Set to -1 to disable matching IPv6 next
         header."
    DEFVAL      { -1 }
    ::= { tIPv6FilterParamsEntry 15 }

tIPv6FilterParamsSourcePortValue1 OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "TCP/UDP port value1. The value of this object is used as per the
         description for tIPv6FilterParamsSourcePortOperator."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 16 }

tIPv6FilterParamsSourcePortValue2 OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "TCP/UDP port value2. The value of this object is used as per the
         description for tIPv6FilterParamsSourcePortOperator."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 17 }

tIPv6FilterParamsSourcePortOperator OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The operator specifies the manner in which
         tIPFilterParamsSourcePortValue1 and tIPFilterParamsSourcePortValue2
         are to be used."
    DEFVAL      { none }
    ::= { tIPv6FilterParamsEntry 18 }

tIPv6FilterParamsDestPortValue1  OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "TCP/UDP port value1. The value of this object is used as per the
         description for tIPv6FilterParamsDestPortOperator."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 19 }

tIPv6FilterParamsDestPortValue2  OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "TCP/UDP port value2. The value of this object is used as per the
         description for tIPv6FilterParamsDestPortOperator."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 20 }

tIPv6FilterParamsDestPortOperator OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The operator specifies the manner in which
         tIPFilterParamsDestPortValue1 and tIPFilterParamsDestPortValue2 are to
         be used."
    DEFVAL      { none }
    ::= { tIPv6FilterParamsEntry 21 }

tIPv6FilterParamsDSCP            OBJECT-TYPE
    SYNTAX      TDSCPNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "DSCP to be matched on the packet."
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsEntry 22 }

tIPv6FilterParamsTcpSyn          OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Syn as per value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsEntry 23 }

tIPv6FilterParamsTcpAck          OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Ack as per value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsEntry 24 }

tIPv6FilterParamsIcmpCode        OBJECT-TYPE
    SYNTAX      TIcmpCodeOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "ICMP code to be matched.

         The value -1 means ICMP code matching is not enabled."
    DEFVAL      { -1 }
    ::= { tIPv6FilterParamsEntry 25 }

tIPv6FilterParamsIcmpType        OBJECT-TYPE
    SYNTAX      TIcmpTypeOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "ICMP type to be matched.

         The value -1 means ICMP type matching is not enabled."
    DEFVAL      { -1 }
    ::= { tIPv6FilterParamsEntry 26 }

tIPv6FilterParamsCflowdSample    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When tIPFilterParamsCflowdSample has a value of 'true',  Cflowd
         sampling and analysis is performed on those packet streams where this
         filter has been applied.  Only packets matching this IPv6 filter entry
         are subjected to Cflowd sampling and analysis.  A Cflowd profile
         controls the sampling and analysis of data flows through the router."
    DEFVAL      { false }
    ::= { tIPv6FilterParamsEntry 27 }

tIPv6FilterParamsCflowdIfSample  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When tIPv6FilterParamsCflowdIfSample has a value of 'true', Cflowd
         sampling and analysis is performed on those packet streams where this
         filter has been applied.  Only packets matching this IPv6 filter entry
         are subjected to Cflowd sampling and analysis.  A Cflowd profile
         controls the sampling and analysis of data flows through the router."
    DEFVAL      { true }
    ::= { tIPv6FilterParamsEntry 28 }

tIPv6FilterParamsForwardNHInterface OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The interface name for the nexthop to which the packet should be
         forwarded if it hits this filter entry. The action of this entry
         should be 'forward' in such a case.

         Note that the value of tIPv6FilterParamsForwardNHInterface  is silently
         cleared by the system if tIPv6FilterParamsAction is set to value other
         than 'forward'(2), or any object related to 'forward' other than
         this one is set."
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsEntry 29 }

tIPv6FilterParamsIngressHitCount OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the number of times an ingress packet matched
         this entry."
    ::= { tIPv6FilterParamsEntry 30 }

tIPv6FilterParamsEgressHitCount  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the number of times an egress packet matched
         this entry."
    ::= { tIPv6FilterParamsEntry 31 }

tIPv6FilterParamsLogInstantiated OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tIPv6FilterParamsLogInstantiated indicates if the filter log for this
         filter entry has been instantiated or not."
    ::= { tIPv6FilterParamsEntry 32 }

tIPv6FilterParamsForwardRedPlcy  OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPv6FilterParamsForwardRedPlcy specifies the redirect policy to be
         used to determine the nexthop.

         Note that the value of tIPv6FilterParamsForwardRedPlcy is silently
         cleared by the system if tIPv6FilterParamsAction is set to value other
         than 'forward'(2), or any object related to 'forward' other than this
         one is set."
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsEntry 33 }

tIPv6FilterParamsActiveDest      OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tIPv6FilterParamsActiveDest indicates the IPv6 address of the active
         destination for this IPv6 filter. A value of 0 indicates that there is
         currently no active destination."
    ::= { tIPv6FilterParamsEntry 34 }

tIPv6FilterParamsTimeRangeName   OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPv6FilterParamsTimeRangeName specifies the tmnxTimeRangeEntry to be
         associated with this filter entry.

         A value for this object can only be specified during row creation, and
         cannot be altered later on. Also, a value is accepted only if the
         tmnxTimeRangeEntry is defined in the
         TIMETRA-SCHEDULER-MIB::tmnxTimeRangeTable.tTimeRangeName.

         This object is obsoleted in release 14.0."
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsEntry 35 }

tIPv6FilterParamsTimeRangeState  OBJECT-TYPE
    SYNTAX      TTimeRangeState
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "tIPv6FilterParamsTimeRangeState indicates whether or not the entry
         is currently in effect.
         - timeRangeNotApplic:
           no time range is applicable for this entry.
         - timeRangeNotActive:
           A time range is defined in tIPv6FilterParamsTimeRangeName, but is not
           active at this moment. Consequently the filter entry is not
           installed.
         - timeRangeActive.
           A time range is defined in tIPv6FilterParamsTimeRangeName, and is
           activated successfully.
         - timeRangeActiveDownloadFailed:
           A time range is defined in tIPv6FilterParamsTimeRangeName, and is
           activated, but the corresponding filter entry could not be
           installed due to resource problems.

         This object is obsoleted in release 14.0."
    ::= { tIPv6FilterParamsEntry 36 }

tIPv6FilterParamsIngrHitByteCount OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterParamsIngrHitByteCount indicates the number of
         bytes of all ingress packets that matched this entry."
    ::= { tIPv6FilterParamsEntry 37 }

tIPv6FilterParamsEgrHitByteCount OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This tIPv6FilterParamsEgrHitByteCount indicates the number of bytes of
         all egress packets that matched this entry."
    ::= { tIPv6FilterParamsEntry 38 }

tIPv6FilterParamsFwdSvcId        OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tIPv6FilterParamsFwdSvcId indicates the service id of the destination
         for this filter entry. The value 0 indicates that there is no active
         SAP or SDP destination."
    ::= { tIPv6FilterParamsEntry 39 }

tIPv6FilterParamsFwdSapPortId    OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPv6FilterParamsFwdSapPortId specifies the sap port id of the
         destination for this filter entry.

         The value 0 indicates that there is no SAP destination defined. A
         value different from 0 can only be specified if the value of the
         tIPv6FilterParamsAction object of this entry is 'forward'. In addition
         a non-zero value can only be given if the object
         tIPv6FilterParamsFwdSdpBind is '0'.

         Note that the value of tIPv6FilterParamsFwdSapPortId is silently
         cleared by the system if tIPv6FilterParamsAction is set to value other
         than 'forward'(2), or any object related to 'forward' other than
         tIPv6FilterParamsFwdSapPortId or tIPv6FilterParamsFwdSapEncapVal is
         set."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 40 }

tIPv6FilterParamsFwdSapEncapVal  OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPv6FilterParamsFwdSapEncapVal specifies the sap port encap value of
         the destination SAP for this filter entry.

         A value different from 0 can only be specified if the value of the
         tIPv6FilterParamsAction object of this entry is 'forward'. In addition
         a non-zero value can only be given if the object
         tIPv6FilterParamsFwdSdpBind has value '0'. The value 0 indicates
         that either
         1) the sap encapsulation value is not specified when
            tIPv6FilterParamsFwdSapPortId and tIPv6FilterParamsFwdSvcId
            have valid values; or
         2) that there is no SAP destination.

         Note that the value of tIPv6FilterParamsFwdSapEncapVal is silently
         cleared by the system if tIPv6FilterParamsAction is set to value other
         than 'forward'(2), or any object related to 'forward' other than
         tIPv6FilterParamsFwdSapPortId or tIPv6FilterParamsFwdSapEncapVal is
         set."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 41 }

tIPv6FilterParamsFwdSdpBind      OBJECT-TYPE
    SYNTAX      SdpBindId
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPv6FilterParamsFwdSdpBind specifies the sdp bind id of the
         destination for this filter entry.

         The value '0' indicates that there is currently no SDP binding
         defined. A value different from '0' can only be specified if the value
         of the tIPv6FilterParamsAction object of this entry is 'forward'. In
         addition a non-zero value can only be given if the objects
         tIPv6FilterParamsFwdSapPortId and tIPv6FilterParamsFwdSapEncapVal have
         value 0.

         Note that the value of tIPv6FilterParamsFwdSdpBind is silently cleared
         by the system if tIPv6FilterParamsAction is set to value other than
         'forward'(2), or any object related to 'forward' other than this one
         is set."
    DEFVAL      { '0000000000000000'H }
    ::= { tIPv6FilterParamsEntry 42 }

tIPv6FilterParamsRedirectURL     OBJECT-TYPE
    SYNTAX      TmnxHttpRedirectUrl
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of tIPv6FilterParamsRedirectURL specifies the URL to
         redirect to, when the value of tIPv6FilterParamsAction is
         'httpRedirect'.

         The following macro substitutions are applicable in this context:
         $URL, $MAC, $IP, $SUB, $SAP, $SAPDESC, $CID, and $RID.

         Note that the value of tIPv6FilterParamsRedirectURL is silently
         cleared by the system if tIPv6FilterParamsAction is set to any value
         other than httpRedirect."
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsEntry 43 }

tIPv6FilterParamsSrcIpPrefixList OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the IPv6 prefix list used as match
         criterion for the source IPv6 address.

         The value specified for this object must correspond to a prefix list
         defined in tFilterPrefixListTable.

         If the value of this object is empty then the values of the objects
         tIPv6FilterParamsSourceIpAddr and tIPv6FilterParamsSourceIpMask are
         used as source IPv6 address match criterion.

         When this object is set to a non-empty value then the objects
         tIPv6FilterParamsSourceIpAddr and tIPv6FilterParamsSourceIpMask are
         reset to their default values by the system.

         Vice versa, when a new (non-default) value is provided for the objects
         tIPv6FilterParamsSourceIpAddr and tIPv6FilterParamsSourceIpMask then
         this object is reset to its default (empty) value by the system."
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsEntry 44 }

tIPv6FilterParamsDstIpPrefixList OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the IPv6 prefix list used as match
         criterion for the destination IPv6 address.

         The value specified for this object must correspond to a prefix list
         defined in tFilterPrefixListTable.

         If the value of this object is empty then the values of the objects
         tIPv6FilterParamsDestinationIpAddr and
         tIPv6FilterParamsDestinationIpMask are used as destination ipv6
         address match criterion.

         When this object is set to a non-empty value then the objects
         tIPv6FilterParamsDestinationIpAddr and
         tIPv6FilterParamsDestinationIpMask are reset to their default values
         by the system.

         Vice versa, when a new (non-default) value is provided for the objects
         tIPv6FilterParamsDestinationIpAddr and
         tIPv6FilterParamsDestinationIpMask then this object is reset to its
         default (empty) value by the system."
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsEntry 45 }

tIPv6FilterParamsFragment        OBJECT-TYPE
    SYNTAX      TFragmentMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches fragmented/unfragmented packets as per value of
         the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsEntry 46 }

tIPv6FilterParamsHopByHopOpt     OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a Hop-By-Hop options Extension Header as per value
         of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsEntry 47 }

tIPv6FilterParamsRoutingType0    OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a Routing Extension Header as per value of the
         object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsEntry 48 }

tIPv6FilterParamsPortSelector    OBJECT-TYPE
    SYNTAX      TFltrPortSelector
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object specifies how the source port objects
         (tIPv6FilterParamsSourcePortValue1, tIPv6FilterParamsSourcePortValue2,
         tIPv6FilterParamsSourcePortOperator, tIPv6FilterParamsSrcPortList) and
         destination port objects (tIPv6FilterParamsDestPortValue1,
         tIPv6FilterParamsDestPortValue2, tIPv6FilterParamsDestPortOperator,
         tIPv6FilterParamsDstPortList) are combined to form the filter match
         criterion. See description of TFltrPortSelector."
    DEFVAL      { and-port }
    ::= { tIPv6FilterParamsEntry 49 }

tIPv6FilterParamsSrcPortList     OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the port-list used as match
         criterion for the source port.

         The value specified for this object must correspond to a port-list
         defined in tFilterPortListTable.

         If the value of this object is empty then the values of the objects
         tIPFilterParamsSourcePortValue1, tIPFilterParamsSourcePortValue2, and
         tIPFilterParamsSourcePortOperator are used as source port match
         criterion.

         When this object is set to a non-empty value then the objects
         tIPFilterParamsSourcePortValue1, tIPFilterParamsSourcePortValue2, and
         tIPFilterParamsSourcePortOperator are reset to their default values by
         the system.

         Vice versa, when a new (non-default) value is provided for one of the
         objects tIPFilterParamsSourcePortValue1,
         tIPFilterParamsSourcePortValue2, or tIPFilterParamsSourcePortOperator
         then tIPv6FilterParamsSrcPortList is reset to its default (empty)
         value by the system.

         Setting any one of the objects tIPFilterParamsSourcePortValue1,
         tIPFilterParamsSourcePortValue2, or tIPFilterParamsSourcePortOperator
         to a non-default value in combination with a non-default value for the
         object tIPv6FilterParamsSrcPortList is rejected by the system"
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsEntry 50 }

tIPv6FilterParamsDstPortList     OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the port-list used as match
         criterion for the destination port.

         The value specified for this object must correspond to a port-list
         defined in tFilterPortListTable.

         If the value of this object is empty then the values of the objects
         tIPFilterParamsDestPortValue1, tIPFilterParamsDestPortValue2, and
         tIPFilterParamsDestPortOperator are used as destination port match
         criterion.

         When this object is set to a non-empty value then the objects
         tIPFilterParamsDestPortValue1, tIPFilterParamsDestPortValue2, and
         tIPFilterParamsDestPortOperator are reset to their default values by
         the system.

         Vice versa, when a new (non-default) value is provided for one of the
         objects tIPFilterParamsDestPortValue1, tIPFilterParamsDestPortValue2,
         or tIPFilterParamsDestPortOperator then tIPv6FilterParamsDstPortList
         is reset to its default (empty) value by the system.

         Setting any one of the objects tIPFilterParamsDestPortValue1,
         tIPFilterParamsDestPortValue2, or tIPFilterParamsDestPortOperator to a
         non-default value in combination with a non-default value for the
         object tIPv6FilterParamsDstPortList is rejected by the system"
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsEntry 51 }

tIPv6FilterParamsRdirAllwRadOvrd OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of this object specifies whether or not the value of
         tIPv6FilterParamsRedirectURL can be overridden by a Radius VSA. The
         default value is false (i.e. the URL cannot be overridden by Radius).
         The value of tIPv6FilterParamsRdirAllwRadOvrd is relevant only if the
         value of tIPv6FilterParamsAction is httpRedirect.

         Setting the value of tIPv6FilterParamsRdirAllwRadOvrd to true is
         ignored by the system if the value of tIPv6FilterParamsAction is not
         httpRedirect. Furthermore, the value of
         tIPv6FilterParamsRdirAllwRadOvrd is silently reset to false by the
         system if tIPv6FilterParamsAction is set to any value other than
         httpRedirect."
    DEFVAL      { false }
    ::= { tIPv6FilterParamsEntry 52 }

tIPv6FilterParamsFwdRtrId        OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "tIPv6FilterParamsFwdRtrId specifies, if different from '0', the router
         id into which the packet should be forwarded if it hits this filter
         entry.

         The action of this entry should be 'forward' in such a case.

         Note that the value of tIPv6FilterParamsFwdRtrId is silently cleared
         by the system if tIPv6FilterParamsAction is set to value other than
         'forward'(2), or any object related to 'forward' other than
         tIPv6FilterParamsFwdRtrId, tIPv6FilterParamsForwardNH or
         tIPv6FilterParamsForwardNHIndirect is set."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 53 }

tIPv6FilterParamsSrcIpFullMask   OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the object tIPv6FilterParamsSrcIpFullMask
         specifies the IPv6 Mask value for this policy IPv6 Filter entry. The
         mask is ANDed with the received Source IPv6 address to match the
         tIPv6FilterParamsSourceIpAddr.

         If the value of tIPv6FilterParamsSourceIpMask is 0, and the value of
         tIPv6FilterParamsSrcIpFullMask is non zero then the value of
         tIPv6FilterParamsSrcIpFullMask is used as a mask.

         If the value of tIPv6FilterParamsSourceIpMask is non zero, it will be
         equal to the mask expressed in the object
         tIPv6FilterParamsSrcIpFullMask.

         If both tIPv6FilterParamsSourceIpMask and
         tIPv6FilterParamsSrcIpFullMask are set to 0, no matching is done on
         the Source IPv6 address.

         If a regular mask is specified for tIPv6FilterParamsSrcIpFullMask then
         the value of tIPv6FilterParamsSourceIpMask will be changed to reflect
         this value."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPv6FilterParamsEntry 54 }

tIPv6FilterParamsDstIpFullMask   OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the object tIPv6FilterParamsDstIpFullMask
         specifies the IPv6 Mask value for this policy IPv6 Filter entry. The
         mask is ANDed with the received Destination IPv6 address to match the
         tIPv6FilterParamsDestinationIpAddr.

         If the value of tIPv6FilterParamsDestinationIpMask is 0, and the value
         of tIPv6FilterParamsDstIpFullMask is non zero then the value of
         tIPv6FilterParamsDstIpFullMask is used as a mask.

         If the value of tIPv6FilterParamsDestinationIpMask is non zero, it
         will be equal to the mask expressed in the object
         tIPv6FilterParamsDstIpFullMask.

         If both tIPv6FilterParamsDestinationIpMask and
         tIPv6FilterParamsDstIpFullMask are set to 0, no matching is done on
         the Destination IPv6 address.

         If a regular mask is specified for tIPv6FilterParamsDstIpFullMask then
         the value of tIPv6FilterParamsDestinationIpMask will be changed to
         reflect this value."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPv6FilterParamsEntry 55 }

tIPv6FilterParamsNatPolicyName   OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of this object specifies the name of the NAT policy to be
         used when the value of tIPv6FilterParamsAction is nat. If the value is
         empty then a default policy is used. If the value is non-empty then it
         must correspond to a policy defined in tmnxNatPlcyTable.

         The value of tIPv6FilterParamsNatPolicyName is relevant only if the
         value of tIPv6FilterParamsAction is nat. Setting the value of
         tIPv6FilterParamsNatPolicyName to a non-empty string is ignored by the
         system if the value of tIPv6FilterParamsAction is not nat.

         Furthermore, the value of tIPv6FilterParamsNatPolicyName is silently
         reset to an empty string by the system if tIPv6FilterParamsAction is
         set to any value other than nat."
    DEFVAL      { "" }
    ::= { tIPv6FilterParamsEntry 56 }

tIPv6FilterParamsFlowLabel       OBJECT-TYPE
    SYNTAX      IPv6FlowLabel
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from -1 the value of the object
         tIPv6FilterParamsFlowLabel specifies the flow label to be used as a
         match criterion."
    DEFVAL      { -1 }
    ::= { tIPv6FilterParamsEntry 57 }

tIPv6FilterParamsFlowLabelMask   OBJECT-TYPE
    SYNTAX      IPv6FlowLabelMask
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsFlowLabelMask specifies the
         flow label mask value for this policy IP Filter entry.

         The mask is ANDed with the received flow label to match the value of
         the object tIPv6FilterParamsFlowLabel.

         If the mask is set to the value 0, it will result in resetting the
         value to default.

         The value is only significant if the value of the object
         tIPv6FilterParamsFlowLabel is different from -1."
    DEFVAL      { '0fffff'H }
    ::= { tIPv6FilterParamsEntry 58 }

tIPv6FilterParamsFwdLsp          OBJECT-TYPE
    SYNTAX      TmnxVRtrMplsLspID
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "If different from zero the value of the object tIPv6FilterParamsFwdLsp
         together with the value of the object tIPv6FilterParamsFwdLspRtrId
         specifies the LSP into which a packet should be forwarded if it hits
         this filter entry.

         The value of the object tIPv6FilterParamsAction of this entry must be
         'forward' in such case. Otherwise the value of the object
         tIPv6FilterParamsFwdLsp is ignored by the system.

         The value is reset to '0' if the value of the object
         tIPv6FilterParamsAction is set to value other than 'forward'(2), or
         any object related to 'forward' other than
         tIPv6FilterParamsFwdLspRtrId or tIPv6FilterParamsFwdLsp is set.

         The value of the object tIPv6FilterParamsFwdLsp cannot be set to a
         non-zero value if other destinations are already specified.

         The value has to be '0' if the value of the object
         tIPv6FilterParamsFwdLspRtrId is not set (i.e. is '0').

         If a non-zero value is set, the value of the object
         tIPv6FilterParamsFwdLspRtrId has to be set as well."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 59 }

tIPv6FilterParamsFwdLspRtrId     OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsFwdLspRtrId specifies the
         router ID that the LSP ID defined by the value of the object
         tIPv6FilterParamsFwdLsp belongs to.

         The value of the object tIPv6FilterParamsAction of this entry must be
         'forward' in such case. Otherwise the value of the object
         tIPv6FilterParamsFwdLspRtrId is ignored by the system.

         The value is reset to '0' if the value of the object
         tIPv6FilterParamsAction is set to other value than 'forward'(2), or
         any object related to 'forward' other than
         tIPv6FilterParamsFwdLspRtrId or tIPv6FilterParamsFwdLsp is set.

         The value of this object cannot be set to a non-zero value if other
         destinations are already specified.

         The value has to be '0' if the value of the object
         tIPv6FilterParamsFwdLsp is not set (i.e. is '0').

         If a non-zero value is set, the value of the object
         tIPv6FilterParamsFwdLsp has to be set as well.

         The ID of the base router and '0' are the only allowed values with
         this version of the product."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsEntry 60 }

tIPv6FilterParamsIpSelector      OBJECT-TYPE
    SYNTAX      TFltrMatchIpSelector
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsIpSelector specifies how the
         source address objects (tIPv6FilterParamsSourceIpAddr,
         tIPv6FilterParamsSourceIpMask, tIPv6FilterParamsSrcIpFullMask,
         tIPv6FilterParamsSrcIpPrefixList) and destination address objects
         (tIPv6FilterParamsSourceIpAddr, tIPv6FilterParamsSourceIpMask,
         tIPv6FilterParamsDstIpFullMask, tIPv6FilterParamsDstIpPrefixList) are
         combined to form the filter match criterion. See description of
         TFltrMatchIpSelector."
    DEFVAL      { and-ip }
    ::= { tIPv6FilterParamsEntry 61 }

tFilterGroupInsertedEntries      OBJECT IDENTIFIER ::= { tFilterObjects 20 }

tFltrGrpInsrtdEntriesFilterType  OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "tFltrGrpInsrtdEntriesFilterType specifies the type of the filter
         referred to by tFltrGrpInsrtdEntriesFilterId. Inserted entries can
         only occur in 'fltrtypeselIp' and 'fltrtypeselIpv6'"
    DEFVAL      { fltrtypeselNone }
    ::= { tFilterGroupInsertedEntries 1 }

tFltrGrpInsrtdEntriesFilterId    OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "tFltrGrpInsrtdEntriesFilterId specifies for which filter the inserted
         entries must be grouped."
    DEFVAL      { 0 }
    ::= { tFilterGroupInsertedEntries 2 }

tFltrGrpInsrtdEntriesApplication OBJECT-TYPE
    SYNTAX      TFltrGrpInsrtdEntriesApplication
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "tFltrGrpInsrtdEntriesApplication specifies for which application the
         inserted entries must be grouped."
    DEFVAL      { none }
    ::= { tFilterGroupInsertedEntries 3 }

tFltrGrpInsrtdEntriesLocation    OBJECT-TYPE
    SYNTAX      INTEGER {
        none   (0),
        top    (1),
        bottom (2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "tFltrGrpInsrtdEntriesLocation specifies at what location the inserted
         entries must be grouped."
    DEFVAL      { none }
    ::= { tFilterGroupInsertedEntries 4 }

tFltrGrpInsrtdEntriesResult      OBJECT-TYPE
    SYNTAX      INTEGER {
        none    (0),
        success (1),
        failure (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tFltrGrpInsrtdEntriesResult indicates the success or failure of the
         last requested grouping request on inserted entries."
    ::= { tFilterGroupInsertedEntries 5 }

tFltrGrpInsrtdEntriesFeedback    OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..254))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "tFltrGrpInsrtdEntriesFeedback may indicate additional info on the last
         inserted filter entries grouping action performed."
    ::= { tFilterGroupInsertedEntries 6 }

tFltrGrpInsrtdEntriesExecute     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Setting the object tFltrGrpInsrtdEntriesExecute to 'true' will cause
         the system to attempt to execute the grouping command as specified by
         the other MIB objects in the tFilterGroupInsertedEntries mibgroup.

         When read the value will always indicate 'false'. The result of the
         command can be found in tFltrGrpInsrtdEntriesResult and
         tFltrGrpInsrtdEntriesFeedback"
    DEFVAL      { false }
    ::= { tFilterGroupInsertedEntries 7 }

tDhcpFilterTableLastChanged      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tDhcpFilterTableLastChanged indicates the sysUpTime at
         the time of the last modification to tDhcpFilterTable by adding,
         deleting an entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 21 }

tDhcpFilterTable                 OBJECT-TYPE
    SYNTAX      SEQUENCE OF TDhcpFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Contains a list of all DHCP filters configured on this system."
    ::= { tFilterObjects 22 }

tDhcpFilterEntry                 OBJECT-TYPE
    SYNTAX      TDhcpFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular DHCP filter. Entries are
         created/deleted by user. Entries have a presumed StorageType of
         nonVolatile."
    INDEX       { tDhcpFilterId }
    ::= { tDhcpFilterTable 1 }

TDhcpFilterEntry                 ::= SEQUENCE
{
    tDhcpFilterId                    TDHCPFilterID,
    tDhcpFilterRowStatus             RowStatus,
    tDhcpFilterLastChanged           TimeStamp,
    tDhcpFilterDescription           TItemDescription,
    tDhcpFilterDefAction             TDhcpFilterAction
}

tDhcpFilterId                    OBJECT-TYPE
    SYNTAX      TDHCPFilterID (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Uniquely identifies a DHCP filter as configures on this system."
    ::= { tDhcpFilterEntry 1 }

tDhcpFilterRowStatus             OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted in the
         tDhcpFilterTable."
    ::= { tDhcpFilterEntry 2 }

tDhcpFilterLastChanged           OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tDhcpFilterLastChanged indicates the timestamp of last
         change to this row in tDhcpFilterTable."
    ::= { tDhcpFilterEntry 3 }

tDhcpFilterDescription           OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "User-provided description for this filter."
    DEFVAL      { ''H }
    ::= { tDhcpFilterEntry 4 }

tDhcpFilterDefAction             OBJECT-TYPE
    SYNTAX      TDhcpFilterAction
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The default action to take for DHCP host creation requests that do not
         match any of this filter's entries.

         The value none(1) specifies normal host creation behaviour, the value
         bypass-host-creation(2) specifies to bypass host creation, the value
         drop(3) specifies to drop the DHCP message."
    DEFVAL      { none }
    ::= { tDhcpFilterEntry 5 }

tDhcpFilterParamsTblLastChanged  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tDhcpFilterParamsTblLastChanged indicates the sysUpTime
         at the time of the last modification to tDhcpFilterParamsTable by
         adding, deleting an entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 23 }

tDhcpFilterParamsTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TDhcpFilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of all DHCP filter match entries for all DHCP filters"
    ::= { tFilterObjects 24 }

tDhcpFilterParamsEntry           OBJECT-TYPE
    SYNTAX      TDhcpFilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular DHCP filter entry. Every DHCP filter
         can have zero or more DHCP filter match entries.

         A filter entry with no match criteria set will match every packet, and
         the entry action will be taken.

         Entries are created/deleted by user.

         There is no StorageType object, entries have a presumed StorageType of
         nonVolatile."
    INDEX       {
        tDhcpFilterId,
        tDhcpFilterParamsId
    }
    ::= { tDhcpFilterParamsTable 1 }

TDhcpFilterParamsEntry           ::= SEQUENCE
{
    tDhcpFilterParamsId              TDhcpEntryId,
    tDhcpFilterParamsRowStatus       RowStatus,
    tDhcpFilterParamsLastChanged     TimeStamp,
    tDhcpFilterParamsOptionNumber    Integer32,
    tDhcpFilterParamsOptionMatch     TDhcpFilterMatch,
    tDhcpFilterParamsAction          TDhcpFilterAction,
    tDhcpFilterParamsOptionValue     OCTET STRING
}

tDhcpFilterParamsId              OBJECT-TYPE
    SYNTAX      TDhcpEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This is the secondary index for the entry. Every DHCP filter can have
         multiple entries, therefore every DHCP filter entry is identified by
         the tDhcpFilterId and tDhcpFilterParamsId."
    ::= { tDhcpFilterParamsEntry 1 }

tDhcpFilterParamsRowStatus       OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted in the
         tDhcpFilterParamsTable."
    ::= { tDhcpFilterParamsEntry 2 }

tDhcpFilterParamsLastChanged     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tDhcpFilterParamsLastChanged indicates the timestamp of
         last change to this row in tDhcpFilterParamsTable."
    ::= { tDhcpFilterParamsEntry 3 }

tDhcpFilterParamsOptionNumber    OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tDhcpFilterParamsOptionNumber specifies the number of the
         DHCP option to filter on."
    REFERENCE
        "RFC 2132, RFC 3315, RFC 3633"
    DEFVAL      { -1 }
    ::= { tDhcpFilterParamsEntry 4 }

tDhcpFilterParamsOptionMatch     OBJECT-TYPE
    SYNTAX      TDhcpFilterMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tDhcpFilterParamsOptionMatch specifies the criteria that
         the DHCP option must match to trigger this filter entry.

         The value present(1) specifies that the DHCP option must be present,
         the value absent(2) specifies that the DHCP option must be absent. In
         these cases tDhcpFilterParamsOptionValue will be reset to an empty
         string.

         A value string(3), string-exact(4), string-invert(5),
         string-exact-invert(6), hex(7), hex-exact(8), hex-invert(9) or
         hex-exact-invert(10) requires an octet string to be present in
         tDhcpFilterParamsOptionValue to match against."
    DEFVAL      { present }
    ::= { tDhcpFilterParamsEntry 5 }

tDhcpFilterParamsAction          OBJECT-TYPE
    SYNTAX      TDhcpFilterAction
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The action to take for DHCP host creation requests that match this
         filter entry. The value none(1) specifies normal host creation
         behaviour, the value bypass-host-creation(2) specifies to bypass host
         creation, the value drop(3) specifies to drop the DHCP message."
    DEFVAL      { none }
    ::= { tDhcpFilterParamsEntry 6 }

tDhcpFilterParamsOptionValue     OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..127))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tDhcpFilterParamsOptionValue specifies the
         matching pattern for the filtered DHCP option.

         This object is mandatory at creation time. A zero length value is only
         allowed when the value of tDhcpFilterParamsOptionMatch is present(1)
         or absent(2)."
    ::= { tDhcpFilterParamsEntry 7 }

tMacFilterNameTableLastChgd      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterNameTableLastChgd indicates the sysUpTime at
         the time of the last modification of tMacFilterNameTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 25 }

tMacFilterNameTable              OBJECT-TYPE
    SYNTAX      SEQUENCE OF TMacFilterNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains MAC filter name information. Entries are created
         automatically by the system when tMacFilterName object is set for the
         MAC filter."
    ::= { tFilterObjects 26 }

tMacFilterNameEntry              OBJECT-TYPE
    SYNTAX      TMacFilterNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Basic information about a specific MAC filter name."
    INDEX       { tMacFilterName }
    ::= { tMacFilterNameTable 1 }

TMacFilterNameEntry              ::= SEQUENCE
{
    tMacFilterNameId                 TAnyFilterID,
    tMacFilterNameRowStatus          RowStatus,
    tMacFilterNameLastChanged        TimeStamp
}

tMacFilterNameId                 OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFilterNameId indicates the filter name
         associated with this MAC filter."
    ::= { tMacFilterNameEntry 1 }

tMacFilterNameRowStatus          OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This value of the object tMacFilterNameRowStatus indicates the status
         of this row."
    ::= { tMacFilterNameEntry 2 }

tMacFilterNameLastChanged        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tMacFilterNameLastChanged indicates the sysUpTime at the
         time of the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tMacFilterNameEntry 3 }

tIpFilterNameTableLastChgd       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tIpFilterNameTableLastChgd indicates the sysUpTime at the
         time of the last modification of tIpFilterNameTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 27 }

tIpFilterNameTable               OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIpFilterNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains IP filter name information. Entries are created
         automatically by the system when tIpFilterName object is set for the
         IP filter."
    ::= { tFilterObjects 28 }

tIpFilterNameEntry               OBJECT-TYPE
    SYNTAX      TIpFilterNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Basic information about a specific IP filter name."
    INDEX       { tIpFilterName }
    ::= { tIpFilterNameTable 1 }

TIpFilterNameEntry               ::= SEQUENCE
{
    tIpFilterNameId                  TAnyFilterID,
    tIpFilterNameRowStatus           RowStatus,
    tIpFilterNameLastChanged         TimeStamp
}

tIpFilterNameId                  OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIpFilterNameId indicates the filter name
         associated with this IP filter."
    ::= { tIpFilterNameEntry 1 }

tIpFilterNameRowStatus           OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This value of the object tIpFilterNameRowStatus indicates the status
         of this row."
    ::= { tIpFilterNameEntry 2 }

tIpFilterNameLastChanged         OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tIpFilterNameLastChanged indicates the sysUpTime at the
         time of the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tIpFilterNameEntry 3 }

tIpv6FilterNameTableLastChgd     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tIpv6FilterNameTableLastChgd indicates the sysUpTime at
         the time of the last modification of tIpv6FilterNameTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 29 }

tIpv6FilterNameTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIpv6FilterNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains IPv6 filter name information. Entries are
         created automatically by the system when tIpv6FilterName object is set
         for the IPv6 filter."
    ::= { tFilterObjects 30 }

tIpv6FilterNameEntry             OBJECT-TYPE
    SYNTAX      TIpv6FilterNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Basic information about a specific IPv6 filter name."
    INDEX       { tIpv6FilterName }
    ::= { tIpv6FilterNameTable 1 }

TIpv6FilterNameEntry             ::= SEQUENCE
{
    tIpv6FilterNameId                TAnyFilterID,
    tIpv6FilterNameRowStatus         RowStatus,
    tIpv6FilterNameLastChanged       TimeStamp
}

tIpv6FilterNameId                OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIpv6FilterNameId indicates the filter name
         associated with this IPv6 filter."
    ::= { tIpv6FilterNameEntry 1 }

tIpv6FilterNameRowStatus         OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This value of the object tIpv6FilterNameRowStatus indicates the status
         of this row."
    ::= { tIpv6FilterNameEntry 2 }

tIpv6FilterNameLastChanged       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tIpv6FilterNameLastChanged indicates the sysUpTime at the
         time of the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tIpv6FilterNameEntry 3 }

tFilterLiObjects                 OBJECT IDENTIFIER ::= { tFilterObjects 31 }

tLiReservedBlockTableLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockTableLastChanged indicates the sysUpTime at
         the time of the last modification of tLiReservedBlockTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterLiObjects 1 }

tLiReservedBlockTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF TLiReservedBlockEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tLiReservedBlockTable describes LI reserved blocks. In this
         release this table can have at most one entry."
    ::= { tFilterLiObjects 2 }

tLiReservedBlockEntry            OBJECT-TYPE
    SYNTAX      TLiReservedBlockEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about an LI reserved block. This block can be associated
         with one or more filters to reserve a number of entries in those
         filters for LI."
    INDEX       { tLiReservedBlockName }
    ::= { tLiReservedBlockTable 1 }

TLiReservedBlockEntry            ::= SEQUENCE
{
    tLiReservedBlockName             TNamedItem,
    tLiReservedBlockRowStatus        RowStatus,
    tLiReservedBlockLastChanged      TimeStamp,
    tLiReservedBlockDescription      TItemDescription,
    tLiReservedBlockStart            TEntryIdOrZero,
    tLiReservedBlockSize             TEntryBlockSize
}

tLiReservedBlockName             OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockName uniquely identifies an LI reserved
         block."
    ::= { tLiReservedBlockEntry 1 }

tLiReservedBlockRowStatus        OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockRowStatus specifies the status of this row."
    ::= { tLiReservedBlockEntry 2 }

tLiReservedBlockLastChanged      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockLastChanged indicates the sysUpTime at the
         time of the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tLiReservedBlockEntry 3 }

tLiReservedBlockDescription      OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockDescription specifies a description for
         this LI reserved block."
    DEFVAL      { ''H }
    ::= { tLiReservedBlockEntry 4 }

tLiReservedBlockStart            OBJECT-TYPE
    SYNTAX      TEntryIdOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockStart specifies the starting entry of the
         LI reserved block.

         If set to '0' no block is reserved. In this case the value of the
         object tLiReservedBlockSize will be set to '0' by the system."
    DEFVAL      { 0 }
    ::= { tLiReservedBlockEntry 5 }

tLiReservedBlockSize             OBJECT-TYPE
    SYNTAX      TEntryBlockSize
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockSize specifies the size of the LI reserved
         block.

         If set to '0' no block is reserved. In this case the value of the
         object tLiReservedBlockStart will be set to '0' by the system.

         The maximum value of this object may be limited depending on hardware
         variants."
    DEFVAL      { 0 }
    ::= { tLiReservedBlockEntry 6 }

tLiReservedBlockFltrTableLastChg OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tLiReservedBlockFltrTableLastChg indicates the sysUpTime
         at the time of the last modification of tLiReservedBlockFltrTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterLiObjects 3 }

tLiReservedBlockFltrTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TLiReservedBlockFltrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tLiReservedBlockFltrTable contains associations between
         normal filters and LI block reservations.

         Setting the value of TIMETRA-SYSTEM-MIB:tmnxSysMgmtIfWriteMode to
         VAL_tmnxSysMgmtIfWriteOperMode_mixed won't be allowed if this table
         contains reference to non existing filter. Before enabling mixed mode
         the loose references should be removed or replaced by name references
         in tLiRsvdBlockFltrAssocTable"
    ::= { tFilterLiObjects 4 }

tLiReservedBlockFltrEntry        OBJECT-TYPE
    SYNTAX      TLiReservedBlockFltrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An association of a normal filter with an LI block reservation. In
         this release MAC and IP/IPv6 filters are supported.

         Entries can be created and deleted via SNMP SET operations to
         tLiReservedBlockFltrRowStatus."
    INDEX       {
        tLiReservedBlockName,
        tLiReservedBlockFltrType,
        tLiReservedBlockFltrIdStart,
        tLiReservedBlockFltrIdEnd
    }
    ::= { tLiReservedBlockFltrTable 1 }

TLiReservedBlockFltrEntry        ::= SEQUENCE
{
    tLiReservedBlockFltrType         TFilterType,
    tLiReservedBlockFltrIdStart      TFilterID,
    tLiReservedBlockFltrIdEnd        TFilterID,
    tLiReservedBlockFltrRowStatus    RowStatus,
    tLiReservedBlockFltrLastChanged  TimeStamp
}

tLiReservedBlockFltrType         OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockFltrType specifies the type of filter this
         LI block reservation applies to.

         In this release MAC and IP/IPv6 filters are supported:
             fltrtypeselIp     (1)
             fltrtypeselMac    (2)
             fltrtypeselIpv6   (4)"
    ::= { tLiReservedBlockFltrEntry 1 }

tLiReservedBlockFltrIdStart      OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockFltrIdStart specifies the ID of the first
         filter to apply an LI block reservation.

         If the value of the object tLiReservedBlockFltrType is equal to 1 or 4
         (IP or IPv6 filter) then the scope of any filter (defined by the value
         of the object tIPFilterScope or tIPv6FilterScope) inside of the range
         defined by the values of the objects tLiReservedBlockFltrIdStart and
         tLiReservedBlockFltrIdEnd must not be equal to embedded (3).

         In this release, tLiReservedBlockFltrIdStart must be equal to
         tLiReservedBlockFltrIdEnd."
    ::= { tLiReservedBlockFltrEntry 2 }

tLiReservedBlockFltrIdEnd        OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockFltrIdEnd specifies the ID of the last
         filter to apply an LI block reservation.

         If the value of the object tLiReservedBlockFltrType is equal to 1 or 4
         (IP or IPv6 filter) then the scope of any filter (defined by the value
         of the object tIPFilterScope or tIPv6FilterScope) inside of the range
         defined by the values of the objects tLiReservedBlockFltrIdStart and
         tLiReservedBlockFltrIdEnd must not be equal to embedded (3).

         In this release, tLiReservedBlockFltrIdEnd must be equal to
         tLiReservedBlockFltrIdStart."
    ::= { tLiReservedBlockFltrEntry 3 }

tLiReservedBlockFltrRowStatus    OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockFltrRowStatus specifies the status of this
         row."
    ::= { tLiReservedBlockFltrEntry 4 }

tLiReservedBlockFltrLastChanged  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiReservedBlockFltrLastChanged indicates the sysUpTime at
         the time of the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tLiReservedBlockFltrEntry 5 }

tLiFilterTableLastChanged        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiFilterTableLastChanged indicates the sysUpTime at the
         time of the last modification of tLiFilterTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterLiObjects 5 }

tLiFilterTable                   OBJECT-TYPE
    SYNTAX      SEQUENCE OF TLiFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tLiFilterTable contains information about all LI filters.

         In this release MAC and IP/IPv6 filters are supported."
    ::= { tFilterLiObjects 6 }

tLiFilterEntry                   OBJECT-TYPE
    SYNTAX      TLiFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry represents an LI filter. In this release MAC and IP/IPv6
         filters are supported.

         Entries can be created and deleted via SNMP SET operations to
         tLiFilterRowStatus."
    INDEX       {
        tLiFilterType,
        tLiFilterName
    }
    ::= { tLiFilterTable 1 }

TLiFilterEntry                   ::= SEQUENCE
{
    tLiFilterType                    TFilterType,
    tLiFilterName                    TNamedItem,
    tLiFilterRowStatus               RowStatus,
    tLiFilterLastChanged             TimeStamp,
    tLiFilterDescription             TItemDescription
}

tLiFilterType                    OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiFilterType specifies the type of this LI filter.

         In this release MAC and IP/IPv6 filters are supported."
    ::= { tLiFilterEntry 1 }

tLiFilterName                    OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiFilterName indicates the unique name of this LI Filter."
    ::= { tLiFilterEntry 2 }

tLiFilterRowStatus               OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiFilterRowStatus specifies the status of this row."
    ::= { tLiFilterEntry 3 }

tLiFilterLastChanged             OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiFilterLastChanged indicates the sysUpTime at the time of
         the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tLiFilterEntry 4 }

tLiFilterDescription             OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiFilterDescription specifies a description for this LI
         filter."
    DEFVAL      { ''H }
    ::= { tLiFilterEntry 5 }

tLiFilterAssociationTableLastChg OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiFilterAssociationTableLastChg indicates the sysUpTime at
         the time of the last modification of tLiFilterAssociationTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterLiObjects 7 }

tLiFilterAssociationTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TLiFilterAssociationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tLiFilterAssociationTable contains information about the
         associations between LI filters and normal filters."
    ::= { tFilterLiObjects 8 }

tLiFilterAssociationEntry        OBJECT-TYPE
    SYNTAX      TLiFilterAssociationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An association between an LI filter and a normal filter."
    INDEX       {
        tLiFilterType,
        tLiFilterName,
        tLiFilterAssociationFltrId
    }
    ::= { tLiFilterAssociationTable 1 }

TLiFilterAssociationEntry        ::= SEQUENCE
{
    tLiFilterAssociationFltrId       TFilterID,
    tLiFilterAssociationRowStatus    RowStatus,
    tLiFilterAssociationLastChg      TimeStamp
}

tLiFilterAssociationFltrId       OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiFilterAssociationFltrId indicates the id of the normal
         filter in the association described by this entry."
    ::= { tLiFilterAssociationEntry 1 }

tLiFilterAssociationRowStatus    OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiFilterAssociationRowStatus specifies the status of this
         row."
    ::= { tLiFilterAssociationEntry 2 }

tLiFilterAssociationLastChg      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiFilterAssociationLastChg indicates the sysUpTime at the
         time of the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tLiFilterAssociationEntry 3 }

tLiMacFilterParamsTableLastChg   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsTableLastChg indicates the sysUpTime at
         the time of the last modification of tLiMacFilterParamsTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterLiObjects 9 }

tLiMacFilterParamsTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF TLiMacFilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tLiMacFilterParamsTable contains all LI MAC filter match
         entries for all LI MAC filters."
    ::= { tFilterLiObjects 10 }

tLiMacFilterParamsEntry          OBJECT-TYPE
    SYNTAX      TLiMacFilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An LI MAC filter match entry."
    INDEX       {
        tLiFilterType,
        tLiFilterName,
        tLiMacFilterParamsId
    }
    ::= { tLiMacFilterParamsTable 1 }

TLiMacFilterParamsEntry          ::= SEQUENCE
{
    tLiMacFilterParamsId             TLimitedEntryId,
    tLiMacFilterParamsRowStatus      RowStatus,
    tLiMacFilterParamsLastChanged    TimeStamp,
    tLiMacFilterParamsDescription    TItemDescription,
    tLiMacFilterParamsFrameType      TFrameType,
    tLiMacFilterParamsSrcMAC         MacAddress,
    tLiMacFilterParamsSrcMACMask     MacAddress,
    tLiMacFilterParamsDstMAC         MacAddress,
    tLiMacFilterParamsDstMACMask     MacAddress,
    tLiMacFilterParamsIngrHitCount   Counter64,
    tLiMacFilterParamsEgrHitCount    Counter64,
    tLiMacFilterParamsIngrHitBytes   Counter64,
    tLiMacFilterParamsEgrHitBytes    Counter64,
    tLiMacFilterParamsSapPortId      TmnxPortID,
    tLiMacFilterParamsSapEncapType   TmnxPortEncapType,
    tLiMacFilterParamsSapEncapVal    TmnxEncapVal,
    tLiMacFilterParamsOuterTagVal    QTagOrNone
}

tLiMacFilterParamsId             OBJECT-TYPE
    SYNTAX      TLimitedEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsId indicates the secondary index for this
         entry. Every LI MAC filter may have multiple match entries, therefore
         every LI MAC filter match entry is identified by the tLiFilterName and
         tLiMacFilterParamsId."
    ::= { tLiMacFilterParamsEntry 1 }

tLiMacFilterParamsRowStatus      OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsRowStatus specifies the status of this
         row."
    ::= { tLiMacFilterParamsEntry 2 }

tLiMacFilterParamsLastChanged    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsLastChanged indicates the sysUpTime at
         the time of the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tLiMacFilterParamsEntry 3 }

tLiMacFilterParamsDescription    OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsDescription specifies a description for
         this entry."
    DEFVAL      { ''H }
    ::= { tLiMacFilterParamsEntry 4 }

tLiMacFilterParamsFrameType      OBJECT-TYPE
    SYNTAX      TFrameType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsFrameType specifies the type of mac frame
         for which we are defining this match criterion."
    DEFVAL      { e802dot3 }
    ::= { tLiMacFilterParamsEntry 5 }

tLiMacFilterParamsSrcMAC         OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsSrcMAC specifies the source MAC address
         to match for this LI MAC filter entry."
    DEFVAL      { '000000000000'H }
    ::= { tLiMacFilterParamsEntry 6 }

tLiMacFilterParamsSrcMACMask     OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsSrcMACMask specifies the source MAC mask
         value for this LI MAC filter match entry. The mask is ANDed with the
         MAC to match tLiMacFilterParamsSrcMAC. A cleared bit means ignore this
         bit, do not match. A set bit means match this bit with
         tLiMacFilterParamsSrcMAC. Use the value 00-00-00-00-00-00 to disable
         this filter criterion. If set to all zero, the value of
         tLiMacFilterParamsSrcMAC will be set to all zero by the system, and
         any attempt to change this value will be ignored."
    DEFVAL      { '000000000000'H }
    ::= { tLiMacFilterParamsEntry 7 }

tLiMacFilterParamsDstMAC         OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsDstMAC specifies the destination MAC to
         match for this LI MAC filter entry."
    DEFVAL      { '000000000000'H }
    ::= { tLiMacFilterParamsEntry 8 }

tLiMacFilterParamsDstMACMask     OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsDstMACMask specifies the destination MAC
         mask value for this LI MAC filter match entry. The mask is ANDed with
         the MAC to match tLiMacFilterParamsDstMAC. A cleared bit means ignore
         this bit, do not match. A set bit means match this bit with
         tLiMacFilterParamsDstMAC. Use the value 00-00-00-00-00-00 to disable
         this filter criteria. If set to all zero, the value of
         tLiMacFilterParamsDstMAC will be set to all zero by the system, and
         any attempt to change this value will be ignored."
    DEFVAL      { '000000000000'H }
    ::= { tLiMacFilterParamsEntry 9 }

tLiMacFilterParamsIngrHitCount   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiMacFilterParamsIngrHitCount indicates the number of
         times an ingress packet matched this entry."
    ::= { tLiMacFilterParamsEntry 10 }

tLiMacFilterParamsEgrHitCount    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object tLiMacFilterParamsEgrHitCount indicates the number of
         times an egress packet matched this entry."
    ::= { tLiMacFilterParamsEntry 11 }

tLiMacFilterParamsIngrHitBytes   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tLiMacFilterParamsIngrHitBytes indicates the number of
         bytes of all ingress packets that matched this entry."
    ::= { tLiMacFilterParamsEntry 12 }

tLiMacFilterParamsEgrHitBytes    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tLiMacFilterParamsEgrHitBytes indicates the number of
         bytes of all egress packets that matched this entry."
    ::= { tLiMacFilterParamsEntry 13 }

tLiMacFilterParamsSapPortId      OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tLiMacFilterParamsSapPortId specifies the sap port id to
         match for this LI MAC filter entry.

         The value 0 indicates that there is no SAP match is defined."
    DEFVAL      { 0 }
    ::= { tLiMacFilterParamsEntry 14 }

tLiMacFilterParamsSapEncapType   OBJECT-TYPE
    SYNTAX      TmnxPortEncapType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tLiMacFilterParamsSapEncapType specifies the sap port
         encap value to match for this LI MAC filter entry.

         The supported values are 'unknown' and 'qinqEncap'."
    DEFVAL      { unknown }
    ::= { tLiMacFilterParamsEntry 15 }

tLiMacFilterParamsSapEncapVal    OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tLiMacFilterParamsSapEncapVal specifies the sap port
         encap value to match for this LI MAC filter entry.

         The supported values are those representing 'val.*'."
    DEFVAL      { 0 }
    ::= { tLiMacFilterParamsEntry 16 }

tLiMacFilterParamsOuterTagVal    OBJECT-TYPE
    SYNTAX      QTagOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tLiMacFilterParamsOuterTagVal specifies the value to
         match against the VID of the first VLAN tag in the packet that is
         carried transparently through the service (the first vlan tag after
         the service delimiting tags).

         This object can only be set if tMacFilterType is set to 'vid(3)'.

         The (default) value of '-1' indicates no outer VLAN tag matching will
         be performed."
    DEFVAL      { -1 }
    ::= { tLiMacFilterParamsEntry 17 }

tLiIpFilterParamsTableLastChg    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsTableLastChg indicates the
         sysUpTime at the time of the last modification of
         tLiIpFilterParamsTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterLiObjects 15 }

tLiIpFilterParamsTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TLiIpFilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tLiIpFilterParamsTable contains information pertaining to
         match entries of LI IP/IPv6 filters."
    ::= { tFilterLiObjects 16 }

tLiIpFilterParamsEntry           OBJECT-TYPE
    SYNTAX      TLiIpFilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry represents a configuration of an LI IP/IPv6 filter entry.

         Entries can be created and deleted via SNMP SET operations to
         tLiIpFilterParamsRowStatus."
    INDEX       {
        tLiFilterType,
        tLiFilterName,
        tLiIpFilterParamsId
    }
    ::= { tLiIpFilterParamsTable 1 }

TLiIpFilterParamsEntry           ::= SEQUENCE
{
    tLiIpFilterParamsId              TLimitedEntryId,
    tLiIpFilterParamsLastChanged     TimeStamp,
    tLiIpFilterParamsRowStatus       RowStatus,
    tLiIpFilterParamsDescription     TItemDescription,
    tLiIpFilterParamsSrcIpAddrType   InetAddressType,
    tLiIpFilterParamsSrcIpAddr       InetAddress,
    tLiIpFilterParamsSrcIpFullMask   InetAddress,
    tLiIpFilterParamsDstIpAddrType   InetAddressType,
    tLiIpFilterParamsDstIpAddr       InetAddress,
    tLiIpFilterParamsDstIpFullMask   InetAddress,
    tLiIpFilterParamsProtocolNextHdr TIpProtocol,
    tLiIpFilterParamsSrcPortValue1   TTcpUdpPort,
    tLiIpFilterParamsSrcPortValue2   TTcpUdpPort,
    tLiIpFilterParamsSrcPortOper     TOperator,
    tLiIpFilterParamsDstPortValue1   TTcpUdpPort,
    tLiIpFilterParamsDstPortValue2   TTcpUdpPort,
    tLiIpFilterParamsDstPortOper     TOperator,
    tLiIpFilterParamsFragment        TItemMatch
}

tLiIpFilterParamsId              OBJECT-TYPE
    SYNTAX      TLimitedEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsId indicates the tertiary
         index for tLiIpFilterParamsEntry.

         Every LI IP filter may have multiple match entries therefore every
         entry is identified by the values of tLiFilterType, tLiFilterName and
         tLiIpFilterParamsId."
    ::= { tLiIpFilterParamsEntry 1 }

tLiIpFilterParamsLastChanged     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsLastChanged indicates the
         sysUpTime at the time of the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tLiIpFilterParamsEntry 2 }

tLiIpFilterParamsRowStatus       OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsRowStatus specifies the
         status of this row in tLiIpFilterParamsTable."
    ::= { tLiIpFilterParamsEntry 3 }

tLiIpFilterParamsDescription     OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsDescription specifies the
         description for this LI IP filter entry."
    DEFVAL      { ''H }
    ::= { tLiIpFilterParamsEntry 4 }

tLiIpFilterParamsSrcIpAddrType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsSrcIpAddrType specifies the
         context in which the values of the objects tLiIpFilterParamsSrcIpAddr
         and tLiIpFilterParamsSrcIpFullMask are interpreted.

         Only following values are supported:
            unknown(0)
            ipv4(1)
            ipv6(2)

         Furthermore the value must be consistent with the filter type given by
         the value of the index object tLiFilterType.

         If the value of this object is set to 'unknown' then the values of the
         objects tLiIpFilterParamsSrcIpAddr and tLiIpFilterParamsSrcIpFullMask
         are automatically set to their default values."
    DEFVAL      { unknown }
    ::= { tLiIpFilterParamsEntry 5 }

tLiIpFilterParamsSrcIpAddr       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsSrcIpAddr specifies the
         source IP address to be matched by this LI IP filter entry.

         The value must be consistent with the IP version value of the
         associated tLiIpFilterParamsSrcIpAddrType object.

         If the value of the object tLiIpFilterParamsSrcIpAddrType is set to
         'unknown' then the value of this object is automatically set to the
         default value."
    DEFVAL      { ''H }
    ::= { tLiIpFilterParamsEntry 6 }

tLiIpFilterParamsSrcIpFullMask   OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsSrcIpFullMask specifies the
         IP mask value that is ANDed with the received source IP address to
         match the value in tLiIpFilterParamsSrcIpAddr.

         The value must be consistent with the IP version value of the
         associated tLiIpFilterParamsSrcIpAddrType object and must not be equal
         to zero.

         If the value of the object tLiIpFilterParamsSrcIpAddrType is set to
         'unknown' then the value of this object is automatically set to the
         default value."
    DEFVAL      { ''H }
    ::= { tLiIpFilterParamsEntry 7 }

tLiIpFilterParamsDstIpAddrType   OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsDstIpAddrType specifies the
         context in which the values of the objects tLiIpFilterParamsDstIpAddr
         and tLiIpFilterParamsDstIpFullMask are interpreted.

         Only following values are supported:
            unknown(0)
            ipv4(1)
            ipv6(2)

         Furthermore the value must always be consistent with the filter type
         given by the value of the index object tLiFilterType.

         If the value of this object is set to 'unknown' then the values of the
         objects tLiIpFilterParamsDstIpAddr and tLiIpFilterParamsDstIpFullMask
         are automatically set to their default values."
    DEFVAL      { unknown }
    ::= { tLiIpFilterParamsEntry 8 }

tLiIpFilterParamsDstIpAddr       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsDstIpAddr specifies the
         destination IP address to be matched by this LI IP filter entry.

         The value must be consistent with the IP version value of the
         associated tLiIpFilterParamsDstIpAddrType object.

         If the value of the object tLiIpFilterParamsDstIpAddrType is set to
         'unknown' then the value of this object is automatically set to the
         default value."
    DEFVAL      { ''H }
    ::= { tLiIpFilterParamsEntry 9 }

tLiIpFilterParamsDstIpFullMask   OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsDstIpFullMask specifies the
         IP mask value that is ANDed with the received destination IP address
         to match the value in tLiIpFilterParamsDstIpAddr.

         The value must be consistent with the IP version value of the
         associated tLiIpFilterParamsDstIpAddrType object and must not be equal
         to zero.

         If the value of the object tLiIpFilterParamsDstIpAddrType is set to
         'unknown' then the value of this object is automatically set to the
         default value."
    DEFVAL      { ''H }
    ::= { tLiIpFilterParamsEntry 10 }

tLiIpFilterParamsProtocolNextHdr OBJECT-TYPE
    SYNTAX      TIpProtocol
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsProtocolNextHdr specifies
         (depending on the filter type defined by the value of the object
         tLiFilterType) the IP protocol / IPv6 next-header value to be matched
         by this LI IP filter entry.

         The value must be set to -1 to disable the protocol / next-header
         matching."
    DEFVAL      { -1 }
    ::= { tLiIpFilterParamsEntry 11 }

tLiIpFilterParamsSrcPortValue1   OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsSrcPortValue1 specifies the
         TCP/UDP source port value1. It is used as per the description of
         tLiIpFilterParamsSrcPortOper."
    DEFVAL      { 0 }
    ::= { tLiIpFilterParamsEntry 12 }

tLiIpFilterParamsSrcPortValue2   OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsSrcPortValue2 specifies the
         TCP/UDP source port value2. It is used as per the description of
         tLiIpFilterParamsSrcPortOper."
    DEFVAL      { 0 }
    ::= { tLiIpFilterParamsEntry 13 }

tLiIpFilterParamsSrcPortOper     OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsSrcPortOper specifies the
         manner in which tLiIpFilterParamsSrcPortValue1 and
         tLiIpFilterParamsSrcPortValue2 are to be used. The values of these
         latter 2 objects and tLiIpFilterParamsSrcPortOper are used as per the
         description of TTcpUdpPortOperator."
    DEFVAL      { none }
    ::= { tLiIpFilterParamsEntry 14 }

tLiIpFilterParamsDstPortValue1   OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsDstPortValue1 specifies the
         TCP/UDP destination port value1. It is used as per the description of
         tLiIpFilterParamsDstPortOper."
    DEFVAL      { 0 }
    ::= { tLiIpFilterParamsEntry 15 }

tLiIpFilterParamsDstPortValue2   OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsDstPortValue2 specifies the
         TCP/UDP destination port value2. It is used as per the description of
         tLiIpFilterParamsDstPortOper."
    DEFVAL      { 0 }
    ::= { tLiIpFilterParamsEntry 16 }

tLiIpFilterParamsDstPortOper     OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFilterParamsDstPortOper specifies the
         manner in which tLiIpFilterParamsDstPortValue1 and
         tLiIpFilterParamsDstPortValue2 are to be used. The values of these
         latter 2 objects and tLiIpFilterParamsDstPortOper are used as per the
         description in TTcpUdpPortOperator."
    DEFVAL      { none }
    ::= { tLiIpFilterParamsEntry 17 }

tLiIpFilterParamsFragment        OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If enabled, matches fragmented/unfragmented packets as per value of
         the object. The fragment match criterion is not supported for IPv6
         filter."
    DEFVAL      { off }
    ::= { tLiIpFilterParamsEntry 18 }

tLiIpFilterParamsInfoTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TLiIpFilterParamsInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tLiIpFilterParamsInfoTable contains read-only information
         pertaining to LI IP filter match entries of LI IP filters."
    ::= { tFilterLiObjects 17 }

tLiIpFilterParamsInfoEntry       OBJECT-TYPE
    SYNTAX      TLiIpFilterParamsInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This row complements the corresponding row in the
         tLiIpFilterParamsTable with read-only operational info.

         Entries are created and deleted automatically by the system when a
         corresponding entry in tLiIpFilterParamsTable is created / deleted."
    AUGMENTS    { tLiIpFilterParamsEntry }
    ::= { tLiIpFilterParamsInfoTable 1 }

TLiIpFilterParamsInfoEntry       ::= SEQUENCE
{
    tLiIpFltrParamsInfIngrHitCount   Counter64,
    tLiIpFltrParamsInfEgrHitCount    Counter64,
    tLiIpFltrParamsInfIngrHitBytes   Counter64,
    tLiIpFltrParamsInfEgrHitBytes    Counter64
}

tLiIpFltrParamsInfIngrHitCount   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFltrParamsInfIngrHitCount indicates the
         number of times an ingress packet matched this entry."
    ::= { tLiIpFilterParamsInfoEntry 1 }

tLiIpFltrParamsInfEgrHitCount    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFltrParamsInfEgrHitCount indicates the
         number of times an egress packet matched this entry."
    ::= { tLiIpFilterParamsInfoEntry 2 }

tLiIpFltrParamsInfIngrHitBytes   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFltrParamsInfIngrHitBytes indicates the
         number of bytes of all ingress packets that matched this entry."
    ::= { tLiIpFilterParamsInfoEntry 3 }

tLiIpFltrParamsInfEgrHitBytes    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tLiIpFltrParamsInfEgrHitBytes indicates the
         number of bytes of all egress packets that matched this entry."
    ::= { tLiIpFilterParamsInfoEntry 4 }

tLiRsvdBlockFltrAssocTableLChg   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tLiRsvdBlockFltrAssocTableLChg indicates the sysUpTime at
         the time of the last modification of tLiRsvdBlockFltrAssocTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterLiObjects 18 }

tLiRsvdBlockFltrAssocTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TLiRsvdBlockFltrAssocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tLiRsvdBlockFltrAssocTable contains associations between
         normal filters and LI block reservations. The
         tLiRsvdBlockFltrAssocTable associates filters by filter name in the
         contrast with tLiReservedBlockFltrTable which contains associations
         via filter id."
    ::= { tFilterLiObjects 19 }

tLiRsvdBlockFltrAssocEntry       OBJECT-TYPE
    SYNTAX      TLiRsvdBlockFltrAssocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An association of a normal filter with an LI block reservation. In
         this release MAC, IP and IPv6 filters are supported."
    INDEX       {
        tLiReservedBlockName,
        tLiRsvdBlockFltrAssocFltrType,
        tLiRsvdBlockFltrAssocFltrName
    }
    ::= { tLiRsvdBlockFltrAssocTable 1 }

TLiRsvdBlockFltrAssocEntry       ::= SEQUENCE
{
    tLiRsvdBlockFltrAssocFltrType    TFilterType,
    tLiRsvdBlockFltrAssocFltrName    TLNamedItem,
    tLiRsvdBlockFltrAssocRowStatus   RowStatus,
    tLiRsvdBlockFltrAssocLastChanged TimeStamp
}

tLiRsvdBlockFltrAssocFltrType    OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiRsvdBlockFltrAssocFltrType specifies the type of filter
         this LI block reservation applies to.

         In this release MAC and IP/IPv6 filters are supported:
             fltrtypeselIp     (1)
             fltrtypeselMac    (2)
             fltrtypeselIpv6   (4)"
    ::= { tLiRsvdBlockFltrAssocEntry 1 }

tLiRsvdBlockFltrAssocFltrName    OBJECT-TYPE
    SYNTAX      TLNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiRsvdBlockFltrAssocFltrName specifies the ID of the
         filter associated with this LI reserved block.

         The scope of associated filter (tIPFilterScope, tIPv6FilterScope,
         tMacFilterScope) must not equal to embedded(3)."
    ::= { tLiRsvdBlockFltrAssocEntry 3 }

tLiRsvdBlockFltrAssocRowStatus   OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiRsvdBlockFltrAssocRowStatus specifies the status of this
         row."
    ::= { tLiRsvdBlockFltrAssocEntry 4 }

tLiRsvdBlockFltrAssocLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiRsvdBlockFltrAssocLastChanged indicates the sysUpTime at
         the time of the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tLiRsvdBlockFltrAssocEntry 5 }

tLiFltrAssocFltrNameTableLastChg OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiFilterAssociationTableLastChg indicates the sysUpTime at
         the time of the last modification of tLiFltrAssocFltrNameTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterLiObjects 20 }

tLiFltrAssocFltrNameTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TLiFltrAssocFltrNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tLiFltrAssocFltrNameTable contains information about the
         associations between LI filters and normal filters."
    ::= { tFilterLiObjects 21 }

tLiFltrAssocFltrNameEntry        OBJECT-TYPE
    SYNTAX      TLiFltrAssocFltrNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An association between an LI filter and a normal filter."
    INDEX       {
        tLiFilterType,
        tLiFilterName,
        tLiFltrAssocFltrName
    }
    ::= { tLiFltrAssocFltrNameTable 1 }

TLiFltrAssocFltrNameEntry        ::= SEQUENCE
{
    tLiFltrAssocFltrName             TLNamedItem,
    tLiFltrAssocFltrNameRowStatus    RowStatus,
    tLiFltrAssocFltrNameLastChg      TimeStamp
}

tLiFltrAssocFltrName             OBJECT-TYPE
    SYNTAX      TLNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tLiFltrAssocFltrName indicates the name of the normal
         filter in the association described by this entry."
    ::= { tLiFltrAssocFltrNameEntry 1 }

tLiFltrAssocFltrNameRowStatus    OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tLiFltrAssocFltrNameRowStatus specifies the status of this
         row."
    ::= { tLiFltrAssocFltrNameEntry 2 }

tLiFltrAssocFltrNameLastChg      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tLiFltrAssocFltrNameLastChg indicates the sysUpTime at the
         time of the last modification of this entry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tLiFltrAssocFltrNameEntry 3 }

tFilterPrefixListTableLstChng    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterPrefixListTableLstChng indicates the sysUpTime at
         the time of the last modification of tFilterPrefixListTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 32 }

tFilterPrefixListTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterPrefixListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterPrefixListTable contains an entry for each prefix
         list defined in the filter area."
    ::= { tFilterObjects 33 }

tFilterPrefixListEntry           OBJECT-TYPE
    SYNTAX      TFilterPrefixListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterPrefixListTable."
    INDEX       {
        tFilterPrefixListType,
        IMPLIED tFilterPrefixListName
    }
    ::= { tFilterPrefixListTable 1 }

TFilterPrefixListEntry           ::= SEQUENCE
{
    tFilterPrefixListType            TFltrPrefixListType,
    tFilterPrefixListName            TNamedItem,
    tFilterPrefixListRowStatus       RowStatus,
    tFilterPrefixListLastChanged     TimeStamp,
    tFilterPrefixListDescription     TItemDescription
}

tFilterPrefixListType            OBJECT-TYPE
    SYNTAX      TFltrPrefixListType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFilterPrefixListType specifies the type of prefix list for
         the prefix list tFilterPrefixListName."
    ::= { tFilterPrefixListEntry 1 }

tFilterPrefixListName            OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFilterPrefixListName specifies the name given to this
         prefix list."
    ::= { tFilterPrefixListEntry 2 }

tFilterPrefixListRowStatus       OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterPrefixListRowStatus specifies the status of this
         row."
    ::= { tFilterPrefixListEntry 3 }

tFilterPrefixListLastChanged     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterPrefixListLastChanged indicates the sysUpTime at the
         time of the last modification of this row.

         If no changes were made to the row since the last re-initialization of
         the local network management subsystem, then this object contains the
         value zero."
    ::= { tFilterPrefixListEntry 4 }

tFilterPrefixListDescription     OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterPrefixListDescription specifies a description for
         this row."
    DEFVAL      { ''H }
    ::= { tFilterPrefixListEntry 5 }

tFilterPrefixListEntryTblLstChg  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterPrefixListEntryTblLstChg indicates the sysUpTime at
         the time of the last modification of tFilterPrefixListEntryTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 34 }

tFilterPrefixListEntryTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterPrefixListEntryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterPrefixListEntryTable contains information pertaining
         to explicitly created prefixes in any prefix list defined in the
         filter area."
    ::= { tFilterObjects 35 }

tFilterPrefixListEntryEntry      OBJECT-TYPE
    SYNTAX      TFilterPrefixListEntryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterPrefixListEntryTable."
    INDEX       {
        tFilterPrefixListType,
        tFilterPrefixListName,
        tFilterPrefixListEntryPrefixType,
        tFilterPrefixListEntryPrefix,
        tFilterPrefixListEntryPrefixLen
    }
    ::= { tFilterPrefixListEntryTable 1 }

TFilterPrefixListEntryEntry      ::= SEQUENCE
{
    tFilterPrefixListEntryPrefixType TmnxAddressAndPrefixType,
    tFilterPrefixListEntryPrefix     TmnxAddressAndPrefixAddress,
    tFilterPrefixListEntryPrefixLen  TmnxAddressAndPrefixPrefix,
    tFilterPrefixListEntryRowStatus  RowStatus
}

tFilterPrefixListEntryPrefixType OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFilterPrefixListEntryPrefixType specifies whether the
         prefix specified in tFilterPrefixListEntryPrefix is an IPv4 or IPv6
         prefix.

         The value of tFilterPrefixListEntryPrefixType must match the value of
         the object tFilterPrefixListType."
    ::= { tFilterPrefixListEntryEntry 1 }

tFilterPrefixListEntryPrefix     OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFilterPrefixListEntryPrefix specifies the IP prefix of
         this prefix list entry."
    ::= { tFilterPrefixListEntryEntry 2 }

tFilterPrefixListEntryPrefixLen  OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixPrefix
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFilterPrefixListEntryPrefixLen specifies the IP prefix
         length of this prefix list entry."
    ::= { tFilterPrefixListEntryEntry 3 }

tFilterPrefixListEntryRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterPrefixListEntryRowStatus specifies the status of
         this row."
    ::= { tFilterPrefixListEntryEntry 4 }

tFilterEmbeddedRefTableLstChg    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterEmbeddedRefTableLstChg indicates the sysUpTime at
         the time of the last modification of tFilterEmbeddedRefTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 36 }

tFilterEmbeddedRefTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterEmbeddedRefTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterEmbeddedRefTable contains an entry for each embedded
         filter inserted in a filter with scope other than 'embedded'."
    ::= { tFilterObjects 37 }

tFilterEmbeddedRefTableEntry     OBJECT-TYPE
    SYNTAX      TFilterEmbeddedRefTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterEmbeddedRefTable."
    INDEX       {
        tFilterEmbeddedRefFilterType,
        tFilterEmbeddedRefInsertFltrId,
        tFilterEmbeddedRefEmbeddedFltrId,
        tFilterEmbeddedRefOffset
    }
    ::= { tFilterEmbeddedRefTable 1 }

TFilterEmbeddedRefTableEntry     ::= SEQUENCE
{
    tFilterEmbeddedRefFilterType     TFilterType,
    tFilterEmbeddedRefInsertFltrId   TFilterID,
    tFilterEmbeddedRefEmbeddedFltrId TFilterID,
    tFilterEmbeddedRefOffset         TFilterEmbedOffset,
    tFilterEmbeddedRefRowStatus      RowStatus,
    tFilterEmbeddedRefAdminState     TmnxEmbeddedFltrAdminState,
    tFilterEmbeddedRefOperState      TmnxEmbeddedFltrOperState,
    tFilterEmbeddedRefLastChanged    TimeStamp
}

tFilterEmbeddedRefFilterType     OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFilterEmbeddedRefFilterType specifies the type of filter
         for the filters specified by tFilterEmbeddedRefEmbeddedFltrId and
         tFilterEmbeddedRefInsertFltrId."
    ::= { tFilterEmbeddedRefTableEntry 1 }

tFilterEmbeddedRefInsertFltrId   OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbeddedRefInsertFltrId specifies the filter where
         the filter specified by tFilterEmbeddedRefEmbeddedFltrId is to be
         inserted."
    ::= { tFilterEmbeddedRefTableEntry 2 }

tFilterEmbeddedRefEmbeddedFltrId OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbeddedRefEmbeddedFltrId specifies the id of the
         filter to be inserted in the filter specified by
         tFilterEmbeddedRefInsertFltrId."
    ::= { tFilterEmbeddedRefTableEntry 3 }

tFilterEmbeddedRefOffset         OBJECT-TYPE
    SYNTAX      TFilterEmbedOffset
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbeddedRefOffset specifies the offset of inserted
         entries."
    ::= { tFilterEmbeddedRefTableEntry 4 }

tFilterEmbeddedRefRowStatus      OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterEmbeddedRefRowStatus specifies the status of this
         row."
    ::= { tFilterEmbeddedRefTableEntry 5 }

tFilterEmbeddedRefAdminState     OBJECT-TYPE
    SYNTAX      TmnxEmbeddedFltrAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbeddedRefAdminState specifies the administrative
         state of the embed request defined by this row.

         If an active embedding cannot be fulfilled due to dynamic events, this
         object will be set to 'inactive' automatically by the system. In those
         cases, the object tFilterEmbeddedRefOperState will indicate the
         failure reason."
    DEFVAL      { active }
    ::= { tFilterEmbeddedRefTableEntry 6 }

tFilterEmbeddedRefOperState      OBJECT-TYPE
    SYNTAX      TmnxEmbeddedFltrOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbeddedRefOperState indicates the operational
         state of the embed request defined by this row."
    ::= { tFilterEmbeddedRefTableEntry 7 }

tFilterEmbeddedRefLastChanged    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbeddedRefLastChanged indicates the sysUpTime at
         the time of last change to this row in tFilterEmbeddedRefTable."
    ::= { tFilterEmbeddedRefTableEntry 8 }

tFilterPortListTableLstChng      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterPortListTableLstChng indicates the sysUpTime at the
         time of the last modification of tFilterPortListTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 38 }

tFilterPortListTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterPortListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterPortListTable contains an entry for each port list
         defined in the filter area."
    ::= { tFilterObjects 39 }

tFilterPortListEntry             OBJECT-TYPE
    SYNTAX      TFilterPortListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterPortListTable."
    INDEX       { IMPLIED tFilterPortListName }
    ::= { tFilterPortListTable 1 }

TFilterPortListEntry             ::= SEQUENCE
{
    tFilterPortListName              TNamedItem,
    tFilterPortListRowStatus         RowStatus,
    tFilterPortListLastChanged       TimeStamp,
    tFilterPortListDescription       TItemDescription
}

tFilterPortListName              OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFilterPortListName specifies the name given to this port
         list."
    ::= { tFilterPortListEntry 1 }

tFilterPortListRowStatus         OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterPortListRowStatus specifies the status of this row."
    ::= { tFilterPortListEntry 2 }

tFilterPortListLastChanged       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterPortListLastChanged indicates the sysUpTime at the
         time of the last modification of this row.

         If no changes were made to the row since the last re-initialization of
         the local network management subsystem, then this object contains the
         value zero."
    ::= { tFilterPortListEntry 3 }

tFilterPortListDescription       OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterPortListDescription specifies a description for this
         row."
    DEFVAL      { ''H }
    ::= { tFilterPortListEntry 4 }

tFilterPortListEntryTblLstChg    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterPortListEntryTblLstChg indicates the sysUpTime at
         the time of the last modification of tFilterPortListEntryTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 40 }

tFilterPortListEntryTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterPortListEntryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterPortListEntryTable contains an entry for each port
         defined in any port list defined in the filter area."
    ::= { tFilterObjects 41 }

tFilterPortListEntryEntry        OBJECT-TYPE
    SYNTAX      TFilterPortListEntryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Specifies an entry in the tFilterPortListEntryTable. Two entries for
         the same port list must not overlap."
    INDEX       {
        tFilterPortListName,
        tFilterPortListEntryPortLow,
        tFilterPortListEntryPortHigh
    }
    ::= { tFilterPortListEntryTable 1 }

TFilterPortListEntryEntry        ::= SEQUENCE
{
    tFilterPortListEntryPortLow      TTcpUdpPort,
    tFilterPortListEntryPortHigh     TTcpUdpPort,
    tFilterPortListEntryRowStatus    RowStatus
}

tFilterPortListEntryPortLow      OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This object specifies the lower value for the TCP/UDP port range. A
         value assigned to this object must be less than or equal to the value
         assigned to the corresponding object tFilterPortListEntryPortHigh."
    ::= { tFilterPortListEntryEntry 1 }

tFilterPortListEntryPortHigh     OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This object specifies the higher value for the TCP/UDP port range. A
         value assigned to this object must be greater than or equal to the
         value assigned to the corresponding object
         tFilterPortListEntryPortLow."
    ::= { tFilterPortListEntryEntry 2 }

tFilterPortListEntryRowStatus    OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterPortListEntryRowStatus specifies the status of this
         row."
    ::= { tFilterPortListEntryEntry 3 }

tFilterApplyPathTableLstChng     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterApplyPathTableLstChng indicates the sysUpTime at the
         time of the last modification of tFilterApplyPathTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 42 }

tFilterApplyPathTable            OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterApplyPathEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterApplyPathTable contains an entry for each apply-path
         rule defined in a prefix list."
    ::= { tFilterObjects 43 }

tFilterApplyPathEntry            OBJECT-TYPE
    SYNTAX      TFilterApplyPathEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterApplyPathTable describing an apply-path rule.

         If an address or prefix configured by the source specified by
         tFilterApplyPathSource matches the conditions specified by
         tFilterApplyPathMatch1 and tFilterApplyPathMatch2, a prefix is
         inserted into the prefix list where this apply-path rule refers to."
    INDEX       {
        tFilterPrefixListType,
        tFilterPrefixListName,
        tFilterApplyPathSource,
        tFilterApplyPathIndex
    }
    ::= { tFilterApplyPathTable 1 }

TFilterApplyPathEntry            ::= SEQUENCE
{
    tFilterApplyPathSource           INTEGER,
    tFilterApplyPathIndex            Unsigned32,
    tFilterApplyPathRowStatus        RowStatus,
    tFilterApplyPathLastChanged      TimeStamp,
    tFilterApplyPathMatch1           TRegularExpression,
    tFilterApplyPathMatch2           TRegularExpression,
    tFilterApplyPathVRtrId           TmnxVRtrID
}

tFilterApplyPathSource           OBJECT-TYPE
    SYNTAX      INTEGER {
        unknown   (0),
        bgp-peers (1)
    }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFilterApplyPathSource specifies the source of the prefixes
         that will be generated by this apply-path rule."
    ::= { tFilterApplyPathEntry 1 }

tFilterApplyPathIndex            OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFilterApplyPathIndex specifies an index for this row."
    ::= { tFilterApplyPathEntry 2 }

tFilterApplyPathRowStatus        OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterApplyPathRowStatus specifies the status of this row."
    ::= { tFilterApplyPathEntry 3 }

tFilterApplyPathLastChanged      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterApplyPathLastChanged indicates the timestamp of the
         last change to this row."
    ::= { tFilterApplyPathEntry 4 }

tFilterApplyPathMatch1           OBJECT-TYPE
    SYNTAX      TRegularExpression
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterApplyPathMatch1 specifies a regular expression. The
         usage of this object depends on the source specified by
         tFilterApplyPathSource.

         If tFilterApplyPathSource is 'bgp-peers', this object specifies a
         match condition on the group-name of configured bgp peers."
    DEFVAL      { ''H }
    ::= { tFilterApplyPathEntry 5 }

tFilterApplyPathMatch2           OBJECT-TYPE
    SYNTAX      TRegularExpression
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFilterApplyPathMatch2 specifies a regular expression. The
         usage of this object depends on the source specified by
         tFilterApplyPathSource.

         If tFilterApplyPathSource is 'bgp-peers', this object specifies a
         match condition on the ip or IPv6 address of configured bgp peers."
    DEFVAL      { ''H }
    ::= { tFilterApplyPathEntry 6 }

tFilterApplyPathVRtrId           OBJECT-TYPE
    SYNTAX      TmnxVRtrID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterApplyPathVRtrId specifies virtual
         router instance. The usage of this object depends on the source
         specified by tFilterApplyPathSource.

         If tFilterApplyPathSource is 'bgp-peers' then prefixes generated by
         apply-path rule will consist of bgp-peers pertaining to virtual router
         instance specified by this object."
    DEFVAL      { 1 }
    ::= { tFilterApplyPathEntry 7 }

tFilterEmbeddedRefInfoTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterEmbeddedRefInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterEmbeddedRefInfoTable contains an entry for each
         embedded filter inserted in a filter with scope other than 'embedded'.

         This row complements the corresponding row in the
         tFilterEmbeddedRefTable with read-only operational info."
    ::= { tFilterObjects 44 }

tFilterEmbeddedRefInfoEntry      OBJECT-TYPE
    SYNTAX      TFilterEmbeddedRefInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterEmbeddedRefInfoTable."
    AUGMENTS    { tFilterEmbeddedRefTableEntry }
    ::= { tFilterEmbeddedRefInfoTable 1 }

TFilterEmbeddedRefInfoEntry      ::= SEQUENCE
{
    tFltrEmbedRefInfEntryCnt         Unsigned32,
    tFltrEmbedRefInfEntryCntInsrtd   Unsigned32
}

tFltrEmbedRefInfEntryCnt         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedRefInfEntryCnt indicates how many entries are
         present in the embedded filter as specified in
         tFilterEmbeddedRefEmbeddedFltrId."
    ::= { tFilterEmbeddedRefInfoEntry 1 }

tFltrEmbedRefInfEntryCntInsrtd   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedRefInfEntryCntInsrtd indicates how many entries
         of the embedded filter (specified by tFilterEmbeddedRefEmbeddedFltrId)
         are actually placed inside the filter (specified by
         tFilterEmbeddedRefInsertFltrId).

         If the object tFilterEmbeddedRefOperState is different from
         'in-service' this object will always be zero.

         Else, the difference between the value of this object and the value of
         tFltrEmbedRefInfEntryCnt indicates how many entries of the embedded
         filter were overwritten by local entries in the embedding filter."
    ::= { tFilterEmbeddedRefInfoEntry 2 }

tFilterEmbeddedEntryRefInfoTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterEmbeddedEntryRefInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterEmbeddedEntryRefInfoTable contains an entry for each
         embedded filter entry inserted in a filter with scope other than
         'embedded'."
    ::= { tFilterObjects 45 }

tFilterEmbeddedEntryRefInfoEntry OBJECT-TYPE
    SYNTAX      TFilterEmbeddedEntryRefInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterEmbeddedEntryRefInfoTable. Rows in the
         tFilterEmbeddedEntryRefInfoTable are created by the SYSTEM when an
         embedded filter is inserted into a filter with scope other than
         'embedded'. They are destroyed by the SYSTEM when an embedded filter
         is removed from a filter with scope other than 'embedded'."
    INDEX       {
        tFltrEmbedEntryFilterType,
        tFltrEmbedEntryInsertFltrId,
        tFltrEmbedEntryEmbeddedFltrId,
        tFltrEmbedEntryEmbeddedEntryId
    }
    ::= { tFilterEmbeddedEntryRefInfoTable 1 }

TFilterEmbeddedEntryRefInfoEntry ::= SEQUENCE
{
    tFltrEmbedEntryFilterType        TFilterType,
    tFltrEmbedEntryInsertFltrId      TFilterID,
    tFltrEmbedEntryEmbeddedFltrId    TFilterID,
    tFltrEmbedEntryEmbeddedEntryId   TEntryId,
    tFltrEmbedEntryInsrtEntryId      TAnyEntryId,
    tFltrEmbedEntryRefOperState      TmnxFltrEmbeddedEntryState
}

tFltrEmbedEntryFilterType        OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrEmbedEntryFilterType specifies a filter type for the
         filters specified by tFltrEmbedEntryInsertFltrId and
         tFltrEmbedEntryEmbeddedFltrId."
    ::= { tFilterEmbeddedEntryRefInfoEntry 1 }

tFltrEmbedEntryInsertFltrId      OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedEntryInsertFltrId specifies the filter where
         the filter specified by tFltrEmbedEntryEmbeddedFltrId is inserted."
    ::= { tFilterEmbeddedEntryRefInfoEntry 2 }

tFltrEmbedEntryEmbeddedFltrId    OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedEntryEmbeddedFltrId specifies the ID of the
         filter inserted in the filter specified by
         tFltrEmbedEntryInsertFltrId."
    ::= { tFilterEmbeddedEntryRefInfoEntry 3 }

tFltrEmbedEntryEmbeddedEntryId   OBJECT-TYPE
    SYNTAX      TEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedEntryEmbeddedEntryId specifies the ID of the
         entry inside of the filter specified by tFltrEmbedEntryEmbeddedFltrId."
    ::= { tFilterEmbeddedEntryRefInfoEntry 4 }

tFltrEmbedEntryInsrtEntryId      OBJECT-TYPE
    SYNTAX      TAnyEntryId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedEntryInsrtEntryId indicates which entry in the
         filter specified by tFltrEmbedEntryInsertFltrId corresponds to the
         entry specified by tFltrEmbedEntryEmbeddedEntryId in the filter
         specified by tFltrEmbedEntryEmbeddedFltrId."
    ::= { tFilterEmbeddedEntryRefInfoEntry 5 }

tFltrEmbedEntryRefOperState      OBJECT-TYPE
    SYNTAX      TmnxFltrEmbeddedEntryState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedEntryRefOperState indicates the current status
         of the entry identified by tFltrEmbedEntryEmbeddedEntryId of the
         filter identified by tFltrEmbedEntryEmbeddedFltrId that is embedded
         into the filter identified by tFltrEmbedEntryInsertFltrId."
    ::= { tFilterEmbeddedEntryRefInfoEntry 6 }

tIPv6FilterParamsExtTbleLstChgd  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterParamsExtTbleLstChgd indicates the sysUpTime
         at the time of the last modification of tIPv6FilterParamsExtTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 46 }

tIPv6FilterParamsExtTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIPv6FilterParamsExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " The table tIPv6FilterParamsExtTable contains, together with the
         table tIPv6FilterParamsTable info about every IPv6 filter entry in
         any of the configured IPv6 filters in the system.

         The table tIPv6FilterParamsExtTable was introduced due to the big size
         of the tIPv6FilterParamsTable."
    ::= { tFilterObjects 47 }

tIPv6FilterParamsExtEntry        OBJECT-TYPE
    SYNTAX      TIPv6FilterParamsExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular IPv6 Filter entry. Every IPv6 Filter
         can have zero or more IPv6 Filter match entries.

         A filter entry with no match criteria set will match every packet, and
         the entry action will be taken.

         Rows are created/deleted by user.

         Additional match criteria can be found in tIPv6FilterParamsTable."
    AUGMENTS    { tIPv6FilterParamsEntry }
    ::= { tIPv6FilterParamsExtTable 1 }

TIPv6FilterParamsExtEntry        ::= SEQUENCE
{
    tIPv6FilterParamsExtLastChanged  TimeStamp,
    tIPv6FilterParamsExtAhExtHdr     TItemMatch,
    tIPv6FilterParamsExtEspExtHdr    TItemMatch,
    tIPv6FilterParamsExtNatType      TmnxNatSubscriberType,
    tIPv6FilterParamsExtPktLenVal1   TFilterPacketLength,
    tIPv6FilterParamsExtPktLenVal2   TFilterPacketLength,
    tIPv6FilterParamsExtPktLenOper   TOperator,
    tIPv6FilterParamsExtHopLimitVal1 TFilterTTL,
    tIPv6FilterParamsExtHopLimitVal2 TFilterTTL,
    tIPv6FilterParamsExtHopLimitOper TOperator,
    tIPv6FilterParamsExtEgressPBR    TFilterEgressPBR,
    tIPv6FilterParamsExtEsi          TFilterEsi,
    tIPv6FilterParamsExtFwdEsiSvcId  TmnxServId,
    tIPv6FilterParamsExtFwdEsiVRtrId TmnxVRtrIDOrZero,
    tIPv6FilterParamsExtFwdEsiSFIp   InetAddressIPv6,
    tIPv6FilterParamsExtPbrDwnActOvr TFilterPbrDownActionOvr,
    tIPv6FilterParamsExtFwdEsiVasIf  InterfaceIndexOrZero,
    tIPv6FilterParamsExtStickyDst    Integer32,
    tIPv6FilterParamsExtHoldRemain   Integer32,
    tIPv6FilterParamsExtDownloadAct  TFilterDownloadedAction,
    tIPv6FilterParamsExtTcpFin       TItemMatch,
    tIPv6FilterParamsExtTcpRst       TItemMatch,
    tIPv6FilterParamsExtTcpPsh       TItemMatch,
    tIPv6FilterParamsExtTcpUrg       TItemMatch,
    tIPv6FilterParamsExtTcpEce       TItemMatch,
    tIPv6FilterParamsExtTcpCwr       TItemMatch,
    tIPv6FilterParamsExtTcpNs        TItemMatch,
    tIPv6FilterParamsExtSrcMac       MacAddress,
    tIPv6FilterParamsExtSrcMacMask   MacAddress,
    tIPv6FilterParamsExtMxPktLenVal1 TFilterIpv6MatchPacketLength,
    tIPv6FilterParamsExtMxPktLenVal2 TFilterIpv6MatchPacketLength,
    tIPv6FilterParamsExtMxPktLenOper TOperator,
    tIPv6FilterParamsExtProtocolList TNamedItemOrEmpty,
    tIPv6FilterParamsExtDestClass    ClassIndexOrNone,
    tIPv6FilterParamsExtSampleProf   TmnxFilterCflowdSampleProfileId,
    tIPv6FilterParamsExtCollectStats TruthValue,
    tIPv6FilterParamsExtMxHopLmtVal1 TFilterTTL,
    tIPv6FilterParamsExtMxHopLmtVal2 TFilterTTL,
    tIPv6FilterParamsExtMxHopLmtOper TOperator,
    tIPv6FilterParamsExtTcpEst       TruthValue,
    tIPv6FilterParamsExtPktLenList   TNamedItemOrEmpty,
    tIPv6FilterParamsExtRoutingType4 TItemMatch
}

tIPv6FilterParamsExtLastChanged  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterParamsExtLastChanged indicates the timestamp
         of last change to this row in tIPv6FilterParamsExtTable."
    ::= { tIPv6FilterParamsExtEntry 1 }

tIPv6FilterParamsExtAhExtHdr     OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches the Authentication Extension Header (51) as per
         value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsExtEntry 2 }

tIPv6FilterParamsExtEspExtHdr    OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches the Encapsulation Security Payload Extension
         Header (50) as per value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsExtEntry 3 }

tIPv6FilterParamsExtNatType      OBJECT-TYPE
    SYNTAX      TmnxNatSubscriberType { dsliteLsnSub (3), nat64LsnSub (4) }
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "This object specifies the NAT type to be used when the value of the
         corresponding tIPv6FilterParamsNatPolicyName object is nat.

         The value of tIPv6FilterParamsExtNatType is relevant only if the value
         of tIPv6FilterParamsAction is nat. Setting the value of
         tIPv6FilterParamsExtNatType to a non-default value is ignored by the
         system if the value of tIPv6FilterParamsAction is not nat.

         Furthermore, the value of tIPv6FilterParamsExtNatType is silently
         reset to the default value by the system if tIPv6FilterParamsAction is
         set to any value other than nat."
    DEFVAL      { dsliteLsnSub }
    ::= { tIPv6FilterParamsExtEntry 4 }

tIPv6FilterParamsExtPktLenVal1   OBJECT-TYPE
    SYNTAX      TFilterPacketLength
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtPktLenVal1 specifies the
         packet length value1 to be compared to the value of the Payload Length
         field of an IPv6 packet header that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPv6FilterParamsExtPktLenOper.

         The value of this object is evaluated only if the value of the object
         tIPv6FilterParamsExtPktLenOper is other than 'none (0)'.

         If the value of tIPv6FilterParamsExtPktLenOper is 'range (2)' then the
         value of this object must be less than the value of
         tIPv6FilterParamsExtPktLenVal2.

         If the value of tIPv6FilterParamsExtPktLenOper is 'lt (3)' then the
         value of this object can be set in range 1..65535.

         If the value of tIPv6FilterParamsExtPktLenOper is 'gt (4)' then the
         value of this object can be set in range 0..65534.

         If both the values of the objects tIPv6FilterParamsExtPktLenOper and
         tIPv6FilterParamsExtPktLenVal1 need to be changed then it must be done
         in the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPv6FilterParamsAction is set to a value other than 'drop (1)' or
         if tIPv6FilterParamsExtPktLenOper is set to 'none (0)' or if
         tIPv6FilterParamsExtHopLimitOper is set to a value other than 'none
         (0)'."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 5 }

tIPv6FilterParamsExtPktLenVal2   OBJECT-TYPE
    SYNTAX      TFilterPacketLength
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtPktLenVal2 specifies the
         packet length value2 to be compared to the value of the Payload Length
         field of an IPv6 packet header that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPv6FilterParamsExtPktLenOper.

         The value of this object is evaluated only if the value of the object
         tIPv6FilterParamsExtPktLenOper is 'range (2)'.

         The value of this object must be greater than the value of
         tIPv6FilterParamsExtPktLenVal1.

         If both the values of the objects tIPv6FilterParamsExtPktLenOper and
         tIPv6FilterParamsExtPktLenVal2 need to be changed then it must be done
         in the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPv6FilterParamsAction is set to a value other than 'drop (1)' or
         if tIPv6FilterParamsExtPktLenOper is set to a value other than 'range
         (2)' or if tIPv6FilterParamsExtHopLimitOper is set to a value other
         than 'none (0)'."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 6 }

tIPv6FilterParamsExtPktLenOper   OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtPktLenOper specifies the
         way how the values of the objects tIPv6FilterParamsExtPktLenVal1 and
         tIPv6FilterParamsExtPktLenVal2 are used to form a condition that must
         be fulfilled in order to execute the action specified by the value of
         tIPv6FilterParamsAction. Otherwise the opposite action is executed.

         The value of this object can be set to a non-default value only if the
         value of the object tIPv6FilterParamsAction is 'drop (1)'.

         If the value of this object is being changed from the default value to
         any non-default value the values of the objects
         tIPv6FilterParamsExtPktLenVal1 and tIPv6FilterParamsExtPktLenVal2 (if
         applicable) must be sent in the same SET SNMP request.

         If the value of this object is 'none (0)' than the values of the
         objects tIPv6FilterParamsExtPktLenVal1 and
         tIPv6FilterParamsExtPktLenVal2 are ignored and TRUE case action is
         always executed (see table below).

         If the value of this object is 'eq (1)' then the value of the Payload
         Length field of the IPv6 header of the packet that has matched this
         filter's entry must be equal to the value of the object
         tIPv6FilterParamsExtPktLenVal1 in order to execute the TRUE case
         action (see table below). Otherwise the FALSE case action is executed.
         The value of the object tIPv6FilterParamsExtPktLenVal2 is ignored.

         If the value of this object is 'range (2)' then the value of the
         Payload Length field of the IPv6 header of the packet that has matched
         this filter's entry must be greater than or equal to the value of the
         object tIPv6FilterParamsExtPktLenVal1 and less than or equal to the
         value of the object tIPv6FilterParamsExtPktLenVal2 in order to execute
         the TRUE case action (see table below). Otherwise the FALSE case
         action is executed.

         If the value of this object is 'lt (3)' then the value of the Payload
         Length field of the IPv6 header of the packet that has matched this
         filter's entry must be less than the value of the object
         tIPv6FilterParamsExtPktLenVal1 in order to execute the TRUE case
         action (see table below). Otherwise the FALSE case action is executed.
         The value of the object tIPv6FilterParamsExtPktLenVal2 is ignored.

         If the value of this object is 'gt (4)' then the value of the Payload
         Length field of the IPv6 header of the packet that has matched this
         filter's entry must be greater than the value of the object
         tIPv6FilterParamsExtPktLenVal1 in order to execute the TRUE case
         action (see table below). Otherwise the FALSE case action is executed.
         The value of the object tIPv6FilterParamsExtPktLenVal2 is ignored.


         tIPFilterParamsAction   |   TRUE case action  |  FALSE case action
         ------------------------------------------------------------------
         drop                    |      drop           |      forward


         Allowed ranges for the values of tIPv6FilterParamsExtPktLenVal1 and
         tIPv6FilterParamsExtPktLenVal2 are:

         Operator                |Packet Length Value 1|Packet Length Value 2
         --------------------------------------------------------------------
         none (0)                |      N/A            |      N/A
         eq(1)                   |    0..65535         |      N/A
         range(2)                |    0..65534         | (Value1 + 1)..65535
         lt(3)                   |    1..65535         |      N/A
         gt(4)                   |    0..65534         |      N/A


         The values of the objects tIPv6FilterParamsExtPktLenVal1 and
         tIPv6FilterParamsExtPktLenVal2 are silently cleared if the value of
         this object is set to default.

         Note that the value of this object is silently cleared by the system
         if tIPv6FilterParamsAction is set to a value other than 'drop (1)' or
         if tIPv6FilterParamsExtHopLimitOper is set to a value other than 'none
         (0)'."
    DEFVAL      { none }
    ::= { tIPv6FilterParamsExtEntry 7 }

tIPv6FilterParamsExtHopLimitVal1 OBJECT-TYPE
    SYNTAX      TFilterTTL
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtHopLimitVal1 specifies the
         Hop Limit value1 to be compared to the value of the Hop Limit field of
         an IPv6 packet header that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPv6FilterParamsExtHopLimitOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPv6FilterParamsExtHopLimitOper is other than
         'none (0)'.

         If the value of tIPv6FilterParamsExtHopLimitOper is 'range (2)' then
         the value of this object must be less than the value of
         tIPv6FilterParamsExtHopLimitVal2.

         If the value of tIPv6FilterParamsExtHopLimitOper is 'lt (3)' then the
         value of this object can be set in range 1..255.

         If the value of tIPv6FilterParamsExtHopLimitOper is 'gt (4)' then the
         value of this object can be set in range 0..254.

         If both the values of the objects tIPv6FilterParamsExtHopLimitOper and
         tIPv6FilterParamsExtHopLimitVal1 need to be changed then it must be
         done in the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPv6FilterParamsAction is set to a value other than 'drop (1)' or
         if tIPv6FilterParamsExtHopLimitOper is set to 'none (0)' or if
         tIPv6FilterParamsExtPktLenOper is set to a value other than 'none
         (0)'."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 8 }

tIPv6FilterParamsExtHopLimitVal2 OBJECT-TYPE
    SYNTAX      TFilterTTL
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtHopLimitVal2 specifies the
         Hop Limit value2 to be compared to the value of the Hop Limit field of
         an IPv6 packet header that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPv6FilterParamsExtHopLimitOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPv6FilterParamsExtHopLimitOper is 'range (2)'.

         The value of this object must be greater than the value of
         tIPv6FilterParamsExtHopLimitVal1.

         If both the values of the objects tIPv6FilterParamsExtHopLimitOper and
         tIPv6FilterParamsExtHopLimitVal2 need to be changed then it must be
         done in the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPv6FilterParamsAction is set to a value other than 'drop (1)' or
         if tIPv6FilterParamsExtHopLimitOper is set to a value other than
         'range (2)' or if tIPv6FilterParamsExtPktLenOper is set to a value
         other than 'none (0)'."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 9 }

tIPv6FilterParamsExtHopLimitOper OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtHopLimitOper specifies the
         way how the values of the objects tIPv6FilterParamsExtHopLimitVal1 and
         tIPv6FilterParamsExtHopLimitVal2 are used to form a condition that
         must be fulfilled in order to execute the action specified by the
         value of tIPv6FilterParamsAction. Otherwise the opposite action is
         executed.

         The value of this object can be set to a non-default value only if the
         value of the object tIPv6FilterParamsAction is 'drop (1)'.

         If the value of this object is being changed from the default value to
         any non-default value the values of the objects
         tIPv6FilterParamsExtHopLimitVal1 and tIPv6FilterParamsExtHopLimitVal2
         (if applicable) must be sent in the same SET SNMP request.

         If the value of this object is 'none (0)' than the values of the
         objects tIPv6FilterParamsExtHopLimitVal1 and
         tIPv6FilterParamsExtHopLimitVal2 are ignored and TRUE case action is
         always executed (see table below).

         If the value of this object is 'eq (1)' then the value of the Hop
         Limit field of the IPv6 header of the packet that has matched this
         filter's entry must be equal to the value of the object
         tIPv6FilterParamsExtHopLimitVal1 in order to execute the TRUE case
         action (see table below). Otherwise the FALSE case action is executed.
         The value of the object tIPv6FilterParamsExtHopLimitVal2 is ignored.

         If the value of this object is 'range (2)' then the value of the Hop
         Limit field of the IPv6 header of the packet that has matched this
         filter's entry must be greater than or equal to the value of the
         object tIPv6FilterParamsExtHopLimitVal1 and less than or equal to the
         value of the object tIPv6FilterParamsExtHopLimitVal2 in order to
         execute the TRUE case action (see table below). Otherwise the FALSE
         case action is executed.

         If the value of this object is 'lt (3)' then the value of the Hop
         Limit field of the IPv6 header of the packet that has matched this
         filter's entry must be less than the value of the object
         tIPv6FilterParamsExtHopLimitVal1 in order to execute the TRUE case
         action (see table below). Otherwise the FALSE case action is executed.
         The value of the object tIPv6FilterParamsExtHopLimitVal2 is ignored.

         If the value of this object is 'gt (4)' then the value of the Hop
         Limit field of the IPv6 header of the packet that has matched this
         filter's entry must be greater than the value of the object
         tIPv6FilterParamsExtHopLimitVal1 in order to execute the TRUE case
         action (see table below). Otherwise the FALSE case action is executed.
         The value of the object tIPv6FilterParamsExtHopLimitVal2 is ignored.


         tIPv6FilterParamsAction |   TRUE case action  |  FALSE case action
         ------------------------------------------------------------------
         drop                    |      drop           |      forward


         Allowed ranges for the values of tIPv6FilterParamsExtHopLimitVal1 and
         tIPv6FilterParamsExtHopLimitVal2 are:

         Operator                |  Hop Limit Value 1  |  Hop Limit Value 2
         --------------------------------------------------------------------
         none (0)                |      N/A            |      N/A
         eq(1)                   |    0..255           |      N/A
         range(2)                |    0..254           | (Value1 + 1)..255
         lt(3)                   |    1..255           |      N/A
         gt(4)                   |    0..254           |      N/A


         The values of the objects tIPv6FilterParamsExtHopLimitVal1 and
         tIPv6FilterParamsExtHopLimitVal2 are silently cleared if the value of
         this object is set to default.

         Note that the value of this object is silently cleared by the system
         if tIPv6FilterParamsAction is set to a value other than 'drop (1)' or
         if tIPv6FilterParamsExtPktLenOper is set to a value other than 'none
         (0)'."
    DEFVAL      { none }
    ::= { tIPv6FilterParamsExtEntry 10 }

tIPv6FilterParamsExtEgressPBR    OBJECT-TYPE
    SYNTAX      TFilterEgressPBR
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtEgressPBR specifies if PBR
         specified by tIPv6FilterParamsExtEntry will have effect when the filter
         is applied on egress.
         tIPv6FilterParamsExtEgressPBR is applicable with these configured
         actions and action state:
         - no action
         - action forward redirect-policy <policy-name>
         - action forward esi <esi> sf-ip <ipv6-address>
           vas-interface <interface-name> router <router-instance>
         - action forward esi <esi> sf-ip <ipv6-address>
           vas-interface <interface-name> router service-name <service-name>
         - action forward next-hop <ipv6-address>
         - action forward next-hop <ipv6-address> router <router-instance>
         - action forward next-hop <ipv6-address> router service-name <service-name>
         - action forward next-hop indirect <ipv6-address>
         - action forward next-hop indirect <ipv6-address> router <router-instance>
         - action forward next-hop indirect <ipv6-address> router
           service-name <service-name>"
    DEFVAL      { disable }
    ::= { tIPv6FilterParamsExtEntry 11 }

tIPv6FilterParamsExtEsi          OBJECT-TYPE
    SYNTAX      TFilterEsi
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtEsi specifies the ethernet
         segment identifier (ESI). ESI is mapped by BGP EVPN to an L2 or L3
         capable appliance based on the value of tIPv6FilterParamsAction.
         Packets matching this entry are steered toward the L2 or L3 appliance.

         The value '0' indicates that there is no ESI specified.

         There are two options how to set the value of tIPv6FilterParamsExtEsi:
         1. Non zero value of tIPv6FilterParamsExtEsi is set together with non
            zero values of tIPv6FilterParamsExtFwdEsiVRtrId,
            tIPv6FilterParamsExtFwdEsiVasIf and tIPv6FilterParamsExtFwdEsiSFIp.
            In this case value of tIPv6FilterParamsAction is set to
            'forwardEsiL3' by the system.

         2. Non zero value of tIPv6FilterParamsExtEsi is set together with a
            non zero value of tIPv6FilterParamsExtFwdEsiSvcId. In this case
            value of tIPv6FilterParamsAction is set to 'forwardEsiL2' by
            the system.

         Note: The value of tIPv6FilterParamsExtEsi is set to '0' by the system
         if the value of tIPv6FilterParamsAction is set to any value other than
         'forwardEsiL2' or 'forwardEsiL3'."
    DEFVAL      { '00000000000000000000'H }
    ::= { tIPv6FilterParamsExtEntry 12 }

tIPv6FilterParamsExtFwdEsiSvcId  OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtFwdEsiSvcId specifies the
         identifier of VPLS used for VPN/DC connectivity.

         The value '0' indicates that there is no VPLS identifier specified.

         The non zero value of tIPv6FilterParamsExtFwdEsiSvcId must be set
         together with a non zero value of tIPv6FilterParamsExtEsi.

         Note: The value of tIPv6FilterParamsExtFwdEsiSvcId is set to '0' by
         the system if the value of the object tIPv6FilterParamsAction is set
         to any value other than 'forwardEsiL2'."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 13 }

tIPv6FilterParamsExtFwdEsiVRtrId OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtFwdEsiVRtrId specifies the
         VPRN/rVPLS virtual router identifier used for VPN/DC connectivity.

         The value '0' indicates that there is no VPRN/rVPLS virtual router
         identifier specified.

         The non zero value of tIPv6FilterParamsExtFwdEsiVRtrId must be set
         together with non zero values of tIPv6FilterParamsExtEsi,
         tIPv6FilterParamsExtFwdEsiVasIf and tIPv6FilterParamsExtFwdEsiSFIp.

         Note: The value of tIPv6FilterParamsExtFwdEsiVRtrId is set to '0' by
         the system if the value of tIPv6FilterParamsAction is set to any value
         other than 'forwardEsiL3'."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 14 }

tIPv6FilterParamsExtFwdEsiSFIp   OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtFwdEsiSFIp specifies the
         IPv6 address of the service function toward which traffic is steered.

         The value '0' indicates that no service function IP address is
         specified.

         The non zero value of tIPv6FilterParamsExtFwdEsiSFIp must be set
         together with non zero values of tIPv6FilterParamsExtFwdEsiVRtrId,
         tIPv6FilterParamsExtFwdEsiVasIf and tIPv6FilterParamsExtEsi.

         Note: The value of tIPv6FilterParamsExtFwdEsiSFIp is set to '0' by the
         system if the value of tIPv6FilterParamsAction is set to any value
         other than 'forwardEsiL3'."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPv6FilterParamsExtEntry 15 }

tIPv6FilterParamsExtPbrDwnActOvr OBJECT-TYPE
    SYNTAX      TFilterPbrDownActionOvr
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtPbrDwnActOvr specifies the
         filter action which will be performed when the PBR/PBF target for this
         entry is not available.

         If the value of tIPvXFltrEntryActAction is not one of the following
         values then tIPv6FilterParamsExtPbrDwnActOvr must be set to the value
         'none':
         - forwardEsiL2
         - forwardEsiL3
         - forwardSap
         - forwardSdp
         - forwardNextHopRtr

         If the value of tIPFilterParamsExtPbrDwnActOvr is different from
         'none' then PBR/PBF destination availability checking for an entry is
         turned on. There is a limit to the number of filter entries with the
         destination availability checking turned on. Entries with the value of
         tIPvXFltrEntryActAction equal to 'forwardEsiL2' or 'forwardEsiL3' are
         not counted against this limit.

         Refer to the description of the textual convention
         TFilterPbrDownActionOvr for more details."
    DEFVAL      { none }
    ::= { tIPv6FilterParamsExtEntry 16 }

tIPv6FilterParamsExtFwdEsiVasIf  OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtFwdEsiVasIf specifies the
         virtual router interface index of VPRN RVPLS interface used for VPN/DC
         connectivity.

         The value '0' indicates that no interface id is specified.

         The non zero value of tIPv6FilterParamsExtFwdEsiVasIf must be set
         together with non zero values of tIPv6FilterParamsExtFwdEsiVRtrId,
         tIPv6FilterParamsExtFwdEsiSFIp and tIPv6FilterParamsExtEsi.

         Note: The value of tIPv6FilterParamsExtFwdEsiVasIf is set to '0' by
         the system if the value of tIPv6FilterParamsAction is set to any value
         other than 'forwardEsiL3'."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 17 }

tIPv6FilterParamsExtStickyDst    OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtStickyDst specifies how
         long will system wait (in seconds) until it activates the best action
         (action with available PBR/PBF destination and the highest priority).
         Until then the action specified by tIPv6FilterParamsExtPbrDwnActOvr
         will be taken on a packet matching the filter entry. After the value
         of the active destination is fixed it will remain unchanged until the
         active PBR/PBF destination becomes unreachable.

         The value of -1 indicates that the property of PBR destination
         stickiness is turned off. When the property of stickiness is turned
         off the active PBR/PBF destination is always the one which is
         available and has the highest priority.

         The countdown starts when there was no PBR/PBF destination reachable
         and any PBR/PBF destination becomes reachable.

         tIPv6FilterParamsExtStickyDst can be set to value other than -1 only if
         the value of tIPvXFltrEntryActAction is one of the following values:
         - forwardSap
         - forwardSdp
         - forwardNextHopRtr"
    DEFVAL      { -1 }
    ::= { tIPv6FilterParamsExtEntry 18 }

tIPv6FilterParamsExtHoldRemain   OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtHoldRemain indicates the
         remaining time in seconds, until the best action will become active
         and will be fixed.

         Best action is:
         - primary action if PBR target status of primary action is up.
         - secondary action if PBR target status of secondary action is up
           and PBR target status of primary action is down.
         - none if both PBR targets are down"
    ::= { tIPv6FilterParamsExtEntry 19 }

tIPv6FilterParamsExtDownloadAct  OBJECT-TYPE
    SYNTAX      TFilterDownloadedAction
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtDownloadAct indicates the
         filter entry action downloaded to IOM.

         Refer to the description of the textual convention
         TFilterDownloadedAction for more information."
    ::= { tIPv6FilterParamsExtEntry 20 }

tIPv6FilterParamsExtTcpFin       OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Fin as per value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsExtEntry 21 }

tIPv6FilterParamsExtTcpRst       OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Rst as per value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsExtEntry 22 }

tIPv6FilterParamsExtTcpPsh       OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Psh as per value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsExtEntry 23 }

tIPv6FilterParamsExtTcpUrg       OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Urg as per value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsExtEntry 24 }

tIPv6FilterParamsExtTcpEce       OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Ece as per value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsExtEntry 25 }

tIPv6FilterParamsExtTcpCwr       OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Cwr as per value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsExtEntry 26 }

tIPv6FilterParamsExtTcpNs        OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Ns as per value of the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsExtEntry 27 }

tIPv6FilterParamsExtSrcMac       OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Source MAC to match for this policy filter entry."
    DEFVAL      { '000000000000'H }
    ::= { tIPv6FilterParamsExtEntry 28 }

tIPv6FilterParamsExtSrcMacMask   OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Source MAC mask value for this policy MAC filter entry. The mask is
         ANDed with the MAC to match tIPv6FilterParamsExtSrcMac. A cleared bit
         means ignore this bit, do not match. A set bit means match this bit
         with tIPv6FilterParamsExtSrcMac. Use the value 00-00-00-00-00-00 to
         disable this filter criteria."
    DEFVAL      { '000000000000'H }
    ::= { tIPv6FilterParamsExtEntry 29 }

tIPv6FilterParamsExtMxPktLenVal1 OBJECT-TYPE
    SYNTAX      TFilterIpv6MatchPacketLength
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtMxPktLenVal1 specifies the
         value1 to be compared to total length of the packet including header.

         The way how the value of this object is used depends on the value of
         the object tIPv6FilterParamsExtMxPktLenOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPv6FilterParamsExtMxPktLenOper is other than
         'none (0)'.

         If the value of tIPv6FilterParamsExtMxPktLenOper is 'range (2)' then
         the value of this object must be less than the value of
         tIPv6FilterParamsExtMxPktLenVal2.

         If the value of tIPv6FilterParamsExtMxPktLenOper is 'lt (3)' then the
         value of this object can be set in range 41..65535.

         If the value of tIPv6FilterParamsExtMxPktLenOper is 'gt (4)' then the
         value of this object can be set in range 40..65574.

         If both the values of the objects tIPv6FilterParamsExtMxPktLenOper and
         tIPv6FilterParamsExtMxPktLenVal1 need to be changed then it must be
         done in the same SET SNMP request."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 30 }

tIPv6FilterParamsExtMxPktLenVal2 OBJECT-TYPE
    SYNTAX      TFilterIpv6MatchPacketLength
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtMxPktLenVal2 specifies the
         value2 to be compared to total length of the packet including header.

         The way how the value of this object is used depends on the value of
         the object tIPv6FilterParamsExtMxPktLenOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPv6FilterParamsExtMxPktLenOper is 'range (2)'.

         The value of this object must be greater than the value of
         tIPv6FilterParamsExtMxPktLenVal1.

         If both the values of the objects tIPv6FilterParamsExtMxPktLenOper and
         tIPv6FilterParamsExtMxPktLenVal2 need to be changed then it must be
         done in the same SET SNMP request."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 31 }

tIPv6FilterParamsExtMxPktLenOper OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtMxPktLenOper specifies the
         way how the values of the objects tIPv6FilterParamsExtMxPktLenVal1 and
         tIPv6FilterParamsExtMxPktLenVal2 are used.

         If the value of this object is 'eq (1)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be equal to the value of the object
         tIPv6FilterParamsExtMxPktLenVal1 (see table below). The value of the
         object tIPv6FilterParamsExtMxPktLenVal2 is ignored.

         If the value of this object is 'range (2)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be greater than or equal to the value of the
         object tIPv6FilterParamsExtMxPktLenVal1 and less than or equal to the
         value of the object tIPv6FilterParamsExtMxPktLenVal2.

         If the value of this object is 'lt (3)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be less than the value of the object
         tIPv6FilterParamsExtMxPktLenVal1 (see table below). The value of the
         object tIPv6FilterParamsExtMxPktLenVal2 is ignored.

         If the value of this object is 'gt (4)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be greater than the value of the object
         tIPv6FilterParamsExtMxPktLenVal1 (see table below). The value of the
         object tIPv6FilterParamsExtMxPktLenVal2 is ignored.


         Allowed ranges for the values of tIPv6FilterParamsExtMxPktLenVal1 and
         tIPv6FilterParamsExtMxPktLenVal2 are:

         Operator                |Packet Length Value 1|Packet Length Value 2
         --------------------------------------------------------------------
         none (0)                |      N/A            |      N/A
         eq(1)                   |    0..65535         |      N/A
         range(2)                |    0..65534         | (Value1 + 1)..65535
         lt(3)                   |    1..65535         |      N/A
         gt(4)                   |    0..65534         |      N/A"
    DEFVAL      { none }
    ::= { tIPv6FilterParamsExtEntry 32 }

tIPv6FilterParamsExtProtocolList OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "."
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsExtEntry 33 }

tIPv6FilterParamsExtDestClass    OBJECT-TYPE
    SYNTAX      ClassIndexOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtDestClass specifies
         destination class to match."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 34 }

tIPv6FilterParamsExtSampleProf   OBJECT-TYPE
    SYNTAX      TmnxFilterCflowdSampleProfileId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the sample profile to be applied to packets matching this
         IPv6 filter entry.

         Setting tIPv6FilterParamsExtSampleProf to a non-default value, will
         set tIPv6FilterParamsCflowdSample to its default value and vice versa."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 35 }

tIPv6FilterParamsExtCollectStats OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPv6FilterParamsExtCollectStats specifies whether or not
         the collection of statistical data for the filter entry is enabled.

         tIPv6FilterParamsExtCollectStats is supported only on IXR J2
         platforms."
    DEFVAL      { false }
    ::= { tIPv6FilterParamsExtEntry 36 }

tIPv6FilterParamsExtMxHopLmtVal1 OBJECT-TYPE
    SYNTAX      TFilterTTL
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtMxHopLmtVal1 specifies the
         value1 to be compared to the value of 'Hop-Limit' field of IPv6 header
         of an IP packet that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPv6FilterParamsExtMxHopLmtOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPv6FilterParamsExtMxHopLmtOper is other than
         'none (0)'.

         If the value of tIPv6FilterParamsExtMxHopLmtOper is 'range (2)' then
         the value of this object must be less than the value of
         tIPv6FilterParamsExtMxHopLmtVal2.

         If the value of tIPv6FilterParamsExtMxHopLmtOper is 'lt (3)' then the
         value of this object can be set in range 1..255.

         If the value of tIPv6FilterParamsExtMxHopLmtOper is 'gt (4)' then the
         value of this object can be set in range 0..254.

         If both the values of the objects tIPv6FilterParamsExtMxHopLmtOper and
         tIPv6FilterParamsExtMxHopLmtVal1 need to be changed then it must be
         done in the same SET SNMP request."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 37 }

tIPv6FilterParamsExtMxHopLmtVal2 OBJECT-TYPE
    SYNTAX      TFilterTTL
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtMxHopLmtVal2 specifies
         value2 to be compared to the value of 'Hop-Limit' field of IPv6 header
         of an IP packet that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPv6FilterParamsExtMxHopLmtOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPv6FilterParamsExtMxHopLmtOper is 'range (2)'.

         The value of this object must be greater than the value of
         tIPv6FilterParamsExtMxHopLmtVal1.

         If both the values of the objects tIPv6FilterParamsExtMxHopLmtOper and
         tIPv6FilterParamsExtMxHopLmtVal2 need to be changed then it must be
         done in the same SET SNMP request."
    DEFVAL      { 0 }
    ::= { tIPv6FilterParamsExtEntry 38 }

tIPv6FilterParamsExtMxHopLmtOper OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6FilterParamsExtMxHopLmtOper specifies the
         way how the values of the objects tIPv6FilterParamsExtMxHopLmtVal1 and
         tIPv6FilterParamsExtMxHopLmtVal2 are used to form a condition for a
         packet match.

         If the value of this object is 'eq (1)' then the value of the
         'Hop-Limit' field of the IPv6 header of the packet must be equal to
         the value of the object tIPv6FilterParamsExtMxHopLmtVal1 in order to
         match this entry. The value of the object
         tIPv6FilterParamsExtMxHopLmtVal2 is ignored.

         If the value of this object is 'range (2)' then the value of the
         'Hop-Limit' field of the IPv6 header of the packet must be greater
         than or equal to the value of the object
         tIPv6FilterParamsExtMxHopLmtVal1 and less than or equal to the value
         of the object tIPv6FilterParamsExtMxHopLmtVal2 in order to match this
         entry.

         If the value of this object is 'lt (3)' then the value of the
         'Hop-Limit' field of the IPv6 header of the packet must be less than
         the value of the object tIPv6FilterParamsExtMxHopLmtVal1 in order to
         match this entry. The value of the object
         tIPv6FilterParamsExtMxHopLmtVal2 is ignored.

         If the value of this object is 'gt (4)' then the value of the
         'Hop-Limit' field of the IPv6 header of the packet must be greater
         than the value of the object tIPv6FilterParamsExtMxHopLmtVal1 in order
         to match this entry. The value of the object
         tIPv6FilterParamsExtMxHopLmtVal2 is ignored.

         Allowed ranges for the values of tIPv6FilterParamsExtMxHopLmtVal1 and
         tIPv6FilterParamsExtMxHopLmtVal2 are:

         Operator                | 'Hop-Limit' Value 1 | 'Hop-Limit' Value 2
         --------------------------------------------------------------------
         none (0)                |      N/A            |      N/A
         eq(1)                   |    0..255           |      N/A
         range(2)                |    0..254           | (Value1 + 1)..255
         lt(3)                   |    1..255           |      N/A
         gt(4)                   |    0..254           |      N/A"
    DEFVAL      { none }
    ::= { tIPv6FilterParamsExtEntry 39 }

tIPv6FilterParamsExtTcpEst       OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Rst or a TCP Ack as per value of the object."
    DEFVAL      { false }
    ::= { tIPv6FilterParamsExtEntry 40 }

tIPv6FilterParamsExtPktLenList   OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the packet length list used as an
         IPv6 filter match criterion.

         The value specified for this object must correspond to a packet length
         list defined in the tFltrPktLenListTable.

         If the value of this object is empty then the values of the objects
         tIPv6FilterParamsExtMxPktLenOper, tIPv6FilterParamsExtMxPktLenVal1 and
         tIPv6FilterParamsExtMxPktLenVal2 are used as packet length match
         criterion.

         When this object is set to a non-empty value then the objects
         tIPv6FilterParamsExtMxPktLenOper, tIPv6FilterParamsExtMxPktLenVal1 and
         tIPv6FilterParamsExtMxPktLenVal2 are reset to their default values by
         the system.

         Vice versa, when a new (non-default) value is provided for the objects
         tIPv6FilterParamsExtMxPktLenOper, tIPv6FilterParamsExtMxPktLenVal1 or
         tIPv6FilterParamsExtMxPktLenVal2, then this object is reset to its
         default (empty) value by the system.

         An attempt to set tIPv6FilterParamsExtPktLenList to a non-default
         value in combination with setting any of
         tIPv6FilterParamsExtMxPktLenOper, tIPv6FilterParamsExtMxPktLenVal1 or
         tIPv6FilterParamsExtMxPktLenVal2 to a non-default value is rejected by
         the system"
    DEFVAL      { ''H }
    ::= { tIPv6FilterParamsExtEntry 41 }

tIPv6FilterParamsExtRoutingType4 OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a Segment Routing Extension Header as per value of
         the object."
    DEFVAL      { off }
    ::= { tIPv6FilterParamsExtEntry 42 }

tFilterEmbedOpenflowTableLstChg  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterEmbedOpenflowTableLstChg indicates the sysUpTime at
         the time of the last modification of tFilterEmbedOpenflowTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 48 }

tFilterEmbedOpenflowTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterEmbedOpenflowEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterEmbedOpenflowTable contains an entry for each
         open-flow flowtable embedded in a filter with scope other than
         'embedded'."
    ::= { tFilterObjects 49 }

tFilterEmbedOpenflowEntry        OBJECT-TYPE
    SYNTAX      TFilterEmbedOpenflowEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterEmbedOpenflowTable."
    INDEX       {
        tFilterEmbedOpenflowOfsName,
        tFilterEmbedOpenflowFilterType,
        tFilterEmbedOpenflowInsertFltrId,
        tFilterEmbedOpenflowOffset
    }
    ::= { tFilterEmbedOpenflowTable 1 }

TFilterEmbedOpenflowEntry        ::= SEQUENCE
{
    tFilterEmbedOpenflowOfsName      TNamedItem,
    tFilterEmbedOpenflowFilterType   TFilterType,
    tFilterEmbedOpenflowInsertFltrId TConfigOrVsdFilterID,
    tFilterEmbedOpenflowOffset       TFilterEmbedOffset,
    tFilterEmbedOpenflowRowStatus    RowStatus,
    tFilterEmbedOpenflowAdminState   TmnxEmbeddedFltrAdminState,
    tFilterEmbedOpenflowOperState    TmnxEmbeddedFltrOperState,
    tFilterEmbedOflowSvcContext      Unsigned32,
    tFilterEmbedOflowSapContextPort  TmnxPortID,
    tFilterEmbedOflowSapContextEncap TmnxEncapVal,
    tFilterEmbedOflowContextType     INTEGER
}

tFilterEmbedOpenflowOfsName      OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedOpenflowOfsName specifies the name of the
         open-flow switch which contains the flowtable to be inserted in the
         filter specified by tFilterEmbedOpenflowInsertFltrId."
    ::= { tFilterEmbedOpenflowEntry 1 }

tFilterEmbedOpenflowFilterType   OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFilterEmbedOpenflowFilterType specifies the type of filter
         for the filter specified by tFilterEmbedOpenflowInsertFltrId."
    ::= { tFilterEmbedOpenflowEntry 2 }

tFilterEmbedOpenflowInsertFltrId OBJECT-TYPE
    SYNTAX      TConfigOrVsdFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedOpenflowInsertFltrId specifies the filter
         where the open-flow switch specified by tFilterEmbedOpenflowOfsName is
         to be embedded.

         Values outside of range 1..65535 are reserved for entries dynamically
         created by the system and cannot be used in any SNMP SET operation."
    ::= { tFilterEmbedOpenflowEntry 3 }

tFilterEmbedOpenflowOffset       OBJECT-TYPE
    SYNTAX      TFilterEmbedOffset
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedOpenflowOffset specifies the offset of
         inserted entries."
    ::= { tFilterEmbedOpenflowEntry 4 }

tFilterEmbedOpenflowRowStatus    OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedOpenflowRowStatus specifies the
         status of a row in tFilterEmbedOpenflowTable. Rows are created and
         destroyed by SNMP SET operations on this object.

         Only values 'active (1)', 'createAndGo(4)', and 'destroy (6)' are
         supported."
    ::= { tFilterEmbedOpenflowEntry 5 }

tFilterEmbedOpenflowAdminState   OBJECT-TYPE
    SYNTAX      TmnxEmbeddedFltrAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedOpenflowAdminState specifies the
         administrative state of the embed request defined by this row.

         If an active embedding cannot be fulfilled due to dynamic events, this
         object will be set to 'inactive' automatically by the system. In those
         cases, the object tFilterEmbedOpenflowOperState will indicate the
         failure reason."
    DEFVAL      { active }
    ::= { tFilterEmbedOpenflowEntry 6 }

tFilterEmbedOpenflowOperState    OBJECT-TYPE
    SYNTAX      TmnxEmbeddedFltrOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedOpenflowOperState indicates the operational
         state of the embed request defined by this row."
    ::= { tFilterEmbedOpenflowEntry 7 }

tFilterEmbedOflowSvcContext      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedOflowSvcContext specifies the service context
         of this open-flow embedding. When no service context is present, this
         object is equal to default value."
    DEFVAL      { 0 }
    ::= { tFilterEmbedOpenflowEntry 8 }

tFilterEmbedOflowSapContextPort  OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedOflowSapContextPort specifies the port-id of
         the sap context of this open-flow embedding. When no sap context is
         present, this object is set to default value."
    DEFVAL      { 0 }
    ::= { tFilterEmbedOpenflowEntry 9 }

tFilterEmbedOflowSapContextEncap OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedOflowSapContextEncap specifies the encap
         value of the sap context of this open-flow embedding. When no sap
         context is present, this object is set to default value."
    DEFVAL      { 0 }
    ::= { tFilterEmbedOpenflowEntry 10 }

tFilterEmbedOflowContextType     OBJECT-TYPE
    SYNTAX      INTEGER {
        grt     (1),
        system  (2),
        service (3),
        sap     (4)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedOflowContextType specifies the context in
         which the open-flow embedding is inserted into filter. When no context
         is present, this object is set to grt value."
    DEFVAL      { grt }
    ::= { tFilterEmbedOpenflowEntry 11 }

tFilterEmbedOpenflowInfoTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterEmbedOpenflowInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterEmbedOpenflowInfoTable contains an entry for each
         open-flow switch embedded in a filter with scope other than
         'embedded'.

         This row complements the corresponding row in the
         tFilterEmbedOpenflowTable with read-only operational info."
    ::= { tFilterObjects 50 }

tFilterEmbedOpenflowInfoEntry    OBJECT-TYPE
    SYNTAX      TFilterEmbedOpenflowInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterEmbedOpenflowInfoTable."
    AUGMENTS    { tFilterEmbedOpenflowEntry }
    ::= { tFilterEmbedOpenflowInfoTable 1 }

TFilterEmbedOpenflowInfoEntry    ::= SEQUENCE
{
    tFltrEmbedOfInfoEntryCnt         Unsigned32,
    tFltrEmbedOfInfoEntryCntInsrtd   Unsigned32
}

tFltrEmbedOfInfoEntryCnt         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedOfInfoEntryCnt indicates how many entries are
         eligible for embedding from the open-flow switch specified by
         tFilterEmbedOpenflowOfsName."
    ::= { tFilterEmbedOpenflowInfoEntry 1 }

tFltrEmbedOfInfoEntryCntInsrtd   OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedOfInfoEntryCntInsrtd indicates how many entries
         are actually placed inside the filter by the open-flow switch
         specified by tFilterEmbedOpenflowOfsName.

         If the object tFilterEmbedOpenflowOperState is different from
         'in-service' this object will always be zero.

         Else, the difference between the value of this object and the value of
         tFltrEmbedOfInfoEntryCnt indicates how many entries were overwritten
         by local entries in the embedding filter."
    ::= { tFilterEmbedOpenflowInfoEntry 2 }

tFilterOpenflowEntryInfoTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterOpenflowEntryInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterOpenflowEntryInfoTable contains an entry for each
         open-flow filter entry inserted in a filter with scope other than
         'embedded'."
    ::= { tFilterObjects 51 }

tFilterOpenflowEntryInfoEntry    OBJECT-TYPE
    SYNTAX      TFilterOpenflowEntryInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterOpenflowEntryInfoTable. Rows in the
         tFilterOpenflowEntryInfoTable are created by the SYSTEM when an
         open-flow switch is embedded into a filter. They are destroyed by the
         SYSTEM when an open-flow switch embedding is removed from a filter."
    INDEX       {
        tFltrEmbedOfEntryOfsName,
        tFltrEmbedOfEntryFilterType,
        tFltrEmbedOfEntryInsertFltrId,
        tFltrEmbedOfEntryOfEntryId
    }
    ::= { tFilterOpenflowEntryInfoTable 1 }

TFilterOpenflowEntryInfoEntry    ::= SEQUENCE
{
    tFltrEmbedOfEntryOfsName         TNamedItem,
    tFltrEmbedOfEntryFilterType      TFilterType,
    tFltrEmbedOfEntryInsertFltrId    TConfigOrVsdFilterID,
    tFltrEmbedOfEntryOfEntryId       TEntryId,
    tFltrEmbedOfEntryInsrtEntryId    TAnyEntryId,
    tFltrEmbedOfEntryInsrtEntryState TmnxFltrEmbeddedEntryState
}

tFltrEmbedOfEntryOfsName         OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedOfEntryOfsName specifies the name of the
         open-flow switch which contains the flowtable to be inserted in the
         filter specified by tFltrEmbedOfEntryInsertFltrId."
    ::= { tFilterOpenflowEntryInfoEntry 1 }

tFltrEmbedOfEntryFilterType      OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrEmbedOfEntryFilterType specifies the type of filter
         for the filter specified by tFltrEmbedOfEntryInsertFltrId."
    ::= { tFilterOpenflowEntryInfoEntry 2 }

tFltrEmbedOfEntryInsertFltrId    OBJECT-TYPE
    SYNTAX      TConfigOrVsdFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedOfEntryInsertFltrId specifies the filter where
         the open-flow switch specified by tFltrEmbedOfEntryOfsName is to be
         embedded.

         Values outside of range 1..65535 are reserved for entries dynamically
         created by the system."
    ::= { tFilterOpenflowEntryInfoEntry 3 }

tFltrEmbedOfEntryOfEntryId       OBJECT-TYPE
    SYNTAX      TEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedOfEntryOfEntryId specifies the base ID of the
         entry as determined by the priority of the corresponding flow-rule in
         the open-flow switch specified by tFltrEmbedOfEntryOfsName."
    ::= { tFilterOpenflowEntryInfoEntry 4 }

tFltrEmbedOfEntryInsrtEntryId    OBJECT-TYPE
    SYNTAX      TAnyEntryId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedOfEntryInsrtEntryId indicates the position of
         the filter entry in the filter specified by
         tFltrEmbedOfEntryInsertFltrId."
    ::= { tFilterOpenflowEntryInfoEntry 5 }

tFltrEmbedOfEntryInsrtEntryState OBJECT-TYPE
    SYNTAX      TmnxFltrEmbeddedEntryState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFltrEmbedOfEntryInsrtEntryState indicates the current
         status of the embedding of the entry identified by
         tFltrEmbedOfEntryOfEntryId from the open-flow switch identified by
         tFltrEmbedOfEntryOfsName that is embedded into the filter identified
         by tFltrEmbedOfEntryInsertFltrId."
    ::= { tFilterOpenflowEntryInfoEntry 6 }

tIPFilterParamsExtTbleLstChgd    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterParamsExtTbleLstChgd indicates the sysUpTime at
         the time of the last modification of tIPFilterParamsExtTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 52 }

tIPFilterParamsExtTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIPFilterParamsExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tIPFilterParamsExtTable contains, together with the table
         tIPFilterParamsTable info about every IP filter entry in any of the
         configured IP filters in the system.

         The table tIPFilterParamsExtTable was introduced due to the big size
         of the tIPFilterParamsTable."
    ::= { tFilterObjects 53 }

tIPFilterParamsExtEntry          OBJECT-TYPE
    SYNTAX      TIPFilterParamsExtEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular IP Filter entry. Every IP Filter can
         have zero or more IP Filter match entries.

         A filter entry with no match criteria set will match every packet, and
         the entry action will be taken.

         Entries are created/deleted by the system when a corresponding
         tIPFilterParamsEntry is created/deleted.

         Additional match criteria can be found in tIPFilterParamsTable."
    AUGMENTS    { tIPFilterParamsEntry }
    ::= { tIPFilterParamsExtTable 1 }

TIPFilterParamsExtEntry          ::= SEQUENCE
{
    tIPFilterParamsExtLastChanged    TimeStamp,
    tIPFilterParamsExtPktLenVal1     TFilterPacketLength,
    tIPFilterParamsExtPktLenVal2     TFilterPacketLength,
    tIPFilterParamsExtPktLenOper     TOperator,
    tIPFilterParamsExtTTLVal1        TFilterTTL,
    tIPFilterParamsExtTTLVal2        TFilterTTL,
    tIPFilterParamsExtTTLOper        TOperator,
    tIPFilterParamsExtEgressPBR      TFilterEgressPBR,
    tIPFilterParamsExtEsi            TFilterEsi,
    tIPFilterParamsExtFwdEsiSvcId    TmnxServId,
    tIPFilterParamsExtFwdEsiVRtrId   TmnxVRtrIDOrZero,
    tIPFilterParamsExtFwdEsiSFIp     InetAddressIPv4,
    tIPFilterParamsExtPbrDwnActOvr   TFilterPbrDownActionOvr,
    tIPFilterParamsExtFwdEsiVasIf    InterfaceIndexOrZero,
    tIPFilterParamsExtStickyDst      Integer32,
    tIPFilterParamsExtHoldRemain     Integer32,
    tIPFilterParamsExtDownloadAct    TFilterDownloadedAction,
    tIPFilterParamsExtTcpFin         TItemMatch,
    tIPFilterParamsExtTcpRst         TItemMatch,
    tIPFilterParamsExtTcpPsh         TItemMatch,
    tIPFilterParamsExtTcpUrg         TItemMatch,
    tIPFilterParamsExtTcpEce         TItemMatch,
    tIPFilterParamsExtTcpCwr         TItemMatch,
    tIPFilterParamsExtTcpNs          TItemMatch,
    tIPFilterParamsExtSrcMac         MacAddress,
    tIPFilterParamsExtSrcMacMask     MacAddress,
    tIPFilterParamsExtMxPktLenVal1   TFilterPacketLength,
    tIPFilterParamsExtMxPktLenVal2   TFilterPacketLength,
    tIPFilterParamsExtMxPktLenOper   TOperator,
    tIPFilterParamsExtProtocolList   TNamedItemOrEmpty,
    tIPFilterParamsExtDestClass      ClassIndexOrNone,
    tIPFilterParamsExtSampleProf     TmnxFilterCflowdSampleProfileId,
    tIPFilterParamsExtCollectStats   TruthValue,
    tIPFilterParamsExtMxTTLVal1      TFilterTTL,
    tIPFilterParamsExtMxTTLVal2      TFilterTTL,
    tIPFilterParamsExtMxTTLOper      TOperator,
    tIPFilterParamsExtTcpEst         TruthValue,
    tIPFilterParamsExtPktLenList     TNamedItemOrEmpty
}

tIPFilterParamsExtLastChanged    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtLastChanged indicates the
         timestamp of last change of this row in tIPFilterParamsExtTable."
    ::= { tIPFilterParamsExtEntry 1 }

tIPFilterParamsExtPktLenVal1     OBJECT-TYPE
    SYNTAX      TFilterPacketLength
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtPktLenVal1 specifies the
         packet length value1 to be compared to the value of the Total Length
         field of an IP packet header that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPFilterParamsExtPktLenOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPFilterParamsExtPktLenOper is other than 'none
         (0)'.

         If the value of tIPFilterParamsExtPktLenOper is 'range (2)' then the
         value of this object must be less than the value of
         tIPFilterParamsExtPktLenVal2.

         If the value of tIPFilterParamsExtPktLenOper is 'lt (3)' then the
         value of this object can be set in range 1..65535.

         If the value of tIPFilterParamsExtPktLenOper is 'gt (4)' then the
         value of this object can be set in range 0..65534.

         If both the values of the objects tIPFilterParamsExtPktLenOper and
         tIPFilterParamsExtPktLenVal1 need to be changed then it must be done
         in the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPFilterParamsAction is set to a value other than 'drop (1)' or if
         tIPFilterParamsExtPktLenOper is set to 'none (0)' or if
         tIPFilterParamsExtTTLOper is set to a value other than 'none (0)'."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 2 }

tIPFilterParamsExtPktLenVal2     OBJECT-TYPE
    SYNTAX      TFilterPacketLength
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtPktLenVal2 specifies the
         packet length value2 to be compared to the value of the Total Length
         field of an IP packet header that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPFilterParamsExtPktLenOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPFilterParamsExtPktLenOper is 'range (2)'.

         The value of this object must be greater than the value of
         tIPFilterParamsExtPktLenVal1.

         If both the values of the objects tIPFilterParamsExtPktLenOper and
         tIPFilterParamsExtPktLenVal2 need to be changed then it must be done
         in the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPFilterParamsAction is set to a value other than 'drop (1)' or if
         tIPFilterParamsExtPktLenOper is set to value other than 'range (2)' or
         if tIPFilterParamsExtTTLOper is set to a value other than 'none (0)'."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 3 }

tIPFilterParamsExtPktLenOper     OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtPktLenOper specifies the way
         how the values of the objects tIPFilterParamsExtPktLenVal1 and
         tIPFilterParamsExtPktLenVal2 are used to form a condition that must be
         fulfilled in order to execute the action specified by the value of
         tIPFilterParamsAction. Otherwise the opposite action is executed.

         The value of this object can be set to a non-default value only if the
         value of the object tIPFilterParamsAction is 'drop (1)'.

         If the value of this object is being changed from the default value to
         any non-default value the values of the objects
         tIPFilterParamsExtPktLenVal1 and tIPFilterParamsExtPktLenVal2 (if
         applicable) must be sent in the same SET SNMP request.

         If the value of this object is 'none (0)' than the values of the
         objects tIPFilterParamsExtPktLenVal1 and tIPFilterParamsExtPktLenVal2
         are ignored and TRUE case action is always executed (see table below).

         If the value of this object is 'eq (1)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be equal to the value of the object
         tIPFilterParamsExtPktLenVal1 in order to execute the TRUE case action
         (see table below). Otherwise the FALSE case action is executed. The
         value of the object tIPFilterParamsExtPktLenVal2 is ignored.

         If the value of this object is 'range (2)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be greater than or equal to the value of the
         object tIPFilterParamsExtPktLenVal1 and less than or equal to the
         value of the object tIPFilterParamsExtPktLenVal2 in order to execute
         the TRUE case action (see table below). Otherwise the FALSE case
         action is executed.

         If the value of this object is 'lt (3)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be less than the value of the object
         tIPFilterParamsExtPktLenVal1 in order to execute the TRUE case action
         (see table below). Otherwise the FALSE case action is executed. The
         value of the object tIPFilterParamsExtPktLenVal2 is ignored.

         If the value of this object is 'gt (4)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be greater than the value of the object
         tIPFilterParamsExtPktLenVal1 in order to execute the TRUE case action
         (see table below). Otherwise the FALSE case action is executed. The
         value of the object tIPFilterParamsExtPktLenVal2 is ignored.


         tIPFilterParamsAction   |   TRUE case action  |  FALSE case action
         ------------------------------------------------------------------
         drop                    |      drop           |      forward


         Allowed ranges for the values of tIPFilterParamsExtPktLenVal1 and
         tIPFilterParamsExtPktLenVal2 are:

         Operator                |Packet Length Value 1|Packet Length Value 2
         --------------------------------------------------------------------
         none (0)                |      N/A            |      N/A
         eq(1)                   |    0..65535         |      N/A
         range(2)                |    0..65534         | (Value1 + 1)..65535
         lt(3)                   |    1..65535         |      N/A
         gt(4)                   |    0..65534         |      N/A


         The values of the objects tIPFilterParamsExtPktLenVal1 and
         tIPFilterParamsExtPktLenVal2 are silently cleared if the value of this
         object is set to default.

         Note that the value of this object is silently cleared by the system
         if tIPFilterParamsAction is set to a value other than 'drop (1)' or if
         tIPFilterParamsExtTTLOper is set to a value other than 'none (0)'."
    DEFVAL      { none }
    ::= { tIPFilterParamsExtEntry 4 }

tIPFilterParamsExtTTLVal1        OBJECT-TYPE
    SYNTAX      TFilterTTL
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtTTLVal1 specifies the
         Time-To-Live value1 to be compared to the value of the Time-To-Live
         field of an IP packet header that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPFilterParamsExtTTLOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPFilterParamsExtTTLOper is other than 'none
         (0)'.

         If the value of tIPFilterParamsExtTTLOper is 'range (2)' then the
         value of this object must be less than the value of
         tIPFilterParamsExtTTLVal2.

         If the value of tIPFilterParamsExtTTLOper is 'lt (3)' then the value
         of this object can be set in range 1..255.

         If the value of tIPFilterParamsExtTTLOper is 'gt (4)' then the value
         of this object can be set in range 0..254.

         If both the values of the objects tIPFilterParamsExtTTLOper and
         tIPFilterParamsExtTTLVal1 need to be changed then it must be done in
         the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPFilterParamsAction is set to a value other than 'drop (1)' or if
         tIPFilterParamsExtTTLOper is set to 'none (0)' or if
         tIPFilterParamsExtPktLenOper is set to a value other than 'none (0)'."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 5 }

tIPFilterParamsExtTTLVal2        OBJECT-TYPE
    SYNTAX      TFilterTTL
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtTTLVal2 specifies the
         Time-To-Live value2 to be compared to the value of the Time-To-Live
         field of an IP packet header that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPFilterParamsExtTTLOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPFilterParamsExtTTLOper is 'range (2)'.

         The value of this object must be greater than the value of
         tIPFilterParamsExtTTLVal1.

         If both the values of the objects tIPFilterParamsExtTTLOper and
         tIPFilterParamsExtTTLVal2 need to be changed then it must be done in
         the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPFilterParamsAction is set to a value other than 'drop (1)' or if
         tIPFilterParamsExtTTLOper is set to a value other than 'range (2)' or
         if tIPFilterParamsExtPktLenOper is set to a value other than 'none
         (0)'."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 6 }

tIPFilterParamsExtTTLOper        OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtTTLOper specifies the way
         how the values of the objects tIPFilterParamsExtTTLVal1 and
         tIPFilterParamsExtTTLVal2 are used to form a condition that must be
         fulfilled in order to execute the action specified by the value of
         tIPFilterParamsAction. Otherwise the opposite action is executed.

         The value of this object can be set to a non-default value only if the
         value of the object tIPFilterParamsAction is 'drop (1)'.

         If the value of this object is being changed from the default value to
         any non-default value the values of the objects
         tIPFilterParamsExtTTLVal1 and tIPFilterParamsExtTTLVal2 (if
         applicable) must be sent in the same SET SNMP request.

         If the value of this object is 'none (0)' than the values of the
         objects tIPFilterParamsExtTTLVal1 and tIPFilterParamsExtTTLVal2 are
         ignored and TRUE case action is always executed (see table below).

         If the value of this object is 'eq (1)' then the value of the
         Time-To-Live field of the IP header of the packet that has matched
         this filter's entry must be equal to the value of the object
         tIPFilterParamsExtTTLVal1 in order to execute the TRUE case action
         (see table below). Otherwise the FALSE case action is executed. The
         value of the object tIPFilterParamsExtTTLVal2 is ignored.

         If the value of this object is 'range (2)' then the value of the
         Time-To-Live field of the IP header of the packet that has matched
         this filter's entry must be greater than or equal to the value of the
         object tIPFilterParamsExtTTLVal1 and less than or equal to the value
         of the object tIPFilterParamsExtTTLVal2 in order to execute the TRUE
         case action (see table below). Otherwise the FALSE case action is
         executed.

         If the value of this object is 'lt (3)' then the value of the
         Time-To-Live field of the IP header of the packet that has matched
         this filter's entry must be less than the value of the object
         tIPFilterParamsExtTTLVal1 in order to execute the TRUE case action
         (see table below). Otherwise the FALSE case action is executed. The
         value of the object tIPFilterParamsExtTTLVal2 is ignored.

         If the value of this object is 'gt (4)' then the value of the
         Time-To-Live field of the IP header of the packet that has matched
         this filter's entry must be greater than the value of the object
         tIPFilterParamsExtTTLVal1 in order to execute the TRUE case action
         (see table below). Otherwise the FALSE case action is executed. The
         value of the object tIPFilterParamsExtTTLVal2 is ignored.


         tIPFilterParamsAction   |   TRUE case action  |  FALSE case action
         ------------------------------------------------------------------
         drop                    |      drop           |      forward


         Allowed ranges for the values of tIPFilterParamsExtTTLVal1 and
         tIPFilterParamsExtTTLVal2 are:

         Operator                | Time-To-Live Value 1| Time-To-Live Value 2
         --------------------------------------------------------------------
         none (0)                |      N/A            |      N/A
         eq(1)                   |    0..255           |      N/A
         range(2)                |    0..254           | (Value1 + 1)..255
         lt(3)                   |    1..255           |      N/A
         gt(4)                   |    0..254           |      N/A


         The values of the objects tIPFilterParamsExtTTLVal1 and
         tIPFilterParamsExtTTLVal2 are silently cleared if the value of this
         object is set to default.

         Note that the value of this object is silently cleared by the system
         if tIPFilterParamsAction is set to a value other than 'drop (1)' or if
         tIPFilterParamsExtPktLenOper is set to a value other than 'none (0)'."
    DEFVAL      { none }
    ::= { tIPFilterParamsExtEntry 7 }

tIPFilterParamsExtEgressPBR      OBJECT-TYPE
    SYNTAX      TFilterEgressPBR
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtEgressPBR specifies if PBR
         specified by tIPFilterParamsExtEntry will have effect when the filter
         is applied on egress.
         tIPFilterParamsExtEgressPBR is applicable with these configured
         actions and action state:
         - no action
         - action forward redirect-policy <policy-name>
         - action forward esi <esi> sf-ip <ip-address> vas-interface <interface-name>
           router <router-instance>
         - action forward esi <esi> sf-ip <ip-address> vas-interface <interface-name>
           router service-name <service-name>
         - action forward next-hop <ip-address>
         - action forward next-hop <ip-address> router <router-instance>
         - action forward next-hop <ip-address> router service-name <service-name>
         - action forward next-hop indirect <ip-address>
         - action forward next-hop indirect <ip-address> router <router-instance>
         - action forward next-hop indirect <ip-address> router
           service-name <service-name>"
    DEFVAL      { disable }
    ::= { tIPFilterParamsExtEntry 8 }

tIPFilterParamsExtEsi            OBJECT-TYPE
    SYNTAX      TFilterEsi
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtEsi specifies the ethernet
         segment identifier (ESI). ESI is mapped by BGP EVPN to an L2 or L3
         capable appliance based on the value of tIPFilterParamsAction. Packets
         matching this entry are steered toward the L2 or L3 appliance.

         The value '0' indicates that there is no ESI specified.

         There are two options how to set the value of tIPFilterParamsExtEsi:
         1. Non zero value of tIPFilterParamsExtEsi is set together with non
            zero values of tIPFilterParamsExtFwdEsiVRtrId,
            tIPFilterParamsExtFwdEsiVasIf and tIPFilterParamsExtFwdEsiSFIp. In
            this case value of tIPFilterParamsAction is set to 'forwardEsiL3' by
            the system.

         2. Non zero value of tIPFilterParamsExtEsi is set together with a non
            zero value of tIPFilterParamsExtFwdEsiSvcId. In this case value of
            tIPFilterParamsAction is set to 'forwardEsiL2' by the system.

         Note: The value of tIPFilterParamsExtEsi is set to '0' by the system
         if the value of tIPFilterParamsAction is set to any value other than
         'forwardEsiL2' or 'forwardEsiL3'."
    DEFVAL      { '00000000000000000000'H }
    ::= { tIPFilterParamsExtEntry 9 }

tIPFilterParamsExtFwdEsiSvcId    OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtFwdEsiSvcId specifies the
         identifier of a VPLS used for VPN/DC connectivity.

         The value '0' indicates that there is no VPLS identifier specified.

         The non zero value of tIPFilterParamsExtFwdEsiSvcId must be set
         together with a non zero value of tIPFilterParamsExtEsi.

         Note: The value of tIPFilterParamsExtFwdEsiSvcId is set to '0' by the
         system if the value of tIPFilterParamsAction is set to any value other
         than 'forwardEsiL2'."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 10 }

tIPFilterParamsExtFwdEsiVRtrId   OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtFwdEsiVRtrId specifies the
         VPRN/rVPLS virtual router identifier used for VPN/DC connectivity.

         The value '0' indicates that there is no VPRN/rVPLS virtual router
         identifier specified.

         The non zero value of tIPFilterParamsExtFwdEsiVRtrId must be set
         together with non zero values of tIPFilterParamsExtEsi,
         tIPFilterParamsExtFwdEsiVasIf and tIPFilterParamsExtFwdEsiSFIp.

         Note: The value of tIPFilterParamsExtFwdEsiVRtrId is set to '0' by the
         system if the value of tIPFilterParamsAction is set to any value other
         than 'forwardEsiL3'."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 11 }

tIPFilterParamsExtFwdEsiSFIp     OBJECT-TYPE
    SYNTAX      InetAddressIPv4
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtFwdEsiSFIp specifies the IP
         address of the service function toward which traffic is steered.

         The value '0' indicates that no service function IP address is
         specified.

         The non zero value of tIPFilterParamsExtFwdEsiSFIp must be set
         together with a non zero values of tIPFilterParamsExtFwdEsiVRtrId,
         tIPFilterParamsExtFwdEsiVasIf and tIPFilterParamsExtEsi.

         Note: The value of tIPFilterParamsExtFwdEsiSFIp is set to default by
         the system if the value of tIPFilterParamsAction is set to any value
         other than 'forwardEsiL3'."
    DEFVAL      { '00000000'H }
    ::= { tIPFilterParamsExtEntry 12 }

tIPFilterParamsExtPbrDwnActOvr   OBJECT-TYPE
    SYNTAX      TFilterPbrDownActionOvr
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtPbrDwnActOvr specifies the
         filter action which will be performed when the PBR/PBF target for this
         entry is not available.

         If the value of tIPvXFltrEntryActAction is not one of the following
         values then tIPFilterParamsExtPbrDwnActOvr must be set to the value
         'none':
         - forwardEsiL2
         - forwardEsiL3
         - forwardSap
         - forwardSdp
         - forwardNextHopRtr

         If the value of tIPFilterParamsExtPbrDwnActOvr is different from
         'none' then PBR/PBF destination availability checking for an entry is
         turned on. There is a limit to the number of filter entries with the
         destination availability checking turned on. Entries with the value of
         tIPvXFltrEntryActAction equal to 'forwardEsiL2' or 'forwardEsiL3' are
         not counted against this limit.

         Refer to the description of the textual convention
         TFilterPbrDownActionOvr for more details."
    DEFVAL      { none }
    ::= { tIPFilterParamsExtEntry 13 }

tIPFilterParamsExtFwdEsiVasIf    OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPFilterParamsExtFwdEsiVasIf specifies the
         virtual router interface index of VPRN RVPLS interface used for VPN/DC
         connectivity.

         The value '0' indicates that no interface id is specified.

         The non zero value of tIPFilterParamsExtFwdEsiVasIf must be set
         together with a non zero values of tIPFilterParamsExtFwdEsiVRtrId,
         tIPFilterParamsExtFwdEsiSFIp and tIPFilterParamsExtEsi.

         Note: The value of tIPFilterParamsExtFwdEsiVasIf is set to '0' by the
         system if the value of tIPFilterParamsAction is set to any value other
         than 'forwardEsiL3'."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 14 }

tIPFilterParamsExtStickyDst      OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtStickyDst specifies how long
         the system will wait (in seconds) until it activates the best action
         (action with available PBR/PBF destination and the highest priority).
         Until then the action specified by tIPFilterParamsExtPbrDwnActOvr will
         be taken on a packet matching the filter entry. After the value of the
         active destination is fixed it will remain unchanged until the active
         PBR/PBF destination becomes unreachable.

         The value of -1 indicates that the property of PBR destination
         stickiness is turned off. When the property of stickiness is turned
         off the active PBR/PBF destination is always the one which is
         available and has the highest priority.

         The countdown starts when there was no PBR/PBF destination reachable
         and any PBR/PBF destination becomes reachable.

         tIPFilterParamsExtStickyDst can be set to value other than -1 only if
         the value of tIPvXFltrEntryActAction is one of following values:
         - forwardSap
         - forwardSdp
         - forwardNextHopRtr"
    DEFVAL      { -1 }
    ::= { tIPFilterParamsExtEntry 15 }

tIPFilterParamsExtHoldRemain     OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtHoldRemain indicates the
         remaining time in seconds, until the best action will become active
         and will be fixed.

         Best action is:
         - primary action if PBR target status of primary action is up.
         - secondary action if PBR target status of secondary action is up
           and PBR target status of primary action is down.
         - none if both PBR targets are down"
    ::= { tIPFilterParamsExtEntry 16 }

tIPFilterParamsExtDownloadAct    OBJECT-TYPE
    SYNTAX      TFilterDownloadedAction
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtDownloadAct indicates the
         filter entry action downloaded to IOM.

         Refer to the description of the textual convention
         TFilterDownloadedAction for more information."
    ::= { tIPFilterParamsExtEntry 17 }

tIPFilterParamsExtTcpFin         OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Fin as per value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsExtEntry 18 }

tIPFilterParamsExtTcpRst         OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Rst as per value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsExtEntry 19 }

tIPFilterParamsExtTcpPsh         OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Psh as per value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsExtEntry 20 }

tIPFilterParamsExtTcpUrg         OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Urg as per value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsExtEntry 21 }

tIPFilterParamsExtTcpEce         OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Ece as per value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsExtEntry 22 }

tIPFilterParamsExtTcpCwr         OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Cwr as per value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsExtEntry 23 }

tIPFilterParamsExtTcpNs          OBJECT-TYPE
    SYNTAX      TItemMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Ns as per value of the object."
    DEFVAL      { off }
    ::= { tIPFilterParamsExtEntry 24 }

tIPFilterParamsExtSrcMac         OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Source MAC to match for this policy filter entry."
    DEFVAL      { '000000000000'H }
    ::= { tIPFilterParamsExtEntry 25 }

tIPFilterParamsExtSrcMacMask     OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Source MAC mask value for this policy MAC filter entry. The mask is
         ANDed with the MAC to match tIPFilterParamsExtSrcMac. A cleared bit
         means ignore this bit, do not match. A set bit means match this bit
         with tIPFilterParamsExtSrcMac. Use the value 00-00-00-00-00-00 to
         disable this filter criteria."
    DEFVAL      { '000000000000'H }
    ::= { tIPFilterParamsExtEntry 26 }

tIPFilterParamsExtMxPktLenVal1   OBJECT-TYPE
    SYNTAX      TFilterPacketLength
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtMxPktLenVal1 specifies the
         value1 to be compared to the value of 'Total Length' field of IPv4
         header of the packet that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPFilterParamsExtMxPktLenOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPFilterParamsExtMxPktLenOper is other than 'none
         (0)'.

         If the value of tIPFilterParamsExtMxPktLenOper is 'range (2)' then the
         value of this object must be less than the value of
         tIPFilterParamsExtMxPktLenVal2.

         If the value of tIPFilterParamsExtMxPktLenOper is 'lt (3)' then the
         value of this object can be set in range 1..65535.

         If the value of tIPFilterParamsExtMxPktLenOper is 'gt (4)' then the
         value of this object can be set in range 0..65534.

         If both the values of the objects tIPFilterParamsExtMxPktLenOper and
         tIPFilterParamsExtMxPktLenVal1 need to be changed then it must be done
         in the same SET SNMP request."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 27 }

tIPFilterParamsExtMxPktLenVal2   OBJECT-TYPE
    SYNTAX      TFilterPacketLength
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtMxPktLenVal2 specifies the
         value2 to be compared to the value of 'Total Length' field of IPv4
         header of the packet that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPFilterParamsExtMxPktLenOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPFilterParamsExtMxPktLenOper is 'range (2)'.

         The value of this object must be greater than the value of
         tIPFilterParamsExtMxPktLenVal1.

         If both the values of the objects tIPFilterParamsExtMxPktLenOper and
         tIPFilterParamsExtMxPktLenVal2 need to be changed then it must be done
         in the same SET SNMP request."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 28 }

tIPFilterParamsExtMxPktLenOper   OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtMxPktLenOper specifies the
         way how the values of the objects tIPFilterParamsExtMxPktLenVal1 and
         tIPFilterParamsExtMxPktLenVal2 are used.

         If the value of this object is 'eq (1)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be equal to the value of the object
         tIPFilterParamsExtMxPktLenVal1 (see table below). The value of the
         object tIPFilterParamsExtMxPktLenVal2 is ignored.

         If the value of this object is 'range (2)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be greater than or equal to the value of the
         object tIPFilterParamsExtMxPktLenVal1 and less than or equal to the
         value of the object tIPFilterParamsExtMxPktLenVal2.

         If the value of this object is 'lt (3)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be less than the value of the object
         tIPFilterParamsExtMxPktLenVal1 (see table below). The value of the
         object tIPFilterParamsExtMxPktLenVal2 is ignored.

         If the value of this object is 'gt (4)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be greater than the value of the object
         tIPFilterParamsExtMxPktLenVal1 (see table below). The value of the
         object tIPFilterParamsExtMxPktLenVal2 is ignored.


         Allowed ranges for the values of tIPFilterParamsExtMxPktLenVal1 and
         tIPFilterParamsExtMxPktLenVal2 are:

         Operator                |Packet Length Value 1|Packet Length Value 2
         --------------------------------------------------------------------
         none (0)                |      N/A            |      N/A
         eq(1)                   |    0..65535         |      N/A
         range(2)                |    0..65534         | (Value1 + 1)..65535
         lt(3)                   |    1..65535         |      N/A
         gt(4)                   |    0..65534         |      N/A"
    DEFVAL      { none }
    ::= { tIPFilterParamsExtEntry 29 }

tIPFilterParamsExtProtocolList   OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "."
    DEFVAL      { ''H }
    ::= { tIPFilterParamsExtEntry 30 }

tIPFilterParamsExtDestClass      OBJECT-TYPE
    SYNTAX      ClassIndexOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtDestClass specifies
         destination class to match."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 31 }

tIPFilterParamsExtSampleProf     OBJECT-TYPE
    SYNTAX      TmnxFilterCflowdSampleProfileId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the sample profile to be applied to packets matching this IP
         filter entry.

         Setting tIPFilterParamsExtSampleProf to a non-default value, will set
         tIPFilterParamsCflowdSample to its default value and vice versa."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 32 }

tIPFilterParamsExtCollectStats   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPFilterParamsExtCollectStats specifies whether or not
         the collection of statistical data for the filter entry is enabled.

         tIPFilterParamsExtCollectStats is supported only on IXR J2 platforms."
    DEFVAL      { false }
    ::= { tIPFilterParamsExtEntry 33 }

tIPFilterParamsExtMxTTLVal1      OBJECT-TYPE
    SYNTAX      TFilterTTL
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtMxTTLVal1 specifies the
         value1 to be compared to the value of 'Time-to-live' field of IPv4
         header of an IP packet that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPFilterParamsExtMxTTLOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPFilterParamsExtMxTTLOper is other than 'none
         (0)'.

         If the value of tIPFilterParamsExtMxTTLOper is 'range (2)' then the
         value of this object must be less than the value of
         tIPFilterParamsExtMxTTLVal2.

         If the value of tIPFilterParamsExtMxTTLOper is 'lt (3)' then the value
         of this object can be set in range 1..255.

         If the value of tIPFilterParamsExtMxTTLOper is 'gt (4)' then the value
         of this object can be set in range 0..254.

         If both the values of the objects tIPFilterParamsExtMxTTLOper and
         tIPFilterParamsExtMxTTLVal1 need to be changed then it must be done in
         the same SET SNMP request."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 34 }

tIPFilterParamsExtMxTTLVal2      OBJECT-TYPE
    SYNTAX      TFilterTTL
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtMxTTLVal2 specifies value2
         to be compared to the value of 'Time-to-live' field of an IP packet
         that has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPFilterParamsExtMxTTLOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPFilterParamsExtMxTTLOper is 'range (2)'.

         The value of this object must be greater than the value of
         tIPFilterParamsExtMxTTLVal1.

         If both the values of the objects tIPFilterParamsExtMxTTLOper and
         tIPFilterParamsExtMxTTLVal2 need to be changed then it must be done in
         the same SET SNMP request."
    DEFVAL      { 0 }
    ::= { tIPFilterParamsExtEntry 35 }

tIPFilterParamsExtMxTTLOper      OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPFilterParamsExtMxTTLOper specifies the way
         how the values of the objects tIPFilterParamsExtMxTTLVal1 and
         tIPFilterParamsExtMxTTLVal2 are used to form a condition for a packet
         match.

         If the value of this object is 'eq (1)' then the value of the
         Time-To-Live field of the IP header of the packet must be equal to the
         value of the object tIPFilterParamsExtMxTTLVal1 in order to match this
         entry. The value of the object tIPFilterParamsExtMxTTLVal2 is ignored.

         If the value of this object is 'range (2)' then the value of the
         Time-To-Live field of the IP header of the packet must be greater than
         or equal to the value of the object tIPFilterParamsExtMxTTLVal1 and
         less than or equal to the value of the object
         tIPFilterParamsExtMxTTLVal2 in order to match this entry.

         If the value of this object is 'lt (3)' then the value of the
         Time-To-Live field of the IP header of the packet must be less than
         the value of the object tIPFilterParamsExtMxTTLVal1 in order to match
         this entry. The value of the object tIPFilterParamsExtMxTTLVal2 is
         ignored.

         If the value of this object is 'gt (4)' then the value of the
         Time-To-Live field of the IP header of the packet must be greater than
         the value of the object tIPFilterParamsExtMxTTLVal1 in order to match
         this entry. The value of the object tIPFilterParamsExtMxTTLVal2 is
         ignored.

         Allowed ranges for the values of tIPFilterParamsExtMxTTLVal1 and
         tIPFilterParamsExtMxTTLVal2 are:

         Operator                | Time-To-Live Value 1| Time-To-Live Value 2
         --------------------------------------------------------------------
         none (0)                |      N/A            |      N/A
         eq(1)                   |    0..255           |      N/A
         range(2)                |    0..254           | (Value1 + 1)..255
         lt(3)                   |    1..255           |      N/A
         gt(4)                   |    0..254           |      N/A"
    DEFVAL      { none }
    ::= { tIPFilterParamsExtEntry 36 }

tIPFilterParamsExtTcpEst         OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If Enabled, matches a TCP Rst or a TCP Ack as per value of the object."
    DEFVAL      { false }
    ::= { tIPFilterParamsExtEntry 37 }

tIPFilterParamsExtPktLenList     OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object specifies the packet length list used as an
         IPv4 filter match criterion.

         The value specified for this object must correspond to a packet length
         list defined in the tFltrPktLenListTable.

         If the value of this object is empty then the values of the objects
         tIPFilterParamsExtMxPktLenOper, tIPFilterParamsExtMxPktLenVal1 and
         tIPFilterParamsExtMxPktLenVal2 are used as packet length match
         criterion.

         When this object is set to a non-empty value then the objects
         tIPFilterParamsExtMxPktLenOper, tIPFilterParamsExtMxPktLenVal1 and
         tIPFilterParamsExtMxPktLenVal2 are reset to their default values by
         the system.

         Vice versa, when a new (non-default) value is provided for the objects
         tIPFilterParamsExtMxPktLenOper, tIPFilterParamsExtMxPktLenVal1 or
         tIPFilterParamsExtMxPktLenVal2, then this object is reset to its
         default (empty) value by the system.

         An attempt to set tIPFilterParamsExtPktLenList to a non-default value
         in combination with setting any of tIPFilterParamsExtMxPktLenOper,
         tIPFilterParamsExtMxPktLenVal1 or tIPFilterParamsExtMxPktLenVal2 to a
         non-default value is rejected by the system"
    DEFVAL      { ''H }
    ::= { tIPFilterParamsExtEntry 38 }

tFilterRPlcyDstTableLastChg      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPlcyDstTableLastChg indicates the
         sysUpTime at the time of the last modification of
         tFilterRPlcyDstTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 54 }

tFilterRPlcyDstTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRPlcyDstEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterRPlcyDstTable contains information pertaining to
         Redirect Policy destinations configured on this system."
    ::= { tFilterObjects 55 }

tFilterRPlcyDstEntry             OBJECT-TYPE
    SYNTAX      TFilterRPlcyDstEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry contains information about a particular Redirect Policy
         destination.

         Rows in the table tFilterRPlcyDstTable are created and destroyed by
         SNMP SET operations on the object tFltrRPDstRowStatus."
    INDEX       {
        tFilterRedirectPolicy,
        tFltrRPDstAddrType,
        tFltrRPDstAddr
    }
    ::= { tFilterRPlcyDstTable 1 }

TFilterRPlcyDstEntry             ::= SEQUENCE
{
    tFltrRPDstAddrType               InetAddressType,
    tFltrRPDstAddr                   InetAddress,
    tFltrRPDstLastChanged            TimeStamp,
    tFltrRPDstRowStatus              RowStatus,
    tFltrRPDstAdminState             TmnxAdminState,
    tFltrRPDstOperState              TmnxOperState,
    tFltrRPDstDescription            TItemDescription,
    tFltrRPDstAdminPriority          Unsigned32,
    tFltrRPDstOperPriority           Unsigned32
}

tFltrRPDstAddrType               OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPDstAddrType specifies the context in
         which the value of the object tFltrRPDstAddr is interpreted.

         Only the following values are supported:
            ipv4(1)
            ipv6(2)

         The value of this object must be the same for all destinations in a
         Redirect Policy."
    ::= { tFilterRPlcyDstEntry 1 }

tFltrRPDstAddr                   OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPDstAddr specifies the IP address of the
         destination.

         The value must be consistent with the IP version value of the
         associated tFltrRPDstAddrType object."
    ::= { tFilterRPlcyDstEntry 2 }

tFltrRPDstLastChanged            OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPDstLastChanged indicates the timestamp
         of last change of this row in tFilterRPlcyDstTable."
    ::= { tFilterRPlcyDstEntry 3 }

tFltrRPDstRowStatus              OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPDstRowStatus specifies the status of
         the conceptual row in tFilterRPlcyDstTable.

         Rows can be created and destroyed by SNMP SET operations on this
         object."
    ::= { tFilterRPlcyDstEntry 4 }

tFltrRPDstAdminState             OBJECT-TYPE
    SYNTAX      TmnxAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPDstAdminState specifies the configured
         administrative state of the destination. If the administrative state
         is 'outOfService' then all tests for this destination will not be
         conducted."
    DEFVAL      { outOfService }
    ::= { tFilterRPlcyDstEntry 5 }

tFltrRPDstOperState              OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPDstOperState indicates the operational
         state of the destination."
    ::= { tFilterRPlcyDstEntry 6 }

tFltrRPDstDescription            OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPDstDescription specifies the
         user-provided description for this destination."
    DEFVAL      { ''H }
    ::= { tFilterRPlcyDstEntry 7 }

tFltrRPDstAdminPriority          OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPDstAdminPriority specifies the
         configured priority for this destination.

         The value is used as a base value for the calculation of the
         operational priority indicated by the value of the object
         tFltrRPDstOperPriority."
    DEFVAL      { 100 }
    ::= { tFilterRPlcyDstEntry 8 }

tFltrRPDstOperPriority           OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPDstOperPriority indicates the current
         dynamic priority of this destination.

         It is derived from the base priority indicated by the value of the
         object tFltrRPDstAdminPriority and results of tests assigned to the
         destination.

         A destination with the highest operational priority across multiple
         destinations in a Redirect Policy is used as the preferred
         destination.

         If the value of the object tFltrRPDstOperState is 'outOfService' then
         the value of this object is '0'."
    ::= { tFilterRPlcyDstEntry 9 }

tFilterRPlcySNMPTestTableLastChg OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFilterRPlcySNMPTestTableLastChg indicates the
         sysUpTime at the time of the last modification of
         tFilterRPlcySNMPTestTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 56 }

tFilterRPlcySNMPTestTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRPlcySNMPTestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The object tFilterRPlcySNMPTestTable contains a list of all redirect
         policies' SNMP tests configured on this system."
    ::= { tFilterObjects 57 }

tFilterRPlcySNMPTestEntry        OBJECT-TYPE
    SYNTAX      TFilterRPlcySNMPTestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The object tFilterRPlcySNMPTestEntry contains information about a
         specific SNMP test. Entries are created/deleted by user. The entry can
         be created only if the value of the object tFltrRPDstAddrType is
         ipv4(1). Entries have a presumed StorageType of nonVolatile."
    INDEX       {
        tFilterRedirectPolicy,
        tFltrRPDstAddrType,
        tFltrRPDstAddr,
        tFltrRPSnmpTest
    }
    ::= { tFilterRPlcySNMPTestTable 1 }

TFilterRPlcySNMPTestEntry        ::= SEQUENCE
{
    tFltrRPSnmpTest                  TNamedItem,
    tFltrRPSnmpTLastChanged          TimeStamp,
    tFltrRPSnmpTRowStatus            RowStatus,
    tFltrRPSnmpTOID                  OBJECT IDENTIFIER,
    tFltrRPSnmpTCommunity            DisplayString,
    tFltrRPSnmpTSnmpVersion          INTEGER,
    tFltrRPSnmpTInterval             Unsigned32,
    tFltrRPSnmpTTimeout              Unsigned32,
    tFltrRPSnmpTDropCount            Unsigned32,
    tFltrRPSnmpTHoldDown             Unsigned32,
    tFltrRPSnmpTHoldDownRemain       Unsigned32,
    tFltrRPSnmpTLastActionTime       TimeStamp,
    tFltrRPSnmpTLastOID              OBJECT IDENTIFIER,
    tFltrRPSnmpTLastType             INTEGER,
    tFltrRPSnmpTLastCounter32Val     Counter32,
    tFltrRPSnmpTLastUnsigned32Val    Unsigned32,
    tFltrRPSnmpTLastTimeTicksVal     TimeTicks,
    tFltrRPSnmpTLastInt32Val         Integer32,
    tFltrRPSnmpTLastOctetStringVal   OCTET STRING,
    tFltrRPSnmpTLastIpAddressVal     IpAddress,
    tFltrRPSnmpTLastOidVal           OBJECT IDENTIFIER,
    tFltrRPSnmpTLastCounter64Val     Counter64,
    tFltrRPSnmpTLastOpaqueVal        Opaque,
    tFltrRPSnmpTLastAction           TmnxFilterRPlcyTestLastAction,
    tFltrRPSnmpTLastPrioChange       Integer32,
    tFltrRPSnmpTNextRespIndex        Integer32
}

tFltrRPSnmpTest                  OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTest specifies the name of the SNMP
         test."
    ::= { tFilterRPlcySNMPTestEntry 1 }

tFltrRPSnmpTLastChanged          OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastChanged indicates the
         timestamp of last change of this row in tFilterRPlcySNMPTestTable."
    ::= { tFilterRPlcySNMPTestEntry 2 }

tFltrRPSnmpTRowStatus            OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTRowStatus specifies the status of
         the conceptual row in tFilterRPlcySNMPTestTable.

         Rows can be created and destroyed by SNMP SET operations on this
         object."
    ::= { tFilterRPlcySNMPTestEntry 3 }

tFltrRPSnmpTOID                  OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTOID specifies the OID of the
         object to be fetched from the destination."
    ::= { tFilterRPlcySNMPTestEntry 4 }

tFltrRPSnmpTCommunity            OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTCommunity specifies the SNMPv1 or
         SNMPv2c Community String or the SNMPv3 Context Name used to conduct
         this SNMP test as described in RFC2571 and RFC2737.

         When the value of tFltrRPSnmpTSnmpVersion is 'snmpv1' or 'snmpv2c'
         this object represents a community string.  When the value of
         tFltrRPSnmpTSnmpVersion is 'snmpv3' this object represents a SNMPv3
         context name."
    DEFVAL      { ''H }
    ::= { tFilterRPlcySNMPTestEntry 5 }

tFltrRPSnmpTSnmpVersion          OBJECT-TYPE
    SYNTAX      INTEGER {
        snmpv1  (1),
        snmpv2c (2),
        snmpv3  (3)
    }
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTSnmpVersion specifies the SNMP PDU
         format to be used while conducting the test. Currently only snmpv2c is
         supported."
    DEFVAL      { snmpv2c }
    ::= { tFilterRPlcySNMPTestEntry 6 }

tFltrRPSnmpTInterval             OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTInterval specifies the amount of
         time in seconds between consecutive requests sent to the far end host."
    DEFVAL      { 1 }
    ::= { tFilterRPlcySNMPTestEntry 7 }

tFltrRPSnmpTTimeout              OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTTimeout specifies the amount of
         time in seconds that is allowed for receiving a response from the far
         end host. If the response is not received within this time the far end
         host is considered unresponsive."
    DEFVAL      { 1 }
    ::= { tFilterRPlcySNMPTestEntry 8 }

tFltrRPSnmpTDropCount            OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTDropCount specifies the number of
         consecutive requests that must fail for the destination to be declared
         unreachable."
    DEFVAL      { 3 }
    ::= { tFilterRPlcySNMPTestEntry 9 }

tFltrRPSnmpTHoldDown             OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTHoldDown specifies the amount of
         time in seconds that the system should be held down if this test has
         marked it unreachable."
    DEFVAL      { 0 }
    ::= { tFilterRPlcySNMPTestEntry 10 }

tFltrRPSnmpTHoldDownRemain       OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTHoldDownRemain indicates the
         amount of time in seconds that the system will remain in held down
         state before being used again."
    ::= { tFilterRPlcySNMPTestEntry 11 }

tFltrRPSnmpTLastActionTime       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastActionTime indicates the time
         stamp when this test received a response for a probe sent out."
    ::= { tFilterRPlcySNMPTestEntry 12 }

tFltrRPSnmpTLastOID              OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastOID indicates the OID received
         in the response."
    ::= { tFilterRPlcySNMPTestEntry 13 }

tFltrRPSnmpTLastType             OBJECT-TYPE
    SYNTAX      INTEGER {
        none        (0),
        counter32   (1),
        unsigned32  (2),
        timeTicks   (3),
        integer32   (4),
        ipAddress   (5),
        octetString (6),
        objectId    (7),
        counter64   (8),
        opaque      (9)
    }
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastType indicates the type of the
         last received SNMP object.

         Value none(0) indicates that no object was received.

         Value 'counter32' indicates that the value of SNMP object is of type
         Counter32.

         Value 'unsigned32' indicates that the value of SNMP object is of type
         Unsigned32.

         Value 'timeTicks' indicates that the value of SNMP object is of type
         timeTicks.

         Value 'integer32' indicates that the value of SNMP object is of type
         integer32.

         Value 'ipAddress' indicates that the value of SNMP object is of type
         ipAddress.

         Value 'octetString' indicates that the value of SNMP object is of type
         OCTET STRING.

         Value 'objectId' indicates that the value of SNMP object is of type
         OBJECT IDENTIFIER.

         Value 'counter64' indicates that the value of SNMP object is of type
         Counter64.

         Value 'unsigned32' indicates that the value of SNMP object is of type
         Unsigned32.

         Value 'opaque' indicates that the value of SNMP object is of type
         Opaque."
    ::= { tFilterRPlcySNMPTestEntry 14 }

tFltrRPSnmpTLastCounter32Val     OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastCounter32Val indicates the
         value of an object received in the last test response, if the type of
         the received object is 'counter32'. When this object is set the value
         of the object tFltrRPSnmpTLastType is 'counter32'."
    ::= { tFilterRPlcySNMPTestEntry 15 }

tFltrRPSnmpTLastUnsigned32Val    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastUnsigned32Val indicates the
         value of an object received in the last test response, if the type of
         the received object is 'unsigned32'. When this object is set the value
         of the object tFltrRPSnmpTLastType is 'unsigned32'."
    ::= { tFilterRPlcySNMPTestEntry 16 }

tFltrRPSnmpTLastTimeTicksVal     OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastTimeTicksVal indicates the
         value of an object received in the last test response, if the type of
         the received object is 'timeTicks'. When this object is set the value
         of the object tFltrRPSnmpTLastType is 'timeTicks'."
    ::= { tFilterRPlcySNMPTestEntry 17 }

tFltrRPSnmpTLastInt32Val         OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastInt32Val indicates the value
         of an object received in the last test response, if the type of the
         received object is 'integer32'. When this object is set the value of
         the object tFltrRPSnmpTLastType is 'integer32'."
    ::= { tFilterRPlcySNMPTestEntry 18 }

tFltrRPSnmpTLastOctetStringVal   OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastOctetStringVal indicates the
         value of an object received in the last test response, if the type of
         the received object is 'octetString'. When this object is set the
         value of the object tFltrRPSnmpTLastType is 'octetString'."
    ::= { tFilterRPlcySNMPTestEntry 19 }

tFltrRPSnmpTLastIpAddressVal     OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastIpAddressVal indicates the
         value of an object received in the last test response, if the type of
         the received object is 'ipAddress'. When this object is set the value
         of the object tFltrRPSnmpTLastType is 'ipAddress'.

         This object is used only for IPv4 addresses. IPv6 addresses are
         represented using TAddress or InetAddress, and so the underlying
         datatype is OCTET STRING, and their value would be stored in the
         tFltrRPSnmpTLastOctetStringVal column."
    ::= { tFilterRPlcySNMPTestEntry 20 }

tFltrRPSnmpTLastOidVal           OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastOidVal indicates the value of
         an object received in the last test response, if the type of the
         received object is 'objectId'. When this object is set the value of
         the object tFltrRPSnmpTLastType is 'objectId'."
    ::= { tFilterRPlcySNMPTestEntry 21 }

tFltrRPSnmpTLastCounter64Val     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastCounter64Val indicates that
         the value of an object received in the last test response, if the type
         of the received object is 'counter64'. When this object is set the
         value of the object tFltrRPSnmpTLastType is 'counter64'."
    ::= { tFilterRPlcySNMPTestEntry 22 }

tFltrRPSnmpTLastOpaqueVal        OBJECT-TYPE
    SYNTAX      Opaque (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastOpaqueVal indicates the value
         of an object received in the last test response, if the type of the
         received object is 'opaque'. When this object is set the value of the
         object tFltrRPSnmpTLastType is 'opaque'."
    ::= { tFilterRPlcySNMPTestEntry 23 }

tFltrRPSnmpTLastAction           OBJECT-TYPE
    SYNTAX      TmnxFilterRPlcyTestLastAction
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastAction indicates an impact
         that the last test probe had on the value of the object
         tFltrRPDstOperState.

         If the value is 'disable', the destination may not be used for
         tFltrRPSnmpTHoldDown seconds."
    ::= { tFilterRPlcySNMPTestEntry 24 }

tFltrRPSnmpTLastPrioChange       OBJECT-TYPE
    SYNTAX      Integer32 (-255..255)
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTLastPrioChange indicates the
         priority change that the last test probe made to the operational
         priority of the destination. This object is significant only if the
         value of the object tFltrRPSnmpTLastAction is 'enable'. Otherwise it
         has no significance and it's holding the value '0'."
    ::= { tFilterRPlcySNMPTestEntry 25 }

tFltrRPSnmpTNextRespIndex        OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 1..2147483647)
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpTNextRespIndex indicates the next
         response index to be used while creating a row in the
         tFilterRPlcySNMPRespTable.

         The value of '-1' means that the maximum number of return values for
         this OID is already configured."
    ::= { tFilterRPlcySNMPTestEntry 26 }

tFilterRPlcySNMPRespTableLastChg OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFilterRPlcySNMPRespTableLastChg indicates the
         sysUpTime at the time of the last modification of
         tFilterRPlcySNMPRespTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 58 }

tFilterRPlcySNMPRespTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRPlcySNMPRespEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Each row in this table holds the effect of the test on the destination
         for a specific return value.

         Each row is created once and cannot be modified after creation. Any
         change attempts will be silently discarded."
    ::= { tFilterObjects 59 }

tFilterRPlcySNMPRespEntry        OBJECT-TYPE
    SYNTAX      TFilterRPlcySNMPRespEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Information about action to be taken for a specific destination when a
         specific response is received.

         Each row is created once and cannot be modified after creation. Any
         change attempts will be silently discarded."
    INDEX       {
        tFilterRedirectPolicy,
        tFltrRPDstAddrType,
        tFltrRPDstAddr,
        tFltrRPSnmpTest,
        tFltrRPSnmpRspId
    }
    ::= { tFilterRPlcySNMPRespTable 1 }

TFilterRPlcySNMPRespEntry        ::= SEQUENCE
{
    tFltrRPSnmpRspId                 Integer32,
    tFltrRPSnmpRspLastChanged        TimeStamp,
    tFltrRPSnmpRspRowStatus          RowStatus,
    tFltrRPSnmpRspAction             TmnxFilterRPlcyTestRespAction,
    tFltrRPSnmpRspPrioChange         Unsigned32,
    tFltrRPSnmpRspOID                OBJECT IDENTIFIER,
    tFltrRPSnmpRspType               INTEGER,
    tFltrRPSnmpRspCounter32Val       Unsigned32,
    tFltrRPSnmpRspUnsigned32Val      Unsigned32,
    tFltrRPSnmpRspTimeTicksVal       Unsigned32,
    tFltrRPSnmpRspInt32Val           Integer32,
    tFltrRPSnmpRspOctetStringVal     OCTET STRING,
    tFltrRPSnmpRspIpAddressVal       IpAddress,
    tFltrRPSnmpRspOidVal             OBJECT IDENTIFIER,
    tFltrRPSnmpRspCounter64Val       Counter64,
    tFltrRPSnmpRspOpaqueVal          Opaque
}

tFltrRPSnmpRspId                 OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspId indicates the ID of the
         response entry."
    ::= { tFilterRPlcySNMPRespEntry 1 }

tFltrRPSnmpRspLastChanged        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspLastChanged indicates the
         timestamp of last change of this row in tFilterRPlcySNMPRespTable."
    ::= { tFilterRPlcySNMPRespEntry 2 }

tFltrRPSnmpRspRowStatus          OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspRowStatus specifies the status
         of the conceptual row in tFilterRPlcySNMPRespTable.

         Rows can be created and destroyed by SNMP SET operations on this
         object."
    ::= { tFilterRPlcySNMPRespEntry 3 }

tFltrRPSnmpRspAction             OBJECT-TYPE
    SYNTAX      TmnxFilterRPlcyTestRespAction
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspAction specifies the action
         which will be taken on the operational priority of a destination
         (tFilterRDOperPriority), if the received object OID and value matches
         the values defined in TFilterRPlcySNMPRespEntry.

         This object cannot be modified after creation."
    DEFVAL      { disable }
    ::= { tFilterRPlcySNMPRespEntry 4 }

tFltrRPSnmpRspPrioChange         OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspPrioChange specifies the offset
         to be applied to the destination base priority
         (tFilterRDAdminPriority) in order to compute the tFilterRDOperPriority
         as a result of this test, if the tFltrRPSnmpRspAction is either
         'increase' or 'decrease'.

         This object cannot be modified after creation."
    DEFVAL      { 0 }
    ::= { tFilterRPlcySNMPRespEntry 5 }

tFltrRPSnmpRspOID                OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspOID specifies the OID to be
         received in the response.

         This field cannot be modified after creation."
    ::= { tFilterRPlcySNMPRespEntry 6 }

tFltrRPSnmpRspType               OBJECT-TYPE
    SYNTAX      INTEGER {
        counter32   (1),
        unsigned32  (2),
        timeTicks   (3),
        integer32   (4),
        ipAddress   (5),
        octetString (6),
        objectId    (7),
        counter64   (8),
        opaque      (9)
    }
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspType specifies the type of the
         SNMP object to be received.

         Note: types 'objectId' and 'counter64' are not supported for now, and
         will be rejected when used.

         This object cannot be modified after creation. Any change attempts
         will be silently discarded.

         Value 'counter32' indicates that the value of SNMP object is of type
         Counter32.

         Value 'unsigned32' indicates that the value of SNMP object is of type
         Unsigned32.

         Value 'timeTicks' indicates that the value of SNMP object is of type
         timeTicks.

         Value 'integer32' indicates that the value of SNMP object is of type
         integer32.

         Value 'ipAddress' indicates that the value of SNMP object is of type
         ipAddress.

         Value 'octetString' indicates that the value of SNMP object is of type
         OCTET STRING.

         Value 'objectId' indicates that the value of SNMP object is of type
         OBJECT IDENTIFIER.

         Value 'counter64' indicates that the value of SNMP object is of type
         Counter64.

         Value 'unsigned32' indicates that the value of SNMP object is of type
         Unsigned32.

         Value 'opaque' indicates that the value of SNMP object is of type
         Opaque."
    ::= { tFilterRPlcySNMPRespEntry 7 }

tFltrRPSnmpRspCounter32Val       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspCounter32Val specifies the value
         of type Counter32 which the object received in the test response
         should have in order to pass the test.

         When this value is specified the value of the object
         tFltrRPSnmpRspType should be set to 'counter32'.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded."
    ::= { tFilterRPlcySNMPRespEntry 8 }

tFltrRPSnmpRspUnsigned32Val      OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspUnsigned32Val specifies the
         value of type Unsigned32 which the object received in the test
         response should have in order to pass the test.

         When this value is specified the value of the object
         tFltrRPSnmpRspType should be set to 'unsigned32'.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded."
    ::= { tFilterRPlcySNMPRespEntry 9 }

tFltrRPSnmpRspTimeTicksVal       OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspTimeTicksVal specifies the value
         of type TimeTicks which the object received in the test response
         should have in order to pass the test.

         When this value is specified the value of the object
         tFltrRPSnmpRspType should be set to 'timeTicks'.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded."
    ::= { tFilterRPlcySNMPRespEntry 10 }

tFltrRPSnmpRspInt32Val           OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspInt32Val specifies the value of
         type Integer32 which the object received in the test response should
         have in order to pass the test.

         When this value is specified the value of the object
         tFltrRPSnmpRspType should be set to 'integer32'.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded."
    ::= { tFilterRPlcySNMPRespEntry 11 }

tFltrRPSnmpRspOctetStringVal     OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..255))
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspOctetStringVal specifies the
         value of type OCTET STRING which the object received in the test
         response should have in order to pass the test.

         When this value is specified the value of the object
         tFltrRPSnmpRspType should be set to 'octetString'.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded."
    ::= { tFilterRPlcySNMPRespEntry 12 }

tFltrRPSnmpRspIpAddressVal       OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspIpAddressVal specifies the  IPv4
         address which the object received in the test response should have
         in order to pass the test.

         When this value is specified the value of the object
         tFltrRPSnmpRspType should be set to 'ipAddress'.

         IPv6 addresses are represented using TAddress or InetAddress, and so
         the underlying data type is OCTET STRING, and their value would be
         stored in the tFltrRPSnmpRspOctetStringVal column.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded."
    ::= { tFilterRPlcySNMPRespEntry 13 }

tFltrRPSnmpRspOidVal             OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspOidVal specifies the OID which
         the object received in the test response should have in order to pass
         the test.

         When this value is specified the value of the object
         tFltrRPSnmpRspType should be set to 'objectId'.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded."
    ::= { tFilterRPlcySNMPRespEntry 14 }

tFltrRPSnmpRspCounter64Val       OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspCounter64Val specifies the value
         of type Counter64 which the object received in the test response
         should have in order to pass the test.

         When this value is specified the value of the object
         tFltrRPSnmpRspType should be set to 'counter64'.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded."
    ::= { tFilterRPlcySNMPRespEntry 15 }

tFltrRPSnmpRspOpaqueVal          OBJECT-TYPE
    SYNTAX      Opaque (SIZE (0..255))
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPSnmpRspOpaqueVal specifies the value of
         type Opaque which the object received in the test response should have
         in order to pass the test.

         When this value is specified the value of the object
         tFltrRPSnmpRspType should be set to 'opaque'.

         This field cannot be modified after creation. Any change attempts will
         be silently discarded."
    ::= { tFilterRPlcySNMPRespEntry 16 }

tFilterRPlcyURLTestTableLastChg  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFilterRPlcyURLTestTableLastChg indicates the
         sysUpTime at the time of the last modification of
         tFilterRPlcyURLTestTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 60 }

tFilterRPlcyURLTestTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRPlcyURLTestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "This table contains a list of all redirect URL tests configured on
         this system."
    ::= { tFilterObjects 61 }

tFilterRPlcyURLTestEntry         OBJECT-TYPE
    SYNTAX      TFilterRPlcyURLTestEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Information about a specific URL test configured for a destination.
         Entries are created/deleted  by user.
         The entry can be created only if the value of the object
         tFltrRPDstAddrType is ipv4(1).
         Entries have a presumed StorageType of nonVolatile."
    INDEX       {
        tFilterRedirectPolicy,
        tFltrRPDstAddrType,
        tFltrRPDstAddr,
        tFltrRPUrlTest
    }
    ::= { tFilterRPlcyURLTestTable 1 }

TFilterRPlcyURLTestEntry         ::= SEQUENCE
{
    tFltrRPUrlTest                   TNamedItem,
    tFltrRPUrlTLastChanged           TimeStamp,
    tFltrRPUrlTRowStatus             RowStatus,
    tFltrRPUrlTUrl                   DisplayString,
    tFltrRPUrlTHttpVersion           DisplayString,
    tFltrRPUrlTInterval              Unsigned32,
    tFltrRPUrlTTimeout               Unsigned32,
    tFltrRPUrlTDropCount             Unsigned32,
    tFltrRPUrlTHoldDown              Unsigned32,
    tFltrRPUrlTHoldDownRemain        Unsigned32,
    tFltrRPUrlTLastActionTime        TimeStamp,
    tFltrRPUrlTLastRetCode           Unsigned32,
    tFltrRPUrlTLastAction            TmnxFilterRPlcyTestLastAction,
    tFltrRPUrlTLastPrioChange        Integer32
}

tFltrRPUrlTest                   OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTest specifies the name of the URL
         test."
    ::= { tFilterRPlcyURLTestEntry 1 }

tFltrRPUrlTLastChanged           OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTLastChanged indicates the timestamp
         of last change of this row in tFilterRPlcyURLTestTable."
    ::= { tFilterRPlcyURLTestEntry 2 }

tFltrRPUrlTRowStatus             OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTRowStatus specifies the status of
         the conceptual row in tFilterRPlcyURLTestTable.

         Rows in tFilterRPlcyURLTestTable can be created and destroyed by SNMP
         SET operations on this object."
    ::= { tFilterRPlcyURLTestEntry 3 }

tFltrRPUrlTUrl                   OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTUrl specifies the URL to be probed."
    DEFVAL      { ''H }
    ::= { tFilterRPlcyURLTestEntry 4 }

tFltrRPUrlTHttpVersion           OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTHttpVersion specifies HTTP Version
         to be used while performing the URL test. The system by default uses
         HTTP Version 1.1 until explicitly specified."
    DEFVAL      { "1.1" }
    ::= { tFilterRPlcyURLTestEntry 5 }

tFltrRPUrlTInterval              OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTInterval specifies the amount of
         time in seconds between consecutive requests sent to the far end host."
    DEFVAL      { 1 }
    ::= { tFilterRPlcyURLTestEntry 6 }

tFltrRPUrlTTimeout               OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTTimeout specifies the amount of
         time in seconds that is allowed for receiving a response from the far
         end host. If the response is not received within this time the far end
         host is considered unresponsive."
    DEFVAL      { 1 }
    ::= { tFilterRPlcyURLTestEntry 7 }

tFltrRPUrlTDropCount             OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTDropCount specifies the number of
         consecutive requests that must fail for the destination to be declared
         unreachable."
    DEFVAL      { 3 }
    ::= { tFilterRPlcyURLTestEntry 8 }

tFltrRPUrlTHoldDown              OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTHoldDown specifies the amount of
         time in seconds that the system should be held down this test has
         marked it unreachable."
    DEFVAL      { 0 }
    ::= { tFilterRPlcyURLTestEntry 9 }

tFltrRPUrlTHoldDownRemain        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTHoldDownRemain indicates the amount
         of time in seconds that the system will remain in held down state
         before being used again."
    ::= { tFilterRPlcyURLTestEntry 10 }

tFltrRPUrlTLastActionTime        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTLastActionTime indicates the time
         stamp when this test received a response for a probe sent out."
    ::= { tFilterRPlcyURLTestEntry 11 }

tFltrRPUrlTLastRetCode           OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTLastRetCode indicates the return
         code received in the last response."
    ::= { tFilterRPlcyURLTestEntry 12 }

tFltrRPUrlTLastAction            OBJECT-TYPE
    SYNTAX      TmnxFilterRPlcyTestLastAction
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTLastAction indicates impact that
         the last test probe had on the operational status of the destination
         as maintained in tFilterRDOperState.

         If the last action was 'disable', the destination may not be used for
         tFltrRPUrlTHoldDown seconds."
    ::= { tFilterRPlcyURLTestEntry 13 }

tFltrRPUrlTLastPrioChange        OBJECT-TYPE
    SYNTAX      Integer32 (-255..255)
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTLastPrioChange indicates the
         priority change that the last test probe made to the operational
         priority of the destination. This object is significant only if the
         value of the object tFltrRPUrlTLastAction is 'enable'. Otherwise it
         has no significance and it's holding the value '0'."
    ::= { tFilterRPlcyURLTestEntry 14 }

tFilterRPlcyURLRespTableLastChg  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFilterRPlcyURLRespTableLastChg indicates the
         sysUpTime at the time of the last modification of
         tFilterRPlcyURLRespTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 62 }

tFilterRPlcyURLRespTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRPlcyURLRespEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Each row in this table specifies the effect of the test on the
         destination for a range of return values."
    ::= { tFilterObjects 63 }

tFilterRPlcyURLRespEntry         OBJECT-TYPE
    SYNTAX      TFilterRPlcyURLRespEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "Entry contains information about an action to be taken for a specific
         destination when a return value within the range specifies by
         tFltrRPUrlTRspLowRspCode and tFltrRPUrlTRspHighRspCode is received."
    INDEX       {
        tFilterRedirectPolicy,
        tFltrRPDstAddrType,
        tFltrRPDstAddr,
        tFltrRPUrlTest,
        tFltrRPUrlTRspLowRspCode,
        tFltrRPUrlTRspHighRspCode
    }
    ::= { tFilterRPlcyURLRespTable 1 }

TFilterRPlcyURLRespEntry         ::= SEQUENCE
{
    tFltrRPUrlTRspLowRspCode         Unsigned32,
    tFltrRPUrlTRspHighRspCode        Unsigned32,
    tFltrRPUrlTRspLastChanged        TimeStamp,
    tFltrRPUrlTRspRowStatus          RowStatus,
    tFltrRPUrlTRspAction             TmnxFilterRPlcyTestRespAction,
    tFltrRPUrlTRspPrioChange         Unsigned32
}

tFltrRPUrlTRspLowRspCode         OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTRspLowRspCode specifies the lower
         return code of the range specified by this entry."
    ::= { tFilterRPlcyURLRespEntry 1 }

tFltrRPUrlTRspHighRspCode        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTRspHighRspCode specifies the higher
         return code of the range specified by this entry."
    ::= { tFilterRPlcyURLRespEntry 2 }

tFltrRPUrlTRspLastChanged        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTRspLastChanged indicates the
         timestamp of last change of this row in tFilterRPlcyURLRespTable."
    ::= { tFilterRPlcyURLRespEntry 3 }

tFltrRPUrlTRspRowStatus          OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTRspRowStatus specifies the status
         of the conceptual row in tFilterRPlcyURLRespTable.

         Rows can be created and destroyed by SNMP SET operations on this
         object."
    ::= { tFilterRPlcyURLRespEntry 4 }

tFltrRPUrlTRspAction             OBJECT-TYPE
    SYNTAX      TmnxFilterRPlcyTestRespAction
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tFltrRPUrlTRspAction specifies the action
         which will be taken on the operational priority of a destination
         (tFilterRDOperPriority), if the received object OID and value matches
         the values defined in TFilterRPlcySNMPRespEntry."
    DEFVAL      { disable }
    ::= { tFilterRPlcyURLRespEntry 5 }

tFltrRPUrlTRspPrioChange         OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "If the tFltrRPUrlTRspAction is either 'increase' or 'decrease', the
         value of the object tFltrRPUrlTRspPrioChange specifies the offset to
         be applied to the destination base priority (tFilterRDAdminPriority)
         in order to compute the tFilterRDOperPriority as a result of this
         test."
    DEFVAL      { 0 }
    ::= { tFilterRPlcyURLRespEntry 6 }

tFilterRPlcyPingTestTableLastChg OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPlcyPingTestTableLastChg indicates the
         sysUpTime at the time of the last modification of
         tFilterRPlcyPingTestTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 64 }

tFilterRPlcyPingTestTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRPlcyPingTestEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterRPlcyPingTestTable contains a list of all redirect
         Ping tests configured on this system."
    ::= { tFilterObjects 65 }

tFilterRPlcyPingTestEntry        OBJECT-TYPE
    SYNTAX      TFilterRPlcyPingTestEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry contains information about a specific Ping test. Entries are
         created/deleted by user and have a presumed StorageType of
         nonVolatile."
    INDEX       {
        tFilterRedirectPolicy,
        tFltrRPDstAddrType,
        tFltrRPDstAddr
    }
    ::= { tFilterRPlcyPingTestTable 1 }

TFilterRPlcyPingTestEntry        ::= SEQUENCE
{
    tFltrRPPingTLastChanged          TimeStamp,
    tFltrRPPingTRowStatus            RowStatus,
    tFltrRPPingTInterval             Unsigned32,
    tFltrRPPingTTimeout              Unsigned32,
    tFltrRPPingTDropCount            Unsigned32,
    tFltrRPPingTHoldDown             Unsigned32,
    tFltrRPPingTHoldDownRemain       Unsigned32,
    tFltrRPPingTLastActionTime       TimeStamp,
    tFltrRPPingTLastAction           TmnxFilterRPlcyTestLastAction,
    tFilterRPPingSrcAddressAddrType  InetAddressType,
    tFilterRPPingSrcAddressAddr      InetAddress
}

tFltrRPPingTLastChanged          OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPPingTLastChanged indicates the
         timestamp of last change of this row in tFilterRPlcyPingTestTable."
    ::= { tFilterRPlcyPingTestEntry 1 }

tFltrRPPingTRowStatus            OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPPingTRowStatus specifies the status of
         the conceptual row in tFilterRPlcyPingTestTable.

         Rows are created and destroyed by SNMP SET operations on this object."
    ::= { tFilterRPlcyPingTestEntry 2 }

tFltrRPPingTInterval             OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPPingTInterval specifies the amount of
         time in seconds between consecutive requests sent to the far end host.

         Note that the value of tFltrRPPingTInterval can only be modified if
         the value of the corresponding tFilterRPAdminState and/or
         tFltrRPDstAdminState object is outOfService."
    DEFVAL      { 1 }
    ::= { tFilterRPlcyPingTestEntry 3 }

tFltrRPPingTTimeout              OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPPingTTimeout specifies the amount of
         time in seconds that is allowed for receiving a response from the far
         end host. If a reply is not received within this time the far end host
         is considered unresponsive.

         Note that the value of tFltrRPPingTTimeout can only be modified if the
         value of the corresponding tFilterRPAdminState and/or
         tFltrRPDstAdminState object is outOfService."
    DEFVAL      { 1 }
    ::= { tFilterRPlcyPingTestEntry 4 }

tFltrRPPingTDropCount            OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPPingTDropCount specifies the number of
         consecutive requests that must fail for the destination to be declared
         unreachable."
    DEFVAL      { 3 }
    ::= { tFilterRPlcyPingTestEntry 5 }

tFltrRPPingTHoldDown             OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPPingTHoldDown specifies the amount of
         time in seconds that the system should be held down if any of the test
         has marked it unreachable."
    DEFVAL      { 0 }
    ::= { tFilterRPlcyPingTestEntry 6 }

tFltrRPPingTHoldDownRemain       OBJECT-TYPE
    SYNTAX      Unsigned32 (0..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPPingTHoldDownRemain indicates the
         amount of time in seconds that the system will remain in held down
         state before being used again."
    ::= { tFilterRPlcyPingTestEntry 7 }

tFltrRPPingTLastActionTime       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPPingTLastActionTime maintains the time
         stamp when this test received a response for a probe sent out."
    ::= { tFilterRPlcyPingTestEntry 8 }

tFltrRPPingTLastAction           OBJECT-TYPE
    SYNTAX      TmnxFilterRPlcyTestLastAction
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPPingTLastAction maintains impact that
         the last test probe made on the operational status of the destination
         as maintained in tFltrRPDstOperState.

         If the last action was 'disable', the destination may not be used for
         tFilterRPTHoldDown seconds."
    ::= { tFilterRPlcyPingTestEntry 9 }

tFilterRPPingSrcAddressAddrType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPPingSrcAddressAddrType indicates the
         context in which the values of the objects tFilterRPPingSrcAddressAddr
         are interpreted.

         Only following values are supported:
           unknown(0)
           ipv4(1)
           ipv6(2)

         The value 'unknown' indicates IP address type is not specified.

         The non zero value of tFilterRPPingSrcAddressAddrType must be set
         together with non zero values of tFilterRPPingSrcAddressAddr."
    DEFVAL      { unknown }
    ::= { tFilterRPlcyPingTestEntry 10 }

tFilterRPPingSrcAddressAddr      OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPPingSrcAddressAddr indicates the
         source IP address to use in the ping test. The value should be a
         router local address to make sure the reply reaches the CPM.

         The value must be consistent with the IP version value of the
         associated tFilterRPActiveDestAddrType object."
    DEFVAL      { ''H }
    ::= { tFilterRPlcyPingTestEntry 11 }

tFilterRPlcyUcastRtTTableLastChg OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPlcyUcastRtTTableLastChg indicates the
         sysUpTime at the time of the last modification of
         tFilterRPlcyUnicastRtTestTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 66 }

tFilterRPlcyUnicastRtTestTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRPlcyUnicastRtTestEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterRPlcyUnicastRtTestTable contains list of all Unicast
         Route Reachability tests configured on this system."
    ::= { tFilterObjects 67 }

tFilterRPlcyUnicastRtTestEntry   OBJECT-TYPE
    SYNTAX      TFilterRPlcyUnicastRtTestEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Entry contains information about a specific Unicast Route Reachability
         test configured for a destination in a Redirect Policy.

         There can be only one Unicast Route Reachability test configured per
         destination.

         Upon creation of the entry the IP address of the destination specified
         by the values of the objects tFltrRPDstAddrType and tFltrRPDstAddr and
         optionally (if not equal to the default value) the virtual router
         instance ID specified by the value of the object tFilterRPVrtrId is
         registered with RTM module.

         Redirect policy is then informed about any change of the reachability
         of the destination (based on availability of a route in a particular
         routing table) and modifies the value of the object
         tFltrRPDstOperState accordingly.

         An entry in the table tFilterRPlcyUnicastRtTestTable is created and
         destroyed by SNMP SET operations on the object
         tFltrRPUcastRtTRowStatus."
    INDEX       {
        tFilterRedirectPolicy,
        tFltrRPDstAddrType,
        tFltrRPDstAddr
    }
    ::= { tFilterRPlcyUnicastRtTestTable 1 }

TFilterRPlcyUnicastRtTestEntry   ::= SEQUENCE
{
    tFltrRPUcastRtTLastChanged       TimeStamp,
    tFltrRPUcastRtTRowStatus         RowStatus,
    tFltrRPUcastRtTLastActionTime    TimeStamp,
    tFltrRPUcastRtTLastAction        TmnxFilterRPlcyTestLastAction
}

tFltrRPUcastRtTLastChanged       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPUcastRtTLastChanged indicates the
         timestamp of last change of this row in
         tFilterRPlcyUnicastRtTestTable."
    ::= { tFilterRPlcyUnicastRtTestEntry 1 }

tFltrRPUcastRtTRowStatus         OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPUcastRtTRowStatus specifies the status
         of the conceptual row in tFilterRPlcyUnicastRtTestTable.

         Rows are created and destroyed by SNMP SET operations on this object."
    ::= { tFilterRPlcyUnicastRtTestEntry 2 }

tFltrRPUcastRtTLastActionTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPUcastRtTLastActionTime indicates the
         time stamp when the last update from RTM module for this destination
         was received."
    ::= { tFilterRPlcyUnicastRtTestEntry 3 }

tFltrRPUcastRtTLastAction        OBJECT-TYPE
    SYNTAX      TmnxFilterRPlcyTestLastAction
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrRPUcastRtTLastAction indicates an impact
         that the last message from RTM module had on the value of the object
         tFltrRPDstOperState."
    ::= { tFilterRPlcyUnicastRtTestEntry 4 }

tFilterSystemFilterTableLastChg  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterSystemFilterTableLastChg indicates the
         sysUpTime at the time of the last modification of
         tFilterSystemFilterTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 68 }

tFilterSystemFilterTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterSystemFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterSystemFilterTable contains information pertaining to
         active IP and IPv6 system filter policies."
    ::= { tFilterObjects 69 }

tFilterSystemFilterEntry         OBJECT-TYPE
    SYNTAX      TFilterSystemFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry contains details about an active system filter policy.

         Only one active system filter policy per filter type can be configured
         in release 0.0.

         Upon creation of the entry the system filter policy identified by the
         values of the objects tFilterSystemFilterType and
         tFilterSystemFilterId is activated and downloaded to all line cards.

         Regular IP or IPv6 filter policies that have the value of the object
         tIPFilterChainToSystemFilter or tIPv6FilterChainToSystemFilter set to
         'true(1)' are then chained to the active system filter policy. The
         system filter policy's rules are executed first before any rules of
         the regular filter policy are executed.

         An entry in the table tFilterSystemFilterTable is created and
         destroyed by SNMP SET operations on the object
         tFilterSystemFilterRowStatus.

         Furthermore an entry in the table tFilterSystemFilterTable is
         destroyed by the system if an entry with the same value of the object
         tFilterSystemFilterType is created so that there is always at most one
         entry for a given value of tFilterSystemFilterType."
    INDEX       {
        tFilterSystemFilterType,
        tFilterSystemFilterId
    }
    ::= { tFilterSystemFilterTable 1 }

TFilterSystemFilterEntry         ::= SEQUENCE
{
    tFilterSystemFilterType          TFilterType,
    tFilterSystemFilterId            TConfigOrVsdFilterID,
    tFilterSystemFilterLastChanged   TimeStamp,
    tFilterSystemFilterRowStatus     RowStatus
}

tFilterSystemFilterType          OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterSystemFilterType specifies the filter
         type of the system filter policy to be selected as the active system
         filter policy.

         Only values 'fltrtypeselIp(1)' and 'fltrtypeselIpv6(4)' are supported."
    ::= { tFilterSystemFilterEntry 1 }

tFilterSystemFilterId            OBJECT-TYPE
    SYNTAX      TConfigOrVsdFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterSystemFilterId specifies the ID of the
         filter policy to be selected as the active system filter policy.
         Values outside of range 1..65535 are reserved for entries dynamically
         created by the system and cannot be used in any SNMP SET operation.

         If the value of the object tFilterSystemFilterType is
         'fltrtypeselIp(1)' then the filter policy with the specified ID must
         exist in tIPFilterTable and must have scope 'system(4)' configured as
         the value of the object tIPFilterScope.

         If the value of the object tFilterSystemFilterType is
         'fltrtypeselIpv6(4)' then the filter policy with the specified ID must
         exist in tIPv6FilterTable and must have scope 'system(4)' configured
         as the value of the object tIPv6FilterScope."
    ::= { tFilterSystemFilterEntry 2 }

tFilterSystemFilterLastChanged   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterSystemFilterLastChanged indicates the
         timestamp of the last change of this row in tFilterSystemFilterTable."
    ::= { tFilterSystemFilterEntry 3 }

tFilterSystemFilterRowStatus     OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterSystemFilterRowStatus specifies the
         status of the conceptual row in tFilterSystemFilterTable.

         Rows are created and destroyed by SNMP SET operations on this object.

         Only values 'active(1)', 'createAndGo(4)' and 'destroy(6)' are
         supported.

         If a row for the same filter type specified by the value of the object
         tFilterSystemFilterType already exists in the table and a new row with
         a different value of the object tFilterSystemFilterId is being created
         the original row is removed by the system."
    ::= { tFilterSystemFilterEntry 4 }

tDhcp6FilterTblLastChanged       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tDhcp6FilterTblLastChanged indicates the sysUpTime at the
         time of the last modification to tDhcp6FilterTable by adding, deleting
         an entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 70 }

tDhcp6FilterTable                OBJECT-TYPE
    SYNTAX      SEQUENCE OF TDhcp6FilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Contains a list of all DHCP6 filters configured on this system."
    ::= { tFilterObjects 71 }

tDhcp6FilterEntry                OBJECT-TYPE
    SYNTAX      TDhcp6FilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular DHCP6 filter. Entries are
         created/deleted by user. Entries have a presumed StorageType of
         nonVolatile."
    INDEX       { tDhcp6FilterId }
    ::= { tDhcp6FilterTable 1 }

TDhcp6FilterEntry                ::= SEQUENCE
{
    tDhcp6FilterId                   TDHCPFilterID,
    tDhcp6FilterRowStatus            RowStatus,
    tDhcp6FilterLastChanged          TimeStamp,
    tDhcp6FilterDescription          TItemDescription,
    tDhcp6FilterDefAction            TDhcpFilterAction,
    tDhcp6FilterDefActionFlags       BITS
}

tDhcp6FilterId                   OBJECT-TYPE
    SYNTAX      TDHCPFilterID (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Uniquely identifies a DHCP6 filter as configures on this system."
    ::= { tDhcp6FilterEntry 1 }

tDhcp6FilterRowStatus            OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted in the
         tDhcp6FilterTable."
    ::= { tDhcp6FilterEntry 2 }

tDhcp6FilterLastChanged          OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the timestamp of the last change to this row."
    ::= { tDhcp6FilterEntry 3 }

tDhcp6FilterDescription          OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "User-provided description for this filter."
    DEFVAL      { ''H }
    ::= { tDhcp6FilterEntry 4 }

tDhcp6FilterDefAction            OBJECT-TYPE
    SYNTAX      TDhcpFilterAction
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The default action to take for DHCP6 host creation requests that do
         not match any of this filter's entries.

         The value none(1) specifies normal host creation behaviour, the value
         bypass-host-creation(2) specifies to bypass host creation, the value
         drop(3) specifies to drop the DHCP6 message."
    DEFVAL      { none }
    ::= { tDhcp6FilterEntry 5 }

tDhcp6FilterDefActionFlags       OBJECT-TYPE
    SYNTAX      BITS {
        na (0),
        pd (1)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tDhcp6FilterDefActionFlags specifies for which
         types of DHCPv6 IAs the bypass-host-creation action is applied."
    REFERENCE
        "RFC 3315"
    ::= { tDhcp6FilterEntry 6 }

tDhcp6FilterParamsTblLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tDhcp6FilterParamsTblLastChanged indicates the sysUpTime
         at the time of the last modification to tDhcp6FilterParamsTable by
         adding, deleting an entry or change to a writable object in the table.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 72 }

tDhcp6FilterParamsTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF TDhcp6FilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of all DHCP6 filter match entries for all DHCP6 filters"
    ::= { tFilterObjects 73 }

tDhcp6FilterParamsEntry          OBJECT-TYPE
    SYNTAX      TDhcp6FilterParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular DHCP6 filter entry. Every DHCP6 filter
         can have zero or more DHCP6 filter match entries.

         A filter entry with no match criteria set will match every packet, and
         the entry action will be taken.

         Entries are created/deleted by user.

         There is no StorageType object, entries have a presumed StorageType of
         nonVolatile."
    INDEX       {
        tDhcp6FilterId,
        tDhcp6FilterParamsId
    }
    ::= { tDhcp6FilterParamsTable 1 }

TDhcp6FilterParamsEntry          ::= SEQUENCE
{
    tDhcp6FilterParamsId             TDhcpEntryId,
    tDhcp6FilterParamsRowStatus      RowStatus,
    tDhcp6FilterParamsLastChanged    TimeStamp,
    tDhcp6FilterParamsOptionNumber   Integer32,
    tDhcp6FilterParamsOptionMatch    TDhcpFilterMatch,
    tDhcp6FilterParamsAction         TDhcpFilterAction,
    tDhcp6FilterParamsOptionValue    OCTET STRING,
    tDhcp6FilterParamsActionFlags    BITS
}

tDhcp6FilterParamsId             OBJECT-TYPE
    SYNTAX      TDhcpEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This is the secondary index for the entry. Every DHCP6 filter can have
         multiple entries, therefore every DHCP6 filter entry is identified by
         the tDhcp6FilterId and tDhcp6FilterParamsId."
    ::= { tDhcp6FilterParamsEntry 1 }

tDhcp6FilterParamsRowStatus      OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted in the
         tDhcp6FilterParamsTable."
    ::= { tDhcp6FilterParamsEntry 2 }

tDhcp6FilterParamsLastChanged    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the timestamp of the last change to this row."
    ::= { tDhcp6FilterParamsEntry 3 }

tDhcp6FilterParamsOptionNumber   OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tDhcp6FilterParamsOptionNumber specifies the number of
         the DHCP6 option to filter on."
    REFERENCE
        "RFC 2132, RFC 3315, RFC 3633"
    DEFVAL      { -1 }
    ::= { tDhcp6FilterParamsEntry 4 }

tDhcp6FilterParamsOptionMatch    OBJECT-TYPE
    SYNTAX      TDhcpFilterMatch
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tDhcp6FilterParamsOptionMatch specifies the criteria that
         the DHCP6 option must match to trigger this filter entry.

         The value present(1) specifies that the DHCP6 option must be present,
         the value absent(2) specifies that the DHCP6 option must be absent. In
         these cases tDhcp6FilterParamsOptionValue will be reset to an empty
         string.

         A value string(3), string-exact(4), string-invert(5),
         string-exact-invert(6), hex(7), hex-exact(8), hex-invert(9) or
         hex-exact-invert(10) requires an octet string to be present in
         tDhcp6FilterParamsOptionValue to match against."
    DEFVAL      { present }
    ::= { tDhcp6FilterParamsEntry 5 }

tDhcp6FilterParamsAction         OBJECT-TYPE
    SYNTAX      TDhcpFilterAction
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The action to take for DHCP6 host creation requests that match this
         filter entry.

         The value none(1) specifies normal host creation behaviour, the value
         bypass-host-creation(2) specifies to bypass host creation, the value
         drop(3) specifies to drop the DHCP6 message."
    DEFVAL      { none }
    ::= { tDhcp6FilterParamsEntry 6 }

tDhcp6FilterParamsOptionValue    OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..127))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tDhcp6FilterParamsOptionValue specifies the
         matching pattern for the filtered DHCP6 option.

         This object is mandatory at creation time. A zero length value is only
         allowed when the value of tDhcp6FilterParamsOptionMatch is present(1)
         or absent(2)."
    ::= { tDhcp6FilterParamsEntry 7 }

tDhcp6FilterParamsActionFlags    OBJECT-TYPE
    SYNTAX      BITS {
        na (0),
        pd (1)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tDhcp6FilterParamsActionFlags specifies for
         which types of DHCPv6 IAs the bypass-host-creation action is applied."
    REFERENCE
        "RFC 3315"
    ::= { tDhcp6FilterParamsEntry 8 }

tFilterEmbedFlowspecTableLstChg  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecTableLstChg indicates the
         sysUpTime at the time of the last modification of
         tFilterEmbedFlowspecTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 74 }

tFilterEmbedFlowspecTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterEmbedFlowspecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterEmbedFlowspecTable contains an entry for each set of
         flowspec rules embedded in an IP or IPv6 filter with scope other than
         'embedded'."
    ::= { tFilterObjects 75 }

tFilterEmbedFlowspecEntry        OBJECT-TYPE
    SYNTAX      TFilterEmbedFlowspecEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the table tFilterEmbedFlowspecTable.

         Entries in this table can be created and deleted via SNMP SET
         operations to tFilterEmbedFlowspecRowStatus.

         Moreover entries are automatically created and deleted by the system
         when a set of flowspec rules is embedded into a filter managed by a
         VSD controller."
    INDEX       {
        tFilterEmbedFlowspecFilterType,
        tFilterEmbedFlowspecInsertFltrId,
        tFilterEmbedFlowspecOffset
    }
    ::= { tFilterEmbedFlowspecTable 1 }

TFilterEmbedFlowspecEntry        ::= SEQUENCE
{
    tFilterEmbedFlowspecFilterType   TFilterType,
    tFilterEmbedFlowspecInsertFltrId TConfigOrVsdFilterID,
    tFilterEmbedFlowspecOffset       TFilterEmbedOffset,
    tFilterEmbedFlowspecRowStatus    RowStatus,
    tFilterEmbedFlowspecLastChanged  TimeStamp,
    tFilterEmbedFlowspecRtrId        TmnxVRtrID,
    tFilterEmbedFlowspecAdminState   TmnxEmbeddedFltrAdminState,
    tFilterEmbedFlowspecOperState    TmnxEmbeddedFltrOperState,
    tFilterEmbedFlowspecGroupId      TFilterFlowspecGroupId
}

tFilterEmbedFlowspecFilterType   OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecFilterType specifies the
         type of filter, either IPv4 or IPv6, for the filter specified by
         tFilterEmbedFlowspecInsertFltrId."
    ::= { tFilterEmbedFlowspecEntry 1 }

tFilterEmbedFlowspecInsertFltrId OBJECT-TYPE
    SYNTAX      TConfigOrVsdFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecInsertFltrId specifies the
         filter where the set of flowspec rules configured for the virtual
         router specified by tFilterEmbedFlowspecRtrId is to be embedded.

         Values outside of range 1..65535 are reserved for entries dynamically
         created by the system and cannot be used in any SNMP SET operation."
    ::= { tFilterEmbedFlowspecEntry 2 }

tFilterEmbedFlowspecOffset       OBJECT-TYPE
    SYNTAX      TFilterEmbedOffset
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecOffset specifies the
         offset of inserted flowspec entries."
    ::= { tFilterEmbedFlowspecEntry 3 }

tFilterEmbedFlowspecRowStatus    OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecRowStatus specifies the
         status of a row in tFilterEmbedFlowspecTable. Rows are created and
         destroyed by SNMP SET operations on this object.

         Only values 'active (1)', 'createAndGo(4)', and 'destroy (6)' are
         supported."
    ::= { tFilterEmbedFlowspecEntry 4 }

tFilterEmbedFlowspecLastChanged  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedFlowspecLastChanged indicates the sysUpTime
         at the time of last change to this row in tFilterEmbedFlowspecEntry."
    ::= { tFilterEmbedFlowspecEntry 5 }

tFilterEmbedFlowspecRtrId        OBJECT-TYPE
    SYNTAX      TmnxVRtrID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecRtrId specifies a virtual
         router for which a set of flowspec rules have been configured by an
         external system. Such flowspec rules will be embedded into the
         embedding filter specified by tFilterEmbedFlowspecFilterType and
         tFilterEmbedFlowspecInsertFltrId.

         At the time of creation of a row via SNMP you can either specify or
         not specify a value for tFilterEmbedFlowspecRtrId.

         If you do not specify the value of tFilterEmbedFlowspecRtrId then the
         system will try to obtain it. This corresponds to the situation when
         the embedding filter has already been assigned to any endpoint.

         If you do not specify the value of tFilterEmbedFlowspecRtrId and the
         embedding filter has not been assigned to any endpoint yet then the
         creation of the row will fail.

         If you specify the value of tFilterEmbedFlowspecRtrId then the system
         will check if the embedding filter has already been assigned to any
         endpoint. If this is not the case it will not be possible to assign
         the embedding filter outside the scope of the virtual router specified
         by tFilterEmbedFlowspecRtrId. If this is the case then the creation of
         the row may be successful only if the value of the virtual router
         specified by tFilterEmbedFlowspecRtrId matches with the value already
         stored in the system.

         In any case the value of tFilterEmbedFlowspecRtrId cannot be changed
         after creation of the row."
    ::= { tFilterEmbedFlowspecEntry 6 }

tFilterEmbedFlowspecAdminState   OBJECT-TYPE
    SYNTAX      TmnxEmbeddedFltrAdminState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecAdminState specifies the
         administrative state of the embed request defined by this row.

         If an active embedding cannot be fulfilled due to dynamic events, this
         object will be set to 'inactive' automatically by the system. In those
         cases, the value of the object tFilterEmbedFlowspecOperState will
         indicate the failure reason."
    DEFVAL      { active }
    ::= { tFilterEmbedFlowspecEntry 7 }

tFilterEmbedFlowspecOperState    OBJECT-TYPE
    SYNTAX      TmnxEmbeddedFltrOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedFlowspecOperState indicates the operational
         state of the embed request defined by this row."
    ::= { tFilterEmbedFlowspecEntry 8 }

tFilterEmbedFlowspecGroupId      OBJECT-TYPE
    SYNTAX      TFilterFlowspecGroupId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecGroupId specifies the
         group id that is used to select subset of flowspec rules and embed
         only those rules. Value of 65535 means insert all rules irregardless
         of their group id"
    DEFVAL      { 65535 }
    ::= { tFilterEmbedFlowspecEntry 9 }

tFltrEmbFlowspecInfoTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrEmbFlowspecInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrEmbFlowspecInfoTable contains an entry for each
         auto-created embedded filter for flowspec rules inserted in an IP or
         IPv6 filter with scope other than 'embedded'.

         This row complements the corresponding row in the
         tFilterEmbedFlowspecTable with read-only operational info."
    ::= { tFilterObjects 76 }

tFltrEmbFlowspecInfoEntry        OBJECT-TYPE
    SYNTAX      TFltrEmbFlowspecInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFltrEmbFlowspecInfoTable."
    AUGMENTS    { tFilterEmbedFlowspecEntry }
    ::= { tFltrEmbFlowspecInfoTable 1 }

TFltrEmbFlowspecInfoEntry        ::= SEQUENCE
{
    tFltrEmbFlowSpecInfoFltrId       TAnyFilterID,
    tFltrEmbFlowSpecInfoEntryCnt     Unsigned32,
    tFltrEmbFlowSpecInfoEntryCntIns  Unsigned32
}

tFltrEmbFlowSpecInfoFltrId       OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEmbFlowSpecInfoFltrId indicates the ID of
         the auto-created embedded filter for flowspec rules related to the
         virtual router specified by tFilterEmbedFlowspecRtrId."
    ::= { tFltrEmbFlowspecInfoEntry 1 }

tFltrEmbFlowSpecInfoEntryCnt     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEmbFlowSpecInfoEntryCnt indicates how
         many entries are present in the embedded filter specified by
         tFltrEmbFlowSpecInfoFltrId."
    ::= { tFltrEmbFlowspecInfoEntry 2 }

tFltrEmbFlowSpecInfoEntryCntIns  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEmbFlowSpecInfoEntryCntIns indicates how
         many entries of the embedded filter (specified by
         tFltrEmbFlowSpecInfoFltrId) are actually inserted into the embedding
         filter (specified by tFilterEmbedFlowspecInsertFltrId).

         If the object tFilterEmbedFlowspecOperState is different from 'active'
         this object will always be zero.

         Otherwise the difference between tFltrEmbFlowSpecInfoEntryCnt and the
         value of this object indicates how many entries of the embedded filter
         were overwritten by local entries in the embedding filter."
    ::= { tFltrEmbFlowspecInfoEntry 3 }

tFltrEmbFlowspecEntryInfoTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrEmbFlowspecEntryInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
        "The table tFltrEmbFlowspecEntryInfoTable contains an entry for each
         entry of an auto-created embedded filter for flowspec rules inserted
         in an IP or IPv6 filter with scope other than 'embedded'. This table
         shows only basic flowspec embeddings (no support for groups, no
         support for filters with scope system and their flowspec embeddings).

         Will be obsoleted in the next release. Please use
         tFilterEmbFlowspecEntryInfoTable instead."
    ::= { tFilterObjects 77 }

tFltrEmbFlowspecEntryInfoEntry   OBJECT-TYPE
    SYNTAX      TFltrEmbFlowspecEntryInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFltrEmbFlowspecEntryInfoTable. Rows in the
         tFltrEmbFlowspecEntryInfoTable are created by the SYSTEM when an
         auto-created embedded filter for flowspec rules is inserted into an IP
         or IPv6 filter with scope other than 'embedded'. They are destroyed by
         the SYSTEM when such auto-created embedded filter is removed from an
         IP or IPv6 filter with scope other than 'embedded'."
    INDEX       {
        tFilterEmbedFlowspecFilterType,
        tFilterEmbedFlowspecInsertFltrId,
        tFltrEmbFlowspecEntryId
    }
    ::= { tFltrEmbFlowspecEntryInfoTable 1 }

TFltrEmbFlowspecEntryInfoEntry   ::= SEQUENCE
{
    tFltrEmbFlowspecEntryId          TEntryId,
    tFltrEmbFlowspecEntryInsEntryId  TAnyEntryId,
    tFltrEmbFlowspecEntryOperState   TmnxFltrEmbeddedEntryState
}

tFltrEmbFlowspecEntryId          OBJECT-TYPE
    SYNTAX      TEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEmbFlowspecEntryId specifies the ID of
         the entry inside of the auto-created embedded filter for flowspec
         rules specified by tFltrEmbFlowSpecInfoFltrId."
    ::= { tFltrEmbFlowspecEntryInfoEntry 1 }

tFltrEmbFlowspecEntryInsEntryId  OBJECT-TYPE
    SYNTAX      TAnyEntryId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEmbFlowspecEntryInsEntryId indicates
         which entry in the IP or IPv6 filter with scope other than 'embedded'
         specified by tFilterEmbedFlowspecInsertFltrId corresponds to the entry
         specified by tFltrEmbFlowspecEntryId in the auto-created embedded
         filter for flowspec rules specified by tFltrEmbFlowSpecInfoFltrId."
    ::= { tFltrEmbFlowspecEntryInfoEntry 2 }

tFltrEmbFlowspecEntryOperState   OBJECT-TYPE
    SYNTAX      TmnxFltrEmbeddedEntryState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEmbFlowspecEntryOperState indicates the
         current operational state of the entry identified by
         tFltrEmbFlowspecEntryId of the embedded filter identified by
         tFltrEmbFlowSpecInfoFltrId that is embedded into the filter identified
         by tFilterEmbedFlowspecInsertFltrId."
    ::= { tFltrEmbFlowspecEntryInfoEntry 3 }

tMacFltrEntryActionTblLChg       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActionTblLChg indicates the
         sysUpTime at the time of the last modification of
         tMacFltrEntryActionTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 82 }

tMacFltrEntryActionTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TMacFltrEntryActionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tMacFltrEntryActionTable contains information pertaining to
         MAC filter actions to be taken for packets that match the filter entry
         identified by tMacFilterId and tMacFilterParamsIndex. The table
         tMacFltrEntryActionTable supports configuration of redundant filter
         entry actions."
    ::= { tFilterObjects 83 }

tMacFltrEntryActionEntry         OBJECT-TYPE
    SYNTAX      TMacFltrEntryActionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The entry contains information pertaining to an action for a
         particular MAC filter entry (object corresponding to MAC filter entry
         is tMacFilterParamsEntry). Per one filter entry up to two actions can
         be configured (primary and secondary).

         Entries with the value of tMacFltrEntryActActionId equal to 'primary'
         are created and destroyed by SNMP SET operations on the object
         tMacFilterParamsRowStatus. Entries with the value of
         tMacFltrEntryActActionId equal to 'secondary' are created by SNMP SET
         operation on the object tMacFltrEntryActRowStatus and destroyed by
         SNMP SET operation on the objects tMacFltrEntryActRowStatus or
         tMacFilterParamsRowStatus."
    INDEX       {
        tMacFilterId,
        tMacFilterParamsIndex,
        tMacFltrEntryActActionId
    }
    ::= { tMacFltrEntryActionTable 1 }

TMacFltrEntryActionEntry         ::= SEQUENCE
{
    tMacFltrEntryActActionId         TFilterEntryActionId,
    tMacFltrEntryActLastChanged      TimeStamp,
    tMacFltrEntryActRowStatus        RowStatus,
    tMacFltrEntryActAction           TMacFilterEntryAction,
    tMacFltrEntryActFwdSapPortId     TmnxPortID,
    tMacFltrEntryActFwdSapEncapVal   TmnxEncapVal,
    tMacFltrEntryActFwdSdpBind       SdpBindId,
    tMacFltrEntryActRedirectURL      TmnxHttpRedirectUrl,
    tMacFltrEntryActEsi              TFilterEsi,
    tMacFltrEntryActFwdEsiSvcId      TmnxServId,
    tMacFltrEntryActRateLimit        TFilterEntryActionRateLimit,
    tMacFltrEntryActPbrTargetStatus  TFilterPbrTargetStatus,
    tMacFltrEntryActFcName           TFCTypeOrNone
}

tMacFltrEntryActActionId         OBJECT-TYPE
    SYNTAX      TFilterEntryActionId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActActionId specifies a unique
         identifier of an action within the filter entry. Per one filter entry
         up to two actions can be configured (the primary and the secondary).
         PBF destination availability checking for an entry is turned on when
         both actions (the primary and the secondary) are configured for an
         entry. This is allowed only for the following combinations of actions:
            - both actions are PBF to SAP
            - both actions are PBF to SDP
            - the primary action is PBF to SAP and the secondary action is
              PBF to SDP or vice versa

         If the PBF destination of the primary action is available, then the
         primary action will be taken on a packet matching the filter entry. If
         the PBF destination of the primary action is not available and the PBF
         destination of the secondary action is available then the secondary
         action will be taken on a packet matching the filter entry. If none of
         the actions for the entry has an available PBF destination then the
         action specified by the object tMacFilterParamsPbrDwnActOvr will be
         taken on a packet matching the filter entry.

         There is a limit to the number of filter entries with the destination
         availability checking turned on."
    ::= { tMacFltrEntryActionEntry 1 }

tMacFltrEntryActLastChanged      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActLastChanged indicates the
         sysUpTime at the time of the last modification of
         tMacFltrEntryActionEntry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tMacFltrEntryActionEntry 2 }

tMacFltrEntryActRowStatus        OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActRowStatus specifies the status
         of the conceptual row in tMacFltrEntryActionTable.

         Rows with value of tMacFltrEntryActActionId equal to 'primary' are
         created and destroyed by SNMP SET operations on the object
         tMacFilterParamsRowStatus. Rows with value of tMacFltrEntryActActionId
         equal to 'secondary' are created by SNMP SET operation on the object
         tMacFltrEntryActRowStatus and destroyed by SNMP SET operation on the
         objects tMacFltrEntryActRowStatus or tMacFilterParamsRowStatus."
    ::= { tMacFltrEntryActionEntry 3 }

tMacFltrEntryActAction           OBJECT-TYPE
    SYNTAX      TMacFilterEntryAction
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActAction specifies the action to
         be taken on a packet matching the filter entry.

         Refer to the description of the textual convention
         TMacFilterEntryAction for more information."
    DEFVAL      { ignoreMatch }
    ::= { tMacFltrEntryActionEntry 4 }

tMacFltrEntryActFwdSapPortId     OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActFwdSapPortId specifies the sap
         port identity of the destination for this MAC filter entry. A value of
         0 indicates that there is currently no SAP destination specified. A
         value different from 0 can only be specified if the value of
         tMacFltrEntryActAction is 'forwardSap' and the value of
         tMacFltrEntryActFwdSdpBind has a zero value.

         Note that the value of tMacFltrEntryActFwdSapPortId is silently
         cleared by the system if tMacFltrEntryActAction is set to value other
         than 'forwardSap'."
    DEFVAL      { 0 }
    ::= { tMacFltrEntryActionEntry 5 }

tMacFltrEntryActFwdSapEncapVal   OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActFwdSapEncapVal specifies the
         sap port encap value of the destination SAP for this MAC filter entry.
         A value different from 0 can only be specified when the
         tMacFltrEntryActFwdSapPortId object has a non zero value, and the
         value of the tMacFltrEntryActAction object of this entry is
         'forwardSap'.
         A value of 0 indicates that either
         1) the sap encapsulation value is not specified when
            tMacFltrEntryActFwdSapPortId and tMacFilterParamsFwdSvcId
            have valid values; or
         2) that there is no SAP destination.

         Note that the value of tMacFltrEntryActFwdSapEncapVal is silently
         cleared by the system if tMacFltrEntryActAction is set to value other
         than 'forwardSap'."
    DEFVAL      { 0 }
    ::= { tMacFltrEntryActionEntry 6 }

tMacFltrEntryActFwdSdpBind       OBJECT-TYPE
    SYNTAX      SdpBindId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActFwdSdpBind specifies the sdp
         bind identity of the destination for this MAC filter entry. A value of
         0 indicates that there is currently no SDP binding defined. A value
         different from 0 can only be specified if the value of
         tMacFltrEntryActAction is 'forwardSdp' and
         tMacFltrEntryActFwdSapPortId and tMacFltrEntryActFwdSapEncapVal have a
         zero value.

         Note that the value of tMacFltrEntryActFwdSdpBind is silently cleared
         by the system if tMacFltrEntryActAction is set to value other than
         'forwardSdp'."
    DEFVAL      { '0000000000000000'H }
    ::= { tMacFltrEntryActionEntry 7 }

tMacFltrEntryActRedirectURL      OBJECT-TYPE
    SYNTAX      TmnxHttpRedirectUrl
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActRedirectURL specifies the URL
         to redirect to, when the value of tMacFltrEntryActAction is
         'httpRedirect'.

         Note that the value of tMacFltrEntryActRedirectURL is silently cleared
         by the system if tMacFltrEntryActAction is set to value other than
         'httpRedirect'."
    DEFVAL      { ''H }
    ::= { tMacFltrEntryActionEntry 8 }

tMacFltrEntryActEsi              OBJECT-TYPE
    SYNTAX      TFilterEsi
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActEsi specifies the ethernet
         segment identifier (ESI) of the first ESI identified appliance in
         Nuage service chain. When the value of tMacFilterParamsAction is
         'forwardEsiL2' packets matching the filter entry are forwarded to the
         appliance using EVPN-resolved VXLAN tunnel in the specified VPLS
         service (tMacFltrEntryActFwdEsiSvcId).

         The value '0' indicates that there is no ESI specified.

         The non zero value of tMacFltrEntryActEsi must be set together with a
         non zero value of tMacFltrEntryActFwdEsiSvcId and value of
         tMacFltrEntryActAction set to 'forwardEsiL2'.

         Note that the value of tMacFltrEntryActEsi is silently cleared by the
         system if the value of tMacFltrEntryActAction is set to any value
         other than 'forwardEsiL2'."
    DEFVAL      { '00000000000000000000'H }
    ::= { tMacFltrEntryActionEntry 9 }

tMacFltrEntryActFwdEsiSvcId      OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActFwdEsiSvcId specifies the
         identifier of the VPLS used for VPN/DC connectivity.

         The value '0' indicates that no VPLS identifier is specified.

         The non zero value of tMacFltrEntryActFwdEsiSvcId must be set together
         with a non zero value of tMacFltrEntryActEsi and value of
         tMacFltrEntryActAction set to 'forwardEsiL2'.

         Note that the value of tMacFltrEntryActFwdEsiSvcId is silently cleared
         by the system if the value of tMacFltrEntryActAction is set to any
         value other than 'forwardEsiL2'."
    DEFVAL      { 0 }
    ::= { tMacFltrEntryActionEntry 10 }

tMacFltrEntryActRateLimit        OBJECT-TYPE
    SYNTAX      TFilterEntryActionRateLimit
    UNITS       "kilobps"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActRateLimit specifies the rate
         to which the traffic matching the filter entry will be limited.

         The value of tMacFltrEntryActRateLimit can be set to non default value
         only if the value of tMacFltrEntryActAction is set to 'rateLimit'.

         Note that the value of tMacFltrEntryActRateLimit is silently cleared
         by the system if the value of tMacFltrEntryActAction is set to any
         value other than 'rateLimit'."
    DEFVAL      { 0 }
    ::= { tMacFltrEntryActionEntry 11 }

tMacFltrEntryActPbrTargetStatus  OBJECT-TYPE
    SYNTAX      TFilterPbrTargetStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActPbrTargetStatus indicates the
         PBR target status.

         Refer to the description of the textual convention
         TFilterPbrTargetStatus for more information."
    ::= { tMacFltrEntryActionEntry 12 }

tMacFltrEntryActFcName           OBJECT-TYPE
    SYNTAX      TFCTypeOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tMacFltrEntryActFcName specifies the
         forwarding class name."
    DEFVAL      { none }
    ::= { tMacFltrEntryActionEntry 13 }

tIPvXFltrEntryActionTblLChg      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActionTblLChg indicates the
         sysUpTime at the time of the last modification of
         tIPvXFltrEntryActionTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 84 }

tIPvXFltrEntryActionTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIPvXFltrEntryActionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tIPvXFltrEntryActionTable contains information pertaining to
         IPv4 and IPv6 filter actions to be taken for packets that match the
         filter entry identified by tIPvXFltrEntryActFltrType
         tIPvXFltrEntryActFltrId and tIPvXFltrEntryActEntryId. The table
         tIPvXFltrEntryActionTable supports configuration of redundant filter
         entry actions."
    ::= { tFilterObjects 85 }

tIPvXFltrEntryActionEntry        OBJECT-TYPE
    SYNTAX      TIPvXFltrEntryActionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The entry contains information pertaining to an action for a
         particular IPv4 or IPv6 filter entry (information pertaining to IPv4
         filter entry is in tIPFilterParamsTable and tIPFilterParamsExtTable
         and information pertaining to IPv6 filter entry is in
         tIPv6FilterParamsTable and tIPv6FilterParamsExtTable). Per one filter
         entry up to two actions can be configured (primary and secondary).

         Entries with the value of tIPvXFltrEntryActActionId equal to 'primary'
         are created and destroyed by SNMP SET operations on the object
         tIPFilterParamsRowStatus or tIPv6FilterParamsRowStatus. Entries with
         the value of tIPvXFltrEntryActActionId equal to 'secondary' are
         created by SNMP SET operation on the object tIPvXFltrEntryActRowStatus
         and destroyed by SNMP SET operation on the object
         tIPvXFltrEntryActRowStatus, tIPFilterParamsRowStatus or
         tIPv6FilterParamsRowStatus."
    INDEX       {
        tIPvXFltrEntryActFltrType,
        tIPvXFltrEntryActFltrId,
        tIPvXFltrEntryActEntryId,
        tIPvXFltrEntryActActionId
    }
    ::= { tIPvXFltrEntryActionTable 1 }

TIPvXFltrEntryActionEntry        ::= SEQUENCE
{
    tIPvXFltrEntryActFltrType        TFilterType,
    tIPvXFltrEntryActFltrId          TAnyFilterID,
    tIPvXFltrEntryActEntryId         TEntryId,
    tIPvXFltrEntryActActionId        TFilterEntryActionId,
    tIPvXFltrEntryActLastChanged     TimeStamp,
    tIPvXFltrEntryActRowStatus       RowStatus,
    tIPvXFltrEntryActAction          TIPvXFilterEntryAction,
    tIPvXFltrEntryActFwdNHIpAddrType InetAddressType,
    tIPvXFltrEntryActFwdNHIpAddr     InetAddress,
    tIPvXFltrEntryActFwdNHIndirect   TruthValue,
    tIPvXFltrEntryActFwdNHInterface  TNamedItemOrEmpty,
    tIPvXFltrEntryActFwdRedPlcy      TNamedItemOrEmpty,
    tIPvXFltrEntryActFwdSapPortId    TmnxPortID,
    tIPvXFltrEntryActFwdSapEncapVal  TmnxEncapVal,
    tIPvXFltrEntryActFwdSdpBind      SdpBindId,
    tIPvXFltrEntryActRedirectURL     TmnxHttpRedirectUrl,
    tIPvXFltrEntryActRdirAllwRadOvr  TruthValue,
    tIPvXFltrEntryActFwdRtrId        TmnxVRtrIDOrZero,
    tIPvXFltrEntryActNatPolicyName   TNamedItemOrEmpty,
    tIPvXFltrEntryActNatType         TmnxNatSubscriberTypeOrNone,
    tIPvXFltrEntryActFwdLsp          TmnxVRtrMplsLspID,
    tIPvXFltrEntryActFwdLspRtrId     TmnxVRtrIDOrZero,
    tIPvXFltrEntryActPktLenVal1      TFilterPacketLength,
    tIPvXFltrEntryActPktLenVal2      TFilterPacketLength,
    tIPvXFltrEntryActPktLenOper      TOperator,
    tIPvXFltrEntryActTTLVal1         TFilterTTL,
    tIPvXFltrEntryActTTLVal2         TFilterTTL,
    tIPvXFltrEntryActTTLOper         TOperator,
    tIPvXFltrEntryActEsi             TFilterEsi,
    tIPvXFltrEntryActFwdEsiSvcId     TmnxServId,
    tIPvXFltrEntryActFwdEsiVRtrId    TmnxVRtrIDOrZero,
    tIPvXFltrEntryActFwdEsiSFIpType  InetAddressType,
    tIPvXFltrEntryActFwdEsiSFIp      InetAddress,
    tIPvXFltrEntryActFwdEsiVasIf     InterfaceIndexOrZero,
    tIPvXFltrEntryActRateLimit       TFilterEntryActionRateLimit,
    tIPvXFltrEntryActPbrTargetStatus TFilterPbrTargetStatus,
    tIPvXFltrEntryActRemarkDSCP      TDSCPNameOrEmpty,
    tIPvXFltrEntryActActionExt       TIPvXFilterEntryActionExt,
    tIPvXFltrEntryActFwdVprnTgtBgNHT InetAddressType,
    tIPvXFltrEntryActFwdVprnTgtBgNH  InetAddress,
    tIPvXFltrEntryActFwdVprnTgtRtrId TmnxVRtrIDOrZero,
    tIPvXFltrEntryActFwdVprnTgtAdPxT TmnxAddressAndPrefixType,
    tIPvXFltrEntryActFwdVprnTgtAdPx  TmnxAddressAndPrefixAddress,
    tIPvXFltrEntryActFwdVprnTgtAdPxL TmnxAddressAndPrefixPrefix,
    tIPvXFltrEntryActFwdVprnTgtLspId TmnxVRtrMplsLspID,
    tIPvXFltrEntryActFwdBondingConn  TmnxSubBondingConnIdOrEmpty,
    tIPvXFltrEntryActFcName          TFCTypeOrNone,
    tIPvXFltrEntryActFwdGreTun       TNamedItemOrEmpty,
    tIPvXFltrEntryActCondExpression  OCTET STRING,
    tIPvXFltrEntryActCondExpMask     OCTET STRING,
    tIPvXFltrEntryActCondOffsetType  INTEGER,
    tIPvXFltrEntryActCondOffsetVal   Integer32,
    tIPvXFltrFwdMplsPlcyEndptAddrTp  InetAddressType,
    tIPvXFltrFwdMplsPlcyEndptAddr    InetAddress,
    tIPvXFltrFwdSrtePlcyEndptAddrTp  InetAddressType,
    tIPvXFltrFwdSrtePlcyEndptAddr    InetAddress,
    tIPvXFltrFwdSrtePlcyColor        Unsigned32,
    tIPvXFltrActL2AwareNatBypass     TruthValue,
    tIPvXFltrEntryActRateLimitPps    TFilterEntryActionRateLimitPps,
    tIPvXFltrFwdSrv6PlcyEndptAddrTp  InetAddressType,
    tIPvXFltrFwdSrv6PlcyEndptAddr    InetAddress,
    tIPvXFltrFwdSrv6PlcyColor        Unsigned32,
    tIPvXFltrFwdSrv6PlcySvcSidAddrTp InetAddressType,
    tIPvXFltrFwdSrv6PlcySvcSid       InetAddress,
    tIPvXFltrEntryActRateLimitMbs    Integer32,
    tIPvXFltrEntryActRateLimitPlcr   TNamedItemOrEmpty
}

tIPvXFltrEntryActFltrType        OBJECT-TYPE
    SYNTAX      TFilterType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFltrType specifies the type
         of the filter to which this action belongs.

         Only values 'fltrtypeselIp' and 'fltrtypeselIpv6' are supported.

         Refer to the description of the textual convention TFilterType for
         more information."
    ::= { tIPvXFltrEntryActionEntry 1 }

tIPvXFltrEntryActFltrId          OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFltrId specifies the filter
         id of the filter to which this action belongs. The filter must exist
         in tIPFilterTable, if the value of tIPvXFltrEntryActFltrType is 'ipv4'
         or it must exist in tIPv6FilterTable if the value of
         tIPvXFltrEntryActFltrType is 'ipv6'.

         Refer to the description of the textual convention TAnyFilterID for
         more information."
    ::= { tIPvXFltrEntryActionEntry 2 }

tIPvXFltrEntryActEntryId         OBJECT-TYPE
    SYNTAX      TEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActEntryId specifies the entry
         id of the entry to which this filter action belongs. The filter entry
         must exist in tIPFilterParamsTable, if the value of
         tIPvXFltrEntryActFltrType is 'ipv4' or it must exist in
         tIPv6FilterParamsTable if the value of tIPvXFltrEntryActFltrType is
         'ipv6'."
    ::= { tIPvXFltrEntryActionEntry 3 }

tIPvXFltrEntryActActionId        OBJECT-TYPE
    SYNTAX      TFilterEntryActionId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActActionId specifies a unique
         identifier of an action within the filter entry. Per one filter entry
         up to two actions can be configured (the primary and the secondary).
         Destination availability checking is turned on when both actions (the
         primary and the secondary) are configured for an entry. This is allowed
         only for the following combinations of actions:
            - both actions are PBF to SAP
            - both actions are PBF to SDP
            - the primary action is PBF to SAP and the secondary action is
              forward SDP or vice versa
            - both actions are PBR to next-hop router

         If the PBR/PBF destination of the primary action is available, then
         the primary action will be taken on a packet matching the filter
         entry. If the PBR/PBF destination of the primary action is not
         available and the PBR/PBF destination of the secondary action is
         available then the secondary action will be taken on a packet matching
         the filter entry. If none of the actions for the entry has an
         available PBR/PBF destination then the action specified by the object
         tIPFilterParamsExtPbrDwnActOvr(for IPv4 filters) or
         tIPv6FilterParamsExtPbrDwnActOvr(for IPv6 filters) will be taken on a
         packet matching the filter entry.

         There is a limit to the number of entries with the destination
         availability checking turned on."
    ::= { tIPvXFltrEntryActionEntry 4 }

tIPvXFltrEntryActLastChanged     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActLastChanged indicates the
         sysUpTime at the time of the last modification of
         tIPvXFltrEntryActionEntry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tIPvXFltrEntryActionEntry 5 }

tIPvXFltrEntryActRowStatus       OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActRowStatus specifies the
         status of the conceptual row in tIPvXFltrEntryActionTable.

         Rows with the value of tIPvXFltrEntryActActionId equal to 'primary'
         are created and destroyed by SNMP SET operations on the object
         tIPFilterParamsRowStatus or tIPv6FilterParamsRowStatus. Rows with the
         value of tIPvXFltrEntryActActionId equal to 'secondary' are created by
         SNMP SET operation on the object tIPvXFltrEntryActRowStatus and
         destroyed by SNMP SET operation on the object
         tIPvXFltrEntryActRowStatus, tIPFilterParamsRowStatus or
         tIPv6FilterParamsRowStatus."
    ::= { tIPvXFltrEntryActionEntry 6 }

tIPvXFltrEntryActAction          OBJECT-TYPE
    SYNTAX      TIPvXFilterEntryAction
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActAction specifies the action
         to be taken on a packet matching the filter entry.

         Refer to the description of the textual convention
         TIPvXFilterEntryAction for more information."
    DEFVAL      { ignoreMatch }
    ::= { tIPvXFltrEntryActionEntry 7 }

tIPvXFltrEntryActFwdNHIpAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdNHIpAddrType specifies the
         context in which the value of the object tIPvXFltrEntryActFwdNHIpAddr
         is interpreted.

         Only following values are supported:
            unknown(0)
            ipv4(1)
            ipv6(2)

         The value of tIPvXFltrEntryActFwdNHIpAddrType must be consistent with
         the value of tIPvXFltrEntryActFltrType.

         Note that the value of tIPvXFltrEntryActFwdNHIpAddrType is silently
         cleared by the system if tIPvXFltrEntryActAction is set to value other
         than 'forwardNextHop' or 'forwardNextHopRtr'."
    DEFVAL      { unknown }
    ::= { tIPvXFltrEntryActionEntry 8 }

tIPvXFltrEntryActFwdNHIpAddr     OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdNHIpAddr specifies the
         IP/IPv6 address of the nexthop to which the packet should be forwarded
         if it hits this filter entry. The action of this entry should be
         'forwardNextHop' or 'forwardNextHopRtr' in such a case.

         Note that the value of tIPvXFltrEntryActFwdNHIpAddr is silently
         cleared by the system if tIPvXFltrEntryActAction is set to value other
         than 'forwardNextHop' or 'forwardNextHopRtr'."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPvXFltrEntryActionEntry 9 }

tIPvXFltrEntryActFwdNHIndirect   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdNHIndirect specifies if
         the nexthop is directly or indirectly reachable. The action of this
         entry should be 'forwardNextHop' or 'forwardNextHopRtr' in such a
         case.

         Note that the value of tIPvXFltrEntryActFwdNHIndirect is silently
         cleared by the system if tIPvXFltrEntryActAction is set to value other
         than 'forwardNextHop' or 'forwardNextHopRtr'."
    DEFVAL      { false }
    ::= { tIPvXFltrEntryActionEntry 10 }

tIPvXFltrEntryActFwdNHInterface  OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdNHInterface specifies the
         interface name for the nexthop to which the packet should be forwarded
         if it hits this filter entry. The action of this entry should be
         'forwardNHInterface' in such a case.

         Note that the value of tIPvXFltrEntryActFwdNHInterface  is silently
         cleared by the system if tIPvXFltrEntryActAction is set to value
         other than 'forwardNHInterface'."
    DEFVAL      { ''H }
    ::= { tIPvXFltrEntryActionEntry 11 }

tIPvXFltrEntryActFwdRedPlcy      OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdRedPlcy specifies the
         redirect policy to be used to determine the nexthop. The action of
         this entry should be 'forwardRPlcy' in such a case.

         Note that the value of tIPvXFltrEntryActFwdRedPlcy is silently cleared
         by the system if tIPvXFltrEntryActAction is set to value other than
         'forwardRPlcy'."
    DEFVAL      { ''H }
    ::= { tIPvXFltrEntryActionEntry 12 }

tIPvXFltrEntryActFwdSapPortId    OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdSapPortId specifies the
         sap port id of the destination for this filter entry.

         The value 0 indicates that there is no SAP destination defined. A value
         different from 0 can only be specified if the value of the
         tIPvXFltrEntryActAction object of this entry is 'forwardSap'.  In
         addition a non-zero value can only be given if the object
         tIPvXFltrEntryActFwdSdpBind is '0'.

         Note that the value of tIPvXFltrEntryActFwdSapPortId is silently
         cleared by the system if tIPvXFltrEntryActAction is set to value other
         than 'forwardSap'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 13 }

tIPvXFltrEntryActFwdSapEncapVal  OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdSapEncapVal specifies the
         sap port encap value of the destination SAP for this filter entry.

         A value different from 0 can only be specified if the value of the
         tIPvXFltrEntryActAction object of this entry is 'forwardSap'. In
         addition a non-zero value can only be given if the object
         tIPvXFltrEntryActFwdSdpBind has value '0'.
         The value 0 indicates that either
         1) the sap encapsulation value is not specified when
            tIPvXFltrEntryActFwdSapPortId and based on the filter type
            tIPFilterParamsFwdSvcId or tIPv6FilterParamsFwdSvcId have valid
            values; or
         2) that there is no SAP destination.

         Note that the value of tIPvXFltrEntryActFwdSapEncapVal is silently
         cleared by the system if tIPvXFltrEntryActAction is set to value other
         than 'forwardSap'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 14 }

tIPvXFltrEntryActFwdSdpBind      OBJECT-TYPE
    SYNTAX      SdpBindId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdSdpBind specifies the sdp
         bind id of the destination for this filter entry.

         The value '0' indicates that there is currently no SDP binding
         defined. A value different from '0' can only be specified if the value
         of the tIPvXFltrEntryActAction object of this entry is 'forwardSdp'.
         In addition a non-zero value can only be given if the objects
         tIPvXFltrEntryActFwdSapPortId and tIPvXFltrEntryActFwdSapEncapVal have
         value 0.

         Note that the value of tIPvXFltrEntryActFwdSdpBind is silently cleared
         by the system if tIPvXFltrEntryActAction is set to value other than
         'forwardSdp', or any object related to 'forward' other than this one
         is set."
    DEFVAL      { '0000000000000000'H }
    ::= { tIPvXFltrEntryActionEntry 15 }

tIPvXFltrEntryActRedirectURL     OBJECT-TYPE
    SYNTAX      TmnxHttpRedirectUrl
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActRedirectURL specifies the URL
         to redirect to, when the value of tIPvXFltrEntryActAction is
         'httpRedirect'.

         The following macro substitutions are applicable in this context:
         $URL, $MAC, $IP, $SUB, $SAP, $SAPDESC, $CID, and $RID.

         Note that the value of tIPvXFltrEntryActRedirectURL is silently
         cleared by the system if tIPvXFltrEntryActAction is set to any value
         other than 'httpRedirect'."
    DEFVAL      { ''H }
    ::= { tIPvXFltrEntryActionEntry 16 }

tIPvXFltrEntryActRdirAllwRadOvr  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActRdirAllwRadOvr specifies
         whether or not the value of tIPvXFltrEntryActRedirectURL can be
         overridden by a Radius VSA. The default value is false (i.e. the URL
         cannot be overridden by Radius).  The value of
         tIPvXFltrEntryActRdirAllwRadOvr is relevant only if the value of
         tIPvXFltrEntryActAction is 'httpRedirect'.

         The value of tIPvXFltrEntryActRdirAllwRadOvr can't be set to true if
         the value of tIPvXFltrEntryActAction is not 'httpRedirect'.
         Furthermore, the value of tIPvXFltrEntryActRdirAllwRadOvr is silently
         reset to false by the system if tIPvXFltrEntryActAction is set to any
         value other than 'httpRedirect'."
    DEFVAL      { false }
    ::= { tIPvXFltrEntryActionEntry 17 }

tIPvXFltrEntryActFwdRtrId        OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdRtrId specifies, if
         different from '0', the routing context in which the packet will be
         forwarded if it hits this filter entry.

         The action of this entry should be 'forwardRtr' or 'forwardNextHopRtr'
         in such a case.

         Note that the value of tIPvXFltrEntryActFwdRtrId is silently cleared
         by the system if tIPvXFltrEntryActAction is set to value other than
         'forwardRtr' or 'forwardNextHopRtr'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 18 }

tIPvXFltrEntryActNatPolicyName   OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActNatPolicyName specifies the
         name of the NAT policy to be used when the value of
         tIPvXFltrEntryActAction is 'nat'. If the value is empty then a default
         policy is used. If the value is non-empty then it must correspond to a
         policy defined in tmnxNatPlcyTable.

         The value of tIPvXFltrEntryActNatPolicyName is relevant only if the
         value of tIPvXFltrEntryActAction is 'nat'. Setting the value of
         tIPvXFltrEntryActNatPolicyName to a non-empty string is allowed only
         if the value of tIPvXFltrEntryActAction is 'nat'.

         Furthermore, the value of tIPvXFltrEntryActNatPolicyName is silently
         reset to an empty string by the system if tIPvXFltrEntryActAction is
         set to any value other than 'nat'."
    DEFVAL      { "" }
    ::= { tIPvXFltrEntryActionEntry 19 }

tIPvXFltrEntryActNatType         OBJECT-TYPE
    SYNTAX      TmnxNatSubscriberTypeOrNone { none (0), dsliteLsnSub (3), nat64LsnSub (4) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActNatType specifies the NAT
         type to be used when the value of tIPvXFltrEntryActAction is 'nat'.

         The object tIPvXFltrEntryActNatType is applicable only for IPv6
         filters. The only supported value for ipv4 filters is value 'none'.

         Note that the value of tIPvXFltrEntryActNatType is silently cleared by
         the system if tIPvXFltrEntryActAction is set to value other than
         'nat'."
    DEFVAL      { dsliteLsnSub }
    ::= { tIPvXFltrEntryActionEntry 20 }

tIPvXFltrEntryActFwdLsp          OBJECT-TYPE
    SYNTAX      TmnxVRtrMplsLspID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdLsp if different from '0'
         together with the value of the object tIPvXFltrEntryActFwdLspRtrId
         specifies the LSP into which a packet should be forwarded if it hits
         this filter entry.

         The value of the object tIPvXFltrEntryActAction of this entry must be
         'forwardLsp' in such case.

         The value is reset to '0' if the value of the object
         tIPvXFltrEntryActAction is set to value other than 'forwardLsp'.

         The value has to be '0' if the value of the object
         tIPvXFltrEntryActFwdLspRtrId is not set (i.e. is '0').

         If a non-zero value is set, the value of the object
         tIPvXFltrEntryActFwdLspRtrId has to be set as well."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 21 }

tIPvXFltrEntryActFwdLspRtrId     OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdLspRtrId specifies the
         router ID that the LSP ID defined by the value of the object
         tIPvXFltrEntryActFwdLsp belongs to.

         The value of the object tIPvXFltrEntryActAction of this entry must be
         'forwardLsp' in such case.

         The value is reset to '0' if the value of the object
         tIPvXFltrEntryActAction is set to other value than 'forwardLsp'.

         The value has to be '0' if the value of the object
         tIPvXFltrEntryActFwdLsp is not set (i.e. is '0').

         If a non-zero value is set, the value of the object
         tIPvXFltrEntryActFwdLsp has to be set as well.

         The ID of the base router and '0' are the only allowed values with
         this version of the product."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 22 }

tIPvXFltrEntryActPktLenVal1      OBJECT-TYPE
    SYNTAX      TFilterPacketLength
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActPktLenVal1 specifies the
         value1 to be compared to the value of 'Total Length' field of IPv4
         header or 'Payload Length' field of IPv6 header of an IP packet that
         has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPvXFltrEntryActPktLenOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPvXFltrEntryActPktLenOper is other than 'none
         (0)'.

         If the value of tIPvXFltrEntryActPktLenOper is 'range (2)' then the
         value of this object must be less than the value of
         tIPvXFltrEntryActPktLenVal2.

         If the value of tIPvXFltrEntryActPktLenOper is 'lt (3)' then the value
         of this object can be set in range 1..65535.

         If the value of tIPvXFltrEntryActPktLenOper is 'gt (4)' then the value
         of this object can be set in range 0..65534.

         If both the values of the objects tIPvXFltrEntryActPktLenOper and
         tIPvXFltrEntryActPktLenVal1 need to be changed then it must be done in
         the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPvXFltrEntryActAction is set to a value other than 'dropPktLen'
         or 'rateLimitPktLen'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 23 }

tIPvXFltrEntryActPktLenVal2      OBJECT-TYPE
    SYNTAX      TFilterPacketLength
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActPktLenVal2 specifies the
         value2 to be compared to the value of 'Total Length' field of IPv4
         header or 'Payload Length' field of IPv6 header of an IP packet that
         has hit this filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPvXFltrEntryActPktLenOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPvXFltrEntryActPktLenOper is 'range (2)'.

         The value of this object must be greater than the value of
         tIPvXFltrEntryActPktLenVal1.

         If both the values of the objects tIPvXFltrEntryActPktLenOper and
         tIPvXFltrEntryActPktLenVal2 need to be changed then it must be done in
         the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPvXFltrEntryActAction is set to a value other than 'dropPktLen'
         or 'rateLimitPktLen'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 24 }

tIPvXFltrEntryActPktLenOper      OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActPktLenOper specifies the way
         how the values of the objects tIPvXFltrEntryActPktLenVal1 and
         tIPvXFltrEntryActPktLenVal2 are used to form a condition that must be
         fulfilled in order to execute the action specified by the value of
         tIPvXFltrEntryActAction. Otherwise the opposite action is executed.

         The value of this object can be set to a non-default value only if the
         value of the object tIPvXFltrEntryActAction is 'dropPktLen' or
         'rateLimitPktLen'.

         If the value of this object is being changed from the default value to
         any non-default value the value of the object tIPvXFltrEntryActAction
         must be sent in the same SET SNMP request.

         If the value of this object is 'eq (1)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be equal to the value of the object
         tIPvXFltrEntryActPktLenVal1 in order to execute the TRUE case action
         (see table below). Otherwise the FALSE case action is executed. The
         value of the object tIPvXFltrEntryActPktLenVal2 is ignored.

         If the value of this object is 'range (2)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be greater than or equal to the value of the
         object tIPvXFltrEntryActPktLenVal1 and less than or equal to the value
         of the object tIPvXFltrEntryActPktLenVal2 in order to execute the TRUE
         case action (see table below). Otherwise the FALSE case action is
         executed.

         If the value of this object is 'lt (3)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be less than the value of the object
         tIPvXFltrEntryActPktLenVal1 in order to execute the TRUE case action
         (see table below). Otherwise the FALSE case action is executed. The
         value of the object tIPvXFltrEntryActPktLenVal2 is ignored.

         If the value of this object is 'gt (4)' then the value of the Total
         Length field of the IP header of the packet that has matched this
         filter's entry must be greater than the value of the object
         tIPvXFltrEntryActPktLenVal1 in order to execute the TRUE case action
         (see table below). Otherwise the FALSE case action is executed. The
         value of the object tIPvXFltrEntryActPktLenVal2 is ignored.


         tIPvXFltrEntryActAction |   TRUE case action  |  FALSE case action
         ------------------------------------------------------------------
         dropPktLen              |      drop           |      forward
         ------------------------------------------------------------------
         rateLimitPktLen         |      rateLimit      |      forward


         Allowed ranges for the values of tIPvXFltrEntryActPktLenVal1 and
         tIPvXFltrEntryActPktLenVal2 are:

         Operator                |Packet Length Value 1|Packet Length Value 2
         --------------------------------------------------------------------
         none (0)                |      N/A            |      N/A
         eq(1)                   |    0..65535         |      N/A
         range(2)                |    0..65534         | (Value1 + 1)..65535
         lt(3)                   |    1..65535         |      N/A
         gt(4)                   |    0..65534         |      N/A

         Note that the value of this object is silently cleared by the system
         if tIPvXFltrEntryActAction is set to a value other than 'dropPktLen'
         or 'rateLimitPktLen'."
    DEFVAL      { none }
    ::= { tIPvXFltrEntryActionEntry 25 }

tIPvXFltrEntryActTTLVal1         OBJECT-TYPE
    SYNTAX      TFilterTTL
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActTTLVal1 specifies the value1
         to be compared to the value of 'Time-to-live' field of IPv4 header or
         'Hop-Limit' field of IPv6 header of an IP packet that has hit this
         filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPvXFltrEntryActTTLOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPvXFltrEntryActTTLOper is other than 'none (0)'.

         If the value of tIPvXFltrEntryActTTLOper is 'range (2)' then the value
         of this object must be less than the value of
         tIPvXFltrEntryActTTLVal2.

         If the value of tIPvXFltrEntryActTTLOper is 'lt (3)' then the value of
         this object can be set in range 1..255.

         If the value of tIPvXFltrEntryActTTLOper is 'gt (4)' then the value of
         this object can be set in range 0..254.

         If both the values of the objects tIPvXFltrEntryActTTLOper and
         tIPvXFltrEntryActTTLVal1 need to be changed then it must be done in
         the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPvXFltrEntryActAction is set to a value other than 'dropTtl' or
         'rateLimitTtl'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 26 }

tIPvXFltrEntryActTTLVal2         OBJECT-TYPE
    SYNTAX      TFilterTTL
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActTTLVal2 specifies value2 to
         be compared to the value of 'Time-to-live' field of IPv4 header or
         'Hop-Limit' field of IPv6 header of an IP packet that has hit this
         filter's entry.

         The way how the value of this object is used depends on the value of
         the object tIPvXFltrEntryActTTLOper.

         The value of this object can be set to a non-default value only if the
         value of the object tIPvXFltrEntryActTTLOper is 'range (2)'.

         The value of this object must be greater than the value of
         tIPvXFltrEntryActTTLVal1.

         If both the values of the objects tIPvXFltrEntryActTTLOper and
         tIPvXFltrEntryActTTLVal2 need to be changed then it must be done in
         the same SET SNMP request.

         Note that the value of this object is silently cleared by the system
         if tIPvXFltrEntryActAction is set to a value other than 'dropTtl' or
         'rateLimitTtl'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 27 }

tIPvXFltrEntryActTTLOper         OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActTTLOper specifies the way how
         the values of the objects tIPvXFltrEntryActTTLVal1 and
         tIPvXFltrEntryActTTLVal2 are used to form a condition that must be
         fulfilled in order to execute the action specified by the value of
         tIPvXFltrEntryActAction. Otherwise the opposite action is executed.

         The value of this object can be set to a non-default value only if the
         value of the object tIPvXFltrEntryActAction is 'dropTtl' or
         'rateLimitTtl'.

         If the value of this object is being changed from the default value to
         any non-default value the value of the object tIPvXFltrEntryActAction
         must be sent in the same SET SNMP request.

         If the value of this object is 'eq (1)' then the value of the
         Time-To-Live field of the IP header of the packet that has matched
         this filter's entry must be equal to the value of the object
         tIPvXFltrEntryActTTLVal1 in order to execute the TRUE case action (see
         table below). Otherwise the FALSE case action is executed. The value
         of the object tIPvXFltrEntryActTTLVal2 is ignored.

         If the value of this object is 'range (2)' then the value of the
         Time-To-Live field of the IP header of the packet that has matched
         this filter's entry must be greater than or equal to the value of the
         object tIPvXFltrEntryActTTLVal1 and less than or equal to the value of
         the object tIPvXFltrEntryActTTLVal2 in order to execute the TRUE case
         action (see table below). Otherwise the FALSE case action is executed.

         If the value of this object is 'lt (3)' then the value of the
         Time-To-Live field of the IP header of the packet that has matched
         this filter's entry must be less than the value of the object
         tIPvXFltrEntryActTTLVal1 in order to execute the TRUE case action (see
         table below). Otherwise the FALSE case action is executed. The value
         of the object tIPvXFltrEntryActTTLVal2 is ignored.

         If the value of this object is 'gt (4)' then the value of the
         Time-To-Live field of the IP header of the packet that has matched
         this filter's entry must be greater than the value of the object
         tIPvXFltrEntryActTTLVal1 in order to execute the TRUE case action (see
         table below). Otherwise the FALSE case action is executed. The value
         of the object tIPvXFltrEntryActTTLVal2 is ignored.


         tIPvXFltrEntryActAction |   TRUE case action  |  FALSE case action
         ------------------------------------------------------------------
         dropTtl                 |      drop           |      forward
         ------------------------------------------------------------------
         rateLimitTtl            |      rateLimit      |      forward


         Allowed ranges for the values of tIPvXFltrEntryActTTLVal1 and
         tIPvXFltrEntryActTTLVal2 are:

         Operator                | Time-To-Live Value 1| Time-To-Live Value 2
         --------------------------------------------------------------------
         none (0)                |      N/A            |      N/A
         eq(1)                   |    0..255           |      N/A
         range(2)                |    0..254           | (Value1 + 1)..255
         lt(3)                   |    1..255           |      N/A
         gt(4)                   |    0..254           |      N/A

         Note that the value of this object is silently cleared by the system
         if tIPvXFltrEntryActAction is set to a value other than 'dropTtl' or
         'rateLimitTtl'."
    DEFVAL      { none }
    ::= { tIPvXFltrEntryActionEntry 28 }

tIPvXFltrEntryActEsi             OBJECT-TYPE
    SYNTAX      TFilterEsi
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActEsi specifies the ethernet
         segment identifier (ESI) of the first ESI identified appliance in
         Nuage service chain. When the value of tMacFilterParamsAction is
         'forwardEsiL2' or 'forwardEsiL3' packets matching the filter entry are
         forwarded to the appliance using EVPN-resolved VXLAN tunnel in the
         specified VPLS/VPRN service
         (tIPvXFltrEntryActFwdEsiSvcId/tIPvXFltrEntryActFwdEsiVRtrId).

         The value '0' indicates that there is no ESI specified.

         There are two options how to set the value of tIPvXFltrEntryActEsi:
         1. Non zero value of tIPvXFltrEntryActEsi is set together
            with non zero values of tIPvXFltrEntryActFwdEsiVRtrId,
            tIPvXFltrEntryActFwdEsiSFIpType and tIPvXFltrEntryActFwdEsiSFIp.
            In this case value of tIPvXFltrEntryActAction is set to
            'forwardEsiL3' by the system.

         2. Non zero value of tIPvXFltrEntryActEsi is set together with a non
            zero value of tIPvXFltrEntryActFwdEsiSvcId. In this case value of
            tIPvXFltrEntryActAction is set to 'forwardEsiL2' by the system.

         Note that the value of tIPvXFltrEntryActEsi is silently cleared by the
         system if the value of tIPvXFltrEntryActAction is set to any value
         other than 'forwardEsiL2' or 'forwardEsiL3'."
    DEFVAL      { '00000000000000000000'H }
    ::= { tIPvXFltrEntryActionEntry 29 }

tIPvXFltrEntryActFwdEsiSvcId     OBJECT-TYPE
    SYNTAX      TmnxServId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdEsiSvcId specifies the
         identifier of a VPLS used for VPN/DC connectivity.

         The value '0' indicates that there is no VPLS identifier specified.

         The non zero value of tIPvXFltrEntryActFwdEsiSvcId must be set
         together with a non zero value of tIPvXFltrEntryActEsi.

         Note that the value of tIPvXFltrEntryActFwdEsiSvcId is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardEsiL2'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 30 }

tIPvXFltrEntryActFwdEsiVRtrId    OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdEsiVRtrId specifies the
         VPRN/rVPLS virtual router identifier used for VPN/DC connectivity.

         The value '0' indicates that there is no VPRN/rVPLS virtual router
         identifier specified.

         The non zero value of tIPvXFltrEntryActFwdEsiVRtrId must be set
         together with non zero values of tIPvXFltrEntryActEsi,
         tIPvXFltrEntryActFwdEsiSFIpType and tIPvXFltrEntryActFwdEsiSFIp.

         Note that the value of tIPvXFltrEntryActFwdEsiVRtrId is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardEsiL3'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 31 }

tIPvXFltrEntryActFwdEsiSFIpType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdEsiSFIpType specifies the
         context in which the value of tIPvXFltrEntryActFwdEsiSFIp is
         interpreted.

         Only following values are supported:
            unknown(0)
            ipv4(1)
            ipv6(2)

         The value 'unknown' indicates that service function IP address type is
         not specified.

         If the value is different from 'unknown' it must be consistent with
         filter type given by the value of the object
         tIPvXFltrEntryActFltrType.

         The non zero value of tIPvXFltrEntryActFwdEsiSFIpType must be set
         together with a non zero values of tIPvXFltrEntryActFwdEsiSFIp,
         tIPvXFltrEntryActFwdEsiVRtrId and tIPvXFltrEntryActEsi.

         Note that the value of tIPvXFltrEntryActFwdEsiSFIpType is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardEsiL3'."
    DEFVAL      { unknown }
    ::= { tIPvXFltrEntryActionEntry 32 }

tIPvXFltrEntryActFwdEsiSFIp      OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdEsiSFIp specifies the IP
         address of the service function toward which traffic is steered.

         The value '0' indicates that no service function IP address is
         specified.

         The non zero value of tIPvXFltrEntryActFwdEsiSFIp must be set together
         with a non zero values of tIPvXFltrEntryActFwdEsiSFIpType,
         tIPvXFltrEntryActFwdEsiVRtrId and tIPvXFltrEntryActEsi.

         Note that the value of tIPvXFltrEntryActFwdEsiSFIp is silently cleared
         by the system if the value of tIPvXFltrEntryActAction is set to any
         value other than 'forwardEsiL3'."
    DEFVAL      { '00000000'H }
    ::= { tIPvXFltrEntryActionEntry 33 }

tIPvXFltrEntryActFwdEsiVasIf     OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdEsiVasIf specifies the
         virtual router interface index of VPRN RVPLS interface used for VPN/DC
         connectivity.

         The value '0' indicates that no interface id is specified.

         The non zero value of tIPvXFltrEntryActFwdEsiVasIf must be set
         together with a non zero values of tIPvXFltrEntryActFwdEsiVRtrId,
         tIPvXFltrEntryActFwdEsiSFIp, tIPvXFltrEntryActFwdEsiSFIpType and
         tIPvXFltrEntryActEsi.

         Note: The value of tIPvXFltrEntryActFwdEsiVasIf is set to '0' by the
         system if the value of tIPvXFltrEntryActAction is set to any value
         other than 'forwardEsiL3'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 34 }

tIPvXFltrEntryActRateLimit       OBJECT-TYPE
    SYNTAX      TFilterEntryActionRateLimit
    UNITS       "kilobps"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActRateLimit specifies the rate
         to which the traffic matching the filter entry will be limited.

         The value of tIPvXFltrEntryActRateLimit can be set to a non default
         value only if the value of tIPvXFltrEntryActAction is set to
         'rateLimit', 'rateLimitPktLen', 'rateLimitTtl', 'rateLimitPattern' or
         'rateLimitExtractedTraffic'.

         Note that the value of tIPvXFltrEntryActRateLimit is silently cleared
         by the system if the value of tIPvXFltrEntryActAction is set to any
         value other than 'rateLimit',  'rateLimitPktLen', 'rateLimitTtl', 'rateLimitPattern' or
         'rateLimitExtractedTraffic' or when 'tIPvXFltrEntryActRateLimitPps' is set to a non-default
         value."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 35 }

tIPvXFltrEntryActPbrTargetStatus OBJECT-TYPE
    SYNTAX      TFilterPbrTargetStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActPbrTargetStatus indicates the
         PBR target status.

         Refer to the description of the textual convention
         TFilterPbrTargetStatus for more information."
    ::= { tIPvXFltrEntryActionEntry 36 }

tIPvXFltrEntryActRemarkDSCP      OBJECT-TYPE
    SYNTAX      TDSCPNameOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActRemarkDSCP specifies the
         value which remarks the DSCP value of packet matching the filter
         entry.

         The value of tIPvXFltrEntryActRemarkDSCP can be set to non default
         value only if the value of tIPvXFltrEntryActAction is set to
         'remarkDscp' or the value of tIPvXFltrEntryActActionExt is set to
         'remarkDscp' and the value of tIPvXFltrEntryActAction is set to one of
         the following values:

         forwardEsiL3 forwardRtr forwardNextHop forwardNextHopRtr
         forwardNHInterface forwardLsp forwardRPlcy

         Note that the value of tIPvXFltrEntryActRemarkDSCP is silently cleared
         by the system if the value of tIPvXFltrEntryActAction is changed from
         'remarkDscp' to any other value or if tIPvXFltrEntryActActionExt is
         changed from 'remarkDscp' to any other value."
    DEFVAL      { ''H }
    ::= { tIPvXFltrEntryActionEntry 37 }

tIPvXFltrEntryActActionExt       OBJECT-TYPE
    SYNTAX      TIPvXFilterEntryActionExt
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActActionExt specifies the
         action to be taken on a packet along with action specified by
         tIPvXFltrEntryActAction.

         Refer to the description of the textual convention
         TIPvXFilterEntryActionExt for more information."
    DEFVAL      { none }
    ::= { tIPvXFltrEntryActionEntry 38 }

tIPvXFltrEntryActFwdVprnTgtBgNHT OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdVprnTgtBgNHT specifies the
         context in which the value of tIPvXFltrEntryActFwdVprnTgtBgNH is
         interpreted.

         Only following values are supported:
            unknown(0)
            ipv4(1)

         The value 'unknown' indicates IP address type is not specified.

         The non zero value of tIPvXFltrEntryActFwdVprnTgtBgNHT must be set
         together with non zero values of tIPvXFltrEntryActFwdVprnTgtBgNH,
         tIPvXFltrEntryActFwdVprnTgtRtrId and tIPvXFltrEntryActAction value
         'forwardVprnTarget'.

         Note that the value of tIPvXFltrEntryActFwdVprnTgtBgNHT is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardVprnTarget'."
    DEFVAL      { unknown }
    ::= { tIPvXFltrEntryActionEntry 39 }

tIPvXFltrEntryActFwdVprnTgtBgNH  OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdVprnTgtBgNH specifies the
         target BGP next-hop IP address.

         The value '0' indicates that no IP address is specified.

         The non zero value of tIPvXFltrEntryActFwdVprnTgtBgNH must be set
         together with non zero values of tIPvXFltrEntryActFwdVprnTgtBgNHT,
         tIPvXFltrEntryActFwdVprnTgtRtrId and tIPvXFltrEntryActAction value
         'forwardVprnTarget'.

         Note that the value of tIPvXFltrEntryActFwdVprnTgtBgNH is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardVprnTarget'."
    DEFVAL      { '00000000'H }
    ::= { tIPvXFltrEntryActionEntry 40 }

tIPvXFltrEntryActFwdVprnTgtRtrId OBJECT-TYPE
    SYNTAX      TmnxVRtrIDOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdVprnTgtRtrId specifies the
         virtual router used for route lookup.

         The value '0' indicates that no virtual router is specified.

         The non zero value of tIPvXFltrEntryActFwdVprnTgtRtrId must be set
         together with non zero values of tIPvXFltrEntryActFwdVprnTgtBgNHT,
         tIPvXFltrEntryActFwdVprnTgtBgNH and tIPvXFltrEntryActAction value
         'forwardVprnTarget'.

         Note that the value of tIPvXFltrEntryActFwdVprnTgtRtrId is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardVprnTarget'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 41 }

tIPvXFltrEntryActFwdVprnTgtAdPxT OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdVprnTgtAdPxT specifies the
         context in which the value of tIPvXFltrEntryActFwdVprnTgtAdPx is
         interpreted.

         Only following values are supported:
            unknown(0)
            ipv4(1)
            ipv6(2)

         The value 'unknown' indicates that IP address type is not specified.

         If the value is different from 'unknown' it must be consistent with
         filter type given by the value of the object
         tIPvXFltrEntryActFltrType.

         The non zero value of tIPvXFltrEntryActFwdVprnTgtAdPxT must be set
         together with a non zero value of tIPvXFltrEntryActFwdVprnTgtAdPx. In
         such case the values of tIPvXFltrEntryActFwdVprnTgtBgNHT,
         tIPvXFltrEntryActFwdVprnTgtBgNH and tIPvXFltrEntryActFwdVprnTgtRtrId
         must have non default value and the value of tIPvXFltrEntryActAction
         must be 'forwardVprnTarget'.

         Note that the value of tIPvXFltrEntryActFwdVprnTgtAdPxT is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardVprnTarget'."
    DEFVAL      { unknown }
    ::= { tIPvXFltrEntryActionEntry 42 }

tIPvXFltrEntryActFwdVprnTgtAdPx  OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdVprnTgtAdPx specifies the
         IP address of the service function toward which traffic is steered.

         The value '0' indicates that no prefix is specified.

         The non zero value of tIPvXFltrEntryActFwdVprnTgtAdPx must be set
         together with non zero value of tIPvXFltrEntryActFwdVprnTgtAdPxT. In
         such case the values of tIPvXFltrEntryActFwdVprnTgtBgNHT,
         tIPvXFltrEntryActFwdVprnTgtBgNH and tIPvXFltrEntryActFwdVprnTgtRtrId
         must have non default values and the value of tIPvXFltrEntryActAction
         must be 'forwardVprnTarget'.

         Note that the value of tIPvXFltrEntryActFwdVprnTgtAdPx is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardVprnTarget'."
    DEFVAL      { "" }
    ::= { tIPvXFltrEntryActionEntry 43 }

tIPvXFltrEntryActFwdVprnTgtAdPxL OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixPrefix
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tIPvXFltrEntryActFwdVprnTgtAdPxL specifies the IP prefix
         length of this prefix list entry."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 44 }

tIPvXFltrEntryActFwdVprnTgtLspId OBJECT-TYPE
    SYNTAX      TmnxVRtrMplsLspID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdVprnTgtLspId specifies LSP
         used for forwarding the packet.

         The value '0' indicates that no prefix is specified.

         The non zero value of tIPvXFltrEntryActFwdVprnTgtLspId can be set only
         when values of tIPvXFltrEntryActFwdVprnTgtBgNHT,
         tIPvXFltrEntryActFwdVprnTgtBgNH and tIPvXFltrEntryActFwdVprnTgtRtrId
         have non default values and the value of tIPvXFltrEntryActAction is
         'forwardVprnTarget'.

         Note that the value of tIPvXFltrEntryActFwdVprnTgtAdPx is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardVprnTarget'."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 45 }

tIPvXFltrEntryActFwdBondingConn  OBJECT-TYPE
    SYNTAX      TmnxSubBondingConnIdOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdBondingConn specifies the
         bonding connection ID."
    DEFVAL      { 0 }
    ::= { tIPvXFltrEntryActionEntry 46 }

tIPvXFltrEntryActFcName          OBJECT-TYPE
    SYNTAX      TFCTypeOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFcName specifies the
         forwarding class name."
    DEFVAL      { none }
    ::= { tIPvXFltrEntryActionEntry 47 }

tIPvXFltrEntryActFwdGreTun       OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActFwdGreTun specifies the GRE
         tunnel template to be used. The action of this entry should be
         'forwardGreTunnel' in such a case.

         Note that the value of tIPvXFltrEntryActFwdGreTun is silently cleared
         by the system if tIPvXFltrEntryActAction is set to value other than
         'forwardGreTunnel'."
    DEFVAL      { ''H }
    ::= { tIPvXFltrEntryActionEntry 48 }

tIPvXFltrEntryActCondExpression  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..8))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActCondExpression specifies the
         expression to be matched.

         tIPvXFltrEntryActCondExpression has to be set together with
         tIPvXFltrEntryActCondExpMask, tIPvXFltrEntryActCondOffsetType,
         tIPvXFltrEntryActCondOffsetVal and tIPvXFltrEntryActAction. The value
         of tIPvXFltrEntryActAction has to be set to one of the following
         values: 'dropPattern', 'rateLimitPattern', 'forwardPattern'.

         Note that the value of tIPvXFltrEntryActCondExpression is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'dropPattern', 'rateLimitPattern',
         'forwardPattern'."
    DEFVAL      { ''H }
    ::= { tIPvXFltrEntryActionEntry 49 }

tIPvXFltrEntryActCondExpMask     OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..8))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActCondExpMask specifies the
         expression mask.

         tIPvXFltrEntryActCondExpMask has to be set together with
         tIPvXFltrEntryActCondExpression, tIPvXFltrEntryActCondOffsetType,
         tIPvXFltrEntryActCondOffsetVal and tIPvXFltrEntryActAction. The value
         of tIPvXFltrEntryActAction has to be set to one of the following
         values: 'dropPattern', 'rateLimitPattern', 'forwardPattern'.

         Note that the value of tIPvXFltrEntryActCondExpMask is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'dropPattern', 'rateLimitPattern',
         'forwardPattern'."
    DEFVAL      { ''H }
    ::= { tIPvXFltrEntryActionEntry 50 }

tIPvXFltrEntryActCondOffsetType  OBJECT-TYPE
    SYNTAX      INTEGER {
        none     (0),
        layer3   (1),
        layer4   (2),
        data     (3),
        dnsQType (4)
    }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActCondOffsetType specifies the
         offset type of the expression.

         tIPvXFltrEntryActCondOffsetType has to be set together with
         tIPvXFltrEntryActCondExpression, tIPvXFltrEntryActCondExpMask,
         tIPvXFltrEntryActCondOffsetVal and tIPvXFltrEntryActAction. The value
         of tIPvXFltrEntryActAction has to be set to one of the following
         values: 'dropPattern', 'rateLimitPattern', 'forwardPattern'.

         Note that the value of tIPvXFltrEntryActCondOffsetType is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'dropPattern', 'rateLimitPattern',
         'forwardPattern'."
    DEFVAL      { none }
    ::= { tIPvXFltrEntryActionEntry 51 }

tIPvXFltrEntryActCondOffsetVal   OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActCondOffsetVal specifies the
         offset of the expression.

         -1 indicates offset is not set.

         tIPvXFltrEntryActCondOffsetVal has to be set together with
         tIPvXFltrEntryActCondExpression, tIPvXFltrEntryActCondOffsetType,
         tIPvXFltrEntryActCondExpMask and tIPvXFltrEntryActAction. The value of
         tIPvXFltrEntryActAction has to be set to one of the following values:
         'dropPattern', 'rateLimitPattern', 'forwardPattern'.

         Note that the value of tIPvXFltrEntryActCondOffsetVal is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'dropPattern', 'rateLimitPattern',
         'forwardPattern'."
    DEFVAL      { -1 }
    ::= { tIPvXFltrEntryActionEntry 52 }

tIPvXFltrFwdMplsPlcyEndptAddrTp  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address type of the MPLS forwarding policy endpoint to be used
         when the value of tIPvXFltrEntryActAction is 'forwardMplsPlcyEndpt'

         Only following values are supported:
            unknown(0)
            ipv4(1)
            ipv6(2)

         The value 'unknown' indicates IP address type is not specified.

         The non zero value of tIPvXFltrFwdMplsPlcyEndptAddrTp must be set
         together with non zero values of tIPvXFltrFwdMplsPlcyEndptAddr, and
         tIPvXFltrEntryActAction value 'forwardMplsPlcyEndpt'.

         Note that the value of tIPvXFltrFwdMplsPlcyEndptAddrTp is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardMplsPlcyEndpt'."
    DEFVAL      { unknown }
    ::= { tIPvXFltrEntryActionEntry 53 }

tIPvXFltrFwdMplsPlcyEndptAddr    OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value specifies the MPLS forwarding policy endpoint address to be
         used when the value of tIPvXFltrEntryActAction is
         'forwardMplsPlcyEndpt'.

         The value '0' indicates that no IP address is specified.

         The non zero value of tIPvXFltrFwdMplsPlcyEndptAddr must be set
         together with non zero values of tIPvXFltrFwdMplsPlcyEndptAddrTp, and
         tIPvXFltrEntryActAction value 'forwardMplsPlcyEndpt'.

         Note that the value of tIPvXFltrFwdMplsPlcyEndptAddr is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardMplsPlcyEndpt'."
    DEFVAL      { '00000000'H }
    ::= { tIPvXFltrEntryActionEntry 54 }

tIPvXFltrFwdSrtePlcyEndptAddrTp  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address type of the SR-TE policy endpoint to be used when the
         value of tIPvXFltrEntryActAction is 'forwardSrtePlcyEndptColor'

         Only following values are supported:
            unknown(0)
            ipv4(1)
            ipv6(2)

         The value 'unknown' indicates IP address type is not specified.

         The non zero value of tIPvXFltrFwdSrtePlcyEndptAddrTp must be set
         together with non zero values of tIPvXFltrFwdSrtePlcyEndptAddr, and
         tIPvXFltrEntryActAction value 'forwardSrtePlcyEndptColor'.

         Note that the value of tIPvXFltrFwdSrtePlcyEndptAddrTp is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardSrtePlcyEndptColor'."
    DEFVAL      { unknown }
    ::= { tIPvXFltrEntryActionEntry 55 }

tIPvXFltrFwdSrtePlcyEndptAddr    OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|4|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value specifies the SR-TE policy endpoint address to be used when
         the value of tIPvXFltrEntryActAction is 'forwardSrtePlcyEndptColor'.

         The value '0' indicates that no IP address is specified.

         The non zero value of tIPvXFltrFwdSrtePlcyEndptAddr must be set
         together with non zero values of tIPvXFltrFwdSrtePlcyEndptAddrTp, and
         tIPvXFltrEntryActAction value 'forwardSrtePlcyEndptColor'.

         Note that the value of tIPvXFltrFwdSrtePlcyEndptAddr is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardSrtePlcyEndptColor'."
    DEFVAL      { '00000000'H }
    ::= { tIPvXFltrEntryActionEntry 56 }

tIPvXFltrFwdSrtePlcyColor        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the SR-TE policy color to be used when the value of
         tIPvXFltrEntryActAction is 'forwardSrtePlcyEndptColor'."
    ::= { tIPvXFltrEntryActionEntry 57 }

tIPvXFltrActL2AwareNatBypass     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrActL2AwareNatBypass specifies whether
         filter classified traffic bypasses L2aware NAT.

         This action is only applicable to L2aware NAT subscribers and it must
         be configured together with action forward. Traffic identified in the
         match condition will bypass L2aware NAT. A common use case is to
         bypass NAT for on-net traffic which terminates within the customer
         network.

         The remaining traffic that is not classified for bypass will
         automatically be diverted to L2aware NAT, unless it is explicitly
         configured to be dropped."
    DEFVAL      { false }
    ::= { tIPvXFltrEntryActionEntry 58 }

tIPvXFltrEntryActRateLimitPps    OBJECT-TYPE
    SYNTAX      TFilterEntryActionRateLimitPps
    UNITS       "packets per second"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActRateLimitPps specifies the
         rate in packets per second, to which the traffic matching the filter
         entry will be limited.

         The value of tIPvXFltrEntryActRateLimitPps can be set to a non default
         value only if the value of tIPvXFltrEntryActAction is set to
         'rateLimit', 'rateLimitPktLen', 'rateLimitTtl', 'rateLimitPattern' or
         'rateLimitExtractedTraffic'.

         It is not allowed to set tIPvXFltrEntryActRateLimitPps and
         tIPvXFltrEntryActRateLimit to non-default values at the same time.

         Note that the value of tIPvXFltrEntryActRateLimitPps is silently cleared
         by the system if the value of tIPvXFltrEntryActAction is set to any
         value other than 'rateLimit',  'rateLimitPktLen', 'rateLimitTtl', 'rateLimitPattern'
         or 'rateLimitExtractedTraffic' or tIPvXFltrEntryActRateLimit is set to a non-default
         value."
    DEFVAL      { -2 }
    ::= { tIPvXFltrEntryActionEntry 59 }

tIPvXFltrFwdSrv6PlcyEndptAddrTp  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address type of the SRv6 policy endpoint to be used when the
         value of tIPvXFltrEntryActAction is 'forwardSrv6Plcy'

         Only following values are supported:
            unknown(0)
            ipv6(2)

         The value 'unknown' indicates IP address type is not specified.

         The non zero value of tIPvXFltrFwdSrv6PlcyEndptAddrTp must be set
         together with non zero values of tIPvXFltrFwdSrv6PlcyEndptAddr, and
         tIPvXFltrEntryActAction value 'forwardSrv6Plcy'.

         Note that the value of tIPvXFltrFwdSrv6PlcyEndptAddrTp is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardSrv6Plcy'."
    DEFVAL      { unknown }
    ::= { tIPvXFltrEntryActionEntry 60 }

tIPvXFltrFwdSrv6PlcyEndptAddr    OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value specifies the SRv6 policy endpoint address to be used when
         the value of tIPvXFltrEntryActAction is 'forwardSrv6Plcy'.

         The default value indicates that no IP address is specified.

         The non zero value of tIPvXFltrFwdSrv6PlcyEndptAddr must be set
         together with non zero values of tIPvXFltrFwdSrv6PlcyEndptAddrTp, and
         tIPvXFltrEntryActAction value 'forwardSrv6Plcy'.

         Note that the value of tIPvXFltrFwdSrv6PlcyEndptAddr is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardSrv6Plcy'."
    DEFVAL      { ''H }
    ::= { tIPvXFltrEntryActionEntry 61 }

tIPvXFltrFwdSrv6PlcyColor        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the SRv6 policy color to be used when the value of
         tIPvXFltrEntryActAction is 'forwardSrv6Plcy'."
    ::= { tIPvXFltrEntryActionEntry 62 }

tIPvXFltrFwdSrv6PlcySvcSidAddrTp OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address type of the SRv6 policy SID to be used when the value
         of tIPvXFltrEntryActAction is 'forwardSrv6Plcy'

         Only following values are supported:
            unknown(0)
            ipv6(2)

         The value 'unknown' indicates IP address type is not specified.

         The non zero value of tIPvXFltrFwdSrv6PlcySvcSidAddrTp must be set
         together with non zero values of tIPvXFltrFwdSrv6PlcySvcSid, and
         tIPvXFltrEntryActAction value 'forwardSrv6Plcy'.

         Note that the value of tIPvXFltrFwdSrv6PlcySvcSidAddrTp is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'forwardSrv6Plcy'."
    DEFVAL      { unknown }
    ::= { tIPvXFltrEntryActionEntry 63 }

tIPvXFltrFwdSrv6PlcySvcSid       OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (0|16))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value specifies the IPv6 address of SRv6 service-SID.

         The default value indicates that no service-SID is specified.

         The non zero value of tIPvXFltrFwdSrv6PlcySvcSid must be set together
         with non zero values of tIPvXFltrFwdSrv6PlcySvcSidAddrTp, and
         tIPvXFltrEntryActAction value 'forwardSrv6Plcy'.

         Note that the value of tIPvXFltrFwdSrv6PlcySvcSid is silently cleared
         by the system if the value of tIPvXFltrEntryActAction is set to any
         value other than 'forwardSrv6Plcy'."
    DEFVAL      { ''H }
    ::= { tIPvXFltrEntryActionEntry 64 }

tIPvXFltrEntryActRateLimitMbs    OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..268435456)
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActRateLimitMbs specifies the
         maximum burst size to which the traffic matching the filter entry will
         be limited.

         This is to be used with the action rateLimit.

         Note that the value of tIPvXFltrEntryActRateLimitMbs is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than 'rateLimit'"
    DEFVAL      { -1 }
    ::= { tIPvXFltrEntryActionEntry 65 }

tIPvXFltrEntryActRateLimitPlcr   OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPvXFltrEntryActRateLimitPlcr specifies the
         policer object name to which the traffic matching the filter entry
         will be limited.

         If the value of tIPvXFltrEntryActRateLimitPlcr is set to a non default
         value then the values of tIPvXFltrEntryActRateLimit,
         tIPvXFltrEntryActRateLimitPps and tIPvXFltrEntryActRateLimitMbs are
         set to defaults.

         The value of tIPvXFltrEntryActRateLimitPlcr can be set to a non
         default value only if the value of tIPvXFltrEntryActAction is set to
         'rateLimitPolicer'.

         Note that the value of tIPvXFltrEntryActRateLimitPlcr is silently
         cleared by the system if the value of tIPvXFltrEntryActAction is set
         to any value other than  'rateLimitPolicer' or when
         tIPvXFltrEntryActRateLimit, tIPvXFltrEntryActRateLimitPps and
         tIPvXFltrEntryActRateLimitMbs are set to a non-default value."
    DEFVAL      { ''H }
    ::= { tIPvXFltrEntryActionEntry 66 }

tFltrEntryStatTable              OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrEntryStatEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrEntryStatTable contains statistics and counters
         pertaining to IPv4, IPv6 and MAC ACL filter entries."
    ::= { tFilterObjects 86 }

tFltrEntryStatEntry              OBJECT-TYPE
    SYNTAX      TFltrEntryStatEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The entry contains statistics pertaining to a particular IPv4, IPv6 or
         MAC ACL filter entry.

         Entries in this table are created by the system."
    INDEX       {
        tFltrEntryStatFltrType,
        tFltrEntryStatFltrId,
        tFltrEntryStatFltrEntryId
    }
    ::= { tFltrEntryStatTable 1 }

TFltrEntryStatEntry              ::= SEQUENCE
{
    tFltrEntryStatFltrType           TFilterType,
    tFltrEntryStatFltrId             TAnyFilterID,
    tFltrEntryStatFltrEntryId        TEntryId,
    tFltrEntryStatIngHitCnt          Counter64,
    tFltrEntryStatIngHitCntB         Counter64,
    tFltrEntryStatEgrHitCnt          Counter64,
    tFltrEntryStatEgrHitCntB         Counter64,
    tFltrEntryStatRateLmtIngHitCnt   Counter64,
    tFltrEntryStatRateLmtIngHitCntB  Counter64,
    tFltrEntryStatRateLmtIngDrop     Counter64,
    tFltrEntryStatRateLmtIngDropB    Counter64,
    tFltrEntryStatRateLmtIngFwd      Counter64,
    tFltrEntryStatRateLmtIngFwdB     Counter64,
    tFltrEntryStatRateLmtEgrHitCnt   Counter64,
    tFltrEntryStatRateLmtEgrHitCntB  Counter64,
    tFltrEntryStatRateLmtEgrDrop     Counter64,
    tFltrEntryStatRateLmtEgrDropB    Counter64,
    tFltrEntryStatRateLmtEgrFwd      Counter64,
    tFltrEntryStatRateLmtEgrFwdB     Counter64
}

tFltrEntryStatFltrType           OBJECT-TYPE
    SYNTAX      TFilterType { fltrtypeselIp (1), fltrtypeselMac (2), fltrtypeselIpv6 (4) }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatFltrType specifies the type of
         ACL filter.

         Refer to the description of the textual convention TFilterType for
         more information."
    ::= { tFltrEntryStatEntry 1 }

tFltrEntryStatFltrId             OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatFltrId specifies the filter id
         of an IP, IPv6 or MAC ACL filter based on the value of
         tFltrEntryStatFltrType.

         Refer to the description of the textual convention TAnyFilterID for
         more information."
    ::= { tFltrEntryStatEntry 2 }

tFltrEntryStatFltrEntryId        OBJECT-TYPE
    SYNTAX      TEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatFltrEntryId specifies the entry
         id of filter of type IP, IPv6 or MAC based on the value of
         tFltrEntryStatFltrType."
    ::= { tFltrEntryStatEntry 3 }

tFltrEntryStatIngHitCnt          OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatIngHitCnt indicates the number
         of times an ingress packet matched the filter entry."
    ::= { tFltrEntryStatEntry 4 }

tFltrEntryStatIngHitCntB         OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFltrEntryStatIngHitCntB indicates the number of bytes of
         all ingress packets that matched this entry."
    ::= { tFltrEntryStatEntry 5 }

tFltrEntryStatEgrHitCnt          OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatEgrHitCnt indicates the number
         of times an egress packet matched the filter entry."
    ::= { tFltrEntryStatEntry 6 }

tFltrEntryStatEgrHitCntB         OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of tFltrEntryStatEgrHitCntB indicates the number of bytes of
         all egress packets that matched this entry."
    ::= { tFltrEntryStatEntry 7 }

tFltrEntryStatRateLmtIngHitCnt   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtIngHitCnt indicates how
         many ingress packets were subjected to rate-limiting filter action."
    ::= { tFltrEntryStatEntry 8 }

tFltrEntryStatRateLmtIngHitCntB  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtIngHitCntB indicates the
         number of bytes of all ingress packets that were subjected to
         rate-limiting filter action."
    ::= { tFltrEntryStatEntry 9 }

tFltrEntryStatRateLmtIngDrop     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtIngDrop indicates how
         many ingress packets which were subjected to rate-limiting filter
         action were dropped."
    ::= { tFltrEntryStatEntry 10 }

tFltrEntryStatRateLmtIngDropB    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtIngDropB indicates the
         number of bytes of all ingress packets which were subjected to
         rate-limiting filter action were dropped."
    ::= { tFltrEntryStatEntry 11 }

tFltrEntryStatRateLmtIngFwd      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtIngFwd indicates how many
         ingress packets which were subjected to rate-limiting filter action
         were forwarded."
    ::= { tFltrEntryStatEntry 12 }

tFltrEntryStatRateLmtIngFwdB     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtIngFwdB indicates the
         number of bytes of all ingress packets which were subjected to
         rate-limiting filter action were forwarded."
    ::= { tFltrEntryStatEntry 13 }

tFltrEntryStatRateLmtEgrHitCnt   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtEgrHitCnt indicates how
         many egress packets were subjected to rate-limiting filter action."
    ::= { tFltrEntryStatEntry 14 }

tFltrEntryStatRateLmtEgrHitCntB  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtEgrHitCntB indicates the
         number of bytes of all egress packets that were subjected to
         rate-limiting filter action."
    ::= { tFltrEntryStatEntry 15 }

tFltrEntryStatRateLmtEgrDrop     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtEgrDrop indicates how
         many egress packets which were subjected to rate-limiting filter
         action were dropped."
    ::= { tFltrEntryStatEntry 16 }

tFltrEntryStatRateLmtEgrDropB    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtEgrDropB indicates the
         number of bytes of all egress packets which were subjected to
         rate-limiting filter action were dropped."
    ::= { tFltrEntryStatEntry 17 }

tFltrEntryStatRateLmtEgrFwd      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtEgrFwd indicates how many
         egress packets which were subjected to rate-limiting filter action
         were forwarded."
    ::= { tFltrEntryStatEntry 18 }

tFltrEntryStatRateLmtEgrFwdB     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrEntryStatRateLmtEgrFwdB indicates the
         number of bytes of all egress packets which were subjected to
         rate-limiting filter action were forwarded."
    ::= { tFltrEntryStatEntry 19 }

tFltrPrefListInfoTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrPrefListInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrPrefListInfoTable contains all prefixes from all prefix
         lists. Both implicitly or explicitly defined."
    ::= { tFilterObjects 87 }

tFltrPrefListInfoEntry           OBJECT-TYPE
    SYNTAX      TFltrPrefListInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFltrPrefListInfoTable contains information pertaining
         to a particular IP address prefix which is part of filter prefix list."
    INDEX       {
        tFilterPrefixListType,
        tFilterPrefixListName,
        tFltrPrefListInfoPrefixSrc,
        tFltrPrefListInfoPrefixSrcIndex,
        tFltrPrefListInfoPrefixType,
        tFltrPrefListInfoPrefix,
        tFltrPrefListInfoPrefixLen
    }
    ::= { tFltrPrefListInfoTable 1 }

TFltrPrefListInfoEntry           ::= SEQUENCE
{
    tFltrPrefListInfoPrefixSrc       INTEGER,
    tFltrPrefListInfoPrefixSrcIndex  Unsigned32,
    tFltrPrefListInfoPrefixType      InetAddressType,
    tFltrPrefListInfoPrefix          InetAddress,
    tFltrPrefListInfoPrefixLen       InetAddressPrefixLength,
    tFltrPrefListInfoPrefixOwner     INTEGER,
    tFltrPrefListInfoPrefixProg      TruthValue
}

tFltrPrefListInfoPrefixSrc       OBJECT-TYPE
    SYNTAX      INTEGER {
        prefixConfig          (0),
        applyPathBgpPeer      (1),
        prefixConfigGenerated (4)
    }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPrefListInfoPrefixSrc indicates source of
         the prefix."
    ::= { tFltrPrefListInfoEntry 1 }

tFltrPrefListInfoPrefixSrcIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPrefListInfoPrefixSrcIndex indicates
         criteria index for specific apply-path source. The value of
         tFltrPrefListInfoPrefixSrcIndex is '0' when tFltrPrefListInfoPrefixSrc
         is 'prefixConfig'."
    ::= { tFltrPrefListInfoEntry 2 }

tFltrPrefListInfoPrefixType      OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPrefListInfoPrefixType indicates whether
         the prefix is an IPv4 or IPv6 prefix."
    ::= { tFltrPrefListInfoEntry 3 }

tFltrPrefListInfoPrefix          OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPrefListInfoPrefix indicates the IP
         prefix."
    ::= { tFltrPrefListInfoEntry 4 }

tFltrPrefListInfoPrefixLen       OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPrefListInfoPrefixLen indicates the IP
         prefix length."
    ::= { tFltrPrefListInfoEntry 5 }

tFltrPrefListInfoPrefixOwner     OBJECT-TYPE
    SYNTAX      INTEGER {
        config        (0),
        applyPath     (1),
        prefixExclude (2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPrefListInfoPrefixOwner indicates whether
         the prefix was inserted implicitly by apply-path, generated by a
         specific prefix and prefix-exclude pair or explicitly by prefix
         configuration."
    ::= { tFltrPrefListInfoEntry 6 }

tFltrPrefListInfoPrefixProg      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPrefListInfoPrefixProg indicates whether
         the prefix is programmed on linecard."
    ::= { tFltrPrefListInfoEntry 7 }

tFilterEmbFlowspecEntryInfoTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterEmbFlowspecEntryInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFilterEmbFlowspecEntryInfoTable contains an entry for each
         entry of an auto-created embedded filter for flowspec rules inserted
         in an IP or IPv6 filter with scope other than 'embedded'"
    ::= { tFilterObjects 94 }

tFilterEmbFlowspecEntryInfoEntry OBJECT-TYPE
    SYNTAX      TFilterEmbFlowspecEntryInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterEmbFlowspecEntryInfoTable. Rows in the
         tFilterEmbFlowspecEntryInfoTable are created by the SYSTEM when an
         auto-created embedded filter for flowspec rules is inserted into an IP
         or IPv6 filter with scope other than 'embedded'. They are destroyed by
         the SYSTEM when such auto-created embedded filter is removed from an
         IP or IPv6 filter with scope other than 'embedded'."
    INDEX       {
        tFilterEmbedFlowspecFilterType,
        tFilterEmbedFlowspecInsertFltrId,
        tFilterEmbedFlowspecEmbFltrId,
        tFilterEmbedFlowspecEmbEntryId
    }
    ::= { tFilterEmbFlowspecEntryInfoTable 1 }

TFilterEmbFlowspecEntryInfoEntry ::= SEQUENCE
{
    tFilterEmbedFlowspecEmbFltrId    TAnyFilterID,
    tFilterEmbedFlowspecEmbEntryId   TEntryId,
    tFilterEmbedFlowspecInsEntryId   TAnyEntryId,
    tFilterEmbedFlowspecEntryOpState TmnxFltrEmbeddedEntryState
}

tFilterEmbedFlowspecEmbFltrId    OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFilterEmbedFlowspecEmbFltrId indicates the ID of the
         auto-created embedded filter for flowspec rules that is used as the
         source of embedded entries."
    ::= { tFilterEmbFlowspecEntryInfoEntry 1 }

tFilterEmbedFlowspecEmbEntryId   OBJECT-TYPE
    SYNTAX      TEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecEmbEntryId specifies the
         ID of the entry inside of the auto-created embedded filter for
         flowspec rules specified by tFilterEmbedFlowspecEmbFltrId."
    ::= { tFilterEmbFlowspecEntryInfoEntry 2 }

tFilterEmbedFlowspecInsEntryId   OBJECT-TYPE
    SYNTAX      TAnyEntryId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecInsEntryId indicates which
         entry in the IP or IPv6 filter with scope other than 'embedded'
         specified by tFilterEmbedFlowspecInsertFltrId corresponds to the entry
         specified by tFilterEmbedFlowspecEmbEntryId in the auto-created
         embedded filter for flowspec rules specified by
         tFilterEmbedFlowspecEmbFltrId."
    ::= { tFilterEmbFlowspecEntryInfoEntry 3 }

tFilterEmbedFlowspecEntryOpState OBJECT-TYPE
    SYNTAX      TmnxFltrEmbeddedEntryState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterEmbedFlowspecEntryOpState indicates the
         current operational state of the entry identified by
         tFilterEmbedFlowspecEmbEntryId of the embedded filter identified by
         tFilterEmbedFlowspecEmbFltrId that is embedded into the filter
         identified by tFilterEmbedFlowspecInsertFltrId."
    ::= { tFilterEmbFlowspecEntryInfoEntry 4 }

tFilterRPlcyBindingTableLastChg  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterRPlcyBindingTableLastChg indicates the sysUpTime at
         the time of the last modification of tFilterRPlcyBindingTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 95 }

tFilterRPlcyBindingTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRPlcyBindingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tFilterRPlcyBindingTable contains redirect policy bindings. Used
         for fate sharing between different destinations"
    ::= { tFilterObjects 96 }

tFilterRPlcyBindingEntry         OBJECT-TYPE
    SYNTAX      TFilterRPlcyBindingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterRPlcyBindingTable."
    INDEX       { tFilterRPlcyBindingName }
    ::= { tFilterRPlcyBindingTable 1 }

TFilterRPlcyBindingEntry         ::= SEQUENCE
{
    tFilterRPlcyBindingName          TNamedItem,
    tFilterRPlcyBindingLastChange    TimeStamp,
    tFilterRPlcyBindingRowStatus     RowStatus,
    tFilterRPlcyBindingOperator      TFilterRPBindingOperator,
    tFilterRPlcyBindingOperState     TmnxOperState
}

tFilterRPlcyBindingName          OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPlcyBindingName specifies the name of
         the filter redirect policy binding."
    ::= { tFilterRPlcyBindingEntry 1 }

tFilterRPlcyBindingLastChange    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPlcyBindingLastChange indicates the
         sysUpTime at the time of the last modification of
         tFilterRPlcyBindingEntry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterRPlcyBindingEntry 2 }

tFilterRPlcyBindingRowStatus     OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPlcyBindingRowStatus specifies the
         status of the conceptual row in tFilterRPlcyBindingTable."
    ::= { tFilterRPlcyBindingEntry 3 }

tFilterRPlcyBindingOperator      OBJECT-TYPE
    SYNTAX      TFilterRPBindingOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPlcyBindingOperator specifies the
         operator to use when combining operation state of tests from multiple
         redirect policy destinations."
    DEFVAL      { and }
    ::= { tFilterRPlcyBindingEntry 4 }

tFilterRPlcyBindingOperState     OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPlcyBindingOperState indicates the
         operational state of the destination."
    ::= { tFilterRPlcyBindingEntry 5 }

tFilterRPlcyBindingDestTableLCh  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFilterRPlcyBindingDestTableLCh indicates the sysUpTime at
         the time of the last modification of tFilterRPlcyBindingDestTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 97 }

tFilterRPlcyBindingDestTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFilterRPlcyBindingDestEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The tFilterRPlcyBindingDestTable contains redirect policy bindings.
         Used for fate sharing between different destinations"
    ::= { tFilterObjects 98 }

tFilterRPlcyBindingDestEntry     OBJECT-TYPE
    SYNTAX      TFilterRPlcyBindingDestEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFilterRPlcyBindingDestTable."
    INDEX       {
        tFilterRPlcyBindingName,
        tFilterRedirectPolicy,
        tFltrRPDstAddrType,
        tFltrRPDstAddr
    }
    ::= { tFilterRPlcyBindingDestTable 1 }

TFilterRPlcyBindingDestEntry     ::= SEQUENCE
{
    tFilterRPlcyBindingDestRowStatus RowStatus,
    tFilterRPlcyBindingDestOperState TmnxOperState
}

tFilterRPlcyBindingDestRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPlcyBindingDestRowStatus specifies the
         status of the conceptual row in tFilterRPlcyBindingDestTable."
    ::= { tFilterRPlcyBindingDestEntry 1 }

tFilterRPlcyBindingDestOperState OBJECT-TYPE
    SYNTAX      TmnxOperState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFilterRPlcyBindingDestOperState indicates the
         operational state of the destination."
    ::= { tFilterRPlcyBindingDestEntry 5 }

tFltrGreTunTempTableLastChg      OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempTableLastChg indicates the sysUpTime at the
         time of the last modification of tFltrGreTunTempTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 99 }

tFltrGreTunTempTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrGreTunTempEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrGreTunTempTable contains an entry for each GRE tunnel
         template"
    ::= { tFilterObjects 100 }

tFltrGreTunTempEntry             OBJECT-TYPE
    SYNTAX      TFltrGreTunTempEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFltrGreTunTempTable."
    INDEX       { IMPLIED tFltrGreTunTempName }
    ::= { tFltrGreTunTempTable 1 }

TFltrGreTunTempEntry             ::= SEQUENCE
{
    tFltrGreTunTempName              TNamedItem,
    tFltrGreTunTempRowStatus         RowStatus,
    tFltrGreTunTempLastChanged       TimeStamp,
    tFltrGreTunTempDescription       TItemDescription,
    tFltrGreTunTempIpv4SrcAddr       IpAddress,
    tFltrGreTunTempIpv4GreKeyIfIndex TruthValue,
    tFltrGreTunTempIpv4SkipTllDecr   TruthValue,
    tFltrGreTunTempIpv6SrcAddr       InetAddressIPv6,
    tFltrGreTunTempIpv6GreKeyIfIndex TruthValue,
    tFltrGreTunTempIpv6SkipHopDecr   TruthValue
}

tFltrGreTunTempName              OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempName specifies the name given to this
         template."
    ::= { tFltrGreTunTempEntry 1 }

tFltrGreTunTempRowStatus         OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempRowStatus specifies the status of this row."
    ::= { tFltrGreTunTempEntry 2 }

tFltrGreTunTempLastChanged       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempLastChanged indicates the sysUpTime at the
         time of the last modification of this row.

         If no changes were made to the row since the last re-initialization of
         the local network management subsystem, then this object contains the
         value zero."
    ::= { tFltrGreTunTempEntry 3 }

tFltrGreTunTempDescription       OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempDescription specifies a description for this
         row."
    DEFVAL      { ''H }
    ::= { tFltrGreTunTempEntry 4 }

tFltrGreTunTempIpv4SrcAddr       OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv4SrcAddr specifies a source IP address of
         the GRE encapsulated packet."
    DEFVAL      { '00000000'H }
    ::= { tFltrGreTunTempEntry 5 }

tFltrGreTunTempIpv4GreKeyIfIndex OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv4GreKeyIfIndex is option to include a key
         value in the GRE header of ifIndex of the ingress interface."
    DEFVAL      { false }
    ::= { tFltrGreTunTempEntry 6 }

tFltrGreTunTempIpv4SkipTllDecr   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv4SkipTllDecr is option to not decrement
         the TTL of the received packet."
    DEFVAL      { false }
    ::= { tFltrGreTunTempEntry 7 }

tFltrGreTunTempIpv6SrcAddr       OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv6SrcAddr specifies a source IP address of
         the GRE encapsulated packet."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tFltrGreTunTempEntry 9 }

tFltrGreTunTempIpv6GreKeyIfIndex OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv6GreKeyIfIndex is option to include a key
         value in the GRE header of ifIndex of the ingress interface."
    DEFVAL      { false }
    ::= { tFltrGreTunTempEntry 10 }

tFltrGreTunTempIpv6SkipHopDecr   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv6SkipHopDecr is option to not decrement
         the hop of the received packet."
    DEFVAL      { false }
    ::= { tFltrGreTunTempEntry 11 }

tFltrGreTunTempIpv4DstTblLstChg  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv4DstTblLstChg indicates the sysUpTime at
         the time of the last modification of tFltrGreTunTempIpv4DstTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 101 }

tFltrGreTunTempIpv4DstTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrGreTunTempIpv4DstEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrGreTunTempIpv4DstTable contains destinations for GRE
         tunnel template"
    ::= { tFilterObjects 102 }

tFltrGreTunTempIpv4DstEntry      OBJECT-TYPE
    SYNTAX      TFltrGreTunTempIpv4DstEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFltrGreTunTempIpv4DstTable."
    INDEX       {
        tFltrGreTunTempName,
        tFltrGreTunTempIpv4DstAddr
    }
    ::= { tFltrGreTunTempIpv4DstTable 1 }

TFltrGreTunTempIpv4DstEntry      ::= SEQUENCE
{
    tFltrGreTunTempIpv4DstAddr       IpAddress,
    tFltrGreTunTempIpv4DstRowStatus  RowStatus,
    tFltrGreTunTempIpv4DstLstChg     TimeStamp
}

tFltrGreTunTempIpv4DstAddr       OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv4DstAddr specifies a destination IP
         address of the GRE encapsulated packet."
    ::= { tFltrGreTunTempIpv4DstEntry 1 }

tFltrGreTunTempIpv4DstRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv4DstRowStatus specifies the status of
         this row."
    ::= { tFltrGreTunTempIpv4DstEntry 2 }

tFltrGreTunTempIpv4DstLstChg     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv4DstLstChg indicates the sysUpTime at the
         time of the last modification of this row.

         If no changes were made to the row since the last re-initialization of
         the local network management subsystem, then this object contains the
         value zero."
    ::= { tFltrGreTunTempIpv4DstEntry 3 }

tFltrPrefListPrefExclTblLstChg   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrPrefListPrefExclTblLstChg indicates the sysUpTime at
         the time of the last modification of tFltrPrefListPrefExclTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 103 }

tFltrPrefListPrefExclTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrPrefListPrefExclEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrPrefListPrefExclTable contains information pertaining
         to explicitly created excluded prefixes in any prefix list defined in
         the filter area."
    ::= { tFilterObjects 104 }

tFltrPrefListPrefExclEntry       OBJECT-TYPE
    SYNTAX      TFltrPrefListPrefExclEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFltrPrefListPrefExclTable."
    INDEX       {
        tFilterPrefixListType,
        tFilterPrefixListName,
        tFltrPrefListPrefExclPrefType,
        tFltrPrefListPrefExclPref,
        tFltrPrefListPrefExclPrefLen
    }
    ::= { tFltrPrefListPrefExclTable 1 }

TFltrPrefListPrefExclEntry       ::= SEQUENCE
{
    tFltrPrefListPrefExclPrefType    TmnxAddressAndPrefixType,
    tFltrPrefListPrefExclPref        TmnxAddressAndPrefixAddress,
    tFltrPrefListPrefExclPrefLen     TmnxAddressAndPrefixPrefix,
    tFltrPrefListPrefExclRowStatus   RowStatus,
    tFltrPrefListPrefExclLastChg     TimeStamp
}

tFltrPrefListPrefExclPrefType    OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrPrefListPrefExclPrefType specifies whether the
         excluded prefix specified in tFltrPrefListPrefExclEntry is an IPv4 or
         IPv6 one.

         The value of tFltrPrefListPrefExclPrefType must match the value of the
         object tFilterPrefixListType."
    ::= { tFltrPrefListPrefExclEntry 1 }

tFltrPrefListPrefExclPref        OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixAddress (SIZE (4|16))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFltrPrefListPrefExclPref specifies the excluded IPv4 or
         IPv6 prefix of this prefix list entry."
    ::= { tFltrPrefListPrefExclEntry 2 }

tFltrPrefListPrefExclPrefLen     OBJECT-TYPE
    SYNTAX      TmnxAddressAndPrefixPrefix
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of tFltrPrefListPrefExclPrefLen specifies the length of the
         excluded IPv4 or IPv6 prefix of this prefix list entry."
    ::= { tFltrPrefListPrefExclEntry 3 }

tFltrPrefListPrefExclRowStatus   OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrPrefListPrefExclRowStatus specifies the status of this
         row."
    ::= { tFltrPrefListPrefExclEntry 4 }

tFltrPrefListPrefExclLastChg     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPrefListPrefExclLastChg indicates the
         sysUpTime at the time of the last modification of
         tFltrPrefListPrefExclEntry.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFltrPrefListPrefExclEntry 5 }

fltrMdAutoIdGroup                OBJECT IDENTIFIER ::= { tFilterObjects 105 }

fltrMdAutoIdFilterRangeStart     OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The fltrMdAutoIdFilterRangeStart specifies start of the ip-filter
         identifier range to be used in model-driven CLI."
    DEFVAL      { 0 }
    ::= { fltrMdAutoIdGroup 1 }

fltrMdAutoIdFilterRangeEnd       OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The fltrMdAutoIdFilterRangeEnd specifies the end of the filter
         identifier range to be used in model-driven CLI."
    DEFVAL      { 0 }
    ::= { fltrMdAutoIdGroup 2 }

fltrMdAutoIdIPv4FilterCount      OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The fltrMdAutoIdIPv4FilterCount indicates Ipv4 filter identifiers
         in-use in model-driven CLI."
    ::= { fltrMdAutoIdGroup 3 }

fltrMdAutoIdIPv6FilterCount      OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The fltrMdAutoIdIPv6FilterCount indicates Ipv6 filter identifiers
         in-use in model-driven CLI."
    ::= { fltrMdAutoIdGroup 4 }

fltrMdAutoIdMacFilterCount       OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The fltrMdAutoIdMacFilterCount indicates Mac filter identifiers in-use
         in model-driven CLI."
    ::= { fltrMdAutoIdGroup 5 }

fltrMdAutoIdIPv4ExceptionCount   OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The fltrMdAutoIdIPv4ExceptionCount indicates Ipv4 exception filter
         identifiers in-use in model-driven CLI."
    ::= { fltrMdAutoIdGroup 6 }

fltrMdAutoIdIPv6ExceptionCount   OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The fltrMdAutoIdIPv6ExceptionCount indicates Ipv6 exception filter
         identifiers in-use in model-driven CLI."
    ::= { fltrMdAutoIdGroup 7 }

tIPv6ExceptionTable              OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIPv6ExceptionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tIPv6ExceptionTable contains all of the IPv6 exceptions
         configured on this system."
    ::= { tFilterObjects 106 }

tIPv6ExceptionEntry              OBJECT-TYPE
    SYNTAX      TIPv6ExceptionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular IPv6 exception entry. Entries are
         created and destroyed by SNMP operations on the object
         tIPv6ExceptionRowStatus."
    INDEX       { tIPv6ExceptionId }
    ::= { tIPv6ExceptionTable 1 }

TIPv6ExceptionEntry              ::= SEQUENCE
{
    tIPv6ExceptionId                 TAnyFilterID,
    tIPv6ExceptionRowStatus          RowStatus,
    tIPv6ExceptionDescription        TItemDescription,
    tIPv6ExceptionName               TLNamedItemOrEmpty
}

tIPv6ExceptionId                 OBJECT-TYPE
    SYNTAX      TAnyFilterID (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExceptionId uniquely identifies an IPv6
         exception."
    ::= { tIPv6ExceptionEntry 1 }

tIPv6ExceptionRowStatus          OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExceptionRowStatus specifies the status
         of the IPv6 exception. The object allows entries to be created and
         deleted in the tIPv6ExceptionTable."
    ::= { tIPv6ExceptionEntry 2 }

tIPv6ExceptionDescription        OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExceptionDescription specifies a
         user-provided description for this IPv6 exception."
    DEFVAL      { ''H }
    ::= { tIPv6ExceptionEntry 3 }

tIPv6ExceptionName               OBJECT-TYPE
    SYNTAX      TLNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExceptionName specifies the name to
         associate with this IPv6 exception."
    DEFVAL      { ''H }
    ::= { tIPv6ExceptionEntry 4 }

tIPv6ExceptionNameTable          OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIPv6ExceptionNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains IPv6 exception name information."
    ::= { tFilterObjects 107 }

tIPv6ExceptionNameEntry          OBJECT-TYPE
    SYNTAX      TIPv6ExceptionNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a specific IPv6 exception name. Entries are created
         and deleted automatically by the system based upon the
         tIPv6ExceptionName objects in the tIPv6ExceptionTable."
    INDEX       { tIPv6ExceptionName }
    ::= { tIPv6ExceptionNameTable 1 }

TIPv6ExceptionNameEntry          ::= SEQUENCE
{ tIPv6ExceptionNameId             TAnyFilterID }

tIPv6ExceptionNameId             OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExceptionNameId indicates the IPv6
         exception associated with this name."
    ::= { tIPv6ExceptionNameEntry 1 }

tIPv6ExceptionParamsTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF TIPv6ExceptionParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of all IPv6 exception match entries for all IPv6 exceptions."
    ::= { tFilterObjects 108 }

tIPv6ExceptionParamsEntry        OBJECT-TYPE
    SYNTAX      TIPv6ExceptionParamsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular IPv6 exception match entry. Every IPv6
         exception can have zero or more IPv6 exception match entries.

         Each match constitutes some criteria by which an unencrypted IPv6
         packet will be accepted at the interface to which the IPv6 exception
         is applied.

         Entries are created/deleted by the user."
    INDEX       {
        tIPv6ExceptionId,
        tIPv6ExcParamsIndex
    }
    ::= { tIPv6ExceptionParamsTable 1 }

TIPv6ExceptionParamsEntry        ::= SEQUENCE
{
    tIPv6ExcParamsIndex              TEntryId,
    tIPv6ExcParamsRowStatus          RowStatus,
    tIPv6ExcParamsDescription        TItemDescription,
    tIPv6ExcParamsNextHeader         TIpProtocol,
    tIPv6ExcParamsSrcIpAddr          InetAddressIPv6,
    tIPv6ExcParamsSrcIpMask          InetAddressPrefixLength,
    tIPv6ExcParamsSrcIpFullMask      InetAddressIPv6,
    tIPv6ExcParamsSrcIpPrefixList    TNamedItemOrEmpty,
    tIPv6ExcParamsDstIpAddr          InetAddressIPv6,
    tIPv6ExcParamsDstIpMask          InetAddressPrefixLength,
    tIPv6ExcParamsDstIpFullMask      InetAddressIPv6,
    tIPv6ExcParamsDstIpPrefixList    TNamedItemOrEmpty,
    tIPv6ExcParamsSourcePortValue1   TTcpUdpPort,
    tIPv6ExcParamsSourcePortValue2   TTcpUdpPort,
    tIPv6ExcParamsSourcePortOperator TOperator,
    tIPv6ExcParamsSourcePortList     TNamedItemOrEmpty,
    tIPv6ExcParamsDestPortValue1     TTcpUdpPort,
    tIPv6ExcParamsDestPortValue2     TTcpUdpPort,
    tIPv6ExcParamsDestPortOperator   TOperator,
    tIPv6ExcParamsDestPortList       TNamedItemOrEmpty,
    tIPv6ExcParamsPortSelector       TFltrPortSelector,
    tIPv6ExcParamsIcmpCode           TIcmpCodeOrNone,
    tIPv6ExcParamsIcmpType           TIcmpTypeOrNone,
    tIPv6ExcParamsIngressHitCount    Counter64,
    tIPv6ExcParamsEgressHitCount     Counter64,
    tIPv6ExcParamsIngrHitByteCount   Counter64,
    tIPv6ExcParamsEgrHitByteCount    Counter64
}

tIPv6ExcParamsIndex              OBJECT-TYPE
    SYNTAX      TEntryId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This is the index for the match entry. Each IPv6 exception can have
         multiple match entries."
    ::= { tIPv6ExceptionParamsEntry 1 }

tIPv6ExcParamsRowStatus          OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows match entries to be created and deleted in the
         tIPv6ExceptionParamsTable."
    ::= { tIPv6ExceptionParamsEntry 2 }

tIPv6ExcParamsDescription        OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsDescription specifies a
         user-provided description for this IPv6 exception match entry."
    DEFVAL      { ''H }
    ::= { tIPv6ExceptionParamsEntry 3 }

tIPv6ExcParamsNextHeader         OBJECT-TYPE
    SYNTAX      TIpProtocol
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsNextHeader specifies the
         IPv6 next header to match.  A value of -1 disables matching the IPv6
         next header."
    DEFVAL      { -1 }
    ::= { tIPv6ExceptionParamsEntry 4 }

tIPv6ExcParamsSrcIpAddr          OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsSrcIpAddr specifies the IPv6
         address to match the source IPv6 address of the packet."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPv6ExceptionParamsEntry 5 }

tIPv6ExcParamsSrcIpMask          OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..128)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the value of the object tIPv6ExcParamsSrcIpMask
         specifies the IPv6 prefix length value for the IPv6 exception entry.
         The mask generated from the prefix length value is ANDed with the
         received source IPv6 address to match the tIPv6ExcParamsSrcIpAddr.

         If the value of tIPv6ExcParamsSrcIpMask is 0, and the value of
         tIPv6ExcParamsSrcIpFullMask is non zero then the value of
         tIPv6ExcParamsSrcIpFullMask is used as a mask.

         If the value of tIPv6ExcParamsSrcIpMask is non zero, it will be equal
         to the mask expressed in the object tIPv6ExcParamsSrcIpFullMask.

         If both tIPv6ExcParamsSrcIpMask and tIPv6ExcParamsSrcIpFullMask are
         set to 0, no matching is done on the source IPv6 address.

         If a value is specified for this object, then the value of the object
         tIPv6ExcParamsSrcIpFullMask will be set to reflect this same mask."
    DEFVAL      { 0 }
    ::= { tIPv6ExceptionParamsEntry 6 }

tIPv6ExcParamsSrcIpFullMask      OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the value of the object
         tIPv6ExcParamsSrcIpFullMask specifies the IPv6 Mask value for this
         IPv6 exception entry. The mask is ANDed with the received source IPv6
         address to match the tIPv6ExcParamsSrcIpAddr.

         If the value of tIPv6ExcParamsSrcIpMask is 0, and the value of
         tIPv6ExcParamsSrcIpFullMask is non zero then the value of
         tIPv6ExcParamsSrcIpFullMask is used as a mask.

         If the value of tIPv6ExcParamsSrcIpMask is non zero, it will be equal
         to the mask expressed in the object tIPv6ExcParamsSrcIpFullMask.

         If both tIPv6ExcParamsSrcIpMask and tIPv6ExcParamsSrcIpFullMask are
         set to 0, no matching is done on the Source IPv6 address.

         If a regular mask is specified for tIPv6ExcParamsSrcIpFullMask then
         the value of tIPv6ExcParamsSrcIpMask will be changed to reflect this
         value."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPv6ExceptionParamsEntry 7 }

tIPv6ExcParamsSrcIpPrefixList    OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsSrcIpPrefixList specifies the
         IPv6 prefix list used as match criterion for the source IPv6 address.

         The value specified for this object must correspond to a prefix list
         defined in tFilterPrefixListTable.

         If the value of this object is empty then the values of the objects
         tIPv6ExcParamsSrcIpAddr and tIPv6ExcParamsSrcIpMask are used as source
         IPv6 address match criterion.

         When this object is set to a non-empty value then the objects
         tIPv6ExcParamsSrcIpAddr and tIPv6ExcParamsSrcIpMask are reset to their
         default values by the system.

         Vice versa, when a new (non-default) value is provided for the objects
         tIPv6ExcParamsSrcIpAddr and tIPv6ExcParamsSrcIpMask then this object
         is reset to its default (empty) value by the system."
    DEFVAL      { ''H }
    ::= { tIPv6ExceptionParamsEntry 8 }

tIPv6ExcParamsDstIpAddr          OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsDstIpAddr specifies the IPv6
         address to match the destination IPv6 address of the packet."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPv6ExceptionParamsEntry 9 }

tIPv6ExcParamsDstIpMask          OBJECT-TYPE
    SYNTAX      InetAddressPrefixLength (0..128)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the value of the object tIPv6ExcParamsDstIpMask
         specifies the IPv6 prefix length value for this IPv6 exception entry.
         The mask generated from the prefix length value is ANDed with the
         received destination IPv6 address to match the
         tIPv6ExcParamsDstIpAddr.

         If the value of tIPv6ExcParamsDstIpMask is 0, and the value of
         tIPv6ExcParamsDstIpFullMask is non zero then the value of
         tIPv6ExcParamsDstIpFullMask is used as a mask.

         If the value of tIPv6ExcParamsDstIpMask is non zero, it will be equal
         to the mask expressed in the object tIPv6ExcParamsDstIpFullMask.

         If both tIPv6ExcParamsDstIpMask and tIPv6ExcParamsDstIpFullMask are
         set to 0, no matching is done on the destination IPv6 address.

         If a value is specified for this object, then the value of the object
         tIPv6ExcParamsDstIpFullMask will be set to reflect this same mask."
    DEFVAL      { 0 }
    ::= { tIPv6ExceptionParamsEntry 10 }

tIPv6ExcParamsDstIpFullMask      OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If different from 0, the value of the object
         tIPv6ExcParamsDstIpFullMask specifies the IPv6 Mask value for this
         policy IPv6 Filter entry. The mask is ANDed with the received
         destination IPv6 address to match the tIPv6ExcParamsDstIpAddr.

         If the value of tIPv6ExcParamsDstIpMask is 0, and the value of
         tIPv6ExcParamsDstIpFullMask is non zero then the value of
         tIPv6ExcParamsDstIpFullMask is used as a mask.

         If the value of tIPv6ExcParamsDstIpMask is non zero, it will be equal
         to the mask expressed in the object tIPv6ExcParamsDstIpFullMask.

         If both tIPv6ExcParamsDstIpMask and tIPv6ExcParamsDstIpFullMask are
         set to 0, no matching is done on the destination IPv6 address.

         If a regular mask is specified for tIPv6ExcParamsDstIpFullMask then
         the value of tIPv6ExcParamsDstIpMask will be changed to reflect this
         value."
    DEFVAL      { '00000000000000000000000000000000'H }
    ::= { tIPv6ExceptionParamsEntry 11 }

tIPv6ExcParamsDstIpPrefixList    OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsDstIpPrefixList specifies the
         IPv6 prefix list used as match criterion for the destination IPv6
         address.

         The value specified for this object must correspond to a prefix list
         defined in tFilterPrefixListTable.

         If the value of this object is empty then the values of the objects
         tIPv6ExcParamsDstIpAddr and tIPv6ExcParamsDstIpMask are used as
         destination IPv6 address match criterion.

         When this object is set to a non-empty value then the objects
         tIPv6ExcParamsDstIpAddr and tIPv6ExcParamsDstIpMask are reset to their
         default values by the system.

         Vice versa, when a new (non-default) value is provided for the objects
         tIPv6ExcParamsDstIpAddr and tIPv6ExcParamsDstIpMask then this object
         is reset to its default (empty) value by the system."
    DEFVAL      { ''H }
    ::= { tIPv6ExceptionParamsEntry 12 }

tIPv6ExcParamsSourcePortValue1   OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsSourcePortValue1 specifies a
         protocol port value. The value of this object is used when matching
         protocol source ports, as per the description for
         tIPv6ExcParamsSourcePortOperator."
    DEFVAL      { 0 }
    ::= { tIPv6ExceptionParamsEntry 13 }

tIPv6ExcParamsSourcePortValue2   OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsSourcePortValue2 specifies a
         second protocol port value. The value of this object is used when
         matching protocol source ports, as per the description for
         tIPv6ExcParamsSourcePortOperator."
    DEFVAL      { 0 }
    ::= { tIPv6ExceptionParamsEntry 14 }

tIPv6ExcParamsSourcePortOperator OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsSourcePortOperator specifies the
         manner in which tIPv6ExcParamsSourcePortValue1 and
         tIPv6ExcParamsSourcePortValue2 are to be used to match protocol source
         ports."
    DEFVAL      { none }
    ::= { tIPv6ExceptionParamsEntry 15 }

tIPv6ExcParamsSourcePortList     OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsSourcePortList specifies the
         port-list used as match criterion for the protocol source port.

         The value specified for this object must correspond to a port-list
         defined in tFilterPortListTable.

         If the value of this object is empty then the values of the objects
         tIPv6ExcParamsSourcePortValue1, tIPv6ExcParamsSourcePortValue2, and
         tIPv6ExcParamsSourcePortOperator are used as source port match
         criterion.

         When this object is set to a non-empty value then the objects
         tIPv6ExcParamsSourcePortValue1, tIPv6ExcParamsSourcePortValue2, and
         tIPv6ExcParamsSourcePortOperator are reset to their default values by
         the system.

         Vice versa, when a new (non-default) value is provided for one of the
         objects tIPv6ExcParamsSourcePortValue1,
         tIPv6ExcParamsSourcePortValue2, or tIPv6ExcParamsSourcePortOperator
         then tIPv6ExcParamsSourcePortList is reset to its default (empty)
         value by the system.

         Setting any one of the objects tIPv6ExcParamsSourcePortValue1,
         tIPv6ExcParamsSourcePortValue2, or tIPv6ExcParamsSourcePortOperator to
         a non-default value in combination with a non-default value for the
         object tIPv6ExcParamsSourcePortList is rejected by the system."
    DEFVAL      { ''H }
    ::= { tIPv6ExceptionParamsEntry 16 }

tIPv6ExcParamsDestPortValue1     OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsDestPortValue1 specifies a
         protocol port value. The value of this object is used when matching
         protocol destination ports, as per the description for
         tIPv6ExcParamsDestPortOperator."
    DEFVAL      { 0 }
    ::= { tIPv6ExceptionParamsEntry 17 }

tIPv6ExcParamsDestPortValue2     OBJECT-TYPE
    SYNTAX      TTcpUdpPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsDestPortValue2 specifies a
         second protocol port value. The value of this object is used when
         matching protocol destination ports, as per the description for
         tIPv6ExcParamsDestPortOperator."
    DEFVAL      { 0 }
    ::= { tIPv6ExceptionParamsEntry 18 }

tIPv6ExcParamsDestPortOperator   OBJECT-TYPE
    SYNTAX      TOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsDestPortOperator specifies the
         manner in which tIPv6ExcParamsDestPortValue1 and
         tIPv6ExcParamsDestPortValue2 are to be used to match protocol
         destination ports."
    DEFVAL      { none }
    ::= { tIPv6ExceptionParamsEntry 19 }

tIPv6ExcParamsDestPortList       OBJECT-TYPE
    SYNTAX      TNamedItemOrEmpty
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsDestPortList specifies the
         port-list used as match criterion for the protocol destination port.

         The value specified for this object must correspond to a port-list
         defined in tFilterPortListTable.

         If the value of this object is empty then the values of the objects
         tIPv6ExcParamsDestPortValue1, tIPv6ExcParamsDestPortValue2, and
         tIPv6ExcParamsDestPortOperator are used as destination port match
         criterion.

         When this object is set to a non-empty value then the objects
         tIPv6ExcParamsDestPortValue1, tIPv6ExcParamsDestPortValue2, and
         tIPv6ExcParamsDestPortOperator are reset to their default values by
         the system.

         Vice versa, when a new (non-default) value is provided for one of the
         objects tIPv6ExcParamsDestPortValue1, tIPv6ExcParamsDestPortValue2, or
         tIPv6ExcParamsDestPortOperator then tIPv6ExcParamsDestPortList is
         reset to its default (empty) value by the system.

         Setting any one of the objects tIPv6ExcParamsDestPortValue1,
         tIPv6ExcParamsDestPortValue2, or tIPv6ExcParamsDestPortOperator to a
         non-default value in combination with a non-default value for the
         object tIPv6ExcParamsDestPortList is rejected by the system."
    DEFVAL      { ''H }
    ::= { tIPv6ExceptionParamsEntry 20 }

tIPv6ExcParamsPortSelector       OBJECT-TYPE
    SYNTAX      TFltrPortSelector
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsPortSelector specifies how the
         source port objects (tIPv6ExcParamsSourcePortValue1,
         tIPv6ExcParamsSourcePortValue2, tIPv6ExcParamsSourcePortOperator,
         tIPv6ExcParamsSourcePortList) and destination port objects
         (tIPv6ExcParamsDestPortValue1, tIPv6ExcParamsDestPortValue2,
         tIPv6ExcParamsDestPortOperator, tIPv6ExcParamsDestPortList) are
         combined to form the filter match criterion. See description of
         TFltrPortSelector."
    DEFVAL      { and-port }
    ::= { tIPv6ExceptionParamsEntry 21 }

tIPv6ExcParamsIcmpCode           OBJECT-TYPE
    SYNTAX      TIcmpCodeOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsIcmpCode specifies the ICMP code
         to be matched.

         The value -1 means ICMP code matching is not enabled."
    DEFVAL      { -1 }
    ::= { tIPv6ExceptionParamsEntry 22 }

tIPv6ExcParamsIcmpType           OBJECT-TYPE
    SYNTAX      TIcmpTypeOrNone
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsIcmpType specifies the ICMP type
         to be matched.

         The value -1 means ICMP type matching is not enabled."
    DEFVAL      { -1 }
    ::= { tIPv6ExceptionParamsEntry 23 }

tIPv6ExcParamsIngressHitCount    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsIngressHitCount indicates the
         number of times an ingress packet matched this entry."
    ::= { tIPv6ExceptionParamsEntry 24 }

tIPv6ExcParamsEgressHitCount     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsEgressHitCount indicates the
         number of times an egress packet matched this entry."
    ::= { tIPv6ExceptionParamsEntry 25 }

tIPv6ExcParamsIngrHitByteCount   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsIngrHitByteCount indicates the
         number of bytes of all ingress packets that matched this entry."
    ::= { tIPv6ExceptionParamsEntry 26 }

tIPv6ExcParamsEgrHitByteCount    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tIPv6ExcParamsEgrHitByteCount indicates the
         number of bytes of all egress packets that matched this entry."
    ::= { tIPv6ExceptionParamsEntry 27 }

tFltrProtocolListTableLstChng    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrProtocolListTableLstChng indicates the sysUpTime at
         the time of the last modification of tFltrProtocolListTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 109 }

tFltrProtocolListTable           OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrProtocolListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrProtocolListTable contains an entry for each Protocol
         list defined in the filter area."
    ::= { tFilterObjects 110 }

tFltrProtocolListEntry           OBJECT-TYPE
    SYNTAX      TFltrProtocolListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFltrProtocolListTable."
    INDEX       { IMPLIED tFltrProtocolListName }
    ::= { tFltrProtocolListTable 1 }

TFltrProtocolListEntry           ::= SEQUENCE
{
    tFltrProtocolListName            TNamedItem,
    tFltrProtocolListRowStatus       RowStatus,
    tFltrProtocolListLastChanged     TimeStamp,
    tFltrProtocolListDescription     TItemDescription
}

tFltrProtocolListName            OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrProtocolListName specifies the name of this Protocol
         list."
    ::= { tFltrProtocolListEntry 1 }

tFltrProtocolListRowStatus       OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrProtocolListRowStatus specifies the status of this
         row."
    ::= { tFltrProtocolListEntry 2 }

tFltrProtocolListLastChanged     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrProtocolListLastChanged indicates the sysUpTime at the
         time of the last modification of this row.

         If no changes were made to the row since the last re-initialization of
         the local network management subsystem, then this object contains the
         value zero."
    ::= { tFltrProtocolListEntry 3 }

tFltrProtocolListDescription     OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrProtocolListDescription specifies a description for
         this row."
    DEFVAL      { ''H }
    ::= { tFltrProtocolListEntry 4 }

tFltrProtocolListItemTblLstChg   OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrProtocolListItemTblLstChg indicates the sysUpTime at
         the time of the last modification of tFltrProtocolListItemTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 111 }

tFltrProtocolListItemTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrProtocolListItemEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrProtocolListItemTable contains an entry for each
         Protocol defined in any Protocol list defined in the filter area."
    ::= { tFilterObjects 112 }

tFltrProtocolListItemEntry       OBJECT-TYPE
    SYNTAX      TFltrProtocolListItemEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Specifies an entry in the tFltrProtocolListItemTable."
    INDEX       {
        tFltrProtocolListName,
        tFltrProtocolListItemProtocol
    }
    ::= { tFltrProtocolListItemTable 1 }

TFltrProtocolListItemEntry       ::= SEQUENCE
{
    tFltrProtocolListItemProtocol    TIpProtocolNumber,
    tFltrProtocolListItemRowStatus   RowStatus
}

tFltrProtocolListItemProtocol    OBJECT-TYPE
    SYNTAX      TIpProtocolNumber
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrProtocolListItemProtocol specifies a
         value to be be matched against IP protocol/IPv6 next-header value of
         the IP packet."
    ::= { tFltrProtocolListItemEntry 1 }

tFltrProtocolListItemRowStatus   OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrProtocolListItemRowStatus specifies the
         status of this row."
    ::= { tFltrProtocolListItemEntry 2 }

tFltrGreTunTempIpv6DstTblLstChg  OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv6DstTblLstChg indicates the sysUpTime at
         the time of the last modification of tFltrGreTunTempIpv6DstTable.

         If no changes were made to the entry since the last re-initialization
         of the local network management subsystem, then this object contains a
         zero value."
    ::= { tFilterObjects 113 }

tFltrGreTunTempIpv6DstTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrGreTunTempIpv6DstEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrGreTunTempIpv6DstTable contains ipv6 destinations for
         GRE tunnel template"
    ::= { tFilterObjects 114 }

tFltrGreTunTempIpv6DstEntry      OBJECT-TYPE
    SYNTAX      TFltrGreTunTempIpv6DstEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFltrGreTunTempIpv6DstTable."
    INDEX       {
        tFltrGreTunTempName,
        tFltrGreTunTempIpv6DstAddr
    }
    ::= { tFltrGreTunTempIpv6DstTable 1 }

TFltrGreTunTempIpv6DstEntry      ::= SEQUENCE
{
    tFltrGreTunTempIpv6DstAddr       InetAddressIPv6,
    tFltrGreTunTempIpv6DstRowStatus  RowStatus,
    tFltrGreTunTempIpv6DstLstChg     TimeStamp
}

tFltrGreTunTempIpv6DstAddr       OBJECT-TYPE
    SYNTAX      InetAddressIPv6
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv6DstAddr specifies a destination IPv6
         address of the GRE encapsulated packet."
    ::= { tFltrGreTunTempIpv6DstEntry 1 }

tFltrGreTunTempIpv6DstRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv6DstRowStatus specifies the status of
         this row."
    ::= { tFltrGreTunTempIpv6DstEntry 2 }

tFltrGreTunTempIpv6DstLstChg     OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrGreTunTempIpv6DstLstChg indicates the sysUpTime at the
         time of the last modification of this row.

         If no changes were made to the row since the last re-initialization of
         the local network management subsystem, then this object contains the
         value zero."
    ::= { tFltrGreTunTempIpv6DstEntry 3 }

tFltrPktLenListTblLastChg        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrPktLenListTblLastChg indicates the sysUpTime at the
         time of the last modification of tFltrPktLenListTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 115 }

tFltrPktLenListTable             OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrPktLenListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrPktLenListTable contains an entry (AKA row) for each
         port list defined in the filter area."
    ::= { tFilterObjects 116 }

tFltrPktLenListEntry             OBJECT-TYPE
    SYNTAX      TFltrPktLenListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of the tFltrPktLenListTable."
    INDEX       {
        tFltrPktLenListType,
        IMPLIED tFltrPktLenListName
    }
    ::= { tFltrPktLenListTable 1 }

TFltrPktLenListEntry             ::= SEQUENCE
{
    tFltrPktLenListType              TFltrPktLenListType,
    tFltrPktLenListName              TNamedItem,
    tFltrPktLenListRowStatus         RowStatus,
    tFltrPktLenListLastChanged       TimeStamp,
    tFltrPktLenListDescription       TItemDescription
}

tFltrPktLenListType              OBJECT-TYPE
    SYNTAX      TFltrPktLenListType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrPktLenListType specifies the type of this packet
         length list."
    ::= { tFltrPktLenListEntry 1 }

tFltrPktLenListName              OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrPktLenListName specifies the name given to this packet
         length list."
    ::= { tFltrPktLenListEntry 2 }

tFltrPktLenListRowStatus         OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrPktLenListRowStatus specifies the status of this row."
    ::= { tFltrPktLenListEntry 3 }

tFltrPktLenListLastChanged       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrPktLenListLastChanged indicates the sysUpTime at the
         time of the last modification of this row.

         If no changes were made to the row since the last re-initialization of
         the local network management subsystem, then this object contains the
         value zero."
    ::= { tFltrPktLenListEntry 4 }

tFltrPktLenListDescription       OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrPktLenListDescription specifies a description for this
         packet length list."
    DEFVAL      { ''H }
    ::= { tFltrPktLenListEntry 5 }

tFltrPktLenListItemTblLastChg    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrPktLenListItemTblLastChg indicates the sysUpTime at
         the time of the last modification of tFltrPktLenListItemTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 117 }

tFltrPktLenListItemTable         OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrPktLenListItemEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrPktLenListItemTable contains an entry for each port
         defined in any port list defined in the filter area."
    ::= { tFilterObjects 118 }

tFltrPktLenListItemEntry         OBJECT-TYPE
    SYNTAX      TFltrPktLenListItemEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Specifies an entry in the tFltrPktLenListItemTable. Intervals
         specified by values tFltrPktLenListItemLow and tFltrPktLenListItemHigh
         must not overlap for any two entries of the same packet length list."
    INDEX       {
        tFltrPktLenListType,
        tFltrPktLenListName,
        tFltrPktLenListItemLow,
        tFltrPktLenListItemHigh
    }
    ::= { tFltrPktLenListItemTable 1 }

TFltrPktLenListItemEntry         ::= SEQUENCE
{
    tFltrPktLenListItemLow           TIPvXFilterPktLen,
    tFltrPktLenListItemHigh          TIPvXFilterPktLen,
    tFltrPktLenListItemRowStatus     RowStatus
}

tFltrPktLenListItemLow           OBJECT-TYPE
    SYNTAX      TIPvXFilterPktLen
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This object specifies the lower value for the packet length range. A
         value assigned to this object must be lower than or equal to the value
         assigned to the corresponding object tFltrPktLenListItemHigh. When the
         tFltrPktLenListType is set to 'ipv4', the tFltrPktLenListItemLow can
         contain a value from 0 to 65535. When it is set to 'ipv6' the allowed
         value range is from 40 to 65575."
    ::= { tFltrPktLenListItemEntry 1 }

tFltrPktLenListItemHigh          OBJECT-TYPE
    SYNTAX      TIPvXFilterPktLen
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This object specifies the higher value for packet length range. A
         value assigned to this object must be greater than or equal to the
         value assigned to the corresponding object tFltrPktLenListItemLow.
         When the tFltrPktLenListType is set to 'ipv4', the
         tFltrPktLenListItemHigh can contain a value from 0 to 65535. When it
         is set to 'ipv6' the allowed value range is from 40 to 65575."
    ::= { tFltrPktLenListItemEntry 2 }

tFltrPktLenListItemRowStatus     OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrPktLenListItemRowStatus specifies the status of this
         row."
    ::= { tFltrPktLenListItemEntry 3 }

tFltrPolicerTblLastChg           OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrPolicerTblLastChg indicates the sysUpTime at the time
         of the last modification of tFltrPolicerTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 119 }

tFltrPolicerTable                OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrPolicerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrPolicerTable contains an entry  for each policer
         defined in the filter area."
    ::= { tFilterObjects 120 }

tFltrPolicerEntry                OBJECT-TYPE
    SYNTAX      TFltrPolicerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of the tFltrPolicerTable."
    INDEX       { IMPLIED tFltrPolicerName }
    ::= { tFltrPolicerTable 1 }

TFltrPolicerEntry                ::= SEQUENCE
{
    tFltrPolicerName                 TNamedItem,
    tFltrPolicerRowStatus            RowStatus,
    tFltrPolicerLastChanged          TimeStamp,
    tFltrPolicerDescription          TItemDescription,
    tFltrPolicerPIR                  TFilterPolicerPIR,
    tFltrPolicerPPSPIR               TFilterPolicerPPSPIR,
    tFltrPolicerMBS                  TPolicerBurstSizeBytes,
    tFltrPolicerScope                TFltrPolicerScope
}

tFltrPolicerName                 OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrPolicerName specifies the name given to this policer."
    ::= { tFltrPolicerEntry 1 }

tFltrPolicerRowStatus            OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrPolicerRowStatus specifies the status of this row."
    ::= { tFltrPolicerEntry 2 }

tFltrPolicerLastChanged          OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrPolicerLastChanged indicates the sysUpTime at the time
         of the last modification of this row.

         If no changes were made to the row since the last re-initialization of
         the local network management subsystem, then this object contains the
         value zero."
    ::= { tFltrPolicerEntry 3 }

tFltrPolicerDescription          OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrPolicerDescription specifies a description for this
         policer."
    DEFVAL      { ''H }
    ::= { tFltrPolicerEntry 4 }

tFltrPolicerPIR                  OBJECT-TYPE
    SYNTAX      TFilterPolicerPIR
    UNITS       "kilobps"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tFltrPolicerPIR specifies the policer peak information
         rate (PIR) specified by the user."
    DEFVAL      { -1 }
    ::= { tFltrPolicerEntry 5 }

tFltrPolicerPPSPIR               OBJECT-TYPE
    SYNTAX      TFilterPolicerPPSPIR
    UNITS       "packets per second"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of tFltrPolicerPPSPIR specifies the policer packets per
         second peak information rate (PPS-PIR) specified by the user."
    DEFVAL      { -1 }
    ::= { tFltrPolicerEntry 6 }

tFltrPolicerMBS                  OBJECT-TYPE
    SYNTAX      TPolicerBurstSizeBytes
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPolicerMBS specifies the maximum burst
         size to which the traffic matching the filter entry will be limited."
    DEFVAL      { -1 }
    ::= { tFltrPolicerEntry 7 }

tFltrPolicerScope                OBJECT-TYPE
    SYNTAX      TFltrPolicerScope
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPolicerScope specifies the scope of this
         policer specified by the user."
    DEFVAL      { filter }
    ::= { tFltrPolicerEntry 8 }

tFltrFilterSetTableLstChng       OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrFilterSetTableLstChng indicates the sysUpTime at the
         time of the last modification of tFltrFilterSetTable.

         If no changes were made to the table since the last re-initialization
         of the local network management subsystem, this object contains the
         value zero."
    ::= { tFilterObjects 121 }

tFltrFilterSetTable              OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrFilterSetEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrFilterSetTable contains an entry for each filter set of
         ipvx and/or mac filter defined in the filter area."
    ::= { tFilterObjects 122 }

tFltrFilterSetEntry              OBJECT-TYPE
    SYNTAX      TFltrFilterSetEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the tFltrFilterSetTable."
    INDEX       { IMPLIED tFltrFilterSetName }
    ::= { tFltrFilterSetTable 1 }

TFltrFilterSetEntry              ::= SEQUENCE
{
    tFltrFilterSetName               TNamedItem,
    tFltrFilterSetRowStatus          RowStatus,
    tFltrFilterSetLastChanged        TimeStamp,
    tFltrFilterSetDescription        TItemDescription,
    tFltrFilterSetMacFilterId        TFilterID,
    tFltrFilterSetIpFilterId         TFilterID,
    tFltrFilterSetIpv6FilterId       TFilterID
}

tFltrFilterSetName               OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrFilterSetName specifies the name given to this filter
         set."
    ::= { tFltrFilterSetEntry 1 }

tFltrFilterSetRowStatus          OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrFilterSetRowStatus specifies the status of this row."
    ::= { tFltrFilterSetEntry 2 }

tFltrFilterSetLastChanged        OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The object tFltrFilterSetLastChanged indicates the sysUpTime at the
         time of the last modification of this row.

         If no changes were made to the row since the last re-initialization of
         the local network management subsystem, then this object contains the
         value zero."
    ::= { tFltrFilterSetEntry 3 }

tFltrFilterSetDescription        OBJECT-TYPE
    SYNTAX      TItemDescription
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object tFltrFilterSetDescription specifies a description for this
         row."
    DEFVAL      { ''H }
    ::= { tFltrFilterSetEntry 4 }

tFltrFilterSetMacFilterId        OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrFilterSetMacFilterId specifies the row
         index in the tMacFilterTable corresponding to this mac filter, or zero
         if no filter is specified."
    DEFVAL      { 0 }
    ::= { tFltrFilterSetEntry 5 }

tFltrFilterSetIpFilterId         OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrFilterSetIpFilterId specifies the row
         index in the tIPFilterTable corresponding to this ip filter, or zero
         if no filter is specified."
    DEFVAL      { 0 }
    ::= { tFltrFilterSetEntry 6 }

tFltrFilterSetIpv6FilterId       OBJECT-TYPE
    SYNTAX      TFilterID
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrFilterSetIpv6FilterId specifies the row
         index in the tIPv6FilterTable corresponding to this ipv6 filter, or
         zero if no filter is specified."
    DEFVAL      { 0 }
    ::= { tFltrFilterSetEntry 7 }

tFltrPlcrStatSysScopeTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrPlcrStatSysScopeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrPlcrStatSysScopeTable contains statistics and counters
         pertaining to filter policer system-scope instances."
    ::= { tFilterObjects 123 }

tFltrPlcrStatSysScopeEntry       OBJECT-TYPE
    SYNTAX      TFltrPlcrStatSysScopeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of the tFltrPlcrStatSysScopeTable table.

         Entries in this table are created by the system."
    INDEX       { tFltrPlcrStatSysScopeName }
    ::= { tFltrPlcrStatSysScopeTable 1 }

TFltrPlcrStatSysScopeEntry       ::= SEQUENCE
{
    tFltrPlcrStatSysScopeName        TNamedItem,
    tFltrPlcrStatSysScopeIngHitCnt   Counter64,
    tFltrPlcrStatSysScopeIngHitCntB  Counter64,
    tFltrPlcrStatSysScopeIngDrop     Counter64,
    tFltrPlcrStatSysScopeIngDropB    Counter64,
    tFltrPlcrStatSysScopeIngFwd      Counter64,
    tFltrPlcrStatSysScopeIngFwdB     Counter64,
    tFltrPlcrStatSysScopeEgrHitCnt   Counter64,
    tFltrPlcrStatSysScopeEgrHitCntB  Counter64,
    tFltrPlcrStatSysScopeEgrDrop     Counter64,
    tFltrPlcrStatSysScopeEgrDropB    Counter64,
    tFltrPlcrStatSysScopeEgrFwd      Counter64,
    tFltrPlcrStatSysScopeEgrFwdB     Counter64
}

tFltrPlcrStatSysScopeName        OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrPlcrStatSysScopeName specifies the name of a filter
         policer associated with this instance."
    ::= { tFltrPlcrStatSysScopeEntry 1 }

tFltrPlcrStatSysScopeIngHitCnt   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeIngHitCnt indicates the
         number of ingress packets which were subjected to this filter policer
         instance."
    ::= { tFltrPlcrStatSysScopeEntry 2 }

tFltrPlcrStatSysScopeIngHitCntB  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeIngHitCntB indicates the
         number of bytes of all ingress packets which were subjected to this
         filter policer instance."
    ::= { tFltrPlcrStatSysScopeEntry 3 }

tFltrPlcrStatSysScopeIngDrop     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeIngDrop indicates the
         number of dropped ingress packets which were subjected to this filter
         policer instance."
    ::= { tFltrPlcrStatSysScopeEntry 4 }

tFltrPlcrStatSysScopeIngDropB    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeIngDropB indicates the
         number of dropped bytes of all ingress packets which were subjected to
         this filter policer instance."
    ::= { tFltrPlcrStatSysScopeEntry 5 }

tFltrPlcrStatSysScopeIngFwd      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeIngFwd indicates the
         number of forwarded ingress packets which were subjected to this
         filter policer instance."
    ::= { tFltrPlcrStatSysScopeEntry 6 }

tFltrPlcrStatSysScopeIngFwdB     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeIngFwdB indicates the
         number of forwarded bytes of all ingress packets which were subjected
         to this filter policer instance."
    ::= { tFltrPlcrStatSysScopeEntry 7 }

tFltrPlcrStatSysScopeEgrHitCnt   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeEgrHitCnt indicates the
         number of egress packets which were subjected to this filter policer
         instance."
    ::= { tFltrPlcrStatSysScopeEntry 8 }

tFltrPlcrStatSysScopeEgrHitCntB  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeEgrHitCntB indicates the
         number of bytes of all egress packets that were subjected to this
         filter policer instance."
    ::= { tFltrPlcrStatSysScopeEntry 9 }

tFltrPlcrStatSysScopeEgrDrop     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeEgrDrop indicates the
         number of dropped egress packets which were subjected to this filter
         policer instance."
    ::= { tFltrPlcrStatSysScopeEntry 10 }

tFltrPlcrStatSysScopeEgrDropB    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeEgrDropB indicates the
         number of dropped bytes of all egress packets which were subjected to
         this filter policer instance."
    ::= { tFltrPlcrStatSysScopeEntry 11 }

tFltrPlcrStatSysScopeEgrFwd      OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeEgrFwd indicates the
         number of forwarded egress packets which were subjected to this filter
         policer instance."
    ::= { tFltrPlcrStatSysScopeEntry 12 }

tFltrPlcrStatSysScopeEgrFwdB     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatSysScopeEgrFwdB indicates the
         number of forwarded bytes of all egress packets which were subjected
         to this filter policer instance."
    ::= { tFltrPlcrStatSysScopeEntry 13 }

tFltrPlcrStatFltrScopeTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF TFltrPlcrStatFltrScopeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table tFltrPlcrStatFltrScopeTable contains statistics and counters
         pertaining to filter policer filter-scope instances."
    ::= { tFilterObjects 124 }

tFltrPlcrStatFltrScopeEntry      OBJECT-TYPE
    SYNTAX      TFltrPlcrStatFltrScopeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of the tFltrPlcrStatFltrScopeTable table.

         Entries in this table are created by the system."
    INDEX       {
        tFltrPlcrStatFltrScopeName,
        tFltrPlcrStatFltrScopeFltrType,
        tFltrPlcrStatFltrScopeFltrId
    }
    ::= { tFltrPlcrStatFltrScopeTable 1 }

TFltrPlcrStatFltrScopeEntry      ::= SEQUENCE
{
    tFltrPlcrStatFltrScopeName       TNamedItem,
    tFltrPlcrStatFltrScopeFltrType   TFilterType,
    tFltrPlcrStatFltrScopeFltrId     TAnyFilterID,
    tFltrPlcrStatFltrScopeIngHitCnt  Counter64,
    tFltrPlcrStatFltrScopeIngHitCntB Counter64,
    tFltrPlcrStatFltrScopeIngDrop    Counter64,
    tFltrPlcrStatFltrScopeIngDropB   Counter64,
    tFltrPlcrStatFltrScopeIngFwd     Counter64,
    tFltrPlcrStatFltrScopeIngFwdB    Counter64,
    tFltrPlcrStatFltrScopeEgrHitCnt  Counter64,
    tFltrPlcrStatFltrScopeEgrHitCntB Counter64,
    tFltrPlcrStatFltrScopeEgrDrop    Counter64,
    tFltrPlcrStatFltrScopeEgrDropB   Counter64,
    tFltrPlcrStatFltrScopeEgrFwd     Counter64,
    tFltrPlcrStatFltrScopeEgrFwdB    Counter64
}

tFltrPlcrStatFltrScopeName       OBJECT-TYPE
    SYNTAX      TNamedItem
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The object tFltrPlcrStatFltrScopeName specifies the name of a filter
         policer associated with this instance."
    ::= { tFltrPlcrStatFltrScopeEntry 1 }

tFltrPlcrStatFltrScopeFltrType   OBJECT-TYPE
    SYNTAX      TFilterType { fltrtypeselIp (1), fltrtypeselIpv6 (4) }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeFltrType specifies the
         type of ACL filter.

         Refer to the description of the textual convention TFilterType for
         more information."
    ::= { tFltrPlcrStatFltrScopeEntry 2 }

tFltrPlcrStatFltrScopeFltrId     OBJECT-TYPE
    SYNTAX      TAnyFilterID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeFltrId specifies a
         filter policer instance IP or IPv6 ACL filter ID. The ACL filter type
         is given by the value of tFltrPlcrStatFltrScopeFltrType.

         Refer to the description of the textual convention TAnyFilterID for
         more information."
    ::= { tFltrPlcrStatFltrScopeEntry 3 }

tFltrPlcrStatFltrScopeIngHitCnt  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeIngHitCnt indicates the
         number of ingress packets which were subjected to this filter policer
         instance."
    ::= { tFltrPlcrStatFltrScopeEntry 4 }

tFltrPlcrStatFltrScopeIngHitCntB OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeIngHitCntB indicates the
         number of bytes of all ingress packets which were subjected to this
         filter policer instance."
    ::= { tFltrPlcrStatFltrScopeEntry 5 }

tFltrPlcrStatFltrScopeIngDrop    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeIngDrop indicates the
         number of dropped ingress packets which were subjected to this filter
         policer instance."
    ::= { tFltrPlcrStatFltrScopeEntry 6 }

tFltrPlcrStatFltrScopeIngDropB   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeIngDropB indicates the
         number of dropped bytes of all ingress packets which were subjected to
         this filter policer instance."
    ::= { tFltrPlcrStatFltrScopeEntry 7 }

tFltrPlcrStatFltrScopeIngFwd     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeIngFwd indicates the
         number of forwarded ingress packets which were subjected to this
         filter policer instance."
    ::= { tFltrPlcrStatFltrScopeEntry 8 }

tFltrPlcrStatFltrScopeIngFwdB    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeIngFwdB indicates the
         number of forwarded bytes of all ingress packets which were subjected
         to this filter policer instance."
    ::= { tFltrPlcrStatFltrScopeEntry 9 }

tFltrPlcrStatFltrScopeEgrHitCnt  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeEgrHitCnt indicates the
         number of egress packets which were subjected to this filter policer
         instance."
    ::= { tFltrPlcrStatFltrScopeEntry 10 }

tFltrPlcrStatFltrScopeEgrHitCntB OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeEgrHitCntB indicates the
         number of bytes of all egress packets that were subjected to this
         filter policer instance."
    ::= { tFltrPlcrStatFltrScopeEntry 11 }

tFltrPlcrStatFltrScopeEgrDrop    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeEgrDrop indicates the
         number of dropped egress packets which were subjected to this filter
         policer instance."
    ::= { tFltrPlcrStatFltrScopeEntry 12 }

tFltrPlcrStatFltrScopeEgrDropB   OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeEgrDropB indicates the
         number of dropped bytes of all egress packets which were subjected to
         this filter policer instance."
    ::= { tFltrPlcrStatFltrScopeEntry 13 }

tFltrPlcrStatFltrScopeEgrFwd     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeEgrFwd indicates the
         number of forwarded egress packets which were subjected to this filter
         policer instance."
    ::= { tFltrPlcrStatFltrScopeEntry 14 }

tFltrPlcrStatFltrScopeEgrFwdB    OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object tFltrPlcrStatFltrScopeEgrFwdB indicates the
         number of forwarded bytes of all egress packets which were subjected
         to this filter policer instance."
    ::= { tFltrPlcrStatFltrScopeEntry 15 }

tFilterMIBConformance            OBJECT IDENTIFIER ::= { tmnxSRConfs 21 }

tFilterMIBCompliances            OBJECT IDENTIFIER ::= { tFilterMIBConformance 1 }

tFilter7450V4v0Compliance        MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         7450 ESS series systems release R4.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV4v0Group,
            tMacFilterV4v0Group,
            tFilterLogGroup,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsGroup
        }
    ::= { tFilterMIBCompliances 4 }

tFilter7750V4v0Compliance        MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         7750 SR series systems release R4.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV4v0Group,
            tMacFilterV4v0Group,
            tFilterLogGroup,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsGroup,
            tIPv6FilterV4v0Group
        }
    ::= { tFilterMIBCompliances 5 }

tFilter7450V5v0Compliance        MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         7450 ESS series systems release R5.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV5v0Group,
            tMacFilterV4v0Group,
            tFilterLogGroup,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsGroup,
            tTodPolicies77450V5v0Group,
            tToDPoliciesV5v0NotifyGroup,
            tFilterLogV5v0Group
        }
    ::= { tFilterMIBCompliances 6 }

tFilter77x0V5v0Compliance        MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         77x0 SPR/SR series systems release R5.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV5v0Group,
            tMacFilterV4v0Group,
            tFilterLogGroup,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsGroup,
            tIPv6FilterV4v0Group,
            tTodPolicies77x0V5v0Group,
            tToDPoliciesV5v0NotifyGroup,
            tFilterLogV5v0Group
        }
    ::= { tFilterMIBCompliances 7 }

tFilter7450V6v0Compliance        MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         7450 ESS series systems release R5.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV6v0Group,
            tMacFilterV6v0Group,
            tFilterLogGroup,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsGroup,
            tTodPolicies77450V5v0Group,
            tToDPoliciesV5v0NotifyGroup,
            tFilterLogV5v0Group
        }
    ::= { tFilterMIBCompliances 8 }

tFilter77x0V6v0Compliance        MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         77x0 SPR/SR series systems release R5.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV6v0Group,
            tMacFilterV6v0Group,
            tFilterLogGroup,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsGroup,
            tIPv6FilterV6v0Group,
            tTodPolicies77x0V5v0Group,
            tToDPoliciesV5v0NotifyGroup,
            tFilterLogV5v0Group
        }
    ::= { tFilterMIBCompliances 9 }

tFilter7450V8v0Compliance        MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         7450 ESS series systems release R8.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsV8v0Group,
            tFilterNotificationObjV8v0Group,
            tTodPolicies77450V5v0Group,
            tToDPoliciesV5v0NotifyGroup
        }
    ::= { tFilterMIBCompliances 10 }

tFilter77x0V8v0Compliance        MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         77x0 SPR/SR series systems release R8.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV8v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsV8v0Group,
            tFilterNotificationObjV8v0Group,
            tIPv6FilterV8v0Group,
            tTodPolicies77x0V5v0Group,
            tToDPoliciesV5v0NotifyGroup
        }
    ::= { tFilterMIBCompliances 11 }

tFilter7xxxV9v0Compliance        MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         77x0 SPR/SR series systems release R9.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV9v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsV9v0Group,
            tFilterNotificationObjV9v0Group,
            tIPv6FilterV8v0Group,
            tTodPolicies77x0V5v0Group,
            tToDPoliciesV5v0NotifyGroup,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV9v0Group
        }
    ::= { tFilterMIBCompliances 12 }

tFilter7xxxV10v0Compliance       MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         77x0 SPR/SR series systems release R10.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV9v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsV9v0Group,
            tFilterNotificationObjV9v0Group,
            tIPv6FilterV10v0Group,
            tTodPolicies77x0V5v0Group,
            tToDPoliciesV5v0NotifyGroup,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tFilterNameV10v0Group,
            tLiFilterV10v0Group,
            tFilterPrefixListV10v0Group
        }
    ::= { tFilterMIBCompliances 13 }

tFilter7xxxV11v0Compliance       MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         77x0 SPR/SR series systems release R11.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV11v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsV11v0Group,
            tFilterNotificationObjV11v0Group,
            tIPv6FilterV11v0Group,
            tTodPolicies77x0V5v0Group,
            tToDPoliciesV5v0NotifyGroup,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tFilterNameV10v0Group,
            tLiFilterV10v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterPortListV11v0Group
        }
    ::= { tFilterMIBCompliances 14 }

tFilter7xxxV12v0Compliance       MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         77x0 SPR/SR series systems release R12.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV12v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyGroup,
            tFilterNotificationsV11v0Group,
            tFilterNotificationsV12v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV12v0Group,
            tTodPolicies77x0V5v0Group,
            tToDPoliciesV5v0NotifyGroup,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterPortListV11v0Group
        }
    ::= { tFilterMIBCompliances 15 }

tFilterV13v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         77x0 SPR/SR series systems release R13.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV12v0Group,
            tIPFilterV13v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV13v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationsV12v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV12v0Group,
            tIPv6FilterV13v0Group,
            tTodPolicies77x0V5v0Group,
            tToDPoliciesV5v0NotifyGroup,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tMacFilterV13v0Group
        }
    ::= { tFilterMIBCompliances 16 }

tFilterV14v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         SROS series systems release R14.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV14v0Group,
            tIPFilterV13v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV13v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationsV12v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV14v0Group,
            tIPv6FilterV13v0Group,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tMacFilterV13v0Group,
            tFilterEmbedFlowspecGroup,
            tFilterNotificationsV14v0Group,
            tFilterIPvXRedundantActionGroup,
            tFilterMacRedundantActionGroup,
            tFilterEntryStatGroup,
            tFilterEmbeddedRefGroup,
            tFilterRemarkDscpGroup,
            tFilterRemarkDscpExtGroup
        }
    ::= { tFilterMIBCompliances 17 }

tFilterV15v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         SROS series systems release R15.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV14v0Group,
            tIPFilterV13v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV13v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV14v0Group,
            tIPv6FilterV13v0Group,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tMacFilterV13v0Group,
            tFilterEmbedFlowspecGroup,
            tFilterNotificationsV14v0Group,
            tFilterIPvXRedundantActionGroup,
            tFilterMacRedundantActionGroup,
            tFilterEntryStatGroup,
            tFilterEmbeddedRefGroup,
            tFilterRemarkDscpGroup,
            tFilterRemarkDscpExtGroup,
            tFilterPrefListRtrBgpPeersGroup,
            tFilterPrefListInfoGroup,
            tFilterForwardVprnTargetGroup,
            tFilterNotificationsV15v0Group,
            tFilterFwdBondingConnectionGroup,
            tFilterSelectiveFlowspecGroup
        }
    ::= { tFilterMIBCompliances 18 }

tFilterV16v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         SROS series systems release R16.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV14v0Group,
            tIPFilterV13v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV13v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV14v0Group,
            tIPv6FilterV13v0Group,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tMacFilterV13v0Group,
            tFilterEmbedFlowspecGroup,
            tFilterNotificationsV14v0Group,
            tFilterIPvXRedundantActionGroup,
            tFilterMacRedundantActionGroup,
            tFilterEntryStatGroup,
            tFilterEmbeddedRefGroup,
            tFilterRemarkDscpGroup,
            tFilterRemarkDscpExtGroup,
            tFilterPrefListRtrBgpPeersGroup,
            tFilterPrefListInfoGroup,
            tFilterForwardVprnTargetGroup,
            tFilterNotificationsV15v0Group,
            tFilterFwdBondingConnectionGroup,
            tFilterSelectiveFlowspecGroup,
            tFilterMatchTcpFlagsGroup,
            tFilterActionFc,
            tFilterRPPingSrcAddressGroup,
            tFilterRPActiveDstChangeNotifGrp,
            tFilterRPActiveDstChangeGrp,
            tFilterRPlcyBindingGroup,
            tFltrGreTunTempGroup,
            tFltrPrefListPrefExcludeGrp,
            fltrMdAutoIdV16v0Group,
            tFltrPatternMatchGroup
        }
    ::= { tFilterMIBCompliances 19 }

tFilterV19v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         SROS series systems release R19.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV14v0Group,
            tIPFilterV13v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV19v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV14v0Group,
            tIPv6FilterV13v0Group,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tMacFilterV13v0Group,
            tFilterEmbedFlowspecGroup,
            tFilterNotificationsV14v0Group,
            tFilterIPvXRedundantActionGroup,
            tFilterMacRedundantActionGroup,
            tFilterEntryStatGroup,
            tFilterEmbeddedRefGroup,
            tFilterRemarkDscpGroup,
            tFilterRemarkDscpExtGroup,
            tFilterPrefListRtrBgpPeersGroup,
            tFilterPrefListInfoGroup,
            tFilterForwardVprnTargetGroup,
            tFilterNotificationsV15v0Group,
            tFilterFwdBondingConnectionGroup,
            tFilterSelectiveFlowspecGroup,
            tFilterMatchTcpFlagsGroup,
            tFilterActionFc,
            tFilterRPPingSrcAddressGroup,
            tFilterRPActiveDstChangeNotifGrp,
            tFilterRPActiveDstChangeGrp,
            tFilterRPlcyBindingGroup,
            tFltrGreTunTempGroup,
            tFltrPrefListPrefExcludeGrp,
            fltrMdAutoIdV16v0Group,
            tFltrPatternMatchGroup,
            tFltrMatchMacForIPvXGroup,
            tFltrMatchPacketLengthGroup,
            tFltrFilterNameInLIGroup,
            tFltrCAMTypeGroup,
            tLiFltrAssocFltrNameGroup,
            tFltrIPv6ExceptionV19v0Group,
            tFltrFwdMplsPlcyEndptGrp,
            tFltrFwdSrtePlcyEndptColorGrp
        }
    ::= { tFilterMIBCompliances 20 }

tFilterV20v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         SROS series systems release R20.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV14v0Group,
            tIPFilterV13v0Group,
            tMacFilterV8v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV19v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV14v0Group,
            tIPv6FilterV13v0Group,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tMacFilterV13v0Group,
            tFilterEmbedFlowspecGroup,
            tFilterNotificationsV14v0Group,
            tFilterIPvXRedundantActionGroup,
            tFilterMacRedundantActionGroup,
            tFilterEntryStatGroup,
            tFilterEmbeddedRefGroup,
            tFilterRemarkDscpGroup,
            tFilterRemarkDscpExtGroup,
            tFilterPrefListRtrBgpPeersGroup,
            tFilterPrefListInfoGroup,
            tFilterForwardVprnTargetGroup,
            tFilterNotificationsV15v0Group,
            tFilterFwdBondingConnectionGroup,
            tFilterSelectiveFlowspecGroup,
            tFilterMatchTcpFlagsGroup,
            tFilterActionFc,
            tFilterRPPingSrcAddressGroup,
            tFilterRPActiveDstChangeNotifGrp,
            tFilterRPActiveDstChangeGrp,
            tFilterRPlcyBindingGroup,
            tFltrGreTunTempGroup,
            tFltrPrefListPrefExcludeGrp,
            fltrMdAutoIdV16v0Group,
            tFltrPatternMatchGroup,
            tFltrMatchMacForIPvXGroup,
            tFltrMatchPacketLengthGroup,
            tFltrFilterNameInLIGroup,
            tFltrCAMTypeGroup,
            tLiFltrAssocFltrNameGroup,
            tFltrIPv6ExceptionV19v0Group,
            tFltrFwdMplsPlcyEndptGrp,
            tFltrFwdSrtePlcyEndptColorGrp,
            tLiFltrMatchFragmentGroup,
            fltrMdAutoIdV20v0Group,
            tFilterMatchProtocolListGroup,
            tFilterMatchDestClassGroup,
            tFilterL2AwareNatBypassGroup,
            tFltrLiRsvdBlockRangeChgNotifGrp,
            tFltrCflowdSampleProfileGroup
        }
    ::= { tFilterMIBCompliances 21 }

tFilterV21v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         SROS series systems release R21.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV21v0Group,
            tMacFilterV21v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV19v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV21v0Group,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tFilterEmbedFlowspecGroup,
            tFilterIPvXRedundantActionGroup,
            tFilterMacRedundantActionGroup,
            tFilterEntryStatGroup,
            tFilterEmbeddedRefGroup,
            tFilterRemarkDscpGroup,
            tFilterRemarkDscpExtGroup,
            tFilterPrefListRtrBgpPeersGroup,
            tFilterPrefListInfoGroup,
            tFilterForwardVprnTargetGroup,
            tFilterNotificationsV15v0Group,
            tFilterFwdBondingConnectionGroup,
            tFilterSelectiveFlowspecGroup,
            tFilterMatchTcpFlagsGroup,
            tFilterActionFc,
            tFilterRPPingSrcAddressGroup,
            tFilterRPActiveDstChangeNotifGrp,
            tFilterRPActiveDstChangeGrp,
            tFilterRPlcyBindingGroup,
            tFltrGreTunTempGroup,
            tFltrPrefListPrefExcludeGrp,
            fltrMdAutoIdV16v0Group,
            tFltrPatternMatchGroup,
            tFltrMatchMacForIPvXGroup,
            tFltrMatchPacketLengthGroup,
            tFltrFilterNameInLIGroup,
            tFltrCAMTypeGroup,
            tLiFltrAssocFltrNameGroup,
            tFltrIPv6ExceptionV19v0Group,
            tFltrFwdMplsPlcyEndptGrp,
            tFltrFwdSrtePlcyEndptColorGrp,
            tLiFltrMatchFragmentGroup,
            fltrMdAutoIdV20v0Group,
            tFilterMatchProtocolListGroup,
            tFilterMatchDestClassGroup,
            tFilterL2AwareNatBypassGroup,
            tFltrLiRsvdBlockRangeChgNotifGrp,
            tFltrCflowdSampleProfileGroup,
            tFltrEntryCollectStatsIPvXGroup,
            tFltrEntryCollectStatsMacGroup,
            tFilterMacFltrActionGroupV21,
            tFilterMatchTTLGroup,
            tFltrMatchSrcOrDstIpGroup
        }
    ::= { tFilterMIBCompliances 22 }

tFilterV22v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         SROS series systems release R22.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV21v0Group,
            tMacFilterV21v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV19v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV21v0Group,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tFilterEmbedFlowspecGroup,
            tFilterIPvXRedundantActionGroup,
            tFilterMacRedundantActionGroup,
            tFilterEntryStatGroup,
            tFilterEmbeddedRefGroup,
            tFilterRemarkDscpGroup,
            tFilterRemarkDscpExtGroup,
            tFilterPrefListRtrBgpPeersGroup,
            tFilterPrefListInfoGroup,
            tFilterForwardVprnTargetGroup,
            tFilterNotificationsV15v0Group,
            tFilterFwdBondingConnectionGroup,
            tFilterSelectiveFlowspecGroup,
            tFilterMatchTcpFlagsGroup,
            tFilterActionFc,
            tFilterRPPingSrcAddressGroup,
            tFilterRPActiveDstChangeNotifGrp,
            tFilterRPActiveDstChangeGrp,
            tFilterRPlcyBindingGroup,
            tFltrGreTunTempGroup,
            tFltrPrefListPrefExcludeGrp,
            fltrMdAutoIdV16v0Group,
            tFltrPatternMatchGroup,
            tFltrMatchMacForIPvXGroup,
            tFltrMatchPacketLengthGroup,
            tFltrFilterNameInLIGroup,
            tFltrCAMTypeGroup,
            tLiFltrAssocFltrNameGroup,
            tFltrIPv6ExceptionV19v0Group,
            tFltrFwdMplsPlcyEndptGrp,
            tFltrFwdSrtePlcyEndptColorGrp,
            tLiFltrMatchFragmentGroup,
            fltrMdAutoIdV20v0Group,
            tFilterMatchProtocolListGroup,
            tFilterMatchDestClassGroup,
            tFilterL2AwareNatBypassGroup,
            tFltrLiRsvdBlockRangeChgNotifGrp,
            tFltrCflowdSampleProfileGroup,
            tFltrEntryCollectStatsIPvXGroup,
            tFltrEntryCollectStatsMacGroup,
            tFilterMacFltrActionGroupV21,
            tFilterMatchTTLGroup,
            tFltrMatchSrcOrDstIpGroup,
            tFltrLagSharedPolicerGroup,
            tFltrGreTunTempIpv6Group,
            tFltrMatchTcpEstGroup,
            tFilterNotificationsV23v0Group
        }
    ::= { tFilterMIBCompliances 23 }

tFilterV23v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         SROS series systems release R23.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV21v0Group,
            tMacFilterV21v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV19v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV21v0Group,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tFilterEmbedFlowspecGroup,
            tFilterIPvXRedundantActionGroup,
            tFilterMacRedundantActionGroup,
            tFilterEntryStatGroup,
            tFilterEmbeddedRefGroup,
            tFilterRemarkDscpGroup,
            tFilterRemarkDscpExtGroup,
            tFilterPrefListRtrBgpPeersGroup,
            tFilterPrefListInfoGroup,
            tFilterForwardVprnTargetGroup,
            tFilterNotificationsV15v0Group,
            tFilterFwdBondingConnectionGroup,
            tFilterSelectiveFlowspecGroup,
            tFilterMatchTcpFlagsGroup,
            tFilterActionFc,
            tFilterRPPingSrcAddressGroup,
            tFilterRPActiveDstChangeNotifGrp,
            tFilterRPActiveDstChangeGrp,
            tFilterRPlcyBindingGroup,
            tFltrGreTunTempGroup,
            tFltrPrefListPrefExcludeGrp,
            fltrMdAutoIdV16v0Group,
            tFltrPatternMatchGroup,
            tFltrMatchMacForIPvXGroup,
            tFltrMatchPacketLengthGroup,
            tFltrFilterNameInLIGroup,
            tFltrCAMTypeGroup,
            tLiFltrAssocFltrNameGroup,
            tFltrIPv6ExceptionV19v0Group,
            tFltrFwdMplsPlcyEndptGrp,
            tFltrFwdSrtePlcyEndptColorGrp,
            tLiFltrMatchFragmentGroup,
            fltrMdAutoIdV20v0Group,
            tFilterMatchProtocolListGroup,
            tFilterMatchDestClassGroup,
            tFilterL2AwareNatBypassGroup,
            tFltrLiRsvdBlockRangeChgNotifGrp,
            tFltrCflowdSampleProfileGroup,
            tFltrEntryCollectStatsIPvXGroup,
            tFltrEntryCollectStatsMacGroup,
            tFilterMacFltrActionGroupV21,
            tFilterMatchTTLGroup,
            tFltrMatchSrcOrDstIpGroup,
            tFltrLagSharedPolicerGroup,
            tFltrGreTunTempIpv6Group,
            tFltrMatchTcpEstGroup,
            tFilterNotificationsV23v0Group,
            tFltrFwdSrv6PlcyGrp,
            tLiMacFilterMatchVlanIdGrp
        }
    ::= { tFilterMIBCompliances 24 }

tFilterV24v0Compliance           MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         SROS series systems release R24.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV21v0Group,
            tMacFilterV21v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV19v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV21v0Group,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tFilterEmbedFlowspecGroup,
            tFilterMacRedundantActionGroup,
            tFilterEntryStatGroup,
            tFilterEmbeddedRefGroup,
            tFilterRemarkDscpGroup,
            tFilterRemarkDscpExtGroup,
            tFilterPrefListRtrBgpPeersGroup,
            tFilterPrefListInfoGroup,
            tFilterForwardVprnTargetGroup,
            tFilterNotificationsV15v0Group,
            tFilterFwdBondingConnectionGroup,
            tFilterSelectiveFlowspecGroup,
            tFilterMatchTcpFlagsGroup,
            tFilterActionFc,
            tFilterRPPingSrcAddressGroup,
            tFilterRPActiveDstChangeNotifGrp,
            tFilterRPActiveDstChangeGrp,
            tFilterRPlcyBindingGroup,
            tFltrGreTunTempGroup,
            tFltrPrefListPrefExcludeGrp,
            fltrMdAutoIdV16v0Group,
            tFltrPatternMatchGroup,
            tFltrMatchMacForIPvXGroup,
            tFltrMatchPacketLengthGroup,
            tFltrFilterNameInLIGroup,
            tFltrCAMTypeGroup,
            tLiFltrAssocFltrNameGroup,
            tFltrIPv6ExceptionV19v0Group,
            tFltrFwdMplsPlcyEndptGrp,
            tFltrFwdSrtePlcyEndptColorGrp,
            tLiFltrMatchFragmentGroup,
            fltrMdAutoIdV20v0Group,
            tFilterMatchProtocolListGroup,
            tFilterMatchDestClassGroup,
            tFilterL2AwareNatBypassGroup,
            tFltrLiRsvdBlockRangeChgNotifGrp,
            tFltrCflowdSampleProfileGroup,
            tFltrEntryCollectStatsIPvXGroup,
            tFltrEntryCollectStatsMacGroup,
            tFilterMacFltrActionGroupV21,
            tFilterMatchTTLGroup,
            tFltrMatchSrcOrDstIpGroup,
            tFltrLagSharedPolicerGroup,
            tFltrGreTunTempIpv6Group,
            tFltrMatchTcpEstGroup,
            tFilterNotificationsV23v0Group,
            tFltrFwdSrv6PlcyGrp,
            tLiMacFilterMatchVlanIdGrp,
            tFltrPktLenListGrp,
            tFilterIPvXRedActionV24v0Group,
            tFilterPolicerGroup,
            tFltrFilterSetGroup
        }
    ::= { tFilterMIBCompliances 25 }

tFilterV25v0Compliance           MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for management of Filter features on Nokia
         SROS series systems release R25.0."
    MODULE
        MANDATORY-GROUPS {
            tFilterScalarGroup,
            tIPFilterV21v0Group,
            tMacFilterV21v0Group,
            tFilterLogGroup,
            tFilterLogV5v0Group,
            tFilterRedirectPolicyV19v0Group,
            tFilterNotificationsV11v0Group,
            tFilterNotificationObjV12v0Group,
            tIPv6FilterV21v0Group,
            tMacFilterVidFilteringV9v0Group,
            tDhcpFilterV10v0Group,
            tDhcpFilterV13v0Group,
            tFilterNameV10v0Group,
            tLiFilterV12v0Group,
            tFilterPrefixListV11v0Group,
            tFilterEmbeddedInsertV11v0Group,
            tFilterEmbeddedInsertV12v0Group,
            tFilterEmbeddedInsertV13v0Group,
            tFilterPortListV11v0Group,
            tFilterSystemFilterV13v0Group,
            tFilterEmbedFlowspecGroup,
            tFilterMacRedundantActionGroup,
            tFilterEntryStatGroup,
            tFilterEmbeddedRefGroup,
            tFilterRemarkDscpGroup,
            tFilterRemarkDscpExtGroup,
            tFilterPrefListRtrBgpPeersGroup,
            tFilterPrefListInfoGroup,
            tFilterForwardVprnTargetGroup,
            tFilterNotificationsV15v0Group,
            tFilterFwdBondingConnectionGroup,
            tFilterSelectiveFlowspecGroup,
            tFilterMatchTcpFlagsGroup,
            tFilterActionFc,
            tFilterRPPingSrcAddressGroup,
            tFilterRPActiveDstChangeNotifGrp,
            tFilterRPActiveDstChangeGrp,
            tFilterRPlcyBindingGroup,
            tFltrGreTunTempGroup,
            tFltrPrefListPrefExcludeGrp,
            fltrMdAutoIdV16v0Group,
            tFltrPatternMatchGroup,
            tFltrMatchMacForIPvXGroup,
            tFltrMatchPacketLengthGroup,
            tFltrFilterNameInLIGroup,
            tFltrCAMTypeGroup,
            tLiFltrAssocFltrNameGroup,
            tFltrIPv6ExceptionV19v0Group,
            tFltrFwdMplsPlcyEndptGrp,
            tFltrFwdSrtePlcyEndptColorGrp,
            tLiFltrMatchFragmentGroup,
            fltrMdAutoIdV20v0Group,
            tFilterMatchProtocolListGroup,
            tFilterMatchDestClassGroup,
            tFilterL2AwareNatBypassGroup,
            tFltrLiRsvdBlockRangeChgNotifGrp,
            tFltrCflowdSampleProfileGroup,
            tFltrEntryCollectStatsIPvXGroup,
            tFltrEntryCollectStatsMacGroup,
            tFilterMacFltrActionGroupV21,
            tFilterMatchTTLGroup,
            tFltrMatchSrcOrDstIpGroup,
            tFltrLagSharedPolicerGroup,
            tFltrGreTunTempIpv6Group,
            tFltrMatchTcpEstGroup,
            tFilterNotificationsV23v0Group,
            tFltrFwdSrv6PlcyGrp,
            tLiMacFilterMatchVlanIdGrp,
            tFltrPktLenListGrp,
            tFilterIPvXRedActionV24v0Group,
            tFilterPolicerGroup,
            tFltrFilterSetGroup,
            tIPvXFilterParamsV25v0Group
        }
    ::= { tFilterMIBCompliances 26 }

tFilterMIBGroups                 OBJECT IDENTIFIER ::= { tFilterMIBConformance 2 }

tFilterLogGroup                  OBJECT-GROUP
    OBJECTS     {
        tFilterLogRowStatus,
        tFilterLogDestination,
        tFilterLogDescription,
        tFilterLogMaxNumEntries,
        tFilterLogSysLogId,
        tFilterLogFileId,
        tFilterLogStopOnFull,
        tFilterLogEnabled,
        tFilterLogMaxInstances,
        tFilterLogInstances,
        tFilterLogBindings
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of filter log objects on
         Nokia SROS series systems."
    ::= { tFilterMIBGroups 3 }

tFilterRedirectPolicyGroup       OBJECT-GROUP
    OBJECTS     {
        tFilterRPRowStatus,
        tFilterRPDescription,
        tFilterRPAdminState,
        tFilterRPActiveDest,
        tFilterRDRowStatus,
        tFilterRDDescription,
        tFilterRDAdminPriority,
        tFilterRDOperPriority,
        tFilterRDAdminState,
        tFilterRDOperState,
        tFilterRSTRowStatus,
        tFilterRSTOID,
        tFilterRSTCommunity,
        tFilterRSTSNMPVersion,
        tFilterRSTInterval,
        tFilterRSTTimeout,
        tFilterRSTDropCount,
        tFilterRSTHoldDown,
        tFilterRSTHoldDownRemain,
        tFilterRSTLastActionTime,
        tFilterRSTLastOID,
        tFilterRSTLastType,
        tFilterRSTLastCounter32Val,
        tFilterRSTLastUnsigned32Val,
        tFilterRSTLastTimeTicksVal,
        tFilterRSTLastInt32Val,
        tFilterRSTLastOctetStringVal,
        tFilterRSTLastIpAddressVal,
        tFilterRSTLastOidVal,
        tFilterRSTLastCounter64Val,
        tFilterRSTLastOpaqueVal,
        tFilterRSTLastAction,
        tFilterRSTLastPrioChange,
        tFilterRSTNextRespIndex,
        tFilterRSTRespRowStatus,
        tFilterRSTRespAction,
        tFilterRSTRespPrioChange,
        tFilterRSTRespOID,
        tFilterRSTRespType,
        tFilterRSTCounter32Val,
        tFilterRSTUnsigned32Val,
        tFilterRSTTimeTicksVal,
        tFilterRSTInt32Val,
        tFilterRSTOctetStringVal,
        tFilterRSTIpAddressVal,
        tFilterRSTOidVal,
        tFilterRSTCounter64Val,
        tFilterRSTOpaqueVal,
        tFilterRUTRowStatus,
        tFilterRUTURL,
        tFilterRUTHTTPVersion,
        tFilterRUTInterval,
        tFilterRUTTimeout,
        tFilterRUTDropCount,
        tFilterRUTHoldDown,
        tFilterRUTHoldDownRemain,
        tFilterRUTLastActionTime,
        tFilterRUTLastRetCode,
        tFilterRUTLastAction,
        tFilterRUTLastPrioChange,
        tFilterRUTRespRowStatus,
        tFilterRUTRespAction,
        tFilterRUTRespPrioChange,
        tFilterRPTRowStatus,
        tFilterRPTInterval,
        tFilterRPTTimeout,
        tFilterRPTDropCount,
        tFilterRPTHoldDown,
        tFilterRPTHoldDownRemain,
        tFilterRPTLastActionTime,
        tFilterRPTLastAction
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of filter redirect policy
         objects on Nokia SROS series systems. This group is obsoleted in
         release 13.0."
    ::= { tFilterMIBGroups 4 }

tFilterScalarGroup               OBJECT-GROUP
    OBJECTS     {
        tFilterDomainLastChanged
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of filter scalar objects on
         Nokia SROS series systems."
    ::= { tFilterMIBGroups 7 }

tFilterNotificationObjGroup      OBJECT-GROUP
    OBJECTS     {
        tFilterPBRDropReason
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of filter notification
         objects on Nokia SROS series systems."
    ::= { tFilterMIBGroups 8 }

tFilterNotificationsGroup        NOTIFICATION-GROUP
    NOTIFICATIONS {
        tIPFilterPBRPacketsDrop
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of notifications supporting management of filter
         notifications on Nokia SROS series systems."
    ::= { tFilterMIBGroups 9 }

tIPv6FilterV4v0Group             OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterRowStatus,
        tIPv6FilterScope,
        tIPv6FilterDescription,
        tIPv6FilterDefaultAction,
        tIPv6FilterParamsRowStatus,
        tIPv6FilterParamsLogId,
        tIPv6FilterParamsDescription,
        tIPv6FilterParamsAction,
        tIPv6FilterParamsForwardNH,
        tIPv6FilterParamsForwardNHIndirect,
        tIPv6FilterParamsRemarkDSCP,
        tIPv6FilterParamsRemarkDSCPMask,
        tIPv6FilterParamsRemarkDot1p,
        tIPv6FilterParamsSourceIpAddr,
        tIPv6FilterParamsSourceIpMask,
        tIPv6FilterParamsDestinationIpAddr,
        tIPv6FilterParamsDestinationIpMask,
        tIPv6FilterParamsNextHeader,
        tIPv6FilterParamsSourcePortValue1,
        tIPv6FilterParamsSourcePortValue2,
        tIPv6FilterParamsSourcePortOperator,
        tIPv6FilterParamsDestPortValue1,
        tIPv6FilterParamsDestPortValue2,
        tIPv6FilterParamsDestPortOperator,
        tIPv6FilterParamsDSCP,
        tIPv6FilterParamsTcpSyn,
        tIPv6FilterParamsTcpAck,
        tIPv6FilterParamsIcmpCode,
        tIPv6FilterParamsIcmpType,
        tIPv6FilterParamsCflowdSample,
        tIPv6FilterParamsCflowdIfSample,
        tIPv6FilterParamsForwardNHInterface,
        tIPv6FilterParamsIngressHitCount,
        tIPv6FilterParamsEgressHitCount,
        tIPv6FilterParamsLogInstantiated,
        tIPv6FilterParamsForwardRedPlcy,
        tIPv6FilterParamsActiveDest
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of IPv6 filter objects on
         Nokia SROS series systems."
    ::= { tFilterMIBGroups 11 }

tIPFilterV4v0Group               OBJECT-GROUP
    OBJECTS     {
        tIPFilterRowStatus,
        tIPFilterScope,
        tIPFilterDescription,
        tIPFilterDefaultAction,
        tIPFilterParamsRowStatus,
        tIPFilterParamsLogId,
        tIPFilterParamsDescription,
        tIPFilterParamsAction,
        tIPFilterParamsForwardNH,
        tIPFilterParamsForwardNHIndirect,
        tIPFilterParamsRemarkDSCP,
        tIPFilterParamsRemarkDSCPMask,
        tIPFilterParamsRemarkDot1p,
        tIPFilterParamsSourceIpAddr,
        tIPFilterParamsSourceIpMask,
        tIPFilterParamsDestinationIpAddr,
        tIPFilterParamsDestinationIpMask,
        tIPFilterParamsProtocol,
        tIPFilterParamsSourcePortValue1,
        tIPFilterParamsSourcePortValue2,
        tIPFilterParamsSourcePortOperator,
        tIPFilterParamsDestPortValue1,
        tIPFilterParamsDestPortValue2,
        tIPFilterParamsDestPortOperator,
        tIPFilterParamsDSCP,
        tIPFilterParamsFragment,
        tIPFilterParamsOptionPresent,
        tIPFilterParamsIpOptionValue,
        tIPFilterParamsIpOptionMask,
        tIPFilterParamsMultipleOption,
        tIPFilterParamsTcpSyn,
        tIPFilterParamsTcpAck,
        tIPFilterParamsIcmpCode,
        tIPFilterParamsIcmpType,
        tIPFilterParamsCflowdSample,
        tIPFilterParamsCflowdIfSample,
        tIPFilterParamsForwardNHInterface,
        tIPFilterParamsIngressHitCount,
        tIPFilterParamsEgressHitCount,
        tIPFilterParamsLogInstantiated,
        tIPFilterParamsForwardRedPlcy,
        tIPFilterParamsActiveDest,
        tIPFilterParamsFwdSvcId,
        tIPFilterParamsFwdSapPortId,
        tIPFilterParamsFwdSapEncapVal,
        tIPFilterParamsFwdSdpBind,
        tIPFilterParamsRedirectURL
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting IP Filters on Nokia 7x50 ESS/SR series
         systems 4.0 release."
    ::= { tFilterMIBGroups 12 }

tMacFilterV4v0Group              OBJECT-GROUP
    OBJECTS     {
        tMacFilterRowStatus,
        tMacFilterScope,
        tMacFilterDescription,
        tMacFilterDefaultAction,
        tMacFilterParamsRowStatus,
        tMacFilterParamsLogId,
        tMacFilterParamsDescription,
        tMacFilterParamsAction,
        tMacFilterParamsFrameType,
        tMacFilterParamsSrcMAC,
        tMacFilterParamsSrcMACMask,
        tMacFilterParamsDstMAC,
        tMacFilterParamsDstMACMask,
        tMacFilterParamsDot1pValue,
        tMacFilterParamsDot1pMask,
        tMacFilterParamsEtherType,
        tMacFilterParamsDsap,
        tMacFilterParamsDsapMask,
        tMacFilterParamsSsap,
        tMacFilterParamsSsapMask,
        tMacFilterParamsSnapPid,
        tMacFilterParamsSnapOui,
        tMacFilterParamsIngressHitCount,
        tMacFilterParamsEgressHitCount,
        tMacFilterParamsLogInstantiated,
        tMacFilterParamsFwdSvcId,
        tMacFilterParamsFwdSapPortId,
        tMacFilterParamsFwdSapEncapVal,
        tMacFilterParamsFwdSdpBind,
        tMacFilterParamsRedirectURL
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of mac filter objects on
         Nokia SROS series systems 4.0 release."
    ::= { tFilterMIBGroups 13 }

tTodPoliciesV4v0Group            OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsTimeRangeName,
        tIPFilterParamsTimeRangeState,
        tMacFilterParamsTimeRangeName,
        tMacFilterParamsTimeRangeState,
        tIPv6FilterParamsTimeRangeName,
        tIPv6FilterParamsTimeRangeState
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of time of day policy
         related objects on Nokia SROS series systems 4.0 release."
    ::= { tFilterMIBGroups 14 }

tmnxFilterObsoleteGroup          OBJECT-GROUP
    OBJECTS     {
        tAutoIPFilterEntrySourceIpMask
    }
    STATUS      current
    DESCRIPTION
        "The group of objects in TIMETRA-FILTER-MIB which are obsoleted."
    ::= { tFilterMIBGroups 15 }

tToDPoliciesV5v0NotifyGroup      NOTIFICATION-GROUP
    NOTIFICATIONS {
        tFilterEntryActivationFailed,
        tFilterEntryActivationRestored
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of notifications generated by the time of time of day policy
         feature on Nokia SROS series systems 5.0 release."
    ::= { tFilterMIBGroups 16 }

tIPFilterV5v0Group               OBJECT-GROUP
    OBJECTS     {
        tIPFilterRowStatus,
        tIPFilterScope,
        tIPFilterDescription,
        tIPFilterDefaultAction,
        tIPFilterParamsRowStatus,
        tIPFilterParamsLogId,
        tIPFilterParamsDescription,
        tIPFilterParamsAction,
        tIPFilterParamsForwardNH,
        tIPFilterParamsForwardNHIndirect,
        tIPFilterParamsRemarkDSCP,
        tIPFilterParamsRemarkDSCPMask,
        tIPFilterParamsRemarkDot1p,
        tIPFilterParamsSourceIpAddr,
        tIPFilterParamsSourceIpMask,
        tIPFilterParamsDestinationIpAddr,
        tIPFilterParamsDestinationIpMask,
        tIPFilterParamsProtocol,
        tIPFilterParamsSourcePortValue1,
        tIPFilterParamsSourcePortValue2,
        tIPFilterParamsSourcePortOperator,
        tIPFilterParamsDestPortValue1,
        tIPFilterParamsDestPortValue2,
        tIPFilterParamsDestPortOperator,
        tIPFilterParamsDSCP,
        tIPFilterParamsFragment,
        tIPFilterParamsOptionPresent,
        tIPFilterParamsIpOptionValue,
        tIPFilterParamsIpOptionMask,
        tIPFilterParamsMultipleOption,
        tIPFilterParamsTcpSyn,
        tIPFilterParamsTcpAck,
        tIPFilterParamsIcmpCode,
        tIPFilterParamsIcmpType,
        tIPFilterParamsCflowdSample,
        tIPFilterParamsCflowdIfSample,
        tIPFilterParamsForwardNHInterface,
        tIPFilterParamsIngressHitCount,
        tIPFilterParamsEgressHitCount,
        tIPFilterParamsLogInstantiated,
        tIPFilterParamsForwardRedPlcy,
        tIPFilterParamsActiveDest,
        tIPFilterParamsFwdSvcId,
        tIPFilterParamsFwdSapPortId,
        tIPFilterParamsFwdSapEncapVal,
        tIPFilterParamsFwdSdpBind,
        tIPFilterParamsRedirectURL,
        tIPFilterParamsSrcIpFullMask,
        tIPFilterParamsDestIpFullMask
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting IP Filters on Nokia 7x50 ESS/SR series
         systems 5.0 release."
    ::= { tFilterMIBGroups 17 }

tFilterLogV5v0Group              OBJECT-GROUP
    OBJECTS     {
        tFilterLogSummaryEnabled,
        tFilterLogSummaryCrit1
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting Filter Log Summarization on Nokia 7x50
         ESS/SR series systems 5.0 release."
    ::= { tFilterMIBGroups 18 }

tTodPolicies77450V5v0Group       OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsTimeRangeName,
        tIPFilterParamsTimeRangeState,
        tMacFilterParamsTimeRangeName,
        tMacFilterParamsTimeRangeState
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of time of day policy
         related objects on Nokia 7450 ESS series systems 5.0 release.

         This group was made obsolete for Nokia SROS Release 9.0."
    ::= { tFilterMIBGroups 19 }

tTodPolicies77x0V5v0Group        OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsTimeRangeName,
        tIPFilterParamsTimeRangeState,
        tMacFilterParamsTimeRangeName,
        tMacFilterParamsTimeRangeState,
        tIPv6FilterParamsTimeRangeName,
        tIPv6FilterParamsTimeRangeState
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of time of day policy
         related objects on Nokia 77x0 series systems 5.0 release."
    ::= { tFilterMIBGroups 20 }

tFilterNotificationObjV5v0Group  OBJECT-GROUP
    OBJECTS     {
        tFilterPBRDropReason,
        tFilterParmRow,
        tFilterAlarmDescription
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of filter notification
         objects on Nokia SROS series systems."
    ::= { tFilterMIBGroups 21 }

tIPFilterV6v0Group               OBJECT-GROUP
    OBJECTS     {
        tIPFilterRowStatus,
        tIPFilterScope,
        tIPFilterDescription,
        tIPFilterDefaultAction,
        tIPFilterParamsRowStatus,
        tIPFilterParamsLogId,
        tIPFilterParamsDescription,
        tIPFilterParamsAction,
        tIPFilterParamsForwardNH,
        tIPFilterParamsForwardNHIndirect,
        tIPFilterParamsRemarkDSCP,
        tIPFilterParamsRemarkDSCPMask,
        tIPFilterParamsRemarkDot1p,
        tIPFilterParamsSourceIpAddr,
        tIPFilterParamsSourceIpMask,
        tIPFilterParamsDestinationIpAddr,
        tIPFilterParamsDestinationIpMask,
        tIPFilterParamsProtocol,
        tIPFilterParamsSourcePortValue1,
        tIPFilterParamsSourcePortValue2,
        tIPFilterParamsSourcePortOperator,
        tIPFilterParamsDestPortValue1,
        tIPFilterParamsDestPortValue2,
        tIPFilterParamsDestPortOperator,
        tIPFilterParamsDSCP,
        tIPFilterParamsFragment,
        tIPFilterParamsOptionPresent,
        tIPFilterParamsIpOptionValue,
        tIPFilterParamsIpOptionMask,
        tIPFilterParamsMultipleOption,
        tIPFilterParamsTcpSyn,
        tIPFilterParamsTcpAck,
        tIPFilterParamsIcmpCode,
        tIPFilterParamsIcmpType,
        tIPFilterParamsCflowdSample,
        tIPFilterParamsCflowdIfSample,
        tIPFilterParamsForwardNHInterface,
        tIPFilterParamsIngressHitCount,
        tIPFilterParamsEgressHitCount,
        tIPFilterParamsLogInstantiated,
        tIPFilterParamsForwardRedPlcy,
        tIPFilterParamsActiveDest,
        tIPFilterParamsFwdSvcId,
        tIPFilterParamsFwdSapPortId,
        tIPFilterParamsFwdSapEncapVal,
        tIPFilterParamsFwdSdpBind,
        tIPFilterParamsRedirectURL,
        tIPFilterParamsSrcIpFullMask,
        tIPFilterParamsDestIpFullMask,
        tIPFilterParamsIngrHitByteCount,
        tIPFilterParamsEgrHitByteCount
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting IP Filters on Nokia 7x50 ESS/SR series
         systems 6.0 release."
    ::= { tFilterMIBGroups 22 }

tMacFilterV6v0Group              OBJECT-GROUP
    OBJECTS     {
        tMacFilterRowStatus,
        tMacFilterScope,
        tMacFilterDescription,
        tMacFilterDefaultAction,
        tMacFilterParamsRowStatus,
        tMacFilterParamsLogId,
        tMacFilterParamsDescription,
        tMacFilterParamsAction,
        tMacFilterParamsFrameType,
        tMacFilterParamsSrcMAC,
        tMacFilterParamsSrcMACMask,
        tMacFilterParamsDstMAC,
        tMacFilterParamsDstMACMask,
        tMacFilterParamsDot1pValue,
        tMacFilterParamsDot1pMask,
        tMacFilterParamsEtherType,
        tMacFilterParamsDsap,
        tMacFilterParamsDsapMask,
        tMacFilterParamsSsap,
        tMacFilterParamsSsapMask,
        tMacFilterParamsSnapPid,
        tMacFilterParamsSnapOui,
        tMacFilterParamsIngressHitCount,
        tMacFilterParamsEgressHitCount,
        tMacFilterParamsLogInstantiated,
        tMacFilterParamsFwdSvcId,
        tMacFilterParamsFwdSapPortId,
        tMacFilterParamsFwdSapEncapVal,
        tMacFilterParamsFwdSdpBind,
        tMacFilterParamsRedirectURL,
        tMacFilterParamsIngrHitByteCount,
        tMacFilterParamsEgrHitByteCount
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of mac filter objects on
         Nokia SROS series systems 6.0 release."
    ::= { tFilterMIBGroups 23 }

tIPv6FilterV6v0Group             OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterRowStatus,
        tIPv6FilterScope,
        tIPv6FilterDescription,
        tIPv6FilterDefaultAction,
        tIPv6FilterParamsRowStatus,
        tIPv6FilterParamsLogId,
        tIPv6FilterParamsDescription,
        tIPv6FilterParamsAction,
        tIPv6FilterParamsForwardNH,
        tIPv6FilterParamsForwardNHIndirect,
        tIPv6FilterParamsRemarkDSCP,
        tIPv6FilterParamsRemarkDSCPMask,
        tIPv6FilterParamsRemarkDot1p,
        tIPv6FilterParamsSourceIpAddr,
        tIPv6FilterParamsSourceIpMask,
        tIPv6FilterParamsDestinationIpAddr,
        tIPv6FilterParamsDestinationIpMask,
        tIPv6FilterParamsNextHeader,
        tIPv6FilterParamsSourcePortValue1,
        tIPv6FilterParamsSourcePortValue2,
        tIPv6FilterParamsSourcePortOperator,
        tIPv6FilterParamsDestPortValue1,
        tIPv6FilterParamsDestPortValue2,
        tIPv6FilterParamsDestPortOperator,
        tIPv6FilterParamsDSCP,
        tIPv6FilterParamsTcpSyn,
        tIPv6FilterParamsTcpAck,
        tIPv6FilterParamsIcmpCode,
        tIPv6FilterParamsIcmpType,
        tIPv6FilterParamsCflowdSample,
        tIPv6FilterParamsCflowdIfSample,
        tIPv6FilterParamsForwardNHInterface,
        tIPv6FilterParamsIngressHitCount,
        tIPv6FilterParamsEgressHitCount,
        tIPv6FilterParamsLogInstantiated,
        tIPv6FilterParamsForwardRedPlcy,
        tIPv6FilterParamsActiveDest,
        tIPv6FilterParamsIngrHitByteCount,
        tIPv6FilterParamsEgrHitByteCount
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of IPv6 filter objects on
         Nokia SROS series systems."
    ::= { tFilterMIBGroups 24 }

tIPFilterV8v0Group               OBJECT-GROUP
    OBJECTS     {
        tIPFilterRowStatus,
        tIPFilterScope,
        tIPFilterDescription,
        tIPFilterDefaultAction,
        tIPFilterRadiusInsertPt,
        tIPFilterRadiusInsertSize,
        tIPFilterCreditCntrlInsertPt,
        tIPFilterCreditCntrlInsertSize,
        tIPFilterSubInsertHighWmark,
        tIPFilterSubInsertLowWmark,
        tIpFilterCreditCntrlNbrInsertd,
        tIpFilterRadiusNbrInsertd,
        tIPFilterParamsRowStatus,
        tIPFilterParamsLogId,
        tIPFilterParamsDescription,
        tIPFilterParamsAction,
        tIPFilterParamsForwardNH,
        tIPFilterParamsForwardNHIndirect,
        tIPFilterParamsRemarkDSCP,
        tIPFilterParamsRemarkDSCPMask,
        tIPFilterParamsRemarkDot1p,
        tIPFilterParamsSourceIpAddr,
        tIPFilterParamsSourceIpMask,
        tIPFilterParamsDestinationIpAddr,
        tIPFilterParamsDestinationIpMask,
        tIPFilterParamsProtocol,
        tIPFilterParamsSourcePortValue1,
        tIPFilterParamsSourcePortValue2,
        tIPFilterParamsSourcePortOperator,
        tIPFilterParamsDestPortValue1,
        tIPFilterParamsDestPortValue2,
        tIPFilterParamsDestPortOperator,
        tIPFilterParamsDSCP,
        tIPFilterParamsFragment,
        tIPFilterParamsOptionPresent,
        tIPFilterParamsIpOptionValue,
        tIPFilterParamsIpOptionMask,
        tIPFilterParamsMultipleOption,
        tIPFilterParamsTcpSyn,
        tIPFilterParamsTcpAck,
        tIPFilterParamsIcmpCode,
        tIPFilterParamsIcmpType,
        tIPFilterParamsCflowdSample,
        tIPFilterParamsCflowdIfSample,
        tIPFilterParamsForwardNHInterface,
        tIPFilterParamsIngressHitCount,
        tIPFilterParamsEgressHitCount,
        tIPFilterParamsLogInstantiated,
        tIPFilterParamsForwardRedPlcy,
        tIPFilterParamsActiveDest,
        tIPFilterParamsFwdSvcId,
        tIPFilterParamsFwdSapPortId,
        tIPFilterParamsFwdSapEncapVal,
        tIPFilterParamsFwdSdpBind,
        tIPFilterParamsRedirectURL,
        tIPFilterParamsSrcIpFullMask,
        tIPFilterParamsDestIpFullMask,
        tIPFilterParamsIngrHitByteCount,
        tIPFilterParamsEgrHitByteCount,
        tFltrGrpInsrtdEntriesFilterType,
        tFltrGrpInsrtdEntriesFilterId,
        tFltrGrpInsrtdEntriesApplication,
        tFltrGrpInsrtdEntriesLocation,
        tFltrGrpInsrtdEntriesResult,
        tFltrGrpInsrtdEntriesFeedback,
        tFltrGrpInsrtdEntriesExecute
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting IP Filters on Nokia 7x50 ESS/SR series
         systems 8.0 release."
    ::= { tFilterMIBGroups 25 }

tIPv6FilterV8v0Group             OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterRowStatus,
        tIPv6FilterScope,
        tIPv6FilterDescription,
        tIPv6FilterDefaultAction,
        tIPv6FilterRadiusInsertPt,
        tIPv6FilterRadiusInsertSize,
        tIPv6FilterCreditCntrlInsertPt,
        tIPv6FilterCreditCntrlInsertSize,
        tIPv6FilterSubInsertHighWmark,
        tIPv6FilterSubInsertLowWmark,
        tIpv6FilterCreditCntrlNbrInsertd,
        tIpv6FilterRadiusNbrInsertd,
        tIPv6FilterParamsRowStatus,
        tIPv6FilterParamsLogId,
        tIPv6FilterParamsDescription,
        tIPv6FilterParamsAction,
        tIPv6FilterParamsForwardNH,
        tIPv6FilterParamsForwardNHIndirect,
        tIPv6FilterParamsRemarkDSCP,
        tIPv6FilterParamsRemarkDSCPMask,
        tIPv6FilterParamsRemarkDot1p,
        tIPv6FilterParamsSourceIpAddr,
        tIPv6FilterParamsSourceIpMask,
        tIPv6FilterParamsDestinationIpAddr,
        tIPv6FilterParamsDestinationIpMask,
        tIPv6FilterParamsNextHeader,
        tIPv6FilterParamsSourcePortValue1,
        tIPv6FilterParamsSourcePortValue2,
        tIPv6FilterParamsSourcePortOperator,
        tIPv6FilterParamsDestPortValue1,
        tIPv6FilterParamsDestPortValue2,
        tIPv6FilterParamsDestPortOperator,
        tIPv6FilterParamsDSCP,
        tIPv6FilterParamsTcpSyn,
        tIPv6FilterParamsTcpAck,
        tIPv6FilterParamsIcmpCode,
        tIPv6FilterParamsIcmpType,
        tIPv6FilterParamsCflowdSample,
        tIPv6FilterParamsCflowdIfSample,
        tIPv6FilterParamsForwardNHInterface,
        tIPv6FilterParamsIngressHitCount,
        tIPv6FilterParamsEgressHitCount,
        tIPv6FilterParamsLogInstantiated,
        tIPv6FilterParamsForwardRedPlcy,
        tIPv6FilterParamsActiveDest,
        tIPv6FilterParamsIngrHitByteCount,
        tIPv6FilterParamsEgrHitByteCount
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of IPv6 filter objects on
         Nokia SROS series systems."
    ::= { tFilterMIBGroups 26 }

tFilterNotificationObjV8v0Group  OBJECT-GROUP
    OBJECTS     {
        tFilterPBRDropReason,
        tFilterParmRow,
        tFilterAlarmDescription,
        tFilterId,
        tFilterType,
        tFilterSubInsSpaceOwner,
        tFilterThresholdReached
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of filter notification
         objects on Nokia SROS series systems."
    ::= { tFilterMIBGroups 27 }

tFilterNotificationsV8v0Group    NOTIFICATION-GROUP
    NOTIFICATIONS {
        tIPFilterPBRPacketsDrop,
        tFilterSubInsSpaceAlarmRaised,
        tFilterSubInsSpaceAlarmCleared,
        tFilterSubInsFltrEntryDropped
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of notifications supporting management of filter
         notifications on Nokia SROS series systems."
    ::= { tFilterMIBGroups 28 }

tMacFilterV8v0Group              OBJECT-GROUP
    OBJECTS     {
        tMacFilterRowStatus,
        tMacFilterScope,
        tMacFilterDescription,
        tMacFilterDefaultAction,
        tMacFilterParamsRowStatus,
        tMacFilterParamsLogId,
        tMacFilterParamsDescription,
        tMacFilterParamsAction,
        tMacFilterParamsFrameType,
        tMacFilterParamsSrcMAC,
        tMacFilterParamsSrcMACMask,
        tMacFilterParamsDstMAC,
        tMacFilterParamsDstMACMask,
        tMacFilterParamsDot1pValue,
        tMacFilterParamsDot1pMask,
        tMacFilterParamsEtherType,
        tMacFilterParamsDsap,
        tMacFilterParamsDsapMask,
        tMacFilterParamsSsap,
        tMacFilterParamsSsapMask,
        tMacFilterParamsSnapPid,
        tMacFilterParamsSnapOui,
        tMacFilterParamsIngressHitCount,
        tMacFilterParamsEgressHitCount,
        tMacFilterParamsLogInstantiated,
        tMacFilterParamsFwdSvcId,
        tMacFilterParamsFwdSapPortId,
        tMacFilterParamsFwdSapEncapVal,
        tMacFilterParamsFwdSdpBind,
        tMacFilterParamsRedirectURL,
        tMacFilterParamsIngrHitByteCount,
        tMacFilterParamsEgrHitByteCount,
        tMacFilterParamsLowISID,
        tMacFilterParamsHighISID,
        tMacFilterType
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of mac filter objects on
         Nokia SROS series systems 8.0 release."
    ::= { tFilterMIBGroups 29 }

tMacFilterVidFilteringV9v0Group  OBJECT-GROUP
    OBJECTS     {
        tMacFilterParamsInnerTagValue,
        tMacFilterParamsInnerTagMask,
        tMacFilterParamsOuterTagValue,
        tMacFilterParamsOuterTagMask
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of mac VID filtering
         objects on Nokia SROS series systems 9.0 release."
    ::= { tFilterMIBGroups 30 }

tIPFilterV9v0Group               OBJECT-GROUP
    OBJECTS     {
        tIPFilterRowStatus,
        tIPFilterScope,
        tIPFilterDescription,
        tIPFilterDefaultAction,
        tIPFilterRadiusInsertPt,
        tIPFilterRadiusInsertSize,
        tIPFilterCreditCntrlInsertPt,
        tIPFilterCreditCntrlInsertSize,
        tIPFilterSubInsertHighWmark,
        tIPFilterSubInsertLowWmark,
        tIpFilterCreditCntrlNbrInsertd,
        tIpFilterRadiusNbrInsertd,
        tIPFilterParamsRowStatus,
        tIPFilterParamsLogId,
        tIPFilterParamsDescription,
        tIPFilterParamsAction,
        tIPFilterParamsForwardNH,
        tIPFilterParamsForwardNHIndirect,
        tIPFilterParamsRemarkDSCP,
        tIPFilterParamsRemarkDSCPMask,
        tIPFilterParamsRemarkDot1p,
        tIPFilterParamsSourceIpAddr,
        tIPFilterParamsSourceIpMask,
        tIPFilterParamsDestinationIpAddr,
        tIPFilterParamsDestinationIpMask,
        tIPFilterParamsProtocol,
        tIPFilterParamsSourcePortValue1,
        tIPFilterParamsSourcePortValue2,
        tIPFilterParamsSourcePortOperator,
        tIPFilterParamsDestPortValue1,
        tIPFilterParamsDestPortValue2,
        tIPFilterParamsDestPortOperator,
        tIPFilterParamsDSCP,
        tIPFilterParamsFragment,
        tIPFilterParamsOptionPresent,
        tIPFilterParamsIpOptionValue,
        tIPFilterParamsIpOptionMask,
        tIPFilterParamsMultipleOption,
        tIPFilterParamsTcpSyn,
        tIPFilterParamsTcpAck,
        tIPFilterParamsIcmpCode,
        tIPFilterParamsIcmpType,
        tIPFilterParamsCflowdSample,
        tIPFilterParamsCflowdIfSample,
        tIPFilterParamsForwardNHInterface,
        tIPFilterParamsIngressHitCount,
        tIPFilterParamsEgressHitCount,
        tIPFilterParamsLogInstantiated,
        tIPFilterParamsForwardRedPlcy,
        tIPFilterParamsActiveDest,
        tIPFilterParamsFwdSvcId,
        tIPFilterParamsFwdSapPortId,
        tIPFilterParamsFwdSapEncapVal,
        tIPFilterParamsFwdSdpBind,
        tIPFilterParamsRedirectURL,
        tIPFilterParamsSrcIpFullMask,
        tIPFilterParamsDestIpFullMask,
        tIPFilterParamsIngrHitByteCount,
        tIPFilterParamsEgrHitByteCount,
        tFltrGrpInsrtdEntriesFilterType,
        tFltrGrpInsrtdEntriesFilterId,
        tFltrGrpInsrtdEntriesApplication,
        tFltrGrpInsrtdEntriesLocation,
        tFltrGrpInsrtdEntriesResult,
        tFltrGrpInsrtdEntriesFeedback,
        tFltrGrpInsrtdEntriesExecute,
        tIPFilterParamsFwdRtrId,
        tIPFilterParamsSrcRouteOption
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting IP Filters on Nokia 7x50 ESS/SR series
         systems 9.0 release."
    ::= { tFilterMIBGroups 31 }

tFilterNotificationsV9v0Group    NOTIFICATION-GROUP
    NOTIFICATIONS {
        tIPFilterPBRPacketsDrop,
        tFilterSubInsSpaceAlarmRaised,
        tFilterSubInsSpaceAlarmCleared,
        tFilterSubInsFltrEntryDropped,
        tFilterBgpFlowSpecProblem
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of notifications supporting management of filter
         notifications on Nokia SROS series systems."
    ::= { tFilterMIBGroups 32 }

tFilterNotificationObjV9v0Group  OBJECT-GROUP
    OBJECTS     {
        tFilterPBRDropReason,
        tFilterParmRow,
        tFilterAlarmDescription,
        tFilterId,
        tFilterType,
        tFilterSubInsSpaceOwner,
        tFilterThresholdReached,
        tFltrFlowSpecProblem,
        tFltrFlowSpecProblemDescription,
        tFltrFLowSpecNLRI,
        tFltrFlowSpecVrtrId
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of filter notification
         objects on Nokia SROS series systems."
    ::= { tFilterMIBGroups 33 }

tDhcpFilterV9v0Group             OBJECT-GROUP
    OBJECTS     {
        tDhcpFilterTableLastChanged,
        tDhcpFilterRowStatus,
        tDhcpFilterLastChanged,
        tDhcpFilterDescription,
        tDhcpFilterParamsTblLastChanged,
        tDhcpFilterParamsRowStatus,
        tDhcpFilterParamsLastChanged,
        tDhcpFilterParamsOptionNumber,
        tDhcpFilterParamsOptionMatch,
        tDhcpFilterParamsAction
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting DHCP Filters on Nokia 7x50 ESS/SR
         series systems 9.0 release."
    ::= { tFilterMIBGroups 34 }

tIPv6FilterV10v0Group            OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterRowStatus,
        tIPv6FilterScope,
        tIPv6FilterDescription,
        tIPv6FilterDefaultAction,
        tIPv6FilterRadiusInsertPt,
        tIPv6FilterRadiusInsertSize,
        tIPv6FilterCreditCntrlInsertPt,
        tIPv6FilterCreditCntrlInsertSize,
        tIPv6FilterSubInsertHighWmark,
        tIPv6FilterSubInsertLowWmark,
        tIpv6FilterCreditCntrlNbrInsertd,
        tIpv6FilterRadiusNbrInsertd,
        tIPv6FilterParamsRowStatus,
        tIPv6FilterParamsLogId,
        tIPv6FilterParamsDescription,
        tIPv6FilterParamsAction,
        tIPv6FilterParamsForwardNH,
        tIPv6FilterParamsForwardNHIndirect,
        tIPv6FilterParamsRemarkDSCP,
        tIPv6FilterParamsRemarkDSCPMask,
        tIPv6FilterParamsRemarkDot1p,
        tIPv6FilterParamsSourceIpAddr,
        tIPv6FilterParamsSourceIpMask,
        tIPv6FilterParamsDestinationIpAddr,
        tIPv6FilterParamsDestinationIpMask,
        tIPv6FilterParamsNextHeader,
        tIPv6FilterParamsSourcePortValue1,
        tIPv6FilterParamsSourcePortValue2,
        tIPv6FilterParamsSourcePortOperator,
        tIPv6FilterParamsDestPortValue1,
        tIPv6FilterParamsDestPortValue2,
        tIPv6FilterParamsDestPortOperator,
        tIPv6FilterParamsDSCP,
        tIPv6FilterParamsTcpSyn,
        tIPv6FilterParamsTcpAck,
        tIPv6FilterParamsIcmpCode,
        tIPv6FilterParamsIcmpType,
        tIPv6FilterParamsCflowdSample,
        tIPv6FilterParamsCflowdIfSample,
        tIPv6FilterParamsForwardNHInterface,
        tIPv6FilterParamsIngressHitCount,
        tIPv6FilterParamsEgressHitCount,
        tIPv6FilterParamsLogInstantiated,
        tIPv6FilterParamsForwardRedPlcy,
        tIPv6FilterParamsActiveDest,
        tIPv6FilterParamsIngrHitByteCount,
        tIPv6FilterParamsEgrHitByteCount,
        tIPv6FilterParamsFwdSvcId,
        tIPv6FilterParamsFwdSapPortId,
        tIPv6FilterParamsFwdSapEncapVal,
        tIPv6FilterParamsFwdSdpBind
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of IPv6 filter objects on
         Nokia SROS series systems."
    ::= { tFilterMIBGroups 35 }

tFilterNameV10v0Group            OBJECT-GROUP
    OBJECTS     {
        tIpFilterName,
        tIpFilterNameId,
        tIpFilterNameLastChanged,
        tIpFilterNameRowStatus,
        tIpFilterNameTableLastChgd,
        tIpv6FilterName,
        tIpv6FilterNameId,
        tIpv6FilterNameLastChanged,
        tIpv6FilterNameRowStatus,
        tIpv6FilterNameTableLastChgd,
        tMacFilterName,
        tMacFilterNameId,
        tMacFilterNameLastChanged,
        tMacFilterNameRowStatus,
        tMacFilterNameTableLastChgd
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of filter-name objects on
         Nokia SROS series systems."
    ::= { tFilterMIBGroups 36 }

tDhcpFilterV10v0Group            OBJECT-GROUP
    OBJECTS     {
        tDhcpFilterTableLastChanged,
        tDhcpFilterRowStatus,
        tDhcpFilterLastChanged,
        tDhcpFilterDescription,
        tDhcpFilterParamsTblLastChanged,
        tDhcpFilterParamsRowStatus,
        tDhcpFilterParamsLastChanged,
        tDhcpFilterParamsOptionNumber,
        tDhcpFilterParamsOptionMatch,
        tDhcpFilterParamsAction,
        tDhcpFilterParamsOptionValue
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting DHCP Filters on Nokia 7x50 ESS/SR
         series systems 10.0 release."
    ::= { tFilterMIBGroups 37 }

tLiFilterV10v0Group              OBJECT-GROUP
    OBJECTS     {
        tLiReservedBlockRowStatus,
        tLiReservedBlockDescription,
        tLiReservedBlockStart,
        tLiReservedBlockSize,
        tLiReservedBlockLastChanged,
        tLiReservedBlockTableLastChanged,
        tLiReservedBlockFltrRowStatus,
        tLiReservedBlockFltrLastChanged,
        tLiReservedBlockFltrTableLastChg,
        tLiFilterDescription,
        tLiFilterRowStatus,
        tLiFilterLastChanged,
        tLiFilterTableLastChanged,
        tLiFilterAssociationRowStatus,
        tLiFilterAssociationLastChg,
        tLiFilterAssociationTableLastChg,
        tLiMacFilterParamsDescription,
        tLiMacFilterParamsDstMAC,
        tLiMacFilterParamsDstMACMask,
        tLiMacFilterParamsFrameType,
        tLiMacFilterParamsRowStatus,
        tLiMacFilterParamsSrcMAC,
        tLiMacFilterParamsSrcMACMask,
        tLiMacFilterParamsLastChanged,
        tLiMacFilterParamsTableLastChg,
        tLiMacFilterParamsIngrHitCount,
        tLiMacFilterParamsEgrHitCount,
        tLiMacFilterParamsIngrHitBytes,
        tLiMacFilterParamsEgrHitBytes
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of LI filter entries on
         Nokia SROS series systems 10.0 release."
    ::= { tFilterMIBGroups 38 }

tFilterPrefixListV10v0Group      OBJECT-GROUP
    OBJECTS     {
        tFilterPrefixListTableLstChng,
        tFilterPrefixListRowStatus,
        tFilterPrefixListLastChanged,
        tFilterPrefixListDescription,
        tFilterPrefixListEntryTblLstChg,
        tFilterPrefixListEntryRowStatus,
        tIPFilterParamsSrcIpPrefixList,
        tIPFilterParamsDstIpPrefixList
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of IP prefix lists in IP
         filters on Nokia SROS series systems 10.0 release."
    ::= { tFilterMIBGroups 39 }

tIPv6FilterV11v0Group            OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterRowStatus,
        tIPv6FilterScope,
        tIPv6FilterDescription,
        tIPv6FilterDefaultAction,
        tIPv6FilterRadiusInsertPt,
        tIPv6FilterRadiusInsertSize,
        tIPv6FilterCreditCntrlInsertPt,
        tIPv6FilterCreditCntrlInsertSize,
        tIPv6FilterSubInsertHighWmark,
        tIPv6FilterSubInsertLowWmark,
        tIpv6FilterCreditCntrlNbrInsertd,
        tIpv6FilterRadiusNbrInsertd,
        tIPv6FilterHostSharedInsertPt,
        tIPv6FilterHostSharedInsertSize,
        tIpv6FilterHostSharedNbrInsertd,
        tIPv6FilterHostSharedHighWmark,
        tIPv6FilterHostSharedLowWmark,
        tIPv6FilterNbrHostSharedFltrs,
        tIPv6FilterParamsRowStatus,
        tIPv6FilterParamsLogId,
        tIPv6FilterParamsDescription,
        tIPv6FilterParamsAction,
        tIPv6FilterParamsForwardNH,
        tIPv6FilterParamsForwardNHIndirect,
        tIPv6FilterParamsRemarkDSCP,
        tIPv6FilterParamsRemarkDSCPMask,
        tIPv6FilterParamsRemarkDot1p,
        tIPv6FilterParamsSourceIpAddr,
        tIPv6FilterParamsSourceIpMask,
        tIPv6FilterParamsDestinationIpAddr,
        tIPv6FilterParamsDestinationIpMask,
        tIPv6FilterParamsNextHeader,
        tIPv6FilterParamsSourcePortValue1,
        tIPv6FilterParamsSourcePortValue2,
        tIPv6FilterParamsSourcePortOperator,
        tIPv6FilterParamsDestPortValue1,
        tIPv6FilterParamsDestPortValue2,
        tIPv6FilterParamsDestPortOperator,
        tIPv6FilterParamsDSCP,
        tIPv6FilterParamsTcpSyn,
        tIPv6FilterParamsTcpAck,
        tIPv6FilterParamsIcmpCode,
        tIPv6FilterParamsIcmpType,
        tIPv6FilterParamsCflowdSample,
        tIPv6FilterParamsCflowdIfSample,
        tIPv6FilterParamsForwardNHInterface,
        tIPv6FilterParamsIngressHitCount,
        tIPv6FilterParamsEgressHitCount,
        tIPv6FilterParamsLogInstantiated,
        tIPv6FilterParamsForwardRedPlcy,
        tIPv6FilterParamsActiveDest,
        tIPv6FilterParamsIngrHitByteCount,
        tIPv6FilterParamsEgrHitByteCount,
        tIPv6FilterParamsFwdSvcId,
        tIPv6FilterParamsFwdSapPortId,
        tIPv6FilterParamsFwdSapEncapVal,
        tIPv6FilterParamsFwdSdpBind,
        tIPv6FilterParamsRedirectURL,
        tIPv6FilterParamsSrcIpPrefixList,
        tIPv6FilterParamsDstIpPrefixList,
        tIPv6FilterParamsFragment,
        tIPv6FilterParamsHopByHopOpt,
        tIPv6FilterParamsRoutingType0,
        tIPv6FilterParamsPortSelector,
        tIPv6FilterParamsSrcPortList,
        tIPv6FilterParamsDstPortList,
        tIPv6FilterParamsFwdRtrId
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of IPv6 filter objects on
         Nokia SROS series systems."
    ::= { tFilterMIBGroups 40 }

tFilterEmbeddedInsertV11v0Group  OBJECT-GROUP
    OBJECTS     {
        tFilterEmbeddedRefRowStatus,
        tFilterEmbeddedRefTableLstChg,
        tFilterEmbeddedRefOperState,
        tFilterEmbeddedRefAdminState,
        tFltrEmbedRefInfEntryCnt,
        tFltrEmbedRefInfEntryCntInsrtd,
        tFltrEmbedEntryInsrtEntryId,
        tFltrEmbedEntryRefOperState
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the creation of embedded filters for
         Nokia SROS systems 11.0 release."
    ::= { tFilterMIBGroups 41 }

tFilterPortListV11v0Group        OBJECT-GROUP
    OBJECTS     {
        tFilterPortListTableLstChng,
        tFilterPortListRowStatus,
        tFilterPortListLastChanged,
        tFilterPortListDescription,
        tFilterPortListEntryTblLstChg,
        tFilterPortListEntryRowStatus
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the management of port lists for
         filters on Nokia SROS series systems 11.0 release."
    ::= { tFilterMIBGroups 42 }

tFilterPrefixListV11v0Group      OBJECT-GROUP
    OBJECTS     {
        tFilterPrefixListTableLstChng,
        tFilterPrefixListRowStatus,
        tFilterPrefixListLastChanged,
        tFilterPrefixListDescription,
        tFilterPrefixListEntryTblLstChg,
        tFilterPrefixListEntryRowStatus,
        tIPFilterParamsSrcIpPrefixList,
        tIPFilterParamsDstIpPrefixList,
        tFilterApplyPathTableLstChng,
        tFilterApplyPathRowStatus,
        tFilterApplyPathLastChanged,
        tFilterApplyPathMatch1,
        tFilterApplyPathMatch2
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of IP prefix lists in IP
         filters on Nokia SROS series systems 11.0 release."
    ::= { tFilterMIBGroups 43 }

tIPFilterV11v0Group              OBJECT-GROUP
    OBJECTS     {
        tIPFilterRowStatus,
        tIPFilterScope,
        tIPFilterDescription,
        tIPFilterDefaultAction,
        tIPFilterRadiusInsertPt,
        tIPFilterRadiusInsertSize,
        tIPFilterCreditCntrlInsertPt,
        tIPFilterCreditCntrlInsertSize,
        tIPFilterSubInsertHighWmark,
        tIPFilterSubInsertLowWmark,
        tIpFilterCreditCntrlNbrInsertd,
        tIpFilterRadiusNbrInsertd,
        tIPFilterHostSharedInsertPt,
        tIPFilterHostSharedInsertSize,
        tIpFilterHostSharedNbrInsertd,
        tIPFilterHostSharedHighWmark,
        tIPFilterHostSharedLowWmark,
        tIPFilterNbrHostSharedFltrs,
        tIPFilterParamsRowStatus,
        tIPFilterParamsLogId,
        tIPFilterParamsDescription,
        tIPFilterParamsAction,
        tIPFilterParamsForwardNH,
        tIPFilterParamsForwardNHIndirect,
        tIPFilterParamsRemarkDSCP,
        tIPFilterParamsRemarkDSCPMask,
        tIPFilterParamsRemarkDot1p,
        tIPFilterParamsSourceIpAddr,
        tIPFilterParamsSourceIpMask,
        tIPFilterParamsDestinationIpAddr,
        tIPFilterParamsDestinationIpMask,
        tIPFilterParamsProtocol,
        tIPFilterParamsSourcePortValue1,
        tIPFilterParamsSourcePortValue2,
        tIPFilterParamsSourcePortOperator,
        tIPFilterParamsDestPortValue1,
        tIPFilterParamsDestPortValue2,
        tIPFilterParamsDestPortOperator,
        tIPFilterParamsDSCP,
        tIPFilterParamsFragment,
        tIPFilterParamsOptionPresent,
        tIPFilterParamsIpOptionValue,
        tIPFilterParamsIpOptionMask,
        tIPFilterParamsMultipleOption,
        tIPFilterParamsTcpSyn,
        tIPFilterParamsTcpAck,
        tIPFilterParamsIcmpCode,
        tIPFilterParamsIcmpType,
        tIPFilterParamsCflowdSample,
        tIPFilterParamsCflowdIfSample,
        tIPFilterParamsForwardNHInterface,
        tIPFilterParamsIngressHitCount,
        tIPFilterParamsEgressHitCount,
        tIPFilterParamsLogInstantiated,
        tIPFilterParamsForwardRedPlcy,
        tIPFilterParamsActiveDest,
        tIPFilterParamsFwdSvcId,
        tIPFilterParamsFwdSapPortId,
        tIPFilterParamsFwdSapEncapVal,
        tIPFilterParamsFwdSdpBind,
        tIPFilterParamsRedirectURL,
        tIPFilterParamsSrcIpFullMask,
        tIPFilterParamsDestIpFullMask,
        tIPFilterParamsIngrHitByteCount,
        tIPFilterParamsEgrHitByteCount,
        tFltrGrpInsrtdEntriesFilterType,
        tFltrGrpInsrtdEntriesFilterId,
        tFltrGrpInsrtdEntriesApplication,
        tFltrGrpInsrtdEntriesLocation,
        tFltrGrpInsrtdEntriesResult,
        tFltrGrpInsrtdEntriesFeedback,
        tFltrGrpInsrtdEntriesExecute,
        tIPFilterParamsFwdRtrId,
        tIPFilterParamsSrcRouteOption,
        tIPFilterParamsPortSelector,
        tIPFilterParamsSrcPortList,
        tIPFilterParamsDstPortList,
        tIPFilterParamsExtTbleLstChgd,
        tIPFilterParamsExtLastChanged,
        tIPFilterParamsExtPktLenVal1,
        tIPFilterParamsExtPktLenVal2,
        tIPFilterParamsExtPktLenOper
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting IP Filters on Nokia 7x50 ESS/SR series
         systems 11.0 release."
    ::= { tFilterMIBGroups 44 }

tFilterNotificationsV11v0Group   NOTIFICATION-GROUP
    NOTIFICATIONS {
        tIPFilterPBRPacketsDrop,
        tFilterSubInsSpaceAlarmRaised,
        tFilterSubInsSpaceAlarmCleared,
        tFilterSubInsFltrEntryDropped,
        tFilterBgpFlowSpecProblem,
        tFilterApplyPathProblem,
        tFilterRadSharedFltrAlarmRaised,
        tFilterRadSharedFltrAlarmClear,
        tFilterEmbeddingOperStateChange
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting management of filter
         notifications on Nokia SROS series systems."
    ::= { tFilterMIBGroups 45 }

tFilterNotificationObjV11v0Group OBJECT-GROUP
    OBJECTS     {
        tFilterPBRDropReason,
        tFilterParmRow,
        tFilterAlarmDescription,
        tFilterId,
        tFilterType,
        tFilterSubInsSpaceOwner,
        tFilterThresholdReached,
        tFltrFlowSpecProblem,
        tFltrFlowSpecProblemDescription,
        tFltrFLowSpecNLRI,
        tFltrFlowSpecVrtrId,
        tFltrPrefixListType,
        tFltrPrefixListName,
        tFltrApplyPathSource,
        tFltrApplyPathIndex,
        tFltrNotifDescription
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of filter notification
         objects on Nokia SROS series systems."
    ::= { tFilterMIBGroups 46 }

tIPFilterV12v0Group              OBJECT-GROUP
    OBJECTS     {
        tIPFilterRowStatus,
        tIPFilterScope,
        tIPFilterDescription,
        tIPFilterDefaultAction,
        tIPFilterRadiusInsertPt,
        tIPFilterRadiusInsertSize,
        tIPFilterCreditCntrlInsertPt,
        tIPFilterCreditCntrlInsertSize,
        tIPFilterSubInsertHighWmark,
        tIPFilterSubInsertLowWmark,
        tIpFilterCreditCntrlNbrInsertd,
        tIpFilterRadiusNbrInsertd,
        tIPFilterHostSharedInsertPt,
        tIPFilterHostSharedInsertSize,
        tIpFilterHostSharedNbrInsertd,
        tIPFilterHostSharedHighWmark,
        tIPFilterHostSharedLowWmark,
        tIPFilterNbrHostSharedFltrs,
        tIPFilterParamsRowStatus,
        tIPFilterParamsLogId,
        tIPFilterParamsDescription,
        tIPFilterParamsAction,
        tIPFilterParamsForwardNH,
        tIPFilterParamsForwardNHIndirect,
        tIPFilterParamsRemarkDSCP,
        tIPFilterParamsRemarkDSCPMask,
        tIPFilterParamsRemarkDot1p,
        tIPFilterParamsSourceIpAddr,
        tIPFilterParamsSourceIpMask,
        tIPFilterParamsDestinationIpAddr,
        tIPFilterParamsDestinationIpMask,
        tIPFilterParamsProtocol,
        tIPFilterParamsSourcePortValue1,
        tIPFilterParamsSourcePortValue2,
        tIPFilterParamsSourcePortOperator,
        tIPFilterParamsDestPortValue1,
        tIPFilterParamsDestPortValue2,
        tIPFilterParamsDestPortOperator,
        tIPFilterParamsDSCP,
        tIPFilterParamsFragment,
        tIPFilterParamsOptionPresent,
        tIPFilterParamsIpOptionValue,
        tIPFilterParamsIpOptionMask,
        tIPFilterParamsMultipleOption,
        tIPFilterParamsTcpSyn,
        tIPFilterParamsTcpAck,
        tIPFilterParamsIcmpCode,
        tIPFilterParamsIcmpType,
        tIPFilterParamsCflowdSample,
        tIPFilterParamsCflowdIfSample,
        tIPFilterParamsForwardNHInterface,
        tIPFilterParamsIngressHitCount,
        tIPFilterParamsEgressHitCount,
        tIPFilterParamsLogInstantiated,
        tIPFilterParamsForwardRedPlcy,
        tIPFilterParamsActiveDest,
        tIPFilterParamsFwdSvcId,
        tIPFilterParamsFwdSapPortId,
        tIPFilterParamsFwdSapEncapVal,
        tIPFilterParamsFwdSdpBind,
        tIPFilterParamsRedirectURL,
        tIPFilterParamsSrcIpFullMask,
        tIPFilterParamsDestIpFullMask,
        tIPFilterParamsIngrHitByteCount,
        tIPFilterParamsEgrHitByteCount,
        tFltrGrpInsrtdEntriesFilterType,
        tFltrGrpInsrtdEntriesFilterId,
        tFltrGrpInsrtdEntriesApplication,
        tFltrGrpInsrtdEntriesLocation,
        tFltrGrpInsrtdEntriesResult,
        tFltrGrpInsrtdEntriesFeedback,
        tFltrGrpInsrtdEntriesExecute,
        tIPFilterParamsFwdRtrId,
        tIPFilterParamsSrcRouteOption,
        tIPFilterParamsPortSelector,
        tIPFilterParamsSrcPortList,
        tIPFilterParamsDstPortList,
        tIPFilterParamsExtTbleLstChgd,
        tIPFilterParamsExtLastChanged,
        tIPFilterParamsExtPktLenVal1,
        tIPFilterParamsExtPktLenVal2,
        tIPFilterParamsExtPktLenOper,
        tIPFilterParamsRdirAllwRadOvrd,
        tIPFilterParamsNatPolicyName,
        tIPFilterParamsFwdLsp,
        tIPFilterParamsFwdLspRtrId
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting IP Filters on Nokia 7x50 ESS/SR series
         systems 12.0 release. This group was made obsolete in release 14.0."
    ::= { tFilterMIBGroups 47 }

tIPv6FilterV12v0Group            OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterRowStatus,
        tIPv6FilterScope,
        tIPv6FilterDescription,
        tIPv6FilterDefaultAction,
        tIPv6FilterRadiusInsertPt,
        tIPv6FilterRadiusInsertSize,
        tIPv6FilterCreditCntrlInsertPt,
        tIPv6FilterCreditCntrlInsertSize,
        tIPv6FilterSubInsertHighWmark,
        tIPv6FilterSubInsertLowWmark,
        tIpv6FilterCreditCntrlNbrInsertd,
        tIpv6FilterRadiusNbrInsertd,
        tIPv6FilterHostSharedInsertPt,
        tIPv6FilterHostSharedInsertSize,
        tIpv6FilterHostSharedNbrInsertd,
        tIPv6FilterHostSharedHighWmark,
        tIPv6FilterHostSharedLowWmark,
        tIPv6FilterNbrHostSharedFltrs,
        tIPv6FilterParamsRowStatus,
        tIPv6FilterParamsLogId,
        tIPv6FilterParamsDescription,
        tIPv6FilterParamsAction,
        tIPv6FilterParamsForwardNH,
        tIPv6FilterParamsForwardNHIndirect,
        tIPv6FilterParamsRemarkDSCP,
        tIPv6FilterParamsRemarkDSCPMask,
        tIPv6FilterParamsRemarkDot1p,
        tIPv6FilterParamsSourceIpAddr,
        tIPv6FilterParamsSourceIpMask,
        tIPv6FilterParamsDestinationIpAddr,
        tIPv6FilterParamsDestinationIpMask,
        tIPv6FilterParamsNextHeader,
        tIPv6FilterParamsSourcePortValue1,
        tIPv6FilterParamsSourcePortValue2,
        tIPv6FilterParamsSourcePortOperator,
        tIPv6FilterParamsDestPortValue1,
        tIPv6FilterParamsDestPortValue2,
        tIPv6FilterParamsDestPortOperator,
        tIPv6FilterParamsDSCP,
        tIPv6FilterParamsTcpSyn,
        tIPv6FilterParamsTcpAck,
        tIPv6FilterParamsIcmpCode,
        tIPv6FilterParamsIcmpType,
        tIPv6FilterParamsCflowdSample,
        tIPv6FilterParamsCflowdIfSample,
        tIPv6FilterParamsForwardNHInterface,
        tIPv6FilterParamsIngressHitCount,
        tIPv6FilterParamsEgressHitCount,
        tIPv6FilterParamsLogInstantiated,
        tIPv6FilterParamsForwardRedPlcy,
        tIPv6FilterParamsActiveDest,
        tIPv6FilterParamsIngrHitByteCount,
        tIPv6FilterParamsEgrHitByteCount,
        tIPv6FilterParamsFwdSvcId,
        tIPv6FilterParamsFwdSapPortId,
        tIPv6FilterParamsFwdSapEncapVal,
        tIPv6FilterParamsFwdSdpBind,
        tIPv6FilterParamsRedirectURL,
        tIPv6FilterParamsSrcIpPrefixList,
        tIPv6FilterParamsDstIpPrefixList,
        tIPv6FilterParamsFragment,
        tIPv6FilterParamsHopByHopOpt,
        tIPv6FilterParamsRoutingType0,
        tIPv6FilterParamsPortSelector,
        tIPv6FilterParamsSrcPortList,
        tIPv6FilterParamsDstPortList,
        tIPv6FilterParamsRdirAllwRadOvrd,
        tIPv6FilterParamsFwdRtrId,
        tIPv6FilterParamsSrcIpFullMask,
        tIPv6FilterParamsDstIpFullMask,
        tIPv6FilterParamsNatPolicyName,
        tIPv6FilterParamsFlowLabel,
        tIPv6FilterParamsFlowLabelMask,
        tIPv6FilterParamsFwdLspRtrId,
        tIPv6FilterParamsFwdLsp,
        tIPv6FilterParamsExtTbleLstChgd,
        tIPv6FilterParamsExtLastChanged,
        tIPv6FilterParamsExtAhExtHdr,
        tIPv6FilterParamsExtEspExtHdr,
        tIPv6FilterParamsExtNatType
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of IPv6 filter objects on
         Nokia 7x50 ESS/SR series systems 12.0 release. This group was made
         obsolete in release 14.0."
    ::= { tFilterMIBGroups 48 }

tLiFilterV12v0Group              OBJECT-GROUP
    OBJECTS     {
        tLiReservedBlockRowStatus,
        tLiReservedBlockDescription,
        tLiReservedBlockStart,
        tLiReservedBlockSize,
        tLiReservedBlockLastChanged,
        tLiReservedBlockTableLastChanged,
        tLiReservedBlockFltrRowStatus,
        tLiReservedBlockFltrLastChanged,
        tLiReservedBlockFltrTableLastChg,
        tLiFilterDescription,
        tLiFilterRowStatus,
        tLiFilterLastChanged,
        tLiFilterTableLastChanged,
        tLiFilterAssociationRowStatus,
        tLiFilterAssociationLastChg,
        tLiFilterAssociationTableLastChg,
        tLiMacFilterParamsDescription,
        tLiMacFilterParamsDstMAC,
        tLiMacFilterParamsDstMACMask,
        tLiMacFilterParamsFrameType,
        tLiMacFilterParamsRowStatus,
        tLiMacFilterParamsSrcMAC,
        tLiMacFilterParamsSrcMACMask,
        tLiMacFilterParamsLastChanged,
        tLiMacFilterParamsTableLastChg,
        tLiMacFilterParamsIngrHitCount,
        tLiMacFilterParamsEgrHitCount,
        tLiMacFilterParamsIngrHitBytes,
        tLiMacFilterParamsEgrHitBytes,
        tLiIpFilterParamsTableLastChg,
        tLiIpFilterParamsLastChanged,
        tLiIpFilterParamsRowStatus,
        tLiIpFilterParamsDescription,
        tLiIpFilterParamsSrcIpAddrType,
        tLiIpFilterParamsSrcIpAddr,
        tLiIpFilterParamsSrcIpFullMask,
        tLiIpFilterParamsDstIpAddrType,
        tLiIpFilterParamsDstIpAddr,
        tLiIpFilterParamsDstIpFullMask,
        tLiIpFilterParamsProtocolNextHdr,
        tLiIpFilterParamsSrcPortValue1,
        tLiIpFilterParamsSrcPortValue2,
        tLiIpFilterParamsSrcPortOper,
        tLiIpFilterParamsDstPortValue1,
        tLiIpFilterParamsDstPortValue2,
        tLiIpFilterParamsDstPortOper,
        tLiIpFltrParamsInfIngrHitCount,
        tLiIpFltrParamsInfEgrHitCount,
        tLiIpFltrParamsInfIngrHitBytes,
        tLiIpFltrParamsInfEgrHitBytes
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of LI filter entries on
         Nokia SROS series systems 12.0 release."
    ::= { tFilterMIBGroups 49 }

tFilterEmbeddedInsertV12v0Group  OBJECT-GROUP
    OBJECTS     {
        tFilterEmbedOpenflowRowStatus,
        tFilterEmbedOpenflowTableLstChg,
        tFilterEmbedOpenflowOperState,
        tFilterEmbedOpenflowAdminState,
        tFltrEmbedOfInfoEntryCnt,
        tFltrEmbedOfInfoEntryCntInsrtd,
        tFltrEmbedOfEntryInsrtEntryId,
        tFltrEmbedOfEntryInsrtEntryState
    }
    STATUS      current
    DESCRIPTION
        "The group of new objects supporting the creation of embedded filters
         for Nokia SROS systems 12.0 release."
    ::= { tFilterMIBGroups 50 }

tFilterNotificationsV12v0Group   NOTIFICATION-GROUP
    NOTIFICATIONS {
        tFilterEmbedOpenflowOperStateChg,
        tFilterTmsEvent
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of notifications supporting management of filter
         notifications on Nokia SROS series systems."
    ::= { tFilterMIBGroups 51 }

tFilterRedirectPolicyV13v0Group  OBJECT-GROUP
    OBJECTS     {
        tFilterRPVrtrId,
        tFilterRPRowStatus,
        tFilterRPDescription,
        tFilterRPAdminState,
        tFilterRPActiveDestAddrType,
        tFilterRPActiveDestAddr,
        tFilterRPDstStickiness,
        tFilterRPBestDstAddrType,
        tFilterRPBestDstAddr,
        tFilterRPStickinessHoldRemain,
        tFilterRPlcyDstTableLastChg,
        tFltrRPDstLastChanged,
        tFltrRPDstRowStatus,
        tFltrRPDstDescription,
        tFltrRPDstAdminPriority,
        tFltrRPDstOperPriority,
        tFltrRPDstAdminState,
        tFltrRPDstOperState,
        tFilterRPlcyPingTestTableLastChg,
        tFltrRPPingTLastChanged,
        tFltrRPPingTRowStatus,
        tFltrRPPingTInterval,
        tFltrRPPingTTimeout,
        tFltrRPPingTDropCount,
        tFltrRPPingTHoldDown,
        tFltrRPPingTHoldDownRemain,
        tFltrRPPingTLastActionTime,
        tFltrRPPingTLastAction,
        tFilterRPlcySNMPTestTableLastChg,
        tFltrRPSnmpTLastChanged,
        tFltrRPSnmpTRowStatus,
        tFltrRPSnmpTOID,
        tFltrRPSnmpTCommunity,
        tFltrRPSnmpTSnmpVersion,
        tFltrRPSnmpTInterval,
        tFltrRPSnmpTTimeout,
        tFltrRPSnmpTDropCount,
        tFltrRPSnmpTHoldDown,
        tFltrRPSnmpTHoldDownRemain,
        tFltrRPSnmpTLastActionTime,
        tFltrRPSnmpTLastOID,
        tFltrRPSnmpTLastType,
        tFltrRPSnmpTLastCounter32Val,
        tFltrRPSnmpTLastUnsigned32Val,
        tFltrRPSnmpTLastTimeTicksVal,
        tFltrRPSnmpTLastInt32Val,
        tFltrRPSnmpTLastOctetStringVal,
        tFltrRPSnmpTLastIpAddressVal,
        tFltrRPSnmpTLastOidVal,
        tFltrRPSnmpTLastCounter64Val,
        tFltrRPSnmpTLastOpaqueVal,
        tFltrRPSnmpTLastAction,
        tFltrRPSnmpTLastPrioChange,
        tFltrRPSnmpTNextRespIndex,
        tFilterRPlcySNMPRespTableLastChg,
        tFltrRPSnmpRspLastChanged,
        tFltrRPSnmpRspRowStatus,
        tFltrRPSnmpRspAction,
        tFltrRPSnmpRspPrioChange,
        tFltrRPSnmpRspOID,
        tFltrRPSnmpRspType,
        tFltrRPSnmpRspCounter32Val,
        tFltrRPSnmpRspUnsigned32Val,
        tFltrRPSnmpRspTimeTicksVal,
        tFltrRPSnmpRspInt32Val,
        tFltrRPSnmpRspOctetStringVal,
        tFltrRPSnmpRspIpAddressVal,
        tFltrRPSnmpRspOidVal,
        tFltrRPSnmpRspCounter64Val,
        tFltrRPSnmpRspOpaqueVal,
        tFilterRPlcyURLTestTableLastChg,
        tFltrRPUrlTLastChanged,
        tFltrRPUrlTRowStatus,
        tFltrRPUrlTUrl,
        tFltrRPUrlTHttpVersion,
        tFltrRPUrlTInterval,
        tFltrRPUrlTTimeout,
        tFltrRPUrlTDropCount,
        tFltrRPUrlTHoldDown,
        tFltrRPUrlTHoldDownRemain,
        tFltrRPUrlTLastActionTime,
        tFltrRPUrlTLastRetCode,
        tFltrRPUrlTLastAction,
        tFltrRPUrlTLastPrioChange,
        tFilterRPlcyURLRespTableLastChg,
        tFltrRPUrlTRspLastChanged,
        tFltrRPUrlTRspRowStatus,
        tFltrRPUrlTRspAction,
        tFltrRPUrlTRspPrioChange,
        tFilterRPlcyUcastRtTTableLastChg,
        tFltrRPUcastRtTLastChanged,
        tFltrRPUcastRtTRowStatus,
        tFltrRPUcastRtTLastActionTime,
        tFltrRPUcastRtTLastAction
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of filter redirect policy
         objects on Nokia SROS series systems new in 13.0 series."
    ::= { tFilterMIBGroups 52 }

tFilterNotificationObjV12v0Group OBJECT-GROUP
    OBJECTS     {
        tFilterPBRDropReason,
        tFilterParmRow,
        tFilterAlarmDescription,
        tFilterId,
        tFilterType,
        tFilterSubInsSpaceOwner,
        tFilterThresholdReached,
        tFltrFlowSpecProblem,
        tFltrFlowSpecProblemDescription,
        tFltrFLowSpecNLRI,
        tFltrFlowSpecVrtrId,
        tFltrPrefixListType,
        tFltrPrefixListName,
        tFltrApplyPathSource,
        tFltrApplyPathIndex,
        tFltrNotifDescription,
        tFltrMdaId
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of filter notification
         objects on Nokia SROS series systems."
    ::= { tFilterMIBGroups 53 }

tIPFilterV13v0Group              OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsExtTbleLstChgd,
        tIPFilterParamsExtLastChanged,
        tIPFilterSharedPccRuleInsrtPt,
        tIPFilterSharedPccRuleInsrtSize,
        tIPFilterSharedPccRuleNbrInsrtd,
        tIPFilterChainToSystemFilter,
        tIPFilterParamsExtTTLVal1,
        tIPFilterParamsExtTTLVal2,
        tIPFilterParamsExtTTLOper,
        tIPFilterParamsExtEgressPBR,
        tIPFilterParamsExtEsi,
        tIPFilterParamsExtFwdEsiSvcId,
        tIPFilterParamsExtFwdEsiVRtrId,
        tIPFilterParamsExtFwdEsiSFIp,
        tIPFilterParamsExtPbrDwnActOvr,
        tIPFilterParamsExtFwdEsiVasIf
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting IP Filters on Nokia 7x50 ESS/SR series
         systems 13.0 release."
    ::= { tFilterMIBGroups 54 }

tIPv6FilterV13v0Group            OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterParamsExtPktLenVal1,
        tIPv6FilterParamsExtPktLenVal2,
        tIPv6FilterParamsExtPktLenOper,
        tIPv6FilterSharedPccRuleInsrtPt,
        tIPv6FilterSharedPccRuleInsrtSiz,
        tIPv6FilterSharedPccRuleNbrInsrt,
        tIPv6FilterChainToSystemFilter,
        tIPv6FilterParamsExtHopLimitVal1,
        tIPv6FilterParamsExtHopLimitVal2,
        tIPv6FilterParamsExtHopLimitOper,
        tIPv6FilterParamsExtEgressPBR,
        tIPv6FilterParamsExtEsi,
        tIPv6FilterParamsExtFwdEsiSvcId,
        tIPv6FilterParamsExtFwdEsiVRtrId,
        tIPv6FilterParamsExtFwdEsiSFIp,
        tIPv6FilterParamsExtPbrDwnActOvr,
        tIPv6FilterParamsExtFwdEsiVasIf
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting IPv6 Filters on Nokia 7x50 ESS/SR
         series systems 13.0 release."
    ::= { tFilterMIBGroups 55 }

tFilterRPlcyV13v0ObsoleteGroup   OBJECT-GROUP
    OBJECTS     {
        tFilterRPActiveDest,
        tFilterRDRowStatus,
        tFilterRDDescription,
        tFilterRDAdminPriority,
        tFilterRDOperPriority,
        tFilterRDAdminState,
        tFilterRDOperState,
        tFilterRSTRowStatus,
        tFilterRSTOID,
        tFilterRSTCommunity,
        tFilterRSTSNMPVersion,
        tFilterRSTInterval,
        tFilterRSTTimeout,
        tFilterRSTDropCount,
        tFilterRSTHoldDown,
        tFilterRSTHoldDownRemain,
        tFilterRSTLastActionTime,
        tFilterRSTLastOID,
        tFilterRSTLastType,
        tFilterRSTLastCounter32Val,
        tFilterRSTLastUnsigned32Val,
        tFilterRSTLastTimeTicksVal,
        tFilterRSTLastInt32Val,
        tFilterRSTLastOctetStringVal,
        tFilterRSTLastIpAddressVal,
        tFilterRSTLastOidVal,
        tFilterRSTLastCounter64Val,
        tFilterRSTLastOpaqueVal,
        tFilterRSTLastAction,
        tFilterRSTLastPrioChange,
        tFilterRSTNextRespIndex,
        tFilterRSTRespRowStatus,
        tFilterRSTRespAction,
        tFilterRSTRespPrioChange,
        tFilterRSTRespOID,
        tFilterRSTRespType,
        tFilterRSTCounter32Val,
        tFilterRSTUnsigned32Val,
        tFilterRSTTimeTicksVal,
        tFilterRSTInt32Val,
        tFilterRSTOctetStringVal,
        tFilterRSTIpAddressVal,
        tFilterRSTOidVal,
        tFilterRSTCounter64Val,
        tFilterRSTOpaqueVal,
        tFilterRUTRowStatus,
        tFilterRUTURL,
        tFilterRUTHTTPVersion,
        tFilterRUTInterval,
        tFilterRUTTimeout,
        tFilterRUTDropCount,
        tFilterRUTHoldDown,
        tFilterRUTHoldDownRemain,
        tFilterRUTLastActionTime,
        tFilterRUTLastRetCode,
        tFilterRUTLastAction,
        tFilterRUTLastPrioChange,
        tFilterRUTRespRowStatus,
        tFilterRUTRespAction,
        tFilterRUTRespPrioChange,
        tFilterRPTRowStatus,
        tFilterRPTInterval,
        tFilterRPTTimeout,
        tFilterRPTDropCount,
        tFilterRPTHoldDown,
        tFilterRPTHoldDownRemain,
        tFilterRPTLastActionTime,
        tFilterRPTLastAction
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted objects in 13.0 supporting management of filter
         redirect policy on Nokia SROS series systems."
    ::= { tFilterMIBGroups 56 }

tFilterSystemFilterV13v0Group    OBJECT-GROUP
    OBJECTS     {
        tFilterSystemFilterTableLastChg,
        tFilterSystemFilterLastChanged,
        tFilterSystemFilterRowStatus
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting system filter policies on Nokia 7x50
         ESS/SR series systems 13.0 release."
    ::= { tFilterMIBGroups 57 }

tFilterEmbeddedInsertV13v0Group  OBJECT-GROUP
    OBJECTS     {
        tFilterEmbedOflowSvcContext,
        tFilterEmbedOflowSapContextPort,
        tFilterEmbedOflowSapContextEncap,
        tFilterEmbedOflowContextType
    }
    STATUS      current
    DESCRIPTION
        "The group of new objects supporting the creation of embedded filters
         for Nokia SROS systems 13.0 release."
    ::= { tFilterMIBGroups 58 }

tDhcpFilterV13v0Group            OBJECT-GROUP
    OBJECTS     {
        tDhcpFilterDefAction,
        tDhcp6FilterTblLastChanged,
        tDhcp6FilterRowStatus,
        tDhcp6FilterLastChanged,
        tDhcp6FilterDescription,
        tDhcp6FilterDefAction,
        tDhcp6FilterParamsTblLastChanged,
        tDhcp6FilterParamsRowStatus,
        tDhcp6FilterParamsLastChanged,
        tDhcp6FilterParamsOptionNumber,
        tDhcp6FilterParamsOptionMatch,
        tDhcp6FilterParamsAction,
        tDhcp6FilterParamsOptionValue,
        tDhcp6FilterDefActionFlags,
        tDhcp6FilterParamsActionFlags
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting DHCP Filters on Nokia 7x50 ESS/SR
         series systems 13.0 release."
    ::= { tFilterMIBGroups 59 }

tMacFilterV13v0Group             OBJECT-GROUP
    OBJECTS     {
        tMacFilterParamsEsi,
        tMacFilterParamsFwdEsiSvcId,
        tMacFilterParamsPbrDwnActOvr
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting MAC Filters on Nokia 7x50 ESS/SR
         series systems 13.0 release."
    ::= { tFilterMIBGroups 60 }

tFilterNotificationsV14v0Group   NOTIFICATION-GROUP
    NOTIFICATIONS {
        tFilterEmbedFlowspecOperStateChg,
        tFilterEmbedVsdOperStateChg
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of notifications supporting management of filter
         notifications on Nokia SROS series systems 14.0 release."
    ::= { tFilterMIBGroups 61 }

tFilterEmbedFlowspecGroup        OBJECT-GROUP
    OBJECTS     {
        tFilterEmbedFlowspecTableLstChg,
        tFilterEmbedFlowspecRowStatus,
        tFilterEmbedFlowspecLastChanged,
        tFilterEmbedFlowspecRtrId,
        tFilterEmbedFlowspecAdminState,
        tFilterEmbedFlowspecOperState,
        tFltrEmbFlowSpecInfoFltrId,
        tFltrEmbFlowSpecInfoEntryCnt,
        tFltrEmbFlowSpecInfoEntryCntIns,
        tFltrEmbFlowspecEntryInsEntryId,
        tFltrEmbFlowspecEntryOperState
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting embedding of flowspec rules on Nokia
         SROS systems 14.0 release."
    ::= { tFilterMIBGroups 62 }

tFilterIPvXRedundantActionGroup  OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrEntryActionTblLChg,
        tIPvXFltrEntryActRowStatus,
        tIPvXFltrEntryActLastChanged,
        tIPvXFltrEntryActAction,
        tIPvXFltrEntryActFwdNHIpAddrType,
        tIPvXFltrEntryActFwdNHIpAddr,
        tIPvXFltrEntryActFwdNHIndirect,
        tIPvXFltrEntryActFwdNHInterface,
        tIPvXFltrEntryActFwdRedPlcy,
        tIPvXFltrEntryActFwdSapPortId,
        tIPvXFltrEntryActFwdSapEncapVal,
        tIPvXFltrEntryActFwdSdpBind,
        tIPvXFltrEntryActRedirectURL,
        tIPvXFltrEntryActRdirAllwRadOvr,
        tIPvXFltrEntryActFwdRtrId,
        tIPvXFltrEntryActNatPolicyName,
        tIPvXFltrEntryActNatType,
        tIPvXFltrEntryActFwdLsp,
        tIPvXFltrEntryActFwdLspRtrId,
        tIPvXFltrEntryActPktLenVal1,
        tIPvXFltrEntryActPktLenVal2,
        tIPvXFltrEntryActPktLenOper,
        tIPvXFltrEntryActTTLVal1,
        tIPvXFltrEntryActTTLVal2,
        tIPvXFltrEntryActTTLOper,
        tIPvXFltrEntryActEsi,
        tIPvXFltrEntryActFwdEsiSvcId,
        tIPvXFltrEntryActFwdEsiVRtrId,
        tIPvXFltrEntryActFwdEsiSFIpType,
        tIPvXFltrEntryActFwdEsiSFIp,
        tIPvXFltrEntryActFwdEsiVasIf,
        tIPFilterParamsExtStickyDst,
        tIPFilterParamsExtDownloadAct,
        tIPFilterParamsExtHoldRemain,
        tIPv6FilterParamsExtStickyDst,
        tIPv6FilterParamsExtDownloadAct,
        tIPv6FilterParamsExtHoldRemain,
        tIPvXFltrEntryActPbrTargetStatus,
        tIPvXFltrEntryActRateLimit,
        tIPvXFltrEntryActRateLimitMbs,
        tIPvXFltrEntryActRateLimitPps
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting redundant ip filter actions on Nokia
         7x50 ESS/SR series systems 14.0 release."
    ::= { tFilterMIBGroups 63 }

tFilterMacRedundantActionGroup   OBJECT-GROUP
    OBJECTS     {
        tMacFltrEntryActionTblLChg,
        tMacFltrEntryActRowStatus,
        tMacFltrEntryActLastChanged,
        tMacFltrEntryActAction,
        tMacFltrEntryActRowStatus,
        tMacFltrEntryActFwdSapPortId,
        tMacFltrEntryActFwdSapEncapVal,
        tMacFltrEntryActFwdSdpBind,
        tMacFltrEntryActRedirectURL,
        tMacFltrEntryActEsi,
        tMacFltrEntryActFwdEsiSvcId,
        tMacFilterParamsStickyDst,
        tMacFilterParamsHoldRemain,
        tMacFilterParamsDownloadAct,
        tMacFltrEntryActPbrTargetStatus,
        tMacFltrEntryActRateLimit
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting redundant mac filter actions on Nokia
         7x50 ESS/SR series systems 14.0 release."
    ::= { tFilterMIBGroups 64 }

tFilterEmbeddedRefGroup          OBJECT-GROUP
    OBJECTS     {
        tFilterEmbeddedRefLastChanged
    }
    STATUS      current
    DESCRIPTION
        "The group of objects extending support of embedding of filters Nokia
         7x50 ESS/SR series systems 14.0 release."
    ::= { tFilterMIBGroups 66 }

tFilterTimeRangeObsoletedGroup   OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsTimeRangeName,
        tIPFilterParamsTimeRangeState,
        tMacFilterParamsTimeRangeName,
        tMacFilterParamsTimeRangeState,
        tIPv6FilterParamsTimeRangeName,
        tIPv6FilterParamsTimeRangeState
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted objects in 14.0 supporting Time Of Day / Time
         Range features on Nokia SROS series systems."
    ::= { tFilterMIBGroups 67 }

tFilterObsoletedNotifsGroup      NOTIFICATION-GROUP
    NOTIFICATIONS {
        tFilterEntryActivationFailed,
        tFilterEntryActivationRestored
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted notifications for filter features on Nokia SROS
         series systems."
    ::= { tFilterMIBGroups 68 }

tFilterEntryStatGroup            OBJECT-GROUP
    OBJECTS     {
        tFltrEntryStatIngHitCnt,
        tFltrEntryStatEgrHitCnt,
        tFltrEntryStatIngHitCntB,
        tFltrEntryStatEgrHitCntB,
        tFltrEntryStatRateLmtIngHitCnt,
        tFltrEntryStatRateLmtIngDrop,
        tFltrEntryStatRateLmtIngFwd,
        tFltrEntryStatRateLmtIngHitCntB,
        tFltrEntryStatRateLmtIngDropB,
        tFltrEntryStatRateLmtIngFwdB,
        tFltrEntryStatRateLmtEgrHitCnt,
        tFltrEntryStatRateLmtEgrDrop,
        tFltrEntryStatRateLmtEgrFwd,
        tFltrEntryStatRateLmtEgrHitCntB,
        tFltrEntryStatRateLmtEgrDropB,
        tFltrEntryStatRateLmtEgrFwdB
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter action rate-limit on Nokia 7x50
         ESS/SR series systems 14.0 release."
    ::= { tFilterMIBGroups 69 }

tFilterRemarkDscpGroup           OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrEntryActRemarkDSCP
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter remark dscp action on Nokia
         7x50 ESS/SR series systems 14.0 release."
    ::= { tFilterMIBGroups 70 }

tIPFilterV14v0Group              OBJECT-GROUP
    OBJECTS     {
        tIPFilterRowStatus,
        tIPFilterScope,
        tIPFilterDescription,
        tIPFilterDefaultAction,
        tIPFilterRadiusInsertPt,
        tIPFilterRadiusInsertSize,
        tIPFilterCreditCntrlInsertPt,
        tIPFilterCreditCntrlInsertSize,
        tIPFilterSubInsertHighWmark,
        tIPFilterSubInsertLowWmark,
        tIpFilterCreditCntrlNbrInsertd,
        tIpFilterRadiusNbrInsertd,
        tIPFilterHostSharedInsertPt,
        tIPFilterHostSharedInsertSize,
        tIpFilterHostSharedNbrInsertd,
        tIPFilterHostSharedHighWmark,
        tIPFilterHostSharedLowWmark,
        tIPFilterNbrHostSharedFltrs,
        tIPFilterParamsRowStatus,
        tIPFilterParamsLogId,
        tIPFilterParamsDescription,
        tIPFilterParamsAction,
        tIPFilterParamsForwardNH,
        tIPFilterParamsForwardNHIndirect,
        tIPFilterParamsSourceIpAddr,
        tIPFilterParamsSourceIpMask,
        tIPFilterParamsDestinationIpAddr,
        tIPFilterParamsDestinationIpMask,
        tIPFilterParamsProtocol,
        tIPFilterParamsSourcePortValue1,
        tIPFilterParamsSourcePortValue2,
        tIPFilterParamsSourcePortOperator,
        tIPFilterParamsDestPortValue1,
        tIPFilterParamsDestPortValue2,
        tIPFilterParamsDestPortOperator,
        tIPFilterParamsDSCP,
        tIPFilterParamsFragment,
        tIPFilterParamsOptionPresent,
        tIPFilterParamsIpOptionValue,
        tIPFilterParamsIpOptionMask,
        tIPFilterParamsMultipleOption,
        tIPFilterParamsTcpSyn,
        tIPFilterParamsTcpAck,
        tIPFilterParamsIcmpCode,
        tIPFilterParamsIcmpType,
        tIPFilterParamsCflowdSample,
        tIPFilterParamsCflowdIfSample,
        tIPFilterParamsForwardNHInterface,
        tIPFilterParamsIngressHitCount,
        tIPFilterParamsEgressHitCount,
        tIPFilterParamsLogInstantiated,
        tIPFilterParamsForwardRedPlcy,
        tIPFilterParamsActiveDest,
        tIPFilterParamsFwdSvcId,
        tIPFilterParamsFwdSapPortId,
        tIPFilterParamsFwdSapEncapVal,
        tIPFilterParamsFwdSdpBind,
        tIPFilterParamsRedirectURL,
        tIPFilterParamsSrcIpFullMask,
        tIPFilterParamsDestIpFullMask,
        tIPFilterParamsIngrHitByteCount,
        tIPFilterParamsEgrHitByteCount,
        tFltrGrpInsrtdEntriesFilterType,
        tFltrGrpInsrtdEntriesFilterId,
        tFltrGrpInsrtdEntriesApplication,
        tFltrGrpInsrtdEntriesLocation,
        tFltrGrpInsrtdEntriesResult,
        tFltrGrpInsrtdEntriesFeedback,
        tFltrGrpInsrtdEntriesExecute,
        tIPFilterParamsFwdRtrId,
        tIPFilterParamsSrcRouteOption,
        tIPFilterParamsPortSelector,
        tIPFilterParamsSrcPortList,
        tIPFilterParamsDstPortList,
        tIPFilterParamsExtTbleLstChgd,
        tIPFilterParamsExtLastChanged,
        tIPFilterParamsExtPktLenVal1,
        tIPFilterParamsExtPktLenVal2,
        tIPFilterParamsExtPktLenOper,
        tIPFilterParamsRdirAllwRadOvrd,
        tIPFilterParamsNatPolicyName,
        tIPFilterParamsFwdLsp,
        tIPFilterParamsFwdLspRtrId
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting IP Filters on Nokia 7x50 ESS/SR series
         systems 14.0 release."
    ::= { tFilterMIBGroups 71 }

tIPv6FilterV14v0Group            OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterRowStatus,
        tIPv6FilterScope,
        tIPv6FilterDescription,
        tIPv6FilterDefaultAction,
        tIPv6FilterRadiusInsertPt,
        tIPv6FilterRadiusInsertSize,
        tIPv6FilterCreditCntrlInsertPt,
        tIPv6FilterCreditCntrlInsertSize,
        tIPv6FilterSubInsertHighWmark,
        tIPv6FilterSubInsertLowWmark,
        tIpv6FilterCreditCntrlNbrInsertd,
        tIpv6FilterRadiusNbrInsertd,
        tIPv6FilterHostSharedInsertPt,
        tIPv6FilterHostSharedInsertSize,
        tIpv6FilterHostSharedNbrInsertd,
        tIPv6FilterHostSharedHighWmark,
        tIPv6FilterHostSharedLowWmark,
        tIPv6FilterNbrHostSharedFltrs,
        tIPv6FilterParamsRowStatus,
        tIPv6FilterParamsLogId,
        tIPv6FilterParamsDescription,
        tIPv6FilterParamsAction,
        tIPv6FilterParamsForwardNH,
        tIPv6FilterParamsForwardNHIndirect,
        tIPv6FilterParamsSourceIpAddr,
        tIPv6FilterParamsSourceIpMask,
        tIPv6FilterParamsDestinationIpAddr,
        tIPv6FilterParamsDestinationIpMask,
        tIPv6FilterParamsNextHeader,
        tIPv6FilterParamsSourcePortValue1,
        tIPv6FilterParamsSourcePortValue2,
        tIPv6FilterParamsSourcePortOperator,
        tIPv6FilterParamsDestPortValue1,
        tIPv6FilterParamsDestPortValue2,
        tIPv6FilterParamsDestPortOperator,
        tIPv6FilterParamsDSCP,
        tIPv6FilterParamsTcpSyn,
        tIPv6FilterParamsTcpAck,
        tIPv6FilterParamsIcmpCode,
        tIPv6FilterParamsIcmpType,
        tIPv6FilterParamsCflowdSample,
        tIPv6FilterParamsCflowdIfSample,
        tIPv6FilterParamsForwardNHInterface,
        tIPv6FilterParamsIngressHitCount,
        tIPv6FilterParamsEgressHitCount,
        tIPv6FilterParamsLogInstantiated,
        tIPv6FilterParamsForwardRedPlcy,
        tIPv6FilterParamsActiveDest,
        tIPv6FilterParamsIngrHitByteCount,
        tIPv6FilterParamsEgrHitByteCount,
        tIPv6FilterParamsFwdSvcId,
        tIPv6FilterParamsFwdSapPortId,
        tIPv6FilterParamsFwdSapEncapVal,
        tIPv6FilterParamsFwdSdpBind,
        tIPv6FilterParamsRedirectURL,
        tIPv6FilterParamsSrcIpPrefixList,
        tIPv6FilterParamsDstIpPrefixList,
        tIPv6FilterParamsFragment,
        tIPv6FilterParamsHopByHopOpt,
        tIPv6FilterParamsRoutingType0,
        tIPv6FilterParamsPortSelector,
        tIPv6FilterParamsSrcPortList,
        tIPv6FilterParamsDstPortList,
        tIPv6FilterParamsRdirAllwRadOvrd,
        tIPv6FilterParamsFwdRtrId,
        tIPv6FilterParamsSrcIpFullMask,
        tIPv6FilterParamsDstIpFullMask,
        tIPv6FilterParamsNatPolicyName,
        tIPv6FilterParamsFlowLabel,
        tIPv6FilterParamsFlowLabelMask,
        tIPv6FilterParamsFwdLspRtrId,
        tIPv6FilterParamsFwdLsp,
        tIPv6FilterParamsExtTbleLstChgd,
        tIPv6FilterParamsExtLastChanged,
        tIPv6FilterParamsExtAhExtHdr,
        tIPv6FilterParamsExtEspExtHdr,
        tIPv6FilterParamsExtNatType
    }
    STATUS      obsolete
    DESCRIPTION
        "The group of objects supporting management of IPv6 filter objects on
         Nokia 7x50 ESS/SR series systems 14.0 release."
    ::= { tFilterMIBGroups 72 }

tFilterParamsObsoletedGroup      OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsRemarkDSCP,
        tIPFilterParamsRemarkDSCPMask,
        tIPFilterParamsRemarkDot1p,
        tIPv6FilterParamsRemarkDSCP,
        tIPv6FilterParamsRemarkDSCPMask,
        tIPv6FilterParamsRemarkDot1p
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of IP/IPv6 filter on Nokia
         7x50 ESS/SR series systems which were obsoleted in 14.0 release."
    ::= { tFilterMIBGroups 73 }

tFilterRemarkDscpExtGroup        OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrEntryActActionExt
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter remark dscp extended action on
         Nokia 7x50 ESS/SR series systems 14.0 release."
    ::= { tFilterMIBGroups 74 }

tFilterPrefListRtrBgpPeersGroup  OBJECT-GROUP
    OBJECTS     {
        tFilterApplyPathVRtrId
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter bgp peer prefix lists in router
         context on Nokia 7x50 ESS/SR series systems 15.0 release."
    ::= { tFilterMIBGroups 75 }

tFilterPrefListInfoGroup         OBJECT-GROUP
    OBJECTS     {
        tFltrPrefListInfoPrefixOwner,
        tFltrPrefListInfoPrefixProg
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting prefix list info table on Nokia 7x50
         ESS/SR series systems."
    ::= { tFilterMIBGroups 76 }

tFilterForwardVprnTargetGroup    OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrEntryActFwdVprnTgtBgNHT,
        tIPvXFltrEntryActFwdVprnTgtBgNH,
        tIPvXFltrEntryActFwdVprnTgtRtrId,
        tIPvXFltrEntryActFwdVprnTgtAdPxT,
        tIPvXFltrEntryActFwdVprnTgtAdPx,
        tIPvXFltrEntryActFwdVprnTgtAdPxL,
        tIPvXFltrEntryActFwdVprnTgtLspId
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter forward to vprn target action
         on Nokia 7x50 ESS/SR series systems 15.0 release."
    ::= { tFilterMIBGroups 77 }

tFilterNotificationsV15v0Group   NOTIFICATION-GROUP
    NOTIFICATIONS {
        tFilterEmbedOpenflowOperStateChg
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting management of filter
         notifications on Nokia SROS series systems release 15.0."
    ::= { tFilterMIBGroups 80 }

tFilterObsoleteNotifsGroup       NOTIFICATION-GROUP
    NOTIFICATIONS {
        tFilterTmsEvent
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted notifications supporting management of filter
         notifications on Nokia SROS series systems release 15.0."
    ::= { tFilterMIBGroups 81 }

tFilterFwdBondingConnectionGroup OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrEntryActFwdBondingConn
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter action forward with specified
         preferred bonding connection on Nokia 7x50 ESS/SR series systems 15.0
         release."
    ::= { tFilterMIBGroups 82 }

tFilterSelectiveFlowspecGroup    OBJECT-GROUP
    OBJECTS     {
        tFilterEmbedFlowspecGroupId,
        tFilterEmbedFlowspecInsEntryId,
        tFilterEmbedFlowspecEntryOpState
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting selective flowspec filter objects on
         Nokia 7x50 ESS/SR series systems 15.0 release."
    ::= { tFilterMIBGroups 83 }

tFilterMatchTcpFlagsGroup        OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsExtTcpFin,
        tIPFilterParamsExtTcpRst,
        tIPFilterParamsExtTcpPsh,
        tIPFilterParamsExtTcpUrg,
        tIPFilterParamsExtTcpEce,
        tIPFilterParamsExtTcpCwr,
        tIPFilterParamsExtTcpNs,
        tIPv6FilterParamsExtTcpFin,
        tIPv6FilterParamsExtTcpRst,
        tIPv6FilterParamsExtTcpPsh,
        tIPv6FilterParamsExtTcpUrg,
        tIPv6FilterParamsExtTcpEce,
        tIPv6FilterParamsExtTcpCwr,
        tIPv6FilterParamsExtTcpNs
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting not present TCP flags match criteria
         till 15.0 release on Nokia 7x50 ESS/SR series systems 16.0 release."
    ::= { tFilterMIBGroups 84 }

tFilterActionFc                  OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrEntryActFcName
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter action fc on Nokia 7x50 ESS/SR
         series systems 16.0 release."
    ::= { tFilterMIBGroups 86 }

tFilterRPPingSrcAddressGroup     OBJECT-GROUP
    OBJECTS     {
        tFilterRPPingSrcAddressAddrType,
        tFilterRPPingSrcAddressAddr
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter redirect policy ping test
         source address setting on Nokia 7x50 ESS/SR series systems 16.0
         release."
    ::= { tFilterMIBGroups 87 }

tFilterRPActiveDstChangeNotifGrp NOTIFICATION-GROUP
    NOTIFICATIONS {
        tFilterRPActiveDestChangeEvent
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting filter redirect policy
         destination change on Nokia 7x50 ESS/SR series systems 16.0 release."
    ::= { tFilterMIBGroups 88 }

tFilterRPActiveDstChangeGrp      OBJECT-GROUP
    OBJECTS     {
        tFilterRPNotifyDestChange
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter redirect policy destination
         change events on Nokia 7x50 ESS/SR series systems 16.0 release."
    ::= { tFilterMIBGroups 89 }

tFilterRPlcyBindingGroup         OBJECT-GROUP
    OBJECTS     {
        tFilterRPlcyBindingTableLastChg,
        tFilterRPlcyBindingLastChange,
        tFilterRPlcyBindingRowStatus,
        tFilterRPlcyBindingOperator,
        tFilterRPlcyBindingOperState,
        tFilterRPlcyBindingDestTableLCh,
        tFilterRPlcyBindingDestRowStatus,
        tFilterRPlcyBindingDestOperState
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter redirect policy fate sharing on
         Nokia 7x50 ESS/SR series systems 16.0 release."
    ::= { tFilterMIBGroups 90 }

tFltrGreTunTempGroup             OBJECT-GROUP
    OBJECTS     {
        tFltrGreTunTempTableLastChg,
        tFltrGreTunTempLastChanged,
        tFltrGreTunTempDescription,
        tFltrGreTunTempIpv4SrcAddr,
        tFltrGreTunTempIpv4GreKeyIfIndex,
        tFltrGreTunTempIpv4SkipTllDecr,
        tFltrGreTunTempRowStatus,
        tFltrGreTunTempIpv4DstTblLstChg,
        tFltrGreTunTempIpv4DstLstChg,
        tFltrGreTunTempIpv4DstRowStatus,
        tIPvXFltrEntryActFwdGreTun
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter gre tunnel template objects on
         Nokia 7x50 ESS/SR series systems 16.0 release."
    ::= { tFilterMIBGroups 91 }

tFltrPrefListPrefExcludeGrp      OBJECT-GROUP
    OBJECTS     {
        tFltrPrefListPrefExclTblLstChg,
        tFltrPrefListPrefExclLastChg,
        tFltrPrefListPrefExclRowStatus
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter prefix-exclude objects on Nokia
         7x50 ESS/SR series systems 16.0 release."
    ::= { tFilterMIBGroups 92 }

fltrMdAutoIdV16v0Group           OBJECT-GROUP
    OBJECTS     {
        fltrMdAutoIdFilterRangeStart,
        fltrMdAutoIdFilterRangeEnd,
        fltrMdAutoIdIPv4FilterCount,
        fltrMdAutoIdIPv6FilterCount,
        fltrMdAutoIdMacFilterCount
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of model-driven CLI auto
         range of identifiers in Nokia SROS series systems in release 16.0."
    ::= { tFilterMIBGroups 93 }

tFltrPatternMatchGroup           OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrEntryActCondExpression,
        tIPvXFltrEntryActCondExpMask,
        tIPvXFltrEntryActCondOffsetType,
        tIPvXFltrEntryActCondOffsetVal
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting pattern match in Nokia SROS series
         systems in release 16.0."
    ::= { tFilterMIBGroups 94 }

tFilterRedirectPolicyV19v0Group  OBJECT-GROUP
    OBJECTS     {
        tFilterRPVrtrId,
        tFilterRPRowStatus,
        tFilterRPDescription,
        tFilterRPAdminState,
        tFilterRPActiveDestAddrType,
        tFilterRPActiveDestAddr,
        tFilterRPDstStickiness,
        tFilterRPBestDstAddrType,
        tFilterRPBestDstAddr,
        tFilterRPStickinessHoldRemain,
        tFilterRPlcyDstTableLastChg,
        tFltrRPDstLastChanged,
        tFltrRPDstRowStatus,
        tFltrRPDstDescription,
        tFltrRPDstAdminPriority,
        tFltrRPDstOperPriority,
        tFltrRPDstAdminState,
        tFltrRPDstOperState,
        tFilterRPlcyPingTestTableLastChg,
        tFltrRPPingTLastChanged,
        tFltrRPPingTRowStatus,
        tFltrRPPingTInterval,
        tFltrRPPingTTimeout,
        tFltrRPPingTDropCount,
        tFltrRPPingTHoldDown,
        tFltrRPPingTHoldDownRemain,
        tFltrRPPingTLastActionTime,
        tFltrRPPingTLastAction,
        tFilterRPlcyUcastRtTTableLastChg,
        tFltrRPUcastRtTLastChanged,
        tFltrRPUcastRtTRowStatus,
        tFltrRPUcastRtTLastActionTime,
        tFltrRPUcastRtTLastAction
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of filter redirect policy
         objects on Nokia SROS series systems new in 19.0 series."
    ::= { tFilterMIBGroups 95 }

tFltrRPTestV19v0ObsoleteGroup    OBJECT-GROUP
    OBJECTS     {
        tFilterRPlcySNMPRespTableLastChg,
        tFilterRPlcySNMPTestTableLastChg,
        tFilterRPlcyURLRespTableLastChg,
        tFilterRPlcyURLTestTableLastChg,
        tFltrRPSnmpRspAction,
        tFltrRPSnmpRspCounter32Val,
        tFltrRPSnmpRspCounter64Val,
        tFltrRPSnmpRspInt32Val,
        tFltrRPSnmpRspIpAddressVal,
        tFltrRPSnmpRspLastChanged,
        tFltrRPSnmpRspOID,
        tFltrRPSnmpRspOctetStringVal,
        tFltrRPSnmpRspOidVal,
        tFltrRPSnmpRspOpaqueVal,
        tFltrRPSnmpRspPrioChange,
        tFltrRPSnmpRspRowStatus,
        tFltrRPSnmpRspTimeTicksVal,
        tFltrRPSnmpRspType,
        tFltrRPSnmpRspUnsigned32Val,
        tFltrRPSnmpTCommunity,
        tFltrRPSnmpTDropCount,
        tFltrRPSnmpTHoldDown,
        tFltrRPSnmpTHoldDownRemain,
        tFltrRPSnmpTInterval,
        tFltrRPSnmpTLastAction,
        tFltrRPSnmpTLastActionTime,
        tFltrRPSnmpTLastChanged,
        tFltrRPSnmpTLastCounter32Val,
        tFltrRPSnmpTLastCounter64Val,
        tFltrRPSnmpTLastInt32Val,
        tFltrRPSnmpTLastIpAddressVal,
        tFltrRPSnmpTLastOID,
        tFltrRPSnmpTLastOctetStringVal,
        tFltrRPSnmpTLastOidVal,
        tFltrRPSnmpTLastOpaqueVal,
        tFltrRPSnmpTLastPrioChange,
        tFltrRPSnmpTLastTimeTicksVal,
        tFltrRPSnmpTLastType,
        tFltrRPSnmpTLastUnsigned32Val,
        tFltrRPSnmpTNextRespIndex,
        tFltrRPSnmpTOID,
        tFltrRPSnmpTRowStatus,
        tFltrRPSnmpTSnmpVersion,
        tFltrRPSnmpTTimeout,
        tFltrRPUrlTDropCount,
        tFltrRPUrlTHoldDown,
        tFltrRPUrlTHoldDownRemain,
        tFltrRPUrlTHttpVersion,
        tFltrRPUrlTInterval,
        tFltrRPUrlTLastAction,
        tFltrRPUrlTLastActionTime,
        tFltrRPUrlTLastChanged,
        tFltrRPUrlTLastPrioChange,
        tFltrRPUrlTLastRetCode,
        tFltrRPUrlTRowStatus,
        tFltrRPUrlTRspAction,
        tFltrRPUrlTRspLastChanged,
        tFltrRPUrlTRspPrioChange,
        tFltrRPUrlTRspRowStatus,
        tFltrRPUrlTTimeout,
        tFltrRPUrlTUrl
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted objects in 19.0 supporting management of filter
         redirect policy SNMP and URL tests on Nokia SROS series systems."
    ::= { tFilterMIBGroups 96 }

tFltrCAMTypeGroup                OBJECT-GROUP
    OBJECTS     {
        tIPFilterType,
        tIPv6FilterType
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting CAM Type for IP-IPv6 Policy in Nokia
         SROS series systems in release 19.5."
    ::= { tFilterMIBGroups 97 }

tFltrMatchMacForIPvXGroup        OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsExtSrcMac,
        tIPFilterParamsExtSrcMacMask,
        tIPv6FilterParamsExtSrcMac,
        tIPv6FilterParamsExtSrcMacMask
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting Src-MAC Criteria for IP-IPv6 Policy in
         Nokia SROS series systems in release 19.5."
    ::= { tFilterMIBGroups 98 }

tFltrMatchPacketLengthGroup      OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsExtMxPktLenVal1,
        tIPFilterParamsExtMxPktLenVal2,
        tIPFilterParamsExtMxPktLenOper,
        tIPv6FilterParamsExtMxPktLenVal1,
        tIPv6FilterParamsExtMxPktLenVal2,
        tIPv6FilterParamsExtMxPktLenOper
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting Packet-Length Criteria for IP-IPv6
         Policy in Nokia SROS series systems in release 19.5."
    ::= { tFilterMIBGroups 99 }

tFltrFilterNameInLIGroup         OBJECT-GROUP
    OBJECTS     {
        tLiRsvdBlockFltrAssocTableLChg,
        tLiRsvdBlockFltrAssocRowStatus,
        tLiRsvdBlockFltrAssocLastChanged
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting association of LI reserved block with
         filter via filter name in Nokia SROS series systems in release 19.5."
    ::= { tFilterMIBGroups 100 }

tLiFltrAssocFltrNameGroup        OBJECT-GROUP
    OBJECTS     {
        tLiFltrAssocFltrNameTableLastChg,
        tLiFltrAssocFltrNameRowStatus,
        tLiFltrAssocFltrNameLastChg
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting association of LI filter with existing
         or not existing normal filter via filter name in Nokia SROS series
         systems in release 19.10."
    ::= { tFilterMIBGroups 102 }

tFltrIPv6ExceptionV19v0Group     OBJECT-GROUP
    OBJECTS     {
        tIPv6ExceptionRowStatus,
        tIPv6ExceptionDescription,
        tIPv6ExceptionName,
        tIPv6ExceptionNameId,
        tIPv6ExcParamsRowStatus,
        tIPv6ExcParamsDescription,
        tIPv6ExcParamsNextHeader,
        tIPv6ExcParamsSrcIpAddr,
        tIPv6ExcParamsSrcIpMask,
        tIPv6ExcParamsSrcIpFullMask,
        tIPv6ExcParamsSrcIpPrefixList,
        tIPv6ExcParamsDstIpAddr,
        tIPv6ExcParamsDstIpMask,
        tIPv6ExcParamsDstIpFullMask,
        tIPv6ExcParamsDstIpPrefixList,
        tIPv6ExcParamsSourcePortValue1,
        tIPv6ExcParamsSourcePortValue2,
        tIPv6ExcParamsSourcePortOperator,
        tIPv6ExcParamsSourcePortList,
        tIPv6ExcParamsDestPortValue1,
        tIPv6ExcParamsDestPortValue2,
        tIPv6ExcParamsDestPortOperator,
        tIPv6ExcParamsDestPortList,
        tIPv6ExcParamsPortSelector,
        tIPv6ExcParamsIcmpCode,
        tIPv6ExcParamsIcmpType,
        tIPv6ExcParamsIngressHitCount,
        tIPv6ExcParamsEgressHitCount,
        tIPv6ExcParamsIngrHitByteCount,
        tIPv6ExcParamsEgrHitByteCount
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting IPv6 exception filters in Nokia SROS
         series systems in release 19.10."
    ::= { tFilterMIBGroups 103 }

tFltrFwdMplsPlcyEndptGrp         OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrFwdMplsPlcyEndptAddrTp,
        tIPvXFltrFwdMplsPlcyEndptAddr
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting forwarding to a tunnel identified by
         an MPLS forwarding policy endpoint for IP-IPv6 in Nokia SROS series
         systems in release 19.10."
    ::= { tFilterMIBGroups 104 }

tFltrFwdSrtePlcyEndptColorGrp    OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrFwdSrtePlcyEndptAddrTp,
        tIPvXFltrFwdSrtePlcyEndptAddr,
        tIPvXFltrFwdSrtePlcyColor
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting forwarding to a tunnel identified by
         an SR-TE policy endpoint and color for IP-IPv6 in Nokia SROS series
         systems in release 19.10."
    ::= { tFilterMIBGroups 105 }

tLiFltrMatchFragmentGroup        OBJECT-GROUP
    OBJECTS     {
        tLiIpFilterParamsFragment
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting LI filter fragment matching in Nokia
         SROS series systems in release 20.2."
    ::= { tFilterMIBGroups 106 }

fltrMdAutoIdV20v0Group           OBJECT-GROUP
    OBJECTS     {
        fltrMdAutoIdIPv4ExceptionCount,
        fltrMdAutoIdIPv6ExceptionCount
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of model-driven CLI auto
         range of identifiers in Nokia SROS series systems in release 20.2."
    ::= { tFilterMIBGroups 107 }

tFilterMatchProtocolListGroup    OBJECT-GROUP
    OBJECTS     {
        tFltrProtocolListTableLstChng,
        tFltrProtocolListRowStatus,
        tFltrProtocolListLastChanged,
        tFltrProtocolListDescription,
        tFltrProtocolListItemTblLstChg,
        tFltrProtocolListItemRowStatus,
        tIPFilterParamsExtProtocolList,
        tIPv6FilterParamsExtProtocolList
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the management of protocol lists for
         filters on Nokia SROS series systems."
    ::= { tFilterMIBGroups 108 }

tFilterMatchDestClassGroup       OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsExtDestClass,
        tIPv6FilterParamsExtDestClass
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the management of BGP destination
         class filtering on Nokia SROS series systems."
    ::= { tFilterMIBGroups 109 }

tFilterL2AwareNatBypassGroup     OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrActL2AwareNatBypass
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the l2-aware-nat-bypass filter action
         on Nokia SROS series systems."
    ::= { tFilterMIBGroups 110 }

tFltrLiRsvdBlockRangeChgNotifGrp NOTIFICATION-GROUP
    NOTIFICATIONS {
        tFltrLiRsvdBlockRangeChangeEvent
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting filter LI reserved block range
         change on Nokia 7x50 ESS/SR series systems 20.0 release."
    ::= { tFilterMIBGroups 111 }

tFltrCflowdSampleProfileGroup    OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsExtSampleProf,
        tIPv6FilterParamsExtSampleProf
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter cflowd sample profile on Nokia
         7x50 ESS/SR series systems 20.7 release."
    ::= { tFilterMIBGroups 112 }

tFltrEntryCollectStatsIPvXGroup  OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsExtCollectStats,
        tIPv6FilterParamsExtCollectStats
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter entry statistic collection on
         Nokia 7x50 ESS/SR series systems 21.2 release."
    ::= { tFilterMIBGroups 113 }

tFltrEntryCollectStatsMacGroup   OBJECT-GROUP
    OBJECTS     {
        tMacFilterParamsCollectStats
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter entry statistic collection on
         Nokia 7x50 ESS/SR series systems 21.10 release."
    ::= { tFilterMIBGroups 114 }

tFilterMacFltrActionGroupV21     OBJECT-GROUP
    OBJECTS     {
        tMacFltrEntryActFcName
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting mac-filter entry FC on Nokia 7x50
         ESS/SR series systems 21.10 release."
    ::= { tFilterMIBGroups 115 }

tFltrParamsActionObsoleteGroup   OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsAction,
        tIPFilterParamsForwardNH,
        tIPFilterParamsForwardNHIndirect,
        tIPFilterParamsForwardNHInterface,
        tIPFilterParamsForwardRedPlcy,
        tIPFilterParamsFwdSapPortId,
        tIPFilterParamsFwdSapEncapVal,
        tIPFilterParamsFwdSdpBind,
        tIPFilterParamsRedirectURL,
        tIPFilterParamsFwdRtrId,
        tIPFilterParamsRdirAllwRadOvrd,
        tIPFilterParamsNatPolicyName,
        tIPFilterParamsFwdLsp,
        tIPFilterParamsFwdLspRtrId,
        tMacFilterParamsAction,
        tMacFilterParamsFwdSapPortId,
        tMacFilterParamsFwdSapEncapVal,
        tMacFilterParamsFwdSdpBind,
        tMacFilterParamsRedirectURL,
        tMacFilterParamsEsi,
        tMacFilterParamsFwdEsiSvcId,
        tIPv6FilterParamsAction,
        tIPv6FilterParamsForwardNH,
        tIPv6FilterParamsForwardNHIndirect,
        tIPv6FilterParamsForwardNHInterface,
        tIPv6FilterParamsForwardRedPlcy,
        tIPv6FilterParamsFwdSapPortId,
        tIPv6FilterParamsFwdSapEncapVal,
        tIPv6FilterParamsFwdSdpBind,
        tIPv6FilterParamsRedirectURL,
        tIPv6FilterParamsRdirAllwRadOvrd,
        tIPv6FilterParamsFwdRtrId,
        tIPv6FilterParamsNatPolicyName,
        tIPv6FilterParamsFwdLsp,
        tIPv6FilterParamsFwdLspRtrId,
        tIPv6FilterParamsExtNatType,
        tIPv6FilterParamsExtPktLenVal1,
        tIPv6FilterParamsExtPktLenVal2,
        tIPv6FilterParamsExtPktLenOper,
        tIPv6FilterParamsExtHopLimitVal1,
        tIPv6FilterParamsExtHopLimitVal2,
        tIPv6FilterParamsExtHopLimitOper,
        tIPv6FilterParamsExtEsi,
        tIPv6FilterParamsExtFwdEsiSvcId,
        tIPv6FilterParamsExtFwdEsiVRtrId,
        tIPv6FilterParamsExtFwdEsiSFIp,
        tIPv6FilterParamsExtFwdEsiVasIf,
        tIPFilterParamsExtPktLenVal1,
        tIPFilterParamsExtPktLenVal2,
        tIPFilterParamsExtPktLenOper,
        tIPFilterParamsExtTTLVal1,
        tIPFilterParamsExtTTLVal2,
        tIPFilterParamsExtTTLOper,
        tIPFilterParamsExtEsi,
        tIPFilterParamsExtFwdEsiSvcId,
        tIPFilterParamsExtFwdEsiVRtrId,
        tIPFilterParamsExtFwdEsiSFIp,
        tIPFilterParamsExtFwdEsiVasIf
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted objects in 21.0 supporting management of filter
         action via Params tables via SNMP and URL tests on Nokia SROS series
         systems."
    ::= { tFilterMIBGroups 116 }

tIPFilterV21v0Group              OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsExtTbleLstChgd,
        tIPFilterParamsExtLastChanged,
        tIPFilterSharedPccRuleInsrtPt,
        tIPFilterSharedPccRuleInsrtSize,
        tIPFilterSharedPccRuleNbrInsrtd,
        tIPFilterChainToSystemFilter,
        tIPFilterParamsExtEgressPBR,
        tIPFilterParamsExtPbrDwnActOvr,
        tIPFilterRowStatus,
        tIPFilterScope,
        tIPFilterDescription,
        tIPFilterDefaultAction,
        tIPFilterRadiusInsertPt,
        tIPFilterRadiusInsertSize,
        tIPFilterCreditCntrlInsertPt,
        tIPFilterCreditCntrlInsertSize,
        tIPFilterSubInsertHighWmark,
        tIPFilterSubInsertLowWmark,
        tIpFilterCreditCntrlNbrInsertd,
        tIpFilterRadiusNbrInsertd,
        tIPFilterHostSharedInsertPt,
        tIPFilterHostSharedInsertSize,
        tIpFilterHostSharedNbrInsertd,
        tIPFilterHostSharedHighWmark,
        tIPFilterHostSharedLowWmark,
        tIPFilterNbrHostSharedFltrs,
        tIPFilterParamsRowStatus,
        tIPFilterParamsLogId,
        tIPFilterParamsDescription,
        tIPFilterParamsSourceIpAddr,
        tIPFilterParamsSourceIpMask,
        tIPFilterParamsDestinationIpAddr,
        tIPFilterParamsDestinationIpMask,
        tIPFilterParamsProtocol,
        tIPFilterParamsSourcePortValue1,
        tIPFilterParamsSourcePortValue2,
        tIPFilterParamsSourcePortOperator,
        tIPFilterParamsDestPortValue1,
        tIPFilterParamsDestPortValue2,
        tIPFilterParamsDestPortOperator,
        tIPFilterParamsDSCP,
        tIPFilterParamsFragment,
        tIPFilterParamsOptionPresent,
        tIPFilterParamsIpOptionValue,
        tIPFilterParamsIpOptionMask,
        tIPFilterParamsMultipleOption,
        tIPFilterParamsTcpSyn,
        tIPFilterParamsTcpAck,
        tIPFilterParamsIcmpCode,
        tIPFilterParamsIcmpType,
        tIPFilterParamsCflowdSample,
        tIPFilterParamsCflowdIfSample,
        tIPFilterParamsFwdSvcId,
        tIPFilterParamsIngressHitCount,
        tIPFilterParamsEgressHitCount,
        tIPFilterParamsLogInstantiated,
        tIPFilterParamsActiveDest,
        tIPFilterParamsSrcIpFullMask,
        tIPFilterParamsDestIpFullMask,
        tIPFilterParamsIngrHitByteCount,
        tIPFilterParamsEgrHitByteCount,
        tFltrGrpInsrtdEntriesFilterType,
        tFltrGrpInsrtdEntriesFilterId,
        tFltrGrpInsrtdEntriesApplication,
        tFltrGrpInsrtdEntriesLocation,
        tFltrGrpInsrtdEntriesResult,
        tFltrGrpInsrtdEntriesFeedback,
        tFltrGrpInsrtdEntriesExecute,
        tIPFilterParamsSrcRouteOption,
        tIPFilterParamsPortSelector,
        tIPFilterParamsSrcPortList,
        tIPFilterParamsDstPortList,
        tIPFilterParamsExtTbleLstChgd,
        tIPFilterParamsExtLastChanged
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting IP Filters on Nokia 7x50 ESS/SR series
         systems 14.0 release."
    ::= { tFilterMIBGroups 117 }

tIPv6FilterV21v0Group            OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterSharedPccRuleInsrtPt,
        tIPv6FilterSharedPccRuleInsrtSiz,
        tIPv6FilterSharedPccRuleNbrInsrt,
        tIPv6FilterChainToSystemFilter,
        tIPv6FilterParamsExtEgressPBR,
        tIPv6FilterParamsExtPbrDwnActOvr,
        tIPv6FilterRowStatus,
        tIPv6FilterScope,
        tIPv6FilterDescription,
        tIPv6FilterDefaultAction,
        tIPv6FilterRadiusInsertPt,
        tIPv6FilterRadiusInsertSize,
        tIPv6FilterCreditCntrlInsertPt,
        tIPv6FilterCreditCntrlInsertSize,
        tIPv6FilterSubInsertHighWmark,
        tIPv6FilterSubInsertLowWmark,
        tIpv6FilterCreditCntrlNbrInsertd,
        tIpv6FilterRadiusNbrInsertd,
        tIPv6FilterHostSharedInsertPt,
        tIPv6FilterHostSharedInsertSize,
        tIpv6FilterHostSharedNbrInsertd,
        tIPv6FilterHostSharedHighWmark,
        tIPv6FilterHostSharedLowWmark,
        tIPv6FilterNbrHostSharedFltrs,
        tIPv6FilterParamsRowStatus,
        tIPv6FilterParamsLogId,
        tIPv6FilterParamsDescription,
        tIPv6FilterParamsSourceIpAddr,
        tIPv6FilterParamsSourceIpMask,
        tIPv6FilterParamsDestinationIpAddr,
        tIPv6FilterParamsDestinationIpMask,
        tIPv6FilterParamsNextHeader,
        tIPv6FilterParamsSourcePortValue1,
        tIPv6FilterParamsSourcePortValue2,
        tIPv6FilterParamsSourcePortOperator,
        tIPv6FilterParamsDestPortValue1,
        tIPv6FilterParamsDestPortValue2,
        tIPv6FilterParamsDestPortOperator,
        tIPv6FilterParamsDSCP,
        tIPv6FilterParamsTcpSyn,
        tIPv6FilterParamsTcpAck,
        tIPv6FilterParamsIcmpCode,
        tIPv6FilterParamsIcmpType,
        tIPv6FilterParamsCflowdSample,
        tIPv6FilterParamsCflowdIfSample,
        tIPv6FilterParamsFwdSvcId,
        tIPv6FilterParamsIngressHitCount,
        tIPv6FilterParamsEgressHitCount,
        tIPv6FilterParamsLogInstantiated,
        tIPv6FilterParamsActiveDest,
        tIPv6FilterParamsIngrHitByteCount,
        tIPv6FilterParamsEgrHitByteCount,
        tIPv6FilterParamsSrcIpPrefixList,
        tIPv6FilterParamsDstIpPrefixList,
        tIPv6FilterParamsFragment,
        tIPv6FilterParamsHopByHopOpt,
        tIPv6FilterParamsRoutingType0,
        tIPv6FilterParamsPortSelector,
        tIPv6FilterParamsSrcPortList,
        tIPv6FilterParamsDstPortList,
        tIPv6FilterParamsSrcIpFullMask,
        tIPv6FilterParamsDstIpFullMask,
        tIPv6FilterParamsFlowLabel,
        tIPv6FilterParamsFlowLabelMask,
        tIPv6FilterParamsExtTbleLstChgd,
        tIPv6FilterParamsExtLastChanged,
        tIPv6FilterParamsExtAhExtHdr,
        tIPv6FilterParamsExtEspExtHdr
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of IPv6 filter objects on
         Nokia 7x50 ESS/SR series systems 14.0 release."
    ::= { tFilterMIBGroups 118 }

tMacFilterV21v0Group             OBJECT-GROUP
    OBJECTS     {
        tMacFilterParamsPbrDwnActOvr,
        tMacFilterRowStatus,
        tMacFilterScope,
        tMacFilterDescription,
        tMacFilterDefaultAction,
        tMacFilterParamsRowStatus,
        tMacFilterParamsLogId,
        tMacFilterParamsDescription,
        tMacFilterParamsFrameType,
        tMacFilterParamsSrcMAC,
        tMacFilterParamsSrcMACMask,
        tMacFilterParamsDstMAC,
        tMacFilterParamsDstMACMask,
        tMacFilterParamsDot1pValue,
        tMacFilterParamsDot1pMask,
        tMacFilterParamsEtherType,
        tMacFilterParamsDsap,
        tMacFilterParamsDsapMask,
        tMacFilterParamsSsap,
        tMacFilterParamsSsapMask,
        tMacFilterParamsSnapPid,
        tMacFilterParamsSnapOui,
        tMacFilterParamsIngressHitCount,
        tMacFilterParamsEgressHitCount,
        tMacFilterParamsLogInstantiated,
        tMacFilterParamsFwdSvcId,
        tMacFilterParamsRedirectURL,
        tMacFilterParamsIngrHitByteCount,
        tMacFilterParamsEgrHitByteCount,
        tMacFilterParamsLowISID,
        tMacFilterParamsHighISID,
        tMacFilterType
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting management of mac filter objects on
         Nokia SROS series systems 8.0 release."
    ::= { tFilterMIBGroups 119 }

tFilterMatchTTLGroup             OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsExtMxTTLVal1,
        tIPFilterParamsExtMxTTLVal2,
        tIPFilterParamsExtMxTTLOper,
        tIPv6FilterParamsExtMxHopLmtVal1,
        tIPv6FilterParamsExtMxHopLmtVal2,
        tIPv6FilterParamsExtMxHopLmtOper
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting match TTL/Hop Limit on Nokia 7x50
         ESS/SR series systems 21.10 release."
    ::= { tFilterMIBGroups 120 }

tFltrMatchSrcOrDstIpGroup        OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterParamsIpSelector,
        tIPFilterParamsIpSelector
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter match source or destination IP
         criterion on Nokia 7x50 ESS/SR series systems 21.2 release."
    ::= { tFilterMIBGroups 121 }

tFltrLagSharedPolicerGroup       OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterSharedPolicer,
        tIPFilterSharedPolicer
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter LAG shared BPS policers on
         Nokia 7x50 ESS/SR series systems 21.2 release."
    ::= { tFilterMIBGroups 122 }

tFltrMatchTcpEstGroup            OBJECT-GROUP
    OBJECTS     {
        tIPFilterParamsExtTcpEst,
        tIPv6FilterParamsExtTcpEst
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter TCP established match on Nokia
         7x50 ESS/SR series systems 21.2 release."
    ::= { tFilterMIBGroups 123 }

tFilterNotificationsV23v0Group   NOTIFICATION-GROUP
    NOTIFICATIONS {
        tFilterEmbedFlowspecOperStateChg
    }
    STATUS      current
    DESCRIPTION
        "The group of notifications supporting management of filter
         notifications on Nokia SROS series systems 23.0 release."
    ::= { tFilterMIBGroups 124 }

tFilterObsoleteNotifGroup        NOTIFICATION-GROUP
    NOTIFICATIONS {
        tFilterEmbedVsdOperStateChg
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted notifications supporting management of filter
         notifications on Nokia SROS series systems 23.0 release."
    ::= { tFilterMIBGroups 125 }

tFltrFwdSrv6PlcyGrp              OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrFwdSrv6PlcyEndptAddrTp,
        tIPvXFltrFwdSrv6PlcyEndptAddr,
        tIPvXFltrFwdSrv6PlcyColor,
        tIPvXFltrFwdSrv6PlcySvcSidAddrTp,
        tIPvXFltrFwdSrv6PlcySvcSid
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting forwarding to a tunnel identified by
         an SRv6 policy endpoint and color in Nokia SROS series systems in
         release 23.7."
    ::= { tFilterMIBGroups 127 }

tLiMacFilterMatchVlanIdGrp       OBJECT-GROUP
    OBJECTS     {
        tLiMacFilterParamsSapPortId,
        tLiMacFilterParamsSapEncapType,
        tLiMacFilterParamsSapEncapVal,
        tLiMacFilterParamsOuterTagVal
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting LI filter vlan id matching in Nokia
         SROS series systems in release 23.10."
    ::= { tFilterMIBGroups 128 }

tFltrPktLenListGrp               OBJECT-GROUP
    OBJECTS     {
        tFltrPktLenListTblLastChg,
        tFltrPktLenListRowStatus,
        tFltrPktLenListLastChanged,
        tFltrPktLenListDescription,
        tFltrPktLenListItemTblLastChg,
        tFltrPktLenListItemRowStatus,
        tIPFilterParamsExtPktLenList,
        tIPv6FilterParamsExtPktLenList
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting the management of packet length lists
         for filters on Nokia SROS series systems release 24.3."
    ::= { tFilterMIBGroups 130 }

tFilterIPvXRedActionV24v0Group   OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrEntryActionTblLChg,
        tIPvXFltrEntryActRowStatus,
        tIPvXFltrEntryActLastChanged,
        tIPvXFltrEntryActAction,
        tIPvXFltrEntryActFwdNHIpAddrType,
        tIPvXFltrEntryActFwdNHIpAddr,
        tIPvXFltrEntryActFwdNHIndirect,
        tIPvXFltrEntryActFwdRedPlcy,
        tIPvXFltrEntryActFwdSapPortId,
        tIPvXFltrEntryActFwdSapEncapVal,
        tIPvXFltrEntryActFwdSdpBind,
        tIPvXFltrEntryActRedirectURL,
        tIPvXFltrEntryActRdirAllwRadOvr,
        tIPvXFltrEntryActFwdRtrId,
        tIPvXFltrEntryActNatPolicyName,
        tIPvXFltrEntryActNatType,
        tIPvXFltrEntryActFwdLsp,
        tIPvXFltrEntryActFwdLspRtrId,
        tIPvXFltrEntryActPktLenVal1,
        tIPvXFltrEntryActPktLenVal2,
        tIPvXFltrEntryActPktLenOper,
        tIPvXFltrEntryActTTLVal1,
        tIPvXFltrEntryActTTLVal2,
        tIPvXFltrEntryActTTLOper,
        tIPvXFltrEntryActEsi,
        tIPvXFltrEntryActFwdEsiSvcId,
        tIPvXFltrEntryActFwdEsiVRtrId,
        tIPvXFltrEntryActFwdEsiSFIpType,
        tIPvXFltrEntryActFwdEsiSFIp,
        tIPvXFltrEntryActFwdEsiVasIf,
        tIPFilterParamsExtStickyDst,
        tIPFilterParamsExtDownloadAct,
        tIPFilterParamsExtHoldRemain,
        tIPv6FilterParamsExtStickyDst,
        tIPv6FilterParamsExtDownloadAct,
        tIPv6FilterParamsExtHoldRemain,
        tIPvXFltrEntryActPbrTargetStatus,
        tIPvXFltrEntryActRateLimit,
        tIPvXFltrEntryActRateLimitMbs,
        tIPvXFltrEntryActRateLimitPps
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting redundant ip filter actions on Nokia
         7x50 ESS/SR series systems 24.0 release."
    ::= { tFilterMIBGroups 131 }

tFilterObsoleteNhItfcGroup       OBJECT-GROUP
    OBJECTS     {
        tIPvXFltrEntryActFwdNHInterface
    }
    STATUS      current
    DESCRIPTION
        "The group of obsoleted object in 24.3 supporting filter action forward
         to  next-hop interface."
    ::= { tFilterMIBGroups 132 }

tFilterPolicerGroup              OBJECT-GROUP
    OBJECTS     {
        tFltrPolicerTblLastChg,
        tFltrPolicerRowStatus,
        tFltrPolicerLastChanged,
        tFltrPolicerDescription,
        tFltrPolicerPIR,
        tFltrPolicerPPSPIR,
        tFltrPolicerMBS,
        tFltrPolicerScope,
        tIPvXFltrEntryActRateLimitPlcr,
        tFltrPlcrStatSysScopeIngHitCnt,
        tFltrPlcrStatSysScopeIngDrop,
        tFltrPlcrStatSysScopeIngFwd,
        tFltrPlcrStatSysScopeIngHitCntB,
        tFltrPlcrStatSysScopeIngDropB,
        tFltrPlcrStatSysScopeIngFwdB,
        tFltrPlcrStatSysScopeEgrHitCnt,
        tFltrPlcrStatSysScopeEgrDrop,
        tFltrPlcrStatSysScopeEgrFwd,
        tFltrPlcrStatSysScopeEgrHitCntB,
        tFltrPlcrStatSysScopeEgrDropB,
        tFltrPlcrStatSysScopeEgrFwdB,
        tFltrPlcrStatFltrScopeIngHitCnt,
        tFltrPlcrStatFltrScopeIngDrop,
        tFltrPlcrStatFltrScopeIngFwd,
        tFltrPlcrStatFltrScopeIngHitCntB,
        tFltrPlcrStatFltrScopeIngDropB,
        tFltrPlcrStatFltrScopeIngFwdB,
        tFltrPlcrStatFltrScopeEgrHitCnt,
        tFltrPlcrStatFltrScopeEgrDrop,
        tFltrPlcrStatFltrScopeEgrFwd,
        tFltrPlcrStatFltrScopeEgrHitCntB,
        tFltrPlcrStatFltrScopeEgrDropB,
        tFltrPlcrStatFltrScopeEgrFwdB
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting policer management for filters  in
         Nokia SROS series systems in release 25.3."
    ::= { tFilterMIBGroups 133 }

tFltrFilterSetGroup              OBJECT-GROUP
    OBJECTS     {
        tFltrFilterSetTableLstChng,
        tFltrFilterSetRowStatus,
        tFltrFilterSetLastChanged,
        tFltrFilterSetDescription,
        tFltrFilterSetMacFilterId,
        tFltrFilterSetIpFilterId,
        tFltrFilterSetIpv6FilterId
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter set management for filters  in
         Nokia SROS series systems in release 24.10."
    ::= { tFilterMIBGroups 134 }

tIPvXFilterParamsV25v0Group      OBJECT-GROUP
    OBJECTS     {
        tIPv6FilterParamsExtRoutingType4
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting filter params for filters in Nokia
         SROS series systems in release 25.7."
    ::= { tFilterMIBGroups 135 }

tFltrGreTunTempIpv6Group         OBJECT-GROUP
    OBJECTS     {
        tFltrGreTunTempIpv6SrcAddr,
        tFltrGreTunTempIpv6GreKeyIfIndex,
        tFltrGreTunTempIpv6SkipHopDecr,
        tFltrGreTunTempIpv6DstTblLstChg,
        tFltrGreTunTempIpv6DstLstChg,
        tFltrGreTunTempIpv6DstRowStatus
    }
    STATUS      current
    DESCRIPTION
        "The group of objects supporting ipv6 setting for GRE tunnel templates
         on Nokia 7x50 ESS/SR series systems 22.7 release."
    ::= { tFilterMIBConformance 123 }

tFilterNotificationsPrefix       OBJECT IDENTIFIER ::= { tmnxSRNotifyPrefix 21 }

tFilterNotifications             OBJECT IDENTIFIER ::= { tFilterNotificationsPrefix 0 }

tIPFilterPBRPacketsDrop          NOTIFICATION-TYPE
    OBJECTS     {
        tIPFilterParamsForwardNHInterface,
        tFilterPBRDropReason
    }
    STATUS      current
    DESCRIPTION
        "The tIPFilterPBRPacketsDrop event is generated either when the
         configuration of a forwarding action refers to an invalid/unconfigured
         next-hop or if the active interface goes down operationally in the
         process of active filtering."
    ::= { tFilterNotifications 1 }

tFilterEntryActivationFailed     NOTIFICATION-TYPE
    OBJECTS     {
        tFilterParmRow,
        tFilterAlarmDescription
    }
    STATUS      obsolete
    DESCRIPTION
        "The tFilterEntryActivationFailed event can only be generated for
         entries that are controlled by a tmnxTimeRangeEntry. If the
         tmnxTimeRangeEntry becomes active the indicated entry must be
         installed. The event is generated when this installation failed
         because of resource problems.

         This object is obsoleted in release 14.0."
    ::= { tFilterNotifications 2 }

tFilterEntryActivationRestored   NOTIFICATION-TYPE
    OBJECTS     {
        tFilterParmRow,
        tFilterAlarmDescription
    }
    STATUS      obsolete
    DESCRIPTION
        "The tFilterEntryActivationRestored event can only be generated for
         entries that are controlled by a tmnxTimeRangeEntry. If the
         tmnxTimeRangeEntry becomes active the indicated entry must be
         installed. The event tFilterEntryActivationFailed is generated when
         this installation originally failed because of resources problems, The
         notification tFilterEntryActivationRestored is sent when either the
         time range associated with the filter is no longer active, or when the
         filter entry was installed due to the availability of new resources.

         This object is obsoleted in release 14.0."
    ::= { tFilterNotifications 3 }

tFilterSubInsSpaceAlarmRaised    NOTIFICATION-TYPE
    OBJECTS     {
        tFilterType,
        tFilterId,
        tFilterSubInsSpaceOwner,
        tFilterThresholdReached
    }
    STATUS      current
    DESCRIPTION
        "The tFilterSubInsSpaceAlarmRaised notification is generated when the
         utilization of a filter entry range that was reserved for filter entry
         insertion increases to the configured high watermark for his filter"
    ::= { tFilterNotifications 4 }

tFilterSubInsSpaceAlarmCleared   NOTIFICATION-TYPE
    OBJECTS     {
        tFilterType,
        tFilterId,
        tFilterSubInsSpaceOwner,
        tFilterThresholdReached
    }
    STATUS      current
    DESCRIPTION
        "The tFilterSubInsSpaceAlarmCleared notification is generated when the
         utilization of a filter entry range that was reserved for filter entry
         insertion dropped below to the configured low watermark for his
         filter."
    ::= { tFilterNotifications 5 }

tFilterSubInsFltrEntryDropped    NOTIFICATION-TYPE
    OBJECTS     {
        tFilterType,
        tFilterId,
        tFilterSubInsSpaceOwner,
        tFilterAlarmDescription
    }
    STATUS      current
    DESCRIPTION
        "The tFilterSubInsFltrEntryDropped notification is generated when a
         request to insert a filter entry was not successful."
    ::= { tFilterNotifications 6 }

tFilterBgpFlowSpecProblem        NOTIFICATION-TYPE
    OBJECTS     {
        tFilterType,
        tFltrFlowSpecVrtrId,
        tFltrFlowSpecProblem,
        tFltrFlowSpecProblemDescription,
        tFltrFLowSpecNLRI
    }
    STATUS      current
    DESCRIPTION
        "The tFilterBgpFlowSpecProblem notification is generated when a BGP
         flowspec NLRI is received in the filter module that cannot be treated
         - i.e. for which no filter entry is installed in the system, or when
         there is a problem inserting (new) or reshuffling (existing) flowspec
         or merged filter entries."
    ::= { tFilterNotifications 7 }

tFilterApplyPathProblem          NOTIFICATION-TYPE
    OBJECTS     {
        tFltrPrefixListType,
        tFltrPrefixListName,
        tFltrApplyPathSource,
        tFltrApplyPathIndex,
        tFilterAlarmDescription
    }
    STATUS      current
    DESCRIPTION
        "The tFilterApplyPathProblem notification is generated when a problem
         is encountered for a configured apply-path rule.

         [CAUSE] Failed to add prefix/prefixes specified by the apply-path rule
         to the prefix list likely due to insufficient resources.

         [EFFECT] Prefix list does not contain all prefixes specified by the
         apply-path rule.

         [RECOVERY] Release resources by removing unnecessary prefixes or
         specify more specific apply-path rule."
    ::= { tFilterNotifications 8 }

tFilterRadSharedFltrAlarmRaised  NOTIFICATION-TYPE
    OBJECTS     {
        tFilterType,
        tFilterId,
        tFilterThresholdReached
    }
    STATUS      current
    DESCRIPTION
        "The tFilterRadSharedFltrAlarmRaised notification is generated when the
         number of Radius Shared Filters that are dynamically created in the
         system increases to the configured high watermark for the indicated
         filter."
    ::= { tFilterNotifications 9 }

tFilterRadSharedFltrAlarmClear   NOTIFICATION-TYPE
    OBJECTS     {
        tFilterType,
        tFilterId,
        tFilterThresholdReached
    }
    STATUS      current
    DESCRIPTION
        "The tFilterRadSharedFltrAlarmClear notification is generated when the
         number of Radius Shared Filters that are dynamically created in the
         system dropped below to the configured low watermark for the indicated
         filter."
    ::= { tFilterNotifications 10 }

tFilterEmbeddingOperStateChange  NOTIFICATION-TYPE
    OBJECTS     {
        tFilterEmbeddedRefOperState,
        tFltrNotifDescription
    }
    STATUS      current
    DESCRIPTION
        "The tFilterEmbeddingOperStateChange notification is generated when the
         operational status of an embedded filter has changed.

         [CAUSE] This notification may be triggered for the following reasons:

         1) An attempt to embed an embedded filter into embedding filter was done.
         2) An attempt to recover an embedding that is operationally down
            was done.
         3) An attempt to change the admin state of an embedding was done.
         4) The operational state of an embedding has changed to inactive
            due to lack of resources.

         [EFFECT] The effect depends on the new state. If the new state is
         'active', the embedding of the filter was successful.

         If the new state is 'embedFailedNoResources' the embedding was not
         successful due to lack of resources.

         If the new state is 'inactive' and the previous state was 'active'
         then the embedded entries were removed. Otherwise the embedding filter
         was not changed.

         [RECOVERY] If the new state is 'active' or 'inactive', no action is
         required.

         If the new state is 'embedFailedNoResources', an attempt to recover
         the operational state can be done by removal and reapplication of the
         embedding."
    ::= { tFilterNotifications 11 }

tFilterEmbedOpenflowOperStateChg NOTIFICATION-TYPE
    OBJECTS     {
        tFilterEmbedOpenflowOperState,
        tFltrNotifDescription
    }
    STATUS      current
    DESCRIPTION
        "The tFilterEmbedOpenflowOperStateChg notification is generated when
         the operational state of an open-flow switch embedded in a filter with
         scope other than 'embedded' has changed.

         [CAUSE] This notification may be triggered for the following reasons:

         1) An attempt to embed an open-flow switch into an embedding filter
            was done.
         2) An attempt to recover an open-flow embedding that is operationally
            down was done.
         3) An attempt to change the admin state of an open-flow embedding
            was done.
         4) The operational state of an open-flow embedding has changed
            to inactive due to lack of resources.

         [EFFECT] The effect depends on the new state. If the new state is
         'active', the embedding of an open-flow switch was successful.

         If the new state is 'embedFailedNoResources' the embedding was not
         successful due to lack of resources.

         If the new state is 'inactive' and the previous state was 'active'
         then the open-flow switch entries were removed. Otherwise the
         embedding filter was not changed.

         [RECOVERY] If the new state is 'active' or 'inactive', no action is
         required.

         If the new state is 'embedFailedNoResources', an attempt to recover
         the operational state can be done by removal and reapplication of the
         open-flow embedding."
    ::= { tFilterNotifications 12 }

tFilterTmsEvent                  NOTIFICATION-TYPE
    OBJECTS     {
        tFltrMdaId,
        tFltrNotifDescription
    }
    STATUS      obsolete
    DESCRIPTION
        "The tFilterTmsEvent notification is generated by the systems filter
         module to report an event related to the Threat Management System
         (TMS).

         Receiving the tFilterTmsEvent notification is an indication that the
         TMS system may not be fully operational."
    ::= { tFilterNotifications 13 }

tFilterEmbedFlowspecOperStateChg NOTIFICATION-TYPE
    OBJECTS     {
        tFilterEmbedFlowspecRtrId,
        tFilterEmbedFlowspecOperState,
        tFltrNotifDescription
    }
    STATUS      current
    DESCRIPTION
        "The tFilterEmbedFlowspecOperStateChg notification is generated when
         the operational state of a set of flowspec rules embedded in an IP or
         IPv6 filter with scope other than 'embedded' has changed.

         [CAUSE] This notification may be triggered for the following reasons:

         1) An attempt to embed a set of flowspec rules into an embedding
            filter was done.
         2) An attempt to recover a flowspec rules embedding that is
            operationally down was done.
         3) An attempt to change the admin state of a flowspec rules embedding
            was done.
         4) The operational state of a flowspec rules embedding has changed
            to inactive due to lack of resources.

         [EFFECT] The effect depends on the new state. If the new state is
         'active', the embedding of a set of flowspec rules was successful.

         If the new state is 'embedFailedNoResources' the embedding was not
         successful due to lack of resources.

         If the new state is 'inactive' and the previous state was 'active'
         then the set of flowspec rules were removed.

         Otherwise the embedding filter was not changed.

         [RECOVERY] If the new state is 'active' or 'inactive', no action is
         required.

         If the new state is 'embedFailedNoResources', an attempt to recover
         the operational state can be done by removal and reapplication of the
         flowspec rules embedding."
    ::= { tFilterNotifications 14 }

tFilterEmbedVsdOperStateChg      NOTIFICATION-TYPE
    OBJECTS     {
        tFltrNotifDescription
    }
    STATUS      obsolete
    DESCRIPTION
        "The tFilterEmbedVsdOperStateChg notification is generated when the
         operational state of an embedding of a filter managed by a VSD
         controller in a filter with scope other than 'embedded' has changed.

         [CAUSE] This notification may be triggered for the following reasons:

         1) An attempt to embed a filter managed by a VSD controller
            into an embedding filter was done.
         2) An attempt to recover an embedding that is operationally down
            was done.
         3) An attempt to change the admin state of an embedding was done.
         4) The operational state of an embedding has changed to inactive
            due to lack of resources.

         [EFFECT] The effect depends on the new state. If the new state is
         'active', the embedding of a filter managed by a VSD controller was
         successful.

         If the new state is 'embedFailedNoResources' the embedding was not
         successful due to lack of resources.

         If the new state is 'inactive' and the previous state was 'active'
         then the embedded entries were removed.

         Otherwise the embedding filter was not changed.

         [RECOVERY] If the new state is 'active' or 'inactive', no action is
         required.

         If the new state is 'embedFailedNoResources', an attempt to recover
         the operational state can be done by removal and reapplication of the
         embedding."
    ::= { tFilterNotifications 15 }

tFilterRPActiveDestChangeEvent   NOTIFICATION-TYPE
    OBJECTS     {
        tFilterRPActiveDestAddrType,
        tFilterRPActiveDestAddr,
        tFltrNotifDescription
    }
    STATUS      current
    DESCRIPTION
        "The tFilterRPActiveDestChangeEvent notification is generated when the
         active destination of a redirect policy changes.

         [CAUSE] This notification was triggered because active destination of
         a redirect policy has changed.

         [EFFECT] Traffic hitting filter entries with forward redirect-policy
         set to this redirect policy will be directed toward the new active
         destination.

         [RECOVERY] No recovery action is required."
    ::= { tFilterNotifications 16 }

tFltrLiRsvdBlockRangeChangeEvent NOTIFICATION-TYPE
    OBJECTS     {
        tLiReservedBlockStart,
        tLiReservedBlockSize
    }
    STATUS      current
    DESCRIPTION
        "The tFltrLiRsvdBlockRangeChangeEvent notification is generated when
         the LI reserved block range changes.

         [CAUSE] This notification was triggered because LI reserved block
         range has changed.

         [EFFECT] This change may rearrange filters entries and may temporarily
         disrupt current interception.

         [RECOVERY] No recovery action is required."
    ::= { tFilterNotifications 17 }

END
