-- Extracted from RFC 7630
SNMP-USM-HMAC-SHA2-MIB DEFINITIONS ::= BEGIN
    IMPORTS
        MODULE-IDENTITY, OBJECT-IDENTITY,
    snmpModules             FROM SNMPv2-SMI          -- [RFC2578]
    snmpAuthProtocols       FROM SNMP-FRAMEWORK-MIB; -- [RFC3411]

snmpUsmHmacSha2MIB MODULE-IDENTITY
    LAST-UPDATED    "201508130000Z"       -- 13 August 2015, midnight
    ORGANIZATION    "SNMPv3 Working Group"
    CONTACT-INFO    "WG email: OPSAWG@ietf.org
                    Subscribe:
                        https://www.ietf.org/mailman/listinfo/opsawg
                    Editor:    Johannes Merkle
                               secunet Security Networks
                    Postal:    Mergenthaler Allee 77
                               D-65760 Eschborn
                               Germany
                    Phone:     +49 20154543091
                    Email:     johannes.merkle@secunet.com
                    Co-Editor: Manfred Lochter
                               Bundesamt fuer Sicherheit in der
                               Informationstechnik (BSI)
                    Postal:    Postfach 200363
                               D-53133 Bonn
                               Germany
                    Phone:     +49 228 9582 5643
                    Email:     manfred.lochter@bsi.bund.de"

    DESCRIPTION     "Definitions of Object Identities needed
                    for the use of HMAC-SHA2 by SNMP's User-based
                    Security Model.

          Copyright (c) 2015 IETF Trust and the persons identified
          as authors of the code.  All rights reserved.

          Redistribution and use in source and binary forms, with
          or without modification, is permitted pursuant to, and
          subject to the license terms contained in, the Simplified
          BSD License set forth in Section 4.c of the IETF Trust's
          Legal Provisions Relating to IETF Documents
          (http://trustee.ietf.org/license-info)."

    REVISION    "201508130000Z"       -- 13 August 2015, midnight
    DESCRIPTION "Initial version, published as RFC 7630"
::= { snmpModules 235 }

usmHMAC128SHA224AuthProtocol OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION "The Authentication Protocol
                usmHMAC128SHA224AuthProtocol uses HMAC-SHA-224 and
                truncates output to 128 bits."
    REFERENCE   "- Krawczyk, H., Bellare, M., and R. Canetti, HMAC:
                Keyed-Hashing for Message Authentication, RFC 2104.
                - National Institute of Standards and Technology,
                Secure Hash Standard (SHS), FIPS PUB 180-4, 2012."
    ::= { snmpAuthProtocols 4 }

usmHMAC192SHA256AuthProtocol OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION "The Authentication Protocol
                usmHMAC192SHA256AuthProtocol uses HMAC-SHA-256 and
                truncates output to 192 bits."
    REFERENCE   "- Krawczyk, H., Bellare, M., and R. Canetti, HMAC:
                Keyed-Hashing for Message Authentication, RFC 2104.
                - National Institute of Standards and Technology,
                Secure Hash Standard (SHS), FIPS PUB 180-4, 2012."
    ::= { snmpAuthProtocols 5 }

usmHMAC256SHA384AuthProtocol OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION "The Authentication Protocol
                usmHMAC256SHA384AuthProtocol uses HMAC-SHA-384 and
                truncates output to 256 bits."
    REFERENCE   "- Krawczyk, H., Bellare, M., and R. Canetti, HMAC:
                Keyed-Hashing for Message Authentication, RFC 2104.
                - National Institute of Standards and Technology,
                Secure Hash Standard (SHS), FIPS PUB 180-4, 2012."
    ::= { snmpAuthProtocols 6 }

usmHMAC384SHA512AuthProtocol OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION "The Authentication Protocol
                usmHMAC384SHA512AuthProtocol uses HMAC-SHA-512 and
                truncates output to 384 bits."
    REFERENCE   "- Krawczyk, H., Bellare, M., and R. Canetti, HMAC:
                Keyed-Hashing for Message Authentication, RFC 2104.
                - National Institute of Standards and Technology,
                Secure Hash Standard (SHS), FIPS PUB 180-4, 2012."
    ::= { snmpAuthProtocols 7 }

END

